**3GPP TSG-RAN WG4 Meeting #97-e *R4-2017178***

**Electronic Meeting, Nov 2 – 13, 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **38.133** | **CR** | **-** | **rev** | **1** | **Current version:** | **16.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | TC for RRC based spatial relation switch associated with a known DL-RS |
|  |  |
| ***Source to WG:*** | Huawei, HiSilicon |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_RRM\_Enh-Perf |  | ***Date:*** | 2020-11-9 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | The test case for RRC based spatial relation switch associated with a known DL-RS in EN-DC is specified. |
|  |  |
| ***Summary of change:*** | Specifying the test case for RRC based spatial relation switch associated with a known DL-RS in EN-DC. |
|  |  |
| ***Consequences if not approved:*** | The specification is incomplete. |
|  |  |
| ***Clauses affected:*** |  New A.5.5.X.Y |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

----------------------------------------------------- Beginning of Change 1 ------------------------------------------------------------

#### A.5.5.X.Y RRC based spatial relation switch

##### A.5.5.X.Y.1 E-UTRAN – NR PSCell FR2 spatial relation switch associated with a known DL-RS

###### A.5.5.X.Y.1.1 Test Purpose and Environment

The purpose of this test is to verify the RRC based spatial relation switch delay requirement defined in clause 8.12.5 by a UE capable of beam correspondence without the need for UL beam sweeping. Supported test configurations are shown in Table A.5.5.X.Y.1.1-1.

The test scenario comprises of one E-UTRA PCell (Cell 1), and one NR PSCell (Cell 2) as given in Table A.5.5.X.Y.1.1-2. Cell-specific parameters of E-UTRA PCell are specified in Table A.3.7.2.1-1 and Cell-specific parameters of NR PSCell is specified in Table A.5.5.X.Y.1.1-3 below. The OTA related test parameters for FR2 is shown in Table A.5.5.X.Y.1.1-4.

Periodic SRS is transmitted on NR PSCell (Cell2), and the SRS configuration is SRSConf.1 given in Table A.5.4.1.1.1-3.

Before the test starts,

- UE is connected to Cell 1 (PCell) on radio channel 1 (PCC), and Cell 2 (PSCell) on radio channel 2 (PSCC).

- UE is configured with 1 SRS-SpatialRelation0 associated with SSB0.

- UE is indicated SRS-SpatialRelation0 as the active SRS spatial relation.

The test consists of two time periods, T1 and T2. During T1 only SSB0 to which SRS-SpatialRelation0 associated is transmitted. UE shall transmits periodic SRS with SRS-SpatialRelation0 of PSCell. At the beginning of T2, the SSB1 corresponding to SRS-SpatialRelation1 starts transmitting. The UE is configured to provide periodic L1-RSRP reports. The test has higher layer parameter *timeRestrictionForChannelMeasurements* configured. In slot n which is within 1280 ms of UE providing L1-RSRP report with results for both SSB0 and SSB1, UE receives a RRC command indicating a switch to transmit periodic SRS with target SRS-SpatialRelation1. The test equipment verifies that UE shall be able to transmit periodic SRS with target spatial relation (SRS-SpatialRelation1) on PSCell in the slot n+ TRRC\_processing+1.

Table A.5.5.X.Y.1.1-1: Supported test configurations

|  |  |
| --- | --- |
| Config | Description |
| 1 | LTE FDD, NR 120 kHz SSB SCS, 100 MHz bandwidth, TDD duplex mode |
| 2 | LTE TDD, NR 120 kHz SSB SCS, 100 MHz bandwidth, TDD duplex mode |
| Note 1: The UE is only required to be tested in one of the supported test configurations. |

Table A.5.5.X.Y.1.1-2: General test parameters for spatial relation switch associated with a known DL-RS

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Unit | Value | Comment |
| E-UTRA RF Channel Number |  | 1 | One E-UTRA radio channel is used for this test |
| NR RF Channel Number |  | 2 | One NR radio channel is used for this test |
| Active PCell |  | Cell 1 | PCell on RF channel number 1. |
| Active PSCell |  | Cell 2 | PSCell on RF channel number 2. |
| CP length |  | Normal |  |
| DRX |  | OFF | For both PCell and PSCell |
| Cell-individual offset for cells on RF channel number 1 | dB | 0 | Individual offset for cells on PCC. |
| Cell-individual offset for cells on RF channel number 2 | dB | 0 | Individual offset for cells on PSCC. |
| T1 | s | 0.2 |  |
| T2 | s | 2 |  |

Table A.5.5.X.Y.1.1-3: NR Cell specific test parameters for spatial relation switch associated with a known DL-RS

|  |  |  |
| --- | --- | --- |
| Parameter | Unit | Cell 2 |
| Frequency Range |  | FR2 |
| Duplex mode |  | TDD |
| TDD configuration |  | TDDConf.3.1 |
| BWchannel |  | 100 MHz: NRB,c = 66 |
| Initial DL BWP Configuration |  | DLBWP.0.2 |
| Dedicated DL BWP Configuration |  | DLBWP.1.1 |
| Initial UL BWP Configuration |  | ULBWP.0.2 |
| Dedicated UL BWP Configuration |  | ULBWP.1.1 |
| PDSCH Reference measurement channel |  | SR.3.1 TDD |
| RMSI CORESET parameters |  | CR.3.1 TDD |
| Dedicated CORESET parameters |  | CCR.3.1 TDD |
| OCNG Patterns |  | OP.1 |
| SSB Configuration |  | SSB.1 FR2 |
| SMTC Configuration |  | SMTC.1 |
| SRS-SpatialRelation0 |  | SRS-SPATIAL.RELATION.0 |
| SRS-SpatialRelation1 |  | SRS-SPATIAL.RELATION.1 |
| reportConfigType |  | ssb-Index-RSRP |
| reportConfigType  |  | periodic |
| Number of reported RS |  | 2 |
| L1-RSRP reporting period | slot | 640 |
| TRS Configuration |  | TRS.2.1 TDD |
| Correlation Matrix and Antenna Configuration |  | 1x2 Low |
| EPRE ratio of PSS to SSS | dB | 0 |
| EPRE ratio of PBCH DMRS to SSS |  |  |
| EPRE ratio of PBCH to PBCH DMRS |  |  |
| EPRE ratio of PDCCH DMRS to SSS |  |  |
| EPRE ratio of PDCCH to PDCCH DMRS |  |  |
| EPRE ratio of PDSCH DMRS to SSS  |  |  |
| EPRE ratio of PDSCH to PDSCH  |  |  |
| EPRE ratio of OCNG DMRS to SSS(Note 1) |  |  |
| EPRE ratio of OCNG to OCNG DMRS (Note 1) |  |  |
| Propagation Condition |  | AWGN |
| Note 1: OCNG shall be used such that both cells are fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols. |

Table A.5.5.X.Y.1.1-4: OTA related test parameters for spatial relation switch associated with a known DL-RS

|  |  |  |
| --- | --- | --- |
| Parameter | Unit | Cell 2 |
|  |  | SSB0 | SSB1 |
|  |  | T1 | T2 | T1 | T2 |
| Angle of arrival  |  | Setup 3 according to clause A.3.15.3 |
| configuration |  | **AoA1** | **AoA2** |
| Assumption for UE beamsNote 6 |  | Rough | Rough |
| NocNote 1 | dBm/15 kHz | -92.1 |
| NocNote 1 | dBm/SCS | -83.1 |
| Ês/Noc | dB | 1 | 1 | 1 | 1 |
| SS-RSRP Note 2 | dBm/120 kHz Note3 | -82.1 | -82.1 | -82.1 | -82.1 |
| IoNote2,Note6 | dBm/95.04 MHz Note4 | -54.9 | -54.9 | -54.9 | -54.9 |
| Note 1: Interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for Noc to be fulfilled.Note 2: SS-RSRP and Io levels have been derived from other parameters for information purposes. They are not settable parameters themselves.Note 3: SS-RSRP minimum requirements are specified assuming independent interference and noise at each receiver antenna port.Note 4: Equivalent power received by an antenna with 0 dBi gain at the centre of the quiet zoneNote 5: As observed with 0dBi gain antenna at the center of the quiet zone.Note 6: Information about types of UE beam is given in B.2.1.3, and does not limit UE implementation or test system implementation |

###### A.5.5.X.Y.1.2 Test Requirements

During T2, UE shall send L1-RSRP report with SSB1 to which SRS-SpatialRelation1 is associated.

After receiving RRC command in slot n, UE shall be able to transmit target periodic SRS with SRS-SpatialRelation1 on PSCell in the slot n+ TRRC\_processing/*NR slot length* +1.

------------------------------------------------------------- End of change 1 ------------------------------------------------------------