**3GPP TSG-RAN WG4 Meeting #97-e *R4-2017199***

**Electronic Meeting, 2nd Nov – 13th Nov 2020**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.133** | **CR** | 1308 | **rev** | **1** | **Current version:** | **16.5.0** |  |
|  | | | | | | | | |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | CR to 38.133: Correction to mandatory gap pattern | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | ZTE | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_newRAT-Core | | | | |  | ***Date:*** | | | 2020-11-10 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | F |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12) Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The UE capability for NR only measurement are introduced as follows.  ***supportedGapPattern-NRonly***  Indicates measurement gap pattern(s) optionally supported by the UE for NR SA and NR-DC when the frequencies to be measured within this measurement gap are all NR frequencies. The leading / leftmost bit (bit 0) corresponds to the gap pattern 2, the next bit corresponds to the gap pattern 3 and so on. The UE shall set the bits corresponding to the measurement gap pattern 2, 3 and 11 to 1.  ***supportedGapPattern-NRonly-NEDC***  Indicates whether the UE supports gap patterns 2, 3 and 11 in NE-DC when the frequencies to be measured within this measurement gap are all NR frequencies.  ***measGapPatterns-NRonly-ENDC-r16***  This field indicates whether the UE supports gap patterns 2, 3 and 11 in (NG)EN-DC when the frequencies to be measured within this measurement gap are all NR frequencies.  The requirements need to be consistent with the UE capability. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | * Revised Note 4 in Table 9.1.2-2 * Revised Note 7 in Table 9.1.2-3 | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The requirements are not consistent with introduced UE capability. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 9.1.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **x** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

*< Start of change #1 >*

### 9.1.2 Measurement gap

If the UE requires measurement gaps to identify and measure intra-frequency cells and/or inter-frequency cells and/or inter-RAT E-UTRAN cells, and the UE does not support independent measurement gap patterns for different frequency ranges as specified in Table 5.1-1 in [18, 19, 20], in order for the requirements in the following clauses to apply the network must provide a single per-UE measurement gap pattern for concurrent monitoring of all frequency layers.

If the UE requires measurement gaps to identify and measure intra-frequency cells and/or inter-frequency cells and/or inter-RAT E-UTRAN cells, and the UE supports independent measurement gap patterns for different frequency ranges as specified in Table 5.1-1 in [18, 19, 20], in order for the requirements in the following clauses to apply the network must provide either per-FR measurement gap patterns for frequency range where UE requires per-FR measurement gap for concurrent monitoring of all frequency layers of each frequency range independently, or a single per-UE measurement gap pattern for concurrent monitoring of all frequency layers of all frequency ranges.

If the UE is configured via LPP [34] to measure PRS for any RSTD, PRS-RSRP, and UE Rx-Tx time difference measurement defined in TS 38.215 [4], in order for the requirements in clauses 9.9.2, 9.9.3, and 9.9.4 to apply, the network must provide

- a single per-UE measurement gap pattern for concurrent monitoring of all positioning frequency layers and intra-frequency, inter-frequency and/or inter-RAT frequency layers of all frequency ranges, or

- for measurement gap patterns other than #24 and #25, if UE supports independent measurement gap patterns for different frequency ranges, per-FR measurement gap pattern for the frequency range for concurrent monitoring of all positioning frequency layers and intra-frequency, inter-frequency cells and/or inter-RAT frequency layers in the corresponding frequency range.

During the per-UE measurement gaps the UE:

- is not required to conduct reception/transmission from/to the corresponding E-UTRAN PCell, E-UTRAN SCell(s) and NR serving cells for E-UTRA-NR dual connectivity except the reception of signals used for RRM measurement(s) and the signals used for random access procedure according to TS38.321 [7].

- is not required to conduct reception/transmission from/to the corresponding NR serving cells for SA (with single carrier or CA configured) except the reception of signals used for RRM measurement(s), PRS measurement(s) and the signals used for random access procedure according to [7].

- is not required to conduct reception/transmission from/to the corresponding PCell, SCell(s) and E-UTRAN serving cells for NR-E-UTRA dual connectivity except the reception of signals used for RRM measurement(s), PRS measurement(s) and the signals used for random access procedure according to [7].

- is not required to conduct reception/transmission from/to the corresponding NR serving cells for NR-DC except the reception of signals used for RRM measurement(s) , PRS measurement(s) and the signals used for random access procedure according to [7].

During the per-FR measurement gaps the UE:

- is not required to conduct reception/transmission from/to the corresponding E-UTRAN PCell, E-UTRAN SCell(s) and NR serving cells in the corresponding frequency range for E-UTRA-NR dual connectivity except the reception of signals used for RRM measurement(s) and the signals used for random access procedure according to TS38.321 [7].

- is not required to conduct reception/transmission from/to the corresponding NR serving cells in the corresponding frequency range for SA (with single carrier or CA configured) except the reception of signals used for RRM measurement(s), PRS measurement(s) and the signals used for random access procedure according to TS38.321 [7].

- is not required to conduct reception/transmission from/to the corresponding PCell, SCell(s) and E-UTRAN serving cells in the corresponding frequency range for NR-E-UTRA dual connectivity except the reception of signals used for RRM measurement(s), PRS measurement(s) and the signals used for random access procedure according to TS38.321 [7].

- is not required to conduct reception/transmission from/to the corresponding NR serving cells in the corresponding frequency range for NR-DC except the reception of signals used for RRM measurement(s), PRS measurement(s) and the signals used for random access procedure according to TS38.321 [7].

UEs shall support the measurement gap patterns listed in Table 9.1.2-1 based on the applicability specified in table 9.1.2-2 and 9.1.2-3. UE determines measurement gap timing based on gap offset configuration and measurement gap timing advance configuration provided by higher layer signalling as specified in TS 38.331 [2] and TS 36.331 [16].

Table 9.1.2-1: Gap Pattern Configurations

|  |  |  |
| --- | --- | --- |
| Gap Pattern Id | Measurement Gap Length (MGL, ms) | Measurement Gap Repetition Period  (MGRP, ms) |
| 0 | 6 | 40 |
| 1 | 6 | 80 |
| 2 | 3 | 40 |
| 3 | 3 | 80 |
| 4 | 6 | 20 |
| 5 | 6 | 160 |
| 6 | 4 | 20 |
| 7 | 4 | 40 |
| 8 | 4 | 80 |
| 9 | 4 | 160 |
| 10 | 3 | 20 |
| 11 | 3 | 160 |
| 12 | 5.5 | 20 |
| 13 | 5.5 | 40 |
| 14 | 5.5 | 80 |
| 15 | 5.5 | 160 |
| 16 | 3.5 | 20 |
| 17 | 3.5 | 40 |
| 18 | 3.5 | 80 |
| 19 | 3.5 | 160 |
| 20 | 1.5 | 20 |
| 21 | 1.5 | 40 |
| 22 | 1.5 | 80 |
| 23 | 1.5 | 160 |
| 24 | 10 | 80 |
| 25 | 20 | 160 |

Table 9.1.2-2: Applicability for Gap Pattern Configurations supported by the E-UTRA-NR dual connectivity UE or NR-E-UTRA dual connectivity UE

|  |  |  |  |
| --- | --- | --- | --- |
| Measurement gap pattern configuration | Serving cell | Measurement PurposeNote 5 | Applicable Gap Pattern Id |
| Per-UE | E-UTRA + FR1, or | non-NR RAT Note1,2 | 0,1,2,3 |
| Measurement gap | E-UTRA + FR2, or E-UTRA + FR1 + FR2 | FR1 and/or FR2 | 0-11, 24, 25 |
|  |  | non-NR RATNote1,2 and FR1 and/or FR2 | 0, 1, 2, 3, 4, 6, 7, 8,10, 24, 25 |
|  | E-UTRA and, FR1 if configured | non-NR RAT Note1,2 | 0,1,2,3 |
|  | FR2 if configured |  | No gap |
|  | E-UTRA and, FR1 if configured | FR1 only | 0-11 |
|  | FR2 if configured |  | No gap |
|  | E-UTRA and, FR1 if configured | FR2 only | No gap |
| Per-FR | FR2 if configured |  | 12-23 |
| measurement gap | E-UTRA and, FR1 if configured | non-NR RAT Note1,2 and FR1 | 0, 1, 2, 3, 4, 6, 7, 8,10 |
|  | FR2 if configured |  | No gap |
|  | E-UTRA and, FR1 if configured | FR1 and FR2 | 0-11 |
|  | FR2 if configured |  | 12-23 |
|  | E-UTRA and, FR1 if configured | non-NR RAT Note1,2 and FR2 | 0, 1, 2, 3, 4, 6, 7, 8,10 |
|  | FR2 if configured |  | 12-23 |
|  | E-UTRA and, FR1 if configured | non-NR RAT Note1,2 and FR1 and FR2 | 0, 1, 2, 3, 4, 6, 7, 8,10 |
|  | FR2 if configured |  | 12-23 |
| Note: In E-UTRA-NR dual connectivity mode, if GSM or UTRA TDD or UTRA FDD inter-RAT frequency layer is configured to be monitored, only measurement gap pattern #0 and #1 can be used for per-FR gap in E-UTRA and FR1 if configured, or for per-UE gap. In NR-E-UTRA dual connectivity mode, if UTRA FDD inter-RAT frequency layer is configured to be monitored for SRVCC, only measurement gap pattern #0 and #1 can be used for per-FR gap in E-UTRA and FR1 if configured, or for per-UE gap.  NOTE 1: In E-UTRA-NR dual connectivity mode, non-NR RAT includes E-UTRA, UTRA and/or GSM. In NR-E-UTRA dual connectivity mode, non-NR RAT means E-UTRA, and UTRA for SRVCC.  NOTE 2: Void  NOTE 3: When E-UTRA inter-frequency RSTD measurements are configured and the UE requires measurement gaps for performing such measurements, only Gap Pattern #0 can be used.  NOTE 4: For UE only supporting *supportedGapPattern-NRonly* for any gap patterns among GP2-11, the corresponding GPs are not applicable to any measurement in this table. For UE supporting *supportedGapPattern-NRonly-NEDC* or *measGapPatterns-NRonly-ENDC-r16* but not supporting *supportedGapPattern* for the corresponding gap patterns among GP2-11, the corresponding gap patterns are not applicable to measurement of non-NR RATs as defined in NOTE 1.  NOTE 5: Inclusion of positioning measurements: Measurement purpose which includes E-UTRA measurements includes also E-UTRA RSRP and E-UTRA RSRQ measurements for E-CID; measurement purpose which includes any of FR1 and FR2 measurements includes also RSTD, UE Rx-Tx, and PRS-RSRP measurements.  NOTE 6: Measurement gap patterns #24 and #25 can be requested [2] only when the UE is configured at least with any of RSTD, UE Rx-Tx, or PRS-RSRP measurements requiring such gaps and can only be used during the corresponding positioning measurement period | | | |

In E-UTRA-NR dual connectivity mode,

- if per-UE measurement gap is configured with MG timing advance of TMG ms, the measurement gap starts at time TMG ms advanced to the end of the latest E-UTRA subframe occurring immediately before the configured measurement gap among MCG serving cells subframes.

- if per-FR measurement gap for FR1 is configured with MG timing advance of TMG ms, the measurement gap for FR1 starts at time TMG ms advanced to the end of the latest E-UTRA subframe occurring immediately before the configured measurement gap among MCG serving cells subframes.

- if per-FR measurement gap for FR2 is configured with MG timing advance of TMG ms, the measurement gap for FR2 starts at time TMG ms advanced to the end of the latest NR subframe occurring immediately before the configured measurement gap among SCG serving cells subframes in FR2.

In NR-E-UTRA dual connectivity mode,

- if per-UE measurement gap is configured with MG timing advance of TMG ms, the measurement gap starts at time TMG ms advanced to the end of the latest NR subframe occurring immediately before the configured measurement gap among MCG serving cells subframes.

- if per-FR measurement gap for FR1 is configured with MG timing advance of TMG ms and UE has NR serving cell in FR1, the measurement gap for FR1 starts at time TMG ms advanced to the end of the latest NR subframe occurring immediately before the configured measurement gap among MCG serving cells subframes in FR1.

- if per-FR measurement gap for FR1 is configured with MG timing advance of TMG ms and UE doesn’t have NR serving cell in FR1, the measurement gap for FR1 starts at time TMG ms advanced to the end of the latest E-UTRA subframe occurring immediately before the configured measurement gap among SCG serving cells subframes.

- if per-FR measurement gap for FR2 is configured with MG timing advance of TMG ms, the measurement gap for FR2 starts at time TMG ms advanced to the end of the latest NR subframe occurring immediately before the configured measurement gap among MCG serving cells subframes in FR2.

In NR-NR dual connectivity mode,

- If per-UE measurement gap is configured with MG timing advance of TMG ms, the measurement gap starts at time TMG ms advanced to the end of the latest MCG subframe occurring immediately before the configured measurement gap among MCG serving cells subframes.

- If per-FR measurement gap for FR1 is configured with MG timing advance of TMG ms, the measurement gap for FR1 starts at time TMG ms advanced to the end of the latest MCG subframe occurring immediately before the configured measurement gap among MCG serving cells subframes.

- If per-FR measurement gap for FR2 is configured with MG timing advance of TMG ms, the measurement gap for FR2 starts at time TMG ms advanced to the end of the latest SCG subframe occurring immediately before the configured measurement gap among SCG serving cells subframes in FR2.

TMG is the MG timing advance value provided in *mgta* according to TS38.331 [2].

In determining the measurement gap starting point, UE shall use the DL timing of the latest E-UTRA or NR subframe occurring immediately before the configured measurement gap among E-UTRA or NR serving cells.

For per-FR measurement gap capable UE configured with E-UTRA-NR dual connectivity or NR-E-UTRA dual connectivity, when serving cells are in E-UTRA and FR1, measurement objects are in both E-UTRA/FR1 and FR2,

- If MN indicates UE that the measurement gap from MN applies to E-UTRA/FR1/FR2 serving cells, UE fulfils the per-UE measurement requirements for both E-UTRA/FR1 and FR2 measurement objects based on the measurement gap pattern configured by MN;

- If MN indicates UE that the measurement gap from MN applies to only LTE/FR1 serving cell(s),

- UE fulfils the measurement requirements for FR1/LTE measurement objects based on the configured measurement gap pattern;

- UE fulfils the requirements for FR2 measurement objects based on effective MGRP=20ms;

For per-FR measurement gap capable configured with E-UTRA-NR dual connectivity, NR-E-UTRA dual connectivity or NR-NR dual connectivity, when serving cells are in E-UTRA, FR1 and FR2, or in E-UTRA and FR2, or in FR1 and FR2, measurement objects are in both E-UTRA /FR1 and FR2,

- If MN indicates UE that the measurement gap from MN applies to E-UTRA/FR1/FR2 serving cells, UE fulfils the per-UE measurement requirements for both E-UTRA/FR1 and FR2 measurement objects based on the measurement gap pattern configured by MN.

Table 9.1.2-3: Applicability for Gap Pattern Configurations supported by the UE with NR standalone operation (with single carrier, NR CA and NR-DC configuration)

|  |  |  |  |
| --- | --- | --- | --- |
| Measurement gap pattern configuration | Serving cell | Measurement Purpose NOTE 2 | Applicable Gap Pattern Id |
|  | FR1 NOTE5, or  FR1 + FR2 | non-NR RAT NOTE3,6 | 0,1,2,3 |
|  |  | FR1 and/or FR2 | 0-11, 24, 25 |
|  |  | non-NR RATand FR1 and/or FR2 NOTE3,6 | 0, 1, 2, 3, 4, 6, 7, 8,10, 24, 25 |
| Per-UE measurement | FR2 NOTE5 | non-NR RATonly  NOTE3,6 | 0,1,2,3 |
| gap |  | FR1 only | 0-11, 24, 25 |
|  |  | FR1 and FR2 | 0-11, 24, 25 |
|  |  | non-NR RATand FR1 and/or FR2 NOTE3,6 | 0, 1, 2, 3, 4, 6, 7, 8,10, 24, 25 |
|  |  | FR2 only | 12-23 |
|  | FR1 if configured | non-NR RATonly | 0,1,2,3 |
|  | FR2 if configured | NOTE3,6 | No gap |
|  | FR1 if configured | FR1 only | 0-11 |
|  | FR2 if configured |  | No gap |
|  | FR1 if configured | FR2 only | No gap |
| Per-FR | FR2 if configured |  | 12-23 |
| measurement | FR1 if configured | non-NR RATand | 0, 1, 2, 3, 4, 6, 7, 8,10 |
| gap | FR2 if configured | FR1 NOTE3,6 | No gap |
|  | FR1 if configured | FR1 and FR2 | 0-11 |
|  | FR2 if configured |  | 12-23 |
|  | FR1 if configured | non-NR RATand | 0, 1, 2, 3, 4, 6, 7, 8,10 |
|  | FR2 if configured | FR2 NOTE3,6 | 12-23 |
|  | FR1 if configured | non-NR RATand | 0, 1, 2, 3, 4, 6, 7, 8,10 |
|  | FR2 if configured | FR1 and FR2 NOTE3,6 | 12-23 |
| NOTE 1: When E-UTRA inter-RAT RSTD measurements are configured and the UE requires measurement gaps for performing such measurements, only Gap Pattern #0 can be used.  NOTE 2: Measurement purpose which includes E-UTRA measurements includes also inter-RAT E-UTRA RSRP and RSRQ measurements for E-CID; measurement purpose which includes E-UTRA measurements includes also E-UTRA RSRP and E-UTRA RSRQ measurements for E-CID; measurement purpose which includes any of FR1 or FR2 measurements includes also RSTD, UE Rx-Tx, and PRS-RSRP measurements.  NOTE 3: Void  NOTE4: If per-UE measurement gap is configured with MG timing advance of TMG ms, the measurement gap starts at time TMG ms advanced to the end of the latest subframe occurring immediately before the configured measurement gap among all serving cells subframes.  If per-FR measurement gap for FR1 is configured with MG timing advance of TMG ms, the measurement gap for FR1 starts at time TMG ms advanced to the end of the latest subframe occurring immediately before the configured measurement gap among serving cells subframes in FR1.  If per-FR measurement gap for FR2 is configured with MG timing advance of TMG ms, the measurement gap for FR2 starts at time TMG ms advanced to the end of the latest subframe occurring immediately before the configured measurement gap among serving cells subframes in FR2.  TMG is the MG timing advance value provided in *mgta* according to [2].  In determining the measurement gap starting point, UE shall use the DL timing of the latest subframe occurring immediately before the configured measurement gap among serving cells.  NOTE 5: NR-DC in Rel-15 only includes the scenarios where all serving cells in MCG in FR1 and all serving cells in SCG in FR2.  NOTE 6: In NR single carrier, NR CA, and NR-DC mode, non-NR RAT means E-UTRA, and UTRA for SRVCC. In NR single carrier, NR CA, and NR-DC mode, if UTRA FDD inter-RAT frequency layer is configured to be monitored for SRVCC, only measurement gap pattern #0 and #1 can be used for per-FR gap in E-UTRA and FR1 if configured, or for per-UE gap.  NOTE 7: For UE only supporting *supportedGapPattern-NRonly* for any gap patterns among GP2-11, the corresponding gap patterns are not applicable to measurement of non-NR RATs as defined in NOTE 6.  NOTE 8: Measurement gap patterns #24 and #25 can be requested [2] only when the UE is configured with any of RSTD, UE Rx-Tx, or PRS-RSRP measurements requiring such gaps and can only be used during the corresponding positioning measurement period. | | | |

For per-FR measurement gap capable UE in NR standalone operation (with single carrier, NR CA and NR-DC configuration), for per-FR gap based measurement, when there is no serving cell in a particular FR, where measurement objects are configured, regardless if explicit per-FR measurement gap is configured in this FR, the effective MGRP in this FR is used to determine requirements;

- 20 ms for FR2 NR measurements

- 40 ms for FR1 NR measurements

- 40 ms for LTE measurements

- 40 ms for FR1+LTE measurements

For per-FR measurement gap capable UE in NR standalone operation (with single carrier, NR CA and NR-DC configuration), when serving cells are in FR1 or FR2, measurement objects are in both E-UTRA /FR1 and FR2,

- If MN indicates UE that the measurement gap from MN applies to E-UTRA/FR1/FR2 serving cells, UE fulfils the per-UE measurement requirements for both E-UTRA/FR1 and FR2 measurement objects based on the measurement gap pattern configured by MN;

If measurement gap is configured in one FR but measurement object is not configured in the FR, the scheduling opportunity in the FR depends on the configured measurement gap pattern.

For E-UTRA-NR dual connectivity, if UE is not capable of per-FR-gap, total interruption time on SCG during MGL is defined only when MGL(N) = 20ms, 10ms, 6ms, 4ms and 3ms. And if UE is capable of per-FR-gap, total interruption time on FR1 serving cells in SCG during MGL is defined only when MGL(N) = 20ms, 10ms, 6ms, 4ms and 3ms, and total interruption time on FR2 serving cells in SCG during MGL is defined only when MGL(N) = 20ms, 10ms, 5.5ms, 3.5ms and 1.5ms.

For NR standalone operation (with single carrier, NR CA and NR-DC configuration), if UE is not capable of per-FR-gap, total interruption time on a serving cell during MGL is defined when MGL(N) = 20ms, 10ms, 6ms, 5.5ms, 4ms, 3.5ms, 3ms, and 1.5ms. And if UE is capable of per-FR-gap, total interruption time on FR1 serving cells during MGL is defined only when MGL(N) = 20ms, 10ms, 6ms, 4ms, and 3ms, and total interruption time on FR2 serving cells during MGL is defined only when MGL(N) = 20ms, 10ms, 5.5ms, 3.5ms, and 1.5ms.

For NR-E-UTRA dual connectivity, if UE is not capable of per-FR-gap, total interruption time on MCG during MGL is defined only when MGL(N) = 20ms, 10ms, 6ms, 4ms, and 3ms. And if UE is capable of per-FR-gap, total interruption time on FR1 serving cells in MCG during MGL is defined only when MGL(N) = 20ms, 10ms, 6ms, 4ms, and 3ms, and total interruption time on FR2 serving cells in MCG during MGL is defined only when MGL(N) = 20ms, 10ms, 5.5ms, 3.5ms, and 1.5ms.



(a) Measurement gap with MGL = N(ms) with MG timing advance of 0ms for all serving cells in synchronous EN-DC, NR standalone operation (with single carrier, NR CA and synchronous NR-DC configuration) and synchronous NE-DC, and for serving cells in MCG in NR standalone operation (with asynchronous NR-DC configuration)



(b) Measurement gap with MGL = N(ms) with MG timing advance of 0.5ms for all serving cells in synchronous EN-DC, NR standalone operation (with single carrier, NR CA and synchronous NR-DC configuration) and synchronous NE-DC, and for serving cells in MCG in NR standalone operation (with asynchronous NR-DC configuration)



(c) Measurement gap with MGL = N(ms) with MG timing advance of 0ms for all serving cells in asynchronous EN-DC and asynchronous NE-DC, and for serving cells in SCG in NR standalone operation (with asynchronous NR-DC configuration)



(d) Measurement gap with MGL = N(ms) with MG timing advance of 0.5ms for all serving cells in asynchronous EN-DC and asynchronous NE-DC, and for serving cells in SCG in NR standalone operation (with asynchronous NR-DC configuration)

Figure 9.1.2-1: Measurement GAP and total interruption time on serving cells for EN-DC, NR standalone operation (with single carrier, NR CA and NR-DC configuration) and NE-DC

The corresponding total number of interrupted slots on serving cells is listed in Table 9.1.2-4 for all serving cells in synchronous EN-DC, NR standalone (with single carrier, NR CA and synchronous NR-DC configuration) and NE-DC, and for serving cells in MCG in NR standalone operation (with asynchronous NR-DC configuration). The corresponding total number of interrupted slots on serving cells is listed in Table 9.1.2-4a for asynchronous EN-DC, and for serving cells in SCG in NR standalone operation (with asynchronous NR-DC configuration).

Table 9.1.2-4: Total number of interrupted slots on all serving cells during MGL for Synchronous EN-DC, NR standalone operation (with single carrier, NR CA and synchronous NR-DC configuration) and NE-DC, and on all serving cells in MCG for NR standalone operation (with asynchronous NR-DC configuration) with per-UE measurement gap or per-FR measurement gap for FR1

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NR | Total number of interrupted slots on serving cells | | | | | | | | | |
| SCS | When MG timing advance of 0ms is applied | | | | | When MG timing advance of 0.5ms is applied | | | | |
| (kHz) | MGL=20ms | MGL=10ms | MGL=6ms | MGL=4ms | MGL=3ms | MGL=20ms | MGL=10ms | MGL=6ms | MGL=4ms | MGL=3ms |
| 15 | 20 | 10 | 6 | 4 | 3 | 21Note3 | 11Note3 | 7Note3 | 5Note3 | 4Note3 |
| 30 | 40 | 20 | 12 | 8 | 6 | 40 | 20 | 12 | 8 | 6 |
| 60 | 80 | 40 | 24 | 16 | 12 | 80 | 40 | 24 | 16 | 12 |
| 120 | 160 | 80 | 48 | 32 | 24 | 160 | 80 | 48 | 32 | 24 |
| NOTE 1: For Gap Pattern ID 0, 1, 2 and 3, total number of interrupted subframes on MCG is MGL subframes when MG timing advance of 0ms is applied, and (MGL+1) subframes when MG timing advance of 0.5ms is applied.  NOTE 2: NR SCS of 120 kHz is only applicable to the case with per-UE measurement gap.  NOTE 3: Non-overlapped half-slots occur before and after the measurement gap. Whether a Rel-15 UE can receive and/or transmit in those half-slots is up to UE implementation. | | | | | | | | | | |

Table 9.1.2-4a: Total number of interrupted slots on serving cells during MGL for Asynchronous EN-DC, and on all serving cells in SCG for NR standalone operation (with asynchronous NR-DC configuration) with per-UE measurement gap or per-FR measurement gap for FR1

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NR | Total number of interrupted slots on serving cells | | | | | | | | | |
| SCS | When MG timing advance of 0ms is applied | | | | | When MG timing advance of 0.5ms is applied | | | | |
| (kHz) | MGL=20ms | MGL=10ms | MGL=6ms | MGL=4ms | MGL=3ms | MGL=20ms | MGL=10ms | MGL=6ms | MGL=4ms | MGL=3ms |
| 15 | 21 | 11 | 7 | 5 | 4 | 21 | 11 | 7 | 5 | 4 |
| 30 | 41 | 21 | 13 | 9 | 7 | 41 | 21 | 13 | 9 | 7 |
| 60 | 81 | 41 | 25 | 17 | 13 | 81 | 41 | 25 | 17 | 13 |
| 120 | 161 | 81 | 49 | 33 | 25 | 161 | 81 | 49 | 33 | 25 |
| NOTE 1: For Gap Pattern ID 0, 1, 2 and 3, total number of interrupted subframes on MCG is MGL subframes when MG timing advance of 0ms is applied, and (MGL+1) subframes when MG timing advance of 0.5ms is applied.  NOTE 2: NR SCS of 120 kHz is only applicable to the case with per-UE measurement gap. | | | | | | | | | | |

In case that UE capable of per-FR measurement gap is configured with per-FR measurement gap for FR2 serving cells, total number of interrupted slots on FR2 serving cells during MGL is listed in Table9.1.2-4b.

**Table 9.1.2-4b: Total number of interrupted slots on FR2 serving cells during MGL for EN-DC, NR standalone operation (with single carrier, NR CA and NR-DC configuration) and NE-DC with per-UE measurement gap or per-FR measurement gap for FR2**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NR | Total number of interrupted slots on FR2 serving cells | | | | | | | | | |
| SCS | When MG timing advance of 0ms is applied | | | | | When MG timing advance of 0.25ms is applied | | | | |
| (kHz) | MGL=  20ms | MGL=  10ms | MGL=  5.5ms | MGL=  3.5ms | MGL=  1.5ms | MGL=  20ms | MGL=  10ms | MGL=  5.5ms | MGL=  3.5ms | MGL=  1.5ms |
| 60 | 80 | 40 | 22 | 14 | 6 | 80 | 40 | 22 | 14 | 6 |
| 120 | 160 | 80 | 44 | 28 | 12 | 160 | 80 | 44 | 28 | 12 |
| NOTE 1: The total number of interrupted slots is based on that SFN and subframe reference for per-FR gap in FR2 indicated by high layer parameter *refServCellIndicator* is an FR2 serving cell.  NOTE 2: Slot occurs before or after the measurement gap may be interrupted additionally if SFN and subframe reference for per-FR gap in FR2 indicated by high layer parameter refServCellIndicator is an FR1 serving cell. | | | | | | | | | | |

It is up to UE implementation whether or not the UE is able to conduct transmission in the following slot(s),

- when MGTA is not applied, in the L consecutive UL slots with respect to the SCS of the UL carrier with the same slot indices as the DL slots occurring immediately after measurement gap

- when MGTA is applied and the SCS of the UL carrier is other than 15kHz, in the L consecutive UL slots with respect to the SCS of the UL carrier with the same slot indices as the DL slots occurring immediately after measurement gap

- when MGTA is applied and the SCS of the UL carrier is 15kHz, in the L consecutive UL slots with respect to the SCS of the UL carrier with the same slot indices as the DL slots occurring immediately after the slot partially overlapped with measurement gap

where UL slot denotes that all the symbols in the slot are uplink symbols, and L=1 if  for the UL transmission is less than the length of one slot; L=2 otherwise.

Note: Network is supposed to take into account the possible difference between the estimated TA at network and actual TA at UE when scheduling UE in the above slot(s).

Table 9.1.2-5: (Void)

*< End of change #1 >*