**3GPP TSG-RAN WG4 Meeting #97-e R4-2017470**

Electronic Meeting, 2nd -13th Nov., 2020

**Title:** Simulation assumptions for V2X single link test cases

**Source:** Huawei, HiSilicon

**Agenda item:** 7.3.7.2

**Document for:** Discussion

# Introduction

In this contribution, we provide the simulation assumptions for NR V2X single-link demodulation requirements only for initial simulation results alignment purpose. Companies are encouraged to submit the simulation results for next meeting. The values with different options or [ ] need be updated in the next RAN4 meeting based on further discussion.

# Simulation assumptions

## PSSCH

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Parameters** | | **Unit** | **Value** | | | |
| Test | |  | SCH\_Test1 | | SCH\_Test2 | SCH\_Test3 |
| Synchronization source | |  | GNSS | | GNSS | GNSS |
| Propagation condition | |  | TDLA30-180 | | TDLA30-1400 | Option 1:TDLA30-2700  Option 2:TDLB100-2700 |
| Channel bandwidth | | MHz | 20 | | 20 | 20 |
| Allocated resource blocks | | RB | Option 1: 10  Option 2: 20 | | [20] | [20] |
| Subcarrier spacing | | kHz | 30 | | 30 | 30 |
| Timing offset | |  | CP/2-12Ts | | CP/2-12Ts | CP/2-12Ts |
| Frequency offset | | Hz | 600 | | 600 | 600 |
| CP-OFDM symbols for slot with PSFCH(Note 1) | |  | 9 | | 9 | 9 |
| CP-OFDM symbols for slot without PSFCH | |  | 12 | | 12 | 12 |
| DMRS symbols for slot with PSFCH | |  | 2 | | 2 | 3 |
| DMRS symbols for slot without PSFCH | |  | Option 1: 2  Option 2: 3 | | 3 | Option 1: 4  Option 2: 3 |
| Modulation order | |  | 2 | | 4 | 6 |
| MCS index | |  | 4 | | 11 | [17] |
| 2nd stage SCI format 2-A configuration | Payloads | Bits | 35 | | 35 | 35 |
|  |  | 1 | 1 | | 1 |
|  |  | [5] | | [5] | [3.5] |
| Transport Block Size for slot with PSFCH | | Bits |  | |  |  |
| Transport Block Size for slot without PSFCH | | Bits |  | |  |  |
| Transport block CRC | | Bits | 24 | | 24 | 24 |
| Maximum number of HARQ transmissions | |  | 1 | | 1 | 1 |
| Binary Channel Bits for slots with PSFCH(Note 2) | |  |  | |  |  |
| Binary Channel Bits for slots without PSFCH | | Bits |  | |  |  |
| PSFCH resource period(Note 4) | | Slot | Option 1: 4  Option 2: 1 | | | |
| MinTimeGapPSFCH | | Slot | 3 | | 3 | 3 |
| Antenna configuration | |  | 1x2 | | 1x2 | 1x2 |
| Performance metric(Note 3) | |  | SNR@10% BLER of PSSCH | | | |
| Note 1: OFDM symbols is for PSCCH/PSSCH transmission not including first symbol (AGC) and PSFCH symbols.  Note 2: 10 RBs and 2 symbols are allocated for PSCCH, and 2nd stage SCI is also allocated.  Note 3: The performance metric is used for PSSCH simulation evaluation.  Note 4: PSFCH is transmitted on every [4] slot. | | | | | | |

## PSCCH

Table Simulation assumption for PSCCH demodulation performance

|  |  |  |
| --- | --- | --- |
| **Parameters** | **Unit** | **Value** |
| Test |  | CCH\_Test1 |
| Synchronization source |  | GNSS |
| Propagation condition |  | TDLA30-1400 |
| Channel bandwidth | MHz | 20 |
| Allocated resource blocks |  | 10 |
| Subcarrier spacing | kHz | 30 |
| Timing offset |  | CP/2-12Ts |
| Frequency offset | Hz | 600 |
| The number of PSCCH symbols |  | 2 |
| Modulation order |  | QPSK |
| Payload size (without CRC) | Bits | Option 1: 26  Option 2: 24 |
| Transport block CRC | Bits | 24 |
| Binary Channel Bits | Bits |  |
| PSCCH performance metric (Note 1) |  | SNRPSCCH@1%BLER |
| Note 1: The performance metric is used for PSCCH simulation evaluation.  Note 2: OCC index *i* (in TS 38.211) for PSCCH DMRS is randomly selected between {0, 1, 2} for each PSCCH transmission.  Note 3: Two propagation conditions are listed as options for alignment purpose, one of the option will be chosen for defining requirement | | |

## PSBCH

Table Simulation assumption for PSBCH demodulation performance

|  |  |  |
| --- | --- | --- |
| **Parameters** | **Unit** | **Value** |
| Test |  | BCH\_Test1 |
| SLID |  | 0 |
| Synchronization source |  | S-SSB |
| Propagation condition |  | TDLA30-180 |
| Channel bandwidth | MHz | 20 |
| Number SSB per SL period() |  | Option 1: 1  Option 2: 2 S-SSB with different contents |
| Allocated resource blocks |  | 11 |
| Subcarrier spacing | kHz | 30 |
| Timing offset |  | 0 |
| Frequency offset | Hz | 0 |
| The number of symbols (Note 1) |  | 8 |
| Modulation order |  | QPSK |
| Transport Block Size (without CRC) | Bits | 32 |
| Transport block CRC | Bits | 24 |
| Binary Channel Bits | Bits | 1782 |
| PSBCH performance metric (Note 2) |  | SNR@1%BLER of PSBCH |
| Note 1: The first symbol is for AGC.  Note 2: The performance metric is used for PSBCH simulation assumption. | | |

## PSFCH

Table 4 Simulation assumption for PSFCH demodulation performance

|  |  |  |
| --- | --- | --- |
| **Parameters** | **Unit** | **Value** |
| Test |  | FCH\_Test1 |
| Synchronization source |  | GNSS |
| Propagation condition |  | TDLA30-180 |
| Channel bandwidth | MHz | 20 |
| Allocated resource blocks |  | 1 |
| Subcarrier spacing | kHz | 30 |
| Timing offset |  | CP/2-12Ts |
| Frequency offset | Hz | 600 |
| The number of PSFCH symbols |  | 2 |
| Number of information bits | bit | 1 |
| PSFCH period | Slot | 1 |
| Cyclic shift pair index |  | 1 |
| PSFCH performance metric (Note 1) |  | SNR@[Pr(ACK miss) =1%], [Pr(NACK to ACK) < 0.1%] and [Pr(DTX to ACK)<1%] |
| Note 1: The performance metric is used for PSFCH simulation assumption.  Note 2: The 1st PSFCH which is used for AGC doesn’t need to be considered in performance evaluation. | | |