**3GPP TSG-RAN WG4 Meeting # 97e *R4-2017535***

**Electronic Meeting, 2-13 November 2020**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.101-4** | **CR** | - | **rev** | 1- | **Current version:** | **16.2.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Draft CR for introduction of Rel-16 Enhanced Type II PMI test cases | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Samsung | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_eMIMO-Perf | | | | |  | ***Date:*** | | | 2020-10-23 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | B |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Introduce PMI tese case to verify UE reporting accuracy for Rel-16 Type II codebook | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Add new test cases for Rel-16 Type II codebook | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | No applicable test cases for Rel-16 TypeII codebook | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | New clauses: 6.3.2.1.6,6.3.2.2.6, 6.3.3.1.6, 6.3.3.2.6 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **x** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | | **x** |  | Test specifications | | | | TS 38.521-4 | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

~~~~~~~~~~~~~~~~~~~~~~~~~ Start of 1st change ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

##### 6.3.2.1.6 Multiple PMI with 16TX Enhanced Type II Codebook

For the parameters specified in Table 6.3.2.1.6-1, and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified in Table 6.3.2.1.6-2.

Table 6.3.2.1.6-1: Test parameters (dual-layer)

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameter** | | **Unit** | **Test 1** |
| Bandwidth | | MHz | 10 |
| Subcarrier spacing | | kHz | 15 |
| Duplex Mode | |  | FDD |
| Propagation channel | |  | [TDLA30-5] |
| Antenna configuration | |  | [XP Medium] 16 x 2  (N1,N2) = (4,2) |
| Beamforming Model | |  | As specified in Annex B.4.1 |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Aperiodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1) |  | Row 5, (4,-) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (9,-) |
| CSI-RS  interval and offset | slot | Not configured |
| ZP CSI-RS trigger |  | 1 in slots i, where mod(i, 5) = 1, otherwise it is equal to 0 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Aperiodic |
| Number of CSI-RS ports (*X*) |  | 16 |
| CDM Type |  | CDM4 (FD2, TD2) |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1, k2, k3) |  | Row 12, (2, 4, 6, 8) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (5, -) |
| CSI-RS  interval and offset | slot | Not configured |
| aperiodicTriggeringOffset |  | 0 |
| CSI-IM configuration | CSI-IM resource Type |  | Aperiodic |
| CSI-IM RE pattern |  | Pattern 0 |
| CSI-IM Resource Mapping  (kCSI-IM,lCSI-IM) |  | (4,9) |
| CSI-IM timeConfig  interval and offset | slot | Not configured |
| ReportConfigType | |  | Aperiodic |
| CQI-table | |  | Table 1 |
| reportQuantity | |  | cri-RI-PMI-CQI |
| timeRestrictionForChannelMeasurements | |  | Not configured |
| timeRestrictionForInterferenceMeasurements | |  | Not configured |
| cqi-FormatIndicator | |  | Wideband |
| pmi-FormatIndicator | |  | Subband |
| Sub-band Size | | RB | 4 |
| csi-ReportingBand | |  | 1111111 |
| CSI-Report interval and offset | | slot | Not configured |
| Aperiodic Report Slot Offset | |  | 5 |
| CSI request | |  | 1 in slots i, where mod(i, 5) = 1, otherwise it is equal to 0 |
| reportTriggerSize | |  | 1 |
| CSI-AperiodicTriggerStateList | |  | One State with one Associated Report Configuration  Associated Report Configuration contains pointers to NZP CSI-RS and CSI-IM |
| Codebook configuration | Codebook Type |  | typeII-r16 |
| *paramCombination-r16* |  | 6  (L =4, *pν* =1/2, β=1/2 ) |
| R*(numberOfPMISubbandsPerCQISubband-r16)* |  | 1 |
| (CodebookConfig-N1,CodebookConfig-N2) |  | (4,2) |
| (CodebookConfig-O1,CodebookConfig-O2) |  | (4,4) |
| CodebookSubsetRestriction |  | [0x 7FF  FFFF FFFF FFFF FFFF] |
| RI Restriction (typeII-RI-Restriction-r16) |  | [0010] |
| Physical channel for CSI report | |  | PUSCH |
| CQI/RI/PMI delay | | ms | 8 |
| Maximum number of HARQ transmission | |  | 4 |
| Measurement channel | |  | [R.PDSCH.1-6.3] |
| Note 1: When Throughput is measured using random precoder selection, the precoder shall be updated in each slot (1 ms granularity) with equal probability of each applicable i1, i2 combination.  Note 2: If the UE reports in an available uplink reporting instance at slot#n based on PMI estimation at a downlink slot not later than slot#(n-4), this reported PMI cannot be applied at the gNB downlink before slot#(n+4).  Note 3: Randomization of the principle beam direction shall be used as specified in TBD. | | | |

Table 6.3.2.1.6-2: Minimum requirement

|  |  |
| --- | --- |
| **Parameter** | **Test 1** |
| ** | TBD |

~~~~~~~~~~~~~~~~~~~~~~~~~ Start of 2nd change ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

##### 6.3.2.2.6 Multiple PMI with 16Tx Enhanced Type II Codebook

For the parameters specified in Table 6.3.2.2.6-1, and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified in Table 6.3.2.2.6-2.

Table 6.3.2.2.6-1: Test parameters (dual-layer)

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameter** | | **Unit** | **Test 1** |
| Bandwidth | | MHz | 40 |
| Subcarrier spacing | | kHz | 30 |
| Duplex Mode | |  | TDD |
| TDD DL-UL configurations | |  | FR1.30-1 as specified in Annex A |
| Propagation channel | |  | [TDLA30-5] |
| Antenna configuration | |  | [XP Medium] 16 x 2  (N1,N2) = (4,2) |
| Beamforming Model | |  | As specified in Annex B.4.1 |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Aperiodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1) |  | Row 5, (4,-) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (9,-) |
| CSI-RS  interval and offset | slot | Not configured |
| ZP CSI-RS trigger |  | 1 in slots i, where mod(i, 10) = 1, otherwise it is equal to 0 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Aperiodic |
| Number of CSI-RS ports (*X*) |  | 16 |
| CDM Type |  | CDM4 (FD2, TD2) |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1, k2, k3) |  | Row 12, (2, 4, 6, 8) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (5, -) |
| CSI-RS  interval and offset | slot | Not configured |
| aperiodicTriggeringOffset |  | 0 |
| CSI-IM configuration | CSI-IM resource Type |  | Aperiodic |
| CSI-IM RE pattern |  | Pattern 0 |
| CSI-IM Resource Mapping  (kCSI-IM,lCSI-IM) |  | (4,9) |
| CSI-IM timeConfig  interval and offset | slot | Not configured |
| ReportConfigType | |  | Aperiodic |
| CQI-table | |  | Table 1 |
| reportQuantity | |  | cri-RI-PMI-CQI |
| timeRestrictionForIChannelMeasurements | |  | Not configured |
| timeRestrictionForInterferenceMeasurements | |  | Not configured |
| cqi-FormatIndicator | |  | Wideband |
| pmi-FormatIndicator | |  | Subband |
| Sub-band Size | | RB | 8 |
| csi-ReportingBand | |  | 1111111 |
| CSI-Report interval and offset | | slot | Not configured |
| Aperiodic Report Slot Offset | |  | 8 |
| CSI request | |  | 1 in slots i, where mod(i, 10) = 1, otherwise it is equal to 0 |
| reportTriggerSize | |  | 1 |
| CSI-AperiodicTriggerStateList | |  | One State with one Associated Report Configuration  Associated Report Configuration contains pointers to NZP CSI-RS and CSI-IM |
| Codebook configuration | Codebook Type |  | typeII-r16 |
| *paramCombination-r16* |  | 6  (L =4, *pν* =1/2, β=1/2 ) |
| R*(numberOfPMISubbandsPerCQISubband-r16)* |  | 1 |
| (CodebookConfig-N1,CodebookConfig-N2) |  | (4,2) |
| (CodebookConfig-O1,CodebookConfig-O2) |  | (4,4) |
| CodebookSubsetRestriction |  | [0x 7FF  FFFF FFFF FFFF FFFF] |
| RI Restriction (typeII-RI-Restriction-r16) |  | [0010] |
| Physical channel for CSI report | |  | PUSCH |
| CQI/RI/PMI delay | | ms | 6.5 |
| Maximum number of HARQ transmission | |  | 4 |
| Measurement channel | |  | [R.PDSCH.2-8.3 TDD] |
| Note 1: When Throughput is measured using random precoder selection, the precoder shall be updated in each slot (0.5 ms granularity) with equal probability of each applicable i1, i2 combination.  Note 2: If the UE reports in an available uplink reporting instance at slot#n based on PMI estimation at a downlink slot not later than slot#(n-6), this reported PMI cannot be applied at the gNB downlink before slot#(n+6).  Note 3: Randomization of the principle beam direction shall be used as specified in TBD. | | | |

Table 6.3.2.2.6-2: Minimum requirement

|  |  |
| --- | --- |
| **Parameter** | **Test 1** |
| ** | TBD |

~~~~~~~~~~~~~~~~~~~~~~~~~ Start of 3rd change ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

##### 6.3.3.1.6 Multiple PMI with 16Tx Enhanced Type II Codebook

For the parameters specified in Table 6.3.3.1.6-1, and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified in Table 6.3.3.1.6-2.

Table 6.3.3.1.6-1: Test parameters (dual-layer)

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameter** | | **Unit** | **Test 1** |
| Bandwidth | | MHz | 10 |
| Subcarrier spacing | | kHz | 15 |
| Duplex Mode | |  | FDD |
| Propagation channel | |  | [TDLA30-5] |
| Antenna configuration | |  | [XP Medium] 16 x 4  (N1,N2) = (4,2) |
| Beamforming Model | |  | As specified in Annex B.4.1 |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Aperiodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1) |  | Row 5, (4,-) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (9,-) |
| CSI-RS  interval and offset | slot | Not configured |
| ZP CSI-RS trigger |  | 1 in slots i, where mod(i, 5) = 1, otherwise it is equal to 0 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Aperiodic |
| Number of CSI-RS ports (*X*) |  | 16 |
| CDM Type |  | CDM4 (FD2, TD2) |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1, k2, k3) |  | Row 12, (2, 4, 6, 8) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (5, -) |
| CSI-RS  interval and offset | slot | Not configured |
| aperiodicTriggeringOffset |  | 0 |
| CSI-IM configuration | CSI-IM resource Type |  | Aperiodic |
| CSI-IM RE pattern |  | Pattern 0 |
| CSI-IM Resource Mapping  (kCSI-IM,lCSI-IM) |  | (4,9) |
| CSI-IM timeConfig  interval and offset | slot | Not configured |
| ReportConfigType | |  | Aperiodic |
| CQI-table | |  | Table 1 |
| reportQuantity | |  | cri-RI-PMI-CQI |
| timeRestrictionForChannelMeasurements | |  | Not configured |
| timeRestrictionForInterferenceMeasurements | |  | Not configured |
| cqi-FormatIndicator | |  | Wideband |
| pmi-FormatIndicator | |  | Subband |
| Sub-band Size | | RB | 4 |
| csi-ReportingBand | |  | 1111111 |
| CSI-Report interval and offset | | slot | Not configured |
| Aperiodic Report Slot Offset | |  | 5 |
| CSI request | |  | 1 in slots i, where mod(i, 5) = 1, otherwise it is equal to 0 |
| reportTriggerSize | |  | 1 |
| CSI-AperiodicTriggerStateList | |  | One State with one Associated Report Configuration  Associated Report Configuration contains pointers to NZP CSI-RS and CSI-IM |
| Codebook configuration | Codebook Type |  | typeII-r16 |
| *paramCombination-r16* |  | 6  (L =4, *pν* =1/2, β=1/2 ) |
| R*(numberOfPMISubbandsPerCQISubband-r16)* |  | 1 |
| (CodebookConfig-N1,CodebookConfig-N2) |  | (4,2) |
| (CodebookConfig-O1,CodebookConfig-O2) |  | (4,4) |
| CodebookSubsetRestriction |  | [0x 7FF  FFFF FFFF FFFF FFFF] |
| RI Restriction (typeII-RI-Restriction-r16) |  | [0010] |
| Physical channel for CSI report | |  | PUSCH |
| CQI/RI/PMI delay | | ms | 8 |
| Maximum number of HARQ transmission | |  | 4 |
| Measurement channel | |  | [R.PDSCH.1-6.3] |
| Note 1: When Throughput is measured using random precoder selection, the precoder shall be updated in each slot (1 ms granularity) with equal probability of each applicable i1, i2 combination.  Note 2: If the UE reports in an available uplink reporting instance at slot#n based on PMI estimation at a downlink slot not later than slot#(n-4), this reported PMI cannot be applied at the gNB downlink before slot#(n+4).  Note 3: Randomization of the principle beam direction shall be used as specified in TBD. | | | |

Table 6.3.3.1.6-2: Minimum requirement

|  |  |
| --- | --- |
| **Parameter** | **Test 1** |
| ** | TBD |

~~~~~~~~~~~~~~~~~~~~~~~~~ Start of 4th change ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

##### 6.3.3.2.6 Multiple PMI with 16Tx Enhanced Type II Codebook

For the parameters specified in Table 6.3.3.2.6-1, and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified in Table 6.3.3.2.6-2.

Table 6.3.3.2.6-1: Test parameters (dual-layer)

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameter** | | **Unit** | **Test 1** |
| Bandwidth | | MHz | 40 |
| Subcarrier spacing | | kHz | 30 |
| Duplex Mode | |  | TDD |
| TDD DL-UL configurations | |  | FR1.30-1 as specified in Annex A |
| Propagation channel | |  | [TDLA30-5] |
| Antenna configuration | |  | [XP Medium] 16 x 4  (N1,N2) = (4,2) |
| Beamforming Model | |  | As specified in Annex B.4.1 |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Aperiodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1) |  | Row 5, (4,-) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (9,-) |
| CSI-RS  interval and offset | slot | Not configured |
| ZP CSI-RS trigger |  | 1 in slots i, where mod(i, 10) = 1, otherwise it is equal to 0 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Aperiodic |
| Number of CSI-RS ports (*X*) |  | 16 |
| CDM Type |  | CDM4 (FD2, TD2) |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1, k2, k3) |  | Row 12, (2, 4, 6, 8) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (5, -) |
| CSI-RS  interval and offset | slot | Not configured |
| aperiodicTriggeringOffset |  | 0 |
| CSI-IM configuration | CSI-IM resource Type |  | Aperiodic |
| CSI-IM RE pattern |  | Pattern 0 |
| CSI-IM Resource Mapping  (kCSI-IM,lCSI-IM) |  | (4,9) |
| CSI-IM timeConfig  interval and offset | slot | Not configured |
| ReportConfigType | |  | Aperiodic |
| CQI-table | |  | Table 1 |
| reportQuantity | |  | cri-RI-PMI-CQI |
| timeRestrictionForIChannelMeasurements | |  | Not configured |
| timeRestrictionForInterferenceMeasurements | |  | Not configured |
| cqi-FormatIndicator | |  | Wideband |
| pmi-FormatIndicator | |  | Subband |
| Sub-band Size | | RB | 8 |
| csi-ReportingBand | |  | 1111111 |
| CSI-Report interval and offset | | slot | Not configured |
| Aperiodic Report Slot Offset | |  | 8 |
| CSI request | |  | 1 in slots i, where mod(i, 10) = 1, otherwise it is equal to 0 |
| reportTriggerSize | |  | 1 |
| CSI-AperiodicTriggerStateList | |  | One State with one Associated Report Configuration  Associated Report Configuration contains pointers to NZP CSI-RS and CSI-IM |
| Codebook configuration | Codebook Type |  | typeII-r16 |
| *paramCombination-r16* |  | 6  (L =4, *pν* =1/2, β=1/2 ) |
| R*(numberOfPMISubbandsPerCQISubband-r16)* |  | 1 |
| (CodebookConfig-N1,CodebookConfig-N2) |  | (4,2) |
| (CodebookConfig-O1,CodebookConfig-O2) |  | (4,4) |
| CodebookSubsetRestriction |  | [0x 7FF  FFFF FFFF FFFF FFFF] |
| RI Restriction (typeII-RI-Restriction-r16) |  | [0010] |
| Physical channel for CSI report | |  | PUSCH |
| CQI/RI/PMI delay | | ms | 6.5 |
| Maximum number of HARQ transmission | |  | 4 |
| Measurement channel | |  | [R.PDSCH.2-8.3 TDD] |
| Note 1: When Throughput is measured using random precoder selection, the precoder shall be updated in each slot (0.5 ms granularity) with equal probability of each applicable i1, i2 combination.  Note 2: If the UE reports in an available uplink reporting instance at slot#n based on PMI estimation at a downlink slot not later than slot#(n-6), this reported PMI cannot be applied at the gNB downlink before slot#(n+6).  Note 3: Randomization of the principle beam direction shall be used as specified in TBD. | | | |

Table 6.3.3.2.6-2: Minimum requirement

|  |  |
| --- | --- |
| **Parameter** | **Test 1** |
| ** | TBD |