**3GPP TSG-RAN WG4 Meeting #97-e *R4-2017556***

**Electronic Meeting, 2 - 13 Nov, 2020**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.141-2** | **CR** | **0256** | **rev** | **1** | **Current version:** | **16.5.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | CR for 38.141-2: | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, HiSilicon | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_HST\_Perf | | | | |  | ***Date:*** | | | 2020-11-11 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases:* *Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | RAN4 agree to introduce PRACH requirements of fading channel and the aligned requirements need to be added into the specfication | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Introduce the PRACH requirements of fading channel | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | PRACH requirements of fading channel are missing | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 8.4.1.6.1 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **x** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **x** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | Revised from R4-2016597 | | | | | | | | |

**<Start of First change>**

##### 8.4.1.6.1 Test requirement for *BS type 1-O*

Pfa shall not exceed 0.1%. Pd shall not be below 99% for the SNRs in tables 8.4.1.6.1-1 to 8.4.1.6.1-4.

Table 8.4.1.6.1-1: PRACH missed detection requirements for high speed train, burst format 0, restricted set type A, 1.25 kHz SCS

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Number of TX antennas | Number of demodulation | Propagation conditions and correlation matrix (annex J) | Frequency offset | SNR (dB) |
|  | branches |  |  | Burst format 0 |
| 1 | 2 | AWGN | 625 Hz | -11.7 |
|  |  | AWGN | 1340 Hz | -13.5 |
|  |  | TDLC300-100 Low | 0 Hz | [-5.8] |

Table 8.4.1.6.1-2: PRACH missed detection requirements for high speed train, burst format 0, restricted set type B, 1.25 kHz SCS

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Number of TX antennas | Number of demodulation | Propagation conditions and correlation matrix (annex J) | Frequency offset | SNR (dB) |
|  | branches |  |  | Burst format 0 |
| 1 | 2 | AWGN | 625 Hz | -11.3 |
|  |  | AWGN | 2334 Hz | -12.8 |
|  |  | TDLC300-100 Low | 0 Hz | [-5.5] |

Table 8.4.1.6.1-3: PRACH missed detection requirements for high speed train, 15 kHz SCS

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Number of | Number of | Propagation | Frequency | SNR (dB) | | |
| TX antennas | demodulation branches | conditions and correlation matrix (Annex G) | offset | Burst format A2 | Burst format B4 | Burst format C2 |
| 1 | 2 | AWGN | 1740 Hz | -11.0 | -14.0 | -10.8 |

Table 8.4.1.6.1-4: PRACH missed detection requirements for high speed train, 30 kHz SCS

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Number of | Number of | Propagation | Frequency | SNR (dB) | | |
| TX antennas | demodulation branches | conditions and correlation matrix (Annex G) | offset | Burst format A2 | Burst format B4 | Burst format C2 |
| 1 | 2 | AWGN | 3334 Hz | -10.9 | -14.3 | -10.7 |

**<end of First change>**