#######################################################################

# Anritsu Generated PICS/PIXIT file

#

# Changes Applied: 3GPP_TS_34.123-3

#######################################################################

pc_1xCSfallback,                             BOOLEAN,       false   #-- @desc  Support of 1xCS fallback

pc_1xRTT,                                    BOOLEAN,       false   #-- @desc  UE supports CDMA2000 1xRTT band class

pc_A5_4_CS,                                  BOOLEAN,       false   #-- Anritsu TTCN CR R5s150121 MCC

pc_A_BDS,                                    BOOLEAN,       false   #-- @desc  Support for A-BDS

pc_A_GLONASS,                                BOOLEAN,       false   #-- @desc  Support for A-GLONASS

pc_A_GPS_ADR,                                BOOLEAN,       false   #-- @desc  Support of ADR measurement reporting for Gps

pc_A_GPS_L1C,                                BOOLEAN,       false   #-- @desc  Support of A-GPS L1C signal

pc_A_GPS_L1C_A,                              BOOLEAN,       false   #-- @desc  Support for A-GPS L1CA

pc_A_GPS_L1C_A_MGPS,                         BOOLEAN,       false   #-- @desc  Support for A-GPS L1CA and Modernized GPS

pc_A_GPS_L2C,                                BOOLEAN,       false   #-- @desc  Support of A-GPS L2C signal

pc_A_GPS_L5,                                 BOOLEAN,       false   #-- @desc  Support of A-GPS L5 signal

pc_A_GPS_VelocityMeas,                       BOOLEAN,       false   #-- @desc  Support of Velocity measurement reporting for Gps

pc_A_Galileo,                                BOOLEAN,       false   #-- @desc  Support for A-Galileo

pc_A_QZSS,                                   BOOLEAN,       false   #-- @desc  Support of A-QZSS

pc_A_SBAS,                                   BOOLEAN,       false   #-- @desc  Support of A-SBAS

pc_Allowed_CSG_list,                         BOOLEAN,       TRUE    #-- @desc  Support of Allowed CSG list

pc_Attach,                                   BOOLEAN,       FALSE   #-- @desc  Support EPS attach (with or without pre-configuration)

pc_AttachWithIMSI,                           BOOLEAN,       false   #-- @desc  Support of Attach With IMSI

pc_Auto_Attach_after_TAU_Reject,             BOOLEAN,       false   #-- @desc  Support of automatic re-activation of the EPS bearer(s) after the TAU Reject

pc_Auto_PDN_Connectivity,                    BOOLEAN,       false   #-- @desc  Support of automatic PDN Connectivity in EUTRAN

pc_AutomaticAttachSwitchON,                  BOOLEAN,       FALSE   #-- @desc  Support of automatic PS attach procedure at switch on.

pc_AutomaticHRPD_PDN_Connection,             BOOLEAN,       FALSE   #-- @desc  Support of automatic PDN connection trigger on HRPD cell

pc_Automatic_EPS_Re_Attach,                  BOOLEAN,       false   #-- @desc  Support of automatic re-activation of the EPS bearer(s)

pc_Automatic_Re_Attach,                      BOOLEAN,       false   #-- @desc  Support of automatic re-activation of the EPS bearer(s) during Network Initiated Detach with detach type set to re-attach required

pc_Available_PLMNs_AcT_Ind,                  BOOLEAN,       false   #-- @desc  Support of AccessTechnology indication in available PLMNs list

pc_BDS,                                      BOOLEAN,       false   #-- @desc  Support for BDS

pc_BDS_ADR,                                  BOOLEAN,       false   #-- @desc  Support of ADR measurement reporting for BDS

pc_BDS_B1I,                                  BOOLEAN,       false   #-- @desc  Support for A-BDS B1I

pc_BDS_DiffCorr,                             BOOLEAN,       false   #-- @desc  Gnss-AuxiliaryInformationSupport for BDS

pc_BDS_GridMod,                              BOOLEAN,       false   #-- @desc  Gnss-AuxiliaryInformationSupport for BDS

pc_BDS_VelocityMeas,                         BOOLEAN,       false   #-- @desc  Support of Velocity measurement reporting for BDS

pc_BI_UG,                                    BOOLEAN,       false   #-- 

pc_BSRVCC,                                   BOOLEAN,       false   #-- @desc  UE indicates g.3gpp.ps2cs-srvcc-orig-pre-alerting media feature tag in INVITE request

pc_Background,                               BOOLEAN,       false   #-- @desc  UE Supports Background QoS class

pc_Band10_Supp,                              BOOLEAN,       false   #-- @desc  UE supports Frequency Band 10

pc_Band11_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 11

pc_Band12_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 12

pc_Band13_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 13

pc_Band14_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 14

pc_Band19_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 19

pc_Band1_Supp,                               BOOLEAN,       TRUE    #-- @desc  UE supports Frequency Band 1

pc_Band20_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 20

pc_Band21_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 21

pc_Band22_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 22

pc_Band25_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 25

pc_Band26_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 26

pc_Band2_Supp,                               BOOLEAN,       TRUE    #-- @desc  UE supports Frequency Band 2

pc_Band32_Supp,                              BOOLEAN,       false   #-- @desc  UE supports Frequency Band 32

pc_Band3_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 3

pc_Band4_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 4

pc_Band5_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 5

pc_Band6_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 6

pc_Band7_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 7

pc_Band8_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 8

pc_Band9_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 9

pc_BidirecVoiceOverIMS,                      BOOLEAN,       false   #-- @desc  UE capable of initiating a bidirectional voice session over IMS

pc_CMAS_Message,                             BOOLEAN,       false   #-- @desc  Support of CMAS message

pc_CS,                                       BOOLEAN,       TRUE    #-- @desc  UE supports CS domain services

pc_CS_Em_Call_in_1xRTT,                      BOOLEAN,       false   #-- @desc  Support for establishing the emergency call using the CS domain in 1xRTT

pc_CS_Em_Call_in_GERAN,                      BOOLEAN,       false   #-- @desc  Support for establishing the emergency call using the CS domain in GERAN

pc_CS_Em_Call_in_UTRA,                       BOOLEAN,       TRUE    #-- @desc  Support for establishing the emergency call using the CS domain in UTRA

pc_CS_Fallback,                              BOOLEAN,       false   #-- @desc  The UE supports CS fallback for voice calls. If true pc_CS and at least one of pc_FDD pc_TDD_HCR pc_TDD_LCR pc_TDD_VHCR or pc_UMTS_GSM is also true.

pc_CS_MO_LR_CSFallback,                      BOOLEAN,       false   #-- @desc  Support for CS-MO-LR with CS Fallback for a position estimate

pc_CS_PS_data_centric,                       BOOLEAN,       false   #-- @desc  Support of CSPS mode 2

pc_CS_PS_voice_centric,                      BOOLEAN,       false   #-- @desc  Support of configuring the UE to voice centric

pc_CS_SMS_only,                              BOOLEAN,       false   #-- @desc  The UE supports registration for SMS only.  If true pc_CS_fallback is false and at least one of pc_SMS_SGs_MT and pc_SMS_SGs_MO is true.

pc_Combined_Attach,                          BOOLEAN,       TRUE    #-- @desc  Support combined EPSIMSI attach (with or without pre-configuration)

pc_CommunicationHold_DuringEmergencyCall,    BOOLEAN,       false   #-- @desc  UE supports Communication Hold during emergency call

pc_DL_256QAM,                                BOOLEAN,       false   #-- @desc  Support of downlink 256 QAM

pc_DL_CA_2Carriers,                          BOOLEAN,       false   #-- @desc  DL CA with 2 carriers

pc_DL_CA_3Carriers,                          BOOLEAN,       false   #-- @desc  DL CA with 3 carriers

pc_DL_InterBand_CaBwclassA,                  BOOLEAN,       false   #-- @desc  DL Inter-band CA BW class A

pc_DL_InterBand_CaBwclassB,                  BOOLEAN,       false   #-- @desc  DL Inter-band CA BW class B

pc_DL_InterBand_CaBwclassC,                  BOOLEAN,       false   #-- @desc  DL Inter-band CA BW class C

pc_DL_IntraBand_ContCaBWclassB,              BOOLEAN,       false   #-- @desc  DL Intra-band contiguous CA BW class B

pc_DL_IntraBand_ContCaBWclassC,              BOOLEAN,       false   #-- @desc  DL Intra-band contiguous CA BW class C

pc_DL_interBand_CaBwClassComb_AA,            BOOLEAN,       false   #-- @desc  DL Inter-band contiguous CA BW class A-A

pc_DL_intraBand_nonContCaBwClassComb_AA,     BOOLEAN,       false   #-- @desc  Support of DL intra-band non-contiguous CA BW Class Combination A-A

pc_DSMIPv6,                                  BOOLEAN,       false   #-- @desc  Support of Mobility management based on Dual-Stack Mobile IPv6

pc_DaylightSavingTime,                       BOOLEAN,       false   #-- @desc  UE storesupdates the daylight saving time when receives information

pc_DualRM_Coding,                            BOOLEAN,       false   #-- @desc  Dual RM Coding

pc_Dynamic_GERAN_Rel_downgrade,              BOOLEAN,       false   #-- @desc  Dynamically downgrades the GERAN release when the support of EPS is disabled

pc_EAB,                                      BOOLEAN,       false   #-- @desc  Support of Extended Access Barring

pc_EAB_override,                             BOOLEAN,       false   #-- @desc  Support of Extended Access Barring Override

pc_ECID,                                     BOOLEAN,       false   #-- @desc  Support of UE assisted ECID

pc_ECID_Rsrp,                                BOOLEAN,       false   #-- @desc  RSRP Supported

pc_ECID_Rsrq,                                BOOLEAN,       false   #-- @desc  RSRQ Supported

pc_ECID_UeRxTx,                              BOOLEAN,       false   #-- @desc  UE Rx-Tx Time Difference Supported

pc_EDCH_UE_Category_FDD,                     INTEGER,       1       #-- @desc  FDD E-DCH physical layer categories

pc_EDCH_UE_Category_TDD,                     INTEGER,       1       #-- @desc  LCR TDD E-DCH physical layer categories

pc_EDTM,                                     BOOLEAN,       false   #-- @desc  Support for EDTM

pc_EMM_Information,                          BOOLEAN,       false   #-- @desc  Support of EMM Information message

pc_EPC_AutomaticAttachSwitchOn,              BOOLEAN,       false   #-- @desc  Support of automatic re-activation oof the EPS bearers during network initiated detach even though UE has initiated a detach procedure with detach type set to EPS detach or combined EPSIMSI detach

pc_EPC_MO_LR_RequestAssistanceData,          BOOLEAN,       false   #-- @desc  Support of EPC-MO-LR request for assistance data

pc_EPC_MO_LR_RequestPositionEstimate,        BOOLEAN,       false   #-- @desc  Support of EPC-MO-LR request for a position estimate

pc_EPS_Disable,                              BOOLEAN,       false   #-- @desc  Support of disabling of EPS capability

pc_EPS_Services_Disable,                     BOOLEAN,       false   #-- @desc  Support of disabling of EPS services

pc_ESM_MO_Bearer_Allocation,                 BOOLEAN,       false   #-- @desc  Support of ESM UE requested bearer resource allocation procedure

pc_ESM_MO_Bearer_Modification,               BOOLEAN,       false   #-- @desc  Support of ESM UE requested bearer resource modification procedure

pc_ESM_Notification,                         BOOLEAN,       false   #-- @desc  Support of ESM Notification procedure

pc_ESM_UE_Modification_NW_TFT,               BOOLEAN,       false   #-- @desc  Support for UE requested modification of network allocated TFTs

pc_ETWS_message,                             BOOLEAN,       false   #-- @desc  Support of ETWS message

pc_ETWS_message_security,                    BOOLEAN,       false   #-- @desc  Support of ETWS message with security

pc_E_UTRAN_2_GERAN_PSHO,                     BOOLEAN,       false   #-- @desc  Support for inter-RAT PS handover from E_UTRAN to GERAN

pc_E_UTRA_WLAN_offload,                      BOOLEAN,       false   #-- @desc  Support Offload tofrom WLAN and supports S2b

pc_EarlyMedia,                               BOOLEAN,       false   #-- @desc  UE supports early media

pc_EmergSpeech,                              BOOLEAN,       TRUE    #-- @desc  Emergency Call

pc_Enhanced_1xCSfallback,                    BOOLEAN,       false   #-- @desc  Support of Enhanced 1xCS fallback

pc_FDD,                                      BOOLEAN,       false   #-- @desc  UE supports UTRA band as defined in TS 25.101

pc_FDD_TypeB_HalfDuplex,                     BOOLEAN,       false   #-- @desc  Support of Type B Half duplex FDD operation

pc_FDPCH,                                    BOOLEAN,       false   #-- @desc  Full support of F-DPCH

pc_FeatrGrp_1,                               BOOLEAN,       false   #-- @desc  Support of Intra-subframe frequency hopping for PUSCH scheduled by UL grant Extended cyclic prefix with f = 7.5kHz for DL resource block DCI format 3a (TPC commands for PUCCH and PUSCH with single bit power adjustments) Multi-user MIMO for PDSCH Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-0 - UE selected subband CQI without PMI Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2 - UE selected subband CQI with multiple PMI

pc_FeatrGrp_10,                              BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to GERAN (Packet_)Idle by Cell Change Order EUTRA RRC_CONNECTED to GERAN (Packet_)Idle by Cell Change Order with NACC (Network Assisted Cell Change)

pc_FeatrGrp_101,                             BOOLEAN,       false   #-- @desc  DMRS with OCC (orthogonal cover code) and SGH (sequence group hopping) disabling

pc_FeatrGrp_101_F,                           BOOLEAN,       false   #-- @desc  DMRS with OCC (orthogonal cover code) and SGH (sequence group hopping) disabling

pc_FeatrGrp_101_T,                           BOOLEAN,       false   #-- @desc  DMRS with OCC (orthogonal cover code) and SGH (sequence group hopping) disabling

pc_FeatrGrp_102,                             BOOLEAN,       false   #-- @desc  Trigger type 1 SRS (aperiodic SRS) transmission (Up to X ports)

pc_FeatrGrp_102_F,                           BOOLEAN,       false   #-- @desc  Trigger type 1 SRS (aperiodic SRS) transmission (Up to X ports)

pc_FeatrGrp_102_T,                           BOOLEAN,       false   #-- @desc  Trigger type 1 SRS (aperiodic SRS) transmission (Up to X ports)

pc_FeatrGrp_103,                             BOOLEAN,       false   #-- @desc  PDSCH transmission mode 9 when up to 4 CSI reference signal ports are configured

pc_FeatrGrp_103_F,                           BOOLEAN,       false   #-- @desc  PDSCH transmission mode 9 when up to 4 CSI reference signal ports are configured

pc_FeatrGrp_103_T,                           BOOLEAN,       false   #-- @desc  PDSCH transmission mode 9 when up to 4 CSI reference signal ports are configured

pc_FeatrGrp_104,                             BOOLEAN,       false   #-- @desc  PDSCH transmission mode 9 for TDD when 8 CSI reference signal ports are configured

pc_FeatrGrp_104_F,                           BOOLEAN,       false   #-- @desc  PDSCH transmission mode 9 for TDD when 8 CSI reference signal ports are configured

pc_FeatrGrp_104_T,                           BOOLEAN,       false   #-- @desc  PDSCH transmission mode 9 for TDD when 8 CSI reference signal ports are configured

pc_FeatrGrp_105,                             BOOLEAN,       false   #-- @desc  Periodic CQIPMIRI reporting on PUCCH: Mode 2-0:UE selected subband CQI without PMI when PDSCH transmission mode 9 is configured.Periodic CQIPMIRI reporting on PUCCH: Mode 2-1:UE selected subband CQI with single PMI when PDSCH transmission mode 9 and up to 4 CSI reference signal ports are configured

pc_FeatrGrp_105_F,                           BOOLEAN,       false   #-- @desc  Periodic CQIPMIRI reporting on PUCCH: Mode 2-0:UE selected subband CQI without PMI when PDSCH transmission mode 9 is configured.Periodic CQIPMIRI reporting on PUCCH: Mode 2-1:UE selected subband CQI with single PMI when PDSCH transmission mode 9 and up to 4 CSI reference signal ports are configured

pc_FeatrGrp_105_T,                           BOOLEAN,       false   #-- @desc  Periodic CQIPMIRI reporting on PUCCH: Mode 2-0:UE selected subband CQI without PMI when PDSCH transmission mode 9 is configured.Periodic CQIPMIRI reporting on PUCCH: Mode 2-1:UE selected subband CQI with single PMI when PDSCH transmission mode 9 and up to 4 CSI reference signal ports are configured

pc_FeatrGrp_106,                             BOOLEAN,       false   #-- @desc  Periodic CQIPMIRIPTI reporting on PUCCH: Mode 2-1: UE selected subband CQI with single PMI when PDSCH transmission mode 9 and 8 CSI reference signal ports are configured

pc_FeatrGrp_106_F,                           BOOLEAN,       false   #-- @desc  Periodic CQIPMIRIPTI reporting on PUCCH: Mode 2-1: UE selected subband CQI with single PMI when PDSCH transmission mode 9 and 8 CSI reference signal ports are configured

pc_FeatrGrp_106_T,                           BOOLEAN,       false   #-- @desc  Periodic CQIPMIRIPTI reporting on PUCCH: Mode 2-1: UE selected subband CQI with single PMI when PDSCH transmission mode 9 and 8 CSI reference signal ports are configured

pc_FeatrGrp_107,                             BOOLEAN,       false   #-- @desc  Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-0: UE selected subband CQI without PMI when PDSCH transmission mode 9 is configured. Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2: UE selected subband CQI with multiple PMI when PDSCH transmission mode 9 and up to 4 CSI reference signal ports are configured

pc_FeatrGrp_107_F,                           BOOLEAN,       false   #-- @desc  Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-0: UE selected subband CQI without PMI when PDSCH transmission mode 9 is configured. Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2: UE selected subband CQI with multiple PMI when PDSCH transmission mode 9 and up to 4 CSI reference signal ports are configured

pc_FeatrGrp_107_T,                           BOOLEAN,       false   #-- @desc  Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-0: UE selected subband CQI without PMI when PDSCH transmission mode 9 is configured. Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2: UE selected subband CQI with multiple PMI when PDSCH transmission mode 9 and up to 4 CSI reference signal ports are configured

pc_FeatrGrp_108,                             BOOLEAN,       false   #-- @desc  Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2: UE selected subband CQI with multiple PMI when PDSCH transmission mode 9 and 8 CSI reference signal ports are configured

pc_FeatrGrp_108_F,                           BOOLEAN,       false   #-- @desc  Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2: UE selected subband CQI with multiple PMI when PDSCH transmission mode 9 and 8 CSI reference signal ports are configured

pc_FeatrGrp_108_T,                           BOOLEAN,       false   #-- @desc  Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2: UE selected subband CQI with multiple PMI when PDSCH transmission mode 9 and 8 CSI reference signal ports are configured

pc_FeatrGrp_109,                             BOOLEAN,       false   #-- @desc  Periodic CQIPMIRI reporting on PUCCH Mode 1-1 submode 1

pc_FeatrGrp_109_F,                           BOOLEAN,       false   #-- @desc  Periodic CQIPMIRI reporting on PUCCH Mode 1-1 submode 1

pc_FeatrGrp_109_T,                           BOOLEAN,       false   #-- @desc  Periodic CQIPMIRI reporting on PUCCH Mode 1-1 submode 1

pc_FeatrGrp_10_F,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to GERAN (Packet_)Idle by Cell Change Order EUTRA RRC_CONNECTED to GERAN (Packet_)Idle by Cell Change Order with NACC (Network Assisted Cell Change)

pc_FeatrGrp_10_T,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to GERAN (Packet_)Idle by Cell Change Order EUTRA RRC_CONNECTED to GERAN (Packet_)Idle by Cell Change Order with NACC (Network Assisted Cell Change)

pc_FeatrGrp_11,                              BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to 1xRTT CS Active handover

pc_FeatrGrp_110,                             BOOLEAN,       false   #-- @desc  Periodic CQIPMIRI reporting on PUCCH Mode 1-1 submode 2

pc_FeatrGrp_110_F,                           BOOLEAN,       false   #-- @desc  Periodic CQIPMIRI reporting on PUCCH Mode 1-1 submode 2

pc_FeatrGrp_110_T,                           BOOLEAN,       false   #-- @desc  Periodic CQIPMIRI reporting on PUCCH Mode 1-1 submode 2

pc_FeatrGrp_111,                             BOOLEAN,       false   #-- @desc  Measurement reporting trigger Event A6

pc_FeatrGrp_111_F,                           BOOLEAN,       false   #-- @desc  Measurement reporting trigger Event A6

pc_FeatrGrp_111_T,                           BOOLEAN,       false   #-- @desc  Measurement reporting trigger Event A6

pc_FeatrGrp_112,                             BOOLEAN,       false   #-- @desc  SCell addition within the Handover to EUTRA procedure

pc_FeatrGrp_112_F,                           BOOLEAN,       false   #-- @desc  SCell addition within the Handover to EUTRA procedure

pc_FeatrGrp_112_T,                           BOOLEAN,       false   #-- @desc  SCell addition within the Handover to EUTRA procedure

pc_FeatrGrp_113,                             BOOLEAN,       false   #-- @desc  Trigger type 0 SRS (periodic SRS) transmission on X Serving Cells

pc_FeatrGrp_113_F,                           BOOLEAN,       false   #-- @desc  Trigger type 0 SRS (periodic SRS) transmission on X Serving Cells

pc_FeatrGrp_113_T,                           BOOLEAN,       false   #-- @desc  Trigger type 0 SRS (periodic SRS) transmission on X Serving Cells

pc_FeatrGrp_114,                             BOOLEAN,       false   #-- @desc  Reporting of both UTRA CPICH RSCP and EcN0 in a Measurement Report

pc_FeatrGrp_114_F,                           BOOLEAN,       false   #-- @desc  Reporting of both UTRA CPICH RSCP and EcN0 in a Measurement Report

pc_FeatrGrp_114_T,                           BOOLEAN,       false   #-- @desc  Reporting of both UTRA CPICH RSCP and EcN0 in a Measurement Report

pc_FeatrGrp_115,                             BOOLEAN,       false   #-- @desc  time domain ICIC RLMRRM measurement subframe restriction for the serving cell. time domain ICIC RRM measurement subframe restriction for neighbour cells. time domain ICIC CSI measurement subframe restriction

pc_FeatrGrp_115_F,                           BOOLEAN,       false   #-- @desc  time domain ICIC RLMRRM measurement subframe restriction for the serving cell. time domain ICIC RRM measurement subframe restriction for neighbour cells. time domain ICIC CSI measurement subframe restriction

pc_FeatrGrp_115_T,                           BOOLEAN,       false   #-- @desc  time domain ICIC RLMRRM measurement subframe restriction for the serving cell. time domain ICIC RRM measurement subframe restriction for neighbour cells. time domain ICIC CSI measurement subframe restriction

pc_FeatrGrp_116,                             BOOLEAN,       false   #-- @desc  Relative transmit phase continuity for spatial multiplexing in UL

pc_FeatrGrp_116_F,                           BOOLEAN,       false   #-- @desc  Relative transmit phase continuity for spatial multiplexing in UL

pc_FeatrGrp_116_T,                           BOOLEAN,       false   #-- @desc  Relative transmit phase continuity for spatial multiplexing in UL

pc_FeatrGrp_11_F,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to 1xRTT CS Active handover

pc_FeatrGrp_11_T,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to 1xRTT CS Active handover

pc_FeatrGrp_12,                              BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to HRPD Active handover

pc_FeatrGrp_12_F,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to HRPD Active handover

pc_FeatrGrp_12_T,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to HRPD Active handover

pc_FeatrGrp_13,                              BOOLEAN,       false   #-- @desc  Support of Inter-frequency handover (within FDD or TDD)

pc_FeatrGrp_13_F,                            BOOLEAN,       false   #-- @desc  Support of Inter-frequency handover (within FDD or TDD)

pc_FeatrGrp_13_T,                            BOOLEAN,       false   #-- @desc  Support of Inter-frequency handover (within FDD or TDD)

pc_FeatrGrp_14,                              BOOLEAN,       false   #-- @desc  Support of Measurement reporting event: Event A4 - Neighbour > threshold Measurement reporting event: Event A5 - Serving < threshold1 & Neighbour > threshold2

pc_FeatrGrp_14_F,                            BOOLEAN,       false   #-- @desc  Support of Measurement reporting event: Event A4 - Neighbour > threshold Measurement reporting event: Event A5 - Serving < threshold1 & Neighbour > threshold2

pc_FeatrGrp_14_T,                            BOOLEAN,       false   #-- @desc  Support of Measurement reporting event: Event A4 - Neighbour > threshold Measurement reporting event: Event A5 - Serving < threshold1 & Neighbour > threshold2

pc_FeatrGrp_15,                              BOOLEAN,       false   #-- @desc  Support of Measurement reporting event: Event B1 - Neighbour > threshold

pc_FeatrGrp_15_F,                            BOOLEAN,       false   #-- @desc  Support of Measurement reporting event: Event B1 - Neighbour > threshold

pc_FeatrGrp_15_T,                            BOOLEAN,       false   #-- @desc  Support of Measurement reporting event: Event B1 - Neighbour > threshold

pc_FeatrGrp_16,                              BOOLEAN,       false   #-- @desc  Support of Periodical measurement reporting for non-ANR related measurements

pc_FeatrGrp_16_F,                            BOOLEAN,       false   #-- @desc  Support of Periodical measurement reporting for non-ANR related measurements

pc_FeatrGrp_16_T,                            BOOLEAN,       false   #-- @desc  Support of Periodical measurement reporting for non-ANR related measurements

pc_FeatrGrp_17,                              BOOLEAN,       false   #-- @desc  Support of Periodical measurement reporting for SON  ANR and ANR related intra-frequency measurement reporting events

pc_FeatrGrp_17_F,                            BOOLEAN,       false   #-- @desc  Support of Periodical measurement reporting for SON  ANR and ANR related intra-frequency measurement reporting events

pc_FeatrGrp_17_T,                            BOOLEAN,       false   #-- @desc  Support of Periodical measurement reporting for SON  ANR and ANR related intra-frequency measurement reporting events

pc_FeatrGrp_18,                              BOOLEAN,       false   #-- @desc  Support of ANR related inter-frequency measurement reporting events

pc_FeatrGrp_18_F,                            BOOLEAN,       false   #-- @desc  Support of ANR related inter-frequency measurement reporting events

pc_FeatrGrp_18_T,                            BOOLEAN,       false   #-- @desc  Support of ANR related inter-frequency measurement reporting events

pc_FeatrGrp_19,                              BOOLEAN,       false   #-- @desc  Support of ANR related inter-RAT measurement reporting events

pc_FeatrGrp_19_F,                            BOOLEAN,       false   #-- @desc  Support of ANR related inter-RAT measurement reporting events

pc_FeatrGrp_19_T,                            BOOLEAN,       false   #-- @desc  Support of ANR related inter-RAT measurement reporting events

pc_FeatrGrp_1_F,                             BOOLEAN,       false   #-- @desc  Support of Intra-subframe frequency hopping for PUSCH scheduled by UL grant Extended cyclic prefix with f = 7.5kHz for DL resource block DCI format 3a (TPC commands for PUCCH and PUSCH with single bit power adjustments) Multi-user MIMO for PDSCH Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-0 - UE selected subband CQI without PMI Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2 - UE selected subband CQI with multiple PMI

pc_FeatrGrp_1_T,                             BOOLEAN,       false   #-- @desc  Support of Intra-subframe frequency hopping for PUSCH scheduled by UL grant Extended cyclic prefix with f = 7.5kHz for DL resource block DCI format 3a (TPC commands for PUCCH and PUSCH with single bit power adjustments) Multi-user MIMO for PDSCH Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-0 - UE selected subband CQI without PMI Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2 - UE selected subband CQI with multiple PMI

pc_FeatrGrp_2,                               BOOLEAN,       false   #-- @desc  Support of Simultaneous CQI and ACKNACK on PUCCH i.e. PUCCH format 2a and 2b Absolute TPC command for PUSCH Resource allocation type 1 for PDSCH Periodic CQIPMIRI reporting on PUCCH: Mode 2- 0 - UE selected subband CQI without PMI Periodic CQIPMIRI reporting on PUCCH: Mode 2-1 - UE selected subband CQI with single PMI

pc_FeatrGrp_20,                              BOOLEAN,       false   #-- @desc  Support of RB combination: SRB1 and SRB2 for DCCH + x AM DRB + x UM DRB

pc_FeatrGrp_20_F,                            BOOLEAN,       false   #-- @desc  Support of RB combination: SRB1 and SRB2 for DCCH + x AM DRB + x UM DRB

pc_FeatrGrp_20_T,                            BOOLEAN,       false   #-- @desc  Support of RB combination: SRB1 and SRB2 for DCCH + x AM DRB + x UM DRB

pc_FeatrGrp_21,                              BOOLEAN,       false   #-- @desc  Support of Predefined intra-subframe frequency hopping for PUSCH with N_sb > 1 Predefined inter-subframe frequency hopping for PUSCH with N_sb > 1

pc_FeatrGrp_21_F,                            BOOLEAN,       false   #-- @desc  Support of Predefined intra-subframe frequency hopping for PUSCH with N_sb > 1 Predefined inter-subframe frequency hopping for PUSCH with N_sb > 1

pc_FeatrGrp_21_T,                            BOOLEAN,       false   #-- @desc  Support of Predefined intra-subframe frequency hopping for PUSCH with N_sb > 1 Predefined inter-subframe frequency hopping for PUSCH with N_sb > 1

pc_FeatrGrp_22,                              BOOLEAN,       false   #-- @desc  Support of UTRAN measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_22_F,                            BOOLEAN,       false   #-- @desc  Support of UTRAN measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_22_T,                            BOOLEAN,       false   #-- @desc  Support of UTRAN measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_23,                              BOOLEAN,       false   #-- @desc  Support of GERAN measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_23_F,                            BOOLEAN,       false   #-- @desc  Support of GERAN measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_23_T,                            BOOLEAN,       false   #-- @desc  Support of GERAN measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_24,                              BOOLEAN,       false   #-- @desc  Support of cdma2000 measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_24_F,                            BOOLEAN,       false   #-- @desc  Support of cdma2000 measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_24_T,                            BOOLEAN,       false   #-- @desc  Support of cdma2000 measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_25,                              BOOLEAN,       false   #-- @desc  Support of Inter-frequency measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_25_F,                            BOOLEAN,       false   #-- @desc  Support of Inter-frequency measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_25_T,                            BOOLEAN,       false   #-- @desc  Support of Inter-frequency measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_26,                              BOOLEAN,       false   #-- @desc  Support of HRPD measurements reporting and measurement reporting event B2 in E-UTRA connected mode

pc_FeatrGrp_26_F,                            BOOLEAN,       false   #-- @desc  Support of HRPD measurements reporting and measurement reporting event B2 in E-UTRA connected mode

pc_FeatrGrp_26_T,                            BOOLEAN,       false   #-- @desc  Support of HRPD measurements reporting and measurement reporting event B2 in E-UTRA connected mode

pc_FeatrGrp_27,                              BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to UTRA CELL_DCH CS handover

pc_FeatrGrp_27_F,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to UTRA CELL_DCH CS handover

pc_FeatrGrp_27_T,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to UTRA CELL_DCH CS handover

pc_FeatrGrp_28,                              BOOLEAN,       false   #-- @desc  Support of TTI bundling

pc_FeatrGrp_28_F,                            BOOLEAN,       false   #-- @desc  Support of TTI bundling

pc_FeatrGrp_28_T,                            BOOLEAN,       false   #-- @desc  Support of TTI bundling

pc_FeatrGrp_29,                              BOOLEAN,       false   #-- @desc  Support of Semi-Persistent Scheduling

pc_FeatrGrp_29_F,                            BOOLEAN,       false   #-- @desc  Support of Semi-Persistent Scheduling

pc_FeatrGrp_29_T,                            BOOLEAN,       false   #-- @desc  Support of Semi-Persistent Scheduling

pc_FeatrGrp_2_F,                             BOOLEAN,       false   #-- @desc  Support of Simultaneous CQI and ACKNACK on PUCCH i.e. PUCCH format 2a and 2b Absolute TPC command for PUSCH Resource allocation type 1 for PDSCH Periodic CQIPMIRI reporting on PUCCH: Mode 2- 0 - UE selected subband CQI without PMI Periodic CQIPMIRI reporting on PUCCH: Mode 2-1 - UE selected subband CQI with single PMI

pc_FeatrGrp_2_T,                             BOOLEAN,       false   #-- @desc  Support of Simultaneous CQI and ACKNACK on PUCCH i.e. PUCCH format 2a and 2b Absolute TPC command for PUSCH Resource allocation type 1 for PDSCH Periodic CQIPMIRI reporting on PUCCH: Mode 2- 0 - UE selected subband CQI without PMI Periodic CQIPMIRI reporting on PUCCH: Mode 2-1 - UE selected subband CQI with single PMI

pc_FeatrGrp_3,                               BOOLEAN,       false   #-- @desc  Support of Semi-persistent scheduling TTI bundling 5bit RLC UM SN 7bit PDCP SN

pc_FeatrGrp_30,                              BOOLEAN,       false   #-- @desc  Support of Handover between FDD and TDD

pc_FeatrGrp_30_F,                            BOOLEAN,       false   #-- @desc  Support of Handover between FDD and TDD

pc_FeatrGrp_30_T,                            BOOLEAN,       false   #-- @desc  Support of Handover between FDD and TDD

pc_FeatrGrp_31,                              BOOLEAN,       false   #-- @desc  Support of the mechanisms defined for cells broadcasting multi band information i.e. comprehending multiBandInfoList

pc_FeatrGrp_31_F,                            BOOLEAN,       false   #-- @desc  Support of the mechanisms defined for cells broadcasting multi band information i.e. comprehending multiBandInfoList

pc_FeatrGrp_31_T,                            BOOLEAN,       false   #-- @desc  Support of the mechanisms defined for cells broadcasting multi band information i.e. comprehending multiBandInfoList

pc_FeatrGrp_33,                              BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for UTRAN including:

pc_FeatrGrp_33_F,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for UTRAN including:  Inter-RAT periodical measurement reporting where triggerType is set to periodical and purpose is set to reportStrongestCellsForSON

pc_FeatrGrp_33_T,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for UTRAN including:

pc_FeatrGrp_34,                              BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for GERAN including:

pc_FeatrGrp_34_F,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for GERAN including:

pc_FeatrGrp_34_T,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for GERAN including:

pc_FeatrGrp_35,                              BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for 1xRTT including:

pc_FeatrGrp_35_F,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for 1xRTT including:

pc_FeatrGrp_35_T,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for 1xRTT including:

pc_FeatrGrp_36,                              BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for HRPD including:

pc_FeatrGrp_36_F,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for HRPD including:

pc_FeatrGrp_36_T,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for HRPD including:  Inter-RAT periodical measurement reporting where triggerType is set to periodical and purpose is set to portStrongestCellsForSON

pc_FeatrGrp_37,                              BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for UTRAN TDD including:

pc_FeatrGrp_37_F,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for UTRAN TDD including:

pc_FeatrGrp_37_T,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for UTRAN TDD including:

pc_FeatrGrp_38,                              BOOLEAN,       false   #-- @desc  EUTRA RRC_CONNECTED to UTRA TDD CELL_DCH PS handover if the UE supports both UTRAN FDD and UTRAN TDD

pc_FeatrGrp_38_F,                            BOOLEAN,       false   #-- @desc  EUTRA RRC_CONNECTED to UTRA TDD CELL_DCH PS handover if the UE supports both UTRAN FDD and UTRAN TDD

pc_FeatrGrp_38_T,                            BOOLEAN,       false   #-- @desc  EUTRA RRC_CONNECTED to UTRA TDD CELL_DCH PS handover if the UE supports both UTRAN FDD and UTRAN TDD

pc_FeatrGrp_39,                              BOOLEAN,       false   #-- @desc  UTRAN TDD measurements reporting and measurement reporting event B2 in E-UTRA connected mode if the UE supports both UTRAN FDD and UTRAN TDD

pc_FeatrGrp_39_F,                            BOOLEAN,       false   #-- @desc  UTRAN TDD measurements reporting and measurement reporting event B2 in E-UTRA connected mode if the UE supports both UTRAN FDD and UTRAN TDD

pc_FeatrGrp_39_T,                            BOOLEAN,       false   #-- @desc  UTRAN TDD measurements reporting and measurement reporting event B2 in E-UTRA connected mode if the UE supports both UTRAN FDD and UTRAN TDD

pc_FeatrGrp_3_F,                             BOOLEAN,       false   #-- @desc  Support of Semi-persistent scheduling TTI bundling 5bit RLC UM SN 7bit PDCP SN

pc_FeatrGrp_3_T,                             BOOLEAN,       false   #-- @desc  Support of Semi-persistent scheduling TTI bundling 5bit RLC UM SN 7bit PDCP SN

pc_FeatrGrp_4,                               BOOLEAN,       false   #-- @desc  Support of Short DRX cycle

pc_FeatrGrp_40,                              BOOLEAN,       false   #-- @desc  EUTRA RRC_CONNECTED to UTRA TDD  CELL_DCH  CS handover if the UE supports both UTRAN FDD and UTRAN TDD

pc_FeatrGrp_40_F,                            BOOLEAN,       false   #-- @desc  EUTRA RRC_CONNECTED to UTRA TDD  CELL_DCH  CS handover if the UE supports both UTRAN FDD and UTRAN TDD

pc_FeatrGrp_40_T,                            BOOLEAN,       false   #-- @desc  EUTRA RRC_CONNECTED to UTRA TDD  CELL_DCH  CS handover if the UE supports both UTRAN FDD and UTRAN TDD

pc_FeatrGrp_41,                              BOOLEAN,       false   #-- @desc  Measurement reporting event: Event B1 û Neighbour > threshold for UTRAN FDD if the UE supports UTRAN FDD and has set bit number 22 to 1

pc_FeatrGrp_41_F,                            BOOLEAN,       false   #-- @desc  Measurement reporting event: Event B1 û Neighbour > threshold for UTRAN FDD if the UE supports UTRAN FDD and has set bit number 22 to 1

pc_FeatrGrp_41_T,                            BOOLEAN,       false   #-- @desc  Measurement reporting event: Event B1 û Neighbour > threshold for UTRAN FDD if the UE supports UTRAN FDD and has set bit number 22 to 1

pc_FeatrGrp_4_F,                             BOOLEAN,       false   #-- @desc  Support of Short DRX cycle

pc_FeatrGrp_4_T,                             BOOLEAN,       false   #-- @desc  Support of Short DRX cycle

pc_FeatrGrp_5,                               BOOLEAN,       false   #-- @desc  Support of Long DRX cycle DRX command MAC control element

pc_FeatrGrp_5_F,                             BOOLEAN,       false   #-- @desc  Support of Long DRX cycle DRX command MAC control element

pc_FeatrGrp_5_T,                             BOOLEAN,       false   #-- @desc  Support of Long DRX cycle DRX command MAC control element

pc_FeatrGrp_6,                               BOOLEAN,       false   #-- @desc  Support of Piroritized bit rate

pc_FeatrGrp_6_F,                             BOOLEAN,       false   #-- @desc  Support of Piroritized bit rate

pc_FeatrGrp_6_T,                             BOOLEAN,       false   #-- @desc  Support of Piroritized bit rate

pc_FeatrGrp_7,                               BOOLEAN,       false   #-- @desc  Support of RLC UM

pc_FeatrGrp_7_F,                             BOOLEAN,       false   #-- @desc  Support of RLC UM

pc_FeatrGrp_7_T,                             BOOLEAN,       false   #-- @desc  Support of RLC UM

pc_FeatrGrp_8,                               BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to UTRA CELL_DCH PS handover

pc_FeatrGrp_8_F,                             BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to UTRA CELL_DCH PS handover

pc_FeatrGrp_8_T,                             BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to UTRA CELL_DCH PS handover

pc_FeatrGrp_9,                               BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to GERAN GSM_Dedicated handover

pc_FeatrGrp_9_F,                             BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to GERAN GSM_Dedicated handover

pc_FeatrGrp_9_T,                             BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to GERAN GSM_Dedicated handover

pc_FullNameNetwork,                          BOOLEAN,       false   #-- @desc  Support of storage of the network full name

pc_Full_FDPCH,                               BOOLEAN,       false   #-- @desc  Full support of F-DPCH

pc_GALILEO,                                  BOOLEAN,       false   #-- @desc  Support for Galileo

pc_GALILEO_ADR,                              BOOLEAN,       false   #-- @desc  Support of ADR measurement reporting for Galileo

pc_GALILEO_E1,                               BOOLEAN,       false   #-- @desc  Support of E1 signal in Galileo

pc_GALILEO_E5a,                              BOOLEAN,       false   #-- @desc  Support of E5a signal in Galileo

pc_GALILEO_E5aE5b,                           BOOLEAN,       false   #-- @desc  Support of E5a+E5b signal in Galileo

pc_GALILEO_E5b,                              BOOLEAN,       false   #-- @desc  Support of E5b signal in Galileo

pc_GALILEO_E6,                               BOOLEAN,       false   #-- @desc  Support of E6 signal in Galileo

pc_GALILEO_VelocityMeas,                     BOOLEAN,       false   #-- @desc  Support of Velocity measurement reporting for Galileo

pc_GBAForXCAPAuthentication,                 BOOLEAN,       false   #-- @desc  UE supports and uses GBA for XCAP authentication

pc_GERAN,                                    BOOLEAN,       TRUE    #-- @desc  UE Supports GSM andor GPRS

pc_GERAN_2_E_UTRAN_PSHO,                     BOOLEAN,       false   #-- @desc  Support of GERAN to E-UTRAN PS Handover

pc_GERAN_2_E_UTRAN_meas,                     BOOLEAN,       false   #-- @desc  Supports Neighbour Cell measurements and Network controlled & autonomous cell reselection to E-UTRAN

pc_GERAN_2_E_UTRAN_measreporting_CCN,        BOOLEAN,       false   #-- @desc  Supports CCN towards E-UTRAN E-UTRAN Neighbour cell measurement reporting and Network controlled cell reselection to E-UTRAN

pc_GLONASS,                                  BOOLEAN,       false   #-- @desc  Support for GLONASS

pc_GLONASS_ADR,                              BOOLEAN,       false   #-- @desc  Support of ADR measurement reporting for Glonass

pc_GLONASS_G1,                               BOOLEAN,       false   #-- @desc  Support of G1 signal in Glonass

pc_GLONASS_G2,                               BOOLEAN,       false   #-- @desc  Support of G2 signal in Glonass

pc_GLONASS_G3,                               BOOLEAN,       false   #-- @desc  Support of G3 signal in Glonass

pc_GLONASS_VelocityMeas,                     BOOLEAN,       false   #-- @desc  Support of Velocity measurement reporting for Glonass

pc_GNSS_AA,                                  BOOLEAN,       false   #-- @desc  Support of GNSS Acquisition Assistance

pc_GNSS_AcquAssistSup_BDS,                   BOOLEAN,       false   #-- @desc  Gnss-AcquisitionAssistanceSupport for BDS

pc_GNSS_AcquAssistSup_Galileo,               BOOLEAN,       false   #-- @desc  Gnss-AcquisitionAssistanceSupport for galileo

pc_GNSS_AcquAssistSup_Glonass,               BOOLEAN,       false   #-- @desc  Gnss-AcquisitionAssistanceSupport for glonass

pc_GNSS_AcquAssistSup_Gps,                   BOOLEAN,       false   #-- @desc  Gnss-AcquisitionAssistanceSupport for gps

pc_GNSS_AcquAssistSup_Qzss,                  BOOLEAN,       false   #-- @desc  Gnss-AcquisitionAssistanceSupport for qzss

pc_GNSS_AcquAssistSup_Sbas,                  BOOLEAN,       false   #-- @desc  Gnss-AcquisitionAssistanceSupport for sbas

pc_GNSS_AlmanacSup_BDS,                      BOOLEAN,       false   #-- @desc  Gnss-AlmanacSupport for BDS

pc_GNSS_AlmanacSup_Galileo,                  BOOLEAN,       false   #-- @desc  Gnss-AlmanacSupport for galileo

pc_GNSS_AlmanacSup_Glonass,                  BOOLEAN,       false   #-- @desc  Gnss-AlmanacSupport for glonass

pc_GNSS_AlmanacSup_Gps,                      BOOLEAN,       false   #-- @desc  Gnss-AlmanacSupport for gps

pc_GNSS_AlmanacSup_Qzss,                     BOOLEAN,       false   #-- @desc  Gnss-AlmanacSupport for qzss

pc_GNSS_AlmanacSup_Sbas,                     BOOLEAN,       false   #-- @desc  Gnss-AlmanacSupport for sbas

pc_GNSS_AuxInfoSup_BDS,                      BOOLEAN,       false   #-- @desc  Gnss-AuxiliaryInformationSupport for BDS

pc_GNSS_AuxInfoSup_Galileo,                  BOOLEAN,       false   #-- @desc  Gnss-AuxiliaryInformationSupport for galileo

pc_GNSS_AuxInfoSup_Glonass,                  BOOLEAN,       false   #-- @desc  Gnss-AuxiliaryInformationSupport for glonass

pc_GNSS_AuxInfoSup_Gps,                      BOOLEAN,       false   #-- @desc  Gnss-AuxiliaryInformationSupport for gps

pc_GNSS_AuxInfoSup_Qzss,                     BOOLEAN,       false   #-- @desc  Gnss-AuxiliaryInformationSupport for qzss

pc_GNSS_AuxInfoSup_Sbas,                     BOOLEAN,       false   #-- @desc  Gnss-AuxiliaryInformationSupport for sbas

pc_GNSS_DGNSS_Sup_BDS,                       BOOLEAN,       false   #-- @desc  Gnss-DifferentialCorrectionsSupport for BDS

pc_GNSS_DGNSS_Sup_Galileo,                   BOOLEAN,       false   #-- @desc  Gnss-DifferentialCorrectionsSupport for galileo

pc_GNSS_DGNSS_Sup_Glonass,                   BOOLEAN,       false   #-- @desc  Gnss-DifferentialCorrectionsSupport for glonass

pc_GNSS_DGNSS_Sup_Gps,                       BOOLEAN,       false   #-- @desc  Gnss-DifferentialCorrectionsSupport for gps

pc_GNSS_DGNSS_Sup_Qzss,                      BOOLEAN,       false   #-- @desc  Gnss-DifferentialCorrectionsSupport for qzss

pc_GNSS_DGNSS_Sup_Sbas,                      BOOLEAN,       false   #-- @desc  Gnss-DifferentialCorrectionsSupport for sbas

pc_GNSS_DataBitsSup_BDS,                     BOOLEAN,       false   #-- @desc  Gnss-DataBitAssistanceSupport for BDS

pc_GNSS_DataBitsSup_Galileo,                 BOOLEAN,       false   #-- @desc  Gnss-DataBitAssistanceSupport for galileo

pc_GNSS_DataBitsSup_Glonass,                 BOOLEAN,       false   #-- @desc  Gnss-DataBitAssistanceSupport for glonass

pc_GNSS_DataBitsSup_Gps,                     BOOLEAN,       false   #-- @desc  Gnss-DataBitAssistanceSupport for gps

pc_GNSS_DataBitsSup_Qzss,                    BOOLEAN,       false   #-- @desc  Gnss-DataBitAssistanceSupport for qzss

pc_GNSS_DataBitsSup_Sbas,                    BOOLEAN,       false   #-- @desc  Gnss-DataBitAssistanceSupport for sbas

pc_GNSS_EOPSup,                              BOOLEAN,       false   #-- @desc  Gnss-EarthOrientationParametersSupport (Common Assistance Data)

pc_GNSS_EllipArc,                            BOOLEAN,       false   #-- @desc  Ellipsoid Arc Support

pc_GNSS_EllipPoint,                          BOOLEAN,       false   #-- @desc  Ellipsoid Point Support

pc_GNSS_EllipPointAlt,                       BOOLEAN,       false   #-- @desc  Ellipsoid Point With Altitude Support

pc_GNSS_EllipPointAltUncertEllip,            BOOLEAN,       false   #-- @desc  Ellipsoid Point With Altitude And Uncertainty Ellipsoid Support

pc_GNSS_EllipPointUncertCircle,              BOOLEAN,       false   #-- @desc  Ellipsoid Point With Uncertainty Circle Support

pc_GNSS_EllipPointUncertEllip,               BOOLEAN,       false   #-- @desc  Ellipsoid Point With Uncertainty Ellipse Support

pc_GNSS_FTA,                                 BOOLEAN,       false   #-- @desc  Support of GNSS Fine Time Assistance

pc_GNSS_FTA_UEA,                             BOOLEAN,       false   #-- @desc  Support of UE Fine Time Assistance measurements for UE-assisted Assisted-GNSS

pc_GNSS_FTA_UEB,                             BOOLEAN,       false   #-- @desc  Support of UE Fine Time Assistance measurements for UE-based Assisted-GNSS

pc_GNSS_HVVel,                               BOOLEAN,       false   #-- @desc  Horizontal With Vertical Velocity Support

pc_GNSS_HVVelUncert,                         BOOLEAN,       false   #-- @desc  Horizontal With Vertical Velocity And Uncertainty Support

pc_GNSS_HVel,                                BOOLEAN,       false   #-- @desc  Horizontal Velocity Support

pc_GNSS_HVelUncert,                          BOOLEAN,       false   #-- @desc  Horizontal Velocity With Uncertainty Support

pc_GNSS_IonoModSup,                          BOOLEAN,       false   #-- @desc  Gnss-IonosphericModelSupport (Common Assistance Data)

pc_GNSS_NavModSup_BDS,                       BOOLEAN,       false   #-- @desc  Gnss-NavigationModelSupport for BDS

pc_GNSS_NavModSup_Galileo,                   BOOLEAN,       false   #-- @desc  Gnss-NavigationModelSupport for galileo

pc_GNSS_NavModSup_Glonass,                   BOOLEAN,       false   #-- @desc  Gnss-NavigationModelSupport for glonass

pc_GNSS_NavModSup_Gps,                       BOOLEAN,       false   #-- @desc  Gnss-NavigationModelSupport for gps

pc_GNSS_NavModSup_Qzss,                      BOOLEAN,       false   #-- @desc  Gnss-NavigationModelSupport for qzss

pc_GNSS_NavModSup_Sbas,                      BOOLEAN,       false   #-- @desc  Gnss-NavigationModelSupport for sbas

pc_GNSS_Polygon,                             BOOLEAN,       false   #-- @desc  Polygon Support

pc_GNSS_RTISup_BDS,                          BOOLEAN,       false   #-- @desc  Gnss-RealTimeIntegritySupport for BDS

pc_GNSS_RTISup_Galileo,                      BOOLEAN,       false   #-- @desc  Gnss-RealTimeIntegritySupport for galileo

pc_GNSS_RTISup_Glonass,                      BOOLEAN,       false   #-- @desc  Gnss-RealTimeIntegritySupport for glonass

pc_GNSS_RTISup_Gps,                          BOOLEAN,       false   #-- @desc  Gnss-RealTimeIntegritySupport for gps

pc_GNSS_RTISup_Qzss,                         BOOLEAN,       false   #-- @desc  Gnss-RealTimeIntegritySupport for qzss

pc_GNSS_RTISup_Sbas,                         BOOLEAN,       false   #-- @desc  Gnss-RealTimeIntegritySupport for sbas

pc_GNSS_RefLocSup,                           BOOLEAN,       false   #-- @desc  Gnss-ReferenceLocationSupport (Common Assistance Data)

pc_GNSS_RefTimeSup,                          BOOLEAN,       false   #-- @desc  Gnss-ReferenceTimeSupport (Common Assistance Data)

pc_GNSS_TimeModSup_BDS,                      BOOLEAN,       false   #-- @desc  Gnss-TimeModelsSupport for BDS

pc_GNSS_TimeModSup_Galileo,                  BOOLEAN,       false   #-- @desc  Gnss-TimeModelsSupport for galileo

pc_GNSS_TimeModSup_Glonass,                  BOOLEAN,       false   #-- @desc  Gnss-TimeModelsSupport for glonass

pc_GNSS_TimeModSup_Gps,                      BOOLEAN,       false   #-- @desc  Gnss-TimeModelsSupport for gps

pc_GNSS_TimeModSup_Qzss,                     BOOLEAN,       false   #-- @desc  Gnss-TimeModelsSupport for qzss

pc_GNSS_TimeModSup_Sbas,                     BOOLEAN,       false   #-- @desc  Gnss-TimeModelsSupport for sbas

pc_GNSS_UTCModSup_BDS,                       BOOLEAN,       false   #-- @desc  Gnss-UTC-ModelSupport for BDS

pc_GNSS_UTCModSup_Galileo,                   BOOLEAN,       false   #-- @desc  Gnss-UTC-ModelSupport for galileo

pc_GNSS_UTCModSup_Glonass,                   BOOLEAN,       false   #-- @desc  Gnss-UTC-ModelSupport for glonass

pc_GNSS_UTCModSup_Gps,                       BOOLEAN,       false   #-- @desc  Gnss-UTC-ModelSupport for gps

pc_GNSS_UTCModSup_Qzss,                      BOOLEAN,       false   #-- @desc  Gnss-UTC-ModelSupport for qzss

pc_GNSS_UTCModSup_Sbas,                      BOOLEAN,       false   #-- @desc  Gnss-UTC-ModelSupport for sbas

pc_GPRS,                                     BOOLEAN,       FALSE   #-- @desc  Support of GPRS

pc_G_operation_mode_C,                       BOOLEAN,       false   #-- @desc  GERAN UE Operation Mode C

pc_HO_from_UTRA,                             BOOLEAN,       false   #-- @desc  Support of Inter-RAT PS handover to E-UTRA from UTRA

pc_HO_from_UTRA_to_eFDD,                     BOOLEAN,       false   #-- @desc  Support of Inter-RAT PS handover to E-UTRA from UTRA (FDD)

pc_HO_from_UTRA_to_eTDD,                     BOOLEAN,       false   #-- @desc  Support of Inter-RAT PS handover to E-UTRA from UTRA (TDD)

pc_HRPD,                                     BOOLEAN,       false   #-- @desc  UE supports CDMA2000 HRPD band class

pc_HSDPA,                                    BOOLEAN,       false   #-- @desc  UE Supports HSDPA

pc_HSDPA_FDD,                                BOOLEAN,       false   #-- @desc  UE Supports HSDPA - FDD

pc_HSDPA_TDD,                                BOOLEAN,       false   #-- @desc  UE Supports HSDPA - TDD

pc_HSDSCH_UE_Category_FDD,                   INTEGER,       5       #-- @desc  FDD HS-DSCH physical layer categories

pc_HSDSCH_UE_Category_TDD,                   INTEGER,       5       #-- @desc  LCR TDD HS-DSCH physical layer categories

pc_HSUPA,                                    BOOLEAN,       false   #-- @desc  UE Supports HSUPA

pc_HSUPA_FDD,                                BOOLEAN,       false   #-- @desc  UE Supports HSUPA - FDD

pc_HSUPA_TDD,                                BOOLEAN,       false   #-- @desc  UE Supports HSUPA - TDD

pc_HttpDigestAuthentication,                 BOOLEAN,       false   #-- @desc  HTTP Digest XCAP Authentication

pc_HttpGAAAuthentication,                    BOOLEAN,       false   #-- @desc  GAA XCAP Authentication

pc_HttpGBAAuthentication,                    BOOLEAN,       false   #-- @desc  GBA XCAP Authentication

pc_IMS,                                      BOOLEAN,       TRUE    #-- @desc  Support of IMS

pc_IMSI_Detach,                              BOOLEAN,       false   #-- @desc  Support of detach for non-EPS services

pc_IMS_APN_default,                          BOOLEAN,       false   #-- @desc  Configured with IMS APN as default APN

pc_IMS_CS_PS_SRVCC,                          BOOLEAN,       false   #-- @desc  UE Supports CS to PS SRVCC

pc_IMS_CS_PS_SRVCCAlert,                     BOOLEAN,       false   #-- @desc  UE Supports CS to PS SRVCC in alerting state

pc_IMS_CS_PS_SRVCCMidCall,                   BOOLEAN,       false   #-- @desc  UE Supports CS to PS SRVCC and the MSC server assisted mid-call feature

pc_IMS_Deregistration,                       BOOLEAN,       false   #-- @desc  UE has the method that supports IMS deregistration

pc_IMS_EmergencyCall,                        BOOLEAN,       TRUE    #-- @desc  UE supports IMS emergency services

pc_IMS_GIBA_Sec,                             BOOLEAN,       false   #-- @desc  UE supports GIBA security only

pc_IMS_GRUUsInSIP,                           BOOLEAN,       false   #-- @desc  UE supports obtaining and using GRUUs in the Session Initiation Protocol (SIP)

pc_IMS_Geolocation,                          BOOLEAN,       false   #-- @desc  UE uses Geolocation header to provide its geographical location for emergency session setup

pc_IMS_RtcpDuringVoiceSession,               BOOLEAN,       TRUE    #-- @desc  RTCP used during voice session

pc_IMS_SRVCCAlert,                           BOOLEAN,       false   #-- @desc  UE indicates g.3gpp.srvcc-alerting media feature tag in INVITE request or 180 response

pc_IMS_Sec,                                  BOOLEAN,       true    #-- @desc  UE supports full IMS security

pc_IMS_SessionIdSupported,                   BOOLEAN,       false   #-- @desc  UE supports session id

pc_IMS_TWS,                                  BOOLEAN,       false   #-- @desc  Three way session

pc_IMS_Video_FeatureTag,                     BOOLEAN,       false   #-- @desc  UE indicates video media feature tag in REGISTER and INVITE request

pc_IMS_emergency_call,                       BOOLEAN,       TRUE    #-- @desc  Support of MS emergency call

pc_IPv4,                                     BOOLEAN,       true    #-- @desc  UE supports IPv4 (used IMS PICS as currently not defined in LTE)

pc_IPv6,                                     BOOLEAN,       TRUE    #-- @desc  UE supports IPv6 (used IMS PICS as currently not defined in LTE)

pc_IR_92,                                    BOOLEAN,       false   #-- @desc  Support of IR.92

pc_ISR,                                      BOOLEAN,       false   #-- @desc  Support of ISR

pc_ImmConnect,                               BOOLEAN,       false   #-- @desc  Immediate connection supported for all circuit switched basic services

pc_IndicateSigcomp,                          BOOLEAN,       false   #-- @desc  Indicate the willingness to receive the responses and requests compressed from initial REGISTER onwards by using the "comp=sigcomp" parameter

pc_InitiateP_CSCFDiscovery_viaDHCPv4,        BOOLEAN,       false   #-- @desc  UE capable of being configured to initiate P-CSCF discovery via DHCPv4

pc_InitiateP_CSCFDiscovery_viaDHCPv6,        BOOLEAN,       false   #-- @desc  UE capable of being configured to initiate P-CSCF discovery via DHCPv6

pc_InitiateP_CSCFDiscovery_viaPCO,           BOOLEAN,       false   #-- @desc  UE capable of being configured to initiate P-CSCF discovery via PCO

pc_InitiateSession,                          BOOLEAN,       false   #-- @desc  Initiating a session

pc_InitiatesDedicatedPDPContext,             BOOLEAN,       false   #-- @desc  UE capable of being configured to initiate Dedicated PDP Context

pc_InterFreq_ProximityIndication,            BOOLEAN,       false   #-- @desc  Support of Inter Frequency Proximity Indication

pc_InterFreq_RSTD_WithGaps,                  BOOLEAN,       false   #-- @desc  Support of inter-frequency RSTD measurements that require measurement gaps

pc_InterFreq_RSTD_withGaps,                  BOOLEAN,       false   #-- @desc  Support of inter-frequency RSTD measurements that require measurement gaps

pc_InterRAT_DL_CompressedModeRequired,       BOOLEAN,       FALSE   #-- @desc  UE supports DL DPCH compressed mode

pc_InterRAT_UL_CompressedModeRequired,       BOOLEAN,       FALSE   #-- @desc  UE supports UL DPCH compressed mode

pc_Interactive,                              BOOLEAN,       false   #-- @desc  UE Supports Interactive QoS class

pc_IntraFreq_ProximityIndication,            BOOLEAN,       false   #-- @desc  Support of Intra Frequency Proximity Indication

pc_KeepEpsBearerParametersAfterNormalDetach, BOOLEAN,       false   #-- @desc  If the UE supports this then the next ATTACH after DETACH shall be done using AT command AT+CGATT=1.

pc_LAP,                                      BOOLEAN,       false   #-- @desc  Support of Low Access Priority Indication

pc_LAP_override,                             BOOLEAN,       false   #-- @desc  Support of Low Access Prioirty Override

pc_LPP,                                      BOOLEAN,       false   #-- @desc  LTE Positioning Protocol (LPP)

pc_LPP_SendingACK_ProvideCapabilities,       BOOLEAN,       false   #-- @desc  Support of sending of acknowledgement request in LPP Provide Capabilities message

pc_LocalTimeZone,                            BOOLEAN,       false   #-- @desc  Support of storage of the local time zone

pc_LoggedMeasurementsIdle,                   BOOLEAN,       false   #-- @desc  Support of logged measurements in RRC_IDLE

pc_MFBI_FrequencyBand1,                      INTEGER,       5       #-- Anritsu TTCN CR required for MFBI

pc_MFBI_FrequencyBand2,                      INTEGER,       18      #-- Anritsu TTCN CR required for MFBI

pc_MFBI_FrequencyBand3,                      INTEGER,       19      #-- Anritsu TTCN CR required for MFBI

pc_MFBI_FrequencyBand4,                      INTEGER,       26      #-- Anritsu TTCN CR required for MFBI

pc_MFBI_FrequencyBand5,                      INTEGER,       27      #-- Anritsu TTCN CR required for MFBI

pc_MFBI_FrequencyBand6,                      INTEGER,       33      #-- Anritsu TTCN CR required for MFBI

pc_MFBI_FrequencyBand7,                      INTEGER,       38      #-- Anritsu TTCN CR required for MFBI

pc_MFBI_FrequencyBand8,                      INTEGER,       41      #-- Anritsu TTCN CR required for MFBI

pc_MGPS,                                     BOOLEAN,       false   #-- @desc  Support for Modernized GPS

pc_MTSI_ACR,                                 BOOLEAN,       false   #-- @desc  MTSI supplementary services - Anonymous Communication Rejection

pc_MTSI_CB,                                  BOOLEAN,       false   #-- @desc  MTSI supplementary services - Communication Barring

pc_MTSI_CommDivert,                          BOOLEAN,       false   #-- @desc  MTSI supplementary services - Communication Diversion

pc_MTSI_CommHold,                            BOOLEAN,       false   #-- @desc  Communication Hold

pc_MTSI_CommWaiting,                         BOOLEAN,       false   #-- @desc  MTSI supplementary services - Communication Waiting

pc_MTSI_Conference,                          BOOLEAN,       false   #-- @desc  MTSI supplementary services - Conference

pc_MTSI_Incoming_CB,                         BOOLEAN,       false   #-- @desc  MTSI supplementary services - Incoming Communication Barring

pc_MTSI_MessageWait,                         BOOLEAN,       false   #-- @desc  MTSI supplementary services - Message Waiting Indication

pc_MTSI_OIP,                                 BOOLEAN,       false   #-- @desc  MTSI supplementary services - Originating Identification Presentation

pc_MTSI_OIR,                                 BOOLEAN,       false   #-- @desc  MTSI supplementary services - Originating Identification Restriction

pc_MTSI_Outgoing_CB,                         BOOLEAN,       false   #-- @desc  MTSI supplementary services - Outgoing Communication Barring

pc_MTSI_Speech,                              BOOLEAN,       false   #-- @desc  MTSI media - Speech

pc_MTSI_Speech_AMRWB,                        BOOLEAN,       false   #-- @desc  MTSI media - Speech AMR wideband

pc_MTSI_Speech_EVS,                          BOOLEAN,       false   #-- @desc  MTSI media - Speech EVS

pc_MTSI_TIP,                                 BOOLEAN,       false   #-- @desc  MTSI supplementary services - Terminating Identification Presentation

pc_MTSI_TIR,                                 BOOLEAN,       false   #-- @desc  MTSI supplementary services - Terminating Identification Restriction

pc_MTSI_Text_RTP,                            BOOLEAN,       false   #-- @desc  MTSI media - Text RTP

pc_MTSI_Video,                               BOOLEAN,       false   #-- @desc   MTSI media - Video

pc_MT_LR,                                    BOOLEAN,       false   #-- @desc  Support of Mobile Terminated location request

pc_MT_LR_loc_notif,                          BOOLEAN,       false   #-- @desc  Support of EPC-MT-LR Location Notification

pc_Manual_CSG_Selection,                     BOOLEAN,       false   #-- @desc  Support of Manual CSG selection

pc_MinimumPeriodicSearchTimer,               BOOLEAN,       false   #-- @desc  Support of Minimum Periodic Search Timer

pc_More_Than_128_CAbandComb,                 BOOLEAN,       false   #-- @desc  Support of more than 128 CA Band Combinations

pc_MultimediaTelephonyService,               BOOLEAN,       false   #-- @desc  Multimedia telephony service participant

pc_Multiple_PDN,                             BOOLEAN,       false   #-- @desc  Support for multiple PDN connections

pc_NMO_I_Behaviour,                          BOOLEAN,       false   #-- @desc  Support of the extended NMO I system information

pc_OMA_LPPe,                                 BOOLEAN,       false   #-- @desc  Support for OMA LPPe

pc_OTDOA,                                    BOOLEAN,       false   #-- @desc  Support of UE assisted OTDOA

pc_PLMN_EF_LRPLMNSI_Automatic_Mode_Exception,BOOLEAN,       false   #-- @desc  Support of Automatic Mode EF_LRPLMSI PLMN Selection Expression

pc_PLMN_Manual_Mode_Exception,               BOOLEAN,       false   #-- @desc  Support of Manual Mode PLMN Selection Expression

pc_PPI_Support,                              BOOLEAN,       false   #-- @desc  Support of Power Preference Indication

pc_PS,                                       BOOLEAN,       FALSE   #-- @desc  Packet Switched

pc_PS_data_centric,                          BOOLEAN,       false   #-- @desc  Support of configuring the UE to PS data centric

pc_PS_voice_centric,                         BOOLEAN,       false   #-- @desc  Support of configuring the UE to PS voice centric

pc_PWS_UpperLayer,                           BOOLEAN,       false   #-- @desc  Presence of PWS upper layer for functions like duplicate definition

pc_P_CSCFDiscovery_viaDHCP,                  BOOLEAN,       FALSE   #-- @desc  UE supports P-CSCF Discovery via DHCP

pc_P_CSCFDiscovery_viaDHCPv4,                BOOLEAN,       false   #-- @desc  UE supports P-CSCF discovery via DHCPv4

pc_P_CSCFDiscovery_viaDHCPv6,                BOOLEAN,       false   #-- @desc  UE supports P-CSCF discovery via DHCPv6

pc_P_CSCFDiscovery_viaPCO,                   BOOLEAN,       FALSE   #-- @desc  UE supports P-CSCF Discovery via PCO

pc_ParamGpsAssisData,                        BOOLEAN,       false   #-- @desc  Support of MO-LR request for assistance data

pc_ParamPosEstimate,                         BOOLEAN,       false   #-- @desc  Support of MO-LR request for a position estimate

pc_Preconditions,                            BOOLEAN,       false   #-- @desc  Integration of resource management and SIP? (use of preconditions)

pc_Provide_IMS_APN,                          BOOLEAN,       false   #-- @desc  Configured to provide IMS APN during initial attach

pc_Provide_IMS_as_second_APN,                BOOLEAN,       false   #-- @desc  Configured to provide IMS APN as the 2nd PDN connection

pc_Provide_Internet_as_second_APN,           BOOLEAN,       false   #-- @desc  Configured to provide Internet APN as the 2nd PDN connection

pc_QZSS_ADR,                                 BOOLEAN,       false   #-- @desc  Support of ADR measurement reporting for Qzss

pc_QZSS_QZS_L1,                              BOOLEAN,       false   #-- @desc  Support of QZS-L1 signal in QZSS

pc_QZSS_QZS_L1C,                             BOOLEAN,       false   #-- @desc  Support of QZS-L1C signal in QZSS

pc_QZSS_QZS_L2C,                             BOOLEAN,       false   #-- @desc  Support of QZS-L2C signal in QZSS

pc_QZSS_QZS_L5,                              BOOLEAN,       false   #-- @desc  Support of QZS-L5 signal in QZSS

pc_QZSS_VelocityMeas,                        BOOLEAN,       false   #-- @desc  Support of Velocity measurement reporting for Qzss

pc_RLF_ReportForInterRAT_MRO,                BOOLEAN,       false   #-- @desc  Support of Radio Link Failure Report for InterRAT MRO

pc_ROHC_profile0x0001,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0001

pc_ROHC_profile0x0002,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0002

pc_ROHC_profile0x0003,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0003

pc_ROHC_profile0x0004,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0004

pc_ROHC_profile0x0006,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0006

pc_ROHC_profile0x0101,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0101

pc_ROHC_profile0x0102,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0102

pc_ROHC_profile0x0103,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0103

pc_ROHC_profile0x0104,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0104

pc_Rach_Report,                              BOOLEAN,       false   #-- @desc  Support of delivery of rachReport upon request from the network

pc_Re_Attach_AfterDetachColl,                BOOLEAN,       false   #-- @desc  Support of automatic re-activation of the EPS bearers during network initiated detach even though UE has initiated a detach procedure with detach type set to EPS detach or combined EPSIMSI detach

pc_RequestIPv4HAAddress_DuringAttach,        BOOLEAN,       false   #-- @desc  Support for being configured to request the IPv4 address of the Home Agent during Attach procedure

pc_RequestIPv6HAAddress_DuringAttach,        BOOLEAN,       false   #-- @desc  Support for being configured to request the IPv6 address of the Home Agent during Attach procedure

pc_SBAS_ADR,                                 BOOLEAN,       false   #-- @desc  Support of ADR measurement reporting for Sbas

pc_SBAS_VelocityMeas,                        BOOLEAN,       false   #-- @desc  Support of Velocity measurement reporting for Sbas

pc_SI_Neighbour_UMTS_Autonomous_Gaps,        BOOLEAN,       false   #-- @desc  Upon configuration of si-RequestForHO by the network supports acquistion of relevant information from a neighbouring UMTS cell by reading the SI of the neighbouring cell using autonomous gaps and reporting

pc_SI_Neighbour_interFreq_Autonomous_Gaps,   BOOLEAN,       false   #-- Anritsu TTCN CR R5s150219 MCC

pc_SI_Neighbour_intraFreq_Autonomous_Gaps,   BOOLEAN,       false   #-- Anritsu TTCN CR R5s150219 MCC

pc_SMS_MO,                                   BOOLEAN,       FALSE   #-- @desc  UE supports SM-over-IP sender

pc_SMS_MT,                                   BOOLEAN,       FALSE   #-- @desc  UE supports SM-over-IP receiver

pc_SMS_SGs,                                  BOOLEAN,       false   #-- @desc  The UE supports SMS over SGs and is configured for SMS over SGs.  If true at least one of pc_SMS_SGs_MT and pc_SMS_SGs_MO is true. If it is set to true pc_combined_attach shall be set to true

pc_SMS_SGs_MO,                               BOOLEAN,       false   #-- @desc  Support of Short Message Service (SMS) MO over SGs

pc_SMS_SGs_MT,                               BOOLEAN,       false   #-- @desc  Support of Short Message Service (SMS) MT over SGs

pc_SMS_SGs_Multi_MO,                         BOOLEAN,       false   #-- @desc  Support of sending concatenated multiple short message over SGs

pc_SRVCC_GERAN_UTRAN,                        BOOLEAN,       false   #-- @desc  Support for SRVCC from E-UTRAN to GERANUTRAN

pc_Semi_Persistence_Scheduling,              BOOLEAN,       false   #-- @desc  Support of semi persistance scheduling

pc_SendRTCPOnlyOnHold,                       BOOLEAN,       true    #-- @desc  UE supports sending RTCP only while call is put on hold

pc_ShortNameNetwork,                         BOOLEAN,       false   #-- @desc  Support of storage of the network short name

pc_Speech,                                   BOOLEAN,       false   #-- @desc  UE supports Speech

pc_Squal_based_CellReselection_between_E_UTRAN_and_GERAN,BOOLEAN,       false   #-- @desc  Support of Squal based cell reselection to E-UTRAN from GERAN

pc_Squal_based_CellReselection_to_E_UTRAN_from_UTRAN,BOOLEAN,       false   #-- @desc  Support of Squal based cell reselection to E-UTRAN from UTRAN

pc_Squal_based_CellReselection_to_UTRAN_from_E_UTRAN,BOOLEAN,       false   #-- @desc  Support of Squal based cell reselection to UTRAN from E-UTRAN

pc_StandaloneGNSS_Location,                  BOOLEAN,       false   #-- @desc  Support of standalone GNSS receiver to provide detailed location information in RRC measurement report and logged measurements in RRC_IDLE

pc_Streaming,                                BOOLEAN,       false   #-- @desc  UE Supports Streaming QoS class

pc_SubscribeConferenceEvent_OutsideINVITEDialog,BOOLEAN,       false   #-- @desc  UE supports subscription to conference event package outside INVITE dialog

pc_Subscribed,                               BOOLEAN,       false   #-- Anritsu Prose CR R5-121434

pc_SupportOpModeA,                           BOOLEAN,       false   #-- @desc  UE supports Operation Mode A

pc_SwitchOnOff,                              BOOLEAN,       true    #-- @desc  switch onoff supported

pc_T3412Extended,                            BOOLEAN,       false   #-- @desc  Support of T3412 extended value IE

pc_TAU_connected,                            BOOLEAN,       false   #-- @desc  Support of TAU in connected mode. Applicable when configured to pc_voice_PS_1_CS_2 and pc_Attach

pc_TAU_connected_in_IMS,                     BOOLEAN,       false   #-- @desc  Support of TAU in connected mode. Applicable when configured to pc_voice_PS_1_CS_2 and pc_Attach

pc_TAU_idle,                                 BOOLEAN,       false   #-- @desc  Support of TAU in idle mode. Applicable when configured to pc_voice_PS_1_CS_2 and pc_Attach

pc_TAU_idle_in_IMS,                          BOOLEAN,       false   #-- @desc  Support of TAU in idle mode. Applicable when configured to pc_voice_PS_1_CS_2 and pc_Attach

pc_TDD_HCR,                                  BOOLEAN,       false   #-- @desc  UE supports UTRA band as defined in TS 25.102

pc_TDD_LCR,                                  BOOLEAN,       false   #-- @desc  UE supports UTRA band as defined in TS 25.102

pc_TDD_SpecialSubframe,                      BOOLEAN,       false   #-- @desc  Support of TDD special subframe

pc_TDD_VHCR,                                 BOOLEAN,       false   #-- @desc  UE supports UTRA band as defined in TS 25.102

pc_TMPI_forGBA,                              BOOLEAN,       false   #-- @desc  UE uses TMPI in HTTP request for GBA

pc_TTI_Bundling,                             BOOLEAN,       false   #-- @desc  Support of TTI Bundling

pc_TestModeforCSGproximity,                  BOOLEAN,       false   #-- @desc  Support of UE radio bearer test mode for CSG proximity testing

pc_UEA_AGNSS,                                BOOLEAN,       false   #-- @desc  Support of UE assisted Assisted-GNSS

pc_UEA_A_GANSS,                              BOOLEAN,       false   #-- @desc  Support of UE-Assisted A-GANSS

pc_UEB_AGNSS,                                BOOLEAN,       false   #-- @desc  Support of UE based Assisted-GNSS

pc_UEB_A_GANSS,                              BOOLEAN,       false   #-- @desc  Support of UE-Based A-GANSS

pc_UE_supports_user_initiated_PDN_disconnect,BOOLEAN,       false   #-- @desc  UE supports user initiated PDN disconnect

pc_UL_64QAM,                                 BOOLEAN,       false   #-- @desc  Support of uplink 64 QAM

pc_UL_CA,                                    BOOLEAN,       false   #-- @desc  Support of UL CA

pc_UL_CA_2Carriers,                          BOOLEAN,       false   #-- @desc  UL CA with 2 carriers

pc_UL_CA_3Carriers,                          BOOLEAN,       false   #-- @desc  UL CA with 3 carriers

pc_UL_CoMP,                                  BOOLEAN,       false   #-- @desc  Support of UL co-ordinated multi-point operation

pc_UL_CoordinatedMultiPointOperation,        BOOLEAN,       false   #-- @desc  Support of UL co-ordinated multi-point operation

pc_UL_IntraBand_ContCaBWclassB,              BOOLEAN,       false   #-- @desc  UL Intra-band contiguous CA BW class B

pc_UL_IntraBand_ContCaBWclassC,              BOOLEAN,       false   #-- @desc  UL Intra-band contiguous CA BW class C

pc_UL_MIMO,                                  BOOLEAN,       false   #-- @desc  Support of UL MIMO

pc_UL_SupportedInAllBandsInCAComb,           BOOLEAN,       false   #-- @desc  UL (Pcell) supported in each band of Inter-band CA combination under test

pc_UL_interBand_CaBwClassComb_AA,            BOOLEAN,       false   #-- @desc  UL Inter-band contiguous CA BW class A-A

pc_UL_intraBand_nonContCaBwClassComb_AA,     BOOLEAN,       false   #-- @desc  Support of UL intra-band non-contiguous CA BW Class Combination A-A

pc_UMI_ProcNeeded_DuringCSFB,                BOOLEAN,       false   #-- @desc  Requiring UMI proceeding to paging response

pc_UMI_ProcNeeded_DuringSRVCC,               BOOLEAN,       false   #-- @desc  Requiring UMI proceeding to paging response

pc_USIM_Removal,                             BOOLEAN,       false   #-- @desc  USIM removable without power down supported

pc_UTRA,                                     BOOLEAN,       TRUE    #-- @desc  UE supports UTRA

pc_UTRAN_ANR,                                BOOLEAN,       false   #-- @desc  Support of UTRAN ANR

pc_UTRAN_ProximityIndication,                BOOLEAN,       false   #-- @desc  Support of UTRAN Proximity Indication

pc_UTRA_CompressedModeRequired,              BOOLEAN,       false   #-- @desc  Support of Compressed Mode

pc_UTRA_FeatrGrp_1,                          BOOLEAN,       false   #-- @desc  Support of UTRA CELL_PCH and URA_PCH to RRC_IDLE cell reselection

pc_UTRA_FeatrGrp_2,                          BOOLEAN,       false   #-- @desc  Support of EUTRAN measurements and reporting in connected mode

pc_UeAssistedAgps,                           BOOLEAN,       false   #-- @desc  Support of UE assisted Network Assisted GPS L1 CA

pc_UeBasedAgps,                              BOOLEAN,       false   #-- @desc  Support of UE based Network Assisted GPS L1 CA

pc_UniversalAndLocalTimeZone,                BOOLEAN,       false   #-- @desc  Support of storage of the universal time and local time zone

pc_UpdateUE_LocationInformation,             BOOLEAN,       false   #-- @desc  Update UE Location Information

pc_UserInitiatedPLMN_Reselection,            BOOLEAN,       false   #-- @desc  Support user initiated PLMN reselection in automatic mode

pc_VideoCodecH264CBP,                        BOOLEAN,       false   #-- @desc  MTSI media - Video codec H.264 CBP Level 1.2

pc_VoLTE,                                    BOOLEAN,       TRUE    #-- @desc  Support of VoLTE in GSMA PRD IR.92: "IMS profile for Voice and SMS"

pc_XCAP_UsernameIsConfiguredInUE,            BOOLEAN,       false   #-- @desc  UE indicated OMA-TS-XDM_MO-V1_1-20080627-A.doc section 5.2.8 "Node: <X>AAUTHNAME" is configured

pc_XCAP_XUIisDefaultPublicUserId,            BOOLEAN,       false   #-- @desc  UE uses the default public user id received in P-Associated-URI header in 200 OK for REGISTER as XCAP User Identity (XUI)

pc_XCAP_only_APN,                            BOOLEAN,       false   #-- @desc  Configured with an APN for XCAP only usage

pc_XCAP_over_Internet_APN,                   BOOLEAN,       false   #-- @desc  Configured to use Internet APN for XCAP signalling

pc_ZUC,                                      BOOLEAN,       false   #-- @desc  Support of ZUC algorithm

pc_data_centric,                             BOOLEAN,       false   #-- @desc  Support of CSPS mode 2

pc_eAttachWithIMSI,                          BOOLEAN,       false   #-- @desc  Support of Attach With IMSI

pc_eBand10_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 10

pc_eBand11_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 11

pc_eBand12_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 12

pc_eBand13_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 13

pc_eBand14_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 14

pc_eBand17_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 17

pc_eBand18_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 18

pc_eBand19_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 19

pc_eBand1_Supp,                              BOOLEAN,       TRUE    #-- @desc  Support of Band 1

pc_eBand20_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 20

pc_eBand21_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 21

pc_eBand22_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 22

pc_eBand23_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 23

pc_eBand24_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 24

pc_eBand25_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 25

pc_eBand26_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 26

pc_eBand27_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 27

pc_eBand28_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 28

pc_eBand29_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 29

pc_eBand2_Supp,                              BOOLEAN,       false   #-- @desc  Support of Band 2

pc_eBand30_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 30

pc_eBand31_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 31

pc_eBand32_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 32

pc_eBand33_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 33

pc_eBand34_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 34

pc_eBand35_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 35

pc_eBand36_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 36

pc_eBand37_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 37

pc_eBand38_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 38

pc_eBand39_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 39

pc_eBand3_Supp,                              BOOLEAN,       false   #-- @desc  Support of Band 3

pc_eBand40_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 40

pc_eBand41_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 41

pc_eBand42_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 42

pc_eBand43_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 43

pc_eBand44_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 44

pc_eBand4_Supp,                              BOOLEAN,       false   #-- @desc  Support of Band 4

pc_eBand5_Supp,                              BOOLEAN,       false   #-- @desc  Support of Band 5

pc_eBand6_Supp,                              BOOLEAN,       false   #-- @desc  Support of Band 6

pc_eBand7_Supp,                              BOOLEAN,       false   #-- @desc  Support of Band 7

pc_eBand8_Supp,                              BOOLEAN,       false   #-- @desc  Support of Band 8

pc_eBand9_Supp,                              BOOLEAN,       false   #-- @desc  Support of Band 9

pc_eFDD,                                     BOOLEAN,       TRUE    #-- @desc  UE supports EUTRA FDD

pc_eFDD_MultiBand,                           BOOLEAN,       false   #-- @desc  Support of multiple E-UTRA FDD bands

pc_eHARQ_Pattern_for_TTI_bundling,           BOOLEAN,       false   #-- @desc  Support of enhanced HARQ pattern for TTI bundling operation for FDD

pc_eLAP,                                     BOOLEAN,       false   #-- @desc  Support of Low Access Priority Indication

pc_eMBMS,                                    BOOLEAN,       false   #-- @desc  Support of eMBMS

pc_eMBMS_SC,                                 BOOLEAN,       false   #-- @desc  Support of eMBMS service continuity

pc_eMinimumPeriodicSearchTimer,              BOOLEAN,       false   #-- @desc  Support of Minimum Periodic Search Timer

pc_ePDCCH,                                   BOOLEAN,       false   #-- @desc  Support of ePDCCH

pc_ePSM,                                     BOOLEAN,       false   #-- @desc  Support of Power Saving Mode (in EUTRA)

pc_eRedirectionUTRA,                         BOOLEAN,       false   #-- @desc  Support of use of the UTRA system information provided by RRCConnectionRelease upon redirection

pc_eTDD,                                     BOOLEAN,       false   #-- @desc  UE supports EUTRA TDD

pc_eTDD_MultiBand,                           BOOLEAN,       false   #-- @desc  Support of multiple E-UTRA TDD bands

pc_multipleTimingAdvance,                    BOOLEAN,       false   #-- @desc  Support of multiple timing advances

pc_not_SMS_only,                             BOOLEAN,       false   #-- @desc  Supports not sending SMS only in the Additional update type IE

pc_reqFreqBands,                             BOOLEAN,       false   #-- @desc  Support of reception of requested Frequency Bands

pc_tdd_FDD_CA_FDD_PCell,                     BOOLEAN,       false   #-- @desc  Support of tdd-FDD-CA-PCellDuplex-r12 with the second bit setting to 1

pc_tdd_FDD_CA_TDD_PCell,                     BOOLEAN,       false   #-- @desc  Support of tdd-FDD-CA-PCellDuplex-r12 with the first bit setting to 1

pc_ue_CategoryDL_0,                          BOOLEAN,       false   #-- @desc  UE Category DL 0

pc_ue_CategoryDL_10,                         BOOLEAN,       false   #-- @desc  UE Category DL 10

pc_ue_CategoryDL_11,                         BOOLEAN,       false   #-- @desc  UE Category DL 11

pc_ue_CategoryDL_12,                         BOOLEAN,       false   #-- @desc  UE Category DL 12

pc_ue_CategoryDL_13,                         BOOLEAN,       false   #-- @desc  UE Category DL 13

pc_ue_CategoryDL_14,                         BOOLEAN,       false   #-- @desc  UE Category DL 14

pc_ue_CategoryDL_15,                         BOOLEAN,       false   #-- @desc  UE Category DL 15

pc_ue_CategoryDL_16,                         BOOLEAN,       false   #-- @desc  UE Category DL 16

pc_ue_CategoryDL_6,                          BOOLEAN,       false   #-- @desc  UE Category DL 6

pc_ue_CategoryDL_7,                          BOOLEAN,       false   #-- @desc  UE Category DL 7

pc_ue_CategoryDL_9,                          BOOLEAN,       false   #-- @desc  UE Category DL 9

pc_ue_CategoryUL_0,                          BOOLEAN,       false   #-- @desc  UE Category UL 0

pc_ue_CategoryUL_13,                         BOOLEAN,       false   #-- @desc  UE Category UL 13

pc_ue_CategoryUL_3,                          BOOLEAN,       false   #-- @desc  UE Category UL 3

pc_ue_CategoryUL_5,                          BOOLEAN,       false   #-- @desc  UE Category UL 5

pc_ue_CategoryUL_7,                          BOOLEAN,       false   #-- @desc  UE Category UL 7

pc_ue_CategoryUL_8,                          BOOLEAN,       false   #-- @desc  UE Category UL 8

pc_ue_Category_1,                            BOOLEAN,       false   #-- @desc  UE Category 1

pc_ue_Category_10,                           BOOLEAN,       false   #-- @desc  UE Category 10

pc_ue_Category_11,                           BOOLEAN,       false   #-- @desc  UE Category 11

pc_ue_Category_12,                           BOOLEAN,       false   #-- @desc  UE Category 12

pc_ue_Category_2,                            BOOLEAN,       false   #-- @desc  UE Category 2

pc_ue_Category_3,                            BOOLEAN,       false   #-- @desc  UE Category 3

pc_ue_Category_4,                            BOOLEAN,       false   #-- @desc  UE Category 4

pc_ue_Category_5,                            BOOLEAN,       false   #-- @desc  UE Category 5

pc_ue_Category_6,                            BOOLEAN,       false   #-- @desc  UE Category 6

pc_ue_Category_7,                            BOOLEAN,       false   #-- @desc  UE Category 7

pc_ue_Category_8,                            BOOLEAN,       false   #-- @desc  UE Category 8

pc_ue_Category_9,                            BOOLEAN,       false   #-- @desc  UE Category 9

pc_voice_PS_1_CS_2,                          BOOLEAN,       false   #-- @desc  Configured voice domain preference

pc_voice_centric,                            BOOLEAN,       false   #-- @desc  Support of configuring the UE to voice centric

px_1XRTT_BandClass,                          INTEGER,       1       #-- @desc  Band Class; Table 1.5-1 of C.S0057_D. Default value corresponds to 1.8 to 2.0 GHz PCS band

px_1XRTT_BaseId_Cell19,                      BITSTRING,     0000000000100111 #-- @desc  Base Id of Cell 19

px_1XRTT_BaseId_Cell20,                      BITSTRING,     0000000000101000 #-- @desc  Base Id of Cell 20

px_1XRTT_BaseId_Cell21,                      BITSTRING,     0000000000101001 #-- @desc  Base Id of Cell 21

px_1XRTT_BaseId_Cell22,                      BITSTRING,     0000000000101010 #-- @desc  Base Id of Cell 22

px_1XRTT_CS_PagingMessage_Cell19,            OCTETSTRING,   123456  #-- @desc  Encoded PDU of CS paging message  to be sent in DLInformationTransfer; The message is encapsulated in a GCSNA1xCircuitService defined in C.S0097 clause 2.4.1

px_1XRTT_HandoffDirectionCell19,             OCTETSTRING,   123456  #-- @desc  Encoded PDU of Handoff Direction Assignment to be sent in MobilityFromEUTRACommand

px_1XRTT_MinProtRev,                         INTEGER,       0       #-- @desc  Minimum protocol revision support by Base Station

px_1XRTT_MobilityParametersCell19,           OCTETSTRING,   123456  #-- @desc  Encoded PDU of mobility parameters to be sent in HandoverfromEUTRAPreparationRequest

px_1XRTT_MobilityParametersCell21,           OCTETSTRING,   123456  #-- @desc  Encoded PDU of mobility parameters to be sent in HandoverfromEUTRAPreparationRequest

px_1XRTT_NID,                                BITSTRING,     0000000001100100 #-- @desc  default Network ID of 1xRTT Cells

px_1XRTT_SID,                                BITSTRING,     000000011001000 #-- @desc  default System ID of 1xRTT Cells

px_1XRTT_Sig_EncMode,                        INTEGER,       2       #-- @desc  Rijndael algorithm

px_1XRTT_TMSI_Def,                           OCTETSTRING,   1234ABCD #-- @desc  TMSI to be used in 1xRTT

px_1XRTT_UserInfo_EncMode,                   INTEGER,       2       #-- @desc  Rijndael algorithm

px_1XRTT_Zone_Timer,                         BITSTRING,     000     #-- @desc  Zone timer sent in 'System Parameters Message' overhead message

px_AccessPointName,                          OCTETSTRING,   03696D73 #-- @desc  Access Point Name

px_AttachTypeTested,                         ENUM-EUTRA_ATTACH_TESTED_Type,COMBINED_ATTACH #-- @desc  Attach Type to be tested if UE supports both pc_Attach and pc_Combined_Attach

px_AuthAMF,                                  BITSTRING,     1001000100010001 #-- @desc  Authentication Management Field (16 bits). The value shall be different from '1111 1111 1111 111'B (AMFresynch).

px_AuthK,                                    BITSTRING,     00000000000000010000001000000011000001000000010100000110000001110000100000001001000010100000101100001100000011010000111000001111 #-- @desc  Authentication Key

px_AuthN,                                    INTEGER,       127     #-- @desc  value of n to initialize tcv_AuthN (length of extended response)

px_BI_deviation,                             BOOLEAN,       false   #-- 

px_BI_deviation_dummy,                       INTEGER,       1       #-- 

px_BcapDataCompression,                      BITSTRING,     0       #-- @desc  Data compression supported (used in the Bearer Capability).Default value: Default IMSI

px_BcapFNUR,                                 BITSTRING,     00001   #-- @desc  Fixed Network User rate supported: '00001'B: FNUR 9.6 kbits '00010'B: FNUR 14.4 kbits '00011'B: FNUR 19.2 kbits '00100'B: FNUR 28.8 kbits '00101'B: FNUR 38.4 kbits '00110'B: FNUR 48.0 kbits '00111'B: FNUR 56.0 kbits '01000'B: FNUR 64.0 kbits '01001'B: FNUR 33.6 kbits '01010'B: FNUR 32.0 kbits.

px_CipherAlg,                                BITSTRING,     010     #-- Anritsu ttCN CR required px_CipherAlg type @desc  NAS Ciphering Algorithm Default value: (GEA2)

px_CipherKey,                                BITSTRING,     0101111001001010101100110101100010010001001101110101110100101010 #-- @desc   Cipher Key

px_CipherKey128,                             BITSTRING,     01011110010010101011001101011000100100010011011101011101001010100101111001001010101100110101100010010001001101110101110100101010 #-- @desc  Cipher key (128 bits) to be used e.g. for A54 and GEA4

px_ColorCode,                                INTEGER,       64      #-- @desc  Color code of the subnet to which the sectors belong; Same for all HRPD cells

px_ColorCodeDiff,                            INTEGER,       128     #-- @desc  Color code of the subnet to which the sectors belong; A different colour code than default

px_DHCPServer_IPAddr,                        CHARSTRING,    10.122.11.24 #-- @desc  DHCP Server address

px_DNSServer_IPAddr,                         CHARSTRING,    10.122.11.23 #-- @desc  DNS Server address

px_DelayBeforeIntraCellHO,                   INTEGER,       300     #-- @desc  Temporary PIXIT used to define the delay before an intra cell handover

px_EDCH_UE_Category_FDD,                     INTEGER,       1       #-- @desc  Reference to other Spec: 34.123-2 Table A.18a.2

px_EDCH_UE_Category_TDD,                     INTEGER,       1       #-- @desc  Reference to other Spec: 34.123-2 Table A.18b.2

px_ETWS_CB_DataPage1,                        CHARSTRING,    warning #-- @desc  ETWS Page 1 warning data message

px_ETWS_CB_DataPage2,                        CHARSTRING,    warning #-- @desc  ETWS Page 2 warning data message

px_ETWS_DigitalSignature,                    OCTETSTRING,   00000000000000000000000000000000000000000000000000000000000000000000000000000000000000 #-- @desc  ETWS Digital Signature

px_EUTRA_CA_BandCombination,                 ENUM-CA_BandCombination_Type,CA_1C   #-- @desc  CA band combination applied in CA test cases

px_EllipsoidPointWithAltitude,               OCTETSTRING,   1234560000000000 #-- @desc  Ellipsoid Point With Altitude value to be provided in Update UE location information (see 36.509 cl 6.12)

px_EmergencyCallNumber,                      CHARSTRING,    112     #-- @desc  Emergency Number used by UE to initiate an emergency call

px_FDD_OperationBand,                        INTEGER,       1       #-- @desc  The operation band under test as defined in 34.108 clause 5.1.1. Value 1 means Band 1 2 means Band 2 etc.This pixit shall be set in synchronisation with the values that are being set to 6 other Pixits viz: px_UARFCN_D_High px_UARFCN_D_Midpx_UARFCN_L_Mid

px_FRESH,                                    BITSTRING,     00001111000011110000111100001111 #-- @desc  no default value can be proposed

px_GERAN_BandUnderTest,                      ENUM-GERAN_BandUnderTestType,GSM_P900 #-- @desc  Indicates which band is under test.  The type is different to the parameter defined in 34.123-3

px_GPRS_CipheringAlgorithm,                  ENUM-GPRS_CipheringAlgorithm_Type,gea2    #-- @desc  NAS Ciphering Algorithm Default value: (GEA2)

px_GSM_CipherAlg,                            BITSTRING,     000     #-- @desc  GSM Cipher algorithm.

px_GSM_CipheringOnOff,                       BITSTRING,     1       #-- @desc  GSM Ciphering to be started or not

px_GeoInfo,                                  OCTETSTRING,   9032B9D66360B600323C3C006544 #-- @desc  Geographical information to be sent as Location Estimate in FACILITY message from the System Simulator.

px_HRPD_BandClass,                           INTEGER,       1       #-- @desc  Band Class; Table 1.5-1 of C.S0057_D. Default value corresponds to 1.8 to 2.0 GHz PCS band

px_HRPD_OpenLoopParametersCell15,            OCTETSTRING,   123456  #-- @desc  The HRPD Open Loop parameters for cell 15 message to be sent; it also includes the Tunneled Header as per C.S0087 clause 5.1.6.3 (default value needs updating FFS)

px_HRPD_SectorID_Cell15,                     BITSTRING,     11111110101000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000001 #-- @desc  Sector ID of Cell 15; Clause 13.9 of C.S0024_B

px_HRPD_SectorID_Cell16,                     BITSTRING,     11111110101000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000010 #-- @desc  Sector ID of Cell 16; Clause 13.9 of C.S0024_B

px_HRPD_SectorID_Cell17,                     BITSTRING,     11111110101000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000011 #-- @desc  Sector ID of Cell 17; Clause 13.9 of C.S0024_B

px_HRPD_SectorID_Cell18,                     BITSTRING,     11111110101000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000100 #-- @desc  Sector ID of Cell 18; Clause 13.9 of C.S0024_B

px_HRPD_SilenceParametersCell15,             OCTETSTRING,   123456  #-- @desc  The HRPD Silence parameters for cell 15 message to be sent; it also includes the Tunneled Header as per C.S0087 clause 5.1.6.3 (default value needs updating FFS)

px_HRPD_TrafficChannelAssignmentCell15,      OCTETSTRING,   123456  #-- 

px_HSDSCH_UE_Category_FDD,                   INTEGER,       5       #-- @desc  Reference to other Spec: 34.123-2 Table A.18a.1

px_HSDSCH_UE_Category_TDD,                   INTEGER,       5       #-- @desc  Reference to other Spec: 34.123-2 Table A.18b.1

px_HorizontalVelocity,                       OCTETSTRING,   123456  #-- @desc  Horizontal Velocity to be provided in Update UE location information (see 36.509 cl 6.12)

px_IMEISV_Def,                               HEXSTRING,     123456789012345 #-- @desc  Default IMEISV value.  No default can be proposed as this is a manufacturer defined value

px_IMEI_Def,                                 HEXSTRING,     351602003395910 #-- @desc  Default IMEI value.  No default can be proposed as this is a manufacturer defined value

px_IMSI_Def,                                 HEXSTRING,     001010000000333 #-- @desc  Default IMSI

px_IMS_AssociatedTelUri,                     CHARSTRING,    tel:+4989364072 #-- @desc  Set as record 3 in EFIMPU as defined in TS 34.229-1[5]

px_IMS_CalleeContactUri,                     CHARSTRING,    sip:User-B-Contact@3gpp.org #-- @desc  URI provided by the remote side (i.e. by SS) to be used by the UE as contact address in further SIP signalling of the dialog

px_IMS_CalleeContactUri2,                    CHARSTRING,    sip:User-C-Contact@3gpp.org #-- @desc  URI provided by the remote side (i.e. by SS) to be used by the UE as contact address in further SIP signalling of the dialog

px_IMS_CalleeUri,                            CHARSTRING,    sip:1234@ims.mnc001.mcc001.3gppnetwork.org #-- @desc  URI of Callee sent by the UE in INVITE (MO call establishment) to address the remote UE

px_IMS_CalleeUri2,                           CHARSTRING,    sip:User-C@3gpp.org #-- @desc  URI of Callee sent by the UE in INVITE (MO call establishment) to address the remote UE

px_IMS_CiphAlgo_Def,                         ENUM-IPsec_CipheringAlgorithm_Type,nociph  #-- @desc  Ciphering Algorithm

px_IMS_ConferenceFactoryUri,                 CHARSTRING,    sip:mmtel@conf-factory.3gpp.org #-- @desc  conference factory URI as used by the UE for IMS conferencing

px_IMS_FinalConferenceUri,                   CHARSTRING,    sip:final@conf-factory.3gpp.org #-- @desc  final conference URI as sent to the UE during MTSI conference creation

px_IMS_HomeDomainName,                       CHARSTRING,    test.3gpp.com #-- @desc  Home Domain Name.

px_IMS_HomeDomainName_Refreshed,             CHARSTRING,    refreshed3gpp.org #-- @desc  Used in 8.15

px_IMS_IPSecAlgorithm,                       ENUM-IPsec_IntegrityAlgorithm_Type,hmac_md5_96 #-- @desc  Integrity Algorithm

px_IMS_MessageAccountIdentity,               CHARSTRING,    testaccountidentity #-- @desc  message accout identity configured at the UE as used for subscription to message-summary event package

px_IMS_Pcscf,                                CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:3333 #-- @desc  P-CSCF fully qualified domain name that resolves to the IP address of SS

px_IMS_Pcscf_Emg,                            CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:4444 #-- @desc  P-CSCF fully qualified domain name that resolves to the IP address of SS for emergency calls

px_IMS_Private_UserId,                       CHARSTRING,    001010123456789@test.3gpp.com #-- @desc  Private User Identity.When usingan ISIM this is set to the same value as EFIMPI.When ISIM is not used just USIM the private user identity is derived from px_IMSI.

px_IMS_Private_UserId_Refreshed,             CHARSTRING,    privateuser@refreshed3gpp.org #-- @desc  Used in 8.15

px_IMS_PublicUserIdentity1,                  CHARSTRING,    sip:001010123456789@ims.mnc001.mcc001.3gppnetwork.org #-- @desc  Public User Identity. It is set to the same value as the first record in EFIMPU.

px_IMS_PublicUserIdentity1_Refreshed,        CHARSTRING,    sip:PublicId1@refreshed3gpp.org #-- @desc  Used in 8.15

px_IMS_PublicUserIdentity2,                  CHARSTRING,    sip:+11234567890@test.3gpp.com #-- @desc  Public User Identity. It is set to the same value as the second record in EFIMPU.

px_IMS_PublicUserIdentity3,                  CHARSTRING,    sip:user@test.3gpp.com #-- @desc  Public User Identity. It is set to the same value as the third record in EFIMPU.

px_IMS_Scscf,                                CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:3333 #-- @desc  S-CSCF fully qualified domain name that resolves to the IP address of SS

px_IMS_TemporaryConferenceUri,               CHARSTRING,    sip:temporary@conf-factory.3gpp.org #-- @desc  temporary conference URI as sent to the UE during MTSI conference creation

px_IMS_ePcscf,                               CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:4444 #-- @desc  P-CSCF fully qualified domain name that resolves to the IP address of SS for emergency calls

px_IP_MTU_Size,                              INTEGER,       1300    #-- @desc  MTU size

px_IPv4_Address,                             CHARSTRING,    192.168.0.1 #-- @desc  IPv4 Address

px_IPv4_Address1_NW,                         CHARSTRING,    192.168.0.3 #-- @desc  IPv4 Gateway Address in PDN1

px_IPv4_Address1_RemoteUE,                   CHARSTRING,    192.168.0.6 #-- @desc  IPv4 Address of remote UE connected to PDN1

px_IPv4_Address1_UE,                         CHARSTRING,    192.168.0.1 #-- @desc  IPv4 Address connected to PDN1

px_IPv4_Address2,                            CHARSTRING,    192.168.0.2 #-- @desc  2nd IPv4 Address @sic R5s110011 sic@

px_IPv4_Address2_NW,                         CHARSTRING,    192.168.0.4 #-- @desc  IPv4 Gateway Address in PDN2

px_IPv4_Address2_RemoteUE,                   CHARSTRING,    192.168.1.6 #-- @desc  IPv4 Address of remote UE connected to PDN2

px_IPv4_Address2_UE,                         CHARSTRING,    192.168.0.2 #-- @desc  IPv4 Address connected to PDN2

px_IPv4_Address2a_UE,                        CHARSTRING,    192.168.1.3 #-- @desc  IPv4 Address connected to PDN2a

px_IPv4_Address_BSF,                         CHARSTRING,            #-- @desc  IPv4 BSF address

px_IPv4_Address_HomeAgent,                   CHARSTRING,    192.168.0.5 #-- @desc  IPv4 Home Address Agent

px_IPv4viaNAS_TestMode,                      BOOLEAN,       false   #-- @desc  This parameter can be set to TRUE so as to force allocation of IPv4 only PDN connection and IP address allocation via NAS signalling in the preamble of test cases using test mode (see TS 36.508 [3] clause 4.5.2A).

px_IPv6_Address,                             CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:1111 #-- @desc  IPv6 Address

px_IPv6_Address1_NW,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:3333 #-- @desc  IPv6 Gateway Address in PDN1

px_IPv6_Address1_RemoteUE,                   CHARSTRING,    0001:0000:0000:0000:0000:0000:0000:0006 #-- @desc  IPv6 Address of remote UE in PDN1

px_IPv6_Address1_UE,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:1111 #-- @desc  IPv6 Address in PDN1

px_IPv6_Address2,                            CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:2222 #-- @desc  2nd IPv6 Address  @sic R5s110011 sic@

px_IPv6_Address2_NW,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:4444 #-- @desc  IPv6 Gateway Address in PDN2

px_IPv6_Address2_RemoteUE,                   CHARSTRING,    0001:0000:0000:0000:0000:0000:0000:0006 #-- @desc  IPv6 Address of remote UE in PDN2

px_IPv6_Address2_UE,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:2222 #-- @desc  IPv6 Address in PDN2

px_IPv6_Address2a_UE,                        CHARSTRING,    0001:0002:0003:0004:0005:0006:0007:0008 #-- @desc  IPv6 Address in PDN2a

px_IPv6_Address_BSF,                         CHARSTRING,            #-- @desc  IPv6 BSF address

px_IPv6_Address_HomeAgent,                   CHARSTRING,    0001:0002:0003:0004:0005:0006:0007:5 #-- @desc  IPv6 Home Address Agent

px_LcsClientAddressDigits,                   CHARSTRING,    0123456 #-- @desc  LCS Client external address Digits

px_LcsClientAddressNPI,                      BITSTRING,     0001    #-- @desc  LCS Client external address NPI

px_LcsClientAddressTOA,                      BITSTRING,     1001    #-- @desc  LCS Client external address TOA

px_LcsClientName,                            CHARSTRING,    OPERATOR #-- @desc  LCS Client name

px_MACIndex,                                 INTEGER,       15      #-- @desc  Reverse link MAC index to be used. C.S0024 clause 12.4.1.3.2.2.  Supported values 0..383

px_MFBI_BandChannelBandwidth,                ENUM-Dl_Bandwidth_Type,n25     #-- @desc  MFBI E-UTRAN Channel Bandwidth

px_MFBI_FrequencyBand,                       INTEGER,       26      #-- @desc  a supported E-UTRA MFBI frequency band

px_MFBI_UTRAN_FrequencyBand,                 INTEGER,       26      #-- @desc  A supported UTRAN MFBI frequency band.

px_MS_ClsmkESIND,                            BITSTRING,     0       #-- @desc  Default Early Sending Indication

px_MS_ClsmkRevLvl,                           BITSTRING,     10      #-- @desc  Default Revision Level

px_MS_TXPWR_MAX_CCH,                         BITSTRING,     01010   #-- @desc  MS_TXPWR_MAX_CCH

px_MaxNumberROHC_ContextSessions,            ENUM-MaxNumberROHC_ContextSessions_Type,cs16    #-- @desc  Maximum number of ROHC context sessions

px_NAS_CipheringAlgorithm,                   BITSTRING,     001     #-- @desc  NAS Ciphering Algorithm (eea1)

px_NAS_IntegrityProtAlgorithm,               BITSTRING,     001     #-- @desc  NAS Integrity Algorithm (eia1)

px_OpenLoopAdjust,                           INTEGER,       10      #-- @desc  The value of open loop adjust to be used by access terminals in the open loop power estimate expressed as an unsigned value in units of 1 dB. The value  used by the access terminal is -1 times the value of this field

px_OverlappingNotSupportedFrequencyBand_MFBI,INTEGER,       27      #-- @desc  a not supported E-UTRA frequency band that is overlapping with a supported MFBI band

px_PSI_SMSC,                                 CHARSTRING,    sip:psi_smsc@3gpp.org #-- @desc  The public service identity of the SMSC set to the same value as the first record in EFPSISMSC

px_PTMSI_Def,                                OCTETSTRING,   C2345678 #-- @desc  Default PTMSI

px_PTMSI_SigDef,                             OCTETSTRING,   AB1234  #-- @desc  Default PTMSI signature (3 octets 3GPP 24.008   10.5.5.8).

px_PWS_CB_DataCodingScheme,                  BITSTRING,     1010    #-- @desc  CMAS or ETWS data coding scheme of the alphabetcodingand the applied language (see TS 23.401)

px_PWS_CB_DataPage1,                         CHARSTRING,    warning #-- @desc  ETWS or CMAS Page 1 warning data message

px_PWS_CB_DataPage2,                         CHARSTRING,    warning #-- @desc  ETWS or CMAS Page 2 warning data message

px_PWS_CB_DataPage3,                         CHARSTRING,    warning #-- @desc  CMAS or ETWS Page 3 warning data message

px_PWS_CB_DataPage4,                         CHARSTRING,    warning #-- @desc  CMAS or ETWS Page 4 warning data message

px_P_CSCF_IPAddr,                            CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:1111 #-- @desc  P-CSCF address

px_PeerUE_IPAddr,                            CHARSTRING,    10.122.11.25 #-- @desc  Peer UE address

px_PowerDownRegEnabled,                      BOOLEAN,       true    #-- @desc  Parameter for power down req in 1xRTT

px_PowerLevel,                               BITSTRING,     00000   #-- @desc  power level value for L1 header

px_RAND,                                     BITSTRING,     00001111000011110000111100001111 #-- @desc  Random challenge data to be included along with mobility parameters in CSFBParametersResponseCDMA2000 or HandoverFromEUTRAPreparationRequest

px_RAND2,                                    BITSTRING,     00001111000011110000111100001111 #-- @desc  Random challenge data to be included along with mobility parameters in CSFBParametersResponseCDMA2000 or HandoverFromEUTRAPreparationRequest

px_RAND_Cell19,                              BITSTRING,     00001111000011110000111100001111 #-- 

px_RAND_Cell21,                              BITSTRING,     00001111000011110000111100001111 #-- 

px_RANTech,                                  ENUM-RANTech,  EUTRA_FDD #-- @desc  Technology to be used

px_RATComb_Tested,                           ENUM-RATComb_Tested_Type,EUTRA_UTRA #-- @desc  This parameter represents the network RAT capabilitypreference and indicates which if any is supported RAT combination is to be tested

px_RRC_CipheringAlgorithm,                   ENUM-CipheringAlgorithm_Type,eea1    #-- @desc  Ciphering Algorithm

px_RRC_CipheringAlgorithm_r12,               ENUM-CipheringAlgorithm_r12,eea1    #-- @desc  Ciphering Algorithm  Anritsu TTCN WA for px_RRC_CipheringAlgorithm backward compatibility

px_RRC_IntegrityProtAlgorithm,               ENUM-IntegrityProtAlgorithm_Type,eia1    #-- @desc  Integrity Algorithm

px_RRC_PS_ServTested,                        ENUM-RRC_ServTested,ps_Interactive #-- @desc  PS Service to be tested

px_RXLEV_ACCESS_MIN,                         BITSTRING,     000000  #-- @desc   minimum received signal level at MS

px_Release,                                  ENUM-AccessStratumRelease,rel8    #-- @desc  Release the UE supports

px_Release_check_in_eMBMS_TCs,               BOOLEAN,       true    #-- @desc The access stratum release indicator will not be checked for Rel11 if set to "false"

px_ResetStoredInfo,                          BOOLEAN,       false   #-- @desc  Support of RESETUEPOSITIONINGSTOREDINFORMATION command as defined in 3GPP TS 34.109 cl. 6.10

px_SMS_ChkMsgReceived,                       BOOLEAN,       true    #-- @desc  Whether the operator can check an MT Short Message received

px_SMS_IndexOffset,                          INTEGER,       0       #-- @desc  Memory location index at UE for SMS storage used in +CMSS command

px_SMS_MsgFrmt,                              CHARSTRING,    1       #-- @desc  Either PDU (0) mode or Text mode (1)  @sic R5s110750 sic@

px_SMS_PrefMem1,                             CHARSTRING,    SM      #-- @desc  SMS Preferred Memory 1 <mem1> of TS 27.005 [31] clause 3.2.2

px_SMS_PrefMem2,                             CHARSTRING,    SM      #-- @desc  SMS Preferred Memory 2 <mem2> of TS 27.005 [31] clause 3.2.2

px_SMS_PrefMem3,                             CHARSTRING,    MT      #-- @desc  SMS Preferred Memory 3 <mem3> of TS 27.005 [31] clause 3.2.2

px_SMS_SMSC_InternationalNumber,             CHARSTRING,    112233445566778 #-- @desc  international number of the SMSC:

px_SMS_Service,                              CHARSTRING,    0       #-- @desc  SMS Service <service> of TS 27.005 [31] clause 3.2.1

px_SRNC_Id,                                  BITSTRING,     000000000001 #-- @desc  SRNC Id

px_SRNTI,                                    BITSTRING,     00000000000000000001 #-- @desc  S RNTI

px_SVN_Def,                                  HEXSTRING,     00      #-- Anritsu TTCN-CR required (ProseCR R5-131832)

px_SinglePLMN_Tested,                        ENUM-SinglePLMN_TestedType,MultiPLMN #-- @desc  This parameter represents the network capabilitypreference to support multi PLMNs on the same test Band and indicates the preference of multi PLMNs or single PLMN test environment

px_SplitOnCCCH,                              BITSTRING,     0       #-- @desc  Split pg cycle on CCCH supported indication

px_StartStop,                                BOOLEAN,       false   #-- Anritsu TTCN WA for Automation EnableDisable

px_StartString,                              CHARSTRING,    StartTest: #-- Anritsu TTCN WA for Automation Starting test cases string e.g.: StartTest:TC_7_1_2_1

px_StopString,                               CHARSTRING,    EndTest: #-- Anritsu TTCN WA for Automation Stopping test cases string e.g.: StopTest:Passed

px_TDD_OperationBand,                        CHARSTRING,    33      #-- @desc  LCR TDD Operation Band

px_TDD_OperationBandCharstring,              CHARSTRING,    a       #-- @desc  Applicable for TDD. Ther operation band under test as defined in 34.108 clause 5.1.2

px_TDD_Sync_cells,                           BOOLEAN,       true    #-- @desc  Used for configuring synchronous TDD cells             Anrisu TTCN CR for TDD Tcell

px_TMSI_Def,                                 OCTETSTRING,   11223344 #-- @desc  Default TMSI

px_TSC,                                      BITSTRING,     011     #-- @desc  Training sequence code for traffic channels.

px_TestLoopModeB_Delay,                      OCTETSTRING,   5A      #-- @desc  This parameter represents the IP PDU delay to be used for UE test loop mode B intest cases where long delay may be needed e.g. because of user interaction.

px_TimingAdvance,                            BITSTRING,     0000000 #-- @desc  Timing advance value for L1 header

px_UARFCN_D_High,                            INTEGER,       10837   #-- @desc  High Range downlink UARFCN value

px_UARFCN_D_Low,                             INTEGER,       10563   #-- @desc  Low Range downlink UARFCN value

px_UARFCN_D_Mid,                             INTEGER,       10700   #-- @desc  Mid Range downlink UARFCN value

px_UARFCN_High,                              INTEGER,       9596    #-- @desc  High Range UARFCN value for LCR TDD

px_UARFCN_High_TDD,                          INTEGER,       9596    #-- @desc  High Range downlink UARFCN value for LCR TDD

px_UARFCN_Low,                               INTEGER,       9504    #-- @desc  Low Range UARFCN value for LCR TDD

px_UARFCN_Low_TDD,                           INTEGER,       9504    #-- @desc  Low Range downlink UARFCN value for LCR TDD

px_UARFCN_Mid,                               INTEGER,       9550    #-- @desc  Mid Range UARFCN value for LCR TDD

px_UARFCN_Mid_TDD,                           INTEGER,       9550    #-- @desc  Mid Range downlink UARFCN value for LCR TDD

px_UARFCN_TDD_D_High,                        INTEGER,       10837   #-- @desc  High Range downlink UARFCN value for LCR TDD

px_UARFCN_TDD_D_Low,                         INTEGER,       10563   #-- @desc  Low Range downlink UARFCN value for LCR TDD

px_UARFCN_TDD_D_Mid,                         INTEGER,       10700   #-- @desc  Mid Range downlink UARFCN value for LCR TDD

px_UATI24,                                   OCTETSTRING,   123456  #-- @desc  UATI to be allocated to the UE.  C.S0024 clause 6.3.7.2.2

px_UE_CS_PS_UsageSetting_Tested,             ENUM-CS_PS_MODE,VOICE_CENTRIC #-- @desc  specifies which CSPS mode is under test @sic R5s120274 sic@

px_UE_IPAddr,                                CHARSTRING,    10.122.11.21 #-- @desc  IP address assigned to UE (in v4 or v6 format)

px_UE_IPAddr2,                               CHARSTRING,    10.122.11.31 #-- @desc  2nd IP address assigned to UE (in v4 or v6 format)

px_UE_PS_UsageSetting_Tested,                ENUM-PS_MODE,  VOICE_CENTRIC #-- @desc  specifies which PS mode is under test @sic R5s120274 sic@

px_UE_Release,                               INTEGER,       8       #-- @desc  Required for 34.229 model only

px_UE_UsageSetting_Tested,                   ENUM-CS_PS_MODE,VOICE_CENTRIC #-- @desc  specifies which CS/PS mode is under test

px_UEwithISIM,                               BOOLEAN,       true    #-- @desc  true - UE has ISIM; false - UE has USIM only

px_UEwithSIM,                                BOOLEAN,       FALSE   #-- @desc  UE has a SIM inserted

px_UTRAN_CipheringAlgorithm,                 ENUM-CipheringAlgorithm_r7,uea1    #-- @desc  UTRAN Ciphering algorithm

px_UTRAN_ModeUnderTest,                      ENUM-UTRAN_FDD_TDD_Type,UTRAN_FDD #-- @desc  specifies which radio access technology is being tested in UTRAN

px_UTRAN_OverlappingNotSupportedFrequencyBandMFBI,INTEGER,       27      #-- @desc  A not supported UTRAN frequency band that is overlapping with a supported MFBI band (px_MFBI_UTRAN_FrequencyBand). This pixit shall be set also in accordance with the values of the 3 Pixits: px_UARFCN_D_High px_UARFCN_D_Midpx_UARFCN_L_Mid.

px_UeLcsNotification,                        INTEGER,       20      #-- @desc  Value for UE LCS Notification timeout timer (in seconds)

px_WLANBand,                                 ENUM-WLAN_Band_Type,Band2_4Ghz #-- @desc  WLAN ISM Band

px_WLAN_RulesToBeTested,                     CHARSTRING,    ANDSF_Rules #-- ChannelUtilization

px_XCAPServerAddress,                        CHARSTRING,    10.122.11.26 #-- @desc  XCAP Server address

px_XCAP_RootUri,                             CHARSTRING,    XCAP.3gpp.org #-- @desc  XCAP Root URI

px_XCAP_TargetUri,                           CHARSTRING,    sip:user@domain.com #-- @desc  Target (SIP or TEL URI) where to forward to

px_XCAP_Username,                            CHARSTRING,    0       #-- @desc  username to be used for HTTP authentication in case of pc_XCAP_UsernameIsConfiguredInUE==true

px_eAuthRAND,                                BITSTRING,     10100011110111100000110001101101001101100011111000110000110000110110010010100100000001111000111100011011111110001101010101110111 #-- @desc  Random Challenge

px_eJapanMCC_Band6,                          HEXSTRING,     442     #-- @desc  Japan MCC code to be used for Band 6. The same value will be used for E-UTRAN and Inter-RAT cells. Type is different to that defined in 34.123-3.

px_eMaxNumberROHC_ContextSessions,           ENUM-MaxNumberROHC_ContextSessions_Type,cs16    #-- @desc  Maximum number of ROHC context sessions @sic R5s130329 sic@

px_ePDG_Ipsec_CipheringAlgorithm,            ENUM-IPsec_CipheringAlgorithm_Type,des_ede3_cbc #-- @desc  Ipsec Ciphering Algorithm used in ePDG

px_ePDG_Ipsec_IntegrityAlgorithm,            ENUM-IPsec_IntegrityAlgorithm_Type,hmac_sha_1_96 #-- @desc  Ipsec Integrity Algorithm used in ePDG

px_ePrimaryBandChannelBandwidth,             ENUM-Dl_Bandwidth_Type,n25     #-- @desc  Primary E-UTRAN Channel Bandwidth

px_ePrimaryFrequencyBand,                    INTEGER,       1       #-- @desc  E-UTRAN primary frequency band

px_eSecondaryBandChannelBandwidth,           ENUM-Dl_Bandwidth_Type,n25     #-- @desc  Secondary Band E-UTRAN Channel Bandwidth

px_eSecondaryFrequencyBand,                  INTEGER,       2       #-- @desc  E-UTRAN secondary frequency band

px_eTDDsubframeConfig,                       ENUM-TDD_SubframeAssignment_Type,sa1     #-- @desc  TDD uplink-downlink subframe configuration

px_eUE_Category_Type,                        INTEGER,       3       #-- @desc  UE Category values 1..5 as defined in 36.306 clause 4.1

