    Log Viewer 37.231.3.0
    Copyright © 2016, Anite Telecoms Ltd.
    LogFile            : TC_9_2_1_1_7c_Log.alf
    Created            : 10/10/2016 5:57:00 AM

    Tester                                                       UUT

    MATCH_MISMATCH:
    ↑	Message Mismatch: IPCAN_RAN_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IPCAN_RAN_Type
    		MATCH_MISMATCH
    			Message Mismatch: IPCAN_RAN_Type
    				IPCAN_RAN_Type = FBBA (6)

    UT_SYSTEM_REQ:
    ↓	Sent from port: MTC_LTE:Ut
    		Source = \Test Control\TTCN3
    		UT_SYSTEM_REQ
    			Cmd
    				MMI
    					Cmd = 'POWER_OFF'
    					ParameterList = Omit
    			CnfRequired = CNF_REQUIRED (1)

    UT_COMMON_CNF:
    ↑	Received on port: MTC_LTE:Ut
    		Source = \Test Control\TTCN3
    		UT_COMMON_CNF
    			Result = True
    			ResultString = Omit

    Timer Event:
    	Timer: t_GuardTimer, Duration: 360s, Started: 17:34:44
    		Source = \Test Control\TTCN3
    		timerEvent = 6
    		fileName = LTE_A_R12_Testsuite.ttcn
    		testName = TC_9_2_1_1_7c
    		lineNo = 1183
    		outStr = Timer: t_GuardTimer, Duration: 360s, Started: 17:34:44

    BCCH-BCH-Message:
    	MasterInformationBlock
    		Source = \Protocol\3GPP\LTE\RRC\
    		BCCH-BCH-Message
    			message
    				dl-Bandwidth = n25
    				phich-Config
    					phich-Duration = normal
    					phich-Resource = one
    				systemFrameNumber = 00000000
    				spare = 0000000000
    ------------------------------------------------------------------------------------------------------------→
    BCCH-DL-SCH-Message:
    	systemInformationBlockType1
    		Source = \Protocol\3GPP\LTE\RRC\
    		BCCH-DL-SCH-Message
    			message = c1 = systemInformationBlockType1 =
    				cellAccessRelatedInfo
    					plmn-IdentityList = SEQUENCE OF PLMN-IdentityInfo
    						PLMN-IdentityInfo(1)
    							plmn-Identity
    								mcc = SEQUENCE OF MCC-MNC-Digit
    									MCC-MNC-Digit(1) = 0
    									MCC-MNC-Digit(2) = 0
    									MCC-MNC-Digit(3) = 1
    								mnc = SEQUENCE OF MCC-MNC-Digit
    									MCC-MNC-Digit(1) = 0
    									MCC-MNC-Digit(2) = 1
    							cellReservedForOperatorUse = notReserved
    					trackingAreaCode = 0000000000000001
    					cellIdentity = 0000000000000001000100000001
    					cellBarred = notBarred
    					intraFreqReselection = notAllowed
    					csg-Indication = FALSE
    				cellSelectionInfo
    					q-RxLevMin = -53
    				freqBandIndicator = 4
    				schedulingInfoList = SEQUENCE OF SchedulingInfo
    					SchedulingInfo(1)
    						si-Periodicity = rf16
    						sib-MappingInfo = SEQUENCE OF
    					SchedulingInfo(2)
    						si-Periodicity = rf32
    						sib-MappingInfo = SEQUENCE OF SIB-Type
    							SIB-Type(1) = sibType3
    				si-WindowLength = ms20
    				systemInfoValueTag = 0
    				nonCriticalExtension
    					nonCriticalExtension
    						ims-EmergencySupport-r9 = true
    ------------------------------------------------------------------------------------------------------------→
    BCCH-DL-SCH-Message:
    	systemInformation
    		Source = \Protocol\3GPP\LTE\RRC\
    		BCCH-DL-SCH-Message
    			message = c1 = systemInformation =
    				criticalExtensions = systemInformation-r8 =
    					sib-TypeAndInfo = SEQUENCE OF CHOICE
    						CHOICE(1) = sib2 =
    							radioResourceConfigCommon
    								rach-ConfigCommon
    									preambleInfo
    										numberOfRA-Preambles = n52
    									powerRampingParameters
    										powerRampingStep = dB2
    										preambleInitialReceivedTargetPower = dBm-104
    									ra-SupervisionInfo
    										preambleTransMax = n6
    										ra-ResponseWindowSize = sf10
    										mac-ContentionResolutionTimer = sf48
    									maxHARQ-Msg3Tx = 4
    								bcch-Config
    									modificationPeriodCoeff = n4
    								pcch-Config
    									defaultPagingCycle = rf128
    									nB = oneT
    								prach-Config
    									rootSequenceIndex = 22
    									prach-ConfigInfo
    										prach-ConfigIndex = 3
    										highSpeedFlag = FALSE
    										zeroCorrelationZoneConfig = 5
    										prach-FreqOffset = 2
    								pdsch-ConfigCommon
    									referenceSignalPower = 18
    									p-b = 0
    								pusch-ConfigCommon
    									pusch-ConfigBasic
    										n-SB = 1
    										hoppingMode = interSubFrame
    										pusch-HoppingOffset = 4
    										enable64QAM = FALSE
    									ul-ReferenceSignalsPUSCH
    										groupHoppingEnabled = TRUE
    										groupAssignmentPUSCH = 0
    										sequenceHoppingEnabled = FALSE
    										cyclicShift = 0
    								pucch-ConfigCommon
    									deltaPUCCH-Shift = ds2
    									nRB-CQI = 2
    									nCS-AN = 6
    									n1PUCCH-AN = 0
    								soundingRS-UL-ConfigCommon = setup =
    									srs-BandwidthConfig = bw3
    									srs-SubframeConfig = sc0
    									ackNackSRS-SimultaneousTransmission = TRUE
    								uplinkPowerControlCommon
    									p0-NominalPUSCH = -85
    									alpha = al08
    									p0-NominalPUCCH = -117
    									deltaFList-PUCCH
    										deltaF-PUCCH-Format1 = deltaF0
    										deltaF-PUCCH-Format1b = deltaF3
    										deltaF-PUCCH-Format2 = deltaF0
    										deltaF-PUCCH-Format2a = deltaF0
    										deltaF-PUCCH-Format2b = deltaF0
    									deltaPreambleMsg3 = 4
    								ul-CyclicPrefixLength = len1
    							ue-TimersAndConstants
    								t300 = ms1000
    								t301 = ms1000
    								t310 = ms1000
    								n310 = n1
    								t311 = ms10000
    								n311 = n1
    							freqInfo
    								additionalSpectrumEmission = 1
    							timeAlignmentTimerCommon = sf750
    ------------------------------------------------------------------------------------------------------------→
    BCCH-DL-SCH-Message:
    	systemInformation
    		Source = \Protocol\3GPP\LTE\RRC\
    		BCCH-DL-SCH-Message
    			message = c1 = systemInformation =
    				criticalExtensions = systemInformation-r8 =
    					sib-TypeAndInfo = SEQUENCE OF CHOICE
    						CHOICE(1) = sib3 =
    							cellReselectionInfoCommon
    								q-Hyst = dB0
    							cellReselectionServingFreqInfo
    								threshServingLow = 0
    								cellReselectionPriority = 4
    							intraFreqCellReselectionInfo
    								q-RxLevMin = -53
    								presenceAntennaPort1 = FALSE
    								neighCellConfig = 01
    								t-ReselectionEUTRA = 0
    ------------------------------------------------------------------------------------------------------------→
    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = True
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				Cell
    					AddOrReconfigure
    						Basic
    							ConfigCapability = fullCell (2)
    							StaticCellInfo
    								Common
    									RAT
    										FDD = True
    									PhysicalCellId = 1
    									eNB_CellId = Omit
    									EutraBand = 4
    									CellTimingInfo
    										Tcell = 0
    										SfnOffset = 0
    										HsfnOffset = 0
    								Downlink
    									Earfcn = 2175
    									Bandwidth = n25 (2)
    									RBSize = n_RB_SC_12 (0)
    									CyclicPrefix = normal (0)
    								Uplink
    									Earfcn = 20175
    									Bandwidth = n25 (2)
    									CyclicPrefix = normal (0)
    							PhysicalLayerConfigDL
    								AntennaGroup
    									AntennaInfoCommon
    										R8
    											antennaPortsCount = an1 (0)
    									AntennaPort
    										AntennaPort_Type
    											Id = 0
    											Config
    												AddOrReconfigure
    													PowerAttenuation = True
    													PropagationDelay = True
    								Pbch
    									RelativeTxPower
    										RA = 0
    										RB = 0
    								Pcfich
    									CfiValue = 3
    									RelativeTxPower
    										RA = 0
    										RB = 0
    								Phich
    									PhichConfig
    										R8
    											phich_Duration = normal (0)
    											phich_Resource = one (2)
    									RelativeTxPower
    										RA = 0
    										RB = 0
    								Pdcch
    									CommonSearchSpaceFormat = 2
    									UeSpecificSearchSpaceFormat = 1
    									PdcchCandidateList
    										PdcchCandidate_Type
    											RNTI = 0001000000000001'B
    											CCE_StartIndexList
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 12
    													CCE_StartIndex_UL = 14
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 14
    													CCE_StartIndex_UL = 16
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 12
    													CCE_StartIndex_UL = 14
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 14
    													CCE_StartIndex_UL = 16
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 10
    													CCE_StartIndex_UL = 12
    										PdcchCandidate_Type
    											RNTI = 0001000000110100'B
    											CCE_StartIndexList
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 12
    													CCE_StartIndex_UL = 14
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 16
    													CCE_StartIndex_UL = 18
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 14
    													CCE_StartIndex_UL = 16
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 10
    													CCE_StartIndex_UL = 12
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 18
    													CCE_StartIndex_UL = 8
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 16
    													CCE_StartIndex_UL = 18
    										PdcchCandidate_Type
    											RNTI = 0001000100010001'B
    											CCE_StartIndexList
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 16
    													CCE_StartIndex_UL = 18
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 10
    													CCE_StartIndex_UL = 12
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 14
    													CCE_StartIndex_UL = 16
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 10
    													CCE_StartIndex_UL = 12
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 14
    													CCE_StartIndex_UL = 16
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 18
    													CCE_StartIndex_UL = 8
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    										PdcchCandidate_Type
    											RNTI = 0001111111110001'B
    											CCE_StartIndexList
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 12
    													CCE_StartIndex_UL = 14
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 12
    													CCE_StartIndex_UL = 14
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 18
    													CCE_StartIndex_UL = 8
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 16
    													CCE_StartIndex_UL = 18
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 18
    													CCE_StartIndex_UL = 8
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 18
    													CCE_StartIndex_UL = 8
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 18
    													CCE_StartIndex_UL = 8
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    										PdcchCandidate_Type
    											RNTI = 0000010011010010'B
    											CCE_StartIndexList
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 10
    													CCE_StartIndex_UL = 12
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 10
    													CCE_StartIndex_UL = 12
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 14
    													CCE_StartIndex_UL = 16
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 14
    													CCE_StartIndex_UL = 16
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 10
    													CCE_StartIndex_UL = 12
    										PdcchCandidate_Type
    											RNTI = 0000100100101001'B
    											CCE_StartIndexList
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 10
    													CCE_StartIndex_UL = 12
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 12
    													CCE_StartIndex_UL = 14
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 14
    													CCE_StartIndex_UL = 16
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    										PdcchCandidate_Type
    											RNTI = 0000110110000000'B
    											CCE_StartIndexList
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 16
    													CCE_StartIndex_UL = 18
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 18
    													CCE_StartIndex_UL = 8
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 14
    													CCE_StartIndex_UL = 16
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 14
    													CCE_StartIndex_UL = 16
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 16
    													CCE_StartIndex_UL = 18
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 14
    													CCE_StartIndex_UL = 16
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    										PdcchCandidate_Type
    											RNTI = 0001000111010111'B
    											CCE_StartIndexList
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 16
    													CCE_StartIndex_UL = 18
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 14
    													CCE_StartIndex_UL = 16
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 16
    													CCE_StartIndex_UL = 18
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    										PdcchCandidate_Type
    											RNTI = 0001011000101110'B
    											CCE_StartIndexList
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 12
    													CCE_StartIndex_UL = 14
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 12
    													CCE_StartIndex_UL = 14
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 16
    													CCE_StartIndex_UL = 18
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 16
    													CCE_StartIndex_UL = 18
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 18
    													CCE_StartIndex_UL = 8
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    										PdcchCandidate_Type
    											RNTI = 0001101010000101'B
    											CCE_StartIndexList
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 16
    													CCE_StartIndex_UL = 18
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 16
    													CCE_StartIndex_UL = 18
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 16
    													CCE_StartIndex_UL = 18
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    												CCE_StartIndex_DL_UL_Type
    													CCE_StartIndex_DL = 8
    													CCE_StartIndex_UL = 10
    									RelativeTxPower
    										RA = 0
    										RB = 0
    								Pdsch
    									RelativeTxPower
    										RachResponse
    											RA = 0
    											RB = 0
    										BcchOnPdsch
    											RA = 0
    											RB = 0
    										PcchOnPdsch
    											RA = 0
    											RB = 0
    										CcchOnPdsch
    											RA = 0
    											RB = 0
    										DcchDtchOnPdsch
    											RA = -3
    											RB = -3
    										OcngOnPdsch = Omit
    									PDSCH_ConfigCommon = Omit
    								Pss
    									RelativeTxPower
    										RA = 0
    										RB = 0
    								Sss
    									RelativeTxPower
    										RA = 0
    										RB = 0
    								CSI_RS_Config = Omit
    								Pmch = Omit
    								Epdcch = Omit
    							InitialCellPower
    								MaxReferencePower = -85
    								Attenuation
    									Off = True
    							BcchConfig
    								Pbch = True
    								Pdsch
    									Sib1Schedul
    										DciInfo
    											Format = dci_1C (4)
    											ResourceAllocType = ra_2_Distributed (3)
    											Modulation_1stCW = qpsk (1)
    											Modulation_2ndCW = unused (0)
    											FreqDomainSchedul
    												FirstRbIndex = 0
    												MaxRbCnt = 4
    											RedundancyVersionList
    												RedundancyVersion_Type = 0
    											RepetitionNumber = Omit
    									SiSchedul
    										WindowLength = ms20 (5)
    										SiList
    											SiSchedul_Type
    												Periodicity = rf16 (1)
    												Window
    													SingleSiSchedul_Type
    														DciInfo
    															Format = dci_1C (4)
    															ResourceAllocType = ra_2_Distributed (3)
    															Modulation_1stCW = qpsk (1)
    															Modulation_2ndCW = unused (0)
    															FreqDomainSchedul
    																FirstRbIndex = 0
    																MaxRbCnt = 4
    															RedundancyVersionList
    																RedundancyVersion_Type = 2
    															RepetitionNumber = Omit
    														SubframeOffset = 1
    											SiSchedul_Type
    												Periodicity = rf32 (2)
    												Window
    													SingleSiSchedul_Type
    														DciInfo
    															Format = dci_1C (4)
    															ResourceAllocType = ra_2_Distributed (3)
    															Modulation_1stCW = qpsk (1)
    															Modulation_2ndCW = unused (0)
    															FreqDomainSchedul
    																FirstRbIndex = 0
    																MaxRbCnt = 4
    															RedundancyVersionList
    																RedundancyVersion_Type = 2
    															RepetitionNumber = Omit
    														SubframeOffset = 1
    										SegmentedSiList = Omit
    								BcchInfo
    									MIB
    										message_
    											dl_Bandwidth = n25 (2)
    											phich_Config
    												phich_Duration = normal (0)
    												phich_Resource = one (2)
    											systemFrameNumber = 00000000'B
    											schedulingInfoSIB1_BR_r13 = 0
    											spare = 00000'B
    									SIB1
    										message_
    											c1
    												systemInformationBlockType1
    													cellAccessRelatedInfo
    														plmn_IdentityList
    															PLMN_IdentityInfo
    																plmn_Identity
    																	mcc
    																		MCC_MNC_Digit = 0
    																		MCC_MNC_Digit = 0
    																		MCC_MNC_Digit = 1
    																	mnc
    																		MCC_MNC_Digit = 0
    																		MCC_MNC_Digit = 1
    																cellReservedForOperatorUse = notReserved (1)
    														trackingAreaCode = 0000000000000001'B
    														cellIdentity = 0000000000000001000100000001'B
    														cellBarred = notBarred (1)
    														intraFreqReselection = notAllowed (1)
    														csg_Indication = False
    														csg_Identity = Omit
    													cellSelectionInfo
    														q_RxLevMin = -53
    														q_RxLevMinOffset = Omit
    													p_Max = Omit
    													freqBandIndicator = 4
    													schedulingInfoList
    														SchedulingInfo
    															si_Periodicity = rf16 (1)
    															sib_MappingInfo
    														SchedulingInfo
    															si_Periodicity = rf32 (2)
    															sib_MappingInfo
    																SIB_Type = sibType3 (0)
    													tdd_Config = Omit
    													si_WindowLength = ms20 (5)
    													systemInfoValueTag = 0
    													nonCriticalExtension
    														lateNonCriticalExtension = Omit
    														nonCriticalExtension
    															ims_EmergencySupport_r9 = true_ (0)
    															cellSelectionInfo_v920 = Omit
    															nonCriticalExtension = Omit
    									SIs
    										BCCH_DL_SCH_Message
    											message_
    												c1
    													systemInformation
    														criticalExtensions
    															systemInformation_r8
    																sib_TypeAndInfo
    																	SystemInformation_r8_IEs___0___oftype
    																		sib2
    																			ac_BarringInfo = Omit
    																			radioResourceConfigCommon
    																				rach_ConfigCommon
    																					preambleInfo
    																						numberOfRA_Preambles = n52 (12)
    																						preamblesGroupAConfig = Omit
    																					powerRampingParameters
    																						powerRampingStep = dB2 (1)
    																						preambleInitialReceivedTargetPower = dBm_104 (8)
    																					ra_SupervisionInfo
    																						preambleTransMax = n6 (3)
    																						ra_ResponseWindowSize = sf10 (7)
    																						mac_ContentionResolutionTimer = sf48 (5)
    																					maxHARQ_Msg3Tx = 4
    																					preambleTransMax_CE_r13 = Omit
    																					rach_CE_LevelInfoList_r13 = Omit
    																				bcch_Config
    																					modificationPeriodCoeff = n4 (1)
    																				pcch_Config
    																					defaultPagingCycle = rf128 (2)
    																					nB = oneT (2)
    																				prach_Config
    																					rootSequenceIndex = 22
    																					prach_ConfigInfo
    																						prach_ConfigIndex = 3
    																						highSpeedFlag = False
    																						zeroCorrelationZoneConfig = 5
    																						prach_FreqOffset = 2
    																				pdsch_ConfigCommon
    																					referenceSignalPower = 18
    																					p_b = 0
    																				pusch_ConfigCommon
    																					pusch_ConfigBasic
    																						n_SB = 1
    																						hoppingMode = interSubFrame (0)
    																						pusch_HoppingOffset = 4
    																						enable64QAM = False
    																					ul_ReferenceSignalsPUSCH
    																						groupHoppingEnabled = True
    																						groupAssignmentPUSCH = 0
    																						sequenceHoppingEnabled = False
    																						cyclicShift = 0
    																				pucch_ConfigCommon
    																					deltaPUCCH_Shift = ds2 (1)
    																					nRB_CQI = 2
    																					nCS_AN = 6
    																					n1PUCCH_AN = 0
    																				soundingRS_UL_ConfigCommon
    																					setup
    																						srs_BandwidthConfig = bw3 (3)
    																						srs_SubframeConfig = sc0 (0)
    																						ackNackSRS_SimultaneousTransmission = True
    																						srs_MaxUpPts = Omit
    																				uplinkPowerControlCommon
    																					p0_NominalPUSCH = -85
    																					alpha = al08 (5)
    																					p0_NominalPUCCH = -117
    																					deltaFList_PUCCH
    																						deltaF_PUCCH_Format1 = deltaF0 (1)
    																						deltaF_PUCCH_Format1b = deltaF3 (1)
    																						deltaF_PUCCH_Format2 = deltaF0 (1)
    																						deltaF_PUCCH_Format2a = deltaF0 (1)
    																						deltaF_PUCCH_Format2b = deltaF0 (1)
    																					deltaPreambleMsg3 = 4
    																				ul_CyclicPrefixLength = len1 (0)
    																				uplinkPowerControlCommon_v1020 = Omit
    																				rach_ConfigCommon_v1250 = Omit
    																				pusch_ConfigCommon_v1270 = Omit
    																				bcch_Config_v1310 = Omit
    																				pcch_Config_v1310 = Omit
    																				freqHoppingParameters_r13 = Omit
    																				pdsch_ConfigCommon_v1310 = Omit
    																				pusch_ConfigCommon_v1310 = Omit
    																				prach_ConfigCommon_v1310 = Omit
    																				pucch_ConfigCommon_v1310 = Omit
    																			ue_TimersAndConstants
    																				t300 = ms1000 (5)
    																				t301 = ms1000 (5)
    																				t310 = ms1000 (5)
    																				n310 = n1 (0)
    																				t311 = ms10000 (3)
    																				n311 = n1 (0)
    																				t300_v1310 = Omit
    																				t301_v1310 = Omit
    																			freqInfo
    																				ul_CarrierFreq = Omit
    																				ul_Bandwidth = Omit
    																				additionalSpectrumEmission = 1
    																			mbsfn_SubframeConfigList = Omit
    																			timeAlignmentTimerCommon = sf750 (1)
    																			lateNonCriticalExtension = Omit
    																			ssac_BarringForMMTEL_Voice_r9 = Omit
    																			ssac_BarringForMMTEL_Video_r9 = Omit
    																			ac_BarringForCSFB_r10 = Omit
    																			ac_BarringSkipForMMTELVoice_r12 = Omit
    																			ac_BarringSkipForMMTELVideo_r12 = Omit
    																			ac_BarringSkipForSMS_r12 = Omit
    																			ac_BarringPerPLMN_List_r12 = Omit
    																			voiceServiceCauseIndication_r12 = Omit
    																			acdc_BarringForCommon_r13 = Omit
    																			acdc_BarringPerPLMN_List_r13 = Omit
    																			udt_RestrictingForCommon_r13 = Omit
    																			udt_RestrictingPerPLMN_List_r13 = Omit
    																			cIoT_EPS_OptimisationInfo_r13 = Omit
    																			useFullResumeID_r13 = Omit
    																nonCriticalExtension = Omit
    										BCCH_DL_SCH_Message
    											message_
    												c1
    													systemInformation
    														criticalExtensions
    															systemInformation_r8
    																sib_TypeAndInfo
    																	SystemInformation_r8_IEs___0___oftype
    																		sib3
    																			cellReselectionInfoCommon
    																				q_Hyst = dB0 (0)
    																				speedStateReselectionPars = Omit
    																			cellReselectionServingFreqInfo
    																				s_NonIntraSearch = Omit
    																				threshServingLow = 0
    																				cellReselectionPriority = 4
    																			intraFreqCellReselectionInfo
    																				q_RxLevMin = -53
    																				p_Max = Omit
    																				s_IntraSearch = Omit
    																				allowedMeasBandwidth = Omit
    																				presenceAntennaPort1 = False
    																				neighCellConfig = 01'B
    																				t_ReselectionEUTRA = 0
    																				t_ReselectionEUTRA_SF = Omit
    																			lateNonCriticalExtension = Omit
    																			s_IntraSearch_v920 = Omit
    																			s_NonIntraSearch_v920 = Omit
    																			q_QualMin_r9 = Omit
    																			threshServingLowQ_r9 = Omit
    																			q_QualMinWB_r11 = Omit
    																			q_QualMinRSRQ_OnAllSymbols_r12 = Omit
    																			cellReselectionServingFreqInfo_v1310 = Omit
    																			redistributionServingInfo_r13 = Omit
    																			cellSelectionInfoCE_r13 = Omit
    																			t_ReselectionEUTRA_CE_r13 = Omit
    																nonCriticalExtension = Omit
    									SegmentedSIs = Omit
    								StopSib1Transmission = Omit
    							PcchConfig
    								DciInfo
    									Format = dci_1C (4)
    									ResourceAllocType = ra_2_Distributed (3)
    									Modulation_1stCW = qpsk (1)
    									Modulation_2ndCW = unused (0)
    									FreqDomainSchedul
    										FirstRbIndex = 4
    										MaxRbCnt = 2
    									RedundancyVersionList
    										RedundancyVersion_Type = 0
    									RepetitionNumber = Omit
    							CA_CellInitialConfig = Omit
    							BRBcchConfig = Omit
    						Active
    							C_RNTI = 0001000000000001'B
    							PhysicalLayerConfigUL
    								Prach
    									R8
    										rootSequenceIndex = 22
    										prach_ConfigInfo
    											prach_ConfigIndex = 3
    											highSpeedFlag = False
    											zeroCorrelationZoneConfig = 5
    											prach_FreqOffset = 2
    								Pucch
    									Common
    										R8
    											deltaPUCCH_Shift = ds2 (1)
    											nRB_CQI = 2
    											nCS_AN = 6
    											n1PUCCH_AN = 0
    									Dedicated
    										R8andLater
    											pucch_ConfigDedicated
    												ackNackRepetition
    													release = Null
    												tdd_AckNackFeedbackMode = Omit
    											pucch_ConfigDedicated_v1020 = Omit
    											pucch_ConfigDedicated_v1130 = Omit
    											pucch_ConfigDedicated_v1250 = Omit
    								Pusch
    									Common
    										R8
    											pusch_ConfigBasic
    												n_SB = 1
    												hoppingMode = interSubFrame (0)
    												pusch_HoppingOffset = 4
    												enable64QAM = False
    											ul_ReferenceSignalsPUSCH
    												groupHoppingEnabled = True
    												groupAssignmentPUSCH = 0
    												sequenceHoppingEnabled = False
    												cyclicShift = 0
    									Dedicated
    										R8andLater
    											pusch_ConfigDedicated
    												betaOffset_ACK_Index = 9
    												betaOffset_RI_Index = 6
    												betaOffset_CQI_Index = 6
    											pusch_ConfigDedicated_v1020 = Omit
    											pusch_ConfigDedicated_v1130 = Omit
    											pusch_ConfigDedicated_v1250 = Omit
    								TimingAdvance
    									InitialValue = 0
    								SRS_UL_Config
    									Common
    										R8
    											setup
    												srs_BandwidthConfig = bw3 (3)
    												srs_SubframeConfig = sc0 (0)
    												ackNackSRS_SimultaneousTransmission = True
    												srs_MaxUpPts = Omit
    									Dedicated
    										R8andLater
    											soundingRS_UL_ConfigDedicated
    												setup
    													srs_Bandwidth = bw0 (0)
    													srs_HoppingBandwidth = hbw0 (0)
    													freqDomainPosition = 0
    													duration = True
    													srs_ConfigIndex = 20
    													transmissionComb = 0
    													cyclicShift = cs0 (0)
    											soundingRS_UL_ConfigDedicated_v1020 = Omit
    											soundingRS_UL_ConfigDedicatedAperiodic_r10 = Omit
    								SR_Config
    									R8andLater
    										schedulingRequestConfig
    											setup
    												sr_PUCCH_ResourceIndex = 20
    												sr_ConfigIndex = 30
    												dsr_TransMax = n4 (0)
    										schedulingRequestConfig_v1020 = Omit
    								CQI_ReportConfig
    									R8andLater
    										cqi_ReportConfig
    											cqi_ReportModeAperiodic = rm30 (3)
    											nomPDSCH_RS_EPRE_Offset = 0
    											cqi_ReportPeriodic
    												setup
    													cqi_PUCCH_ResourceIndex = 0
    													cqi_pmi_ConfigIndex = 25
    													cqi_FormatIndicatorPeriodic
    														widebandCQI = Null
    													ri_ConfigIndex = 483
    													simultaneousAckNackAndCQI = False
    										cqi_ReportConfig_v920 = Omit
    								UplinkPowerControlCommon
    									R8andLater
    										uplinkPowerControlCommon
    											p0_NominalPUSCH = -85
    											alpha = al08 (5)
    											p0_NominalPUCCH = -117
    											deltaFList_PUCCH
    												deltaF_PUCCH_Format1 = deltaF0 (1)
    												deltaF_PUCCH_Format1b = deltaF3 (1)
    												deltaF_PUCCH_Format2 = deltaF0 (1)
    												deltaF_PUCCH_Format2a = deltaF0 (1)
    												deltaF_PUCCH_Format2b = deltaF0 (1)
    											deltaPreambleMsg3 = 4
    										uplinkPowerControlCommon_v1020 = Omit
    										uplinkPowerControlCommonSCell_v1130 = Omit
    										uplinkPowerControlCommonPSCell_r12 = Omit
    								UplinkPowerControlDedicated
    									R8andLater
    										uplinkPowerControlDedicated
    											p0_UE_PUSCH = 0
    											deltaMCS_Enabled = en0 (0)
    											accumulationEnabled = True
    											p0_UE_PUCCH = 0
    											pSRS_Offset = 3
    											filterCoefficient = fc4 (4)
    										uplinkPowerControlDedicated_v1020 = Omit
    										pathlossReferenceLinking = Omit
    										uplinkPowerControlDedicated_v1130 = Omit
    										uplinkPowerControlDedicated_v1250 = Omit
    							RachProcedureConfig
    								RACH_ConfigCommon
    									R8
    										preambleInfo
    											numberOfRA_Preambles = n52 (12)
    											preamblesGroupAConfig = Omit
    										powerRampingParameters
    											powerRampingStep = dB2 (1)
    											preambleInitialReceivedTargetPower = dBm_104 (8)
    										ra_SupervisionInfo
    											preambleTransMax = n6 (3)
    											ra_ResponseWindowSize = sf10 (7)
    											mac_ContentionResolutionTimer = sf48 (5)
    										maxHARQ_Msg3Tx = 4
    										preambleTransMax_CE_r13 = Omit
    										rach_CE_LevelInfoList_r13 = Omit
    								RACH_ConfigDedicated = Omit
    								RachProcedureList
    									RachProcedure_Type
    										RAResponse
    											Ctrl
    												DciInfo
    													Format = dci_1C (4)
    													ResourceAllocType = ra_2_Distributed (3)
    													Modulation_1stCW = qpsk (1)
    													Modulation_2ndCW = unused (0)
    													FreqDomainSchedul
    														FirstRbIndex = 6
    														MaxRbCnt = 4
    													RedundancyVersionList
    														RedundancyVersion_Type = 0
    														RedundancyVersion_Type = 2
    														RedundancyVersion_Type = 3
    														RedundancyVersion_Type = 1
    														RedundancyVersion_Type = 0
    													RepetitionNumber = Omit
    												Rar
    													List
    														RandomAccessResponseParameters_Type
    															RapId
    																Automatic = True
    															InitialGrant
    																HoppingFlag = 0'B
    																RB_Allocation = 0000000000'B
    																ModAndCodScheme = 1111'B
    																TPC_Command = 011'B
    																UL_Delay = 0'B
    																CQI_Req = 0'B
    															TimingAdvance = 0
    															TempC_RNTI
    																SameAsC_RNTI = True
    															InitialGrantCE_Mode = Omit
    												BackoffInd
    													None = True
    										ContentionResolutionCtrl
    											TCRNTI_Based
    												MacPdu
    													ContainedId
    														XorMask = 000000000000000000000000000000000000000000000000'B
    													ContainedRlcPdu
    														RlcPdu = '60129B3E8603B579E89664307B3800064F1A0082818141E0'O
    							CcchDcchDtchConfig
    								MeasGapCtrl
    									None = True
    								DL
    									DciInfo
    										Auto
    											Format = dci_1 (1)
    											ResourceAllocType = ra_0 (0)
    											Modulation_1stCW = qam64 (3)
    											Modulation_2ndCW = unused (0)
    											FreqDomainSchedul
    												FirstRbIndex = 2
    												MaxRbCnt = 23
    											RedundancyVersionList
    												RedundancyVersion_Type = 0
    												RedundancyVersion_Type = 2
    												RedundancyVersion_Type = 3
    												RedundancyVersion_Type = 1
    												RedundancyVersion_Type = 0
    											RepetitionNumber = Omit
    									AntennaInfo
    										R8andLater
    											antennaInfo
    												transmissionMode = tm1 (0)
    												codebookSubsetRestriction = Omit
    												ue_TransmitAntennaSelection
    													release = Null
    											antennaInfo_v920 = Omit
    									HarqProcessConfig
    										AllProcesses = True
    								UL
    									DciInfo
    										Imcs
    											Value = 9
    										TransRetransmissionList
    											UL_TransRetransmission_Type
    												NewTransmission = True
    										FreqDomainSchedul
    											FirstRbIndex = 0
    											Nprb = 25
    										RepetitionNumber = Omit
    									Hopping
    										Deactivated = True
    									PUCCH_Synch
    										None = True
    									UL_GrantConfig
    										None = True
    								DrxCtrl
    									None = True
    								TtiBundling
    									R8 = False
    								CifPresence = Omit
    							ServingCellConfig = Omit
    							SciSchedulingConfig = Omit
    							EIMTA_Config = Omit
    							CE_Mode = Omit

    SYSTEM_CTRL_CNF:
    ↑	Received on port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_CNF
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				Result
    					Success = True
    			Confirm
    				Cell = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: CharacterStringType
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: CharacterStringType
    		MATCH_MISMATCH
    			Message Mismatch: CharacterStringType
    				CharacterStringType = 'TC_9_2_1_1_7c'

    MATCH_MISMATCH:
    ↑	Message Mismatch: CharacterStringType
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: CharacterStringType
    		MATCH_MISMATCH
    			Message Mismatch: CharacterStringType
    				CharacterStringType = 'TC_9_2_1_1_7c'

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = True
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				RadioBearerList
    					RadioBearer_Type
    						Id
    							Srb = 0
    						Config
    							AddOrReconfigure
    								Pdcp
    									None = True
    								Rlc
    									Rb
    										TM = True
    									TestMode
    										None = True
    								LogicalChannelId = 0
    								Mac
    									LogicalChannel
    										Priority = 1
    										PrioritizedBitRate = infinity_ (7)
    									TestMode
    										None = True
    								DiscardULData = Omit
    					RadioBearer_Type
    						Id
    							Srb = 1
    						Config
    							AddOrReconfigure
    								Pdcp
    									Config
    										Rb
    											Srb = True
    										TestMode
    											None = True
    								Rlc
    									Rb
    										AM
    											Tx
    												R8
    													t_PollRetransmit = ms45 (8)
    													pollPDU = pInfinity (7)
    													pollByte = kBinfinity (14)
    													maxRetxThreshold = t4 (3)
    											Rx
    												R8
    													t_Reordering = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    											ExtendedLI = Omit
    									TestMode
    										None = True
    								LogicalChannelId = 1
    								Mac
    									LogicalChannel
    										Priority = 1
    										PrioritizedBitRate = infinity_ (7)
    									TestMode
    										None = True
    								DiscardULData = Omit
    					RadioBearer_Type
    						Id
    							Srb = 2
    						Config
    							AddOrReconfigure
    								Pdcp
    									Config
    										Rb
    											Srb = True
    										TestMode
    											None = True
    								Rlc
    									Rb
    										AM
    											Tx
    												R8
    													t_PollRetransmit = ms45 (8)
    													pollPDU = pInfinity (7)
    													pollByte = kBinfinity (14)
    													maxRetxThreshold = t4 (3)
    											Rx
    												R8
    													t_Reordering = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    											ExtendedLI = Omit
    									TestMode
    										None = True
    								LogicalChannelId = 2
    								Mac
    									LogicalChannel
    										Priority = 3
    										PrioritizedBitRate = infinity_ (7)
    									TestMode
    										None = True
    								DiscardULData = Omit

    SYSTEM_CTRL_CNF:
    ↑	Received on port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_CNF
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				Result
    					Success = True
    			Confirm
    				RadioBearerList = True

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = True
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				UE_Cat_Info
    					ue_Category = 4
    					ue_Category_V1020 = 7
    					ue_Category_v1170 = 10
    					ue_Category_v11a0 = 12
    					ue_Category_v1250 = Omit
    					UE_CategoryUL_v1310 = Omit
    					UE_CategoryDL_v1310 = Omit

    SYSTEM_CTRL_CNF:
    ↑	Received on port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_CNF
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				Result
    					Success = True
    			Confirm
    				UE_Cat_Info = True

    UT_COMMON_CMD:
    ↓	Inter-component message: PTC_Ut -> MTC_LTE:PTC_Ut
    		Source = \Test Control\TTCN3
    		UT_COMMON_CMD
    			Cmd = SWITCH_ON (100)
    			CnfReq = CNF_REQUIRED (1)
    			ParameterList = Omit

    UT_SYSTEM_REQ:
    ↓	Sent from port: MTC_LTE:Ut
    		Source = \Test Control\TTCN3
    		UT_SYSTEM_REQ
    			Cmd
    				MMI
    					Cmd = 'SWITCH_ON'
    					ParameterList = Omit
    			CnfRequired = CNF_REQUIRED (1)

    UT_COMMON_CNF:
    ↑	Received on port: MTC_LTE:Ut
    		Source = \Test Control\TTCN3
    		UT_COMMON_CNF
    			Result = True
    			ResultString = Omit

    UT_COMMON_CNF:
    ↑	Inter-component message: UT -> EUTRA_PTC:UT
    		Source = \Test Control\TTCN3
    		UT_COMMON_CNF
    			Result = True
    			ResultString = Omit

    UT_COMMON_CMD:
    ↓	Inter-component message: PTC_Ut -> MTC_LTE:PTC_Ut
    		Source = \Test Control\TTCN3
    		UT_COMMON_CMD
    			Cmd = CONFIGURE_CEMODE (36)
    			CnfReq = CNF_REQUIRED (1)
    			ParameterList
    				Ut_Parameter_Type
    					Name = 'CE MODE'
    					Value = '3'

    UT_SYSTEM_REQ:
    ↓	Sent from port: MTC_LTE:Ut
    		Source = \Test Control\TTCN3
    		UT_SYSTEM_REQ
    			Cmd
    				AT = 'AT+CEMODE=3'
    			CnfRequired = CNF_REQUIRED (1)

    UT_COMMON_CNF:
    ↑	Received on port: MTC_LTE:Ut
    		Source = \Test Control\TTCN3
    		UT_COMMON_CNF
    			Result = True
    			ResultString = 'OK'

    UT_COMMON_CNF:
    ↑	Inter-component message: UT -> EUTRA_PTC:UT
    		Source = \Test Control\TTCN3
    		UT_COMMON_CNF
    			Result = True
    			ResultString = 'OK'

    UT_COMMON_CMD:
    ↓	Inter-component message: PTC_Ut -> MTC_LTE:PTC_Ut
    		Source = \Test Control\TTCN3
    		UT_COMMON_CMD
    			Cmd = SWITCH_OFF (99)
    			CnfReq = CNF_REQUIRED (1)
    			ParameterList = Omit

    UT_SYSTEM_REQ:
    ↓	Sent from port: MTC_LTE:Ut
    		Source = \Test Control\TTCN3
    		UT_SYSTEM_REQ
    			Cmd
    				MMI
    					Cmd = 'SWITCH_OFF'
    					ParameterList = Omit
    			CnfRequired = CNF_REQUIRED (1)

    UT_COMMON_CNF:
    ↑	Received on port: MTC_LTE:Ut
    		Source = \Test Control\TTCN3
    		UT_COMMON_CNF
    			Result = True
    			ResultString = Omit

    UT_COMMON_CNF:
    ↑	Inter-component message: UT -> EUTRA_PTC:UT
    		Source = \Test Control\TTCN3
    		UT_COMMON_CNF
    			Result = True
    			ResultString = Omit

    Timer Event:
    	Timer: t_GuardTimer, Duration: 180s, Started: 17:34:50
    		Source = \Test Control\TTCN3
    		timerEvent = 6
    		fileName = C:\CT_LTE\ETSI\v41_Dev\RC1\Final PSM MKS\LTE_A_R12_IWD_16wk37\Common\EUTRA\EUTRA_CommonProcedures.ttcn
    		testName = TC_9_2_1_1_7c
    		lineNo = 83
    		outStr = Timer: t_GuardTimer, Duration: 180s, Started: 17:34:50

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_Cell_NonSpecific (0)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = True
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				CellAttenuationList
    					CellAttenuationConfig_Type
    						CellId = eutra_CellA (16)
    						Attenuation
    							Value = 0
    						TimingInfo = Omit

    SYSTEM_CTRL_CNF:
    ↑	Received on port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_CNF
    			Common
    				CellId = eutra_Cell_NonSpecific (0)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				Result
    					Success = True
    			Confirm
    				CellAttenuationList = True

    IMS_IPCAN_Coordination_MSG:
    ↑	Inter-component message: IPCAN -> IMS_PTC:IPCAN
    		Source = \Test Control\TTCN3
    		IMS_IPCAN_Coordination_MSG
    			IPCAN_IMS_Control
    				Reset = True

    IP_ConfigReq_Type:
    ↓	Inter-component message: EUTRA_CTRL -> IP_PTC:EUTRA_CTRL
    		Source = \Test Control\TTCN3
    		IP_ConfigReq_Type
    			StartIP
    				PdnId = PDN_1 (0)
    				DrbInfo
    					Eutra
    						CellId = eutra_CellA (16)
    						DrbId = 1

    MATCH_MISMATCH:
    ↑	Message Mismatch: CharacterStringType
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: CharacterStringType
    		MATCH_MISMATCH
    			Message Mismatch: CharacterStringType
    				ServerAddr = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: CharacterStringType
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: CharacterStringType
    		MATCH_MISMATCH
    			Message Mismatch: CharacterStringType
    				ServerAddr = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: CharacterStringType
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: CharacterStringType
    		MATCH_MISMATCH
    			Message Mismatch: CharacterStringType
    				ServerAddr = Omit

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 67
    					Remote = Omit
    				Req
    					UDP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 67
    					Remote = Omit
    				Req
    					UDP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    MESSAGE_MISMATCH:
    ↑	Message Mismatch: IP_SOCKET_IND
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_SOCKET_IND
    		MESSAGE_MISMATCH
    			Message Mismatch: IP_SOCKET_IND
    				CTRL
    					ConnectionId
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 67
    						Remote
    							IpAddr = Omit
    							Port = Omit
    					Ind
    						UDP
    							SocketCnf = True

    IP_SOCKET_IND:
    ↑	Received on port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 67
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					UDP
    						SocketCnf = True

    IP_SOCKET_IND:
    ↑	Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 67
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					UDP
    						SocketCnf = True

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 67
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 53
    					Remote = Omit
    				Req
    					UDP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 53
    					Remote = Omit
    				Req
    					UDP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    MESSAGE_MISMATCH:
    ↑	Message Mismatch: IP_SOCKET_IND
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_SOCKET_IND
    		MESSAGE_MISMATCH
    			Message Mismatch: IP_SOCKET_IND
    				CTRL
    					ConnectionId
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 53
    						Remote
    							IpAddr = Omit
    							Port = Omit
    					Ind
    						UDP
    							SocketCnf = True

    IP_SOCKET_IND:
    ↑	Received on port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 53
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					UDP
    						SocketCnf = True

    IP_SOCKET_IND:
    ↑	Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 53
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					UDP
    						SocketCnf = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 67
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: CharacterStringType
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: CharacterStringType
    		MATCH_MISMATCH
    			Message Mismatch: CharacterStringType
    				ICMPv6_ServerAddress = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 53
    					Remote = Omit
    				Req
    					UDP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 53
    					Remote = Omit
    				Req
    					UDP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    MESSAGE_MISMATCH:
    ↑	Message Mismatch: IP_SOCKET_IND
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_SOCKET_IND
    		MESSAGE_MISMATCH
    			Message Mismatch: IP_SOCKET_IND
    				CTRL
    					ConnectionId
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 53
    						Remote
    							IpAddr = Omit
    							Port = Omit
    					Ind
    						UDP
    							SocketCnf = True

    IP_SOCKET_IND:
    ↑	Received on port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 53
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					UDP
    						SocketCnf = True

    IP_SOCKET_IND:
    ↑	Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 53
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					UDP
    						SocketCnf = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 67
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = icmpv6 (3)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = Omit
    					Remote = Omit
    				Req
    					ICMP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = icmpv6 (3)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = Omit
    					Remote = Omit
    				Req
    					ICMP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    MESSAGE_MISMATCH:
    ↑	Message Mismatch: IP_SOCKET_IND
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_SOCKET_IND
    		MESSAGE_MISMATCH
    			Message Mismatch: IP_SOCKET_IND
    				CTRL
    					ConnectionId
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote
    							IpAddr = Omit
    							Port = Omit
    					Ind
    						ICMP
    							SocketCnf = True

    IP_SOCKET_IND:
    ↑	Received on port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = icmpv6 (3)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = Omit
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					ICMP
    						SocketCnf = True

    IP_SOCKET_IND:
    ↑	Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = icmpv6 (3)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = Omit
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					ICMP
    						SocketCnf = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 67
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = icmpv6 (3)
    					Local
    						IpAddr
    							V6
    								Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = Omit
    					Remote = Omit
    				Req
    					ICMP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = icmpv6 (3)
    					Local
    						IpAddr
    							V6
    								Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = Omit
    					Remote = Omit
    				Req
    					ICMP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    MESSAGE_MISMATCH:
    ↑	Message Mismatch: IP_SOCKET_IND
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_SOCKET_IND
    		MESSAGE_MISMATCH
    			Message Mismatch: IP_SOCKET_IND
    				CTRL
    					ConnectionId
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote
    							IpAddr = Omit
    							Port = Omit
    					Ind
    						ICMP
    							SocketCnf = True

    IP_SOCKET_IND:
    ↑	Received on port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = icmpv6 (3)
    					Local
    						IpAddr
    							V6
    								Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = Omit
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					ICMP
    						SocketCnf = True

    IP_SOCKET_IND:
    ↑	Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = icmpv6 (3)
    					Local
    						IpAddr
    							V6
    								Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = Omit
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					ICMP
    						SocketCnf = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 67
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 5060
    					Remote = Omit
    				Req
    					UDP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 5060
    					Remote = Omit
    				Req
    					UDP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    MESSAGE_MISMATCH:
    ↑	Message Mismatch: IP_SOCKET_IND
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_SOCKET_IND
    		MESSAGE_MISMATCH
    			Message Mismatch: IP_SOCKET_IND
    				CTRL
    					ConnectionId
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote
    							IpAddr = Omit
    							Port = Omit
    					Ind
    						UDP
    							SocketCnf = True

    IP_SOCKET_IND:
    ↑	Received on port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 5060
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					UDP
    						SocketCnf = True

    IP_SOCKET_IND:
    ↑	Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 5060
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					UDP
    						SocketCnf = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 67
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 5060
    					Remote = Omit
    				Req
    					UDP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 5060
    					Remote = Omit
    				Req
    					UDP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    MESSAGE_MISMATCH:
    ↑	Message Mismatch: IP_SOCKET_IND
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_SOCKET_IND
    		MESSAGE_MISMATCH
    			Message Mismatch: IP_SOCKET_IND
    				CTRL
    					ConnectionId
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote
    							IpAddr = Omit
    							Port = Omit
    					Ind
    						UDP
    							SocketCnf = True

    IP_SOCKET_IND:
    ↑	Received on port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 5060
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					UDP
    						SocketCnf = True

    IP_SOCKET_IND:
    ↑	Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 5060
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					UDP
    						SocketCnf = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 67
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = tcp (1)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 5060
    					Remote = Omit
    				Req
    					TCP
    						Listen
    							SockOptList
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500
    							Application = ims (0)
    							TLSInfo = Omit

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = tcp (1)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 5060
    					Remote = Omit
    				Req
    					TCP
    						Listen
    							SockOptList
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500
    							Application = ims (0)
    							TLSInfo = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 67
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = tcp (1)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 5060
    					Remote = Omit
    				Req
    					TCP
    						Listen
    							SockOptList
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500
    							Application = ims (0)
    							TLSInfo = Omit

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = tcp (1)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 5060
    					Remote = Omit
    				Req
    					TCP
    						Listen
    							SockOptList
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500
    							Application = ims (0)
    							TLSInfo = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 67
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    IP_Indication_Type:
    ↑	Inter-component message: IP -> EUTRA_PTC:IP
    		Source = \Test Control\TTCN3
    		IP_Indication_Type
    			Cnf = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: Ut_CnfReq_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: Ut_CnfReq_Type
    		MATCH_MISMATCH
    			Message Mismatch: Ut_CnfReq_Type
    				Ut_CnfReq_Type = CNF_REQUIRED (1)

    MATCH_MISMATCH:
    ↑	Message Mismatch: Ut_CnfReq_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: Ut_CnfReq_Type
    		MATCH_MISMATCH
    			Message Mismatch: Ut_CnfReq_Type
    				Ut_CnfReq_Type = LOCAL_CNF_REQUIRED (2)

    MESSAGE_MISMATCH:
    ↑	Message Mismatch: IMS_CONFIG_REQ
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IMS_CONFIG_REQ
    		MESSAGE_MISMATCH
    			Message Mismatch: IMS_CONFIG_REQ
    				RegInfoRelease = True

    MESSAGE_MISMATCH:
    ↑	Message Mismatch: IMS_CONFIG_REQ
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IMS_CONFIG_REQ
    		MESSAGE_MISMATCH
    			Message Mismatch: IMS_CONFIG_REQ
    				RegInfoRelease = True

    MESSAGE_MISMATCH:
    ↑	Message Mismatch: IMS_CONFIG_REQ
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IMS_CONFIG_REQ
    		MESSAGE_MISMATCH
    			Message Mismatch: IMS_CONFIG_REQ
    				RegInfoRelease = True

    IMS_CONFIG_REQ:
    ↓	Inter-component message: IMS_CTRL -> IP_PTC:IMS_CTRL
    		Source = \Test Control\TTCN3
    		IMS_CONFIG_REQ
    			RegInfoRelease = True

    UT_COMMON_CMD:
    ↓	Inter-component message: PTC_Ut -> MTC_LTE:PTC_Ut
    		Source = \Test Control\TTCN3
    		UT_COMMON_CMD
    			Cmd = SWITCH_ON (100)
    			CnfReq = NO_CNF_REQUIRED (0)
    			ParameterList = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: Ut_CnfReq_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: Ut_CnfReq_Type
    		MATCH_MISMATCH
    			Message Mismatch: Ut_CnfReq_Type
    				Ut_CnfReq_Type = CNF_REQUIRED (1)

    MATCH_MISMATCH:
    ↑	Message Mismatch: Ut_CnfReq_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: Ut_CnfReq_Type
    		MATCH_MISMATCH
    			Message Mismatch: Ut_CnfReq_Type
    				Ut_CnfReq_Type = LOCAL_CNF_REQUIRED (2)

    IMS_CONFIG_CNF:
    ↑	Inter-component message: IMS_CTRL -> IMS_PTC:IMS_CTRL
    		Source = \Test Control\TTCN3
    		IMS_CONFIG_CNF
    			RegInfoRelease = True

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				Cell
    					AddOrReconfigure
    						Basic = Omit
    						Active
    							C_RNTI = Omit
    							PhysicalLayerConfigUL = Omit
    							RachProcedureConfig = Omit
    							CcchDcchDtchConfig
    								MeasGapCtrl = Omit
    								DL = Omit
    								UL
    									DciInfo
    										Imcs
    											Value = 9
    										TransRetransmissionList
    											UL_TransRetransmission_Type
    												NewTransmission = True
    										FreqDomainSchedul
    											FirstRbIndex = 0
    											Nprb = 25
    										RepetitionNumber = Omit
    									Hopping
    										Deactivated = True
    									PUCCH_Synch
    										None = True
    									UL_GrantConfig
    										OnSR_Reception = True
    								DrxCtrl = Omit
    								TtiBundling = Omit
    								CifPresence = Omit
    							ServingCellConfig = Omit
    							SciSchedulingConfig = Omit
    							EIMTA_Config = Omit
    							CE_Mode = Omit

    UT_SYSTEM_REQ:
    ↓	Sent from port: MTC_LTE:Ut
    		Source = \Test Control\TTCN3
    		UT_SYSTEM_REQ
    			Cmd
    				MMI
    					Cmd = 'SWITCH_ON'
    					ParameterList = Omit
    			CnfRequired = NO_CNF_REQUIRED (0)

    UL-CCCH-Message:
    	rrcConnectionRequest
    		Source = \Protocol\3GPP\LTE\RRC\
    		UL-CCCH-Message
    			message = c1 = rrcConnectionRequest =
    				criticalExtensions = rrcConnectionRequest-r8 =
    					ue-Identity = randomValue = 0010101111010111101111010011111010100011
    					establishmentCause = mo-Signalling
    					spare = 0
    ←------------------------------------------------------------------------------------------------------------
    UL-DCCH-Message:
    	rrcConnectionSetupComplete
    		Source = \Protocol\3GPP\LTE\RRC\
    		UL-DCCH-Message
    			message = c1 = rrcConnectionSetupComplete =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = c1 = rrcConnectionSetupComplete-r8 =
    					selectedPLMN-Identity = 1
    					dedicatedInfoNAS = 07417108091010103254769805F070C0401100290207D03127238080211001000010810600000000830600000000000D00000300000A000005000010005C0A003103E5E03E11035758A6200C601404EF65233B8878D2F28040080402600000021F00C16A01225E0160
    ←------------------------------------------------------------------------------------------------------------
    RRC_PDU_IND:
    ↑	Received on port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 0
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 281
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			RrcPdu
    				Ccch
    					message_
    						c1
    							rrcConnectionRequest
    								criticalExtensions
    									rrcConnectionRequest_r8
    										ue_Identity
    											randomValue = 0010101111010111101111010011111010100011'B
    										establishmentCause = mo_Signalling (3)
    										spare = 0'B

    SRB_COMMON_IND:
    ↑	Inter-component message: SRB -> EUTRA_PTC:SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 0
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 281
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Ccch
    						message_
    							c1
    								rrcConnectionRequest
    									criticalExtensions
    										rrcConnectionRequest_r8
    											ue_Identity
    												randomValue = 0010101111010111101111010011111010100011'B
    											establishmentCause = mo_Signalling (3)
    											spare = 0'B
    				Nas = Omit

    Attach Request:
    	Attach Request PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Attach Request
    			Security header type [4 bits] = 0x0 [ 0 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			Message Type [8 bits] = 0x41 - Attach Request [ 65 ]
    			NAS key set identifier
    				Type of security context flag [1 bit] = 0x0 [ 0 ]
    				key sequence indicator [3 bits] = 0x7 [ 7 ]
    			EPS attach type
    				Spare Bits [1 bit] = 0x0 [ 0 ]
    				Value [3 bits] = 0x1 [ 1 ]
    			EPS Mobile Identity
    				IE Length [8 bits] = 0x8 [ 8 ]
    				constant / IMSI Identity Digit 1 [4 bits] = 0x0 [ 0 ]
    				Odd / Even Indicator [1 bit] = 0x1 [ 1 ]
    				EPS Type of Identity [3 bits] = 0x1 - IMSI [ 1 ]
    				other IMSI Identity Digits = 0x10101032547698
    			UE network capability
    				IE Length [8 bits] = 0x5 [ 5 ]
    				eea0_128 [1 bit] = 0x1 [ 1 ]
    				eea1_128 [1 bit] = 0x1 [ 1 ]
    				eea2_128 [1 bit] = 0x1 [ 1 ]
    				eea3 [1 bit] = 0x1 [ 1 ]
    				eea4 [1 bit] = 0x0 [ 0 ]
    				eea5 [1 bit] = 0x0 [ 0 ]
    				eea6 [1 bit] = 0x0 [ 0 ]
    				eea7 [1 bit] = 0x0 [ 0 ]
    				eia0 [1 bit] = 0x0 [ 0 ]
    				eia1_128 [1 bit] = 0x1 [ 1 ]
    				eia2_128 [1 bit] = 0x1 [ 1 ]
    				eia3 [1 bit] = 0x1 [ 1 ]
    				eia4 [1 bit] = 0x0 [ 0 ]
    				eia5 [1 bit] = 0x0 [ 0 ]
    				eia6 [1 bit] = 0x0 [ 0 ]
    				eia7 [1 bit] = 0x0 [ 0 ]
    				uea0_7 [8 bits] = 0xC0 [ 192 ]
    				Ucs2 Treatment [1 bit] = 0x0 - The ME Has a Preference for the Default Alphabet Over UCS2 [ 0 ]
    				uia1_7 [7 bits] = 0x40 [ 64 ]
    				spare Bits_1 [2 bits] = 0x0 [ 0 ]
    				h245_ash [1 bit] = 0x0 [ 0 ]
    				acc_csfb [1 bit] = 0x1 [ 1 ]
    				lpp [1 bit] = 0x0 [ 0 ]
    				lcs [1 bit] = 0x0 [ 0 ]
    				xsr_vcc [1 bit] = 0x0 [ 0 ]
    				nf [1 bit] = 0x1 [ 1 ]
    			ESM message container
    				IE Length [16 bits] = 0x29 [ 41 ]
    				ESM message container contents = 0x0207D03127238080211001000010810600000000830600000000000D00000300000A00000500001000
    			DRX Parameter
    				IE Identifier [8 bits] = 0x5C [ 92 ]
    				split_code = 0x0A [ 10 ]
    				DRX cycle lengtn coeff and value for S1 mode [4 bits] = 0x0 [ 0 ]
    				Split on CCCH [1 bit] = 0x0 - Split PG Cycle on CCCH is Not Supported by the Mobile Station [ 0 ]
    				non-DRX timer [3 bits] = 0x0 [ 0 ]
    			MS Network Capability
    				IE Identifier [8 bits] = 0x31 [ 49 ]
    				IE Length [8 bits] = 0x3 [ 3 ]
    				Value
    					Gea1Bits
    						Gea1 [1 bit] = 0x1 [ 1 ]
    					SmCapabilitiesViaDedicatedChannels [1 bit] = 0x1 [ 1 ]
    					SmCapabilitiesViaGprsChannels [1 bit] = 0x1 [ 1 ]
    					Ucs2Support [1 bit] = 0x0 [ 0 ]
    					SsScreeningIndicator [2 bits] = 0x1 [ 1 ]
    					SolsaCapability [1 bit] = 0x0 [ 0 ]
    					Revision Level Indicator [1 bit] = 0x1 - The ME is Release '98 Onwards [ 1 ]
    					BSS Packet Flow Support [1 bit] = 0x1 - Mobile Station Does Support BSS Packet Flow Procedures [ 1 ]
    					ExtendedGeaBits
    						Gea2 [1 bit] = 0x1 [ 1 ]
    						Gea3 [1 bit] = 0x1 [ 1 ]
    						Gea4 [1 bit] = 0x0 [ 0 ]
    						Gea5 [1 bit] = 0x0 [ 0 ]
    						Gea6 [1 bit] = 0x0 [ 0 ]
    						Gea7 [1 bit] = 0x0 [ 0 ]
    					LcsVaCapability [1 bit] = 0x0 [ 0 ]
    					PsInterRatHoFromGeranToUtranIuModeCapability [1 bit] = 0x0 [ 0 ]
    					PsInterRatHoFromGeranToEUtranS1ModeCapability [1 bit] = 0x0 [ 0 ]
    					EmmCombinedProceduresCapability [1 bit] = 0x1 [ 1 ]
    					IsrSupport [1 bit] = 0x1 [ 1 ]
    					SrvccToGeranOrUtranCapability [1 bit] = 0x1 [ 1 ]
    					EpcCapability [1 bit] = 0x1 [ 1 ]
    					NfCapability [1 bit] = 0x1 [ 1 ]
    					GeranNetworkSharingCapability [1 bit] = 0x0 [ 0 ]
    					{ Spare Padding1 =
    					}
    			MS classmark 2
    				IE Identifier [8 bits] = 0x11 [ 17 ]
    				IE Length [8 bits] = 0x3 [ 3 ]
    				Spare Bits [1 bit] = 0x0 [ 0 ]
    				rev_level [2 bits] = 0x2 [ 2 ]
    				es_ind [1 bit] = 0x1 [ 1 ]
    				A5/1 Algorithm Supported [1 bit] = 0x0 - Encryption Algorithm A5/1 Available [ 0 ]
    				rf_pwr_capability [3 bits] = 0x7 [ 7 ]
    				spare2 [1 bit] = 0x0 [ 0 ]
    				ps_capability [1 bit] = 0x1 [ 1 ]
    				ss_ind [2 bits] = 0x1 [ 1 ]
    				sm_capability [1 bit] = 0x1 [ 1 ]
    				VBS Notification Reception [1 bit] = 0x0 - No VBS Capability or No Notifications Wanted [ 0 ]
    				Voice Group Call Service [1 bit] = 0x0 - No VGCS capability or no notifications wanted [ 0 ]
    				Frequency Capability  [1 bit] = 0x0 - The MS does Not Support the E-GSM or R-GSM  Band [ 0 ]
    				Classmark 3 Indicator [1 bit] = 0x1 - The MS Supports Options that are Indicated in Classmark 3 IE [ 1 ]
    				spare3 [1 bit] = 0x0 [ 0 ]
    				LCS Value Added Capability [1 bit] = 0x1 - Location Request Notification via CS domain Supported [ 1 ]
    				vcs_2 [1 bit] = 0x0 [ 0 ]
    				so_lsa [1 bit] = 0x0 [ 0 ]
    				CM Service Prompt [1 bit] = 0x1 - Network Initiated MO CM Connection Request Supported for Atleast One CM Protocol [ 1 ]
    				A5/3 Algorithm Supported [1 bit] = 0x1 - Encryption Algorithm A5/3 Available [ 1 ]
    				A5/2 Algorithm Supported [1 bit] = 0x0 - Encryption Algorithm A5/2 Not Available [ 0 ]
    			MS classmark 3
    				IE Identifier [8 bits] = 0x20 [ 32 ]
    				IE Length [8 bits] = 0xC [ 12 ]
    				SpareBit [1 bit] = 0x0 [ 0 ]
    				{ 110
    					A5Bits6
    						A57 [1 bit] = 0x0 - Encryption Algorithm A5/7 not Available [ 0 ]
    						A56 [1 bit] = 0x0 - Encryption Algorithm A5/6 not Available [ 0 ]
    						A55 [1 bit] = 0x0 - Encryption algorithm A5/5 not available [ 0 ]
    						A54 [1 bit] = 0x0 [ 0 ]
    					Associated Radio Capability26 [4 bits] = 0x1 [ 1 ]
    					Associated Radio Capability16 [4 bits] = 0x4 [ 4 ]
    				}
    				{ 0
    				}
    				{ 0
    				}
    				{ UCS2 Treatment [1 bit] = 0x0 - The ME has a Preference for the Default Alphabet Over UCS2 [ 0 ]
    				}
    				{ Extended Measurement Capability [1 bit] = 0x0 - The MS Does Not Support Extended Measurements [ 0 ]
    				}
    				{ 0
    				}
    				{ 1
    					MS Positioning Method Capability
    						MS Positioning Method [5 bits] = 0x7 [ 7 ]
    				}
    				{ 0
    				}
    				{ 1
    					EcsdStruct
    						Modulation Capability [1 bit] = 0x1 - 8-PSK Supported for Uplink Transmission and Downlink Reception [ 1 ]
    						{ 1
    							EcsdRfPowerCapability1 [2 bits] = 0x2 [ 2 ]
    						}
    						{ 1
    							EcsdRfPowerCapability2 [2 bits] = 0x2 [ 2 ]
    						}
    				}
    				{ 0
    				}
    				{ 1
    					GSM 850 Associated Radio Capability [4 bits] = 0x4 [ 4 ]
    				}
    				{ 1
    					PCS 1900 Associated Radio Capability [4 bits] = 0x1 [ 1 ]
    				}
    				{ UMTS FDD Access Technology Capability [1 bit] = 0x1 - Supported [ 1 ]
    				}
    				{ UMTS TDD Access Technology Capability [1 bit] = 0x0 - UMTS 3.84 Mcps TDD Not Supported [ 0 ]
    				}
    				{ CDMA 2000 Radio Access Technology Capability [1 bit] = 0x0 - Not Supported [ 0 ]
    				}
    				{ 1
    					DTM GPRS Multi Slot Subclass [2 bits] = 0x3 - Multislot Class 11 Supported [ 3 ]
    					Single Slot DTM [1 bit] = 0x0 [ 0 ]
    					{ 1
    						DtmEgprsMultiSlotSubClass [2 bits] = 0x3 [ 3 ]
    					}
    				}
    				{ 0
    				}
    				{ 0
    				}
    				{ Umts128McpsTddRadioAccessTechnologyCapability [1 bit] = 0x0 [ 0 ]
    				}
    				{ GERAN Feature Package 1 [1 bit] = 0x1 - Supported [ 1 ]
    				}
    				{ 0
    				}
    				{ 0
    				}
    				{ GERAN Feature Package 2 [1 bit] = 0x0 - Not supported [ 0 ]
    				}
    				{ GMSK Multislot Power Profile [2 bits] = 0x3 - GMSK_MULTISLOT_POWER_PROFILE 3 [ 3 ]
    				}
    				{ 8-PSK Multislot Power Profile [2 bits] = 0x3 - 8-PSK_MULTISLOT_POWER_PROFILE 3 [ 3 ]
    				}
    				{ 0
    				}
    				{ Downlink Advanced Receiver Performance [2 bits] = 0x1 - Downlink Advanced Receiver Performance - phase I supported [ 1 ]
    				}
    				{ DTM Enhancements Capability [1 bit] = 0x1 - The mobile station supports enhanced DTM CS establishment and enhanced DTM CS release procedures [ 1 ]
    				}
    				{ 0
    				}
    				{ RepeatedAcchCapability [1 bit] = 0x1 [ 1 ]
    				}
    				{ 0
    				}
    				{ 0
    				}
    				{ CipheringModeSettingCapability [1 bit] = 0x1 [ 1 ]
    				}
    				{ AdditionalPositioningCapabilities [1 bit] = 0x0 [ 0 ]
    				}
    				{ EUtraFddSupport [1 bit] = 0x1 [ 1 ]
    				}
    				{ EUtraTddSupport [1 bit] = 0x1 [ 1 ]
    				}
    				{ EUtraMeasurementAndReportingSupport [1 bit] = 0x1 [ 1 ]
    				}
    				{ PriorityBasedReselectionSupport [1 bit] = 0x1 [ 1 ]
    				}
    				{ UtraCsgCellsReporting [1 bit] = 0x0 [ 0 ]
    				}
    				{ Vamos Level [2 bits] = 0x1 - VAMOS I supported [ 1 ]
    				}
    				{ Tighter Capability [2 bits] = 0x1 - TIGHTER supported for speech and signalling channels only [ 1 ]
    				}
    				{ Selective Ciphering Of Downlink SACCH [1 bit] = 0x0 - Selective Ciphering of Downlink SACCH not supported [ 0 ]
    				}
    				{ CsToPsSrvccFromGeranToUtra [2 bits] = 0x0 [ 0 ]
    				}
    				{ CsToPsSrvccFromGeranToEUtra [2 bits] = 0x0 [ 0 ]
    				}
    				{ GeranNetworkSharingSupport [1 bit] = 0x0 [ 0 ]
    				}
    				{ EUtraWidebandRsrqMeasurementsSupport [1 bit] = 0x0 [ 0 ]
    				}
    				N Spare Bits1 =
    			Supported codecs
    				IE Identifier [8 bits] = 0x40 [ 64 ]
    				IE Length [8 bits] = 0x8 [ 8 ]
    				system identification 1 = 0x04 [ 4 ]
    				Length Of Bitmap for SysID 1 = 0x02 [ 2 ]
    				codec bitmap sysID 1_b1_b8 = 0x60 [ 96 ]
    				codec bitmap sysID1_b9_b16 = 0x00 [ 0 ]
    				system identification 2 = 0x00 [ 0 ]
    				Length Of Bitmap for SysID 2 = 0x02 [ 2 ]
    				codec bitmap sysID2_b1_b8 = 0x1F [ 31 ]
    				codec bitmap sysID2_b9_b16 = 0x00 [ 0 ]
    			ms_nfs
    				IE Identifier [4 bits] = 0xC [ 12 ]
    				Spare Bits [3 bits] = 0x0 [ 0 ]
    				ext_prio_timer [1 bit] = 0x1 [ 1 ]
    			t3324_value
    				IE Identifier [8 bits] = 0x6A [ 106 ]
    				IE Length [8 bits] = 0x1 [ 1 ]
    				Timer Value Unit [3 bits] = 0x1 - Value is Incremented in Multiples of 1 Minute  [ 1 ]
    				Value [5 bits] = 0x2 [ 2 ]
    			t3412_ext_val
    				IE Identifier [8 bits] = 0x5E [ 94 ]
    				IE Length [8 bits] = 0x1 [ 1 ]
    				Timer Value Unit [3 bits] = 0x3 - value is incremented in multiples of 2 seconds [ 3 ]
    				Value [5 bits] = 0x0 [ 0 ]
    ←------------------------------------------------------------------------------------------------------------
    PDN Connectivity Request:
    	PDN Connectivity Request PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		PDN Connectivity Request
    			EPS bearer identity [4 bits] = 0x0 [ 0 ]
    			Protocol Discriminator [4 bits] = 0x2 - EPS Session Management Messages [ 2 ]
    			Procedure transaction identifier [8 bits] = 0x7 [ 7 ]
    			Message Type [8 bits] = 0xD0 - PDN Connectivity Request [ 208 ]
    			PDN type
    				Spare Bits [1 bit] = 0x0 [ 0 ]
    				Value [3 bits] = 0x3 [ 3 ]
    			Request type
    				Spare Bits [1 bit] = 0x0 [ 0 ]
    				Value [3 bits] = 0x1 [ 1 ]
    			Protocol Configuration Options
    				IE Identifier [8 bits] = 0x27 [ 39 ]
    				IE Length [8 bits] = 0x23 [ 35 ]
    				Extension Bit [1 bit] = 0x1 - Outgoing Calls Barred within CUG [ 1 ]
    				Spare Bits [4 bits] = 0x0 [ 0 ]
    				Configuration Protocol [3 bits] = 0x0 - PPP for Use with IP PDP Type [ 0 ]
    				Option1
    					Identifier = 0x8021 - Internet Protocol Control Protocol [ 32801 ]
    					Length [8 bits] = 0x10 [ 16 ]
    					value = 0x01000010810600000000830600000000
    				Option2
    					Identifier = 0x000D [ 13 ]
    					Length [8 bits] = 0x0 [ 0 ]
    				Option3
    					Identifier = 0x0003 - DNS Server Address Request [ 3 ]
    					Length [8 bits] = 0x0 [ 0 ]
    				Option4
    					Identifier = 0x000A [ 10 ]
    					Length [8 bits] = 0x0 [ 0 ]
    				Option5
    					Identifier = 0x0005 [ 5 ]
    					Length [8 bits] = 0x0 [ 0 ]
    				Option6
    					Identifier = 0x0010 [ 16 ]
    					Length [8 bits] = 0x0 [ 0 ]
    ←------------------------------------------------------------------------------------------------------------
    RRC_PDU_IND:
    ↑	Received on port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 284
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							rrcConnectionSetupComplete
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									c1
    										rrcConnectionSetupComplete_r8
    											selectedPLMN_Identity = 1
    											registeredMME = Omit
    											dedicatedInfoNAS = '07417108091010103254769805F070C0401100290207D03127238080211001000010810600000000830600000000000D00000300000A000005000010005C0A003103E5E03E11035758A6200C601404EF65233B8878D2F28040080402600000021F00C16A01225E0160'O
    											nonCriticalExtension = Omit

    SRB_COMMON_IND:
    ↑	Inter-component message: SRB -> EUTRA_PTC:SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 284
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Dcch
    						message_
    							c1
    								rrcConnectionSetupComplete
    									rrc_TransactionIdentifier = 0
    									criticalExtensions
    										c1
    											rrcConnectionSetupComplete_r8
    												selectedPLMN_Identity = 1
    												registeredMME = Omit
    												dedicatedInfoNAS = '07417108091010103254769805F070C0401100290207D03127238080211001000010810600000000830600000000000D00000300000A000005000010005C0A003103E5E03E11035758A6200C601404EF65233B8878D2F28040080402600000021F00C16A01225E0160'O
    												nonCriticalExtension = Omit
    				Nas
    					NasIndication
    						SecurityProtection
    							Status = 0000'B
    							NasCount = '00FFFFFF'O
    						Pdu
    							Msg
    								aTTACH_REQUEST
    									securityHeaderType = 0000'B
    									protocolDiscriminator = 0111'B
    									messageType = 01000001'B
    									nasKeySetId
    										iei = Omit
    										tsc = 0'B
    										nasKeySetId = 111'B
    									epsAttachType
    										spare = 0'B
    										typeValue = 001'B
    									epsMobileIdentity
    										iei = Omit
    										iel = '08'O
    										idDigit1 = 0000'B
    										oddEvenInd = 1'B
    										typeOfId = 001'B
    										otherDigits = '10101032547698'O
    									ueNetworkCapability
    										iei = Omit
    										iel = '05'O
    										eeaCap = 'F0'O
    										eiaCap = '70'O
    										ueaCap = 'C0'O
    										uiaCap = '40'O
    										srvcc_LPP_ProSeCap = '11'O
    										cIoT_proSeCap = Omit
    										spare = Omit
    									esmMessage
    										iei = Omit
    										iel = '0029'O
    										esmPdu = '0207D03127238080211001000010810600000000830600000000000D00000300000A00000500001000'O
    									oldPtmsiSignature = Omit
    									additionalGuti = Omit
    									lastVisitedRegisteredTai = Omit
    									drxParameter
    										iei = '5C'O
    										splitPGcycleCode = 00001010'B
    										cnDRXcoef = 0000'B
    										splitOnCCCH = 0'B
    										nonDRXtimer = 000'B
    									msNetworkCapability
    										iei = '31'O
    										iel = '03'O
    										gea1 = 1'B
    										smCapDedicated = 1'B
    										smCapGPRS = 1'B
    										ucs2 = 0'B
    										ssScreeningIndicator = 01'B
    										soLSACap = 0'B
    										revLevelIndicator = 1'B
    										pfcFeatureMode = 1'B
    										gea2 = 1'B
    										gea3 = 1'B
    										gea4 = 0'B
    										gea5 = 0'B
    										gea6 = 0'B
    										gea7 = 0'B
    										lcsVACap = 0'B
    										psHOtoUTRAN_IuModeCap = 0'B
    										psHOtoEUTRAN_S1ModeCap = 0'B
    										emmCombinedCap = 1'B
    										isrSupport = 1'B
    										srvccToGERAN_UTRANCap = 1'B
    										epcCap = 1'B
    										nfCap = 1'B
    										gERANNtwkShareCap = 0'B
    										userPlaneIntegrityProtSupport = Omit
    										gia4 = Omit
    										gia5 = Omit
    										gia6 = Omit
    										gia7 = Omit
    										spareBits = Omit
    									oldLai = Omit
    									tmsiStatus = Omit
    									msClassmark2
    										iei = '11'O
    										iel = '03'O
    										spare1_1 = 0'B
    										revLvl = 10'B
    										eSIND = 1'B
    										a5_1 = 0'B
    										rFPwrCap = 111'B
    										spare1_2 = 0'B
    										pSCap = 1'B
    										sSSI = 01'B
    										sMCap = 1'B
    										vBS = 0'B
    										vGCS = 0'B
    										fC = 0'B
    										cM3 = 1'B
    										spare1_3 = 0'B
    										lCSVA = 1'B
    										uCS2 = 0'B
    										soLSA = 0'B
    										cMSP = 1'B
    										a5_3 = 1'B
    										a5_2 = 0'B
    									msClassmark3
    										iei = '20'O
    										iel = '0C'O
    										spareBit = 0'B
    										multibandSupported = 110'B
    										a5_7 = 0'B
    										a5_6 = 0'B
    										a5_5 = 0'B
    										a5_4 = 0'B
    										associatedRadioCapabilty2 = 0001'B
    										spareBits1 = Omit
    										associatedRadioCapabilty1 = 0100'B
    										maskBit1 = 0'B
    										rGSM_RadioCapability = Omit
    										maskBit2 = 0'B
    										multiSlotClass = Omit
    										uCS2Treatment = 0'B
    										extMeasurementCapability = 0'B
    										maskBit3 = 0'B
    										msMeasurementCapability = Omit
    										maskBit4 = 1'B
    										msPositioningMethod = 00111'B
    										maskBit5 = 0'B
    										eDGE_MultiSlot = Omit
    										maskBit6 = 1'B
    										psk8_Struct
    											modulationCapability = 1'B
    											pwrMask1 = 1'B
    											eDGE_RF_PowerCapability1 = 10'B
    											pwrMask2 = 1'B
    											eDGE_RF_PowerCapability2 = 10'B
    										maskBit7 = 0'B
    										gSM400BandsSupported = Omit
    										gSM400AssociatedRadioCapability = Omit
    										maskBit8 = 1'B
    										gSM850AssociatedRadiioCapability = 0100'B
    										maskBit9 = 1'B
    										pCS1900AssociatedRadiioCapability = 0001'B
    										uMTS_FDD_RAT_Capability = 1'B
    										uMTS384TDD_RAT_Capability = 0'B
    										cDMA2000_RAT_Capability = 0'B
    										maskBit10 = 1'B
    										dTM_GPRS_MultiSlotSubclass = 11'B
    										singleSlotDTM = 0'B
    										maskBit11 = 1'B
    										dTM_EGPRS_MultiSlorSubclass = 11'B
    										maskBit12 = 0'B
    										singleBandSupport = Omit
    										maskBit13 = 0'B
    										gSM700AssociatedRadioCapability = Omit
    										uMTS128TDD_RAT_Capability = 0'B
    										gERANFeatPack1 = 1'B
    										mask14 = 0'B
    										extDTM_GPRS_MultiSlotSubclass = Omit
    										etxDTM_EGPRS_MultiSlotSubclass = Omit
    										mask15 = 0'B
    										highMultislotCap = Omit
    										spare2 = 0'B
    										gERANFeatPack2 = 0'B
    										gMSKMultislotPowerProfile = 11'B
    										pSKMultislotPowerProfile = 11'B
    										mask17 = 0'B
    										tGSM400BandsSupported = Omit
    										tGSM400AssocRadioCap = Omit
    										spare = 0'B
    										dlAdvancedRxPerf = 01'B
    										dTMEhancCap = 1'B
    										mask19 = 0'B
    										dTMGPRSHighMultislotClass = Omit
    										offsetReq = Omit
    										mask20 = Omit
    										dTMEGPRSHighMultislotClass = Omit
    										rptdACCHCap = 1'B
    										mask21 = 0'B
    										gsm710AssocRadioCap = Omit
    										mask22 = 0'B
    										tgsm810AssocRadioCap = Omit
    										cipheringModeSettingCap = 1'B
    										addPositionCap = 0'B
    										eutraFDDSupport = 1'B
    										eutraTDDSupport = 1'B
    										eutraMeasAndReporting = 1'B
    										priorityBasedReselection = 1'B
    										utraCSGCellsReporting = 0'B
    										vamosLevel = 01'B
    										tighterCap = 01'B
    										selectCipheringDLSACCH = 0'B
    										csPS_SRVCC_G2U = Omit
    										csPS_SRVCC_G2E = Omit
    										geranNwkSharing = Omit
    										eutraWidebandRSRQMeas = Omit
    										erBandSupport = Omit
    										utraMultipleFreqBandInd = Omit
    										eutraMultipleFreqBandInd = Omit
    										xtdTSCSetCap = Omit
    										xtdEARFCNValueRange = Omit
    										spareBits2 = 000000'B
    									supportedCodecList
    										iei = '40'O
    										iel = '08'O
    										codec
    											Codec
    												sysId = '04'O
    												len = '02'O
    												bitMap1to8 = 01100000'B
    												bitMap9to16 = 00000000'B
    											Codec
    												sysId = '00'O
    												len = '02'O
    												bitMap1to8 = 00011111'B
    												bitMap9to16 = 00000000'B
    									addUpdateType = Omit
    									voiceDomainPref = Omit
    									deviceProperties = Omit
    									oldGUTI_Type = Omit
    									msNetworkFeatureSupport
    										iei = 'C'H
    										spare = 000'B
    										extdPeriodicTimers = 1'B
    									tmsiBasedNRIContainer = Omit
    									t3324Value
    										iei = '6A'O
    										iel = '01'O
    										unit = 001'B
    										gprsTimerValue = 00010'B
    									t3412ExtdValue
    										iei = '5E'O
    										iel = '01'O
    										unit = 011'B
    										gprsTimerValue = 00000'B
    									extendedDRXParams = Omit
    							PiggybackedPduList
    								NAS_UL_Pdu_Type
    									Msg
    										pDN_CONNECTIVITY_REQUEST
    											epsBearerId = '0'H
    											protocolDiscriminator = 0010'B
    											procedureTransactionIdentifier = '07'O
    											messageType = 11010000'B
    											pdnType
    												spare = 0'B
    												typeValue = 011'B
    											requestType
    												spare = 0'B
    												typeValue = 001'B
    											esmInfoTransferFlag = Omit
    											accessPointName = Omit
    											protocolConfigurationOptions
    												iei = '27'O
    												iel = '23'O
    												ext = 1'B
    												spare = 0000'B
    												configProtocol = 000'B
    												pco
    													ProtocolContainer
    														protocolID = '8021'O
    														protocolLength = '10'O
    														content = '01000010810600000000830600000000'O
    													ProtocolContainer
    														protocolID = '000D'O
    														protocolLength = '00'O
    														content = Omit
    													ProtocolContainer
    														protocolID = '0003'O
    														protocolLength = '00'O
    														content = Omit
    													ProtocolContainer
    														protocolID = '000A'O
    														protocolLength = '00'O
    														content = Omit
    													ProtocolContainer
    														protocolID = '0005'O
    														protocolLength = '00'O
    														content = Omit
    													ProtocolContainer
    														protocolID = '0010'O
    														protocolLength = '00'O
    														content = Omit
    											deviceProperties = Omit
    											nbifomContainer = Omit
    											headerCompressionConfig = Omit
    											extdProtocolConfigurationOptions = Omit
    									PiggybackedPduList = Omit

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = True
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				Cell
    					AddOrReconfigure
    						Basic = Omit
    						Active
    							C_RNTI = Omit
    							PhysicalLayerConfigUL = Omit
    							RachProcedureConfig = Omit
    							CcchDcchDtchConfig
    								MeasGapCtrl = Omit
    								DL = Omit
    								UL
    									DciInfo = Omit
    									Hopping
    										Deactivated = True
    									PUCCH_Synch
    										Auto
    											TimingAdvance = 31
    											TA_Period = 600
    											TA_Repetition
    												Continuous = True
    									UL_GrantConfig = Omit
    								DrxCtrl = Omit
    								TtiBundling = Omit
    								CifPresence = Omit
    							ServingCellConfig = Omit
    							SciSchedulingConfig = Omit
    							EIMTA_Config = Omit
    							CE_Mode = Omit

    SYSTEM_CTRL_CNF:
    ↑	Received on port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_CNF
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				Result
    					Success = True
    			Confirm
    				Cell = True

    SRB_COMMON_REQ:
    ↓	Inter-component message: TC_SRB -> NASEMU_LTE_PTC:TC_SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Signalling
    				Rrc = Omit
    				Nas
    					NAS_MSG_Request_Type
    						SecurityProtection
    							Status = 0000'B
    							ForceMacError = False
    						Pdu
    							Msg
    								aUTHENTICATION_REQUEST
    									securityHeaderType = 0000'B
    									protocolDiscriminator = 0111'B
    									messageType = 01010010'B
    									spareHalfOctet = '0'H
    									asmeNasKeySetId
    										iei = Omit
    										tsc = 0'B
    										nasKeySetId = 000'B
    									rand
    										iei = Omit
    										randValue = 10100011110111100000110001101101001101100011111000110000110000110110010010100100000001111000111100011011111110001101010101110111'B
    									autn
    										iei = Omit
    										iel = '10'O
    										aUTN = 01101110001100100011101100110110110001000110110010000000000000001010001111011111000011100110111000110010001110111011011011000100'B
    							PiggybackedPduList = Omit

    DL-DCCH-Message:
    	dlInformationTransfer
    		Source = \Protocol\3GPP\LTE\RRC\
    		DL-DCCH-Message
    			message = c1 = dlInformationTransfer =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = c1 = dlInformationTransfer-r8 =
    					dedicatedInfoType = dedicatedInfoNAS = 075200A3DE0C6D363E30C364A4078F1BF8D577106E323B36C46C8000A3DF0E6E323BB6C4
    ------------------------------------------------------------------------------------------------------------→
    Authentication Request:
    	Authentication Request PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Authentication Request
    			Security header type [4 bits] = 0x0 [ 0 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			Message Type [8 bits] = 0x52 - Authentication Request [ 82 ]
    			Spare Half Octet [4 bits] = 0x0 [ 0 ]
    			NAS key set identifierASME
    				Type of security context flag [1 bit] = 0x0 [ 0 ]
    				key sequence indicator [3 bits] = 0x0 [ 0 ]
    				Authentication parameter random = 0xA3DE0C6D363E30C364A4078F1BF8D577
    			Authentication Parameter AUTN
    				IE Length [8 bits] = 0x10 [ 16 ]
    				value = 0x6E323B36C46C8000A3DF0E6E323BB6C4
    ------------------------------------------------------------------------------------------------------------→
    RRC_PDU_REQ:
    ↓	Sent from port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							dlInformationTransfer
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									c1
    										dlInformationTransfer_r8
    											dedicatedInfoType
    												dedicatedInfoNAS = '075200A3DE0C6D363E30C364A4078F1BF8D577106E323B36C46C8000A3DF0E6E323BB6C4'O
    											nonCriticalExtension = Omit

    UL-DCCH-Message:
    	ulInformationTransfer
    		Source = \Protocol\3GPP\LTE\RRC\
    		UL-DCCH-Message
    			message = c1 = ulInformationTransfer =
    				criticalExtensions = c1 = ulInformationTransfer-r8 =
    					dedicatedInfoType = dedicatedInfoNAS = 075308A3DF0E6E323B36C4
    ←------------------------------------------------------------------------------------------------------------
    Authentication Response:
    	Authentication Response PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Authentication Response
    			Security header type [4 bits] = 0x0 [ 0 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			Message Type [8 bits] = 0x53 - Authentication Response [ 83 ]
    			Authentication response parameter
    				IE Length [8 bits] = 0x8 [ 8 ]
    				Authentication response parameter information = 0x235F0E6E323B3644
    ←------------------------------------------------------------------------------------------------------------
    Ciphered NAS Message UL:
    	Ciphered NAS Message UL PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Ciphered NAS Message =
    			0x6E323B3644
    ←------------------------------------------------------------------------------------------------------------
    RRC_PDU_IND:
    ↑	Received on port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 328
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							ulInformationTransfer
    								criticalExtensions
    									c1
    										ulInformationTransfer_r8
    											dedicatedInfoType
    												dedicatedInfoNAS = '075308A3DF0E6E323B36C4'O
    											nonCriticalExtension = Omit

    SRB_COMMON_IND:
    ↑	Inter-component message: SRB -> EUTRA_PTC:SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 328
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			Signalling
    				Rrc = Omit
    				Nas
    					NasIndication
    						SecurityProtection
    							Status = 0000'B
    							NasCount = '00FFFFFF'O
    						Pdu
    							Msg
    								aUTHENTICATION_RESPONSE
    									securityHeaderType = 0000'B
    									protocolDiscriminator = 0111'B
    									messageType = 01010011'B
    									authenticationResponseParameter
    										iei = Omit
    										iel = '08'O
    										res = 1010001111011111000011100110111000110010001110110011011011000100'B
    							PiggybackedPduList = Omit

    NAS_CTRL_REQ:
    ↓	Inter-component message: CTRL -> NASEMU_LTE_PTC:CTRL
    		Source = \Test Control\TTCN3
    		NAS_CTRL_REQ
    			Common
    				ControlInfo
    					CnfFlag = True
    			Request
    				Security
    					StartRestart
    						Integrity
    							Algorithm = 001'B
    							K_NAS = 01101111111110011000110110100011010010100010110100011011110001100010101010100110110101001011101100011010011000101010011001100100'B
    						Ciphering
    							Algorithm = 001'B
    							K_NAS = 00110010100110111011010001000010000101000111011000010111000110011110011011000000000100000101011110100001010001000001111110100001'B
    						NasCountReset = True

    NAS_CTRL_CNF:
    ↑	Inter-component message: NASCTRL -> EUTRA_PTC:NASCTRL
    		Source = \Test Control\TTCN3
    		NAS_CTRL_CNF
    			Common
    			Confirm
    				Security = True

    SRB_COMMON_REQ:
    ↓	Inter-component message: TC_SRB -> NASEMU_LTE_PTC:TC_SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Signalling
    				Rrc = Omit
    				Nas
    					NAS_MSG_Request_Type
    						SecurityProtection
    							Status = 0011'B
    							ForceMacError = False
    						Pdu
    							Msg
    								sECURITY_MODE_COMMAND
    									securityHeaderType = 0000'B
    									protocolDiscriminator = 0111'B
    									messageType = 01011101'B
    									nasSecurityAlgorithms
    										iei = Omit
    										spare1 = 0'B
    										cipheringType = 001'B
    										spare2 = 0'B
    										integrityType = 001'B
    									spareHalfOctet = '0'H
    									asmeNasKeySetId
    										iei = Omit
    										tsc = 0'B
    										nasKeySetId = 000'B
    									replayedSecurityCapability
    										iel = '05'O
    										eeaCap = 'F0'O
    										eiaCap = '70'O
    										ueaCap = 'C0'O
    										uiaCap = '40'O
    										geaCap = '70'O
    									imeisvRequest = Omit
    									replayedNonceUe = Omit
    									nonceMme = Omit
    							PiggybackedPduList = Omit

    DL-DCCH-Message:
    	dlInformationTransfer
    		Source = \Protocol\3GPP\LTE\RRC\
    		DL-DCCH-Message
    			message = c1 = dlInformationTransfer =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = c1 = dlInformationTransfer-r8 =
    					dedicatedInfoType = dedicatedInfoNAS = 37513B372000075D110005F070C04070
    ------------------------------------------------------------------------------------------------------------→
    Security Protected NAS Message DL:
    	Security Protected NAS Message DL PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Security Protected NAS Message
    			Security header type [4 bits] = 0x3 [ 3 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			MAC = 0x513B3720 [ 1362835232 ]
    			Sequence Number = 0x00 [ 0 ]
    			NAS message = 0x075D110005F070C04070
    ------------------------------------------------------------------------------------------------------------→
    Security Mode Command:
    	Security Mode Command PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Security Mode Command
    			Security header type [4 bits] = 0x0 [ 0 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			Message Type [8 bits] = 0x5D - Security Mode Command [ 93 ]
    			Selected NAS security algorithms
    				Spare Bits [1 bit] = 0x0 [ 0 ]
    				Type of ciphering algorithm [3 bits] = 0x1 [ 1 ]
    				spare Bits_1 [1 bit] = 0x0 [ 0 ]
    				Type of integrity protection algorithm [3 bits] = 0x1 [ 1 ]
    			Spare Half Octet [4 bits] = 0x0 [ 0 ]
    			NAS key set identifierASME
    				Type of security context flag [1 bit] = 0x0 [ 0 ]
    				key sequence indicator [3 bits] = 0x0 [ 0 ]
    			Replayed UE security capabilities
    				IE Length [8 bits] = 0x5 [ 5 ]
    				eea0_128 [1 bit] = 0x1 [ 1 ]
    				eea1_128 [1 bit] = 0x1 [ 1 ]
    				eea2_128 [1 bit] = 0x1 [ 1 ]
    				eea3 [1 bit] = 0x1 [ 1 ]
    				eea4 [1 bit] = 0x0 [ 0 ]
    				eea5 [1 bit] = 0x0 [ 0 ]
    				eea6 [1 bit] = 0x0 [ 0 ]
    				eea7 [1 bit] = 0x0 [ 0 ]
    				Spare Bits [1 bit] = 0x0 [ 0 ]
    				eia1_128 [1 bit] = 0x1 [ 1 ]
    				eia2_128 [1 bit] = 0x1 [ 1 ]
    				eia3 [1 bit] = 0x1 [ 1 ]
    				eia4 [1 bit] = 0x0 [ 0 ]
    				eia5 [1 bit] = 0x0 [ 0 ]
    				eia6 [1 bit] = 0x0 [ 0 ]
    				eia7 [1 bit] = 0x0 [ 0 ]
    				uea0_7 [8 bits] = 0xC0 [ 192 ]
    				spare Bits_1 [1 bit] = 0x0 [ 0 ]
    				uia1_7 [7 bits] = 0x40 [ 64 ]
    				spare2 [1 bit] = 0x0 [ 0 ]
    				gea1_7 [7 bits] = 0x70 [ 112 ]
    ------------------------------------------------------------------------------------------------------------→
    RRC_PDU_REQ:
    ↓	Sent from port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							dlInformationTransfer
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									c1
    										dlInformationTransfer_r8
    											dedicatedInfoType
    												dedicatedInfoNAS = '37513B372000075D110005F070C04070'O
    											nonCriticalExtension = Omit

    UL-DCCH-Message:
    	ulInformationTransfer
    		Source = \Protocol\3GPP\LTE\RRC\
    		UL-DCCH-Message
    			message = c1 = ulInformationTransfer =
    				criticalExtensions = c1 = ulInformationTransfer-r8 =
    					dedicatedInfoType = dedicatedInfoNAS = 4765DF4F7D000022
    ←------------------------------------------------------------------------------------------------------------
    Security Protected NAS Message UL:
    	Security Protected NAS Message UL PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Security Protected NAS Message
    			Security header type [4 bits] = 0x4 [ 4 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			MAC = 0x655F4F7D [ 1700745085 ]
    			Sequence Number = 0x00 [ 0 ]
    			NAS message = 0x0022 [ 34 ]
    ←------------------------------------------------------------------------------------------------------------
    Ciphered NAS Message UL:
    	Ciphered NAS Message UL PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Ciphered NAS Message =
    			0x0022
    ←------------------------------------------------------------------------------------------------------------
    RRC_PDU_IND:
    ↑	Received on port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 334
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							ulInformationTransfer
    								criticalExtensions
    									c1
    										ulInformationTransfer_r8
    											dedicatedInfoType
    												dedicatedInfoNAS = '4765DF4F7D000022'O
    											nonCriticalExtension = Omit

    Security Mode Complete:
    	Security Mode Complete PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Security Mode Complete
    			Security header type [4 bits] = 0x0 [ 0 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			Message Type [8 bits] = 0x5E - Security Mode Complete [ 94 ]
    ←------------------------------------------------------------------------------------------------------------
    SRB_COMMON_IND:
    ↑	Inter-component message: SRB -> EUTRA_PTC:SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 334
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			Signalling
    				Rrc = Omit
    				Nas
    					NasIndication
    						SecurityProtection
    							Status = 0100'B
    							NasCount = '00000000'O
    						Pdu
    							Msg
    								sECURITY_MODE_COMPLETE
    									securityHeaderType = 0000'B
    									protocolDiscriminator = 0111'B
    									messageType = 01011110'B
    									imeisv = Omit
    							PiggybackedPduList = Omit

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = True
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				RadioBearerList
    					RadioBearer_Type
    						Id
    							Drb = 1
    						Config
    							AddOrReconfigure
    								Pdcp
    									Config
    										Rb
    											Drb
    												R8
    													discardTimer = infinity_ (7)
    													rlc_AM
    														statusReportRequired = True
    													rlc_UM = Omit
    													headerCompression
    														notUsed = Null
    													rn_IntegrityProtection_r10 = Omit
    													pdcp_SN_Size_v1130 = Omit
    													ul_DataSplitDRB_ViaSCG_r12 = Omit
    													t_Reordering_r12 = Omit
    													ul_DataSplitThreshold_r13 = Omit
    													pdcp_SN_Size_v1310 = Omit
    													statusFeedback_r13 = Omit
    										TestMode
    											None = True
    								Rlc
    									Rb
    										AM
    											Tx
    												R8
    													t_PollRetransmit = ms80 (15)
    													pollPDU = p128 (5)
    													pollByte = kB125 (4)
    													maxRetxThreshold = t4 (3)
    											Rx
    												R8
    													t_Reordering = ms80 (16)
    													t_StatusProhibit = ms60 (12)
    											ExtendedLI = Omit
    									TestMode
    										None = True
    								LogicalChannelId = 3
    								Mac
    									LogicalChannel
    										Priority = 13
    										PrioritizedBitRate = kBps0 (0)
    									TestMode
    										None = True
    								DiscardULData = Omit

    SYSTEM_CTRL_CNF:
    ↑	Received on port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_CNF
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				Result
    					Success = True
    			Confirm
    				RadioBearerList = True

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = True
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				PdcpCount
    					Get
    						AllRBs = True

    SYSTEM_CTRL_CNF:
    ↑	Received on port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_CNF
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				Result
    					Success = True
    			Confirm
    				PdcpCount
    					Get
    						PdcpCountInfo_Type
    							RadioBearerId
    								Srb = 1
    							UL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000011'B
    							DL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000010'B
    						PdcpCountInfo_Type
    							RadioBearerId
    								Srb = 2
    							UL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000000'B
    							DL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000000'B
    						PdcpCountInfo_Type
    							RadioBearerId
    								Drb = 1
    							UL
    								Format = PdcpCount_DrbShortSQN (2)
    								Value = 00000000000000000000000000000000'B
    							DL
    								Format = PdcpCount_DrbShortSQN (2)
    								Value = 00000000000000000000000000000000'B

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = True
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				AS_Security
    					StartRestart
    						Integrity
    							Algorithm = eia1 (1)
    							KRRCint = 10001100011101101101010000010100100110110001001111000110110100001011000111101111101101010100111100101100100100110000111000100100'B
    							ActTimeList = Omit
    						Ciphering
    							Algorithm = eea1 (1)
    							KRRCenc = 10011101101111111000111001000000000111100110010111101011111110001100011010011101010111000111111100011000110000001111111110111001'B
    							KUPenc = 01010000000101011110110101010000010000100010010010001011001001000011010001111100011001000111000100100010000100010011011111100000'B
    							ActTimeList
    								SecurityActTime_Type
    									RadioBearerId
    										Srb = 1
    									UL
    										SQN
    											Format = PdcpCount_Srb (0)
    											Value = 4
    									DL
    										SQN
    											Format = PdcpCount_Srb (0)
    											Value = 3
    								SecurityActTime_Type
    									RadioBearerId
    										Srb = 2
    									UL
    										SQN
    											Format = PdcpCount_Srb (0)
    											Value = 0
    									DL
    										SQN
    											Format = PdcpCount_Srb (0)
    											Value = 0
    								SecurityActTime_Type
    									RadioBearerId
    										Drb = 1
    									UL
    										SQN
    											Format = PdcpCount_DrbShortSQN (2)
    											Value = 0
    									DL
    										SQN
    											Format = PdcpCount_DrbShortSQN (2)
    											Value = 0

    SYSTEM_CTRL_CNF:
    ↑	Received on port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_CNF
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				Result
    					Success = True
    			Confirm
    				AS_Security = True

    SRB_COMMON_REQ:
    ↓	Inter-component message: TC_SRB -> NASEMU_LTE_PTC:TC_SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Dcch
    						message_
    							c1
    								securityModeCommand
    									rrc_TransactionIdentifier = 0
    									criticalExtensions
    										c1
    											securityModeCommand_r8
    												securityConfigSMC
    													securityAlgorithmConfig
    														cipheringAlgorithm = eea1 (1)
    														integrityProtAlgorithm = eia1 (1)
    												nonCriticalExtension = Omit
    				Nas = Omit

    DL-DCCH-Message:
    	securityModeCommand
    		Source = \Protocol\3GPP\LTE\RRC\
    		DL-DCCH-Message
    			message = c1 = securityModeCommand =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = c1 = securityModeCommand-r8 =
    					securityConfigSMC
    						securityAlgorithmConfig
    							cipheringAlgorithm = eea1
    							integrityProtAlgorithm = eia1
    ------------------------------------------------------------------------------------------------------------→
    RRC_PDU_REQ:
    ↓	Sent from port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							securityModeCommand
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									c1
    										securityModeCommand_r8
    											securityConfigSMC
    												securityAlgorithmConfig
    													cipheringAlgorithm = eea1 (1)
    													integrityProtAlgorithm = eia1 (1)
    											nonCriticalExtension = Omit

    UL-DCCH-Message:
    	securityModeComplete
    		Source = \Protocol\3GPP\LTE\RRC\
    		UL-DCCH-Message
    			message = c1 = securityModeComplete =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = securityModeComplete-r8 =
    ←------------------------------------------------------------------------------------------------------------
    RRC_PDU_IND:
    ↑	Received on port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 362
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							securityModeComplete
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									securityModeComplete_r8
    										nonCriticalExtension = Omit

    SRB_COMMON_IND:
    ↑	Inter-component message: SRB -> EUTRA_PTC:SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 362
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Dcch
    						message_
    							c1
    								securityModeComplete
    									rrc_TransactionIdentifier = 0
    									criticalExtensions
    										securityModeComplete_r8
    											nonCriticalExtension = Omit
    				Nas = Omit

    SRB_COMMON_REQ:
    ↓	Inter-component message: TC_SRB -> NASEMU_LTE_PTC:TC_SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Dcch
    						message_
    							c1
    								ueCapabilityEnquiry
    									rrc_TransactionIdentifier = 0
    									criticalExtensions
    										c1
    											ueCapabilityEnquiry_r8
    												ue_CapabilityRequest
    													RAT_Type = eutra (0)
    												nonCriticalExtension = Omit
    				Nas = Omit

    DL-DCCH-Message:
    	ueCapabilityEnquiry
    		Source = \Protocol\3GPP\LTE\RRC\
    		DL-DCCH-Message
    			message = c1 = ueCapabilityEnquiry =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = c1 = ueCapabilityEnquiry-r8 =
    					ue-CapabilityRequest = SEQUENCE OF RAT-Type
    						RAT-Type(1) = eutra
    ------------------------------------------------------------------------------------------------------------→
    RRC_PDU_REQ:
    ↓	Sent from port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							ueCapabilityEnquiry
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									c1
    										ueCapabilityEnquiry_r8
    											ue_CapabilityRequest
    												RAT_Type = eutra (0)
    											nonCriticalExtension = Omit

    UL-DCCH-Message:
    	ueCapabilityInformation
    		Source = \Protocol\3GPP\LTE\RRC\
    		UL-DCCH-Message
    			message = c1 = ueCapabilityInformation =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = c1 = ueCapabilityInformation-r8 =
    					ue-CapabilityRAT-ContainerList = SEQUENCE OF UE-CapabilityRAT-Container
    						UE-CapabilityRAT-Container(1)
    							rat-Type = eutra
    							ueCapabilityRAT-Container = C81808FA0610300C001081838B2248A193A3E7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFDFF3FFAFA20C008C87428329D2A4B81C163000000000228008000000
    			UE-CapabilityRAT-Container(1)
    				UE-EUTRA-Capability
    					accessStratumRelease = rel10
    					ue-Category = 1
    					pdcp-Parameters
    						supportedROHC-Profiles
    							profile0x0001 = TRUE
    							profile0x0002 = TRUE
    							profile0x0003 = FALSE
    							profile0x0004 = FALSE
    							profile0x0006 = FALSE
    							profile0x0101 = FALSE
    							profile0x0102 = FALSE
    							profile0x0103 = FALSE
    							profile0x0104 = FALSE
    						maxNumberROHC-ContextSessions  = cs16
    					phyLayerParameters
    						ue-TxAntennaSelectionSupported = TRUE
    						ue-SpecificRefSigsSupported = FALSE
    					rf-Parameters
    						supportedBandListEUTRA = SEQUENCE OF SupportedBandEUTRA
    							SupportedBandEUTRA(1)
    								bandEUTRA = 41
    								halfDuplex = FALSE
    							SupportedBandEUTRA(2)
    								bandEUTRA = 13
    								halfDuplex = FALSE
    							SupportedBandEUTRA(3)
    								bandEUTRA = 17
    								halfDuplex = FALSE
    							SupportedBandEUTRA(4)
    								bandEUTRA = 25
    								halfDuplex = FALSE
    							SupportedBandEUTRA(5)
    								bandEUTRA = 4
    								halfDuplex = FALSE
    							SupportedBandEUTRA(6)
    								bandEUTRA = 1
    								halfDuplex = FALSE
    							SupportedBandEUTRA(7)
    								bandEUTRA = 2
    								halfDuplex = FALSE
    							SupportedBandEUTRA(8)
    								bandEUTRA = 5
    								halfDuplex = FALSE
    							SupportedBandEUTRA(9)
    								bandEUTRA = 7
    								halfDuplex = FALSE
    							SupportedBandEUTRA(10)
    								bandEUTRA = 8
    								halfDuplex = FALSE
    							SupportedBandEUTRA(11)
    								bandEUTRA = 12
    								halfDuplex = FALSE
    							SupportedBandEUTRA(12)
    								bandEUTRA = 18
    								halfDuplex = FALSE
    							SupportedBandEUTRA(13)
    								bandEUTRA = 19
    								halfDuplex = FALSE
    							SupportedBandEUTRA(14)
    								bandEUTRA = 21
    								halfDuplex = FALSE
    							SupportedBandEUTRA(15)
    								bandEUTRA = 26
    								halfDuplex = FALSE
    							SupportedBandEUTRA(16)
    								bandEUTRA = 30
    								halfDuplex = FALSE
    					measParameters
    						bandListEUTRA = SEQUENCE OF BandInfoEUTRA
    							BandInfoEUTRA(1)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(2)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(3)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(4)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(5)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(6)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(7)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(8)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(9)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(10)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(11)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(12)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(13)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(14)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(15)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(16)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    					featureGroupIndicators = 01111111110011111111111010111110
    					interRAT-Parameters
    						utraFDD
    							supportedBandListUTRA-FDD = SEQUENCE OF SupportedBandUTRA-FDD
    								SupportedBandUTRA-FDD(1) = bandI
    								SupportedBandUTRA-FDD(2) = bandII
    								SupportedBandUTRA-FDD(3) = bandIV
    								SupportedBandUTRA-FDD(4) = bandV
    								SupportedBandUTRA-FDD(5) = bandVIII
    								SupportedBandUTRA-FDD(6) = bandIX
    								SupportedBandUTRA-FDD(7) = bandXI
    						geran
    							supportedBandListGERAN = SEQUENCE OF SupportedBandGERAN
    								SupportedBandGERAN(1) = gsm850
    								SupportedBandGERAN(2) = gsm900E
    								SupportedBandGERAN(3) = gsm1800
    								SupportedBandGERAN(4) = gsm1900
    							interRAT-PS-HO-ToGERAN = FALSE
    					nonCriticalExtension
    						phyLayerParameters-v920
    							enhancedDualLayerTDD-r9 = supported
    						interRAT-ParametersGERAN-v920
    							dtm-r9 = supported
    							e-RedirectionGERAN-r9 = supported
    						interRAT-ParametersUTRA-v920
    							e-RedirectionUTRA-r9 = supported
    						csg-ProximityIndicationParameters-r9
    						neighCellSI-AcquisitionParameters-r9
    						son-Parameters-r9
    							rach-Report-r9 = supported
    						nonCriticalExtension
    							lateNonCriticalExtension = CONTAINING =
    								featureGroupIndRel9Add-r9 = 11000000000000000000000000000000
    							nonCriticalExtension
    								featureGroupIndRel10-r10 = 01000000000001000000000000000000
    								nonCriticalExtension
    ←------------------------------------------------------------------------------------------------------------
    RRC_PDU_IND:
    ↑	Received on port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 366
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							ueCapabilityInformation
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									c1
    										ueCapabilityInformation_r8
    											ue_CapabilityRAT_ContainerList
    												UE_CapabilityRAT_Container
    													rat_Type = eutra (0)
    													ueCapabilityRAT_Container = 'C81808FA0610300C001081838B2248A193A3E7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFDFF3FFAFA20C008C87428329D2A4B81C163000000000228008000000'O
    											nonCriticalExtension = Omit

    SRB_COMMON_IND:
    ↑	Inter-component message: SRB -> EUTRA_PTC:SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 366
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Dcch
    						message_
    							c1
    								ueCapabilityInformation
    									rrc_TransactionIdentifier = 0
    									criticalExtensions
    										c1
    											ueCapabilityInformation_r8
    												ue_CapabilityRAT_ContainerList
    													UE_CapabilityRAT_Container
    														rat_Type = eutra (0)
    														ueCapabilityRAT_Container = 'C81808FA0610300C001081838B2248A193A3E7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFDFF3FFAFA20C008C87428329D2A4B81C163000000000228008000000'O
    												nonCriticalExtension = Omit
    				Nas = Omit

    IP_ConfigReq_Type:
    ↓	Inter-component message: EUTRA_CTRL -> IP_PTC:EUTRA_CTRL
    		Source = \Test Control\TTCN3
    		IP_ConfigReq_Type
    			ChangeEutraCell = eutra_CellA (16)

    IP_Indication_Type:
    ↑	Inter-component message: IP -> EUTRA_PTC:IP
    		Source = \Test Control\TTCN3
    		IP_Indication_Type
    			Cnf = True

    SRB_COMMON_REQ:
    ↓	Inter-component message: TC_SRB -> NASEMU_LTE_PTC:TC_SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Dcch
    						message_
    							c1
    								rrcConnectionReconfiguration
    									rrc_TransactionIdentifier = 0
    									criticalExtensions
    										c1
    											rrcConnectionReconfiguration_r8
    												measConfig = Omit
    												mobilityControlInfo = Omit
    												dedicatedInfoNASList = Omit
    												radioResourceConfigDedicated
    													srb_ToAddModList
    														SRB_ToAddMod
    															srb_Identity = 2
    															rlc_Config
    																defaultValue = Null
    															logicalChannelConfig
    																defaultValue = Null
    													drb_ToAddModList
    														DRB_ToAddMod
    															eps_BearerIdentity = 5
    															drb_Identity = 1
    															pdcp_Config
    																discardTimer = infinity_ (7)
    																rlc_AM
    																	statusReportRequired = True
    																rlc_UM = Omit
    																headerCompression
    																	notUsed = Null
    																rn_IntegrityProtection_r10 = Omit
    																pdcp_SN_Size_v1130 = Omit
    																ul_DataSplitDRB_ViaSCG_r12 = Omit
    																t_Reordering_r12 = Omit
    																ul_DataSplitThreshold_r13 = Omit
    																pdcp_SN_Size_v1310 = Omit
    																statusFeedback_r13 = Omit
    															rlc_Config
    																am
    																	ul_AM_RLC
    																		t_PollRetransmit = ms80 (15)
    																		pollPDU = p128 (5)
    																		pollByte = kB125 (4)
    																		maxRetxThreshold = t4 (3)
    																	dl_AM_RLC
    																		t_Reordering = ms80 (16)
    																		t_StatusProhibit = ms60 (12)
    															logicalChannelIdentity = 3
    															logicalChannelConfig
    																ul_SpecificParameters
    																	priority = 6
    																	prioritisedBitRate = kBps0 (0)
    																	bucketSizeDuration = ms100 (1)
    																	logicalChannelGroup = 1
    																logicalChannelSR_Mask_r9 = Omit
    																logicalChannelSR_Prohibit_r12 = Omit
    															drb_TypeChange_r12 = Omit
    															rlc_Config_v1250 = Omit
    															rlc_Config_v1310 = Omit
    															drb_TypeLWA_r13 = Omit
    															drb_TypeLWIP_r13 = Omit
    													drb_ToReleaseList = Omit
    													mac_MainConfig
    														explicitValue
    															ul_SCH_Config
    																maxHARQ_Tx = n5 (4)
    																periodicBSR_Timer = sf20 (3)
    																retxBSR_Timer = sf320 (0)
    																ttiBundling = False
    															drx_Config
    																setup
    																	onDurationTimer = psf6 (5)
    																	drx_InactivityTimer = psf1920 (20)
    																	drx_RetransmissionTimer = psf16 (5)
    																	longDRX_CycleStartOffset
    																		sf1280 = 4
    																	shortDRX = Omit
    															timeAlignmentTimerDedicated = sf750 (1)
    															phr_Config
    																setup
    																	periodicPHR_Timer = sf500 (5)
    																	prohibitPHR_Timer = sf200 (5)
    																	dl_PathlossChange = dB3 (1)
    															sr_ProhibitTimer_r9 = Omit
    															mac_MainConfig_v1020 = Omit
    															stag_ToReleaseList_r11 = Omit
    															stag_ToAddModList_r11 = Omit
    															drx_Config_v1130 = Omit
    															e_HARQ_Pattern_r12 = Omit
    															dualConnectivityPHR = Omit
    															logicalChannelSR_Config_r12 = Omit
    															drx_Config_v1310 = Omit
    															extendedPHR2_r13 = Omit
    															eDRX_Config_CycleStartOffset_r13 = Omit
    															drx_Config_r13 = Omit
    													sps_Config = Omit
    													physicalConfigDedicated
    														pdsch_ConfigDedicated = Omit
    														pucch_ConfigDedicated = Omit
    														pusch_ConfigDedicated = Omit
    														uplinkPowerControlDedicated = Omit
    														tpc_PDCCH_ConfigPUCCH
    															setup
    																tpc_RNTI = 0000001111111111'B
    																tpc_Index
    																	indexOfFormat3 = 1
    														tpc_PDCCH_ConfigPUSCH
    															setup
    																tpc_RNTI = 0000000111111010'B
    																tpc_Index
    																	indexOfFormat3 = 1
    														cqi_ReportConfig
    															cqi_ReportModeAperiodic = rm30 (3)
    															nomPDSCH_RS_EPRE_Offset = 0
    															cqi_ReportPeriodic
    																setup
    																	cqi_PUCCH_ResourceIndex = 0
    																	cqi_pmi_ConfigIndex = 25
    																	cqi_FormatIndicatorPeriodic
    																		widebandCQI = Null
    																	ri_ConfigIndex = 483
    																	simultaneousAckNackAndCQI = False
    														soundingRS_UL_ConfigDedicated
    															setup
    																srs_Bandwidth = bw0 (0)
    																srs_HoppingBandwidth = hbw0 (0)
    																freqDomainPosition = 0
    																duration = True
    																srs_ConfigIndex = 20
    																transmissionComb = 0
    																cyclicShift = cs0 (0)
    														antennaInfo
    															defaultValue = Null
    														schedulingRequestConfig = Omit
    														cqi_ReportConfig_v920 = Omit
    														antennaInfo_v920 = Omit
    														antennaInfo_r10 = Omit
    														antennaInfoUL_r10 = Omit
    														cif_Presence_r10 = Omit
    														cqi_ReportConfig_r10 = Omit
    														csi_RS_Config_r10 = Omit
    														pucch_ConfigDedicated_v1020 = Omit
    														pusch_ConfigDedicated_v1020 = Omit
    														schedulingRequestConfig_v1020 = Omit
    														soundingRS_UL_ConfigDedicated_v1020 = Omit
    														soundingRS_UL_ConfigDedicatedAperiodic_r10 = Omit
    														uplinkPowerControlDedicated_v1020 = Omit
    														additionalSpectrumEmissionCA_r10 = Omit
    														csi_RS_ConfigNZPToReleaseList_r11 = Omit
    														csi_RS_ConfigNZPToAddModList_r11 = Omit
    														csi_RS_ConfigZPToReleaseList_r11 = Omit
    														csi_RS_ConfigZPToAddModList_r11 = Omit
    														epdcch_Config_r11 = Omit
    														pdsch_ConfigDedicated_v1130 = Omit
    														cqi_ReportConfig_v1130 = Omit
    														pucch_ConfigDedicated_v1130 = Omit
    														pusch_ConfigDedicated_v1130 = Omit
    														uplinkPowerControlDedicated_v1130 = Omit
    														antennaInfo_v1250 = Omit
    														eimta_MainConfig_r12 = Omit
    														eimta_MainConfigPCell_r12 = Omit
    														pucch_ConfigDedicated_v1250 = Omit
    														cqi_ReportConfigPCell_v1250 = Omit
    														uplinkPowerControlDedicated_v1250 = Omit
    														pusch_ConfigDedicated_v1250 = Omit
    														csi_RS_Config_v1250 = Omit
    														pdsch_ConfigDedicated_v1280 = Omit
    														pdsch_ConfigDedicated_v1310 = Omit
    														pucch_ConfigDedicated_r13 = Omit
    														pusch_ConfigDedicated_r13 = Omit
    														pdcch_CandidateReductions_r13 = Omit
    														cqi_ReportConfig_v1310 = Omit
    														soundingRS_UL_ConfigDedicated_v1310 = Omit
    														soundingRS_UL_ConfigDedicatedUpPTsExt_r13 = Omit
    														soundingRS_UL_ConfigDedicatedAperiodic_v1310 = Omit
    														soundingRS_UL_ConfigDedicatedAperiodicUpPTsExt_r13 = Omit
    														csi_RS_Config_v1310 = Omit
    														ce_Mode_r13 = Omit
    														csi_RS_ConfigNZPToAddModListExt_r13 = Omit
    														csi_RS_ConfigNZPToReleaseListExt_r13 = Omit
    														cqi_ReportConfig_v1320 = Omit
    													rlf_TimersAndConstants_r9 = Omit
    													measSubframePatternPCell_r10 = Omit
    													neighCellsCRS_Info_r11 = Omit
    													naics_Info_r12 = Omit
    													neighCellsCRS_Info_r13 = Omit
    													rlf_TimersAndConstants_r13 = Omit
    												securityConfigHO = Omit
    												nonCriticalExtension = Omit
    				Nas
    					NAS_MSG_Request_Type
    						SecurityProtection
    							Status = 0010'B
    							ForceMacError = False
    						Pdu
    							Msg
    								aTTACH_ACCEPT
    									securityHeaderType = 0000'B
    									protocolDiscriminator = 0111'B
    									messageType = 01000010'B
    									spareHalfOctet = '0'H
    									epsAttachResult
    										spare = 0'B
    										resultValue = 001'B
    									t3412
    										iei = Omit
    										unit = 111'B
    										timerValue = 00000'B
    									taiList
    										iei = Omit
    										iel = '06'O
    										listOfPartialTais
    											ListOfPartialTaiList
    												spareBit = 0'B
    												typeOfList = 00'B
    												numberOfElements = 00000'B
    												partialTaiList
    													type0List
    														Type0Element
    															plmnId = '00F110'O
    															tacList
    																NAS_Tac = '0001'O
    									esmMessage
    										iei = Omit
    										iel = '0000'O
    										esmPdu = ''O
    									guti
    										iei = '50'O
    										iel = '0B'O
    										idDigit1 = 1111'B
    										oddEvenInd = 0'B
    										typeOfId = 110'B
    										otherDigits = '00F110800101C2345678'O
    									lai = Omit
    									msIdentity = Omit
    									emmCause = Omit
    									t3402 = Omit
    									t3423 = Omit
    									equivalentPlmns = Omit
    									emergencyNumberList = Omit
    									epsNetworkFeatureSupport
    										iei = '64'O
    										iel = '01'O
    										cp_CIOT = 0'B
    										emmRegistered_withoutPDN = 0'B
    										esrps = 0'B
    										csLCS = 00'B
    										epcLCS = 0'B
    										emcBS = 0'B
    										imsVoPS = 1'B
    										spareBits = Omit
    										extdPCO = Omit
    										headerComp_CP_CIOT = Omit
    										s1_U_data = Omit
    										up_CIOT = Omit
    									addUpdateResult = Omit
    									t3412ExtdValue = Omit
    									t3324Value = Omit
    									extendedDRXParams = Omit
    							PiggybackedPduList
    								NAS_DL_Pdu_Type
    									Msg
    										aCTIVATE_DEFAULT_EPS_BEARER_CONTEXT_REQUEST
    											epsBearerId = '5'H
    											protocolDiscriminator = 0010'B
    											procedureTransactionIdentifier = '07'O
    											messageType = 11000001'B
    											epsQos
    												iei = Omit
    												iel = '09'O
    												qci = 00001001'B
    												maxBitRateUl = 01000000'B
    												maxBitRateDl = 01000000'B
    												guaranteedBitRateUl = 01000000'B
    												guaranteedBitRateDl = 01000000'B
    												maxBitRateUlExt = 00000000'B
    												maxBitRateDlExt = 00000000'B
    												guaranteedBitRateUlExt = 00000000'B
    												guaranteedBitRateDlExt = 00000000'B
    												maxBitRateDL_Ext2 = Omit
    												guaranteedBitRateDL_Ext2 = Omit
    												maxBitRateUL_Ext2 = Omit
    												guaranteedBitRateUL_Ext2 = Omit
    											accessPointName
    												iei = Omit
    												iel = '04'O
    												nameValue = '0361706E'O
    											pdnAdress
    												iei = Omit
    												iel = '0D'O
    												spare = 00000'B
    												typeValue = 011'B
    												adressInfo = '0000000000000002C0A8001A'O
    											transactionIdentifier
    												iei = '5D'O
    												iel = '01'O
    												tiFlag = 0'B
    												tiValue = 000'B
    												spare = 0000'B
    												ext = Omit
    												tiValue_2 = Omit
    											negotiatedQos
    												iei = '30'O
    												iel = '10'O
    												spare1 = 00'B
    												delayClass = 100'B
    												relabilityClass = 011'B
    												peakThroughput = 0101'B
    												spare2 = 0'B
    												precedenceClass = 010'B
    												spare3 = 000'B
    												meanThroughput = 10000'B
    												trafficClass = 100'B
    												deliveryOrder = 01'B
    												deliveryErrorSDU = 011'B
    												maxSduSize = 10010110'B
    												maxBitRateUL = 01001000'B
    												maxBitRateDL = 01001000'B
    												residualBER = 0111'B
    												sduErrorRatio = 0100'B
    												transferDelay = 000000'B
    												trafficHandlingPrio = 00'B
    												guaranteedBitRateUL = 00000000'B
    												guaranteedBitRateDL = 00000000'B
    												spare4 = 000'B
    												signallingInd = 0'B
    												sourceStatisticsDescriptor = 0000'B
    												maxBitRateDL_Ext = 00000000'B
    												guaranteedBitRateDL_Ext = 00000000'B
    												maxBitRateUL_Ext = 00000000'B
    												guaranteedBitRateUL_Ext = 00000000'B
    												maxBitRateDL_Ext2 = Omit
    												guaranteedBitRateDL_Ext2 = Omit
    												maxBitRateUL_Ext2 = Omit
    												guaranteedBitRateUL_Ext2 = Omit
    											negotiatedLlcSapi
    												iei = '32'O
    												spare = 0000'B
    												llcSapiValue = 1011'B
    											radioPriority
    												iei = '8'H
    												spare = 0'B
    												levelValue = 100'B
    											packetFlowIdentifier
    												iei = '34'O
    												iel = '01'O
    												spare = 0'B
    												idValue = 0000000'B
    											apnAggMaxBitRate = Omit
    											esmCause = Omit
    											protocolConfigurationOptions
    												iei = '27'O
    												iel = '1B'O
    												ext = 1'B
    												spare = 0000'B
    												configProtocol = 000'B
    												pco
    													ProtocolContainer
    														protocolID = '000D'O
    														protocolLength = '04'O
    														content = 'C0A8C637'O
    													ProtocolContainer
    														protocolID = '0003'O
    														protocolLength = '10'O
    														content = 'fd29cc437fb90002020c29fffe66b4c7'O
    											connectivityType = Omit
    											wlanOffloadInd = Omit
    											nbifomContainer = Omit
    											headerCompressionConfig = Omit
    											controlPlaneOnlyIndication = Omit
    											extdProtocolConfigurationOptions = Omit
    											servingPLMNRateControl = Omit
    									PiggybackedPduList = Omit

    Attach Accept:
    	Attach Accept PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Attach Accept
    			Security header type [4 bits] = 0x0 [ 0 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			Message Type [8 bits] = 0x42 - Attach Accept [ 66 ]
    			Spare Half Octet [4 bits] = 0x0 [ 0 ]
    			EPS attach result
    				Spare Bits [1 bit] = 0x0 [ 0 ]
    				Value [3 bits] = 0x1 [ 1 ]
    			T3412 value
    				Timer Value Unit [3 bits] = 0x7 - Value Indicates that the Timer is Deactivated [ 7 ]
    				Value [5 bits] = 0x0 [ 0 ]
    			Tracking area identity list
    				IE Length [8 bits] = 0x6 [ 6 ]
    				Spare Bits [1 bit] = 0x0 [ 0 ]
    				Type of list [2 bits] = 0x0 [ 0 ]
    				number of elements [5 bits] = 0x0 [ 0 ]
    				Mobile Country Code 1st and 2nd  Digits = 0x00 [ 0 ]
    				Mobile Network Code 3rd Digit = 0xF [ 15 ]
    				Mobile Country Code 3rd Digit = 0x1 [ 1 ]
    				Mobile Network Code 1st and 2nd  Digits = 0x10 [ 16 ]
    				Tracking area code 1 = 0x00 [ 0 ]
    				Tracking area code 1 continued = 0x01 [ 1 ]
    			ESM message container
    				IE Length [16 bits] = 0x58 [ 88 ]
    				ESM message container contents = 0x5207C109094040404000000000040361706E0D030000000000000002C0A8001A5D010030102352108B964848740000000000000000320B84340100271B80000D04C0A8C637000310FD29CC437FB90002020C29FFFE66B4C7
    			EPS mobile identity
    				IE Identifier [8 bits] = 0x50 [ 80 ]
    				IE Length [8 bits] = 0xB [ 11 ]
    				constant / IMSI Identity Digit 1 [4 bits] = 0xF [ 15 ]
    				Odd / Even Indicator [1 bit] = 0x0 [ 0 ]
    				EPS Type of Identity [3 bits] = 0x6 - GUTI [ 6 ]
    				Mobile Country Code 1st and 2nd  Digits = 0x00 [ 0 ]
    				Mobile Network Code 3rd Digit = 0xF [ 15 ]
    				Mobile Country Code 3rd Digit = 0x1 [ 1 ]
    				Mobile Network Code 1st and 2nd  Digits = 0x10 [ 16 ]
    				MME group Id = 0x8001 [ 32769 ]
    				MME code = 0x01 [ 1 ]
    				M-TMSI = 0xC2345678 [ 3258209912 ]
    			EPS Network feature support
    				IE Identifier [8 bits] = 0x64 [ 100 ]
    				IE Length [8 bits] = 0x1 [ 1 ]
    				Spare Bits [2 bits] = 0x0 [ 0 ]
    				esr_ps [1 bit] = 0x0 [ 0 ]
    				Location Services Indicator in CS  [2 bits] = 0x0 - No information about support of location services via CS domain is available [ 0 ]
    				Location Services Indicator in EPC [1 bit] = 0x0 - Location services via EPC not supported [ 0 ]
    				Emergency Bearer Services Indicator  [1 bit] = 0x0 - Emergency bearer services in S1 mode not supported [ 0 ]
    				IMS VoPS [1 bit] = 0x1 [ 1 ]
    ------------------------------------------------------------------------------------------------------------→
    Activate Default EPS Bearer Context Request:
    	Activate Default EPS Bearer Context Request PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Activate Default EPS Bearer Context Request
    			EPS bearer identity [4 bits] = 0x5 [ 5 ]
    			Protocol Discriminator [4 bits] = 0x2 - EPS Session Management Messages [ 2 ]
    			Procedure transaction identifier [8 bits] = 0x7 [ 7 ]
    			Message Type [8 bits] = 0xC1 - Activate Default EPS Bearer Context Request [ 193 ]
    			EPS QoS
    				IE Length [8 bits] = 0x9 [ 9 ]
    				QCI = 0x09 [ 9 ]
    				Maximum Bit Rate for Uplink = 0x40 - The Maximum Bit Rate is 64 kbps +  ((The Binary Coded Value in 8 Bits -01000000) * 8 Kbps) [ 64 ]
    				Maximum Bit Rate for Dlink = 0x40 - The Maximum Bit Rate is 64 kbps +  ((The Binary Coded Value in 8 Bits -01000000) * 8 Kbps) [ 64 ]
    				Guaranteed Bit Rate for Ulink = 0x40 [ 64 ]
    				Guaranteed Bit Rate for Dlink = 0x40 [ 64 ]
    				Maximum bit rate for uplink (extended) = 0x00 [ 0 ]
    				Maximum bit rate for downlink (extended) = 0x00 [ 0 ]
    				Guaranteed bit rate for uplink (extended) = 0x00 [ 0 ]
    				Guaranteed bit rate for downlink (extended) = 0x00 [ 0 ]
    			APN Address
    				IE Length [8 bits] = 0x4 [ 4 ]
    				Value = 0x0361706E [ 56717422 ]
    			PDN address
    				IE Length [8 bits] = 0xD [ 13 ]
    				Spare Bits [5 bits] = 0x0 [ 0 ]
    				PDN type value [3 bits] = 0x3 [ 3 ]
    				PDN address information = 0x0000000000000002C0A8001A
    			Transaction Identifier
    				IE Identifier [8 bits] = 0x5D [ 93 ]
    				IE Length [8 bits] = 0x1 [ 1 ]
    				Flag [1 bit] = 0x0 - The Message is Sent from the Side That Originates the TI [ 0 ]
    				TI Value [3 bits] = 0x0 [ 0 ]
    				Spare Bits [4 bits] = 0x0 [ 0 ]
    			Negotiated Quality of Service
    				IE Identifier [8 bits] = 0x30 [ 48 ]
    				IE Length [8 bits] = 0x10 [ 16 ]
    				Spare Bits [2 bits] = 0x0 [ 0 ]
    				Delay Class  [3 bits] = 0x4 - Delay Class 4(Best Effort) [ 4 ]
    				Reliability Class  [3 bits] = 0x3 - Unacknowledged GTP and LLC; Acknowledged RLC, Protected Data [ 3 ]
    				Peak Throughput  [4 bits] = 0x5 - Up to 16000 Octet/s [ 5 ]
    				Spare bits B [1 bit] = 0x0 [ 0 ]
    				Precedence Class  [3 bits] = 0x2 - Normal Priority [ 2 ]
    				Spare bits C [3 bits] = 0x0 [ 0 ]
    				Mean Throughput  [5 bits] = 0x10 - 10000000 Octet/h [ 16 ]
    				Traffic Class  [3 bits] = 0x4 - Background Class [ 4 ]
    				Delivery Order  [2 bits] = 0x1 - With Delivery Order ('Yes') [ 1 ]
    				Delivery of Erroneous SDU  [3 bits] = 0x3 - Erroneous SDUs are Not Delivered [ 3 ]
    				Maximum SDU Size  [8 bits] = 0x96 [ 150 ]
    				Maximum Bit Rate for Uplink [8 bits] = 0x48 [ 72 ]
    				Maximum Bit Rate for Dlink [8 bits] = 0x48 [ 72 ]
    				Residual BER  [4 bits] = 0x7 - 1*10E-5  [ 7 ]
    				SDU Error Ratio [4 bits] = 0x4 - 1*10E-4  [ 4 ]
    				Transfer Delay  [6 bits] = 0x0 - Subscribed Traffic Class [ 0 ]
    				Traffic Handler Priority  [2 bits] = 0x0 - Subscribed Traffic Handling Priority [ 0 ]
    				Guaranteed Bit Rate for Ulink [8 bits] = 0x0 [ 0 ]
    				Guaranteed Bit Rate for Dlink  [8 bits] = 0x0 [ 0 ]
    				Spare Bits D [3 bits] = 0x0 [ 0 ]
    				Signalling Indication [1 bit] = 0x0 [ 0 ]
    				Source Statistics Descriptor [4 bits] = 0x0 [ 0 ]
    				Maximum bit rate for downlink (Extended) [8 bits] = 0x0 [ 0 ]
    				Guaranteed bit rate for downlink (Extended) [8 bits] = 0x0 [ 0 ]
    				Max bit rate Uplink extd [8 bits] = 0x0 [ 0 ]
    				Guaranteed bit rate Uplink extd [8 bits] = 0x0 [ 0 ]
    			Negotiated LLC SAPI
    				IE Identifier [8 bits] = 0x32 [ 50 ]
    				Spare Bits [4 bits] = 0x0 [ 0 ]
    				value [4 bits] = 0xB - SAPI 11 [ 11 ]
    			Radio Priority
    				IE Identifier [4 bits] = 0x8 [ 8 ]
    				Spare Bits [1 bit] = 0x0 [ 0 ]
    				value [3 bits] = 0x4 - Priority Level 4 [ 4 ]
    			Packet Flow Identifier
    				IE Identifier [8 bits] = 0x34 [ 52 ]
    				IE Length [8 bits] = 0x1 [ 1 ]
    				Spare Bits [1 bit] = 0x0 [ 0 ]
    				value [7 bits] = 0x0 - Best Effort [ 0 ]
    			Protocol Configuration Options
    				IE Identifier [8 bits] = 0x27 [ 39 ]
    				IE Length [8 bits] = 0x1B [ 27 ]
    				Extension Bit [1 bit] = 0x1 - Outgoing Calls Barred within CUG [ 1 ]
    				Spare Bits [4 bits] = 0x0 [ 0 ]
    				Configuration Protocol [3 bits] = 0x0 - PPP for Use with IP PDP Type [ 0 ]
    				Option1
    					Identifier = 0x000D [ 13 ]
    					Length [8 bits] = 0x4 [ 4 ]
    					value = 0xC0A8C637 [ 3232286263 ]
    				Option2
    					Identifier = 0x0003 - DNS Server Address [ 3 ]
    					Length [8 bits] = 0x10 [ 16 ]
    					Value = 0xFD29CC437FB90002020C29FFFE66B4C7
    ------------------------------------------------------------------------------------------------------------→
    DL-DCCH-Message:
    	rrcConnectionReconfiguration
    		Source = \Protocol\3GPP\LTE\RRC\
    		DL-DCCH-Message
    			message = c1 = rrcConnectionReconfiguration =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = c1 = rrcConnectionReconfiguration-r8 =
    					dedicatedInfoNASList = SEQUENCE OF DedicatedInfoNAS
    						DedicatedInfoNAS(1) = 273CF56C01015C7FD5658A70ECD7585A1AC17A7641CA841F72C06CC567D274980DF884FD91B75592BF2D212DE333B64EC60FCF3FF9CA0EEEC342D4CB31E19277799AED7A84675E86984CEEAFAC3E5D79A311DE3A095A7F374AE6C3517977B17EC6D1AF77AFF3C13692FB55688D97751B730684BCE594F9A14DD513
    					radioResourceConfigDedicated
    						srb-ToAddModList = SEQUENCE OF SRB-ToAddMod
    							SRB-ToAddMod(1)
    								srb-Identity = 2
    								rlc-Config = defaultValue = NULL
    								logicalChannelConfig = defaultValue = NULL
    						drb-ToAddModList = SEQUENCE OF DRB-ToAddMod
    							DRB-ToAddMod(1)
    								eps-BearerIdentity = 5
    								drb-Identity = 1
    								pdcp-Config
    									discardTimer = infinity
    									rlc-AM
    										statusReportRequired = TRUE
    									headerCompression = notUsed = NULL
    								rlc-Config = am =
    									ul-AM-RLC
    										t-PollRetransmit = ms80
    										pollPDU = p128
    										pollByte = kB125
    										maxRetxThreshold = t4
    									dl-AM-RLC
    										t-Reordering = ms80
    										t-StatusProhibit = ms60
    								logicalChannelIdentity = 3
    								logicalChannelConfig
    									ul-SpecificParameters
    										priority = 6
    										prioritisedBitRate = kBps0
    										bucketSizeDuration = ms100
    										logicalChannelGroup = 1
    						mac-MainConfig = explicitValue =
    							ul-SCH-Config
    								maxHARQ-Tx = n5
    								periodicBSR-Timer = sf20
    								retxBSR-Timer = sf320
    								ttiBundling = FALSE
    							drx-Config = setup =
    								onDurationTimer = psf6
    								drx-InactivityTimer = psf1920
    								drx-RetransmissionTimer = psf16
    								longDRX-CycleStartOffset = sf1280 = 4
    							timeAlignmentTimerDedicated = sf750
    							phr-Config = setup =
    								periodicPHR-Timer = sf500
    								prohibitPHR-Timer = sf200
    								dl-PathlossChange = dB3
    						physicalConfigDedicated
    							tpc-PDCCH-ConfigPUCCH = setup =
    								tpc-RNTI = 0000001111111111
    								tpc-Index = indexOfFormat3 = 1
    							tpc-PDCCH-ConfigPUSCH = setup =
    								tpc-RNTI = 0000000111111010
    								tpc-Index = indexOfFormat3 = 1
    							cqi-ReportConfig
    								cqi-ReportModeAperiodic = rm30
    								nomPDSCH-RS-EPRE-Offset = 0
    								cqi-ReportPeriodic = setup =
    									cqi-PUCCH-ResourceIndex = 0
    									cqi-pmi-ConfigIndex = 25
    									cqi-FormatIndicatorPeriodic = widebandCQI = NULL
    									ri-ConfigIndex = 483
    									simultaneousAckNackAndCQI = FALSE
    							soundingRS-UL-ConfigDedicated = setup =
    								srs-Bandwidth = bw0
    								srs-HoppingBandwidth = hbw0
    								freqDomainPosition = 0
    								duration = TRUE
    								srs-ConfigIndex = 20
    								transmissionComb = 0
    								cyclicShift = cs0
    							antennaInfo = defaultValue = NULL
    ------------------------------------------------------------------------------------------------------------→
    Security Protected NAS Message DL:
    	Security Protected NAS Message DL PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Security Protected NAS Message
    			Security header type [4 bits] = 0x2 [ 2 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			MAC = 0x3CF56C01 [ 1022716929 ]
    			Sequence Number = 0x01 [ 1 ]
    			NAS message = 0x5C7FD5658A70ECD7585A1AC17A7641CA841F72C06CC567D274980DF884FD91B75592BF2D212DE333B64EC60FCF3FF9CA0EEEC342D4CB31E19277799AED7A84675E86984CEEAFAC3E5D79A311DE3A095A7F374AE6C3517977B17EC6D1AF77AFF3C13692FB55688D97751B730684BCE594F9A14DD513
    ------------------------------------------------------------------------------------------------------------→
    Ciphered NAS Message DL:
    	Ciphered NAS Message DL PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Ciphered NAS Message =
    			0x5C7FD5658A70ECD7585A1AC17A7641CA841F72C06CC567D274980DF884FD91B75592BF2D212DE333B64EC60FCF3FF9CA0EEEC342D4CB31E19277799AED7A84675E86984CEEAFAC3E5D79A311DE3A095A7F374AE6C3517977B17EC6D1AF77AFF3C13692FB55688D97751B730684BCE594F9A14DD513
    ------------------------------------------------------------------------------------------------------------→
    RRC_PDU_REQ:
    ↓	Sent from port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							rrcConnectionReconfiguration
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									c1
    										rrcConnectionReconfiguration_r8
    											measConfig = Omit
    											mobilityControlInfo = Omit
    											dedicatedInfoNASList
    												NAS_Message = '273CF56C01015C7FD5658A70ECD7585A1AC17A7641CA841F72C06CC567D274980DF884FD91B75592BF2D212DE333B64EC60FCF3FF9CA0EEEC342D4CB31E19277799AED7A84675E86984CEEAFAC3E5D79A311DE3A095A7F374AE6C3517977B17EC6D1AF77AFF3C13692FB55688D97751B730684BCE594F9A14DD513'O
    											radioResourceConfigDedicated
    												srb_ToAddModList
    													SRB_ToAddMod
    														srb_Identity = 2
    														rlc_Config
    															defaultValue = Null
    														logicalChannelConfig
    															defaultValue = Null
    												drb_ToAddModList
    													DRB_ToAddMod
    														eps_BearerIdentity = 5
    														drb_Identity = 1
    														pdcp_Config
    															discardTimer = infinity_ (7)
    															rlc_AM
    																statusReportRequired = True
    															rlc_UM = Omit
    															headerCompression
    																notUsed = Null
    															rn_IntegrityProtection_r10 = Omit
    															pdcp_SN_Size_v1130 = Omit
    															ul_DataSplitDRB_ViaSCG_r12 = Omit
    															t_Reordering_r12 = Omit
    															ul_DataSplitThreshold_r13 = Omit
    															pdcp_SN_Size_v1310 = Omit
    															statusFeedback_r13 = Omit
    														rlc_Config
    															am
    																ul_AM_RLC
    																	t_PollRetransmit = ms80 (15)
    																	pollPDU = p128 (5)
    																	pollByte = kB125 (4)
    																	maxRetxThreshold = t4 (3)
    																dl_AM_RLC
    																	t_Reordering = ms80 (16)
    																	t_StatusProhibit = ms60 (12)
    														logicalChannelIdentity = 3
    														logicalChannelConfig
    															ul_SpecificParameters
    																priority = 6
    																prioritisedBitRate = kBps0 (0)
    																bucketSizeDuration = ms100 (1)
    																logicalChannelGroup = 1
    															logicalChannelSR_Mask_r9 = Omit
    															logicalChannelSR_Prohibit_r12 = Omit
    														drb_TypeChange_r12 = Omit
    														rlc_Config_v1250 = Omit
    														rlc_Config_v1310 = Omit
    														drb_TypeLWA_r13 = Omit
    														drb_TypeLWIP_r13 = Omit
    												drb_ToReleaseList = Omit
    												mac_MainConfig
    													explicitValue
    														ul_SCH_Config
    															maxHARQ_Tx = n5 (4)
    															periodicBSR_Timer = sf20 (3)
    															retxBSR_Timer = sf320 (0)
    															ttiBundling = False
    														drx_Config
    															setup
    																onDurationTimer = psf6 (5)
    																drx_InactivityTimer = psf1920 (20)
    																drx_RetransmissionTimer = psf16 (5)
    																longDRX_CycleStartOffset
    																	sf1280 = 4
    																shortDRX = Omit
    														timeAlignmentTimerDedicated = sf750 (1)
    														phr_Config
    															setup
    																periodicPHR_Timer = sf500 (5)
    																prohibitPHR_Timer = sf200 (5)
    																dl_PathlossChange = dB3 (1)
    														sr_ProhibitTimer_r9 = Omit
    														mac_MainConfig_v1020 = Omit
    														stag_ToReleaseList_r11 = Omit
    														stag_ToAddModList_r11 = Omit
    														drx_Config_v1130 = Omit
    														e_HARQ_Pattern_r12 = Omit
    														dualConnectivityPHR = Omit
    														logicalChannelSR_Config_r12 = Omit
    														drx_Config_v1310 = Omit
    														extendedPHR2_r13 = Omit
    														eDRX_Config_CycleStartOffset_r13 = Omit
    														drx_Config_r13 = Omit
    												sps_Config = Omit
    												physicalConfigDedicated
    													pdsch_ConfigDedicated = Omit
    													pucch_ConfigDedicated = Omit
    													pusch_ConfigDedicated = Omit
    													uplinkPowerControlDedicated = Omit
    													tpc_PDCCH_ConfigPUCCH
    														setup
    															tpc_RNTI = 0000001111111111'B
    															tpc_Index
    																indexOfFormat3 = 1
    													tpc_PDCCH_ConfigPUSCH
    														setup
    															tpc_RNTI = 0000000111111010'B
    															tpc_Index
    																indexOfFormat3 = 1
    													cqi_ReportConfig
    														cqi_ReportModeAperiodic = rm30 (3)
    														nomPDSCH_RS_EPRE_Offset = 0
    														cqi_ReportPeriodic
    															setup
    																cqi_PUCCH_ResourceIndex = 0
    																cqi_pmi_ConfigIndex = 25
    																cqi_FormatIndicatorPeriodic
    																	widebandCQI = Null
    																ri_ConfigIndex = 483
    																simultaneousAckNackAndCQI = False
    													soundingRS_UL_ConfigDedicated
    														setup
    															srs_Bandwidth = bw0 (0)
    															srs_HoppingBandwidth = hbw0 (0)
    															freqDomainPosition = 0
    															duration = True
    															srs_ConfigIndex = 20
    															transmissionComb = 0
    															cyclicShift = cs0 (0)
    													antennaInfo
    														defaultValue = Null
    													schedulingRequestConfig = Omit
    													cqi_ReportConfig_v920 = Omit
    													antennaInfo_v920 = Omit
    													antennaInfo_r10 = Omit
    													antennaInfoUL_r10 = Omit
    													cif_Presence_r10 = Omit
    													cqi_ReportConfig_r10 = Omit
    													csi_RS_Config_r10 = Omit
    													pucch_ConfigDedicated_v1020 = Omit
    													pusch_ConfigDedicated_v1020 = Omit
    													schedulingRequestConfig_v1020 = Omit
    													soundingRS_UL_ConfigDedicated_v1020 = Omit
    													soundingRS_UL_ConfigDedicatedAperiodic_r10 = Omit
    													uplinkPowerControlDedicated_v1020 = Omit
    													additionalSpectrumEmissionCA_r10 = Omit
    													csi_RS_ConfigNZPToReleaseList_r11 = Omit
    													csi_RS_ConfigNZPToAddModList_r11 = Omit
    													csi_RS_ConfigZPToReleaseList_r11 = Omit
    													csi_RS_ConfigZPToAddModList_r11 = Omit
    													epdcch_Config_r11 = Omit
    													pdsch_ConfigDedicated_v1130 = Omit
    													cqi_ReportConfig_v1130 = Omit
    													pucch_ConfigDedicated_v1130 = Omit
    													pusch_ConfigDedicated_v1130 = Omit
    													uplinkPowerControlDedicated_v1130 = Omit
    													antennaInfo_v1250 = Omit
    													eimta_MainConfig_r12 = Omit
    													eimta_MainConfigPCell_r12 = Omit
    													pucch_ConfigDedicated_v1250 = Omit
    													cqi_ReportConfigPCell_v1250 = Omit
    													uplinkPowerControlDedicated_v1250 = Omit
    													pusch_ConfigDedicated_v1250 = Omit
    													csi_RS_Config_v1250 = Omit
    													pdsch_ConfigDedicated_v1280 = Omit
    													pdsch_ConfigDedicated_v1310 = Omit
    													pucch_ConfigDedicated_r13 = Omit
    													pusch_ConfigDedicated_r13 = Omit
    													pdcch_CandidateReductions_r13 = Omit
    													cqi_ReportConfig_v1310 = Omit
    													soundingRS_UL_ConfigDedicated_v1310 = Omit
    													soundingRS_UL_ConfigDedicatedUpPTsExt_r13 = Omit
    													soundingRS_UL_ConfigDedicatedAperiodic_v1310 = Omit
    													soundingRS_UL_ConfigDedicatedAperiodicUpPTsExt_r13 = Omit
    													csi_RS_Config_v1310 = Omit
    													ce_Mode_r13 = Omit
    													csi_RS_ConfigNZPToAddModListExt_r13 = Omit
    													csi_RS_ConfigNZPToReleaseListExt_r13 = Omit
    													cqi_ReportConfig_v1320 = Omit
    												rlf_TimersAndConstants_r9 = Omit
    												measSubframePatternPCell_r10 = Omit
    												neighCellsCRS_Info_r11 = Omit
    												naics_Info_r12 = Omit
    												neighCellsCRS_Info_r13 = Omit
    												rlf_TimersAndConstants_r13 = Omit
    											securityConfigHO = Omit
    											nonCriticalExtension = Omit

    UL-DCCH-Message:
    	rrcConnectionReconfigurationComplete
    		Source = \Protocol\3GPP\LTE\RRC\
    		UL-DCCH-Message
    			message = c1 = rrcConnectionReconfigurationComplete =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = rrcConnectionReconfigurationComplete-r8 =
    ←------------------------------------------------------------------------------------------------------------
    RRC_PDU_IND:
    ↑	Received on port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 422
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							rrcConnectionReconfigurationComplete
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									rrcConnectionReconfigurationComplete_r8
    										nonCriticalExtension = Omit

    SRB_COMMON_IND:
    ↑	Inter-component message: SRB -> EUTRA_PTC:SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 422
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Dcch
    						message_
    							c1
    								rrcConnectionReconfigurationComplete
    									rrc_TransactionIdentifier = 0
    									criticalExtensions
    										rrcConnectionReconfigurationComplete_r8
    											nonCriticalExtension = Omit
    				Nas = Omit

    UL-DCCH-Message:
    	ulInformationTransfer
    		Source = \Protocol\3GPP\LTE\RRC\
    		UL-DCCH-Message
    			message = c1 = ulInformationTransfer =
    				criticalExtensions = c1 = ulInformationTransfer-r8 =
    					dedicatedInfoType = dedicatedInfoNAS = 2714DCDAF701D390BB9B16B4E5
    ←------------------------------------------------------------------------------------------------------------
    Security Protected NAS Message UL:
    	Security Protected NAS Message UL PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Security Protected NAS Message
    			Security header type [4 bits] = 0x2 [ 2 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			MAC = 0x145C5A77 [ 341596791 ]
    			Sequence Number = 0x01 [ 1 ]
    			NAS message = 0x53103B1B163465
    ←------------------------------------------------------------------------------------------------------------
    Ciphered NAS Message UL:
    	Ciphered NAS Message UL PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Ciphered NAS Message =
    			0x53103B1B163465
    ←------------------------------------------------------------------------------------------------------------
    RRC_PDU_IND:
    ↑	Received on port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 2
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 424
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							ulInformationTransfer
    								criticalExtensions
    									c1
    										ulInformationTransfer_r8
    											dedicatedInfoType
    												dedicatedInfoNAS = '2714DCDAF701D390BB9B16B4E5'O
    											nonCriticalExtension = Omit

    Attach Complete:
    	Attach Complete PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Attach Complete
    			Security header type [4 bits] = 0x0 [ 0 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			Message Type [8 bits] = 0x43 - Attach Complete [ 67 ]
    			ESM message container
    				IE Length [16 bits] = 0x3 [ 3 ]
    				ESM message container contents = 0x5200C2 [ 5374146 ]
    ←------------------------------------------------------------------------------------------------------------
    Activate Default EPS Bearer Context Accept:
    	Activate Default EPS Bearer Context Accept PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Activate Default EPS Bearer Context Accept
    			EPS bearer identity [4 bits] = 0x5 [ 5 ]
    			Protocol Discriminator [4 bits] = 0x2 - EPS Session Management Messages [ 2 ]
    			Procedure transaction identifier [8 bits] = 0x0 [ 0 ]
    			Message Type [8 bits] = 0xC2 - Activate Default EPS Bearer Context Accept [ 194 ]
    ←------------------------------------------------------------------------------------------------------------
    SRB_COMMON_IND:
    ↑	Inter-component message: SRB -> EUTRA_PTC:SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 2
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 424
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			Signalling
    				Rrc = Omit
    				Nas
    					NasIndication
    						SecurityProtection
    							Status = 0010'B
    							NasCount = '00000001'O
    						Pdu
    							Msg
    								aTTACH_COMPLETE
    									securityHeaderType = 0000'B
    									protocolDiscriminator = 0111'B
    									messageType = 01000011'B
    									esmMessage
    										iei = Omit
    										iel = '0003'O
    										esmPdu = '5200C2'O
    							PiggybackedPduList
    								NAS_UL_Pdu_Type
    									Msg
    										aCTIVATE_DEFAULT_EPS_BEARER_CONTEXT_ACCEPT
    											epsBearerId = '5'H
    											protocolDiscriminator = 0010'B
    											procedureTransactionIdentifier = '00'O
    											messageType = 11000010'B
    											protocolConfigurationOptions = Omit
    											extdProtocolConfigurationOptions = Omit
    									PiggybackedPduList = Omit

    Timer Event:
    	Timer: t_WaitForUPlaneSignalling, Duration: 1.2s, Started: 17:34:59
    		Source = \Test Control\TTCN3
    		timerEvent = 6
    		fileName = C:\CT_LTE\ETSI\v41_Dev\RC1\Final PSM MKS\LTE_A_R12_IWD_16wk37\Common\IMS\IMS_PTC_CoordMsg.ttcn
    		testName = TC_9_2_1_1_7c
    		lineNo = 413
    		outStr = Timer: t_WaitForUPlaneSignalling, Duration: 1.2s, Started: 17:34:59

    Timer Event:
    	Timer: t_WaitForUPlaneSignalling, Expired: 17:35:00
    		Source = \Test Control\TTCN3
    		timerEvent = 9
    		fileName = C:\CT_LTE\ETSI\v41_Dev\RC1\Final PSM MKS\LTE_A_R12_IWD_16wk37\Common\IMS\IMS_PTC_CoordMsg.ttcn
    		testName = TC_9_2_1_1_7c
    		lineNo = 415
    		outStr = Timer: t_WaitForUPlaneSignalling, Expired: 17:35:00

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = True
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				EnquireTiming = True

    SYSTEM_CTRL_CNF:
    ↑	Received on port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_CNF
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 555
    						Subframe
    							Number = 6
    						HSFN
    							Number = 0
    				Result
    					Success = True
    			Confirm
    				EnquireTiming = True

    Timer Event:
    	Timer: t_Timer, Duration: 1.22s, Started: 17:35:00
    		Source = \Test Control\TTCN3
    		timerEvent = 6
    		fileName = C:\CT_LTE\ETSI\v41_Dev\RC1\Final PSM MKS\LTE_A_R12_IWD_16wk37\Common\EUTRA\EUTRA_RRCSteps.ttcn
    		testName = TC_9_2_1_1_7c
    		lineNo = 1418
    		outStr = Timer: t_Timer, Duration: 1.22s, Started: 17:35:00

    SRB_COMMON_REQ:
    ↓	Inter-component message: TC_SRB -> NASEMU_LTE_PTC:TC_SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 586
    						Subframe
    							Number = 4
    						HSFN
    							Number = 0
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Dcch
    						message_
    							c1
    								rrcConnectionRelease
    									rrc_TransactionIdentifier = 0
    									criticalExtensions
    										c1
    											rrcConnectionRelease_r8
    												releaseCause = other (1)
    												redirectedCarrierInfo = Omit
    												idleModeMobilityControlInfo = Omit
    												nonCriticalExtension = Omit
    				Nas = Omit

    DL-DCCH-Message:
    	rrcConnectionRelease
    		Source = \Protocol\3GPP\LTE\RRC\
    		DL-DCCH-Message
    			message = c1 = rrcConnectionRelease =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = c1 = rrcConnectionRelease-r8 =
    					releaseCause = other
    ------------------------------------------------------------------------------------------------------------→
    RRC_PDU_REQ:
    ↓	Sent from port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 586
    						Subframe
    							Number = 4
    						HSFN
    							Number = 0
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							rrcConnectionRelease
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									c1
    										rrcConnectionRelease_r8
    											releaseCause = other (1)
    											redirectedCarrierInfo = Omit
    											idleModeMobilityControlInfo = Omit
    											nonCriticalExtension = Omit

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = True
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				PdcpCount
    					Get
    						AllRBs = True

    SYSTEM_CTRL_CNF:
    ↑	Received on port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_CNF
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				Result
    					Success = True
    			Confirm
    				PdcpCount
    					Get
    						PdcpCountInfo_Type
    							RadioBearerId
    								Srb = 1
    							UL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000110'B
    							DL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000110'B
    						PdcpCountInfo_Type
    							RadioBearerId
    								Srb = 2
    							UL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000001'B
    							DL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000000'B
    						PdcpCountInfo_Type
    							RadioBearerId
    								Drb = 1
    							UL
    								Format = PdcpCount_DrbShortSQN (2)
    								Value = 00000000000000000000000000000000'B
    							DL
    								Format = PdcpCount_DrbShortSQN (2)
    								Value = 00000000000000000000000000000000'B

    MATCH_MISMATCH:
    ↑	Message Mismatch: TimingInfo_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: TimingInfo_Type
    		MATCH_MISMATCH
    			Message Mismatch: TimingInfo_Type
    				SubFrame
    					SFN
    						Number = 586
    					Subframe
    						Number = 4
    					HSFN
    						Number = 0

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 586
    						Subframe
    							Number = 4
    						HSFN
    							Number = 0
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				Cell
    					AddOrReconfigure
    						Basic = Omit
    						Active
    							C_RNTI = Omit
    							PhysicalLayerConfigUL = Omit
    							RachProcedureConfig = Omit
    							CcchDcchDtchConfig
    								MeasGapCtrl = Omit
    								DL = Omit
    								UL
    									DciInfo = Omit
    									Hopping
    										Deactivated = True
    									PUCCH_Synch
    										None = True
    									UL_GrantConfig
    										None = True
    								DrxCtrl = Omit
    								TtiBundling = Omit
    								CifPresence = Omit
    							ServingCellConfig = Omit
    							SciSchedulingConfig = Omit
    							EIMTA_Config = Omit
    							CE_Mode = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: TimingInfo_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: TimingInfo_Type
    		MATCH_MISMATCH
    			Message Mismatch: TimingInfo_Type
    				SubFrame
    					SFN
    						Number = 586
    					Subframe
    						Number = 9
    					HSFN
    						Number = 0

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 586
    						Subframe
    							Number = 9
    						HSFN
    							Number = 0
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				AS_Security
    					Release = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: TimingInfo_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: TimingInfo_Type
    		MATCH_MISMATCH
    			Message Mismatch: TimingInfo_Type
    				SubFrame
    					SFN
    						Number = 591
    					Subframe
    						Number = 9
    					HSFN
    						Number = 0

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 591
    						Subframe
    							Number = 9
    						HSFN
    							Number = 0
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				RadioBearerList
    					RadioBearer_Type
    						Id
    							Srb = 1
    						Config
    							Release = True
    					RadioBearer_Type
    						Id
    							Srb = 2
    						Config
    							Release = True
    					RadioBearer_Type
    						Id
    							Drb = 1
    						Config
    							Release = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: TimingInfo_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: TimingInfo_Type
    		MATCH_MISMATCH
    			Message Mismatch: TimingInfo_Type
    				SubFrame
    					SFN
    						Number = 592
    					Subframe
    						Number = 4
    					HSFN
    						Number = 0

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 592
    						Subframe
    							Number = 4
    						HSFN
    							Number = 0
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				RadioBearerList
    					RadioBearer_Type
    						Id
    							Srb = 1
    						Config
    							AddOrReconfigure
    								Pdcp
    									Config
    										Rb
    											Srb = True
    										TestMode
    											None = True
    								Rlc
    									Rb
    										AM
    											Tx
    												R8
    													t_PollRetransmit = ms45 (8)
    													pollPDU = pInfinity (7)
    													pollByte = kBinfinity (14)
    													maxRetxThreshold = t4 (3)
    											Rx
    												R8
    													t_Reordering = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    											ExtendedLI = Omit
    									TestMode
    										None = True
    								LogicalChannelId = 1
    								Mac
    									LogicalChannel
    										Priority = 1
    										PrioritizedBitRate = infinity_ (7)
    									TestMode
    										None = True
    								DiscardULData = Omit
    					RadioBearer_Type
    						Id
    							Srb = 2
    						Config
    							AddOrReconfigure
    								Pdcp
    									Config
    										Rb
    											Srb = True
    										TestMode
    											None = True
    								Rlc
    									Rb
    										AM
    											Tx
    												R8
    													t_PollRetransmit = ms45 (8)
    													pollPDU = pInfinity (7)
    													pollByte = kBinfinity (14)
    													maxRetxThreshold = t4 (3)
    											Rx
    												R8
    													t_Reordering = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    											ExtendedLI = Omit
    									TestMode
    										None = True
    								LogicalChannelId = 2
    								Mac
    									LogicalChannel
    										Priority = 3
    										PrioritizedBitRate = infinity_ (7)
    									TestMode
    										None = True
    								DiscardULData = Omit

    Timer Event:
    	Timer: t_Timer, Expired: 17:35:01
    		Source = \Test Control\TTCN3
    		timerEvent = 9
    		fileName = C:\CT_LTE\ETSI\v41_Dev\RC1\Final PSM MKS\LTE_A_R12_IWD_16wk37\Common\EUTRA\EUTRA_RRCSteps.ttcn
    		testName = TC_9_2_1_1_7c
    		lineNo = 1427
    		outStr = Timer: t_Timer, Expired: 17:35:01

    Timer Event:
    	Timer: t_GuardTimer, Stopped: 17:35:01
    		Source = \Test Control\TTCN3
    		timerEvent = 7
    		fileName = C:\CT_LTE\ETSI\v41_Dev\RC1\Final PSM MKS\LTE_A_R12_IWD_16wk37\Common\EUTRA\EUTRA_CommonProcedures.ttcn
    		testName = TC_9_2_1_1_7c
    		lineNo = 102
    		outStr = Timer: t_GuardTimer, Stopped: 17:35:01

    IP_ConfigReq_Type:
    ↓	Inter-component message: EUTRA_CTRL -> IP_PTC:EUTRA_CTRL
    		Source = \Test Control\TTCN3
    		IP_ConfigReq_Type
    			ChangeDrbInfo
    				PdnId = PDN_1 (0)
    				DrbInfo
    					Eutra
    						CellId = eutra_CellA (16)
    						DrbId = 1

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 67
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    IP_Indication_Type:
    ↑	Inter-component message: IP -> EUTRA_PTC:IP
    		Source = \Test Control\TTCN3
    		IP_Indication_Type
    			Cnf = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: Ut_CnfReq_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: Ut_CnfReq_Type
    		MATCH_MISMATCH
    			Message Mismatch: Ut_CnfReq_Type
    				Ut_CnfReq_Type = CNF_REQUIRED (1)

    MATCH_MISMATCH:
    ↑	Message Mismatch: Ut_CnfReq_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: Ut_CnfReq_Type
    		MATCH_MISMATCH
    			Message Mismatch: Ut_CnfReq_Type
    				Ut_CnfReq_Type = LOCAL_CNF_REQUIRED (2)

    UT_COMMON_CMD:
    ↓	Inter-component message: PTC_Ut -> MTC_LTE:PTC_Ut
    		Source = \Test Control\TTCN3
    		UT_COMMON_CMD
    			Cmd = SWITCH_OFF (99)
    			CnfReq = NO_CNF_REQUIRED (0)
    			ParameterList = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: BitStringType
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: BitStringType
    		MATCH_MISMATCH
    			Message Mismatch: BitStringType = 111'B
    				BitStringType =

    MATCH_MISMATCH:
    ↑	Message Mismatch: Ut_CnfReq_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: Ut_CnfReq_Type
    		MATCH_MISMATCH
    			Message Mismatch: Ut_CnfReq_Type
    				Ut_CnfReq_Type = CNF_REQUIRED (1)

    MATCH_MISMATCH:
    ↑	Message Mismatch: Ut_CnfReq_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: Ut_CnfReq_Type
    		MATCH_MISMATCH
    			Message Mismatch: Ut_CnfReq_Type
    				Ut_CnfReq_Type = LOCAL_CNF_REQUIRED (2)

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				Cell
    					AddOrReconfigure
    						Basic = Omit
    						Active
    							C_RNTI = Omit
    							PhysicalLayerConfigUL = Omit
    							RachProcedureConfig = Omit
    							CcchDcchDtchConfig
    								MeasGapCtrl = Omit
    								DL = Omit
    								UL
    									DciInfo
    										Imcs
    											Value = 9
    										TransRetransmissionList
    											UL_TransRetransmission_Type
    												NewTransmission = True
    										FreqDomainSchedul
    											FirstRbIndex = 0
    											Nprb = 25
    										RepetitionNumber = Omit
    									Hopping
    										Deactivated = True
    									PUCCH_Synch
    										None = True
    									UL_GrantConfig
    										OnSR_Reception = True
    								DrxCtrl = Omit
    								TtiBundling = Omit
    								CifPresence = Omit
    							ServingCellConfig = Omit
    							SciSchedulingConfig = Omit
    							EIMTA_Config = Omit
    							CE_Mode = Omit

    UT_SYSTEM_REQ:
    ↓	Sent from port: MTC_LTE:Ut
    		Source = \Test Control\TTCN3
    		UT_SYSTEM_REQ
    			Cmd
    				MMI
    					Cmd = 'SWITCH_OFF'
    					ParameterList = Omit
    			CnfRequired = NO_CNF_REQUIRED (0)

    UL-CCCH-Message:
    	rrcConnectionRequest
    		Source = \Protocol\3GPP\LTE\RRC\
    		UL-CCCH-Message
    			message = c1 = rrcConnectionRequest =
    				criticalExtensions = rrcConnectionRequest-r8 =
    					ue-Identity = s-TMSI =
    						mmec = 00000001
    						m-TMSI = 11000010001101000101011001111000
    					establishmentCause = mo-Signalling
    					spare = 0
    ←------------------------------------------------------------------------------------------------------------
    RRC_PDU_IND:
    ↑	Received on port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 0
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 305
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			RrcPdu
    				Ccch
    					message_
    						c1
    							rrcConnectionRequest
    								criticalExtensions
    									rrcConnectionRequest_r8
    										ue_Identity
    											s_TMSI
    												mmec = 00000001'B
    												m_TMSI = 11000010001101000101011001111000'B
    										establishmentCause = mo_Signalling (3)
    										spare = 0'B

    SRB_COMMON_IND:
    ↑	Inter-component message: SRB -> EUTRA_PTC:SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 0
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 305
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Ccch
    						message_
    							c1
    								rrcConnectionRequest
    									criticalExtensions
    										rrcConnectionRequest_r8
    											ue_Identity
    												s_TMSI
    													mmec = 00000001'B
    													m_TMSI = 11000010001101000101011001111000'B
    											establishmentCause = mo_Signalling (3)
    											spare = 0'B
    				Nas = Omit

    UL-DCCH-Message:
    	rrcConnectionSetupComplete
    		Source = \Protocol\3GPP\LTE\RRC\
    		UL-DCCH-Message
    			message = c1 = rrcConnectionSetupComplete =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = c1 = rrcConnectionSetupComplete-r8 =
    					selectedPLMN-Identity = 1
    					dedicatedInfoNAS = 17347A8263020745090BF600F110800101C2345678
    ←------------------------------------------------------------------------------------------------------------
    Security Protected NAS Message UL:
    	Security Protected NAS Message UL PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Security Protected NAS Message
    			Security header type [4 bits] = 0x1 [ 1 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			MAC = 0x347A8263 [ 880444003 ]
    			Sequence Number = 0x02 [ 2 ]
    			NAS message = 0x0745090BF600F110800101C2345678
    ←------------------------------------------------------------------------------------------------------------
    Detach Request UE Originating:
    	Detach Request UE Originating PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Detach Request UE Originating
    			Security header type [4 bits] = 0x0 [ 0 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			Message Type [8 bits] = 0x45 - Detach Request UE Originating [ 69 ]
    			NAS key set identifier
    				Type of security context flag [1 bit] = 0x0 [ 0 ]
    				key sequence indicator [3 bits] = 0x0 [ 0 ]
    			Detach Type
    				switch off [1 bit] = 0x1 - switch off [ 1 ]
    				EPS Detach type [3 bits] = 0x1 - EPS Detach [ 1 ]
    			GUTI or IMSI
    				IE Length [8 bits] = 0xB [ 11 ]
    				constant / IMSI Identity Digit 1 [4 bits] = 0xF [ 15 ]
    				Odd / Even Indicator [1 bit] = 0x0 [ 0 ]
    				EPS Type of Identity [3 bits] = 0x6 - GUTI [ 6 ]
    				Mobile Country Code 1st and 2nd  Digits = 0x00 [ 0 ]
    				Mobile Network Code 3rd Digit = 0xF [ 15 ]
    				Mobile Country Code 3rd Digit = 0x1 [ 1 ]
    				Mobile Network Code 1st and 2nd  Digits = 0x10 [ 16 ]
    				MME group Id = 0x8001 [ 32769 ]
    				MME code = 0x01 [ 1 ]
    				M-TMSI = 0xC2345678 [ 3258209912 ]
    ←------------------------------------------------------------------------------------------------------------
    RRC_PDU_IND:
    ↑	Received on port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 308
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							rrcConnectionSetupComplete
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									c1
    										rrcConnectionSetupComplete_r8
    											selectedPLMN_Identity = 1
    											registeredMME = Omit
    											dedicatedInfoNAS = '17347A8263020745090BF600F110800101C2345678'O
    											nonCriticalExtension = Omit

    SRB_COMMON_IND:
    ↑	Inter-component message: SRB -> EUTRA_PTC:SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 308
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Dcch
    						message_
    							c1
    								rrcConnectionSetupComplete
    									rrc_TransactionIdentifier = 0
    									criticalExtensions
    										c1
    											rrcConnectionSetupComplete_r8
    												selectedPLMN_Identity = 1
    												registeredMME = Omit
    												dedicatedInfoNAS = '17347A8263020745090BF600F110800101C2345678'O
    												nonCriticalExtension = Omit
    				Nas
    					NasIndication
    						SecurityProtection
    							Status = 0001'B
    							NasCount = '00000002'O
    						Pdu
    							Msg
    								dETACH_REQUEST_MO
    									securityHeaderType = 0000'B
    									protocolDiscriminator = 0111'B
    									messageType = 01000101'B
    									asmeNasKeySetId
    										iei = Omit
    										tsc = 0'B
    										nasKeySetId = 000'B
    									detachType
    										switchOff = 1'B
    										typeOfDetach = 001'B
    									epsMobileIdentity
    										iei = Omit
    										iel = '0B'O
    										idDigit1 = 1111'B
    										oddEvenInd = 0'B
    										typeOfId = 110'B
    										otherDigits = '00F110800101C2345678'O
    							PiggybackedPduList = Omit

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = True
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				Cell
    					AddOrReconfigure
    						Basic = Omit
    						Active
    							C_RNTI = Omit
    							PhysicalLayerConfigUL = Omit
    							RachProcedureConfig = Omit
    							CcchDcchDtchConfig
    								MeasGapCtrl = Omit
    								DL = Omit
    								UL
    									DciInfo = Omit
    									Hopping
    										Deactivated = True
    									PUCCH_Synch
    										Auto
    											TimingAdvance = 31
    											TA_Period = 600
    											TA_Repetition
    												Continuous = True
    									UL_GrantConfig = Omit
    								DrxCtrl = Omit
    								TtiBundling = Omit
    								CifPresence = Omit
    							ServingCellConfig = Omit
    							SciSchedulingConfig = Omit
    							EIMTA_Config = Omit
    							CE_Mode = Omit

    SYSTEM_CTRL_CNF:
    ↑	Received on port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_CNF
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				Result
    					Success = True
    			Confirm
    				Cell = True

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = True
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				EnquireTiming = True

    SYSTEM_CTRL_CNF:
    ↑	Received on port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_CNF
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 310
    						Subframe
    							Number = 6
    						HSFN
    							Number = 0
    				Result
    					Success = True
    			Confirm
    				EnquireTiming = True

    Timer Event:
    	Timer: t_Timer, Duration: 1.22s, Started: 17:35:08
    		Source = \Test Control\TTCN3
    		timerEvent = 6
    		fileName = C:\CT_LTE\ETSI\v41_Dev\RC1\Final PSM MKS\LTE_A_R12_IWD_16wk37\Common\EUTRA\EUTRA_RRCSteps.ttcn
    		testName = TC_9_2_1_1_7c
    		lineNo = 1418
    		outStr = Timer: t_Timer, Duration: 1.22s, Started: 17:35:08

    SRB_COMMON_REQ:
    ↓	Inter-component message: TC_SRB -> NASEMU_LTE_PTC:TC_SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 341
    						Subframe
    							Number = 4
    						HSFN
    							Number = 0
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Dcch
    						message_
    							c1
    								rrcConnectionRelease
    									rrc_TransactionIdentifier = 0
    									criticalExtensions
    										c1
    											rrcConnectionRelease_r8
    												releaseCause = other (1)
    												redirectedCarrierInfo = Omit
    												idleModeMobilityControlInfo = Omit
    												nonCriticalExtension = Omit
    				Nas = Omit

    DL-DCCH-Message:
    	rrcConnectionRelease
    		Source = \Protocol\3GPP\LTE\RRC\
    		DL-DCCH-Message
    			message = c1 = rrcConnectionRelease =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = c1 = rrcConnectionRelease-r8 =
    					releaseCause = other
    ------------------------------------------------------------------------------------------------------------→
    RRC_PDU_REQ:
    ↓	Sent from port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 341
    						Subframe
    							Number = 4
    						HSFN
    							Number = 0
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							rrcConnectionRelease
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									c1
    										rrcConnectionRelease_r8
    											releaseCause = other (1)
    											redirectedCarrierInfo = Omit
    											idleModeMobilityControlInfo = Omit
    											nonCriticalExtension = Omit

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = True
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				PdcpCount
    					Get
    						AllRBs = True

    SYSTEM_CTRL_CNF:
    ↑	Received on port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_CNF
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				Result
    					Success = True
    			Confirm
    				PdcpCount
    					Get
    						PdcpCountInfo_Type
    							RadioBearerId
    								Srb = 1
    							UL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000001'B
    							DL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000000'B
    						PdcpCountInfo_Type
    							RadioBearerId
    								Srb = 2
    							UL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000000'B
    							DL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000000'B
    						PdcpCountInfo_Type
    							RadioBearerId
    								Drb = 1
    							UL
    								Format = PdcpCount_DrbShortSQN (2)
    								Value = 00000000000000000000000000000000'B
    							DL
    								Format = PdcpCount_DrbShortSQN (2)
    								Value = 00000000000000000000000000000000'B

    MATCH_MISMATCH:
    ↑	Message Mismatch: TimingInfo_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: TimingInfo_Type
    		MATCH_MISMATCH
    			Message Mismatch: TimingInfo_Type
    				SubFrame
    					SFN
    						Number = 341
    					Subframe
    						Number = 4
    					HSFN
    						Number = 0

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 341
    						Subframe
    							Number = 4
    						HSFN
    							Number = 0
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				Cell
    					AddOrReconfigure
    						Basic = Omit
    						Active
    							C_RNTI = Omit
    							PhysicalLayerConfigUL = Omit
    							RachProcedureConfig = Omit
    							CcchDcchDtchConfig
    								MeasGapCtrl = Omit
    								DL = Omit
    								UL
    									DciInfo = Omit
    									Hopping
    										Deactivated = True
    									PUCCH_Synch
    										None = True
    									UL_GrantConfig
    										None = True
    								DrxCtrl = Omit
    								TtiBundling = Omit
    								CifPresence = Omit
    							ServingCellConfig = Omit
    							SciSchedulingConfig = Omit
    							EIMTA_Config = Omit
    							CE_Mode = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: TimingInfo_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: TimingInfo_Type
    		MATCH_MISMATCH
    			Message Mismatch: TimingInfo_Type
    				SubFrame
    					SFN
    						Number = 341
    					Subframe
    						Number = 9
    					HSFN
    						Number = 0

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 341
    						Subframe
    							Number = 9
    						HSFN
    							Number = 0
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				AS_Security
    					Release = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: TimingInfo_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: TimingInfo_Type
    		MATCH_MISMATCH
    			Message Mismatch: TimingInfo_Type
    				SubFrame
    					SFN
    						Number = 346
    					Subframe
    						Number = 9
    					HSFN
    						Number = 0

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 346
    						Subframe
    							Number = 9
    						HSFN
    							Number = 0
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				RadioBearerList
    					RadioBearer_Type
    						Id
    							Srb = 1
    						Config
    							Release = True
    					RadioBearer_Type
    						Id
    							Srb = 2
    						Config
    							Release = True
    					RadioBearer_Type
    						Id
    							Drb = 1
    						Config
    							Release = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: TimingInfo_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: TimingInfo_Type
    		MATCH_MISMATCH
    			Message Mismatch: TimingInfo_Type
    				SubFrame
    					SFN
    						Number = 347
    					Subframe
    						Number = 4
    					HSFN
    						Number = 0

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 347
    						Subframe
    							Number = 4
    						HSFN
    							Number = 0
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				RadioBearerList
    					RadioBearer_Type
    						Id
    							Srb = 1
    						Config
    							AddOrReconfigure
    								Pdcp
    									Config
    										Rb
    											Srb = True
    										TestMode
    											None = True
    								Rlc
    									Rb
    										AM
    											Tx
    												R8
    													t_PollRetransmit = ms45 (8)
    													pollPDU = pInfinity (7)
    													pollByte = kBinfinity (14)
    													maxRetxThreshold = t4 (3)
    											Rx
    												R8
    													t_Reordering = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    											ExtendedLI = Omit
    									TestMode
    										None = True
    								LogicalChannelId = 1
    								Mac
    									LogicalChannel
    										Priority = 1
    										PrioritizedBitRate = infinity_ (7)
    									TestMode
    										None = True
    								DiscardULData = Omit
    					RadioBearer_Type
    						Id
    							Srb = 2
    						Config
    							AddOrReconfigure
    								Pdcp
    									Config
    										Rb
    											Srb = True
    										TestMode
    											None = True
    								Rlc
    									Rb
    										AM
    											Tx
    												R8
    													t_PollRetransmit = ms45 (8)
    													pollPDU = pInfinity (7)
    													pollByte = kBinfinity (14)
    													maxRetxThreshold = t4 (3)
    											Rx
    												R8
    													t_Reordering = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    											ExtendedLI = Omit
    									TestMode
    										None = True
    								LogicalChannelId = 2
    								Mac
    									LogicalChannel
    										Priority = 3
    										PrioritizedBitRate = infinity_ (7)
    									TestMode
    										None = True
    								DiscardULData = Omit

    Timer Event:
    	Timer: t_Timer, Expired: 17:35:09
    		Source = \Test Control\TTCN3
    		timerEvent = 9
    		fileName = C:\CT_LTE\ETSI\v41_Dev\RC1\Final PSM MKS\LTE_A_R12_IWD_16wk37\Common\EUTRA\EUTRA_RRCSteps.ttcn
    		testName = TC_9_2_1_1_7c
    		lineNo = 1427
    		outStr = Timer: t_Timer, Expired: 17:35:09

    MATCH_MISMATCH:
    ↑	Message Mismatch: Ut_CnfReq_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: Ut_CnfReq_Type
    		MATCH_MISMATCH
    			Message Mismatch: Ut_CnfReq_Type
    				Ut_CnfReq_Type = CNF_REQUIRED (1)

    UT_COMMON_CMD:
    ↓	Inter-component message: PTC_Ut -> MTC_LTE:PTC_Ut
    		Source = \Test Control\TTCN3
    		UT_COMMON_CMD
    			Cmd = PSM (78)
    			CnfReq = NO_CNF_REQUIRED (0)
    			ParameterList
    				Ut_Parameter_Type
    					Name = 'PSM'
    					Value = '1,,,,00100010'

    MATCH_MISMATCH:
    ↑	Message Mismatch: Ut_CnfReq_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: Ut_CnfReq_Type
    		MATCH_MISMATCH
    			Message Mismatch: Ut_CnfReq_Type
    				Ut_CnfReq_Type = LOCAL_CNF_REQUIRED (2)

    MATCH_MISMATCH:
    ↑	Message Mismatch: Ut_CnfReq_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: Ut_CnfReq_Type
    		MATCH_MISMATCH
    			Message Mismatch: Ut_CnfReq_Type
    				Ut_CnfReq_Type = CNF_REQUIRED (1)

    MATCH_MISMATCH:
    ↑	Message Mismatch: Ut_CnfReq_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: Ut_CnfReq_Type
    		MATCH_MISMATCH
    			Message Mismatch: Ut_CnfReq_Type
    				Ut_CnfReq_Type = LOCAL_CNF_REQUIRED (2)

    TTCN Test Step:
    	Preamble
    		Source = \Test Control\TTCN3
    		recordType = 24
    		summary = Preamble

    Verdict Intermediate Pass:
    	Intermediate verdict: (PASS)
    	TTCN-3 message: initial preliminary pass
    		Source = \Test Control\TTCN3
    		IntermediateVerdict = (Pass)
    		summary = Intermediate verdict: (PASS)
    		TTCN-3 message: initial preliminary pass

    TTCN Test Step:
    	Step 1
    		Source = \Test Control\TTCN3
    		recordType = 24
    		summary = Step 1

    IMS_IPCAN_Coordination_MSG:
    ↑	Inter-component message: IPCAN -> IMS_PTC:IPCAN
    		Source = \Test Control\TTCN3
    		IMS_IPCAN_Coordination_MSG
    			IPCAN_IMS_Control
    				Reset = True

    IP_ConfigReq_Type:
    ↓	Inter-component message: EUTRA_CTRL -> IP_PTC:EUTRA_CTRL
    		Source = \Test Control\TTCN3
    		IP_ConfigReq_Type
    			StartIP
    				PdnId = PDN_1 (0)
    				DrbInfo
    					Eutra
    						CellId = eutra_CellA (16)
    						DrbId = 1

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 67
    					Remote = Omit
    				Req
    					UDP
    						Close = True

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 67
    					Remote = Omit
    				Req
    					UDP
    						Close = True

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 53
    					Remote = Omit
    				Req
    					UDP
    						Close = True

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 53
    					Remote = Omit
    				Req
    					UDP
    						Close = True

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: CharacterStringType
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: CharacterStringType
    		MATCH_MISMATCH
    			Message Mismatch: CharacterStringType
    				ServerAddr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 53
    					Remote = Omit
    				Req
    					UDP
    						Close = True

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 53
    					Remote = Omit
    				Req
    					UDP
    						Close = True

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = icmpv6 (3)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = Omit
    					Remote = Omit
    				Req
    					ICMP
    						Close = True

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = icmpv6 (3)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = Omit
    					Remote = Omit
    				Req
    					ICMP
    						Close = True

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = icmpv6 (3)
    					Local
    						IpAddr
    							V6
    								Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = Omit
    					Remote = Omit
    				Req
    					ICMP
    						Close = True

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = icmpv6 (3)
    					Local
    						IpAddr
    							V6
    								Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = Omit
    					Remote = Omit
    				Req
    					ICMP
    						Close = True

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 67
    					Remote = Omit
    				Req
    					UDP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 67
    					Remote = Omit
    				Req
    					UDP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    MESSAGE_MISMATCH:
    ↑	Message Mismatch: IP_SOCKET_IND
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_SOCKET_IND
    		MESSAGE_MISMATCH
    			Message Mismatch: IP_SOCKET_IND
    				CTRL
    					ConnectionId
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 67
    						Remote
    							IpAddr = Omit
    							Port = Omit
    					Ind
    						UDP
    							SocketCnf = True

    IP_SOCKET_IND:
    ↑	Received on port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 67
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					UDP
    						SocketCnf = True

    IP_SOCKET_IND:
    ↑	Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 67
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					UDP
    						SocketCnf = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 67
    				Remote = Omit

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 67
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 53
    					Remote = Omit
    				Req
    					UDP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 53
    					Remote = Omit
    				Req
    					UDP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    MESSAGE_MISMATCH:
    ↑	Message Mismatch: IP_SOCKET_IND
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_SOCKET_IND
    		MESSAGE_MISMATCH
    			Message Mismatch: IP_SOCKET_IND
    				CTRL
    					ConnectionId
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 53
    						Remote
    							IpAddr = Omit
    							Port = Omit
    					Ind
    						UDP
    							SocketCnf = True

    IP_SOCKET_IND:
    ↑	Received on port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 53
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					UDP
    						SocketCnf = True

    IP_SOCKET_IND:
    ↑	Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 53
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					UDP
    						SocketCnf = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 67
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: CharacterStringType
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: CharacterStringType
    		MATCH_MISMATCH
    			Message Mismatch: CharacterStringType
    				ICMPv6_ServerAddress = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 53
    					Remote = Omit
    				Req
    					UDP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 53
    					Remote = Omit
    				Req
    					UDP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    MESSAGE_MISMATCH:
    ↑	Message Mismatch: IP_SOCKET_IND
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_SOCKET_IND
    		MESSAGE_MISMATCH
    			Message Mismatch: IP_SOCKET_IND
    				CTRL
    					ConnectionId
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 53
    						Remote
    							IpAddr = Omit
    							Port = Omit
    					Ind
    						UDP
    							SocketCnf = True

    IP_SOCKET_IND:
    ↑	Received on port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 53
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					UDP
    						SocketCnf = True

    IP_SOCKET_IND:
    ↑	Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 53
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					UDP
    						SocketCnf = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 67
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = icmpv6 (3)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = Omit
    					Remote = Omit
    				Req
    					ICMP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = icmpv6 (3)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = Omit
    					Remote = Omit
    				Req
    					ICMP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    MESSAGE_MISMATCH:
    ↑	Message Mismatch: IP_SOCKET_IND
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_SOCKET_IND
    		MESSAGE_MISMATCH
    			Message Mismatch: IP_SOCKET_IND
    				CTRL
    					ConnectionId
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote
    							IpAddr = Omit
    							Port = Omit
    					Ind
    						ICMP
    							SocketCnf = True

    IP_SOCKET_IND:
    ↑	Received on port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = icmpv6 (3)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = Omit
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					ICMP
    						SocketCnf = True

    IP_SOCKET_IND:
    ↑	Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = icmpv6 (3)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = Omit
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					ICMP
    						SocketCnf = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 67
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = icmpv6 (3)
    					Local
    						IpAddr
    							V6
    								Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = Omit
    					Remote = Omit
    				Req
    					ICMP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = icmpv6 (3)
    					Local
    						IpAddr
    							V6
    								Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = Omit
    					Remote = Omit
    				Req
    					ICMP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    MESSAGE_MISMATCH:
    ↑	Message Mismatch: IP_SOCKET_IND
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_SOCKET_IND
    		MESSAGE_MISMATCH
    			Message Mismatch: IP_SOCKET_IND
    				CTRL
    					ConnectionId
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote
    							IpAddr = Omit
    							Port = Omit
    					Ind
    						ICMP
    							SocketCnf = True

    IP_SOCKET_IND:
    ↑	Received on port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = icmpv6 (3)
    					Local
    						IpAddr
    							V6
    								Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = Omit
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					ICMP
    						SocketCnf = True

    IP_SOCKET_IND:
    ↑	Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = icmpv6 (3)
    					Local
    						IpAddr
    							V6
    								Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = Omit
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					ICMP
    						SocketCnf = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 67
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 5060
    					Remote = Omit
    				Req
    					UDP
    						Close = True

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 5060
    					Remote = Omit
    				Req
    					UDP
    						Close = True

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 67
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 5060
    					Remote = Omit
    				Req
    					UDP
    						Close = True

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 5060
    					Remote = Omit
    				Req
    					UDP
    						Close = True

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 67
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = tcp (1)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 5060
    					Remote = Omit
    				Req
    					TCP
    						Close = True

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = tcp (1)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 5060
    					Remote = Omit
    				Req
    					TCP
    						Close = True

    MESSAGE_MISMATCH:
    ↑	Message Mismatch: IP_SOCKET_IND
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_SOCKET_IND
    		MESSAGE_MISMATCH
    			Message Mismatch: IP_SOCKET_IND
    				CTRL
    					ConnectionId
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					Ind
    						TCP
    							CloseCnf = True

    IP_SOCKET_IND:
    ↑	Received on port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = tcp (1)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 5060
    					Remote = Omit
    				Ind
    					TCP
    						CloseCnf = True

    IP_SOCKET_IND:
    ↑	Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = tcp (1)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 5060
    					Remote = Omit
    				Ind
    					TCP
    						CloseCnf = True

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 67
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = tcp (1)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 5060
    					Remote = Omit
    				Req
    					TCP
    						Close = True

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = tcp (1)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 5060
    					Remote = Omit
    				Req
    					TCP
    						Close = True

    MESSAGE_MISMATCH:
    ↑	Message Mismatch: IP_SOCKET_IND
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_SOCKET_IND
    		MESSAGE_MISMATCH
    			Message Mismatch: IP_SOCKET_IND
    				CTRL
    					ConnectionId
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					Ind
    						TCP
    							CloseCnf = True

    IP_SOCKET_IND:
    ↑	Received on port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = tcp (1)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 5060
    					Remote = Omit
    				Ind
    					TCP
    						CloseCnf = True

    IP_SOCKET_IND:
    ↑	Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = tcp (1)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 5060
    					Remote = Omit
    				Ind
    					TCP
    						CloseCnf = True

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 67
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 5060
    					Remote = Omit
    				Req
    					UDP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 5060
    					Remote = Omit
    				Req
    					UDP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    MESSAGE_MISMATCH:
    ↑	Message Mismatch: IP_SOCKET_IND
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_SOCKET_IND
    		MESSAGE_MISMATCH
    			Message Mismatch: IP_SOCKET_IND
    				CTRL
    					ConnectionId
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote
    							IpAddr = Omit
    							Port = Omit
    					Ind
    						UDP
    							SocketCnf = True

    IP_SOCKET_IND:
    ↑	Received on port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 5060
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					UDP
    						SocketCnf = True

    IP_SOCKET_IND:
    ↑	Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 5060
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					UDP
    						SocketCnf = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.Port
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.Port
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.Port
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 67
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 5060
    					Remote = Omit
    				Req
    					UDP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 5060
    					Remote = Omit
    				Req
    					UDP
    						SocketReq
    							SockOptList
    								IP_SockOpt_Type
    									SO_BROADCAST = True
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500

    MESSAGE_MISMATCH:
    ↑	Message Mismatch: IP_SOCKET_IND
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_SOCKET_IND
    		MESSAGE_MISMATCH
    			Message Mismatch: IP_SOCKET_IND
    				CTRL
    					ConnectionId
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote
    							IpAddr = Omit
    							Port = Omit
    					Ind
    						UDP
    							SocketCnf = True

    IP_SOCKET_IND:
    ↑	Received on port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 5060
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					UDP
    						SocketCnf = True

    IP_SOCKET_IND:
    ↑	Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_IND
    			CTRL
    				ConnectionId
    					Protocol = udp (0)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 5060
    					Remote
    						IpAddr = Omit
    						Port = Omit
    				Ind
    					UDP
    						SocketCnf = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Local.IpAddr
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 67
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = tcp (1)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 5060
    					Remote = Omit
    				Req
    					TCP
    						Listen
    							SockOptList
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500
    							Application = ims (0)
    							TLSInfo = Omit

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = tcp (1)
    					Local
    						IpAddr
    							V4
    								Addr = '192.168.198.55'
    						Port = 5060
    					Remote = Omit
    				Req
    					TCP
    						Listen
    							SockOptList
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500
    							Application = ims (0)
    							TLSInfo = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 67
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    IP_SOCKET_REQ:
    ↓	Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = tcp (1)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 5060
    					Remote = Omit
    				Req
    					TCP
    						Listen
    							SockOptList
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500
    							Application = ims (0)
    							TLSInfo = Omit

    IP_SOCKET_REQ:
    ↓	Sent from port: IPMUX_PTC:IP_SOCK
    		Source = \Test Control\TTCN3
    		IP_SOCKET_REQ
    			CTRL
    				ConnectionId
    					Protocol = tcp (1)
    					Local
    						IpAddr
    							V6
    								Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    								ScopeId = Omit
    						Port = 5060
    					Remote = Omit
    				Req
    					TCP
    						Listen
    							SockOptList
    								IP_SockOpt_Type
    									IP_MTU_SIZE = 1500
    							Application = ims (0)
    							TLSInfo = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 67
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    							 =
    					Port = 5060
    				Remote = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: IP_Connection_Type.Protocol
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IP_Connection_Type.Protocol
    		MATCH_MISMATCH
    			Message Mismatch: IP_Connection_Type.Protocol
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 67
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    IP_Indication_Type:
    ↑	Inter-component message: IP -> EUTRA_PTC:IP
    		Source = \Test Control\TTCN3
    		IP_Indication_Type
    			Cnf = True

    MESSAGE_MISMATCH:
    ↑	Message Mismatch: IMS_CONFIG_REQ
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IMS_CONFIG_REQ
    		MESSAGE_MISMATCH
    			Message Mismatch: IMS_CONFIG_REQ
    				RegInfoRelease = True

    MESSAGE_MISMATCH:
    ↑	Message Mismatch: IMS_CONFIG_REQ
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IMS_CONFIG_REQ
    		MESSAGE_MISMATCH
    			Message Mismatch: IMS_CONFIG_REQ
    				RegInfoRelease = True

    MESSAGE_MISMATCH:
    ↑	Message Mismatch: IMS_CONFIG_REQ
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: IMS_CONFIG_REQ
    		MESSAGE_MISMATCH
    			Message Mismatch: IMS_CONFIG_REQ
    				RegInfoRelease = True

    IMS_CONFIG_REQ:
    ↓	Inter-component message: IMS_CTRL -> IP_PTC:IMS_CTRL
    		Source = \Test Control\TTCN3
    		IMS_CONFIG_REQ
    			RegInfoRelease = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: Ut_CnfReq_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: Ut_CnfReq_Type
    		MATCH_MISMATCH
    			Message Mismatch: Ut_CnfReq_Type
    				Ut_CnfReq_Type = CNF_REQUIRED (1)

    MATCH_MISMATCH:
    ↑	Message Mismatch: Ut_CnfReq_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: Ut_CnfReq_Type
    		MATCH_MISMATCH
    			Message Mismatch: Ut_CnfReq_Type
    				Ut_CnfReq_Type = LOCAL_CNF_REQUIRED (2)

    IMS_CONFIG_CNF:
    ↑	Inter-component message: IMS_CTRL -> IMS_PTC:IMS_CTRL
    		Source = \Test Control\TTCN3
    		IMS_CONFIG_CNF
    			RegInfoRelease = True

    TTCN Test Step:
    	Step 2
    		Source = \Test Control\TTCN3
    		recordType = 24
    		summary = Step 2

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				Cell
    					AddOrReconfigure
    						Basic = Omit
    						Active
    							C_RNTI = Omit
    							PhysicalLayerConfigUL = Omit
    							RachProcedureConfig = Omit
    							CcchDcchDtchConfig
    								MeasGapCtrl = Omit
    								DL = Omit
    								UL
    									DciInfo
    										Imcs
    											Value = 9
    										TransRetransmissionList
    											UL_TransRetransmission_Type
    												NewTransmission = True
    										FreqDomainSchedul
    											FirstRbIndex = 0
    											Nprb = 25
    										RepetitionNumber = Omit
    									Hopping
    										Deactivated = True
    									PUCCH_Synch
    										None = True
    									UL_GrantConfig
    										OnSR_Reception = True
    								DrxCtrl = Omit
    								TtiBundling = Omit
    								CifPresence = Omit
    							ServingCellConfig = Omit
    							SciSchedulingConfig = Omit
    							EIMTA_Config = Omit
    							CE_Mode = Omit

    UT_SYSTEM_REQ:
    ↓	Sent from port: MTC_LTE:Ut
    		Source = \Test Control\TTCN3
    		UT_SYSTEM_REQ
    			Cmd
    				AT = 'AT+CPSMS=1,,,,00100010'
    			CnfRequired = NO_CNF_REQUIRED (0)

    UT_COMMON_CMD:
    ↓	Inter-component message: PTC_Ut -> MTC_LTE:PTC_Ut
    		Source = \Test Control\TTCN3
    		UT_COMMON_CMD
    			Cmd = SWITCH_ON (100)
    			CnfReq = NO_CNF_REQUIRED (0)
    			ParameterList = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: Ut_CnfReq_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: Ut_CnfReq_Type
    		MATCH_MISMATCH
    			Message Mismatch: Ut_CnfReq_Type
    				Ut_CnfReq_Type = CNF_REQUIRED (1)

    MATCH_MISMATCH:
    ↑	Message Mismatch: Ut_CnfReq_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: Ut_CnfReq_Type
    		MATCH_MISMATCH
    			Message Mismatch: Ut_CnfReq_Type
    				Ut_CnfReq_Type = LOCAL_CNF_REQUIRED (2)

    UT_SYSTEM_REQ:
    ↓	Sent from port: MTC_LTE:Ut
    		Source = \Test Control\TTCN3
    		UT_SYSTEM_REQ
    			Cmd
    				MMI
    					Cmd = 'SWITCH_ON'
    					ParameterList = Omit
    			CnfRequired = NO_CNF_REQUIRED (0)

    UL-CCCH-Message:
    	rrcConnectionRequest
    		Source = \Protocol\3GPP\LTE\RRC\
    		UL-CCCH-Message
    			message = c1 = rrcConnectionRequest =
    				criticalExtensions = rrcConnectionRequest-r8 =
    					ue-Identity = randomValue = 0011100011111101110111011000011100111110
    					establishmentCause = mo-Signalling
    					spare = 0
    ←------------------------------------------------------------------------------------------------------------
    RRC_PDU_IND:
    ↑	Received on port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 0
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 920
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			RrcPdu
    				Ccch
    					message_
    						c1
    							rrcConnectionRequest
    								criticalExtensions
    									rrcConnectionRequest_r8
    										ue_Identity
    											randomValue = 0011100011111101110111011000011100111110'B
    										establishmentCause = mo_Signalling (3)
    										spare = 0'B

    SRB_COMMON_IND:
    ↑	Inter-component message: SRB -> EUTRA_PTC:SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 0
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 920
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Ccch
    						message_
    							c1
    								rrcConnectionRequest
    									criticalExtensions
    										rrcConnectionRequest_r8
    											ue_Identity
    												randomValue = 0011100011111101110111011000011100111110'B
    											establishmentCause = mo_Signalling (3)
    											spare = 0'B
    				Nas = Omit

    TTCN Test Step:
    	Step 3
    		Source = \Test Control\TTCN3
    		recordType = 24
    		summary = Step 3

    TTCN Test Step:
    	Step 4
    		Source = \Test Control\TTCN3
    		recordType = 24
    		summary = Step 4

    UL-DCCH-Message:
    	rrcConnectionSetupComplete
    		Source = \Protocol\3GPP\LTE\RRC\
    		UL-DCCH-Message
    			message = c1 = rrcConnectionSetupComplete =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = c1 = rrcConnectionSetupComplete-r8 =
    					selectedPLMN-Identity = 1
    					registeredMME
    						mmegi = 1000000000000001
    						mmec = 00000001
    					dedicatedInfoNAS = 17B4ACDBCE030741010BF600F110800101C234567805F070C0401100290208D03127238080211001000010810600000000830600000000000D00000300000A000005000010005200F11000015C0A003103E5E03E11035758A6200C601404EF65233B8878D2F28040080402600000021F00E0C16A01225E0160
    					nonCriticalExtension
    						nonCriticalExtension
    							gummei-Type-r10 = native
    ←------------------------------------------------------------------------------------------------------------
    Security Protected NAS Message UL:
    	Security Protected NAS Message UL PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Security Protected NAS Message
    			Security header type [4 bits] = 0x1 [ 1 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			MAC = 0xB4ACDBCE [ 3031227342 ]
    			Sequence Number = 0x03 [ 3 ]
    			NAS message = 0x0741010BF600F110800101C234567805F070C0401100290208D03127238080211001000010810600000000830600000000000D00000300000A000005000010005200F11000015C0A003103E5E03E11035758A6200C601404EF65233B8878D2F28040080402600000021F00E0C16A01225E0160
    ←------------------------------------------------------------------------------------------------------------
    Attach Request:
    	Attach Request PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Attach Request
    			Security header type [4 bits] = 0x0 [ 0 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			Message Type [8 bits] = 0x41 - Attach Request [ 65 ]
    			NAS key set identifier
    				Type of security context flag [1 bit] = 0x0 [ 0 ]
    				key sequence indicator [3 bits] = 0x0 [ 0 ]
    			EPS attach type
    				Spare Bits [1 bit] = 0x0 [ 0 ]
    				Value [3 bits] = 0x1 [ 1 ]
    			EPS Mobile Identity
    				IE Length [8 bits] = 0xB [ 11 ]
    				constant / IMSI Identity Digit 1 [4 bits] = 0xF [ 15 ]
    				Odd / Even Indicator [1 bit] = 0x0 [ 0 ]
    				EPS Type of Identity [3 bits] = 0x6 - GUTI [ 6 ]
    				Mobile Country Code 1st and 2nd  Digits = 0x00 [ 0 ]
    				Mobile Network Code 3rd Digit = 0xF [ 15 ]
    				Mobile Country Code 3rd Digit = 0x1 [ 1 ]
    				Mobile Network Code 1st and 2nd  Digits = 0x10 [ 16 ]
    				MME group Id = 0x8001 [ 32769 ]
    				MME code = 0x01 [ 1 ]
    				M-TMSI = 0xC2345678 [ 3258209912 ]
    			UE network capability
    				IE Length [8 bits] = 0x5 [ 5 ]
    				eea0_128 [1 bit] = 0x1 [ 1 ]
    				eea1_128 [1 bit] = 0x1 [ 1 ]
    				eea2_128 [1 bit] = 0x1 [ 1 ]
    				eea3 [1 bit] = 0x1 [ 1 ]
    				eea4 [1 bit] = 0x0 [ 0 ]
    				eea5 [1 bit] = 0x0 [ 0 ]
    				eea6 [1 bit] = 0x0 [ 0 ]
    				eea7 [1 bit] = 0x0 [ 0 ]
    				eia0 [1 bit] = 0x0 [ 0 ]
    				eia1_128 [1 bit] = 0x1 [ 1 ]
    				eia2_128 [1 bit] = 0x1 [ 1 ]
    				eia3 [1 bit] = 0x1 [ 1 ]
    				eia4 [1 bit] = 0x0 [ 0 ]
    				eia5 [1 bit] = 0x0 [ 0 ]
    				eia6 [1 bit] = 0x0 [ 0 ]
    				eia7 [1 bit] = 0x0 [ 0 ]
    				uea0_7 [8 bits] = 0xC0 [ 192 ]
    				Ucs2 Treatment [1 bit] = 0x0 - The ME Has a Preference for the Default Alphabet Over UCS2 [ 0 ]
    				uia1_7 [7 bits] = 0x40 [ 64 ]
    				spare Bits_1 [2 bits] = 0x0 [ 0 ]
    				h245_ash [1 bit] = 0x0 [ 0 ]
    				acc_csfb [1 bit] = 0x1 [ 1 ]
    				lpp [1 bit] = 0x0 [ 0 ]
    				lcs [1 bit] = 0x0 [ 0 ]
    				xsr_vcc [1 bit] = 0x0 [ 0 ]
    				nf [1 bit] = 0x1 [ 1 ]
    			ESM message container
    				IE Length [16 bits] = 0x29 [ 41 ]
    				ESM message container contents = 0x0208D03127238080211001000010810600000000830600000000000D00000300000A00000500001000
    			Last visited registered TAI
    				IE Identifier [8 bits] = 0x52 [ 82 ]
    				Mobile Country Code 1st and 2nd  Digits = 0x00 [ 0 ]
    				Mobile Network Code 3rd Digit = 0xF [ 15 ]
    				Mobile Country Code 3rd Digit = 0x1 [ 1 ]
    				Mobile Network Code 1st and 2nd  Digits = 0x10 [ 16 ]
    				Tracking area code = 0x0001 [ 1 ]
    			DRX Parameter
    				IE Identifier [8 bits] = 0x5C [ 92 ]
    				split_code = 0x0A [ 10 ]
    				DRX cycle lengtn coeff and value for S1 mode [4 bits] = 0x0 [ 0 ]
    				Split on CCCH [1 bit] = 0x0 - Split PG Cycle on CCCH is Not Supported by the Mobile Station [ 0 ]
    				non-DRX timer [3 bits] = 0x0 [ 0 ]
    			MS Network Capability
    				IE Identifier [8 bits] = 0x31 [ 49 ]
    				IE Length [8 bits] = 0x3 [ 3 ]
    				Value
    					Gea1Bits
    						Gea1 [1 bit] = 0x1 [ 1 ]
    					SmCapabilitiesViaDedicatedChannels [1 bit] = 0x1 [ 1 ]
    					SmCapabilitiesViaGprsChannels [1 bit] = 0x1 [ 1 ]
    					Ucs2Support [1 bit] = 0x0 [ 0 ]
    					SsScreeningIndicator [2 bits] = 0x1 [ 1 ]
    					SolsaCapability [1 bit] = 0x0 [ 0 ]
    					Revision Level Indicator [1 bit] = 0x1 - The ME is Release '98 Onwards [ 1 ]
    					BSS Packet Flow Support [1 bit] = 0x1 - Mobile Station Does Support BSS Packet Flow Procedures [ 1 ]
    					ExtendedGeaBits
    						Gea2 [1 bit] = 0x1 [ 1 ]
    						Gea3 [1 bit] = 0x1 [ 1 ]
    						Gea4 [1 bit] = 0x0 [ 0 ]
    						Gea5 [1 bit] = 0x0 [ 0 ]
    						Gea6 [1 bit] = 0x0 [ 0 ]
    						Gea7 [1 bit] = 0x0 [ 0 ]
    					LcsVaCapability [1 bit] = 0x0 [ 0 ]
    					PsInterRatHoFromGeranToUtranIuModeCapability [1 bit] = 0x0 [ 0 ]
    					PsInterRatHoFromGeranToEUtranS1ModeCapability [1 bit] = 0x0 [ 0 ]
    					EmmCombinedProceduresCapability [1 bit] = 0x1 [ 1 ]
    					IsrSupport [1 bit] = 0x1 [ 1 ]
    					SrvccToGeranOrUtranCapability [1 bit] = 0x1 [ 1 ]
    					EpcCapability [1 bit] = 0x1 [ 1 ]
    					NfCapability [1 bit] = 0x1 [ 1 ]
    					GeranNetworkSharingCapability [1 bit] = 0x0 [ 0 ]
    					{ Spare Padding1 =
    					}
    			MS classmark 2
    				IE Identifier [8 bits] = 0x11 [ 17 ]
    				IE Length [8 bits] = 0x3 [ 3 ]
    				Spare Bits [1 bit] = 0x0 [ 0 ]
    				rev_level [2 bits] = 0x2 [ 2 ]
    				es_ind [1 bit] = 0x1 [ 1 ]
    				A5/1 Algorithm Supported [1 bit] = 0x0 - Encryption Algorithm A5/1 Available [ 0 ]
    				rf_pwr_capability [3 bits] = 0x7 [ 7 ]
    				spare2 [1 bit] = 0x0 [ 0 ]
    				ps_capability [1 bit] = 0x1 [ 1 ]
    				ss_ind [2 bits] = 0x1 [ 1 ]
    				sm_capability [1 bit] = 0x1 [ 1 ]
    				VBS Notification Reception [1 bit] = 0x0 - No VBS Capability or No Notifications Wanted [ 0 ]
    				Voice Group Call Service [1 bit] = 0x0 - No VGCS capability or no notifications wanted [ 0 ]
    				Frequency Capability  [1 bit] = 0x0 - The MS does Not Support the E-GSM or R-GSM  Band [ 0 ]
    				Classmark 3 Indicator [1 bit] = 0x1 - The MS Supports Options that are Indicated in Classmark 3 IE [ 1 ]
    				spare3 [1 bit] = 0x0 [ 0 ]
    				LCS Value Added Capability [1 bit] = 0x1 - Location Request Notification via CS domain Supported [ 1 ]
    				vcs_2 [1 bit] = 0x0 [ 0 ]
    				so_lsa [1 bit] = 0x0 [ 0 ]
    				CM Service Prompt [1 bit] = 0x1 - Network Initiated MO CM Connection Request Supported for Atleast One CM Protocol [ 1 ]
    				A5/3 Algorithm Supported [1 bit] = 0x1 - Encryption Algorithm A5/3 Available [ 1 ]
    				A5/2 Algorithm Supported [1 bit] = 0x0 - Encryption Algorithm A5/2 Not Available [ 0 ]
    			MS classmark 3
    				IE Identifier [8 bits] = 0x20 [ 32 ]
    				IE Length [8 bits] = 0xC [ 12 ]
    				SpareBit [1 bit] = 0x0 [ 0 ]
    				{ 110
    					A5Bits6
    						A57 [1 bit] = 0x0 - Encryption Algorithm A5/7 not Available [ 0 ]
    						A56 [1 bit] = 0x0 - Encryption Algorithm A5/6 not Available [ 0 ]
    						A55 [1 bit] = 0x0 - Encryption algorithm A5/5 not available [ 0 ]
    						A54 [1 bit] = 0x0 [ 0 ]
    					Associated Radio Capability26 [4 bits] = 0x1 [ 1 ]
    					Associated Radio Capability16 [4 bits] = 0x4 [ 4 ]
    				}
    				{ 0
    				}
    				{ 0
    				}
    				{ UCS2 Treatment [1 bit] = 0x0 - The ME has a Preference for the Default Alphabet Over UCS2 [ 0 ]
    				}
    				{ Extended Measurement Capability [1 bit] = 0x0 - The MS Does Not Support Extended Measurements [ 0 ]
    				}
    				{ 0
    				}
    				{ 1
    					MS Positioning Method Capability
    						MS Positioning Method [5 bits] = 0x7 [ 7 ]
    				}
    				{ 0
    				}
    				{ 1
    					EcsdStruct
    						Modulation Capability [1 bit] = 0x1 - 8-PSK Supported for Uplink Transmission and Downlink Reception [ 1 ]
    						{ 1
    							EcsdRfPowerCapability1 [2 bits] = 0x2 [ 2 ]
    						}
    						{ 1
    							EcsdRfPowerCapability2 [2 bits] = 0x2 [ 2 ]
    						}
    				}
    				{ 0
    				}
    				{ 1
    					GSM 850 Associated Radio Capability [4 bits] = 0x4 [ 4 ]
    				}
    				{ 1
    					PCS 1900 Associated Radio Capability [4 bits] = 0x1 [ 1 ]
    				}
    				{ UMTS FDD Access Technology Capability [1 bit] = 0x1 - Supported [ 1 ]
    				}
    				{ UMTS TDD Access Technology Capability [1 bit] = 0x0 - UMTS 3.84 Mcps TDD Not Supported [ 0 ]
    				}
    				{ CDMA 2000 Radio Access Technology Capability [1 bit] = 0x0 - Not Supported [ 0 ]
    				}
    				{ 1
    					DTM GPRS Multi Slot Subclass [2 bits] = 0x3 - Multislot Class 11 Supported [ 3 ]
    					Single Slot DTM [1 bit] = 0x0 [ 0 ]
    					{ 1
    						DtmEgprsMultiSlotSubClass [2 bits] = 0x3 [ 3 ]
    					}
    				}
    				{ 0
    				}
    				{ 0
    				}
    				{ Umts128McpsTddRadioAccessTechnologyCapability [1 bit] = 0x0 [ 0 ]
    				}
    				{ GERAN Feature Package 1 [1 bit] = 0x1 - Supported [ 1 ]
    				}
    				{ 0
    				}
    				{ 0
    				}
    				{ GERAN Feature Package 2 [1 bit] = 0x0 - Not supported [ 0 ]
    				}
    				{ GMSK Multislot Power Profile [2 bits] = 0x3 - GMSK_MULTISLOT_POWER_PROFILE 3 [ 3 ]
    				}
    				{ 8-PSK Multislot Power Profile [2 bits] = 0x3 - 8-PSK_MULTISLOT_POWER_PROFILE 3 [ 3 ]
    				}
    				{ 0
    				}
    				{ Downlink Advanced Receiver Performance [2 bits] = 0x1 - Downlink Advanced Receiver Performance - phase I supported [ 1 ]
    				}
    				{ DTM Enhancements Capability [1 bit] = 0x1 - The mobile station supports enhanced DTM CS establishment and enhanced DTM CS release procedures [ 1 ]
    				}
    				{ 0
    				}
    				{ RepeatedAcchCapability [1 bit] = 0x1 [ 1 ]
    				}
    				{ 0
    				}
    				{ 0
    				}
    				{ CipheringModeSettingCapability [1 bit] = 0x1 [ 1 ]
    				}
    				{ AdditionalPositioningCapabilities [1 bit] = 0x0 [ 0 ]
    				}
    				{ EUtraFddSupport [1 bit] = 0x1 [ 1 ]
    				}
    				{ EUtraTddSupport [1 bit] = 0x1 [ 1 ]
    				}
    				{ EUtraMeasurementAndReportingSupport [1 bit] = 0x1 [ 1 ]
    				}
    				{ PriorityBasedReselectionSupport [1 bit] = 0x1 [ 1 ]
    				}
    				{ UtraCsgCellsReporting [1 bit] = 0x0 [ 0 ]
    				}
    				{ Vamos Level [2 bits] = 0x1 - VAMOS I supported [ 1 ]
    				}
    				{ Tighter Capability [2 bits] = 0x1 - TIGHTER supported for speech and signalling channels only [ 1 ]
    				}
    				{ Selective Ciphering Of Downlink SACCH [1 bit] = 0x0 - Selective Ciphering of Downlink SACCH not supported [ 0 ]
    				}
    				{ CsToPsSrvccFromGeranToUtra [2 bits] = 0x0 [ 0 ]
    				}
    				{ CsToPsSrvccFromGeranToEUtra [2 bits] = 0x0 [ 0 ]
    				}
    				{ GeranNetworkSharingSupport [1 bit] = 0x0 [ 0 ]
    				}
    				{ EUtraWidebandRsrqMeasurementsSupport [1 bit] = 0x0 [ 0 ]
    				}
    				N Spare Bits1 =
    			Supported codecs
    				IE Identifier [8 bits] = 0x40 [ 64 ]
    				IE Length [8 bits] = 0x8 [ 8 ]
    				system identification 1 = 0x04 [ 4 ]
    				Length Of Bitmap for SysID 1 = 0x02 [ 2 ]
    				codec bitmap sysID 1_b1_b8 = 0x60 [ 96 ]
    				codec bitmap sysID1_b9_b16 = 0x00 [ 0 ]
    				system identification 2 = 0x00 [ 0 ]
    				Length Of Bitmap for SysID 2 = 0x02 [ 2 ]
    				codec bitmap sysID2_b1_b8 = 0x1F [ 31 ]
    				codec bitmap sysID2_b9_b16 = 0x00 [ 0 ]
    			old_guti_type
    				IE Identifier [4 bits] = 0xE [ 14 ]
    				Spare Bits [3 bits] = 0x0 [ 0 ]
    				GUTI_type [1 bit] = 0x0 [ 0 ]
    			ms_nfs
    				IE Identifier [4 bits] = 0xC [ 12 ]
    				Spare Bits [3 bits] = 0x0 [ 0 ]
    				ext_prio_timer [1 bit] = 0x1 [ 1 ]
    			t3324_value
    				IE Identifier [8 bits] = 0x6A [ 106 ]
    				IE Length [8 bits] = 0x1 [ 1 ]
    				Timer Value Unit [3 bits] = 0x1 - Value is Incremented in Multiples of 1 Minute  [ 1 ]
    				Value [5 bits] = 0x2 [ 2 ]
    			t3412_ext_val
    				IE Identifier [8 bits] = 0x5E [ 94 ]
    				IE Length [8 bits] = 0x1 [ 1 ]
    				Timer Value Unit [3 bits] = 0x3 - value is incremented in multiples of 2 seconds [ 3 ]
    				Value [5 bits] = 0x0 [ 0 ]
    ←------------------------------------------------------------------------------------------------------------
    PDN Connectivity Request:
    	PDN Connectivity Request PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		PDN Connectivity Request
    			EPS bearer identity [4 bits] = 0x0 [ 0 ]
    			Protocol Discriminator [4 bits] = 0x2 - EPS Session Management Messages [ 2 ]
    			Procedure transaction identifier [8 bits] = 0x8 [ 8 ]
    			Message Type [8 bits] = 0xD0 - PDN Connectivity Request [ 208 ]
    			PDN type
    				Spare Bits [1 bit] = 0x0 [ 0 ]
    				Value [3 bits] = 0x3 [ 3 ]
    			Request type
    				Spare Bits [1 bit] = 0x0 [ 0 ]
    				Value [3 bits] = 0x1 [ 1 ]
    			Protocol Configuration Options
    				IE Identifier [8 bits] = 0x27 [ 39 ]
    				IE Length [8 bits] = 0x23 [ 35 ]
    				Extension Bit [1 bit] = 0x1 - Outgoing Calls Barred within CUG [ 1 ]
    				Spare Bits [4 bits] = 0x0 [ 0 ]
    				Configuration Protocol [3 bits] = 0x0 - PPP for Use with IP PDP Type [ 0 ]
    				Option1
    					Identifier = 0x8021 - Internet Protocol Control Protocol [ 32801 ]
    					Length [8 bits] = 0x10 [ 16 ]
    					value = 0x01000010810600000000830600000000
    				Option2
    					Identifier = 0x000D [ 13 ]
    					Length [8 bits] = 0x0 [ 0 ]
    				Option3
    					Identifier = 0x0003 - DNS Server Address Request [ 3 ]
    					Length [8 bits] = 0x0 [ 0 ]
    				Option4
    					Identifier = 0x000A [ 10 ]
    					Length [8 bits] = 0x0 [ 0 ]
    				Option5
    					Identifier = 0x0005 [ 5 ]
    					Length [8 bits] = 0x0 [ 0 ]
    				Option6
    					Identifier = 0x0010 [ 16 ]
    					Length [8 bits] = 0x0 [ 0 ]
    ←------------------------------------------------------------------------------------------------------------
    RRC_PDU_IND:
    ↑	Received on port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 924
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							rrcConnectionSetupComplete
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									c1
    										rrcConnectionSetupComplete_r8
    											selectedPLMN_Identity = 1
    											registeredMME
    												plmn_Identity = Omit
    												mmegi = 1000000000000001'B
    												mmec = 00000001'B
    											dedicatedInfoNAS = '17B4ACDBCE030741010BF600F110800101C234567805F070C0401100290208D03127238080211001000010810600000000830600000000000D00000300000A000005000010005200F11000015C0A003103E5E03E11035758A6200C601404EF65233B8878D2F28040080402600000021F00E0C16A01225E0160'O
    											nonCriticalExtension
    												lateNonCriticalExtension = Omit
    												nonCriticalExtension
    													gummei_Type_r10 = native (0)
    													rlf_InfoAvailable_r10 = Omit
    													logMeasAvailable_r10 = Omit
    													rn_SubframeConfigReq_r10 = Omit
    													nonCriticalExtension = Omit

    SRB_COMMON_IND:
    ↑	Inter-component message: SRB -> EUTRA_PTC:SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 924
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Dcch
    						message_
    							c1
    								rrcConnectionSetupComplete
    									rrc_TransactionIdentifier = 0
    									criticalExtensions
    										c1
    											rrcConnectionSetupComplete_r8
    												selectedPLMN_Identity = 1
    												registeredMME
    													plmn_Identity = Omit
    													mmegi = 1000000000000001'B
    													mmec = 00000001'B
    												dedicatedInfoNAS = '17B4ACDBCE030741010BF600F110800101C234567805F070C0401100290208D03127238080211001000010810600000000830600000000000D00000300000A000005000010005200F11000015C0A003103E5E03E11035758A6200C601404EF65233B8878D2F28040080402600000021F00E0C16A01225E0160'O
    												nonCriticalExtension
    													lateNonCriticalExtension = Omit
    													nonCriticalExtension
    														gummei_Type_r10 = native (0)
    														rlf_InfoAvailable_r10 = Omit
    														logMeasAvailable_r10 = Omit
    														rn_SubframeConfigReq_r10 = Omit
    														nonCriticalExtension = Omit
    				Nas
    					NasIndication
    						SecurityProtection
    							Status = 0001'B
    							NasCount = '00000003'O
    						Pdu
    							Msg
    								aTTACH_REQUEST
    									securityHeaderType = 0000'B
    									protocolDiscriminator = 0111'B
    									messageType = 01000001'B
    									nasKeySetId
    										iei = Omit
    										tsc = 0'B
    										nasKeySetId = 000'B
    									epsAttachType
    										spare = 0'B
    										typeValue = 001'B
    									epsMobileIdentity
    										iei = Omit
    										iel = '0B'O
    										idDigit1 = 1111'B
    										oddEvenInd = 0'B
    										typeOfId = 110'B
    										otherDigits = '00F110800101C2345678'O
    									ueNetworkCapability
    										iei = Omit
    										iel = '05'O
    										eeaCap = 'F0'O
    										eiaCap = '70'O
    										ueaCap = 'C0'O
    										uiaCap = '40'O
    										srvcc_LPP_ProSeCap = '11'O
    										cIoT_proSeCap = Omit
    										spare = Omit
    									esmMessage
    										iei = Omit
    										iel = '0029'O
    										esmPdu = '0208D03127238080211001000010810600000000830600000000000D00000300000A00000500001000'O
    									oldPtmsiSignature = Omit
    									additionalGuti = Omit
    									lastVisitedRegisteredTai
    										iei = '52'O
    										plmnId = '00F110'O
    										tac = '0001'O
    									drxParameter
    										iei = '5C'O
    										splitPGcycleCode = 00001010'B
    										cnDRXcoef = 0000'B
    										splitOnCCCH = 0'B
    										nonDRXtimer = 000'B
    									msNetworkCapability
    										iei = '31'O
    										iel = '03'O
    										gea1 = 1'B
    										smCapDedicated = 1'B
    										smCapGPRS = 1'B
    										ucs2 = 0'B
    										ssScreeningIndicator = 01'B
    										soLSACap = 0'B
    										revLevelIndicator = 1'B
    										pfcFeatureMode = 1'B
    										gea2 = 1'B
    										gea3 = 1'B
    										gea4 = 0'B
    										gea5 = 0'B
    										gea6 = 0'B
    										gea7 = 0'B
    										lcsVACap = 0'B
    										psHOtoUTRAN_IuModeCap = 0'B
    										psHOtoEUTRAN_S1ModeCap = 0'B
    										emmCombinedCap = 1'B
    										isrSupport = 1'B
    										srvccToGERAN_UTRANCap = 1'B
    										epcCap = 1'B
    										nfCap = 1'B
    										gERANNtwkShareCap = 0'B
    										userPlaneIntegrityProtSupport = Omit
    										gia4 = Omit
    										gia5 = Omit
    										gia6 = Omit
    										gia7 = Omit
    										spareBits = Omit
    									oldLai = Omit
    									tmsiStatus = Omit
    									msClassmark2
    										iei = '11'O
    										iel = '03'O
    										spare1_1 = 0'B
    										revLvl = 10'B
    										eSIND = 1'B
    										a5_1 = 0'B
    										rFPwrCap = 111'B
    										spare1_2 = 0'B
    										pSCap = 1'B
    										sSSI = 01'B
    										sMCap = 1'B
    										vBS = 0'B
    										vGCS = 0'B
    										fC = 0'B
    										cM3 = 1'B
    										spare1_3 = 0'B
    										lCSVA = 1'B
    										uCS2 = 0'B
    										soLSA = 0'B
    										cMSP = 1'B
    										a5_3 = 1'B
    										a5_2 = 0'B
    									msClassmark3
    										iei = '20'O
    										iel = '0C'O
    										spareBit = 0'B
    										multibandSupported = 110'B
    										a5_7 = 0'B
    										a5_6 = 0'B
    										a5_5 = 0'B
    										a5_4 = 0'B
    										associatedRadioCapabilty2 = 0001'B
    										spareBits1 = Omit
    										associatedRadioCapabilty1 = 0100'B
    										maskBit1 = 0'B
    										rGSM_RadioCapability = Omit
    										maskBit2 = 0'B
    										multiSlotClass = Omit
    										uCS2Treatment = 0'B
    										extMeasurementCapability = 0'B
    										maskBit3 = 0'B
    										msMeasurementCapability = Omit
    										maskBit4 = 1'B
    										msPositioningMethod = 00111'B
    										maskBit5 = 0'B
    										eDGE_MultiSlot = Omit
    										maskBit6 = 1'B
    										psk8_Struct
    											modulationCapability = 1'B
    											pwrMask1 = 1'B
    											eDGE_RF_PowerCapability1 = 10'B
    											pwrMask2 = 1'B
    											eDGE_RF_PowerCapability2 = 10'B
    										maskBit7 = 0'B
    										gSM400BandsSupported = Omit
    										gSM400AssociatedRadioCapability = Omit
    										maskBit8 = 1'B
    										gSM850AssociatedRadiioCapability = 0100'B
    										maskBit9 = 1'B
    										pCS1900AssociatedRadiioCapability = 0001'B
    										uMTS_FDD_RAT_Capability = 1'B
    										uMTS384TDD_RAT_Capability = 0'B
    										cDMA2000_RAT_Capability = 0'B
    										maskBit10 = 1'B
    										dTM_GPRS_MultiSlotSubclass = 11'B
    										singleSlotDTM = 0'B
    										maskBit11 = 1'B
    										dTM_EGPRS_MultiSlorSubclass = 11'B
    										maskBit12 = 0'B
    										singleBandSupport = Omit
    										maskBit13 = 0'B
    										gSM700AssociatedRadioCapability = Omit
    										uMTS128TDD_RAT_Capability = 0'B
    										gERANFeatPack1 = 1'B
    										mask14 = 0'B
    										extDTM_GPRS_MultiSlotSubclass = Omit
    										etxDTM_EGPRS_MultiSlotSubclass = Omit
    										mask15 = 0'B
    										highMultislotCap = Omit
    										spare2 = 0'B
    										gERANFeatPack2 = 0'B
    										gMSKMultislotPowerProfile = 11'B
    										pSKMultislotPowerProfile = 11'B
    										mask17 = 0'B
    										tGSM400BandsSupported = Omit
    										tGSM400AssocRadioCap = Omit
    										spare = 0'B
    										dlAdvancedRxPerf = 01'B
    										dTMEhancCap = 1'B
    										mask19 = 0'B
    										dTMGPRSHighMultislotClass = Omit
    										offsetReq = Omit
    										mask20 = Omit
    										dTMEGPRSHighMultislotClass = Omit
    										rptdACCHCap = 1'B
    										mask21 = 0'B
    										gsm710AssocRadioCap = Omit
    										mask22 = 0'B
    										tgsm810AssocRadioCap = Omit
    										cipheringModeSettingCap = 1'B
    										addPositionCap = 0'B
    										eutraFDDSupport = 1'B
    										eutraTDDSupport = 1'B
    										eutraMeasAndReporting = 1'B
    										priorityBasedReselection = 1'B
    										utraCSGCellsReporting = 0'B
    										vamosLevel = 01'B
    										tighterCap = 01'B
    										selectCipheringDLSACCH = 0'B
    										csPS_SRVCC_G2U = Omit
    										csPS_SRVCC_G2E = Omit
    										geranNwkSharing = Omit
    										eutraWidebandRSRQMeas = Omit
    										erBandSupport = Omit
    										utraMultipleFreqBandInd = Omit
    										eutraMultipleFreqBandInd = Omit
    										xtdTSCSetCap = Omit
    										xtdEARFCNValueRange = Omit
    										spareBits2 = 000000'B
    									supportedCodecList
    										iei = '40'O
    										iel = '08'O
    										codec
    											Codec
    												sysId = '04'O
    												len = '02'O
    												bitMap1to8 = 01100000'B
    												bitMap9to16 = 00000000'B
    											Codec
    												sysId = '00'O
    												len = '02'O
    												bitMap1to8 = 00011111'B
    												bitMap9to16 = 00000000'B
    									addUpdateType = Omit
    									voiceDomainPref = Omit
    									deviceProperties = Omit
    									oldGUTI_Type
    										iei = 'E'H
    										spare = 000'B
    										gutiType = 0'B
    									msNetworkFeatureSupport
    										iei = 'C'H
    										spare = 000'B
    										extdPeriodicTimers = 1'B
    									tmsiBasedNRIContainer = Omit
    									t3324Value
    										iei = '6A'O
    										iel = '01'O
    										unit = 001'B
    										gprsTimerValue = 00010'B
    									t3412ExtdValue
    										iei = '5E'O
    										iel = '01'O
    										unit = 011'B
    										gprsTimerValue = 00000'B
    									extendedDRXParams = Omit
    							PiggybackedPduList
    								NAS_UL_Pdu_Type
    									Msg
    										pDN_CONNECTIVITY_REQUEST
    											epsBearerId = '0'H
    											protocolDiscriminator = 0010'B
    											procedureTransactionIdentifier = '08'O
    											messageType = 11010000'B
    											pdnType
    												spare = 0'B
    												typeValue = 011'B
    											requestType
    												spare = 0'B
    												typeValue = 001'B
    											esmInfoTransferFlag = Omit
    											accessPointName = Omit
    											protocolConfigurationOptions
    												iei = '27'O
    												iel = '23'O
    												ext = 1'B
    												spare = 0000'B
    												configProtocol = 000'B
    												pco
    													ProtocolContainer
    														protocolID = '8021'O
    														protocolLength = '10'O
    														content = '01000010810600000000830600000000'O
    													ProtocolContainer
    														protocolID = '000D'O
    														protocolLength = '00'O
    														content = Omit
    													ProtocolContainer
    														protocolID = '0003'O
    														protocolLength = '00'O
    														content = Omit
    													ProtocolContainer
    														protocolID = '000A'O
    														protocolLength = '00'O
    														content = Omit
    													ProtocolContainer
    														protocolID = '0005'O
    														protocolLength = '00'O
    														content = Omit
    													ProtocolContainer
    														protocolID = '0010'O
    														protocolLength = '00'O
    														content = Omit
    											deviceProperties = Omit
    											nbifomContainer = Omit
    											headerCompressionConfig = Omit
    											extdProtocolConfigurationOptions = Omit
    									PiggybackedPduList = Omit

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = True
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				Cell
    					AddOrReconfigure
    						Basic = Omit
    						Active
    							C_RNTI = Omit
    							PhysicalLayerConfigUL = Omit
    							RachProcedureConfig = Omit
    							CcchDcchDtchConfig
    								MeasGapCtrl = Omit
    								DL = Omit
    								UL
    									DciInfo = Omit
    									Hopping
    										Deactivated = True
    									PUCCH_Synch
    										Auto
    											TimingAdvance = 31
    											TA_Period = 600
    											TA_Repetition
    												Continuous = True
    									UL_GrantConfig = Omit
    								DrxCtrl = Omit
    								TtiBundling = Omit
    								CifPresence = Omit
    							ServingCellConfig = Omit
    							SciSchedulingConfig = Omit
    							EIMTA_Config = Omit
    							CE_Mode = Omit

    SYSTEM_CTRL_CNF:
    ↑	Received on port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_CNF
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				Result
    					Success = True
    			Confirm
    				Cell = True

    Verdict Intermediate Pass:
    	Intermediate verdict: (PASS)
    	TTCN-3 message: Step 4
    		Source = \Test Control\TTCN3
    		IntermediateVerdict = (Pass)
    		summary = Intermediate verdict: (PASS)
    		TTCN-3 message: Step 4

    TTCN Test Step:
    	Steps 5 - 13Eb1
    		Source = \Test Control\TTCN3
    		recordType = 24
    		summary = Steps 5 - 13Eb1

    SRB_COMMON_REQ:
    ↓	Inter-component message: TC_SRB -> NASEMU_LTE_PTC:TC_SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Signalling
    				Rrc = Omit
    				Nas
    					NAS_MSG_Request_Type
    						SecurityProtection
    							Status = 0000'B
    							ForceMacError = False
    						Pdu
    							Msg
    								aUTHENTICATION_REQUEST
    									securityHeaderType = 0000'B
    									protocolDiscriminator = 0111'B
    									messageType = 01010010'B
    									spareHalfOctet = '0'H
    									asmeNasKeySetId
    										iei = Omit
    										tsc = 0'B
    										nasKeySetId = 001'B
    									rand
    										iei = Omit
    										randValue = 10100011110111100000110001101101001101100011111000110000110000110110010010100100000001111000111100011011111110001101010101110111'B
    									autn
    										iei = Omit
    										iel = '10'O
    										aUTN = 01101110001100100011101100110110110001000110110010000000000000001010001111011111000011100110111000110010001110111011011011000100'B
    							PiggybackedPduList = Omit

    DL-DCCH-Message:
    	dlInformationTransfer
    		Source = \Protocol\3GPP\LTE\RRC\
    		DL-DCCH-Message
    			message = c1 = dlInformationTransfer =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = c1 = dlInformationTransfer-r8 =
    					dedicatedInfoType = dedicatedInfoNAS = 075201A3DE0C6D363E30C364A4078F1BF8D577106E323B36C46C8000A3DF0E6E323BB6C4
    ------------------------------------------------------------------------------------------------------------→
    Authentication Request:
    	Authentication Request PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Authentication Request
    			Security header type [4 bits] = 0x0 [ 0 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			Message Type [8 bits] = 0x52 - Authentication Request [ 82 ]
    			Spare Half Octet [4 bits] = 0x0 [ 0 ]
    			NAS key set identifierASME
    				Type of security context flag [1 bit] = 0x0 [ 0 ]
    				key sequence indicator [3 bits] = 0x1 [ 1 ]
    				Authentication parameter random = 0xA3DE0C6D363E30C364A4078F1BF8D577
    			Authentication Parameter AUTN
    				IE Length [8 bits] = 0x10 [ 16 ]
    				value = 0x6E323B36C46C8000A3DF0E6E323BB6C4
    ------------------------------------------------------------------------------------------------------------→
    RRC_PDU_REQ:
    ↓	Sent from port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							dlInformationTransfer
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									c1
    										dlInformationTransfer_r8
    											dedicatedInfoType
    												dedicatedInfoNAS = '075201A3DE0C6D363E30C364A4078F1BF8D577106E323B36C46C8000A3DF0E6E323BB6C4'O
    											nonCriticalExtension = Omit

    UL-DCCH-Message:
    	ulInformationTransfer
    		Source = \Protocol\3GPP\LTE\RRC\
    		UL-DCCH-Message
    			message = c1 = ulInformationTransfer =
    				criticalExtensions = c1 = ulInformationTransfer-r8 =
    					dedicatedInfoType = dedicatedInfoNAS = 17D74F7D4104075308A3DF0E6E323B36C4
    ←------------------------------------------------------------------------------------------------------------
    Security Protected NAS Message UL:
    	Security Protected NAS Message UL PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Security Protected NAS Message
    			Security header type [4 bits] = 0x1 [ 1 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			MAC = 0x574F7D41 [ 1464827201 ]
    			Sequence Number = 0x04 [ 4 ]
    			NAS message = 0x075308235F0E6E323B3644
    ←------------------------------------------------------------------------------------------------------------
    Authentication Response:
    	Authentication Response PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Authentication Response
    			Security header type [4 bits] = 0x0 [ 0 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			Message Type [8 bits] = 0x53 - Authentication Response [ 83 ]
    			Authentication response parameter
    				IE Length [8 bits] = 0x8 [ 8 ]
    				Authentication response parameter information = 0x235F0E6E323B3644
    ←------------------------------------------------------------------------------------------------------------
    RRC_PDU_IND:
    ↑	Received on port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 938
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							ulInformationTransfer
    								criticalExtensions
    									c1
    										ulInformationTransfer_r8
    											dedicatedInfoType
    												dedicatedInfoNAS = '17D74F7D4104075308A3DF0E6E323B36C4'O
    											nonCriticalExtension = Omit

    SRB_COMMON_IND:
    ↑	Inter-component message: SRB -> EUTRA_PTC:SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 938
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			Signalling
    				Rrc = Omit
    				Nas
    					NasIndication
    						SecurityProtection
    							Status = 0001'B
    							NasCount = '00000004'O
    						Pdu
    							Msg
    								aUTHENTICATION_RESPONSE
    									securityHeaderType = 0000'B
    									protocolDiscriminator = 0111'B
    									messageType = 01010011'B
    									authenticationResponseParameter
    										iei = Omit
    										iel = '08'O
    										res = 1010001111011111000011100110111000110010001110110011011011000100'B
    							PiggybackedPduList = Omit

    NAS_CTRL_REQ:
    ↓	Inter-component message: CTRL -> NASEMU_LTE_PTC:CTRL
    		Source = \Test Control\TTCN3
    		NAS_CTRL_REQ
    			Common
    				ControlInfo
    					CnfFlag = True
    			Request
    				Security
    					StartRestart
    						Integrity
    							Algorithm = 001'B
    							K_NAS = 01101111111110011000110110100011010010100010110100011011110001100010101010100110110101001011101100011010011000101010011001100100'B
    						Ciphering
    							Algorithm = 001'B
    							K_NAS = 00110010100110111011010001000010000101000111011000010111000110011110011011000000000100000101011110100001010001000001111110100001'B
    						NasCountReset = True

    NAS_CTRL_CNF:
    ↑	Inter-component message: NASCTRL -> EUTRA_PTC:NASCTRL
    		Source = \Test Control\TTCN3
    		NAS_CTRL_CNF
    			Common
    			Confirm
    				Security = True

    SRB_COMMON_REQ:
    ↓	Inter-component message: TC_SRB -> NASEMU_LTE_PTC:TC_SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Signalling
    				Rrc = Omit
    				Nas
    					NAS_MSG_Request_Type
    						SecurityProtection
    							Status = 0011'B
    							ForceMacError = False
    						Pdu
    							Msg
    								sECURITY_MODE_COMMAND
    									securityHeaderType = 0000'B
    									protocolDiscriminator = 0111'B
    									messageType = 01011101'B
    									nasSecurityAlgorithms
    										iei = Omit
    										spare1 = 0'B
    										cipheringType = 001'B
    										spare2 = 0'B
    										integrityType = 001'B
    									spareHalfOctet = '0'H
    									asmeNasKeySetId
    										iei = Omit
    										tsc = 0'B
    										nasKeySetId = 001'B
    									replayedSecurityCapability
    										iel = '05'O
    										eeaCap = 'F0'O
    										eiaCap = '70'O
    										ueaCap = 'C0'O
    										uiaCap = '40'O
    										geaCap = '70'O
    									imeisvRequest = Omit
    									replayedNonceUe = Omit
    									nonceMme = Omit
    							PiggybackedPduList = Omit

    DL-DCCH-Message:
    	dlInformationTransfer
    		Source = \Protocol\3GPP\LTE\RRC\
    		DL-DCCH-Message
    			message = c1 = dlInformationTransfer =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = c1 = dlInformationTransfer-r8 =
    					dedicatedInfoType = dedicatedInfoNAS = 372CAD8DD600075D110105F070C04070
    ------------------------------------------------------------------------------------------------------------→
    Security Protected NAS Message DL:
    	Security Protected NAS Message DL PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Security Protected NAS Message
    			Security header type [4 bits] = 0x3 [ 3 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			MAC = 0x2CAD8DD6 [ 749571542 ]
    			Sequence Number = 0x00 [ 0 ]
    			NAS message = 0x075D110105F070C04070
    ------------------------------------------------------------------------------------------------------------→
    Security Mode Command:
    	Security Mode Command PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Security Mode Command
    			Security header type [4 bits] = 0x0 [ 0 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			Message Type [8 bits] = 0x5D - Security Mode Command [ 93 ]
    			Selected NAS security algorithms
    				Spare Bits [1 bit] = 0x0 [ 0 ]
    				Type of ciphering algorithm [3 bits] = 0x1 [ 1 ]
    				spare Bits_1 [1 bit] = 0x0 [ 0 ]
    				Type of integrity protection algorithm [3 bits] = 0x1 [ 1 ]
    			Spare Half Octet [4 bits] = 0x0 [ 0 ]
    			NAS key set identifierASME
    				Type of security context flag [1 bit] = 0x0 [ 0 ]
    				key sequence indicator [3 bits] = 0x1 [ 1 ]
    			Replayed UE security capabilities
    				IE Length [8 bits] = 0x5 [ 5 ]
    				eea0_128 [1 bit] = 0x1 [ 1 ]
    				eea1_128 [1 bit] = 0x1 [ 1 ]
    				eea2_128 [1 bit] = 0x1 [ 1 ]
    				eea3 [1 bit] = 0x1 [ 1 ]
    				eea4 [1 bit] = 0x0 [ 0 ]
    				eea5 [1 bit] = 0x0 [ 0 ]
    				eea6 [1 bit] = 0x0 [ 0 ]
    				eea7 [1 bit] = 0x0 [ 0 ]
    				Spare Bits [1 bit] = 0x0 [ 0 ]
    				eia1_128 [1 bit] = 0x1 [ 1 ]
    				eia2_128 [1 bit] = 0x1 [ 1 ]
    				eia3 [1 bit] = 0x1 [ 1 ]
    				eia4 [1 bit] = 0x0 [ 0 ]
    				eia5 [1 bit] = 0x0 [ 0 ]
    				eia6 [1 bit] = 0x0 [ 0 ]
    				eia7 [1 bit] = 0x0 [ 0 ]
    				uea0_7 [8 bits] = 0xC0 [ 192 ]
    				spare Bits_1 [1 bit] = 0x0 [ 0 ]
    				uia1_7 [7 bits] = 0x40 [ 64 ]
    				spare2 [1 bit] = 0x0 [ 0 ]
    				gea1_7 [7 bits] = 0x70 [ 112 ]
    ------------------------------------------------------------------------------------------------------------→
    RRC_PDU_REQ:
    ↓	Sent from port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							dlInformationTransfer
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									c1
    										dlInformationTransfer_r8
    											dedicatedInfoType
    												dedicatedInfoNAS = '372CAD8DD600075D110105F070C04070'O
    											nonCriticalExtension = Omit

    UL-DCCH-Message:
    	ulInformationTransfer
    		Source = \Protocol\3GPP\LTE\RRC\
    		UL-DCCH-Message
    			message = c1 = ulInformationTransfer =
    				criticalExtensions = c1 = ulInformationTransfer-r8 =
    					dedicatedInfoType = dedicatedInfoNAS = 4765DF4F7D000022
    ←------------------------------------------------------------------------------------------------------------
    Security Protected NAS Message UL:
    	Security Protected NAS Message UL PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Security Protected NAS Message
    			Security header type [4 bits] = 0x4 [ 4 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			MAC = 0x655F4F7D [ 1700745085 ]
    			Sequence Number = 0x00 [ 0 ]
    			NAS message = 0x0022 [ 34 ]
    ←------------------------------------------------------------------------------------------------------------
    Ciphered NAS Message UL:
    	Ciphered NAS Message UL PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Ciphered NAS Message =
    			0x0022
    ←------------------------------------------------------------------------------------------------------------
    RRC_PDU_IND:
    ↑	Received on port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 942
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							ulInformationTransfer
    								criticalExtensions
    									c1
    										ulInformationTransfer_r8
    											dedicatedInfoType
    												dedicatedInfoNAS = '4765DF4F7D000022'O
    											nonCriticalExtension = Omit

    Security Mode Complete:
    	Security Mode Complete PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Security Mode Complete
    			Security header type [4 bits] = 0x0 [ 0 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			Message Type [8 bits] = 0x5E - Security Mode Complete [ 94 ]
    ←------------------------------------------------------------------------------------------------------------
    SRB_COMMON_IND:
    ↑	Inter-component message: SRB -> EUTRA_PTC:SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 942
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			Signalling
    				Rrc = Omit
    				Nas
    					NasIndication
    						SecurityProtection
    							Status = 0100'B
    							NasCount = '00000000'O
    						Pdu
    							Msg
    								sECURITY_MODE_COMPLETE
    									securityHeaderType = 0000'B
    									protocolDiscriminator = 0111'B
    									messageType = 01011110'B
    									imeisv = Omit
    							PiggybackedPduList = Omit

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = True
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				RadioBearerList
    					RadioBearer_Type
    						Id
    							Drb = 1
    						Config
    							AddOrReconfigure
    								Pdcp
    									Config
    										Rb
    											Drb
    												R8
    													discardTimer = infinity_ (7)
    													rlc_AM
    														statusReportRequired = True
    													rlc_UM = Omit
    													headerCompression
    														notUsed = Null
    													rn_IntegrityProtection_r10 = Omit
    													pdcp_SN_Size_v1130 = Omit
    													ul_DataSplitDRB_ViaSCG_r12 = Omit
    													t_Reordering_r12 = Omit
    													ul_DataSplitThreshold_r13 = Omit
    													pdcp_SN_Size_v1310 = Omit
    													statusFeedback_r13 = Omit
    										TestMode
    											None = True
    								Rlc
    									Rb
    										AM
    											Tx
    												R8
    													t_PollRetransmit = ms80 (15)
    													pollPDU = p128 (5)
    													pollByte = kB125 (4)
    													maxRetxThreshold = t4 (3)
    											Rx
    												R8
    													t_Reordering = ms80 (16)
    													t_StatusProhibit = ms60 (12)
    											ExtendedLI = Omit
    									TestMode
    										None = True
    								LogicalChannelId = 3
    								Mac
    									LogicalChannel
    										Priority = 13
    										PrioritizedBitRate = kBps0 (0)
    									TestMode
    										None = True
    								DiscardULData = Omit

    SYSTEM_CTRL_CNF:
    ↑	Received on port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_CNF
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				Result
    					Success = True
    			Confirm
    				RadioBearerList = True

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = True
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				PdcpCount
    					Get
    						AllRBs = True

    SYSTEM_CTRL_CNF:
    ↑	Received on port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_CNF
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				Result
    					Success = True
    			Confirm
    				PdcpCount
    					Get
    						PdcpCountInfo_Type
    							RadioBearerId
    								Srb = 1
    							UL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000011'B
    							DL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000010'B
    						PdcpCountInfo_Type
    							RadioBearerId
    								Srb = 2
    							UL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000000'B
    							DL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000000'B
    						PdcpCountInfo_Type
    							RadioBearerId
    								Drb = 1
    							UL
    								Format = PdcpCount_DrbShortSQN (2)
    								Value = 00000000000000000000000000000000'B
    							DL
    								Format = PdcpCount_DrbShortSQN (2)
    								Value = 00000000000000000000000000000000'B

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = True
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				AS_Security
    					StartRestart
    						Integrity
    							Algorithm = eia1 (1)
    							KRRCint = 10001100011101101101010000010100100110110001001111000110110100001011000111101111101101010100111100101100100100110000111000100100'B
    							ActTimeList = Omit
    						Ciphering
    							Algorithm = eea1 (1)
    							KRRCenc = 10011101101111111000111001000000000111100110010111101011111110001100011010011101010111000111111100011000110000001111111110111001'B
    							KUPenc = 01010000000101011110110101010000010000100010010010001011001001000011010001111100011001000111000100100010000100010011011111100000'B
    							ActTimeList
    								SecurityActTime_Type
    									RadioBearerId
    										Srb = 1
    									UL
    										SQN
    											Format = PdcpCount_Srb (0)
    											Value = 4
    									DL
    										SQN
    											Format = PdcpCount_Srb (0)
    											Value = 3
    								SecurityActTime_Type
    									RadioBearerId
    										Srb = 2
    									UL
    										SQN
    											Format = PdcpCount_Srb (0)
    											Value = 0
    									DL
    										SQN
    											Format = PdcpCount_Srb (0)
    											Value = 0
    								SecurityActTime_Type
    									RadioBearerId
    										Drb = 1
    									UL
    										SQN
    											Format = PdcpCount_DrbShortSQN (2)
    											Value = 0
    									DL
    										SQN
    											Format = PdcpCount_DrbShortSQN (2)
    											Value = 0

    SYSTEM_CTRL_CNF:
    ↑	Received on port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_CNF
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				Result
    					Success = True
    			Confirm
    				AS_Security = True

    SRB_COMMON_REQ:
    ↓	Inter-component message: TC_SRB -> NASEMU_LTE_PTC:TC_SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Dcch
    						message_
    							c1
    								securityModeCommand
    									rrc_TransactionIdentifier = 0
    									criticalExtensions
    										c1
    											securityModeCommand_r8
    												securityConfigSMC
    													securityAlgorithmConfig
    														cipheringAlgorithm = eea1 (1)
    														integrityProtAlgorithm = eia1 (1)
    												nonCriticalExtension = Omit
    				Nas = Omit

    DL-DCCH-Message:
    	securityModeCommand
    		Source = \Protocol\3GPP\LTE\RRC\
    		DL-DCCH-Message
    			message = c1 = securityModeCommand =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = c1 = securityModeCommand-r8 =
    					securityConfigSMC
    						securityAlgorithmConfig
    							cipheringAlgorithm = eea1
    							integrityProtAlgorithm = eia1
    ------------------------------------------------------------------------------------------------------------→
    RRC_PDU_REQ:
    ↓	Sent from port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							securityModeCommand
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									c1
    										securityModeCommand_r8
    											securityConfigSMC
    												securityAlgorithmConfig
    													cipheringAlgorithm = eea1 (1)
    													integrityProtAlgorithm = eia1 (1)
    											nonCriticalExtension = Omit

    UL-DCCH-Message:
    	securityModeComplete
    		Source = \Protocol\3GPP\LTE\RRC\
    		UL-DCCH-Message
    			message = c1 = securityModeComplete =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = securityModeComplete-r8 =
    ←------------------------------------------------------------------------------------------------------------
    RRC_PDU_IND:
    ↑	Received on port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 950
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							securityModeComplete
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									securityModeComplete_r8
    										nonCriticalExtension = Omit

    SRB_COMMON_IND:
    ↑	Inter-component message: SRB -> EUTRA_PTC:SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 950
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Dcch
    						message_
    							c1
    								securityModeComplete
    									rrc_TransactionIdentifier = 0
    									criticalExtensions
    										securityModeComplete_r8
    											nonCriticalExtension = Omit
    				Nas = Omit

    SRB_COMMON_REQ:
    ↓	Inter-component message: TC_SRB -> NASEMU_LTE_PTC:TC_SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Dcch
    						message_
    							c1
    								ueCapabilityEnquiry
    									rrc_TransactionIdentifier = 0
    									criticalExtensions
    										c1
    											ueCapabilityEnquiry_r8
    												ue_CapabilityRequest
    													RAT_Type = eutra (0)
    												nonCriticalExtension = Omit
    				Nas = Omit

    DL-DCCH-Message:
    	ueCapabilityEnquiry
    		Source = \Protocol\3GPP\LTE\RRC\
    		DL-DCCH-Message
    			message = c1 = ueCapabilityEnquiry =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = c1 = ueCapabilityEnquiry-r8 =
    					ue-CapabilityRequest = SEQUENCE OF RAT-Type
    						RAT-Type(1) = eutra
    ------------------------------------------------------------------------------------------------------------→
    RRC_PDU_REQ:
    ↓	Sent from port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							ueCapabilityEnquiry
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									c1
    										ueCapabilityEnquiry_r8
    											ue_CapabilityRequest
    												RAT_Type = eutra (0)
    											nonCriticalExtension = Omit

    UL-DCCH-Message:
    	ueCapabilityInformation
    		Source = \Protocol\3GPP\LTE\RRC\
    		UL-DCCH-Message
    			message = c1 = ueCapabilityInformation =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = c1 = ueCapabilityInformation-r8 =
    					ue-CapabilityRAT-ContainerList = SEQUENCE OF UE-CapabilityRAT-Container
    						UE-CapabilityRAT-Container(1)
    							rat-Type = eutra
    							ueCapabilityRAT-Container = C81808FA0610300C001081838B2248A193A3E7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFDFF3FFAFA20C008C87428329D2A4B81C163000000000228008000000
    			UE-CapabilityRAT-Container(1)
    				UE-EUTRA-Capability
    					accessStratumRelease = rel10
    					ue-Category = 1
    					pdcp-Parameters
    						supportedROHC-Profiles
    							profile0x0001 = TRUE
    							profile0x0002 = TRUE
    							profile0x0003 = FALSE
    							profile0x0004 = FALSE
    							profile0x0006 = FALSE
    							profile0x0101 = FALSE
    							profile0x0102 = FALSE
    							profile0x0103 = FALSE
    							profile0x0104 = FALSE
    						maxNumberROHC-ContextSessions  = cs16
    					phyLayerParameters
    						ue-TxAntennaSelectionSupported = TRUE
    						ue-SpecificRefSigsSupported = FALSE
    					rf-Parameters
    						supportedBandListEUTRA = SEQUENCE OF SupportedBandEUTRA
    							SupportedBandEUTRA(1)
    								bandEUTRA = 41
    								halfDuplex = FALSE
    							SupportedBandEUTRA(2)
    								bandEUTRA = 13
    								halfDuplex = FALSE
    							SupportedBandEUTRA(3)
    								bandEUTRA = 17
    								halfDuplex = FALSE
    							SupportedBandEUTRA(4)
    								bandEUTRA = 25
    								halfDuplex = FALSE
    							SupportedBandEUTRA(5)
    								bandEUTRA = 4
    								halfDuplex = FALSE
    							SupportedBandEUTRA(6)
    								bandEUTRA = 1
    								halfDuplex = FALSE
    							SupportedBandEUTRA(7)
    								bandEUTRA = 2
    								halfDuplex = FALSE
    							SupportedBandEUTRA(8)
    								bandEUTRA = 5
    								halfDuplex = FALSE
    							SupportedBandEUTRA(9)
    								bandEUTRA = 7
    								halfDuplex = FALSE
    							SupportedBandEUTRA(10)
    								bandEUTRA = 8
    								halfDuplex = FALSE
    							SupportedBandEUTRA(11)
    								bandEUTRA = 12
    								halfDuplex = FALSE
    							SupportedBandEUTRA(12)
    								bandEUTRA = 18
    								halfDuplex = FALSE
    							SupportedBandEUTRA(13)
    								bandEUTRA = 19
    								halfDuplex = FALSE
    							SupportedBandEUTRA(14)
    								bandEUTRA = 21
    								halfDuplex = FALSE
    							SupportedBandEUTRA(15)
    								bandEUTRA = 26
    								halfDuplex = FALSE
    							SupportedBandEUTRA(16)
    								bandEUTRA = 30
    								halfDuplex = FALSE
    					measParameters
    						bandListEUTRA = SEQUENCE OF BandInfoEUTRA
    							BandInfoEUTRA(1)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(2)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(3)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(4)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(5)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(6)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(7)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(8)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(9)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(10)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(11)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(12)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(13)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(14)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(15)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    							BandInfoEUTRA(16)
    								interFreqBandList = SEQUENCE OF InterFreqBandInfo
    									InterFreqBandInfo(1)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(2)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(3)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(4)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(5)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(6)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(7)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(8)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(9)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(10)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(11)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(12)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(13)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(14)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(15)
    										interFreqNeedForGaps = TRUE
    									InterFreqBandInfo(16)
    										interFreqNeedForGaps = TRUE
    								interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    									InterRAT-BandInfo(1)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(2)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(3)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(4)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(5)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(6)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(7)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(8)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(9)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(10)
    										interRAT-NeedForGaps = TRUE
    									InterRAT-BandInfo(11)
    										interRAT-NeedForGaps = TRUE
    					featureGroupIndicators = 01111111110011111111111010111110
    					interRAT-Parameters
    						utraFDD
    							supportedBandListUTRA-FDD = SEQUENCE OF SupportedBandUTRA-FDD
    								SupportedBandUTRA-FDD(1) = bandI
    								SupportedBandUTRA-FDD(2) = bandII
    								SupportedBandUTRA-FDD(3) = bandIV
    								SupportedBandUTRA-FDD(4) = bandV
    								SupportedBandUTRA-FDD(5) = bandVIII
    								SupportedBandUTRA-FDD(6) = bandIX
    								SupportedBandUTRA-FDD(7) = bandXI
    						geran
    							supportedBandListGERAN = SEQUENCE OF SupportedBandGERAN
    								SupportedBandGERAN(1) = gsm850
    								SupportedBandGERAN(2) = gsm900E
    								SupportedBandGERAN(3) = gsm1800
    								SupportedBandGERAN(4) = gsm1900
    							interRAT-PS-HO-ToGERAN = FALSE
    					nonCriticalExtension
    						phyLayerParameters-v920
    							enhancedDualLayerTDD-r9 = supported
    						interRAT-ParametersGERAN-v920
    							dtm-r9 = supported
    							e-RedirectionGERAN-r9 = supported
    						interRAT-ParametersUTRA-v920
    							e-RedirectionUTRA-r9 = supported
    						csg-ProximityIndicationParameters-r9
    						neighCellSI-AcquisitionParameters-r9
    						son-Parameters-r9
    							rach-Report-r9 = supported
    						nonCriticalExtension
    							lateNonCriticalExtension = CONTAINING =
    								featureGroupIndRel9Add-r9 = 11000000000000000000000000000000
    							nonCriticalExtension
    								featureGroupIndRel10-r10 = 01000000000001000000000000000000
    								nonCriticalExtension
    ←------------------------------------------------------------------------------------------------------------
    RRC_PDU_IND:
    ↑	Received on port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 954
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							ueCapabilityInformation
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									c1
    										ueCapabilityInformation_r8
    											ue_CapabilityRAT_ContainerList
    												UE_CapabilityRAT_Container
    													rat_Type = eutra (0)
    													ueCapabilityRAT_Container = 'C81808FA0610300C001081838B2248A193A3E7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFDFF3FFAFA20C008C87428329D2A4B81C163000000000228008000000'O
    											nonCriticalExtension = Omit

    SRB_COMMON_IND:
    ↑	Inter-component message: SRB -> EUTRA_PTC:SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 954
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Dcch
    						message_
    							c1
    								ueCapabilityInformation
    									rrc_TransactionIdentifier = 0
    									criticalExtensions
    										c1
    											ueCapabilityInformation_r8
    												ue_CapabilityRAT_ContainerList
    													UE_CapabilityRAT_Container
    														rat_Type = eutra (0)
    														ueCapabilityRAT_Container = 'C81808FA0610300C001081838B2248A193A3E7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFE7FFFF95FFDFF3FFAFA20C008C87428329D2A4B81C163000000000228008000000'O
    												nonCriticalExtension = Omit
    				Nas = Omit

    IP_ConfigReq_Type:
    ↓	Inter-component message: EUTRA_CTRL -> IP_PTC:EUTRA_CTRL
    		Source = \Test Control\TTCN3
    		IP_ConfigReq_Type
    			ChangeEutraCell = eutra_CellA (16)

    IP_Indication_Type:
    ↑	Inter-component message: IP -> EUTRA_PTC:IP
    		Source = \Test Control\TTCN3
    		IP_Indication_Type
    			Cnf = True

    SRB_COMMON_REQ:
    ↓	Inter-component message: TC_SRB -> NASEMU_LTE_PTC:TC_SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Dcch
    						message_
    							c1
    								rrcConnectionReconfiguration
    									rrc_TransactionIdentifier = 0
    									criticalExtensions
    										c1
    											rrcConnectionReconfiguration_r8
    												measConfig = Omit
    												mobilityControlInfo = Omit
    												dedicatedInfoNASList = Omit
    												radioResourceConfigDedicated
    													srb_ToAddModList
    														SRB_ToAddMod
    															srb_Identity = 2
    															rlc_Config
    																defaultValue = Null
    															logicalChannelConfig
    																defaultValue = Null
    													drb_ToAddModList
    														DRB_ToAddMod
    															eps_BearerIdentity = 5
    															drb_Identity = 1
    															pdcp_Config
    																discardTimer = infinity_ (7)
    																rlc_AM
    																	statusReportRequired = True
    																rlc_UM = Omit
    																headerCompression
    																	notUsed = Null
    																rn_IntegrityProtection_r10 = Omit
    																pdcp_SN_Size_v1130 = Omit
    																ul_DataSplitDRB_ViaSCG_r12 = Omit
    																t_Reordering_r12 = Omit
    																ul_DataSplitThreshold_r13 = Omit
    																pdcp_SN_Size_v1310 = Omit
    																statusFeedback_r13 = Omit
    															rlc_Config
    																am
    																	ul_AM_RLC
    																		t_PollRetransmit = ms80 (15)
    																		pollPDU = p128 (5)
    																		pollByte = kB125 (4)
    																		maxRetxThreshold = t4 (3)
    																	dl_AM_RLC
    																		t_Reordering = ms80 (16)
    																		t_StatusProhibit = ms60 (12)
    															logicalChannelIdentity = 3
    															logicalChannelConfig
    																ul_SpecificParameters
    																	priority = 6
    																	prioritisedBitRate = kBps0 (0)
    																	bucketSizeDuration = ms100 (1)
    																	logicalChannelGroup = 1
    																logicalChannelSR_Mask_r9 = Omit
    																logicalChannelSR_Prohibit_r12 = Omit
    															drb_TypeChange_r12 = Omit
    															rlc_Config_v1250 = Omit
    															rlc_Config_v1310 = Omit
    															drb_TypeLWA_r13 = Omit
    															drb_TypeLWIP_r13 = Omit
    													drb_ToReleaseList = Omit
    													mac_MainConfig
    														explicitValue
    															ul_SCH_Config
    																maxHARQ_Tx = n5 (4)
    																periodicBSR_Timer = sf20 (3)
    																retxBSR_Timer = sf320 (0)
    																ttiBundling = False
    															drx_Config
    																setup
    																	onDurationTimer = psf6 (5)
    																	drx_InactivityTimer = psf1920 (20)
    																	drx_RetransmissionTimer = psf16 (5)
    																	longDRX_CycleStartOffset
    																		sf1280 = 4
    																	shortDRX = Omit
    															timeAlignmentTimerDedicated = sf750 (1)
    															phr_Config
    																setup
    																	periodicPHR_Timer = sf500 (5)
    																	prohibitPHR_Timer = sf200 (5)
    																	dl_PathlossChange = dB3 (1)
    															sr_ProhibitTimer_r9 = Omit
    															mac_MainConfig_v1020 = Omit
    															stag_ToReleaseList_r11 = Omit
    															stag_ToAddModList_r11 = Omit
    															drx_Config_v1130 = Omit
    															e_HARQ_Pattern_r12 = Omit
    															dualConnectivityPHR = Omit
    															logicalChannelSR_Config_r12 = Omit
    															drx_Config_v1310 = Omit
    															extendedPHR2_r13 = Omit
    															eDRX_Config_CycleStartOffset_r13 = Omit
    															drx_Config_r13 = Omit
    													sps_Config = Omit
    													physicalConfigDedicated
    														pdsch_ConfigDedicated = Omit
    														pucch_ConfigDedicated = Omit
    														pusch_ConfigDedicated = Omit
    														uplinkPowerControlDedicated = Omit
    														tpc_PDCCH_ConfigPUCCH
    															setup
    																tpc_RNTI = 0000001111111111'B
    																tpc_Index
    																	indexOfFormat3 = 1
    														tpc_PDCCH_ConfigPUSCH
    															setup
    																tpc_RNTI = 0000000111111010'B
    																tpc_Index
    																	indexOfFormat3 = 1
    														cqi_ReportConfig
    															cqi_ReportModeAperiodic = rm30 (3)
    															nomPDSCH_RS_EPRE_Offset = 0
    															cqi_ReportPeriodic
    																setup
    																	cqi_PUCCH_ResourceIndex = 0
    																	cqi_pmi_ConfigIndex = 25
    																	cqi_FormatIndicatorPeriodic
    																		widebandCQI = Null
    																	ri_ConfigIndex = 483
    																	simultaneousAckNackAndCQI = False
    														soundingRS_UL_ConfigDedicated
    															setup
    																srs_Bandwidth = bw0 (0)
    																srs_HoppingBandwidth = hbw0 (0)
    																freqDomainPosition = 0
    																duration = True
    																srs_ConfigIndex = 20
    																transmissionComb = 0
    																cyclicShift = cs0 (0)
    														antennaInfo
    															defaultValue = Null
    														schedulingRequestConfig = Omit
    														cqi_ReportConfig_v920 = Omit
    														antennaInfo_v920 = Omit
    														antennaInfo_r10 = Omit
    														antennaInfoUL_r10 = Omit
    														cif_Presence_r10 = Omit
    														cqi_ReportConfig_r10 = Omit
    														csi_RS_Config_r10 = Omit
    														pucch_ConfigDedicated_v1020 = Omit
    														pusch_ConfigDedicated_v1020 = Omit
    														schedulingRequestConfig_v1020 = Omit
    														soundingRS_UL_ConfigDedicated_v1020 = Omit
    														soundingRS_UL_ConfigDedicatedAperiodic_r10 = Omit
    														uplinkPowerControlDedicated_v1020 = Omit
    														additionalSpectrumEmissionCA_r10 = Omit
    														csi_RS_ConfigNZPToReleaseList_r11 = Omit
    														csi_RS_ConfigNZPToAddModList_r11 = Omit
    														csi_RS_ConfigZPToReleaseList_r11 = Omit
    														csi_RS_ConfigZPToAddModList_r11 = Omit
    														epdcch_Config_r11 = Omit
    														pdsch_ConfigDedicated_v1130 = Omit
    														cqi_ReportConfig_v1130 = Omit
    														pucch_ConfigDedicated_v1130 = Omit
    														pusch_ConfigDedicated_v1130 = Omit
    														uplinkPowerControlDedicated_v1130 = Omit
    														antennaInfo_v1250 = Omit
    														eimta_MainConfig_r12 = Omit
    														eimta_MainConfigPCell_r12 = Omit
    														pucch_ConfigDedicated_v1250 = Omit
    														cqi_ReportConfigPCell_v1250 = Omit
    														uplinkPowerControlDedicated_v1250 = Omit
    														pusch_ConfigDedicated_v1250 = Omit
    														csi_RS_Config_v1250 = Omit
    														pdsch_ConfigDedicated_v1280 = Omit
    														pdsch_ConfigDedicated_v1310 = Omit
    														pucch_ConfigDedicated_r13 = Omit
    														pusch_ConfigDedicated_r13 = Omit
    														pdcch_CandidateReductions_r13 = Omit
    														cqi_ReportConfig_v1310 = Omit
    														soundingRS_UL_ConfigDedicated_v1310 = Omit
    														soundingRS_UL_ConfigDedicatedUpPTsExt_r13 = Omit
    														soundingRS_UL_ConfigDedicatedAperiodic_v1310 = Omit
    														soundingRS_UL_ConfigDedicatedAperiodicUpPTsExt_r13 = Omit
    														csi_RS_Config_v1310 = Omit
    														ce_Mode_r13 = Omit
    														csi_RS_ConfigNZPToAddModListExt_r13 = Omit
    														csi_RS_ConfigNZPToReleaseListExt_r13 = Omit
    														cqi_ReportConfig_v1320 = Omit
    													rlf_TimersAndConstants_r9 = Omit
    													measSubframePatternPCell_r10 = Omit
    													neighCellsCRS_Info_r11 = Omit
    													naics_Info_r12 = Omit
    													neighCellsCRS_Info_r13 = Omit
    													rlf_TimersAndConstants_r13 = Omit
    												securityConfigHO = Omit
    												nonCriticalExtension = Omit
    				Nas
    					NAS_MSG_Request_Type
    						SecurityProtection
    							Status = 0010'B
    							ForceMacError = False
    						Pdu
    							Msg
    								aTTACH_ACCEPT
    									securityHeaderType = 0000'B
    									protocolDiscriminator = 0111'B
    									messageType = 01000010'B
    									spareHalfOctet = '0'H
    									epsAttachResult
    										spare = 0'B
    										resultValue = 001'B
    									t3412
    										iei = Omit
    										unit = 111'B
    										timerValue = 00000'B
    									taiList
    										iei = Omit
    										iel = '06'O
    										listOfPartialTais
    											ListOfPartialTaiList
    												spareBit = 0'B
    												typeOfList = 00'B
    												numberOfElements = 00000'B
    												partialTaiList
    													type0List
    														Type0Element
    															plmnId = '00F110'O
    															tacList
    																NAS_Tac = '0001'O
    									esmMessage
    										iei = Omit
    										iel = '0000'O
    										esmPdu = ''O
    									guti
    										iei = '50'O
    										iel = '0B'O
    										idDigit1 = 1111'B
    										oddEvenInd = 0'B
    										typeOfId = 110'B
    										otherDigits = '00F110800101C2345678'O
    									lai = Omit
    									msIdentity = Omit
    									emmCause = Omit
    									t3402 = Omit
    									t3423 = Omit
    									equivalentPlmns = Omit
    									emergencyNumberList = Omit
    									epsNetworkFeatureSupport
    										iei = '64'O
    										iel = '01'O
    										cp_CIOT = 0'B
    										emmRegistered_withoutPDN = 0'B
    										esrps = 0'B
    										csLCS = 00'B
    										epcLCS = 0'B
    										emcBS = 0'B
    										imsVoPS = 1'B
    										spareBits = Omit
    										extdPCO = Omit
    										headerComp_CP_CIOT = Omit
    										s1_U_data = Omit
    										up_CIOT = Omit
    									addUpdateResult = Omit
    									t3412ExtdValue = Omit
    									t3324Value
    										iei = '6A'O
    										iel = '01'O
    										unit = 001'B
    										gprsTimerValue = 00010'B
    									extendedDRXParams = Omit
    							PiggybackedPduList
    								NAS_DL_Pdu_Type
    									Msg
    										aCTIVATE_DEFAULT_EPS_BEARER_CONTEXT_REQUEST
    											epsBearerId = '5'H
    											protocolDiscriminator = 0010'B
    											procedureTransactionIdentifier = '08'O
    											messageType = 11000001'B
    											epsQos
    												iei = Omit
    												iel = '09'O
    												qci = 00001001'B
    												maxBitRateUl = 01000000'B
    												maxBitRateDl = 01000000'B
    												guaranteedBitRateUl = 01000000'B
    												guaranteedBitRateDl = 01000000'B
    												maxBitRateUlExt = 00000000'B
    												maxBitRateDlExt = 00000000'B
    												guaranteedBitRateUlExt = 00000000'B
    												guaranteedBitRateDlExt = 00000000'B
    												maxBitRateDL_Ext2 = Omit
    												guaranteedBitRateDL_Ext2 = Omit
    												maxBitRateUL_Ext2 = Omit
    												guaranteedBitRateUL_Ext2 = Omit
    											accessPointName
    												iei = Omit
    												iel = '04'O
    												nameValue = '0361706E'O
    											pdnAdress
    												iei = Omit
    												iel = '0D'O
    												spare = 00000'B
    												typeValue = 011'B
    												adressInfo = '0000000000000002C0A8001A'O
    											transactionIdentifier
    												iei = '5D'O
    												iel = '01'O
    												tiFlag = 0'B
    												tiValue = 000'B
    												spare = 0000'B
    												ext = Omit
    												tiValue_2 = Omit
    											negotiatedQos
    												iei = '30'O
    												iel = '10'O
    												spare1 = 00'B
    												delayClass = 100'B
    												relabilityClass = 011'B
    												peakThroughput = 0101'B
    												spare2 = 0'B
    												precedenceClass = 010'B
    												spare3 = 000'B
    												meanThroughput = 10000'B
    												trafficClass = 100'B
    												deliveryOrder = 01'B
    												deliveryErrorSDU = 011'B
    												maxSduSize = 10010110'B
    												maxBitRateUL = 01001000'B
    												maxBitRateDL = 01001000'B
    												residualBER = 0111'B
    												sduErrorRatio = 0100'B
    												transferDelay = 000000'B
    												trafficHandlingPrio = 00'B
    												guaranteedBitRateUL = 00000000'B
    												guaranteedBitRateDL = 00000000'B
    												spare4 = 000'B
    												signallingInd = 0'B
    												sourceStatisticsDescriptor = 0000'B
    												maxBitRateDL_Ext = 00000000'B
    												guaranteedBitRateDL_Ext = 00000000'B
    												maxBitRateUL_Ext = 00000000'B
    												guaranteedBitRateUL_Ext = 00000000'B
    												maxBitRateDL_Ext2 = Omit
    												guaranteedBitRateDL_Ext2 = Omit
    												maxBitRateUL_Ext2 = Omit
    												guaranteedBitRateUL_Ext2 = Omit
    											negotiatedLlcSapi
    												iei = '32'O
    												spare = 0000'B
    												llcSapiValue = 1011'B
    											radioPriority
    												iei = '8'H
    												spare = 0'B
    												levelValue = 100'B
    											packetFlowIdentifier
    												iei = '34'O
    												iel = '01'O
    												spare = 0'B
    												idValue = 0000000'B
    											apnAggMaxBitRate = Omit
    											esmCause = Omit
    											protocolConfigurationOptions
    												iei = '27'O
    												iel = '1B'O
    												ext = 1'B
    												spare = 0000'B
    												configProtocol = 000'B
    												pco
    													ProtocolContainer
    														protocolID = '000D'O
    														protocolLength = '04'O
    														content = 'C0A8C637'O
    													ProtocolContainer
    														protocolID = '0003'O
    														protocolLength = '10'O
    														content = 'fd29cc437fb90002020c29fffe66b4c7'O
    											connectivityType = Omit
    											wlanOffloadInd = Omit
    											nbifomContainer = Omit
    											headerCompressionConfig = Omit
    											controlPlaneOnlyIndication = Omit
    											extdProtocolConfigurationOptions = Omit
    											servingPLMNRateControl = Omit
    									PiggybackedPduList = Omit

    Attach Accept:
    	Attach Accept PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Attach Accept
    			Security header type [4 bits] = 0x0 [ 0 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			Message Type [8 bits] = 0x42 - Attach Accept [ 66 ]
    			Spare Half Octet [4 bits] = 0x0 [ 0 ]
    			EPS attach result
    				Spare Bits [1 bit] = 0x0 [ 0 ]
    				Value [3 bits] = 0x1 [ 1 ]
    			T3412 value
    				Timer Value Unit [3 bits] = 0x7 - Value Indicates that the Timer is Deactivated [ 7 ]
    				Value [5 bits] = 0x0 [ 0 ]
    			Tracking area identity list
    				IE Length [8 bits] = 0x6 [ 6 ]
    				Spare Bits [1 bit] = 0x0 [ 0 ]
    				Type of list [2 bits] = 0x0 [ 0 ]
    				number of elements [5 bits] = 0x0 [ 0 ]
    				Mobile Country Code 1st and 2nd  Digits = 0x00 [ 0 ]
    				Mobile Network Code 3rd Digit = 0xF [ 15 ]
    				Mobile Country Code 3rd Digit = 0x1 [ 1 ]
    				Mobile Network Code 1st and 2nd  Digits = 0x10 [ 16 ]
    				Tracking area code 1 = 0x00 [ 0 ]
    				Tracking area code 1 continued = 0x01 [ 1 ]
    			ESM message container
    				IE Length [16 bits] = 0x58 [ 88 ]
    				ESM message container contents = 0x5208C109094040404000000000040361706E0D030000000000000002C0A8001A5D010030102352108B964848740000000000000000320B84340100271B80000D04C0A8C637000310FD29CC437FB90002020C29FFFE66B4C7
    			EPS mobile identity
    				IE Identifier [8 bits] = 0x50 [ 80 ]
    				IE Length [8 bits] = 0xB [ 11 ]
    				constant / IMSI Identity Digit 1 [4 bits] = 0xF [ 15 ]
    				Odd / Even Indicator [1 bit] = 0x0 [ 0 ]
    				EPS Type of Identity [3 bits] = 0x6 - GUTI [ 6 ]
    				Mobile Country Code 1st and 2nd  Digits = 0x00 [ 0 ]
    				Mobile Network Code 3rd Digit = 0xF [ 15 ]
    				Mobile Country Code 3rd Digit = 0x1 [ 1 ]
    				Mobile Network Code 1st and 2nd  Digits = 0x10 [ 16 ]
    				MME group Id = 0x8001 [ 32769 ]
    				MME code = 0x01 [ 1 ]
    				M-TMSI = 0xC2345678 [ 3258209912 ]
    			EPS Network feature support
    				IE Identifier [8 bits] = 0x64 [ 100 ]
    				IE Length [8 bits] = 0x1 [ 1 ]
    				Spare Bits [2 bits] = 0x0 [ 0 ]
    				esr_ps [1 bit] = 0x0 [ 0 ]
    				Location Services Indicator in CS  [2 bits] = 0x0 - No information about support of location services via CS domain is available [ 0 ]
    				Location Services Indicator in EPC [1 bit] = 0x0 - Location services via EPC not supported [ 0 ]
    				Emergency Bearer Services Indicator  [1 bit] = 0x0 - Emergency bearer services in S1 mode not supported [ 0 ]
    				IMS VoPS [1 bit] = 0x1 [ 1 ]
    			t3324_value
    				IE Identifier [8 bits] = 0x6A [ 106 ]
    				IE Length [8 bits] = 0x1 [ 1 ]
    				Timer Value Unit [3 bits] = 0x1 - Value is Incremented in Multiples of 1 Minute  [ 1 ]
    				Value [5 bits] = 0x2 [ 2 ]
    ------------------------------------------------------------------------------------------------------------→
    Activate Default EPS Bearer Context Request:
    	Activate Default EPS Bearer Context Request PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Activate Default EPS Bearer Context Request
    			EPS bearer identity [4 bits] = 0x5 [ 5 ]
    			Protocol Discriminator [4 bits] = 0x2 - EPS Session Management Messages [ 2 ]
    			Procedure transaction identifier [8 bits] = 0x8 [ 8 ]
    			Message Type [8 bits] = 0xC1 - Activate Default EPS Bearer Context Request [ 193 ]
    			EPS QoS
    				IE Length [8 bits] = 0x9 [ 9 ]
    				QCI = 0x09 [ 9 ]
    				Maximum Bit Rate for Uplink = 0x40 - The Maximum Bit Rate is 64 kbps +  ((The Binary Coded Value in 8 Bits -01000000) * 8 Kbps) [ 64 ]
    				Maximum Bit Rate for Dlink = 0x40 - The Maximum Bit Rate is 64 kbps +  ((The Binary Coded Value in 8 Bits -01000000) * 8 Kbps) [ 64 ]
    				Guaranteed Bit Rate for Ulink = 0x40 [ 64 ]
    				Guaranteed Bit Rate for Dlink = 0x40 [ 64 ]
    				Maximum bit rate for uplink (extended) = 0x00 [ 0 ]
    				Maximum bit rate for downlink (extended) = 0x00 [ 0 ]
    				Guaranteed bit rate for uplink (extended) = 0x00 [ 0 ]
    				Guaranteed bit rate for downlink (extended) = 0x00 [ 0 ]
    			APN Address
    				IE Length [8 bits] = 0x4 [ 4 ]
    				Value = 0x0361706E [ 56717422 ]
    			PDN address
    				IE Length [8 bits] = 0xD [ 13 ]
    				Spare Bits [5 bits] = 0x0 [ 0 ]
    				PDN type value [3 bits] = 0x3 [ 3 ]
    				PDN address information = 0x0000000000000002C0A8001A
    			Transaction Identifier
    				IE Identifier [8 bits] = 0x5D [ 93 ]
    				IE Length [8 bits] = 0x1 [ 1 ]
    				Flag [1 bit] = 0x0 - The Message is Sent from the Side That Originates the TI [ 0 ]
    				TI Value [3 bits] = 0x0 [ 0 ]
    				Spare Bits [4 bits] = 0x0 [ 0 ]
    			Negotiated Quality of Service
    				IE Identifier [8 bits] = 0x30 [ 48 ]
    				IE Length [8 bits] = 0x10 [ 16 ]
    				Spare Bits [2 bits] = 0x0 [ 0 ]
    				Delay Class  [3 bits] = 0x4 - Delay Class 4(Best Effort) [ 4 ]
    				Reliability Class  [3 bits] = 0x3 - Unacknowledged GTP and LLC; Acknowledged RLC, Protected Data [ 3 ]
    				Peak Throughput  [4 bits] = 0x5 - Up to 16000 Octet/s [ 5 ]
    				Spare bits B [1 bit] = 0x0 [ 0 ]
    				Precedence Class  [3 bits] = 0x2 - Normal Priority [ 2 ]
    				Spare bits C [3 bits] = 0x0 [ 0 ]
    				Mean Throughput  [5 bits] = 0x10 - 10000000 Octet/h [ 16 ]
    				Traffic Class  [3 bits] = 0x4 - Background Class [ 4 ]
    				Delivery Order  [2 bits] = 0x1 - With Delivery Order ('Yes') [ 1 ]
    				Delivery of Erroneous SDU  [3 bits] = 0x3 - Erroneous SDUs are Not Delivered [ 3 ]
    				Maximum SDU Size  [8 bits] = 0x96 [ 150 ]
    				Maximum Bit Rate for Uplink [8 bits] = 0x48 [ 72 ]
    				Maximum Bit Rate for Dlink [8 bits] = 0x48 [ 72 ]
    				Residual BER  [4 bits] = 0x7 - 1*10E-5  [ 7 ]
    				SDU Error Ratio [4 bits] = 0x4 - 1*10E-4  [ 4 ]
    				Transfer Delay  [6 bits] = 0x0 - Subscribed Traffic Class [ 0 ]
    				Traffic Handler Priority  [2 bits] = 0x0 - Subscribed Traffic Handling Priority [ 0 ]
    				Guaranteed Bit Rate for Ulink [8 bits] = 0x0 [ 0 ]
    				Guaranteed Bit Rate for Dlink  [8 bits] = 0x0 [ 0 ]
    				Spare Bits D [3 bits] = 0x0 [ 0 ]
    				Signalling Indication [1 bit] = 0x0 [ 0 ]
    				Source Statistics Descriptor [4 bits] = 0x0 [ 0 ]
    				Maximum bit rate for downlink (Extended) [8 bits] = 0x0 [ 0 ]
    				Guaranteed bit rate for downlink (Extended) [8 bits] = 0x0 [ 0 ]
    				Max bit rate Uplink extd [8 bits] = 0x0 [ 0 ]
    				Guaranteed bit rate Uplink extd [8 bits] = 0x0 [ 0 ]
    			Negotiated LLC SAPI
    				IE Identifier [8 bits] = 0x32 [ 50 ]
    				Spare Bits [4 bits] = 0x0 [ 0 ]
    				value [4 bits] = 0xB - SAPI 11 [ 11 ]
    			Radio Priority
    				IE Identifier [4 bits] = 0x8 [ 8 ]
    				Spare Bits [1 bit] = 0x0 [ 0 ]
    				value [3 bits] = 0x4 - Priority Level 4 [ 4 ]
    			Packet Flow Identifier
    				IE Identifier [8 bits] = 0x34 [ 52 ]
    				IE Length [8 bits] = 0x1 [ 1 ]
    				Spare Bits [1 bit] = 0x0 [ 0 ]
    				value [7 bits] = 0x0 - Best Effort [ 0 ]
    			Protocol Configuration Options
    				IE Identifier [8 bits] = 0x27 [ 39 ]
    				IE Length [8 bits] = 0x1B [ 27 ]
    				Extension Bit [1 bit] = 0x1 - Outgoing Calls Barred within CUG [ 1 ]
    				Spare Bits [4 bits] = 0x0 [ 0 ]
    				Configuration Protocol [3 bits] = 0x0 - PPP for Use with IP PDP Type [ 0 ]
    				Option1
    					Identifier = 0x000D [ 13 ]
    					Length [8 bits] = 0x4 [ 4 ]
    					value = 0xC0A8C637 [ 3232286263 ]
    				Option2
    					Identifier = 0x0003 - DNS Server Address [ 3 ]
    					Length [8 bits] = 0x10 [ 16 ]
    					Value = 0xFD29CC437FB90002020C29FFFE66B4C7
    ------------------------------------------------------------------------------------------------------------→
    DL-DCCH-Message:
    	rrcConnectionReconfiguration
    		Source = \Protocol\3GPP\LTE\RRC\
    		DL-DCCH-Message
    			message = c1 = rrcConnectionReconfiguration =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = c1 = rrcConnectionReconfiguration-r8 =
    					dedicatedInfoNASList = SEQUENCE OF DedicatedInfoNAS
    						DedicatedInfoNAS(1) = 279A96DD49015C7FD5658A70ECD7585A1AC17A764ECA841F72C06CC567D274980DF884FD91B75592BF2D212DE333B64EC60FCF3FF9CA0EEEC342D4CB31E19277799AED7A84675E86984CEEAFAC3E5D79A311DE3A095A7F374AE6C3517977B17EC6D1AF77AFF3C13692FB55688D97751B730684BCE594F9A14DD5131A6200
    					radioResourceConfigDedicated
    						srb-ToAddModList = SEQUENCE OF SRB-ToAddMod
    							SRB-ToAddMod(1)
    								srb-Identity = 2
    								rlc-Config = defaultValue = NULL
    								logicalChannelConfig = defaultValue = NULL
    						drb-ToAddModList = SEQUENCE OF DRB-ToAddMod
    							DRB-ToAddMod(1)
    								eps-BearerIdentity = 5
    								drb-Identity = 1
    								pdcp-Config
    									discardTimer = infinity
    									rlc-AM
    										statusReportRequired = TRUE
    									headerCompression = notUsed = NULL
    								rlc-Config = am =
    									ul-AM-RLC
    										t-PollRetransmit = ms80
    										pollPDU = p128
    										pollByte = kB125
    										maxRetxThreshold = t4
    									dl-AM-RLC
    										t-Reordering = ms80
    										t-StatusProhibit = ms60
    								logicalChannelIdentity = 3
    								logicalChannelConfig
    									ul-SpecificParameters
    										priority = 6
    										prioritisedBitRate = kBps0
    										bucketSizeDuration = ms100
    										logicalChannelGroup = 1
    						mac-MainConfig = explicitValue =
    							ul-SCH-Config
    								maxHARQ-Tx = n5
    								periodicBSR-Timer = sf20
    								retxBSR-Timer = sf320
    								ttiBundling = FALSE
    							drx-Config = setup =
    								onDurationTimer = psf6
    								drx-InactivityTimer = psf1920
    								drx-RetransmissionTimer = psf16
    								longDRX-CycleStartOffset = sf1280 = 4
    							timeAlignmentTimerDedicated = sf750
    							phr-Config = setup =
    								periodicPHR-Timer = sf500
    								prohibitPHR-Timer = sf200
    								dl-PathlossChange = dB3
    						physicalConfigDedicated
    							tpc-PDCCH-ConfigPUCCH = setup =
    								tpc-RNTI = 0000001111111111
    								tpc-Index = indexOfFormat3 = 1
    							tpc-PDCCH-ConfigPUSCH = setup =
    								tpc-RNTI = 0000000111111010
    								tpc-Index = indexOfFormat3 = 1
    							cqi-ReportConfig
    								cqi-ReportModeAperiodic = rm30
    								nomPDSCH-RS-EPRE-Offset = 0
    								cqi-ReportPeriodic = setup =
    									cqi-PUCCH-ResourceIndex = 0
    									cqi-pmi-ConfigIndex = 25
    									cqi-FormatIndicatorPeriodic = widebandCQI = NULL
    									ri-ConfigIndex = 483
    									simultaneousAckNackAndCQI = FALSE
    							soundingRS-UL-ConfigDedicated = setup =
    								srs-Bandwidth = bw0
    								srs-HoppingBandwidth = hbw0
    								freqDomainPosition = 0
    								duration = TRUE
    								srs-ConfigIndex = 20
    								transmissionComb = 0
    								cyclicShift = cs0
    							antennaInfo = defaultValue = NULL
    ------------------------------------------------------------------------------------------------------------→
    Security Protected NAS Message DL:
    	Security Protected NAS Message DL PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Security Protected NAS Message
    			Security header type [4 bits] = 0x2 [ 2 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			MAC = 0x9A96DD49 [ 2593578313 ]
    			Sequence Number = 0x01 [ 1 ]
    			NAS message = 0x5C7FD5658A70ECD7585A1AC17A764ECA841F72C06CC567D274980DF884FD91B75592BF2D212DE333B64EC60FCF3FF9CA0EEEC342D4CB31E19277799AED7A84675E86984CEEAFAC3E5D79A311DE3A095A7F374AE6C3517977B17EC6D1AF77AFF3C13692FB55688D97751B730684BCE594F9A14DD5131A6200
    ------------------------------------------------------------------------------------------------------------→
    Ciphered NAS Message DL:
    	Ciphered NAS Message DL PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Ciphered NAS Message =
    			0x5C7FD5658A70ECD7585A1AC17A764ECA841F72C06CC567D274980DF884FD91B75592BF2D212DE333B64EC60FCF3FF9CA0EEEC342D4CB31E19277799AED7A84675E86984CEEAFAC3E5D79A311DE3A095A7F374AE6C3517977B17EC6D1AF77AFF3C13692FB55688D97751B730684BCE594F9A14DD5131A6200
    ------------------------------------------------------------------------------------------------------------→
    RRC_PDU_REQ:
    ↓	Sent from port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							rrcConnectionReconfiguration
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									c1
    										rrcConnectionReconfiguration_r8
    											measConfig = Omit
    											mobilityControlInfo = Omit
    											dedicatedInfoNASList
    												NAS_Message = '279A96DD49015C7FD5658A70ECD7585A1AC17A764ECA841F72C06CC567D274980DF884FD91B75592BF2D212DE333B64EC60FCF3FF9CA0EEEC342D4CB31E19277799AED7A84675E86984CEEAFAC3E5D79A311DE3A095A7F374AE6C3517977B17EC6D1AF77AFF3C13692FB55688D97751B730684BCE594F9A14DD5131A6200'O
    											radioResourceConfigDedicated
    												srb_ToAddModList
    													SRB_ToAddMod
    														srb_Identity = 2
    														rlc_Config
    															defaultValue = Null
    														logicalChannelConfig
    															defaultValue = Null
    												drb_ToAddModList
    													DRB_ToAddMod
    														eps_BearerIdentity = 5
    														drb_Identity = 1
    														pdcp_Config
    															discardTimer = infinity_ (7)
    															rlc_AM
    																statusReportRequired = True
    															rlc_UM = Omit
    															headerCompression
    																notUsed = Null
    															rn_IntegrityProtection_r10 = Omit
    															pdcp_SN_Size_v1130 = Omit
    															ul_DataSplitDRB_ViaSCG_r12 = Omit
    															t_Reordering_r12 = Omit
    															ul_DataSplitThreshold_r13 = Omit
    															pdcp_SN_Size_v1310 = Omit
    															statusFeedback_r13 = Omit
    														rlc_Config
    															am
    																ul_AM_RLC
    																	t_PollRetransmit = ms80 (15)
    																	pollPDU = p128 (5)
    																	pollByte = kB125 (4)
    																	maxRetxThreshold = t4 (3)
    																dl_AM_RLC
    																	t_Reordering = ms80 (16)
    																	t_StatusProhibit = ms60 (12)
    														logicalChannelIdentity = 3
    														logicalChannelConfig
    															ul_SpecificParameters
    																priority = 6
    																prioritisedBitRate = kBps0 (0)
    																bucketSizeDuration = ms100 (1)
    																logicalChannelGroup = 1
    															logicalChannelSR_Mask_r9 = Omit
    															logicalChannelSR_Prohibit_r12 = Omit
    														drb_TypeChange_r12 = Omit
    														rlc_Config_v1250 = Omit
    														rlc_Config_v1310 = Omit
    														drb_TypeLWA_r13 = Omit
    														drb_TypeLWIP_r13 = Omit
    												drb_ToReleaseList = Omit
    												mac_MainConfig
    													explicitValue
    														ul_SCH_Config
    															maxHARQ_Tx = n5 (4)
    															periodicBSR_Timer = sf20 (3)
    															retxBSR_Timer = sf320 (0)
    															ttiBundling = False
    														drx_Config
    															setup
    																onDurationTimer = psf6 (5)
    																drx_InactivityTimer = psf1920 (20)
    																drx_RetransmissionTimer = psf16 (5)
    																longDRX_CycleStartOffset
    																	sf1280 = 4
    																shortDRX = Omit
    														timeAlignmentTimerDedicated = sf750 (1)
    														phr_Config
    															setup
    																periodicPHR_Timer = sf500 (5)
    																prohibitPHR_Timer = sf200 (5)
    																dl_PathlossChange = dB3 (1)
    														sr_ProhibitTimer_r9 = Omit
    														mac_MainConfig_v1020 = Omit
    														stag_ToReleaseList_r11 = Omit
    														stag_ToAddModList_r11 = Omit
    														drx_Config_v1130 = Omit
    														e_HARQ_Pattern_r12 = Omit
    														dualConnectivityPHR = Omit
    														logicalChannelSR_Config_r12 = Omit
    														drx_Config_v1310 = Omit
    														extendedPHR2_r13 = Omit
    														eDRX_Config_CycleStartOffset_r13 = Omit
    														drx_Config_r13 = Omit
    												sps_Config = Omit
    												physicalConfigDedicated
    													pdsch_ConfigDedicated = Omit
    													pucch_ConfigDedicated = Omit
    													pusch_ConfigDedicated = Omit
    													uplinkPowerControlDedicated = Omit
    													tpc_PDCCH_ConfigPUCCH
    														setup
    															tpc_RNTI = 0000001111111111'B
    															tpc_Index
    																indexOfFormat3 = 1
    													tpc_PDCCH_ConfigPUSCH
    														setup
    															tpc_RNTI = 0000000111111010'B
    															tpc_Index
    																indexOfFormat3 = 1
    													cqi_ReportConfig
    														cqi_ReportModeAperiodic = rm30 (3)
    														nomPDSCH_RS_EPRE_Offset = 0
    														cqi_ReportPeriodic
    															setup
    																cqi_PUCCH_ResourceIndex = 0
    																cqi_pmi_ConfigIndex = 25
    																cqi_FormatIndicatorPeriodic
    																	widebandCQI = Null
    																ri_ConfigIndex = 483
    																simultaneousAckNackAndCQI = False
    													soundingRS_UL_ConfigDedicated
    														setup
    															srs_Bandwidth = bw0 (0)
    															srs_HoppingBandwidth = hbw0 (0)
    															freqDomainPosition = 0
    															duration = True
    															srs_ConfigIndex = 20
    															transmissionComb = 0
    															cyclicShift = cs0 (0)
    													antennaInfo
    														defaultValue = Null
    													schedulingRequestConfig = Omit
    													cqi_ReportConfig_v920 = Omit
    													antennaInfo_v920 = Omit
    													antennaInfo_r10 = Omit
    													antennaInfoUL_r10 = Omit
    													cif_Presence_r10 = Omit
    													cqi_ReportConfig_r10 = Omit
    													csi_RS_Config_r10 = Omit
    													pucch_ConfigDedicated_v1020 = Omit
    													pusch_ConfigDedicated_v1020 = Omit
    													schedulingRequestConfig_v1020 = Omit
    													soundingRS_UL_ConfigDedicated_v1020 = Omit
    													soundingRS_UL_ConfigDedicatedAperiodic_r10 = Omit
    													uplinkPowerControlDedicated_v1020 = Omit
    													additionalSpectrumEmissionCA_r10 = Omit
    													csi_RS_ConfigNZPToReleaseList_r11 = Omit
    													csi_RS_ConfigNZPToAddModList_r11 = Omit
    													csi_RS_ConfigZPToReleaseList_r11 = Omit
    													csi_RS_ConfigZPToAddModList_r11 = Omit
    													epdcch_Config_r11 = Omit
    													pdsch_ConfigDedicated_v1130 = Omit
    													cqi_ReportConfig_v1130 = Omit
    													pucch_ConfigDedicated_v1130 = Omit
    													pusch_ConfigDedicated_v1130 = Omit
    													uplinkPowerControlDedicated_v1130 = Omit
    													antennaInfo_v1250 = Omit
    													eimta_MainConfig_r12 = Omit
    													eimta_MainConfigPCell_r12 = Omit
    													pucch_ConfigDedicated_v1250 = Omit
    													cqi_ReportConfigPCell_v1250 = Omit
    													uplinkPowerControlDedicated_v1250 = Omit
    													pusch_ConfigDedicated_v1250 = Omit
    													csi_RS_Config_v1250 = Omit
    													pdsch_ConfigDedicated_v1280 = Omit
    													pdsch_ConfigDedicated_v1310 = Omit
    													pucch_ConfigDedicated_r13 = Omit
    													pusch_ConfigDedicated_r13 = Omit
    													pdcch_CandidateReductions_r13 = Omit
    													cqi_ReportConfig_v1310 = Omit
    													soundingRS_UL_ConfigDedicated_v1310 = Omit
    													soundingRS_UL_ConfigDedicatedUpPTsExt_r13 = Omit
    													soundingRS_UL_ConfigDedicatedAperiodic_v1310 = Omit
    													soundingRS_UL_ConfigDedicatedAperiodicUpPTsExt_r13 = Omit
    													csi_RS_Config_v1310 = Omit
    													ce_Mode_r13 = Omit
    													csi_RS_ConfigNZPToAddModListExt_r13 = Omit
    													csi_RS_ConfigNZPToReleaseListExt_r13 = Omit
    													cqi_ReportConfig_v1320 = Omit
    												rlf_TimersAndConstants_r9 = Omit
    												measSubframePatternPCell_r10 = Omit
    												neighCellsCRS_Info_r11 = Omit
    												naics_Info_r12 = Omit
    												neighCellsCRS_Info_r13 = Omit
    												rlf_TimersAndConstants_r13 = Omit
    											securityConfigHO = Omit
    											nonCriticalExtension = Omit

    UL-DCCH-Message:
    	rrcConnectionReconfigurationComplete
    		Source = \Protocol\3GPP\LTE\RRC\
    		UL-DCCH-Message
    			message = c1 = rrcConnectionReconfigurationComplete =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = rrcConnectionReconfigurationComplete-r8 =
    ←------------------------------------------------------------------------------------------------------------
    RRC_PDU_IND:
    ↑	Received on port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 962
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							rrcConnectionReconfigurationComplete
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									rrcConnectionReconfigurationComplete_r8
    										nonCriticalExtension = Omit

    SRB_COMMON_IND:
    ↑	Inter-component message: SRB -> EUTRA_PTC:SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 962
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Dcch
    						message_
    							c1
    								rrcConnectionReconfigurationComplete
    									rrc_TransactionIdentifier = 0
    									criticalExtensions
    										rrcConnectionReconfigurationComplete_r8
    											nonCriticalExtension = Omit
    				Nas = Omit

    UL-DCCH-Message:
    	ulInformationTransfer
    		Source = \Protocol\3GPP\LTE\RRC\
    		UL-DCCH-Message
    			message = c1 = ulInformationTransfer =
    				criticalExtensions = c1 = ulInformationTransfer-r8 =
    					dedicatedInfoType = dedicatedInfoNAS = 2714DCDAF701D390BB9B16B4E5
    ←------------------------------------------------------------------------------------------------------------
    Security Protected NAS Message UL:
    	Security Protected NAS Message UL PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Security Protected NAS Message
    			Security header type [4 bits] = 0x2 [ 2 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			MAC = 0x145C5A77 [ 341596791 ]
    			Sequence Number = 0x01 [ 1 ]
    			NAS message = 0x53103B1B163465
    ←------------------------------------------------------------------------------------------------------------
    Ciphered NAS Message UL:
    	Ciphered NAS Message UL PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Ciphered NAS Message =
    			0x53103B1B163465
    ←------------------------------------------------------------------------------------------------------------
    RRC_PDU_IND:
    ↑	Received on port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 2
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 964
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							ulInformationTransfer
    								criticalExtensions
    									c1
    										ulInformationTransfer_r8
    											dedicatedInfoType
    												dedicatedInfoNAS = '2714DCDAF701D390BB9B16B4E5'O
    											nonCriticalExtension = Omit

    Attach Complete:
    	Attach Complete PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Attach Complete
    			Security header type [4 bits] = 0x0 [ 0 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			Message Type [8 bits] = 0x43 - Attach Complete [ 67 ]
    			ESM message container
    				IE Length [16 bits] = 0x3 [ 3 ]
    				ESM message container contents = 0x5200C2 [ 5374146 ]
    ←------------------------------------------------------------------------------------------------------------
    Activate Default EPS Bearer Context Accept:
    	Activate Default EPS Bearer Context Accept PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Activate Default EPS Bearer Context Accept
    			EPS bearer identity [4 bits] = 0x5 [ 5 ]
    			Protocol Discriminator [4 bits] = 0x2 - EPS Session Management Messages [ 2 ]
    			Procedure transaction identifier [8 bits] = 0x0 [ 0 ]
    			Message Type [8 bits] = 0xC2 - Activate Default EPS Bearer Context Accept [ 194 ]
    ←------------------------------------------------------------------------------------------------------------
    SRB_COMMON_IND:
    ↑	Inter-component message: SRB -> EUTRA_PTC:SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 2
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 964
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			Signalling
    				Rrc = Omit
    				Nas
    					NasIndication
    						SecurityProtection
    							Status = 0010'B
    							NasCount = '00000001'O
    						Pdu
    							Msg
    								aTTACH_COMPLETE
    									securityHeaderType = 0000'B
    									protocolDiscriminator = 0111'B
    									messageType = 01000011'B
    									esmMessage
    										iei = Omit
    										iel = '0003'O
    										esmPdu = '5200C2'O
    							PiggybackedPduList
    								NAS_UL_Pdu_Type
    									Msg
    										aCTIVATE_DEFAULT_EPS_BEARER_CONTEXT_ACCEPT
    											epsBearerId = '5'H
    											protocolDiscriminator = 0010'B
    											procedureTransactionIdentifier = '00'O
    											messageType = 11000010'B
    											protocolConfigurationOptions = Omit
    											extdProtocolConfigurationOptions = Omit
    									PiggybackedPduList = Omit

    Timer Event:
    	Timer: t_WaitForUPlaneSignalling, Duration: 1.2s, Started: 17:35:14
    		Source = \Test Control\TTCN3
    		timerEvent = 6
    		fileName = C:\CT_LTE\ETSI\v41_Dev\RC1\Final PSM MKS\LTE_A_R12_IWD_16wk37\Common\IMS\IMS_PTC_CoordMsg.ttcn
    		testName = TC_9_2_1_1_7c
    		lineNo = 413
    		outStr = Timer: t_WaitForUPlaneSignalling, Duration: 1.2s, Started: 17:35:14

    Timer Event:
    	Timer: t_WaitForUPlaneSignalling, Expired: 17:35:15
    		Source = \Test Control\TTCN3
    		timerEvent = 9
    		fileName = C:\CT_LTE\ETSI\v41_Dev\RC1\Final PSM MKS\LTE_A_R12_IWD_16wk37\Common\IMS\IMS_PTC_CoordMsg.ttcn
    		testName = TC_9_2_1_1_7c
    		lineNo = 415
    		outStr = Timer: t_WaitForUPlaneSignalling, Expired: 17:35:15

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = True
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				EnquireTiming = True

    SYSTEM_CTRL_CNF:
    ↑	Received on port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_CNF
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 62
    						Subframe
    							Number = 2
    						HSFN
    							Number = 0
    				Result
    					Success = True
    			Confirm
    				EnquireTiming = True

    Timer Event:
    	Timer: t_Timer, Duration: 1.22s, Started: 17:35:15
    		Source = \Test Control\TTCN3
    		timerEvent = 6
    		fileName = C:\CT_LTE\ETSI\v41_Dev\RC1\Final PSM MKS\LTE_A_R12_IWD_16wk37\Common\EUTRA\EUTRA_RRCSteps.ttcn
    		testName = TC_9_2_1_1_7c
    		lineNo = 1418
    		outStr = Timer: t_Timer, Duration: 1.22s, Started: 17:35:15

    SRB_COMMON_REQ:
    ↓	Inter-component message: TC_SRB -> NASEMU_LTE_PTC:TC_SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 92
    						Subframe
    							Number = 4
    						HSFN
    							Number = 0
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Dcch
    						message_
    							c1
    								rrcConnectionRelease
    									rrc_TransactionIdentifier = 0
    									criticalExtensions
    										c1
    											rrcConnectionRelease_r8
    												releaseCause = other (1)
    												redirectedCarrierInfo = Omit
    												idleModeMobilityControlInfo = Omit
    												nonCriticalExtension = Omit
    				Nas = Omit

    DL-DCCH-Message:
    	rrcConnectionRelease
    		Source = \Protocol\3GPP\LTE\RRC\
    		DL-DCCH-Message
    			message = c1 = rrcConnectionRelease =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = c1 = rrcConnectionRelease-r8 =
    					releaseCause = other
    ------------------------------------------------------------------------------------------------------------→
    RRC_PDU_REQ:
    ↓	Sent from port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 92
    						Subframe
    							Number = 4
    						HSFN
    							Number = 0
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							rrcConnectionRelease
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									c1
    										rrcConnectionRelease_r8
    											releaseCause = other (1)
    											redirectedCarrierInfo = Omit
    											idleModeMobilityControlInfo = Omit
    											nonCriticalExtension = Omit

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = True
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				PdcpCount
    					Get
    						AllRBs = True

    SYSTEM_CTRL_CNF:
    ↑	Received on port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_CNF
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				Result
    					Success = True
    			Confirm
    				PdcpCount
    					Get
    						PdcpCountInfo_Type
    							RadioBearerId
    								Srb = 1
    							UL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000110'B
    							DL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000101'B
    						PdcpCountInfo_Type
    							RadioBearerId
    								Srb = 2
    							UL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000001'B
    							DL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000000'B
    						PdcpCountInfo_Type
    							RadioBearerId
    								Drb = 1
    							UL
    								Format = PdcpCount_DrbShortSQN (2)
    								Value = 00000000000000000000000000000000'B
    							DL
    								Format = PdcpCount_DrbShortSQN (2)
    								Value = 00000000000000000000000000000000'B

    MATCH_MISMATCH:
    ↑	Message Mismatch: TimingInfo_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: TimingInfo_Type
    		MATCH_MISMATCH
    			Message Mismatch: TimingInfo_Type
    				SubFrame
    					SFN
    						Number = 92
    					Subframe
    						Number = 4
    					HSFN
    						Number = 0

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 92
    						Subframe
    							Number = 4
    						HSFN
    							Number = 0
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				Cell
    					AddOrReconfigure
    						Basic = Omit
    						Active
    							C_RNTI = Omit
    							PhysicalLayerConfigUL = Omit
    							RachProcedureConfig = Omit
    							CcchDcchDtchConfig
    								MeasGapCtrl = Omit
    								DL = Omit
    								UL
    									DciInfo = Omit
    									Hopping
    										Deactivated = True
    									PUCCH_Synch
    										None = True
    									UL_GrantConfig
    										None = True
    								DrxCtrl = Omit
    								TtiBundling = Omit
    								CifPresence = Omit
    							ServingCellConfig = Omit
    							SciSchedulingConfig = Omit
    							EIMTA_Config = Omit
    							CE_Mode = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: TimingInfo_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: TimingInfo_Type
    		MATCH_MISMATCH
    			Message Mismatch: TimingInfo_Type
    				SubFrame
    					SFN
    						Number = 92
    					Subframe
    						Number = 9
    					HSFN
    						Number = 0

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 92
    						Subframe
    							Number = 9
    						HSFN
    							Number = 0
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				AS_Security
    					Release = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: TimingInfo_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: TimingInfo_Type
    		MATCH_MISMATCH
    			Message Mismatch: TimingInfo_Type
    				SubFrame
    					SFN
    						Number = 97
    					Subframe
    						Number = 9
    					HSFN
    						Number = 0

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 97
    						Subframe
    							Number = 9
    						HSFN
    							Number = 0
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				RadioBearerList
    					RadioBearer_Type
    						Id
    							Srb = 1
    						Config
    							Release = True
    					RadioBearer_Type
    						Id
    							Srb = 2
    						Config
    							Release = True
    					RadioBearer_Type
    						Id
    							Drb = 1
    						Config
    							Release = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: TimingInfo_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: TimingInfo_Type
    		MATCH_MISMATCH
    			Message Mismatch: TimingInfo_Type
    				SubFrame
    					SFN
    						Number = 98
    					Subframe
    						Number = 4
    					HSFN
    						Number = 0

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 98
    						Subframe
    							Number = 4
    						HSFN
    							Number = 0
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				RadioBearerList
    					RadioBearer_Type
    						Id
    							Srb = 1
    						Config
    							AddOrReconfigure
    								Pdcp
    									Config
    										Rb
    											Srb = True
    										TestMode
    											None = True
    								Rlc
    									Rb
    										AM
    											Tx
    												R8
    													t_PollRetransmit = ms45 (8)
    													pollPDU = pInfinity (7)
    													pollByte = kBinfinity (14)
    													maxRetxThreshold = t4 (3)
    											Rx
    												R8
    													t_Reordering = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    											ExtendedLI = Omit
    									TestMode
    										None = True
    								LogicalChannelId = 1
    								Mac
    									LogicalChannel
    										Priority = 1
    										PrioritizedBitRate = infinity_ (7)
    									TestMode
    										None = True
    								DiscardULData = Omit
    					RadioBearer_Type
    						Id
    							Srb = 2
    						Config
    							AddOrReconfigure
    								Pdcp
    									Config
    										Rb
    											Srb = True
    										TestMode
    											None = True
    								Rlc
    									Rb
    										AM
    											Tx
    												R8
    													t_PollRetransmit = ms45 (8)
    													pollPDU = pInfinity (7)
    													pollByte = kBinfinity (14)
    													maxRetxThreshold = t4 (3)
    											Rx
    												R8
    													t_Reordering = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    											ExtendedLI = Omit
    									TestMode
    										None = True
    								LogicalChannelId = 2
    								Mac
    									LogicalChannel
    										Priority = 3
    										PrioritizedBitRate = infinity_ (7)
    									TestMode
    										None = True
    								DiscardULData = Omit

    Timer Event:
    	Timer: t_Timer, Expired: 17:35:17
    		Source = \Test Control\TTCN3
    		timerEvent = 9
    		fileName = C:\CT_LTE\ETSI\v41_Dev\RC1\Final PSM MKS\LTE_A_R12_IWD_16wk37\Common\EUTRA\EUTRA_RRCSteps.ttcn
    		testName = TC_9_2_1_1_7c
    		lineNo = 1427
    		outStr = Timer: t_Timer, Expired: 17:35:17

    Timer Event:
    	Timer: t_Delay, Duration: 60s, Started: 17:35:17
    		Source = \Test Control\TTCN3
    		timerEvent = 6
    		fileName = C:\CT_LTE\ETSI\v41_Dev\RC1\Final PSM MKS\LTE_A_R12_IWD_16wk37\Common\Common\CommonDefs.ttcn
    		testName = TC_9_2_1_1_7c
    		lineNo = 404
    		outStr = Timer: t_Delay, Duration: 60s, Started: 17:35:17

    Timer Event:
    	Timer: t_Delay, Expired: 17:36:17
    		Source = \Test Control\TTCN3
    		timerEvent = 9
    		fileName = C:\CT_LTE\ETSI\v41_Dev\RC1\Final PSM MKS\LTE_A_R12_IWD_16wk37\Common\Common\CommonDefs.ttcn
    		testName = TC_9_2_1_1_7c
    		lineNo = 405
    		outStr = Timer: t_Delay, Expired: 17:36:17

    TTCN Test Step:
    	Step 14-24
    		Source = \Test Control\TTCN3
    		recordType = 24
    		summary = Step 14-24

    Timer Event:
    	Timer: t_Delay, Duration: 1s, Started: 17:36:17
    		Source = \Test Control\TTCN3
    		timerEvent = 6
    		fileName = C:\CT_LTE\ETSI\v41_Dev\RC1\Final PSM MKS\LTE_A_R12_IWD_16wk37\Common\Common\CommonDefs.ttcn
    		testName = TC_9_2_1_1_7c
    		lineNo = 404
    		outStr = Timer: t_Delay, Duration: 1s, Started: 17:36:17

    Timer Event:
    	Timer: t_Delay, Expired: 17:36:18
    		Source = \Test Control\TTCN3
    		timerEvent = 9
    		fileName = C:\CT_LTE\ETSI\v41_Dev\RC1\Final PSM MKS\LTE_A_R12_IWD_16wk37\Common\Common\CommonDefs.ttcn
    		testName = TC_9_2_1_1_7c
    		lineNo = 405
    		outStr = Timer: t_Delay, Expired: 17:36:18

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = True
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				EnquireTiming = True

    SYSTEM_CTRL_CNF:
    ↑	Received on port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_CNF
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 145
    						Subframe
    							Number = 2
    						HSFN
    							Number = 0
    				Result
    					Success = True
    			Confirm
    				EnquireTiming = True

    PCCH-Message:
    	paging
    		Source = \Protocol\3GPP\LTE\RRC\
    		PCCH-Message
    			message = c1 = paging =
    				pagingRecordList = SEQUENCE OF PagingRecord
    					PagingRecord(1)
    						ue-Identity = s-TMSI =
    							mmec = 00000001
    							m-TMSI = 11000010001101000101011001111000
    						cn-Domain = ps
    ------------------------------------------------------------------------------------------------------------→
    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 277
    						Subframe
    							Number = 9
    						HSFN
    							Number = 0
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				Paging
    					Paging
    						message_
    							c1
    								paging
    									pagingRecordList
    										PagingRecord
    											ue_Identity
    												s_TMSI
    													mmec = 00000001'B
    													m_TMSI = 11000010001101000101011001111000'B
    											cn_Domain = ps (0)
    									systemInfoModification = Omit
    									etws_Indication = Omit
    									nonCriticalExtension = Omit
    					SubframeOffsetList = Omit

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				Cell
    					AddOrReconfigure
    						Basic = Omit
    						Active
    							C_RNTI = Omit
    							PhysicalLayerConfigUL = Omit
    							RachProcedureConfig = Omit
    							CcchDcchDtchConfig
    								MeasGapCtrl = Omit
    								DL = Omit
    								UL
    									DciInfo
    										Imcs
    											Value = 9
    										TransRetransmissionList
    											UL_TransRetransmission_Type
    												NewTransmission = True
    										FreqDomainSchedul
    											FirstRbIndex = 0
    											Nprb = 25
    										RepetitionNumber = Omit
    									Hopping
    										Deactivated = True
    									PUCCH_Synch
    										None = True
    									UL_GrantConfig
    										OnSR_Reception = True
    								DrxCtrl = Omit
    								TtiBundling = Omit
    								CifPresence = Omit
    							ServingCellConfig = Omit
    							SciSchedulingConfig = Omit
    							EIMTA_Config = Omit
    							CE_Mode = Omit

    UL-CCCH-Message:
    	rrcConnectionRequest
    		Source = \Protocol\3GPP\LTE\RRC\
    		UL-CCCH-Message
    			message = c1 = rrcConnectionRequest =
    				criticalExtensions = rrcConnectionRequest-r8 =
    					ue-Identity = s-TMSI =
    						mmec = 00000001
    						m-TMSI = 11000010001101000101011001111000
    					establishmentCause = mt-Access
    					spare = 0
    ←------------------------------------------------------------------------------------------------------------
    RRC_PDU_IND:
    ↑	Received on port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 0
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 283
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			RrcPdu
    				Ccch
    					message_
    						c1
    							rrcConnectionRequest
    								criticalExtensions
    									rrcConnectionRequest_r8
    										ue_Identity
    											s_TMSI
    												mmec = 00000001'B
    												m_TMSI = 11000010001101000101011001111000'B
    										establishmentCause = mt_Access (2)
    										spare = 0'B

    SRB_COMMON_IND:
    ↑	Inter-component message: SRB -> EUTRA_PTC:SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 0
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 283
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Ccch
    						message_
    							c1
    								rrcConnectionRequest
    									criticalExtensions
    										rrcConnectionRequest_r8
    											ue_Identity
    												s_TMSI
    													mmec = 00000001'B
    													m_TMSI = 11000010001101000101011001111000'B
    											establishmentCause = mt_Access (2)
    											spare = 0'B
    				Nas = Omit

    UL-DCCH-Message:
    	rrcConnectionSetupComplete
    		Source = \Protocol\3GPP\LTE\RRC\
    		UL-DCCH-Message
    			message = c1 = rrcConnectionSetupComplete =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = c1 = rrcConnectionSetupComplete-r8 =
    					selectedPLMN-Identity = 1
    					dedicatedInfoNAS = C7223FCC
    ←------------------------------------------------------------------------------------------------------------
    Service Request:
    	Service Request PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Service Request
    			Security header type [4 bits] = 0xC [ 12 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			KSI and sequence number
    				key set identifier [3 bits] = 0x1 [ 1 ]
    				Sequence number (short) [5 bits] = 0x2 [ 2 ]
    			Message authentication code (short)
    				mac value = 0x3FCC [ 16332 ]
    ←------------------------------------------------------------------------------------------------------------
    RRC_PDU_IND:
    ↑	Received on port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 286
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							rrcConnectionSetupComplete
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									c1
    										rrcConnectionSetupComplete_r8
    											selectedPLMN_Identity = 1
    											registeredMME = Omit
    											dedicatedInfoNAS = 'C7223FCC'O
    											nonCriticalExtension = Omit

    SRB_COMMON_IND:
    ↑	Inter-component message: SRB -> EUTRA_PTC:SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 286
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Dcch
    						message_
    							c1
    								rrcConnectionSetupComplete
    									rrc_TransactionIdentifier = 0
    									criticalExtensions
    										c1
    											rrcConnectionSetupComplete_r8
    												selectedPLMN_Identity = 1
    												registeredMME = Omit
    												dedicatedInfoNAS = 'C7223FCC'O
    												nonCriticalExtension = Omit
    				Nas
    					NasIndication
    						SecurityProtection
    							Status = 0001'B
    							NasCount = '00000002'O
    						Pdu
    							Msg
    								sERVICE_REQUEST
    									securityHeaderType = 1100'B
    									protocolDiscriminator = 0111'B
    									ksiAndSN
    										iei = Omit
    										ksi = 001'B
    										sn = 00010'B
    									shortMAC
    										iei = Omit
    										macValue = 0011111111001100'B
    							PiggybackedPduList = Omit

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = True
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				Cell
    					AddOrReconfigure
    						Basic = Omit
    						Active
    							C_RNTI = Omit
    							PhysicalLayerConfigUL = Omit
    							RachProcedureConfig = Omit
    							CcchDcchDtchConfig
    								MeasGapCtrl = Omit
    								DL = Omit
    								UL
    									DciInfo = Omit
    									Hopping
    										Deactivated = True
    									PUCCH_Synch
    										Auto
    											TimingAdvance = 31
    											TA_Period = 600
    											TA_Repetition
    												Continuous = True
    									UL_GrantConfig = Omit
    								DrxCtrl = Omit
    								TtiBundling = Omit
    								CifPresence = Omit
    							ServingCellConfig = Omit
    							SciSchedulingConfig = Omit
    							EIMTA_Config = Omit
    							CE_Mode = Omit

    SYSTEM_CTRL_CNF:
    ↑	Received on port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_CNF
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				Result
    					Success = True
    			Confirm
    				Cell = True

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = True
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				RadioBearerList
    					RadioBearer_Type
    						Id
    							Drb = 1
    						Config
    							AddOrReconfigure
    								Pdcp
    									Config
    										Rb
    											Drb
    												R8
    													discardTimer = infinity_ (7)
    													rlc_AM
    														statusReportRequired = True
    													rlc_UM = Omit
    													headerCompression
    														notUsed = Null
    													rn_IntegrityProtection_r10 = Omit
    													pdcp_SN_Size_v1130 = Omit
    													ul_DataSplitDRB_ViaSCG_r12 = Omit
    													t_Reordering_r12 = Omit
    													ul_DataSplitThreshold_r13 = Omit
    													pdcp_SN_Size_v1310 = Omit
    													statusFeedback_r13 = Omit
    										TestMode
    											None = True
    								Rlc
    									Rb
    										AM
    											Tx
    												R8
    													t_PollRetransmit = ms80 (15)
    													pollPDU = p128 (5)
    													pollByte = kB125 (4)
    													maxRetxThreshold = t4 (3)
    											Rx
    												R8
    													t_Reordering = ms80 (16)
    													t_StatusProhibit = ms60 (12)
    											ExtendedLI = Omit
    									TestMode
    										None = True
    								LogicalChannelId = 3
    								Mac
    									LogicalChannel
    										Priority = 13
    										PrioritizedBitRate = kBps0 (0)
    									TestMode
    										None = True
    								DiscardULData = Omit

    SYSTEM_CTRL_CNF:
    ↑	Received on port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_CNF
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				Result
    					Success = True
    			Confirm
    				RadioBearerList = True

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = True
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				PdcpCount
    					Get
    						AllRBs = True

    SYSTEM_CTRL_CNF:
    ↑	Received on port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_CNF
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				Result
    					Success = True
    			Confirm
    				PdcpCount
    					Get
    						PdcpCountInfo_Type
    							RadioBearerId
    								Srb = 1
    							UL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000001'B
    							DL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000000'B
    						PdcpCountInfo_Type
    							RadioBearerId
    								Srb = 2
    							UL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000000'B
    							DL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000000'B
    						PdcpCountInfo_Type
    							RadioBearerId
    								Drb = 1
    							UL
    								Format = PdcpCount_DrbShortSQN (2)
    								Value = 00000000000000000000000000000000'B
    							DL
    								Format = PdcpCount_DrbShortSQN (2)
    								Value = 00000000000000000000000000000000'B

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = True
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				AS_Security
    					StartRestart
    						Integrity
    							Algorithm = eia1 (1)
    							KRRCint = 01001100101010000111000001001101010110101101011101001101111000001100010011110100001111111000000000011100110101110100010011011110'B
    							ActTimeList = Omit
    						Ciphering
    							Algorithm = eea1 (1)
    							KRRCenc = 01010010110101110110010010010000111101011010010011100001110100000111011000000001100000010011111101011101100011110001100100001010'B
    							KUPenc = 01000000110111001000100101100111000111111001111101100111111111111011011111001111011011100000000001011010001011100000001000010001'B
    							ActTimeList
    								SecurityActTime_Type
    									RadioBearerId
    										Srb = 1
    									UL
    										SQN
    											Format = PdcpCount_Srb (0)
    											Value = 2
    									DL
    										SQN
    											Format = PdcpCount_Srb (0)
    											Value = 1
    								SecurityActTime_Type
    									RadioBearerId
    										Srb = 2
    									UL
    										SQN
    											Format = PdcpCount_Srb (0)
    											Value = 0
    									DL
    										SQN
    											Format = PdcpCount_Srb (0)
    											Value = 0
    								SecurityActTime_Type
    									RadioBearerId
    										Drb = 1
    									UL
    										SQN
    											Format = PdcpCount_DrbShortSQN (2)
    											Value = 0
    									DL
    										SQN
    											Format = PdcpCount_DrbShortSQN (2)
    											Value = 0

    SYSTEM_CTRL_CNF:
    ↑	Received on port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_CNF
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				Result
    					Success = True
    			Confirm
    				AS_Security = True

    SRB_COMMON_REQ:
    ↓	Inter-component message: TC_SRB -> NASEMU_LTE_PTC:TC_SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Dcch
    						message_
    							c1
    								securityModeCommand
    									rrc_TransactionIdentifier = 0
    									criticalExtensions
    										c1
    											securityModeCommand_r8
    												securityConfigSMC
    													securityAlgorithmConfig
    														cipheringAlgorithm = eea1 (1)
    														integrityProtAlgorithm = eia1 (1)
    												nonCriticalExtension = Omit
    				Nas = Omit

    DL-DCCH-Message:
    	securityModeCommand
    		Source = \Protocol\3GPP\LTE\RRC\
    		DL-DCCH-Message
    			message = c1 = securityModeCommand =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = c1 = securityModeCommand-r8 =
    					securityConfigSMC
    						securityAlgorithmConfig
    							cipheringAlgorithm = eea1
    							integrityProtAlgorithm = eia1
    ------------------------------------------------------------------------------------------------------------→
    RRC_PDU_REQ:
    ↓	Sent from port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							securityModeCommand
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									c1
    										securityModeCommand_r8
    											securityConfigSMC
    												securityAlgorithmConfig
    													cipheringAlgorithm = eea1 (1)
    													integrityProtAlgorithm = eia1 (1)
    											nonCriticalExtension = Omit

    UL-DCCH-Message:
    	securityModeComplete
    		Source = \Protocol\3GPP\LTE\RRC\
    		UL-DCCH-Message
    			message = c1 = securityModeComplete =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = securityModeComplete-r8 =
    ←------------------------------------------------------------------------------------------------------------
    RRC_PDU_IND:
    ↑	Received on port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 294
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							securityModeComplete
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									securityModeComplete_r8
    										nonCriticalExtension = Omit

    SRB_COMMON_IND:
    ↑	Inter-component message: SRB -> EUTRA_PTC:SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 294
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Dcch
    						message_
    							c1
    								securityModeComplete
    									rrc_TransactionIdentifier = 0
    									criticalExtensions
    										securityModeComplete_r8
    											nonCriticalExtension = Omit
    				Nas = Omit

    SRB_COMMON_REQ:
    ↓	Inter-component message: TC_SRB -> NASEMU_LTE_PTC:TC_SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Dcch
    						message_
    							c1
    								rrcConnectionReconfiguration
    									rrc_TransactionIdentifier = 0
    									criticalExtensions
    										c1
    											rrcConnectionReconfiguration_r8
    												measConfig = Omit
    												mobilityControlInfo = Omit
    												dedicatedInfoNASList = Omit
    												radioResourceConfigDedicated
    													srb_ToAddModList
    														SRB_ToAddMod
    															srb_Identity = 2
    															rlc_Config
    																defaultValue = Null
    															logicalChannelConfig
    																defaultValue = Null
    													drb_ToAddModList
    														DRB_ToAddMod
    															eps_BearerIdentity = 5
    															drb_Identity = 1
    															pdcp_Config
    																discardTimer = infinity_ (7)
    																rlc_AM
    																	statusReportRequired = True
    																rlc_UM = Omit
    																headerCompression
    																	notUsed = Null
    																rn_IntegrityProtection_r10 = Omit
    																pdcp_SN_Size_v1130 = Omit
    																ul_DataSplitDRB_ViaSCG_r12 = Omit
    																t_Reordering_r12 = Omit
    																ul_DataSplitThreshold_r13 = Omit
    																pdcp_SN_Size_v1310 = Omit
    																statusFeedback_r13 = Omit
    															rlc_Config
    																am
    																	ul_AM_RLC
    																		t_PollRetransmit = ms80 (15)
    																		pollPDU = p128 (5)
    																		pollByte = kB125 (4)
    																		maxRetxThreshold = t4 (3)
    																	dl_AM_RLC
    																		t_Reordering = ms80 (16)
    																		t_StatusProhibit = ms60 (12)
    															logicalChannelIdentity = 3
    															logicalChannelConfig
    																ul_SpecificParameters
    																	priority = 6
    																	prioritisedBitRate = kBps0 (0)
    																	bucketSizeDuration = ms100 (1)
    																	logicalChannelGroup = 1
    																logicalChannelSR_Mask_r9 = Omit
    																logicalChannelSR_Prohibit_r12 = Omit
    															drb_TypeChange_r12 = Omit
    															rlc_Config_v1250 = Omit
    															rlc_Config_v1310 = Omit
    															drb_TypeLWA_r13 = Omit
    															drb_TypeLWIP_r13 = Omit
    													drb_ToReleaseList = Omit
    													mac_MainConfig
    														explicitValue
    															ul_SCH_Config
    																maxHARQ_Tx = n5 (4)
    																periodicBSR_Timer = sf20 (3)
    																retxBSR_Timer = sf320 (0)
    																ttiBundling = False
    															drx_Config
    																setup
    																	onDurationTimer = psf6 (5)
    																	drx_InactivityTimer = psf1920 (20)
    																	drx_RetransmissionTimer = psf16 (5)
    																	longDRX_CycleStartOffset
    																		sf1280 = 4
    																	shortDRX = Omit
    															timeAlignmentTimerDedicated = sf750 (1)
    															phr_Config
    																setup
    																	periodicPHR_Timer = sf500 (5)
    																	prohibitPHR_Timer = sf200 (5)
    																	dl_PathlossChange = dB3 (1)
    															sr_ProhibitTimer_r9 = Omit
    															mac_MainConfig_v1020 = Omit
    															stag_ToReleaseList_r11 = Omit
    															stag_ToAddModList_r11 = Omit
    															drx_Config_v1130 = Omit
    															e_HARQ_Pattern_r12 = Omit
    															dualConnectivityPHR = Omit
    															logicalChannelSR_Config_r12 = Omit
    															drx_Config_v1310 = Omit
    															extendedPHR2_r13 = Omit
    															eDRX_Config_CycleStartOffset_r13 = Omit
    															drx_Config_r13 = Omit
    													sps_Config = Omit
    													physicalConfigDedicated
    														pdsch_ConfigDedicated = Omit
    														pucch_ConfigDedicated = Omit
    														pusch_ConfigDedicated = Omit
    														uplinkPowerControlDedicated = Omit
    														tpc_PDCCH_ConfigPUCCH
    															setup
    																tpc_RNTI = 0000001111111111'B
    																tpc_Index
    																	indexOfFormat3 = 1
    														tpc_PDCCH_ConfigPUSCH
    															setup
    																tpc_RNTI = 0000000111111010'B
    																tpc_Index
    																	indexOfFormat3 = 1
    														cqi_ReportConfig
    															cqi_ReportModeAperiodic = rm30 (3)
    															nomPDSCH_RS_EPRE_Offset = 0
    															cqi_ReportPeriodic
    																setup
    																	cqi_PUCCH_ResourceIndex = 0
    																	cqi_pmi_ConfigIndex = 25
    																	cqi_FormatIndicatorPeriodic
    																		widebandCQI = Null
    																	ri_ConfigIndex = 483
    																	simultaneousAckNackAndCQI = False
    														soundingRS_UL_ConfigDedicated
    															setup
    																srs_Bandwidth = bw0 (0)
    																srs_HoppingBandwidth = hbw0 (0)
    																freqDomainPosition = 0
    																duration = True
    																srs_ConfigIndex = 20
    																transmissionComb = 0
    																cyclicShift = cs0 (0)
    														antennaInfo
    															defaultValue = Null
    														schedulingRequestConfig = Omit
    														cqi_ReportConfig_v920 = Omit
    														antennaInfo_v920 = Omit
    														antennaInfo_r10 = Omit
    														antennaInfoUL_r10 = Omit
    														cif_Presence_r10 = Omit
    														cqi_ReportConfig_r10 = Omit
    														csi_RS_Config_r10 = Omit
    														pucch_ConfigDedicated_v1020 = Omit
    														pusch_ConfigDedicated_v1020 = Omit
    														schedulingRequestConfig_v1020 = Omit
    														soundingRS_UL_ConfigDedicated_v1020 = Omit
    														soundingRS_UL_ConfigDedicatedAperiodic_r10 = Omit
    														uplinkPowerControlDedicated_v1020 = Omit
    														additionalSpectrumEmissionCA_r10 = Omit
    														csi_RS_ConfigNZPToReleaseList_r11 = Omit
    														csi_RS_ConfigNZPToAddModList_r11 = Omit
    														csi_RS_ConfigZPToReleaseList_r11 = Omit
    														csi_RS_ConfigZPToAddModList_r11 = Omit
    														epdcch_Config_r11 = Omit
    														pdsch_ConfigDedicated_v1130 = Omit
    														cqi_ReportConfig_v1130 = Omit
    														pucch_ConfigDedicated_v1130 = Omit
    														pusch_ConfigDedicated_v1130 = Omit
    														uplinkPowerControlDedicated_v1130 = Omit
    														antennaInfo_v1250 = Omit
    														eimta_MainConfig_r12 = Omit
    														eimta_MainConfigPCell_r12 = Omit
    														pucch_ConfigDedicated_v1250 = Omit
    														cqi_ReportConfigPCell_v1250 = Omit
    														uplinkPowerControlDedicated_v1250 = Omit
    														pusch_ConfigDedicated_v1250 = Omit
    														csi_RS_Config_v1250 = Omit
    														pdsch_ConfigDedicated_v1280 = Omit
    														pdsch_ConfigDedicated_v1310 = Omit
    														pucch_ConfigDedicated_r13 = Omit
    														pusch_ConfigDedicated_r13 = Omit
    														pdcch_CandidateReductions_r13 = Omit
    														cqi_ReportConfig_v1310 = Omit
    														soundingRS_UL_ConfigDedicated_v1310 = Omit
    														soundingRS_UL_ConfigDedicatedUpPTsExt_r13 = Omit
    														soundingRS_UL_ConfigDedicatedAperiodic_v1310 = Omit
    														soundingRS_UL_ConfigDedicatedAperiodicUpPTsExt_r13 = Omit
    														csi_RS_Config_v1310 = Omit
    														ce_Mode_r13 = Omit
    														csi_RS_ConfigNZPToAddModListExt_r13 = Omit
    														csi_RS_ConfigNZPToReleaseListExt_r13 = Omit
    														cqi_ReportConfig_v1320 = Omit
    													rlf_TimersAndConstants_r9 = Omit
    													measSubframePatternPCell_r10 = Omit
    													neighCellsCRS_Info_r11 = Omit
    													naics_Info_r12 = Omit
    													neighCellsCRS_Info_r13 = Omit
    													rlf_TimersAndConstants_r13 = Omit
    												securityConfigHO = Omit
    												nonCriticalExtension = Omit
    				Nas = Omit

    DL-DCCH-Message:
    	rrcConnectionReconfiguration
    		Source = \Protocol\3GPP\LTE\RRC\
    		DL-DCCH-Message
    			message = c1 = rrcConnectionReconfiguration =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = c1 = rrcConnectionReconfiguration-r8 =
    					radioResourceConfigDedicated
    						srb-ToAddModList = SEQUENCE OF SRB-ToAddMod
    							SRB-ToAddMod(1)
    								srb-Identity = 2
    								rlc-Config = defaultValue = NULL
    								logicalChannelConfig = defaultValue = NULL
    						drb-ToAddModList = SEQUENCE OF DRB-ToAddMod
    							DRB-ToAddMod(1)
    								eps-BearerIdentity = 5
    								drb-Identity = 1
    								pdcp-Config
    									discardTimer = infinity
    									rlc-AM
    										statusReportRequired = TRUE
    									headerCompression = notUsed = NULL
    								rlc-Config = am =
    									ul-AM-RLC
    										t-PollRetransmit = ms80
    										pollPDU = p128
    										pollByte = kB125
    										maxRetxThreshold = t4
    									dl-AM-RLC
    										t-Reordering = ms80
    										t-StatusProhibit = ms60
    								logicalChannelIdentity = 3
    								logicalChannelConfig
    									ul-SpecificParameters
    										priority = 6
    										prioritisedBitRate = kBps0
    										bucketSizeDuration = ms100
    										logicalChannelGroup = 1
    						mac-MainConfig = explicitValue =
    							ul-SCH-Config
    								maxHARQ-Tx = n5
    								periodicBSR-Timer = sf20
    								retxBSR-Timer = sf320
    								ttiBundling = FALSE
    							drx-Config = setup =
    								onDurationTimer = psf6
    								drx-InactivityTimer = psf1920
    								drx-RetransmissionTimer = psf16
    								longDRX-CycleStartOffset = sf1280 = 4
    							timeAlignmentTimerDedicated = sf750
    							phr-Config = setup =
    								periodicPHR-Timer = sf500
    								prohibitPHR-Timer = sf200
    								dl-PathlossChange = dB3
    						physicalConfigDedicated
    							tpc-PDCCH-ConfigPUCCH = setup =
    								tpc-RNTI = 0000001111111111
    								tpc-Index = indexOfFormat3 = 1
    							tpc-PDCCH-ConfigPUSCH = setup =
    								tpc-RNTI = 0000000111111010
    								tpc-Index = indexOfFormat3 = 1
    							cqi-ReportConfig
    								cqi-ReportModeAperiodic = rm30
    								nomPDSCH-RS-EPRE-Offset = 0
    								cqi-ReportPeriodic = setup =
    									cqi-PUCCH-ResourceIndex = 0
    									cqi-pmi-ConfigIndex = 25
    									cqi-FormatIndicatorPeriodic = widebandCQI = NULL
    									ri-ConfigIndex = 483
    									simultaneousAckNackAndCQI = FALSE
    							soundingRS-UL-ConfigDedicated = setup =
    								srs-Bandwidth = bw0
    								srs-HoppingBandwidth = hbw0
    								freqDomainPosition = 0
    								duration = TRUE
    								srs-ConfigIndex = 20
    								transmissionComb = 0
    								cyclicShift = cs0
    							antennaInfo = defaultValue = NULL
    ------------------------------------------------------------------------------------------------------------→
    RRC_PDU_REQ:
    ↓	Sent from port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							rrcConnectionReconfiguration
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									c1
    										rrcConnectionReconfiguration_r8
    											measConfig = Omit
    											mobilityControlInfo = Omit
    											dedicatedInfoNASList = Omit
    											radioResourceConfigDedicated
    												srb_ToAddModList
    													SRB_ToAddMod
    														srb_Identity = 2
    														rlc_Config
    															defaultValue = Null
    														logicalChannelConfig
    															defaultValue = Null
    												drb_ToAddModList
    													DRB_ToAddMod
    														eps_BearerIdentity = 5
    														drb_Identity = 1
    														pdcp_Config
    															discardTimer = infinity_ (7)
    															rlc_AM
    																statusReportRequired = True
    															rlc_UM = Omit
    															headerCompression
    																notUsed = Null
    															rn_IntegrityProtection_r10 = Omit
    															pdcp_SN_Size_v1130 = Omit
    															ul_DataSplitDRB_ViaSCG_r12 = Omit
    															t_Reordering_r12 = Omit
    															ul_DataSplitThreshold_r13 = Omit
    															pdcp_SN_Size_v1310 = Omit
    															statusFeedback_r13 = Omit
    														rlc_Config
    															am
    																ul_AM_RLC
    																	t_PollRetransmit = ms80 (15)
    																	pollPDU = p128 (5)
    																	pollByte = kB125 (4)
    																	maxRetxThreshold = t4 (3)
    																dl_AM_RLC
    																	t_Reordering = ms80 (16)
    																	t_StatusProhibit = ms60 (12)
    														logicalChannelIdentity = 3
    														logicalChannelConfig
    															ul_SpecificParameters
    																priority = 6
    																prioritisedBitRate = kBps0 (0)
    																bucketSizeDuration = ms100 (1)
    																logicalChannelGroup = 1
    															logicalChannelSR_Mask_r9 = Omit
    															logicalChannelSR_Prohibit_r12 = Omit
    														drb_TypeChange_r12 = Omit
    														rlc_Config_v1250 = Omit
    														rlc_Config_v1310 = Omit
    														drb_TypeLWA_r13 = Omit
    														drb_TypeLWIP_r13 = Omit
    												drb_ToReleaseList = Omit
    												mac_MainConfig
    													explicitValue
    														ul_SCH_Config
    															maxHARQ_Tx = n5 (4)
    															periodicBSR_Timer = sf20 (3)
    															retxBSR_Timer = sf320 (0)
    															ttiBundling = False
    														drx_Config
    															setup
    																onDurationTimer = psf6 (5)
    																drx_InactivityTimer = psf1920 (20)
    																drx_RetransmissionTimer = psf16 (5)
    																longDRX_CycleStartOffset
    																	sf1280 = 4
    																shortDRX = Omit
    														timeAlignmentTimerDedicated = sf750 (1)
    														phr_Config
    															setup
    																periodicPHR_Timer = sf500 (5)
    																prohibitPHR_Timer = sf200 (5)
    																dl_PathlossChange = dB3 (1)
    														sr_ProhibitTimer_r9 = Omit
    														mac_MainConfig_v1020 = Omit
    														stag_ToReleaseList_r11 = Omit
    														stag_ToAddModList_r11 = Omit
    														drx_Config_v1130 = Omit
    														e_HARQ_Pattern_r12 = Omit
    														dualConnectivityPHR = Omit
    														logicalChannelSR_Config_r12 = Omit
    														drx_Config_v1310 = Omit
    														extendedPHR2_r13 = Omit
    														eDRX_Config_CycleStartOffset_r13 = Omit
    														drx_Config_r13 = Omit
    												sps_Config = Omit
    												physicalConfigDedicated
    													pdsch_ConfigDedicated = Omit
    													pucch_ConfigDedicated = Omit
    													pusch_ConfigDedicated = Omit
    													uplinkPowerControlDedicated = Omit
    													tpc_PDCCH_ConfigPUCCH
    														setup
    															tpc_RNTI = 0000001111111111'B
    															tpc_Index
    																indexOfFormat3 = 1
    													tpc_PDCCH_ConfigPUSCH
    														setup
    															tpc_RNTI = 0000000111111010'B
    															tpc_Index
    																indexOfFormat3 = 1
    													cqi_ReportConfig
    														cqi_ReportModeAperiodic = rm30 (3)
    														nomPDSCH_RS_EPRE_Offset = 0
    														cqi_ReportPeriodic
    															setup
    																cqi_PUCCH_ResourceIndex = 0
    																cqi_pmi_ConfigIndex = 25
    																cqi_FormatIndicatorPeriodic
    																	widebandCQI = Null
    																ri_ConfigIndex = 483
    																simultaneousAckNackAndCQI = False
    													soundingRS_UL_ConfigDedicated
    														setup
    															srs_Bandwidth = bw0 (0)
    															srs_HoppingBandwidth = hbw0 (0)
    															freqDomainPosition = 0
    															duration = True
    															srs_ConfigIndex = 20
    															transmissionComb = 0
    															cyclicShift = cs0 (0)
    													antennaInfo
    														defaultValue = Null
    													schedulingRequestConfig = Omit
    													cqi_ReportConfig_v920 = Omit
    													antennaInfo_v920 = Omit
    													antennaInfo_r10 = Omit
    													antennaInfoUL_r10 = Omit
    													cif_Presence_r10 = Omit
    													cqi_ReportConfig_r10 = Omit
    													csi_RS_Config_r10 = Omit
    													pucch_ConfigDedicated_v1020 = Omit
    													pusch_ConfigDedicated_v1020 = Omit
    													schedulingRequestConfig_v1020 = Omit
    													soundingRS_UL_ConfigDedicated_v1020 = Omit
    													soundingRS_UL_ConfigDedicatedAperiodic_r10 = Omit
    													uplinkPowerControlDedicated_v1020 = Omit
    													additionalSpectrumEmissionCA_r10 = Omit
    													csi_RS_ConfigNZPToReleaseList_r11 = Omit
    													csi_RS_ConfigNZPToAddModList_r11 = Omit
    													csi_RS_ConfigZPToReleaseList_r11 = Omit
    													csi_RS_ConfigZPToAddModList_r11 = Omit
    													epdcch_Config_r11 = Omit
    													pdsch_ConfigDedicated_v1130 = Omit
    													cqi_ReportConfig_v1130 = Omit
    													pucch_ConfigDedicated_v1130 = Omit
    													pusch_ConfigDedicated_v1130 = Omit
    													uplinkPowerControlDedicated_v1130 = Omit
    													antennaInfo_v1250 = Omit
    													eimta_MainConfig_r12 = Omit
    													eimta_MainConfigPCell_r12 = Omit
    													pucch_ConfigDedicated_v1250 = Omit
    													cqi_ReportConfigPCell_v1250 = Omit
    													uplinkPowerControlDedicated_v1250 = Omit
    													pusch_ConfigDedicated_v1250 = Omit
    													csi_RS_Config_v1250 = Omit
    													pdsch_ConfigDedicated_v1280 = Omit
    													pdsch_ConfigDedicated_v1310 = Omit
    													pucch_ConfigDedicated_r13 = Omit
    													pusch_ConfigDedicated_r13 = Omit
    													pdcch_CandidateReductions_r13 = Omit
    													cqi_ReportConfig_v1310 = Omit
    													soundingRS_UL_ConfigDedicated_v1310 = Omit
    													soundingRS_UL_ConfigDedicatedUpPTsExt_r13 = Omit
    													soundingRS_UL_ConfigDedicatedAperiodic_v1310 = Omit
    													soundingRS_UL_ConfigDedicatedAperiodicUpPTsExt_r13 = Omit
    													csi_RS_Config_v1310 = Omit
    													ce_Mode_r13 = Omit
    													csi_RS_ConfigNZPToAddModListExt_r13 = Omit
    													csi_RS_ConfigNZPToReleaseListExt_r13 = Omit
    													cqi_ReportConfig_v1320 = Omit
    												rlf_TimersAndConstants_r9 = Omit
    												measSubframePatternPCell_r10 = Omit
    												neighCellsCRS_Info_r11 = Omit
    												naics_Info_r12 = Omit
    												neighCellsCRS_Info_r13 = Omit
    												rlf_TimersAndConstants_r13 = Omit
    											securityConfigHO = Omit
    											nonCriticalExtension = Omit

    UL-DCCH-Message:
    	rrcConnectionReconfigurationComplete
    		Source = \Protocol\3GPP\LTE\RRC\
    		UL-DCCH-Message
    			message = c1 = rrcConnectionReconfigurationComplete =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = rrcConnectionReconfigurationComplete-r8 =
    ←------------------------------------------------------------------------------------------------------------
    RRC_PDU_IND:
    ↑	Received on port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 298
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							rrcConnectionReconfigurationComplete
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									rrcConnectionReconfigurationComplete_r8
    										nonCriticalExtension = Omit

    SRB_COMMON_IND:
    ↑	Inter-component message: SRB -> EUTRA_PTC:SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 298
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Dcch
    						message_
    							c1
    								rrcConnectionReconfigurationComplete
    									rrc_TransactionIdentifier = 0
    									criticalExtensions
    										rrcConnectionReconfigurationComplete_r8
    											nonCriticalExtension = Omit
    				Nas = Omit

    Verdict Intermediate Pass:
    	Intermediate verdict: (PASS)
    	TTCN-3 message: Step 14-24
    		Source = \Test Control\TTCN3
    		IntermediateVerdict = (Pass)
    		summary = Intermediate verdict: (PASS)
    		TTCN-3 message: Step 14-24

    IP_ConfigReq_Type:
    ↓	Inter-component message: EUTRA_CTRL -> IP_PTC:EUTRA_CTRL
    		Source = \Test Control\TTCN3
    		IP_ConfigReq_Type
    			ChangeDrbInfo
    				PdnId = PDN_1 (0)
    				DrbInfo
    					Eutra
    						CellId = eutra_CellA (16)
    						DrbId = 1

    DRBMUX_CONFIG_REQ:
    ↓	Sent from port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_CONFIG_REQ
    			RoutingInfo
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 67
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 53
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = icmpv6 (3)
    						Local
    							IpAddr
    								V6
    									Addr = 'FE80:0000:0000:0000:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = Omit
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = udp (0)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V4
    									Addr = '192.168.198.55'
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit
    				IP_RoutingInfo_Type
    					IpInfo
    						Protocol = tcp (1)
    						Local
    							IpAddr
    								V6
    									Addr = 'fd29:cc43:7fb9:0002:020c:29ff:fe66:b4c7'
    									ScopeId = Omit
    							Port = 5060
    						Remote = Omit
    					DRB
    						Eutra
    							CellId = eutra_CellA (16)
    							DrbId = 1
    					DataMode = Omit

    DRBMUX_COMMON_IND_CNF:
    ↑	Received on port: IP_PTC:IP_CTRL
    		Source = \Test Control\TTCN3
    		DRBMUX_COMMON_IND_CNF
    			Confirm = True

    IP_Indication_Type:
    ↑	Inter-component message: IP -> EUTRA_PTC:IP
    		Source = \Test Control\TTCN3
    		IP_Indication_Type
    			Cnf = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: Ut_CnfReq_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: Ut_CnfReq_Type
    		MATCH_MISMATCH
    			Message Mismatch: Ut_CnfReq_Type
    				Ut_CnfReq_Type = CNF_REQUIRED (1)

    MATCH_MISMATCH:
    ↑	Message Mismatch: Ut_CnfReq_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: Ut_CnfReq_Type
    		MATCH_MISMATCH
    			Message Mismatch: Ut_CnfReq_Type
    				Ut_CnfReq_Type = LOCAL_CNF_REQUIRED (2)

    MATCH_MISMATCH:
    ↑	Message Mismatch: BitStringType
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: BitStringType
    		MATCH_MISMATCH
    			Message Mismatch: BitStringType = 111'B
    				BitStringType =

    UT_COMMON_CMD:
    ↓	Inter-component message: PTC_Ut -> MTC_LTE:PTC_Ut
    		Source = \Test Control\TTCN3
    		UT_COMMON_CMD
    			Cmd = SWITCH_OFF (99)
    			CnfReq = NO_CNF_REQUIRED (0)
    			ParameterList = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: Ut_CnfReq_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: Ut_CnfReq_Type
    		MATCH_MISMATCH
    			Message Mismatch: Ut_CnfReq_Type
    				Ut_CnfReq_Type = CNF_REQUIRED (1)

    MATCH_MISMATCH:
    ↑	Message Mismatch: Ut_CnfReq_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: Ut_CnfReq_Type
    		MATCH_MISMATCH
    			Message Mismatch: Ut_CnfReq_Type
    				Ut_CnfReq_Type = LOCAL_CNF_REQUIRED (2)

    UT_SYSTEM_REQ:
    ↓	Sent from port: MTC_LTE:Ut
    		Source = \Test Control\TTCN3
    		UT_SYSTEM_REQ
    			Cmd
    				MMI
    					Cmd = 'SWITCH_OFF'
    					ParameterList = Omit
    			CnfRequired = NO_CNF_REQUIRED (0)

    UL-DCCH-Message:
    	ulInformationTransfer
    		Source = \Protocol\3GPP\LTE\RRC\
    		UL-DCCH-Message
    			message = c1 = ulInformationTransfer =
    				criticalExtensions = c1 = ulInformationTransfer-r8 =
    					dedicatedInfoType = dedicatedInfoNAS = 27D4414B1903B3EB0E55FE42B103BD564DFA2D9F2A
    ←------------------------------------------------------------------------------------------------------------
    Security Protected NAS Message UL:
    	Security Protected NAS Message UL PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Security Protected NAS Message
    			Security header type [4 bits] = 0x2 [ 2 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			MAC = 0x54414B19 [ 1413565209 ]
    			Sequence Number = 0x03 [ 3 ]
    			NAS message = 0x336B0E557E4231033D564D7A2D1F2A
    ←------------------------------------------------------------------------------------------------------------
    Ciphered NAS Message UL:
    	Ciphered NAS Message UL PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Ciphered NAS Message =
    			0x336B0E557E4231033D564D7A2D1F2A
    ←------------------------------------------------------------------------------------------------------------
    RRC_PDU_IND:
    ↑	Received on port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 2
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 896
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							ulInformationTransfer
    								criticalExtensions
    									c1
    										ulInformationTransfer_r8
    											dedicatedInfoType
    												dedicatedInfoNAS = '27D4414B1903B3EB0E55FE42B103BD564DFA2D9F2A'O
    											nonCriticalExtension = Omit

    Detach Request UE Terminated:
    	Detach Request UE Terminated PDU
    		Source = \Protocol\CommonLteEpcEncoders
    		Detach Request UE Terminated
    			Security header type [4 bits] = 0x0 [ 0 ]
    			Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    			Message Type [8 bits] = 0x45 - Detach Request UE Terminated [ 69 ]
    			Spare Half Octet [4 bits] = 0x1 [ 1 ]
    			Detach Type
    				switch off [1 bit] = 0x1 - switch off [ 1 ]
    				EPS Detach type [3 bits] = 0x1 - Re-attach Required [ 1 ]
    ------------------------------------------------------------------------------------------------------------→
    SRB_COMMON_IND:
    ↑	Inter-component message: SRB -> EUTRA_PTC:SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_IND
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 2
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 896
    						Subframe
    							Number = 3
    						HSFN
    							Number = 0
    				Status
    					Ok = True
    				CA_Info = Omit
    			Signalling
    				Rrc = Omit
    				Nas
    					NasIndication
    						SecurityProtection
    							Status = 0010'B
    							NasCount = '00000003'O
    						Pdu
    							Msg
    								dETACH_REQUEST_MO
    									securityHeaderType = 0000'B
    									protocolDiscriminator = 0111'B
    									messageType = 01000101'B
    									asmeNasKeySetId
    										iei = Omit
    										tsc = 0'B
    										nasKeySetId = 001'B
    									detachType
    										switchOff = 1'B
    										typeOfDetach = 001'B
    									epsMobileIdentity
    										iei = Omit
    										iel = '0B'O
    										idDigit1 = 1111'B
    										oddEvenInd = 0'B
    										typeOfId = 110'B
    										otherDigits = '00F110800101C2345678'O
    							PiggybackedPduList = Omit

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = True
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				EnquireTiming = True

    SYSTEM_CTRL_CNF:
    ↑	Received on port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_CNF
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 897
    						Subframe
    							Number = 8
    						HSFN
    							Number = 0
    				Result
    					Success = True
    			Confirm
    				EnquireTiming = True

    Timer Event:
    	Timer: t_Timer, Duration: 1.22s, Started: 17:36:25
    		Source = \Test Control\TTCN3
    		timerEvent = 6
    		fileName = C:\CT_LTE\ETSI\v41_Dev\RC1\Final PSM MKS\LTE_A_R12_IWD_16wk37\Common\EUTRA\EUTRA_RRCSteps.ttcn
    		testName = TC_9_2_1_1_7c
    		lineNo = 1418
    		outStr = Timer: t_Timer, Duration: 1.22s, Started: 17:36:25

    SRB_COMMON_REQ:
    ↓	Inter-component message: TC_SRB -> NASEMU_LTE_PTC:TC_SRB
    		Source = \Test Control\TTCN3
    		SRB_COMMON_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 928
    						Subframe
    							Number = 4
    						HSFN
    							Number = 0
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Signalling
    				Rrc
    					Dcch
    						message_
    							c1
    								rrcConnectionRelease
    									rrc_TransactionIdentifier = 0
    									criticalExtensions
    										c1
    											rrcConnectionRelease_r8
    												releaseCause = other (1)
    												redirectedCarrierInfo = Omit
    												idleModeMobilityControlInfo = Omit
    												nonCriticalExtension = Omit
    				Nas = Omit

    DL-DCCH-Message:
    	rrcConnectionRelease
    		Source = \Protocol\3GPP\LTE\RRC\
    		DL-DCCH-Message
    			message = c1 = rrcConnectionRelease =
    				rrc-TransactionIdentifier = 0
    				criticalExtensions = c1 = rrcConnectionRelease-r8 =
    					releaseCause = other
    ------------------------------------------------------------------------------------------------------------→
    RRC_PDU_REQ:
    ↓	Sent from port: NASEMU_LTE_PTC:SYS_SRB
    		Source = \Test Control\TTCN3
    		RRC_PDU_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					RadioBearerId
    						Srb = 1
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 928
    						Subframe
    							Number = 4
    						HSFN
    							Number = 0
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			RrcPdu
    				Dcch
    					message_
    						c1
    							rrcConnectionRelease
    								rrc_TransactionIdentifier = 0
    								criticalExtensions
    									c1
    										rrcConnectionRelease_r8
    											releaseCause = other (1)
    											redirectedCarrierInfo = Omit
    											idleModeMobilityControlInfo = Omit
    											nonCriticalExtension = Omit

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = True
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				PdcpCount
    					Get
    						AllRBs = True

    SYSTEM_CTRL_CNF:
    ↑	Received on port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_CNF
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				Result
    					Success = True
    			Confirm
    				PdcpCount
    					Get
    						PdcpCountInfo_Type
    							RadioBearerId
    								Srb = 1
    							UL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000011'B
    							DL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000011'B
    						PdcpCountInfo_Type
    							RadioBearerId
    								Srb = 2
    							UL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000001'B
    							DL
    								Format = PdcpCount_Srb (0)
    								Value = 00000000000000000000000000000000'B
    						PdcpCountInfo_Type
    							RadioBearerId
    								Drb = 1
    							UL
    								Format = PdcpCount_DrbShortSQN (2)
    								Value = 00000000000000000000000000000000'B
    							DL
    								Format = PdcpCount_DrbShortSQN (2)
    								Value = 00000000000000000000000000000000'B

    MATCH_MISMATCH:
    ↑	Message Mismatch: TimingInfo_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: TimingInfo_Type
    		MATCH_MISMATCH
    			Message Mismatch: TimingInfo_Type
    				SubFrame
    					SFN
    						Number = 928
    					Subframe
    						Number = 4
    					HSFN
    						Number = 0

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 928
    						Subframe
    							Number = 4
    						HSFN
    							Number = 0
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				Cell
    					AddOrReconfigure
    						Basic = Omit
    						Active
    							C_RNTI = Omit
    							PhysicalLayerConfigUL = Omit
    							RachProcedureConfig = Omit
    							CcchDcchDtchConfig
    								MeasGapCtrl = Omit
    								DL = Omit
    								UL
    									DciInfo = Omit
    									Hopping
    										Deactivated = True
    									PUCCH_Synch
    										None = True
    									UL_GrantConfig
    										None = True
    								DrxCtrl = Omit
    								TtiBundling = Omit
    								CifPresence = Omit
    							ServingCellConfig = Omit
    							SciSchedulingConfig = Omit
    							EIMTA_Config = Omit
    							CE_Mode = Omit

    MATCH_MISMATCH:
    ↑	Message Mismatch: TimingInfo_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: TimingInfo_Type
    		MATCH_MISMATCH
    			Message Mismatch: TimingInfo_Type
    				SubFrame
    					SFN
    						Number = 928
    					Subframe
    						Number = 9
    					HSFN
    						Number = 0

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 928
    						Subframe
    							Number = 9
    						HSFN
    							Number = 0
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				AS_Security
    					Release = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: TimingInfo_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: TimingInfo_Type
    		MATCH_MISMATCH
    			Message Mismatch: TimingInfo_Type
    				SubFrame
    					SFN
    						Number = 933
    					Subframe
    						Number = 9
    					HSFN
    						Number = 0

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 933
    						Subframe
    							Number = 9
    						HSFN
    							Number = 0
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				RadioBearerList
    					RadioBearer_Type
    						Id
    							Srb = 1
    						Config
    							Release = True
    					RadioBearer_Type
    						Id
    							Srb = 2
    						Config
    							Release = True
    					RadioBearer_Type
    						Id
    							Drb = 1
    						Config
    							Release = True

    MATCH_MISMATCH:
    ↑	Message Mismatch: TimingInfo_Type
    		Source = \Test Control\TTCN3
    		summary = Message Mismatch: TimingInfo_Type
    		MATCH_MISMATCH
    			Message Mismatch: TimingInfo_Type
    				SubFrame
    					SFN
    						Number = 934
    					Subframe
    						Number = 4
    					HSFN
    						Number = 0

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_CellA (16)
    				RoutingInfo
    					None = True
    				TimingInfo
    					SubFrame
    						SFN
    							Number = 934
    						Subframe
    							Number = 4
    						HSFN
    							Number = 0
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				RadioBearerList
    					RadioBearer_Type
    						Id
    							Srb = 1
    						Config
    							AddOrReconfigure
    								Pdcp
    									Config
    										Rb
    											Srb = True
    										TestMode
    											None = True
    								Rlc
    									Rb
    										AM
    											Tx
    												R8
    													t_PollRetransmit = ms45 (8)
    													pollPDU = pInfinity (7)
    													pollByte = kBinfinity (14)
    													maxRetxThreshold = t4 (3)
    											Rx
    												R8
    													t_Reordering = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    											ExtendedLI = Omit
    									TestMode
    										None = True
    								LogicalChannelId = 1
    								Mac
    									LogicalChannel
    										Priority = 1
    										PrioritizedBitRate = infinity_ (7)
    									TestMode
    										None = True
    								DiscardULData = Omit
    					RadioBearer_Type
    						Id
    							Srb = 2
    						Config
    							AddOrReconfigure
    								Pdcp
    									Config
    										Rb
    											Srb = True
    										TestMode
    											None = True
    								Rlc
    									Rb
    										AM
    											Tx
    												R8
    													t_PollRetransmit = ms45 (8)
    													pollPDU = pInfinity (7)
    													pollByte = kBinfinity (14)
    													maxRetxThreshold = t4 (3)
    											Rx
    												R8
    													t_Reordering = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    											ExtendedLI = Omit
    									TestMode
    										None = True
    								LogicalChannelId = 2
    								Mac
    									LogicalChannel
    										Priority = 3
    										PrioritizedBitRate = infinity_ (7)
    									TestMode
    										None = True
    								DiscardULData = Omit

    Timer Event:
    	Timer: t_Timer, Expired: 17:36:26
    		Source = \Test Control\TTCN3
    		timerEvent = 9
    		fileName = C:\CT_LTE\ETSI\v41_Dev\RC1\Final PSM MKS\LTE_A_R12_IWD_16wk37\Common\EUTRA\EUTRA_RRCSteps.ttcn
    		testName = TC_9_2_1_1_7c
    		lineNo = 1427
    		outStr = Timer: t_Timer, Expired: 17:36:26

    SYSTEM_CTRL_REQ:
    ↓	Sent from port: EUTRA_PTC:SYS
    		Source = \Test Control\TTCN3
    		SYSTEM_CTRL_REQ
    			Common
    				CellId = eutra_Cell_NonSpecific (0)
    				RoutingInfo
    					None = True
    				TimingInfo
    					Now = True
    				ControlInfo
    					CnfFlag = False
    					FollowOnFlag = False
    				CA_Info = Omit
    			Request
    				Cell
    					Release = True

    TTCN Test Step:
    	Postamble
    		Source = \Test Control\TTCN3
    		recordType = 24
    		summary = Postamble

    Verdict Intermediate Pass:
    	Intermediate verdict: (PASS)
    		Source = \Test Control\TTCN3
    		IntermediateVerdict = (Pass)
    		summary = Intermediate verdict: (PASS)

    Verdict Intermediate Pass:
    	Intermediate verdict: (PASS)
    		Source = \Test Control\TTCN3
    		IntermediateVerdict = (Pass)
    		summary = Intermediate verdict: (PASS)

    Verdict Pass:
    	Test case ended: TC_9_2_1_1_7c, Verdict: PASS
    		Source = \Test Control\TTCN3
    		verdict = PASS
    		summary = Test case ended: TC_9_2_1_1_7c, Verdict: PASS

    TTCN Test Step:
    	Final Verdict
    		Source = \Test Control\TTCN3
    		recordType = 24
    		summary = Final Verdict

    Verdict Pass:
    	TEST CASE ENDED: TC_9_2_1_1_7c
    		Source = \Test Control\TTCN3
    		verdict = PASS
    		summary = TEST CASE ENDED: TC_9_2_1_1_7c

    Verdict Intermediate None:
    	Intermediate verdict: (NONE)
    		Source = \Test Control\TTCN3
    		IntermediateVerdict = (None)
    		summary = Intermediate verdict: (NONE)

    Verdict Intermediate None:
    	Intermediate verdict: (NONE)
    		Source = \Test Control\TTCN3
    		IntermediateVerdict = (None)
    		summary = Intermediate verdict: (NONE)

    Verdict Intermediate None:
    	Intermediate verdict: (NONE)
    		Source = \Test Control\TTCN3
    		IntermediateVerdict = (None)
    		summary = Intermediate verdict: (NONE)

    Verdict Intermediate None:
    	Intermediate verdict: (NONE)
    		Source = \Test Control\TTCN3
    		IntermediateVerdict = (None)
    		summary = Intermediate verdict: (NONE)