#######################################################################

# Anritsu Generated PICS/PIXIT file

#

# Changes Applied: 3GPP_TS_34.123-3_AND_E2265_AND_TestSequence-2076702433_AND_E2265_AND_TestSequence-2076702433

#######################################################################

pc_1xCSfallback,                             BOOLEAN,       false   #-- @desc  Support of 1xCS fallback

pc_1xRTT,                                    BOOLEAN,       false   #-- @desc  UE supports CDMA2000 1xRTT band class

pc_4Layer_spatial_mux_tm3_tm4,               BOOLEAN,       false   #-- @desc  Support of 4 layer spatial multiplexing with transmission mode 3 and transmission mode 4

pc_5GCN,                                     BOOLEAN,       false   #-- @desc  UE supports 5GS Core

pc_A5_4_CS,                                  BOOLEAN,       false   #-- @desc  Support of A54

pc_APN_RateControl,                          BOOLEAN,       false   #-- @desc  The UE supports APN rate control

pc_Allowed_CSG_list,                         BOOLEAN,       false   #-- @desc  Support of Allowed CSG list

pc_Attach,                                   BOOLEAN,       false   #-- @desc  Support EPS attach (with or without pre-configuration)

pc_AttachWithIMSI,                           BOOLEAN,       TRUE    #-- @desc  Support of Attach With IMSI

pc_AttachWithPDN,                            BOOLEAN,       TRUE    #-- @desc  Support of EMM-REGISTERED with PDN

pc_AttachWithoutPDN,                         BOOLEAN,       false   #-- @desc  Support of EMM-REGISTERED without PDN

pc_Auto_Attach_after_TAU_Reject,             BOOLEAN,       false   #-- @desc  Support of automatic re-activation of the EPS bearer(s) after the TAU Reject

pc_Auto_PDN_Connectivity,                    BOOLEAN,       TRUE    #-- @desc  Support of automatic PDN Connectivity in EUTRAN

pc_Automatic_EPS_Re_Attach,                  BOOLEAN,       TRUE    #-- @desc  Support of automatic re-activation of the EPS bearer(s)

pc_Automatic_Re_Attach,                      BOOLEAN,       TRUE    #-- @desc  Support of automatic re-activation of the EPS bearer(s) during Network Initiated Detach with detach type set to re-attach required

pc_Available_PLMNs_AcT_Ind,                  BOOLEAN,       false   #-- @desc  Support of AccessTechnology indication in available PLMNs list

pc_B41_UE_PC2,                               BOOLEAN,       false   #-- @desc  Support of TDD Band 41 Power class 2 operation

pc_BSRVCC,                                   BOOLEAN,       false   #-- @desc  UE indicates g.3gpp.ps2cs-srvcc-orig-pre-alerting media feature tag in INVITE request

pc_BidirecVoiceOverIMS,                      BOOLEAN,       TRUE    #-- @desc  UE capable of initiating a bidirectional voice session over IMS

pc_CEmodeA,                                  BOOLEAN,       false   #-- @desc  Support of CE mode A

pc_CEmodeB,                                  BOOLEAN,       false   #-- @desc  Support of CE mode B

pc_CMAS_Message,                             BOOLEAN,       TRUE    #-- @desc  Support of CMAS message

pc_CRS_Interference_Handling,                BOOLEAN,       false   #-- @desc  Support of CRS interference handling

pc_CS,                                       BOOLEAN,       false   #-- @desc  UE supports CS domain services

pc_CSI_RS_DS_Meas,                           BOOLEAN,       TRUE    #-- @desc  Support of CSI-RS based discovery signals measurement

pc_CS_Em_Call_in_1xRTT,                      BOOLEAN,       false   #-- @desc  Support for establishing the emergency call using the CS domain in 1xRTT

pc_CS_Em_Call_in_GERAN,                      BOOLEAN,       TRUE    #-- @desc  Support for establishing the emergency call using the CS domain in GERAN

pc_CS_Em_Call_in_UTRA,                       BOOLEAN,       TRUE    #-- @desc  Support for establishing the emergency call using the CS domain in UTRA

pc_CS_Fallback,                              BOOLEAN,       TRUE    #-- @desc  The UE supports CS fallback for voice calls. If true pc_CS and at least one of pc_FDD pc_TDD_HCR pc_TDD_LCR pc_TDD_VHCR or pc_UMTS_GSM is also true.

pc_CS_PS_data_centric,                       BOOLEAN,       false   #-- @desc  Support of CSPS mode 2

pc_CS_PS_voice_centric,                      BOOLEAN,       TRUE    #-- @desc  Support of configuring the UE to voice centric

pc_Category_M1_voice,                        BOOLEAN,       false   #-- @desc  Support for GSMA PRD NG.108 "IMS Profile for Voice and SMS for UE Category M1"

pc_Combined_Attach,                          BOOLEAN,       TRUE    #-- @desc  Support combined EPSIMSI attach (with or without pre-configuration)

pc_CommunicationHold_DuringEmergencyCall,    BOOLEAN,       false   #-- @desc  UE supports Communication Hold during emergency call

pc_Control_Plane_CIoT_Optimisation,          BOOLEAN,       false   #-- @desc  Support of Control Plane CIoT

pc_DC_SCG_DRB,                               BOOLEAN,       TRUE    #-- @desc  Support of DC SCG DRB

pc_DC_Split_DRB,                             BOOLEAN,       false   #-- @desc  Support of DC Split DRB

pc_DL_256QAM,                                BOOLEAN,       false   #-- @desc  Support of downlink 256 QAM

pc_DL_CA_2Carriers,                          BOOLEAN,       false   #-- @desc  DL CA with 2 carriers

pc_DL_CA_3Carriers,                          BOOLEAN,       false   #-- @desc  DL CA with 3 carriers

pc_DL_interBand_CaBwClassComb_AA,            BOOLEAN,       TRUE    #-- @desc  DL Inter-band contiguous CA BW class A-A

pc_DL_intraBand_ContCaBWclassB,              BOOLEAN,       TRUE    #-- @desc  DL Intra-band contiguous CA BW class B

pc_DL_intraBand_ContCaBWclassC,              BOOLEAN,       TRUE    #-- @desc  DL Intra-band contiguous CA BW class C

pc_DL_intraBand_nonContCaBwClassComb_AA,     BOOLEAN,       TRUE    #-- @desc  Support of DL intra-band non-contiguous CA BW Class Combination A-A

pc_DSMIPv6,                                  BOOLEAN,       false   #-- @desc  Support of Mobility management based on Dual-Stack Mobile IPv6

pc_DaylightSavingTime,                       BOOLEAN,       false   #-- @desc  UE storesupdates the daylight saving time when receives information

pc_DualRM_Coding,                            BOOLEAN,       false   #-- @desc  Dual RM Coding

pc_EAB,                                      BOOLEAN,       false   #-- @desc  Support of Extended Access Barring

pc_EAB_override,                             BOOLEAN,       false   #-- @desc  Support of Extended Access Barring Override

pc_EDTM,                                     BOOLEAN,       false   #-- @desc  Support for EDTM

pc_EMM_Information,                          BOOLEAN,       false   #-- @desc  Support of EMM Information message

pc_EN_DC,                                    BOOLEAN,       TRUE    #-- @desc  EN-DC (Option 3)

pc_EPS_Services_Disable,                     BOOLEAN,       false   #-- @desc  Support of disabling of EPS services

pc_ESM_MO_Bearer_Allocation,                 BOOLEAN,       TRUE    #-- @desc  Support of ESM UE requested bearer resource allocation procedure

pc_ESM_MO_Bearer_Modification,               BOOLEAN,       TRUE    #-- @desc  Support of ESM UE requested bearer resource modification procedure

pc_ESM_Notification,                         BOOLEAN,       TRUE    #-- @desc  Support of ESM Notification procedure

pc_ESM_UE_Modification_NW_TFT,               BOOLEAN,       TRUE    #-- @desc  Support for UE requested modification of network allocated TFTs

pc_ETWS_message,                             BOOLEAN,       TRUE    #-- @desc  Support of ETWS message

pc_E_UTRAN_2_GERAN_PSHO,                     BOOLEAN,       false   #-- @desc  Support for inter-RAT PS handover from E_UTRAN to GERAN

pc_E_UTRA_WLAN_offload,                      BOOLEAN,       false   #-- @desc  Support Offload tofrom WLAN and supports S2b

pc_EarlyMedia,                               BOOLEAN,       false   #-- @desc  UE supports early media

pc_EmergSpeech,                              BOOLEAN,       TRUE    #-- @desc  Emergency Call

pc_Enhanced_1xCSfallback,                    BOOLEAN,       false   #-- @desc  Support of Enhanced 1xCS fallback

pc_FDD,                                      BOOLEAN,       TRUE    #-- @desc  UE supports UTRA band as defined in TS 25.101

pc_FDD_TypeB_HalfDuplex,                     BOOLEAN,       false   #-- @desc  Support of Type B Half duplex FDD operation

pc_Fast_First_HPPLMN_Search,                 BOOLEAN,       false   #-- @desc  Support of Fast First Higher Piority PLMN search

pc_FeatrGrp_101_F,                           BOOLEAN,       TRUE    #-- @desc  DMRS with OCC (orthogonal cover code) and SGH (sequence group hopping) disabling

pc_FeatrGrp_101_T,                           BOOLEAN,       TRUE    #-- @desc  DMRS with OCC (orthogonal cover code) and SGH (sequence group hopping) disabling

pc_FeatrGrp_102_F,                           BOOLEAN,       TRUE    #-- @desc  Trigger type 1 SRS (aperiodic SRS) transmission (Up to X ports)

pc_FeatrGrp_102_T,                           BOOLEAN,       TRUE    #-- @desc  Trigger type 1 SRS (aperiodic SRS) transmission (Up to X ports)

pc_FeatrGrp_103_F,                           BOOLEAN,       false   #-- @desc  PDSCH transmission mode 9 when up to 4 CSI reference signal ports are configured

pc_FeatrGrp_103_T,                           BOOLEAN,       false   #-- @desc  PDSCH transmission mode 9 when up to 4 CSI reference signal ports are configured

pc_FeatrGrp_104_F,                           BOOLEAN,       false   #-- @desc  PDSCH transmission mode 9 for TDD when 8 CSI reference signal ports are configured

pc_FeatrGrp_104_T,                           BOOLEAN,       false   #-- @desc  PDSCH transmission mode 9 for TDD when 8 CSI reference signal ports are configured

pc_FeatrGrp_105_F,                           BOOLEAN,       false   #-- @desc  Periodic CQIPMIRI reporting on PUCCH: Mode 2-0:UE selected subband CQI without PMI when PDSCH transmission mode 9 is configured.Periodic CQIPMIRI reporting on PUCCH: Mode 2-1:UE selected subband CQI with single PMI when PDSCH transmission mode 9 and up to 4 CSI reference signal ports are configured

pc_FeatrGrp_105_T,                           BOOLEAN,       false   #-- @desc  Periodic CQIPMIRI reporting on PUCCH: Mode 2-0:UE selected subband CQI without PMI when PDSCH transmission mode 9 is configured.Periodic CQIPMIRI reporting on PUCCH: Mode 2-1:UE selected subband CQI with single PMI when PDSCH transmission mode 9 and up to 4 CSI reference signal ports are configured

pc_FeatrGrp_106_F,                           BOOLEAN,       false   #-- @desc  Periodic CQIPMIRIPTI reporting on PUCCH: Mode 2-1: UE selected subband CQI with single PMI when PDSCH transmission mode 9 and 8 CSI reference signal ports are configured

pc_FeatrGrp_106_T,                           BOOLEAN,       false   #-- @desc  Periodic CQIPMIRIPTI reporting on PUCCH: Mode 2-1: UE selected subband CQI with single PMI when PDSCH transmission mode 9 and 8 CSI reference signal ports are configured

pc_FeatrGrp_107_F,                           BOOLEAN,       false   #-- @desc  Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-0: UE selected subband CQI without PMI when PDSCH transmission mode 9 is configured. Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2: UE selected subband CQI with multiple PMI when PDSCH transmission mode 9 and up to 4 CSI reference signal ports are configured

pc_FeatrGrp_107_T,                           BOOLEAN,       false   #-- @desc  Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-0: UE selected subband CQI without PMI when PDSCH transmission mode 9 is configured. Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2: UE selected subband CQI with multiple PMI when PDSCH transmission mode 9 and up to 4 CSI reference signal ports are configured

pc_FeatrGrp_108_F,                           BOOLEAN,       false   #-- @desc  Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2: UE selected subband CQI with multiple PMI when PDSCH transmission mode 9 and 8 CSI reference signal ports are configured

pc_FeatrGrp_108_T,                           BOOLEAN,       false   #-- @desc  Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2: UE selected subband CQI with multiple PMI when PDSCH transmission mode 9 and 8 CSI reference signal ports are configured

pc_FeatrGrp_109_F,                           BOOLEAN,       false   #-- @desc  Periodic CQIPMIRI reporting on PUCCH Mode 1-1 submode 1

pc_FeatrGrp_109_T,                           BOOLEAN,       false   #-- @desc  Periodic CQIPMIRI reporting on PUCCH Mode 1-1 submode 1

pc_FeatrGrp_10_F,                            BOOLEAN,       TRUE    #-- @desc  Support of EUTRA RRC_CONNECTED to GERAN (Packet_)Idle by Cell Change Order EUTRA RRC_CONNECTED to GERAN (Packet_)Idle by Cell Change Order with NACC (Network Assisted Cell Change)

pc_FeatrGrp_10_T,                            BOOLEAN,       TRUE    #-- @desc  Support of EUTRA RRC_CONNECTED to GERAN (Packet_)Idle by Cell Change Order EUTRA RRC_CONNECTED to GERAN (Packet_)Idle by Cell Change Order with NACC (Network Assisted Cell Change)

pc_FeatrGrp_110_F,                           BOOLEAN,       false   #-- @desc  Periodic CQIPMIRI reporting on PUCCH Mode 1-1 submode 2

pc_FeatrGrp_110_T,                           BOOLEAN,       false   #-- @desc  Periodic CQIPMIRI reporting on PUCCH Mode 1-1 submode 2

pc_FeatrGrp_111_F,                           BOOLEAN,       TRUE    #-- @desc  Measurement reporting trigger Event A6

pc_FeatrGrp_111_T,                           BOOLEAN,       TRUE    #-- @desc  Measurement reporting trigger Event A6

pc_FeatrGrp_112_F,                           BOOLEAN,       TRUE    #-- @desc  SCell addition within the Handover to EUTRA procedure

pc_FeatrGrp_112_T,                           BOOLEAN,       TRUE    #-- @desc  SCell addition within the Handover to EUTRA procedure

pc_FeatrGrp_113_F,                           BOOLEAN,       false   #-- @desc  Trigger type 0 SRS (periodic SRS) transmission on X Serving Cells

pc_FeatrGrp_113_T,                           BOOLEAN,       false   #-- @desc  Trigger type 0 SRS (periodic SRS) transmission on X Serving Cells

pc_FeatrGrp_114_F,                           BOOLEAN,       TRUE    #-- @desc  Reporting of both UTRA CPICH RSCP and EcN0 in a Measurement Report

pc_FeatrGrp_114_T,                           BOOLEAN,       TRUE    #-- @desc  Reporting of both UTRA CPICH RSCP and EcN0 in a Measurement Report

pc_FeatrGrp_115_F,                           BOOLEAN,       false   #-- @desc  time domain ICIC RLMRRM measurement subframe restriction for the serving cell. time domain ICIC RRM measurement subframe restriction for neighbour cells. time domain ICIC CSI measurement subframe restriction

pc_FeatrGrp_115_T,                           BOOLEAN,       false   #-- @desc  time domain ICIC RLMRRM measurement subframe restriction for the serving cell. time domain ICIC RRM measurement subframe restriction for neighbour cells. time domain ICIC CSI measurement subframe restriction

pc_FeatrGrp_116_F,                           BOOLEAN,       false   #-- @desc  Relative transmit phase continuity for spatial multiplexing in UL

pc_FeatrGrp_116_T,                           BOOLEAN,       false   #-- @desc  Relative transmit phase continuity for spatial multiplexing in UL

pc_FeatrGrp_11_F,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to 1xRTT CS Active handover

pc_FeatrGrp_11_T,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to 1xRTT CS Active handover

pc_FeatrGrp_12_F,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to HRPD Active handover

pc_FeatrGrp_12_T,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to HRPD Active handover

pc_FeatrGrp_13_F,                            BOOLEAN,       TRUE    #-- @desc  Support of Inter-frequency handover (within FDD or TDD)

pc_FeatrGrp_13_T,                            BOOLEAN,       TRUE    #-- @desc  Support of Inter-frequency handover (within FDD or TDD)

pc_FeatrGrp_14_F,                            BOOLEAN,       TRUE    #-- @desc  Support of Measurement reporting event: Event A4 - Neighbour > threshold Measurement reporting event: Event A5 - Serving < threshold1 & Neighbour > threshold2

pc_FeatrGrp_14_T,                            BOOLEAN,       TRUE    #-- @desc  Support of Measurement reporting event: Event A4 - Neighbour > threshold Measurement reporting event: Event A5 - Serving < threshold1 & Neighbour > threshold2

pc_FeatrGrp_15_F,                            BOOLEAN,       TRUE    #-- @desc  Support of Measurement reporting event: Event B1 - Neighbour > threshold

pc_FeatrGrp_15_T,                            BOOLEAN,       TRUE    #-- @desc  Support of Measurement reporting event: Event B1 - Neighbour > threshold

pc_FeatrGrp_16_F,                            BOOLEAN,       TRUE    #-- @desc  Support of Periodical measurement reporting for non-ANR related measurements

pc_FeatrGrp_16_T,                            BOOLEAN,       TRUE    #-- @desc  Support of Periodical measurement reporting for non-ANR related measurements

pc_FeatrGrp_17_F,                            BOOLEAN,       TRUE    #-- @desc  Support of Periodical measurement reporting for SON  ANR and ANR related intra-frequency measurement reporting events

pc_FeatrGrp_17_T,                            BOOLEAN,       TRUE    #-- @desc  Support of Periodical measurement reporting for SON  ANR and ANR related intra-frequency measurement reporting events

pc_FeatrGrp_18_F,                            BOOLEAN,       TRUE    #-- @desc  Support of ANR related inter-frequency measurement reporting events

pc_FeatrGrp_18_T,                            BOOLEAN,       TRUE    #-- @desc  Support of ANR related inter-frequency measurement reporting events

pc_FeatrGrp_19_F,                            BOOLEAN,       TRUE    #-- @desc  Support of ANR related inter-RAT measurement reporting events

pc_FeatrGrp_19_T,                            BOOLEAN,       TRUE    #-- @desc  Support of ANR related inter-RAT measurement reporting events

pc_FeatrGrp_1_F,                             BOOLEAN,       TRUE    #-- @desc  Support of Intra-subframe frequency hopping for PUSCH scheduled by UL grant Extended cyclic prefix with f = 7.5kHz for DL resource block DCI format 3a (TPC commands for PUCCH and PUSCH with single bit power adjustments) Multi-user MIMO for PDSCH Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-0 - UE selected subband CQI without PMI Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2 - UE selected subband CQI with multiple PMI

pc_FeatrGrp_1_T,                             BOOLEAN,       TRUE    #-- @desc  Support of Intra-subframe frequency hopping for PUSCH scheduled by UL grant Extended cyclic prefix with f = 7.5kHz for DL resource block DCI format 3a (TPC commands for PUCCH and PUSCH with single bit power adjustments) Multi-user MIMO for PDSCH Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-0 - UE selected subband CQI without PMI Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2 - UE selected subband CQI with multiple PMI

pc_FeatrGrp_20_F,                            BOOLEAN,       TRUE    #-- @desc  Support of RB combination: SRB1 and SRB2 for DCCH + x AM DRB + x UM DRB

pc_FeatrGrp_20_T,                            BOOLEAN,       TRUE    #-- @desc  Support of RB combination: SRB1 and SRB2 for DCCH + x AM DRB + x UM DRB

pc_FeatrGrp_21_F,                            BOOLEAN,       TRUE    #-- @desc  Support of Predefined intra-subframe frequency hopping for PUSCH with N_sb > 1 Predefined inter-subframe frequency hopping for PUSCH with N_sb > 1

pc_FeatrGrp_21_T,                            BOOLEAN,       TRUE    #-- @desc  Support of Predefined intra-subframe frequency hopping for PUSCH with N_sb > 1 Predefined inter-subframe frequency hopping for PUSCH with N_sb > 1

pc_FeatrGrp_22_F,                            BOOLEAN,       TRUE    #-- @desc  Support of UTRAN measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_22_T,                            BOOLEAN,       TRUE    #-- @desc  Support of UTRAN measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_23_F,                            BOOLEAN,       TRUE    #-- @desc  Support of GERAN measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_23_T,                            BOOLEAN,       TRUE    #-- @desc  Support of GERAN measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_24_F,                            BOOLEAN,       false   #-- @desc  Support of cdma2000 measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_24_T,                            BOOLEAN,       false   #-- @desc  Support of cdma2000 measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_25_F,                            BOOLEAN,       TRUE    #-- @desc  Support of Inter-frequency measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_25_T,                            BOOLEAN,       TRUE    #-- @desc  Support of Inter-frequency measurements and reporting in E-UTRA connected mode

pc_FeatrGrp_26_F,                            BOOLEAN,       false   #-- @desc  Support of HRPD measurements reporting and measurement reporting event B2 in E-UTRA connected mode

pc_FeatrGrp_26_T,                            BOOLEAN,       false   #-- @desc  Support of HRPD measurements reporting and measurement reporting event B2 in E-UTRA connected mode

pc_FeatrGrp_27_F,                            BOOLEAN,       TRUE    #-- @desc  Support of EUTRA RRC_CONNECTED to UTRA CELL_DCH CS handover

pc_FeatrGrp_27_T,                            BOOLEAN,       TRUE    #-- @desc  Support of EUTRA RRC_CONNECTED to UTRA CELL_DCH CS handover

pc_FeatrGrp_28_F,                            BOOLEAN,       TRUE    #-- @desc  Support of TTI bundling

pc_FeatrGrp_28_T,                            BOOLEAN,       TRUE    #-- @desc  Support of TTI bundling

pc_FeatrGrp_29_F,                            BOOLEAN,       TRUE    #-- @desc  Support of Semi-Persistent Scheduling

pc_FeatrGrp_29_T,                            BOOLEAN,       TRUE    #-- @desc  Support of Semi-Persistent Scheduling

pc_FeatrGrp_2_F,                             BOOLEAN,       TRUE    #-- @desc  Support of Simultaneous CQI and ACKNACK on PUCCH i.e. PUCCH format 2a and 2b Absolute TPC command for PUSCH Resource allocation type 1 for PDSCH Periodic CQIPMIRI reporting on PUCCH: Mode 2- 0 - UE selected subband CQI without PMI Periodic CQIPMIRI reporting on PUCCH: Mode 2-1 - UE selected subband CQI with single PMI

pc_FeatrGrp_2_T,                             BOOLEAN,       TRUE    #-- @desc  Support of Simultaneous CQI and ACKNACK on PUCCH i.e. PUCCH format 2a and 2b Absolute TPC command for PUSCH Resource allocation type 1 for PDSCH Periodic CQIPMIRI reporting on PUCCH: Mode 2- 0 - UE selected subband CQI without PMI Periodic CQIPMIRI reporting on PUCCH: Mode 2-1 - UE selected subband CQI with single PMI

pc_FeatrGrp_30_F,                            BOOLEAN,       TRUE    #-- @desc  Support of Handover between FDD and TDD

pc_FeatrGrp_30_T,                            BOOLEAN,       TRUE    #-- @desc  Support of Handover between FDD and TDD

pc_FeatrGrp_31_F,                            BOOLEAN,       TRUE    #-- @desc  Support of the mechanisms defined for cells broadcasting multi band information i.e. comprehending multiBandInfoList

pc_FeatrGrp_31_T,                            BOOLEAN,       TRUE    #-- @desc  Support of the mechanisms defined for cells broadcasting multi band information i.e. comprehending multiBandInfoList

pc_FeatrGrp_33_F,                            BOOLEAN,       TRUE    #-- @desc  Inter-RAT ANR features for UTRAN including:  Inter-RAT periodical measurement reporting where triggerType is set to periodical and purpose is set to reportStrongestCellsForSON

pc_FeatrGrp_33_T,                            BOOLEAN,       TRUE    #-- @desc  Inter-RAT ANR features for UTRAN including:

pc_FeatrGrp_34_F,                            BOOLEAN,       TRUE    #-- @desc  Inter-RAT ANR features for GERAN including:

pc_FeatrGrp_34_T,                            BOOLEAN,       TRUE    #-- @desc  Inter-RAT ANR features for GERAN including:

pc_FeatrGrp_35_F,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for 1xRTT including:

pc_FeatrGrp_35_T,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for 1xRTT including:

pc_FeatrGrp_36_F,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for HRPD including:

pc_FeatrGrp_36_T,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for HRPD including:  Inter-RAT periodical measurement reporting where triggerType is set to periodical and purpose is set to portStrongestCellsForSON

pc_FeatrGrp_37_F,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for UTRAN TDD including:

pc_FeatrGrp_37_T,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for UTRAN TDD including:

pc_FeatrGrp_38_F,                            BOOLEAN,       false   #-- @desc  EUTRA RRC_CONNECTED to UTRA TDD CELL_DCH PS handover if the UE supports both UTRAN FDD and UTRAN TDD

pc_FeatrGrp_38_T,                            BOOLEAN,       false   #-- @desc  EUTRA RRC_CONNECTED to UTRA TDD CELL_DCH PS handover if the UE supports both UTRAN FDD and UTRAN TDD

pc_FeatrGrp_39_F,                            BOOLEAN,       false   #-- @desc  UTRAN TDD measurements reporting and measurement reporting event B2 in E-UTRA connected mode if the UE supports both UTRAN FDD and UTRAN TDD

pc_FeatrGrp_39_T,                            BOOLEAN,       false   #-- @desc  UTRAN TDD measurements reporting and measurement reporting event B2 in E-UTRA connected mode if the UE supports both UTRAN FDD and UTRAN TDD

pc_FeatrGrp_3_F,                             BOOLEAN,       TRUE    #-- @desc  Support of Semi-persistent scheduling TTI bundling 5bit RLC UM SN 7bit PDCP SN

pc_FeatrGrp_3_T,                             BOOLEAN,       TRUE    #-- @desc  Support of Semi-persistent scheduling TTI bundling 5bit RLC UM SN 7bit PDCP SN

pc_FeatrGrp_40_F,                            BOOLEAN,       TRUE    #-- @desc  EUTRA RRC_CONNECTED to UTRA TDD  CELL_DCH  CS handover if the UE supports both UTRAN FDD and UTRAN TDD

pc_FeatrGrp_40_T,                            BOOLEAN,       TRUE    #-- @desc  EUTRA RRC_CONNECTED to UTRA TDD  CELL_DCH  CS handover if the UE supports both UTRAN FDD and UTRAN TDD

pc_FeatrGrp_41_F,                            BOOLEAN,       TRUE    #-- @desc  Measurement reporting event: Event B1 Neighbour > threshold for UTRAN FDD if the UE supports UTRAN FDD and has set bit number 22 to 1

pc_FeatrGrp_41_T,                            BOOLEAN,       TRUE    #-- @desc  Measurement reporting event: Event B1 Neighbour > threshold for UTRAN FDD if the UE supports UTRAN FDD and has set bit number 22 to 1

pc_FeatrGrp_42_F,                            BOOLEAN,       false   #-- @desc  DCI format 3a (TPC commands for PUCCH and PUSCH with single bit power adjustments)

pc_FeatrGrp_42_T,                            BOOLEAN,       false   #-- @desc  DCI format 3a (TPC commands for PUCCH and PUSCH with single bit power adjustments)

pc_FeatrGrp_4_F,                             BOOLEAN,       TRUE    #-- @desc  Support of Short DRX cycle

pc_FeatrGrp_4_T,                             BOOLEAN,       TRUE    #-- @desc  Support of Short DRX cycle

pc_FeatrGrp_5_F,                             BOOLEAN,       false   #-- @desc  Support of Long DRX cycle DRX command MAC control element

pc_FeatrGrp_5_T,                             BOOLEAN,       false   #-- @desc  Support of Long DRX cycle DRX command MAC control element

pc_FeatrGrp_6_F,                             BOOLEAN,       TRUE    #-- @desc  Support of Piroritized bit rate

pc_FeatrGrp_6_T,                             BOOLEAN,       TRUE    #-- @desc  Support of Piroritized bit rate

pc_FeatrGrp_7_F,                             BOOLEAN,       TRUE    #-- @desc  Support of RLC UM

pc_FeatrGrp_7_T,                             BOOLEAN,       TRUE    #-- @desc  Support of RLC UM

pc_FeatrGrp_8_F,                             BOOLEAN,       TRUE    #-- @desc  Support of EUTRA RRC_CONNECTED to UTRA CELL_DCH PS handover

pc_FeatrGrp_8_T,                             BOOLEAN,       TRUE    #-- @desc  Support of EUTRA RRC_CONNECTED to UTRA CELL_DCH PS handover

pc_FeatrGrp_9_F,                             BOOLEAN,       TRUE    #-- @desc  Support of EUTRA RRC_CONNECTED to GERAN GSM_Dedicated handover

pc_FeatrGrp_9_T,                             BOOLEAN,       TRUE    #-- @desc  Support of EUTRA RRC_CONNECTED to GERAN GSM_Dedicated handover

pc_FixedBroadband,                           BOOLEAN,       false   #-- @desc  UE supports Fixed Broadband

pc_FullNameNetwork,                          BOOLEAN,       false   #-- @desc  Support of storage of the network full name

pc_GERAN,                                    BOOLEAN,       false   #-- @desc  UE Supports GSM andor GPRS

pc_GERAN_2_E_UTRAN_PSHO,                     BOOLEAN,       false   #-- @desc  Support of GERAN to E-UTRAN PS Handover

pc_GERAN_2_E_UTRAN_meas,                     BOOLEAN,       TRUE    #-- @desc  Supports Neighbour Cell measurements and Network controlled & autonomous cell reselection to E-UTRAN

pc_GERAN_2_E_UTRAN_measreporting_CCN,        BOOLEAN,       TRUE    #-- @desc  Supports CCN towards E-UTRAN E-UTRAN Neighbour cell measurement reporting and Network controlled cell reselection to E-UTRAN

pc_HO_from_UTRA_to_eFDD,                     BOOLEAN,       false   #-- @desc  Support of Inter-RAT PS handover to E-UTRA from UTRA (FDD)

pc_HO_from_UTRA_to_eTDD,                     BOOLEAN,       TRUE    #-- @desc  Support of Inter-RAT PS handover to E-UTRA from UTRA (TDD)

pc_HRPD,                                     BOOLEAN,       false   #-- @desc  UE supports CDMA2000 HRPD band class

pc_Highspeed_Enh_Prach,                      BOOLEAN,       false   #-- @desc  Support high speed enhancement for random access preambles generated from restricted set type B in high speed scenario as specifed in TS 36.211

pc_HttpDigestAuthentication,                 BOOLEAN,       false   #-- @desc  HTTP Digest XCAP Authentication

pc_HttpGBAAuthentication,                    BOOLEAN,       false   #-- @desc  GBA XCAP Authentication

pc_IMS,                                      BOOLEAN,       false   #-- @desc  Support of IMS

pc_IMSI_Detach,                              BOOLEAN,       false   #-- @desc  Support of detach for non-EPS services

pc_IMS_APN_default,                          BOOLEAN,       false   #-- @desc  Configured with IMS APN as default APN

pc_IMS_Audio_FeatureTag,                     BOOLEAN,       false   #-- @desc  UE supports audio media feature tag

pc_IMS_CS_PS_SRVCC,                          BOOLEAN,       false   #-- @desc  UE Supports CS to PS SRVCC

pc_IMS_CS_PS_SRVCCAlert,                     BOOLEAN,       false   #-- @desc  UE Supports CS to PS SRVCC in alerting state

pc_IMS_CS_PS_SRVCCMidCall,                   BOOLEAN,       false   #-- @desc  UE Supports CS to PS SRVCC and the MSC server assisted mid-call feature

pc_IMS_Deregistration,                       BOOLEAN,       false   #-- @desc  UE has the method that supports IMS deregistration

pc_IMS_E2ae,                                 BOOLEAN,       false   #-- @desc  UE supports end-to-access-edge media security using SDES

pc_IMS_EmergencyCall,                        BOOLEAN,       false   #-- @desc  UE supports IMS emergency services

pc_IMS_ExplicitConsultativeTransfer,         BOOLEAN,       false   #-- @desc  Explicit Communication Transfer - consultative transfer

pc_IMS_GIBA_Sec,                             BOOLEAN,       false   #-- @desc  UE supports GIBA security only

pc_IMS_GRUUsInSIP,                           BOOLEAN,       false   #-- @desc  UE supports obtaining and using GRUUs in the Session Initiation Protocol (SIP)

pc_IMS_Geolocation,                          BOOLEAN,       false   #-- @desc  UE is capable of obtaining location information

pc_IMS_SRVCCAlert,                           BOOLEAN,       false   #-- @desc  UE indicates g.3gpp.srvcc-alerting media feature tag in INVITE request or 180 response

pc_IMS_Sec,                                  BOOLEAN,       TRUE    #-- @desc  UE supports full IMS security

pc_IMS_TWS,                                  BOOLEAN,       false   #-- @desc  Three way session

pc_IMS_Video_FeatureTag,                     BOOLEAN,       false   #-- @desc  UE indicates video media feature tag in REGISTER and INVITE request

pc_IMS_after_EmReg_rejection,                BOOLEAN,       false   #-- @desc  UE reattempts IMS emergency service without registration after rejection of emergency registration

pc_IMS_eCall_Capable,                        BOOLEAN,       false   #-- @desc  UE supports IMS eCall type of emergency services

pc_IMS_eCall_Only,                           BOOLEAN,       false   #-- @desc  UE supports IMS eCall Only type of emergency services

pc_IMS_emergency_call,                       BOOLEAN,       false   #-- @desc  Support of MS emergency call

pc_IP_Ping,                                  BOOLEAN,       false   #-- @desc  Support of ICMP or ICMP IPv6

pc_IPv4,                                     BOOLEAN,       TRUE    #-- @desc  UE supports IPv4 (used IMS PICS as currently not defined in LTE)

pc_IPv4_Link_MTU_Parameter,                  BOOLEAN,       false   #-- @desc  UE supports IPv4 Link MTU parameter

pc_IPv6,                                     BOOLEAN,       false   #-- @desc  UE supports IPv6 (used IMS PICS as currently not defined in LTE)

pc_ISR,                                      BOOLEAN,       TRUE    #-- @desc  Support of ISR

pc_ImmConnect,                               BOOLEAN,       false   #-- @desc  Immediate connection supported for all circuit switched basic services

pc_IndicateSigcomp,                          BOOLEAN,       false   #-- @desc  Indicate the willingness to receive the responses and requests compressed from initial REGISTER onwards by using the "comp=sigcomp" parameter

pc_InitiateP_CSCFDiscovery_viaDHCPv4,        BOOLEAN,       false   #-- @desc  UE capable of being configured to initiate P-CSCF discovery via DHCPv4

pc_InitiateP_CSCFDiscovery_viaDHCPv6,        BOOLEAN,       false   #-- @desc  UE capable of being configured to initiate P-CSCF discovery via DHCPv6

pc_InitiateP_CSCFDiscovery_viaPCO,           BOOLEAN,       false   #-- @desc  UE capable of being configured to initiate P-CSCF discovery via PCO

pc_InitiateSession,                          BOOLEAN,       TRUE    #-- @desc  Initiating a session

pc_InitiatesDedicatedPDPContext,             BOOLEAN,       TRUE    #-- @desc  UE capable of being configured to initiate Dedicated PDP Context

pc_InterBand_ENDC_IncludingFR1_FR2,          BOOLEAN,       false   #-- @desc  Inter-Band EN-DC including both FR1 and FR2

pc_InterBand_ENDC_IncludingFR2,              BOOLEAN,       false   #-- @desc  Inter-Band EN-DC including FR2

pc_InterBand_ENDC_WithinFR1,                 BOOLEAN,       false   #-- @desc  Inter-Band EN-DC within FR1

pc_InterBand_NRDC_BetweenFR1_FR2,            BOOLEAN,       false   #-- @desc  Inter-Band EN-DC bewtween FR1 and FR2

pc_InterFreq_ProximityIndication,            BOOLEAN,       false   #-- @desc  Support of Inter Frequency Proximity Indication

pc_IntraBand_Contiguous_ENDC,                BOOLEAN,       false   #-- @desc  Intra-Band Contiguous EN-DC

pc_IntraBand_NonContiguous_ENDC,             BOOLEAN,       false   #-- @desc  Intra-Band Non-Contiguous EN-DC

pc_IntraFreqA3_CE_ModeA,                     BOOLEAN,       false   #-- @desc  Support of eventA3 for intra-frequency neighbouring cells in normal coverage and CE Mode A

pc_IntraFreqHO_CE_ModeA,                     BOOLEAN,       false   #-- @desc  Support of intra-frequency handover to target cell in normal coverage and CE Mode A

pc_IntraFreq_ProximityIndication,            BOOLEAN,       false   #-- @desc  Support of Intra Frequency Proximity Indication

pc_KeepEpsBearerParametersAfterNormalDetach, BOOLEAN,       false   #-- @desc  If the UE supports this then the next ATTACH after DETACH shall be done using AT command AT+CGATT=1.

pc_LAP,                                      BOOLEAN,       false   #-- @desc  Support of Low Access Priority Indication.

pc_LAP_override,                             BOOLEAN,       false   #-- @desc  Support of Low Access Prioirty Override

pc_LocalTimeZone,                            BOOLEAN,       TRUE    #-- @desc  Support of storage of the local time zone

pc_LoggedMeasurementsIdle,                   BOOLEAN,       TRUE    #-- @desc  Support of logged measurements in RRC_IDLE

pc_MTSI_ACR,                                 BOOLEAN,       false   #-- @desc  MTSI supplementary services - Anonymous Communication Rejection

pc_MTSI_CommDivert,                          BOOLEAN,       TRUE    #-- @desc  MTSI supplementary services - Communication Diversion

pc_MTSI_CommHold,                            BOOLEAN,       TRUE    #-- @desc  Communication Hold

pc_MTSI_CommWaiting,                         BOOLEAN,       TRUE    #-- @desc  MTSI supplementary services - Communication Waiting

pc_MTSI_Conference,                          BOOLEAN,       TRUE    #-- @desc  MTSI supplementary services - Conference

pc_MTSI_Incoming_CB,                         BOOLEAN,       false   #-- @desc  MTSI supplementary services - Incoming Communication Barring

pc_MTSI_MessageWait,                         BOOLEAN,       TRUE    #-- @desc  MTSI supplementary services - Message Waiting Indication

pc_MTSI_NetworkInvitationToConference,       BOOLEAN,       false   #-- @desc  MTSI supplementary services - Network Invitation to Conference

pc_MTSI_OIP,                                 BOOLEAN,       TRUE    #-- @desc  MTSI supplementary services - Originating Identification Presentation

pc_MTSI_OIR,                                 BOOLEAN,       false   #-- @desc  MTSI supplementary services - Originating Identification Restriction

pc_MTSI_OIR_C,                               BOOLEAN,       false   #-- @desc  MTSI supplementary services - Originating Identification Restriction - Configuration

pc_MTSI_OOD_REFER,                           BOOLEAN,       false   #-- @desc  UE supports Fixed Out of Dialog REFER

pc_MTSI_Outgoing_CB,                         BOOLEAN,       false   #-- @desc  MTSI supplementary services - Outgoing Communication Barring

pc_MTSI_Speech,                              BOOLEAN,       TRUE    #-- @desc  MTSI media - Speech

pc_MTSI_Speech_AMRWB,                        BOOLEAN,       TRUE    #-- @desc  MTSI media - Speech AMR wideband

pc_MTSI_Speech_EVS,                          BOOLEAN,       false   #-- @desc  MTSI media - Speech EVS

pc_MTSI_TIP,                                 BOOLEAN,       false   #-- @desc  MTSI supplementary services - Terminating Identification Presentation

pc_MTSI_TIR,                                 BOOLEAN,       false   #-- @desc  MTSI supplementary services - Terminating Identification Restriction

pc_MTSI_TIR_C,                               BOOLEAN,       false   #-- @desc  MTSI supplementary services - Terminating Identification Restriction - Configuration

pc_MTSI_Text_RTP,                            BOOLEAN,       false   #-- @desc  MTSI media - Text RTP

pc_MTSI_Video,                               BOOLEAN,       TRUE    #-- @desc   MTSI media - Video

pc_Manual_CSG_Selection,                     BOOLEAN,       TRUE    #-- @desc  Support of Manual CSG selection

pc_More_Than_128_CAbandComb,                 BOOLEAN,       false   #-- @desc  Support of more than 128 CA Band Combinations

pc_MultimediaTelephonyService,               BOOLEAN,       TRUE    #-- @desc  Multimedia telephony service participant

pc_MultipleIMPU,                             BOOLEAN,       false   #-- @desc  UE supports multiple IMPU

pc_Multiple_PDN,                             BOOLEAN,       TRUE    #-- @desc  Support for multiple PDN connections

pc_NE_DC,                                    BOOLEAN,       false   #-- @desc  NE-DC (Option 4)

pc_NG102_Call_Combined_Registration_EUTRA,   BOOLEAN,       false   #-- @desc  Voice call after combined Registration E-UTRA

pc_NG102_Call_Combined_Registration_WLAN,    BOOLEAN,       false   #-- @desc  Voice call after combined Registration WLAN

pc_NG102_Combined_Registration_EUTRA,        BOOLEAN,       false   #-- @desc  Combined Registration E-UTRA

pc_NG102_Combined_Registration_WLAN,         BOOLEAN,       false   #-- @desc  Combined Registration WLAN

pc_NG102_Dual_Registration_EUTRA,            BOOLEAN,       false   #-- @desc  Dual Registration E-UTRA

pc_NGEN_DC,                                  BOOLEAN,       false   #-- @desc  NE-DC (Option 7)

pc_NG_RAN_EUTRA,                             BOOLEAN,       false   #-- @desc  NG-RAN E-UTRA (Option 5)

pc_NG_RAN_NR,                                BOOLEAN,       false   #-- @desc  NG-RAN NR (Option 2)

pc_NGeFDD,                                   BOOLEAN,       false   #-- @desc  NG-RAN E-UTRA FDD (Option 5)

pc_NGeTDD,                                   BOOLEAN,       false   #-- @desc  NG-RAN E-UTRA TDD (Option 5)

pc_NonIP_Link_MTU_Parameter,                 BOOLEAN,       false   #-- @desc  UE supports Non-IP Link MTU parameter

pc_P2X_UE,                                   BOOLEAN,       false   #-- @desc  Support of V2X communicatin as Pedestrian UE

pc_PDCP_PktDelay,                            BOOLEAN,       false   #-- @desc  Support for PDCP Packet Delay per QCI

pc_PLMN_EF_LRPLMNSI_Automatic_Mode_Exception,BOOLEAN,       false   #-- @desc  Support of Automatic Mode EF_LRPLMSI PLMN Selection Expression

pc_PLMN_Manual_Mode_Exception,               BOOLEAN,       false   #-- @desc  Support of Manual Mode PLMN Selection Expression

pc_PPI_Support,                              BOOLEAN,       TRUE    #-- @desc  Support of Power Preference Indication

pc_PS,                                       BOOLEAN,       TRUE    #-- @desc  Packet Switched

pc_PS_data_centric,                          BOOLEAN,       false   #-- @desc  Support of configuring the UE to PS data centric

pc_PS_voice_centric,                         BOOLEAN,       TRUE    #-- @desc  Support of configuring the UE to PS voice centric

pc_PWS_UpperLayer,                           BOOLEAN,       false   #-- @desc  Presence of PWS upper layer for functions like duplicate definition

pc_P_CSCFDiscovery_viaDHCPv4,                BOOLEAN,       TRUE    #-- @desc  UE supports P-CSCF discovery via DHCPv4

pc_P_CSCFDiscovery_viaDHCPv6,                BOOLEAN,       TRUE    #-- @desc  UE supports P-CSCF discovery via DHCPv6

pc_P_CSCFDiscovery_viaPCO,                   BOOLEAN,       TRUE    #-- @desc  UE supports P-CSCF Discovery via PCO

pc_Preconditions,                            BOOLEAN,       TRUE    #-- @desc  Integration of resource management and SIP? (use of preconditions)

pc_ProvideDST_inUse,                         BOOLEAN,       false   #-- @desc  UE supports a mechanism to provide daylight saving time

pc_Provide_IMS_APN,                          BOOLEAN,       false   #-- @desc  Configured to provide IMS APN during initial attach

pc_Provide_IMS_as_second_APN,                BOOLEAN,       false   #-- @desc  Configured to provide IMS APN as the 2nd PDN connection

pc_Provide_Internet_as_second_APN,           BOOLEAN,       false   #-- @desc  Configured to provide Internet APN as the 2nd PDN connection

pc_RLF_ReportForInterRAT_MRO,                BOOLEAN,       false   #-- @desc  Support of Radio Link Failure Report for InterRAT MRO

pc_ROHC_profile0x0001,                       BOOLEAN,       TRUE    #-- @desc  Support for ROHC profile0x0001

pc_ROHC_profile0x0002,                       BOOLEAN,       TRUE    #-- @desc  Support for ROHC profile0x0002

pc_ROHC_profile0x0003,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0003

pc_ROHC_profile0x0004,                       BOOLEAN,       TRUE    #-- @desc  Support for ROHC profile0x0004

pc_ROHC_profile0x0006,                       BOOLEAN,       TRUE    #-- @desc  Support for ROHC profile0x0006

pc_ROHC_profile0x0101,                       BOOLEAN,       TRUE    #-- @desc  Support for ROHC profile0x0101

pc_ROHC_profile0x0102,                       BOOLEAN,       TRUE    #-- @desc  Support for ROHC profile0x0102

pc_ROHC_profile0x0103,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0103

pc_ROHC_profile0x0104,                       BOOLEAN,       TRUE    #-- @desc  Support for ROHC profile0x0104

pc_Rach_Report,                              BOOLEAN,       false   #-- @desc  Support of delivery of rachReport upon request from the network

pc_Re_Attach_AfterDetachColl,                BOOLEAN,       false   #-- @desc  Support of automatic re-activation of the EPS bearers during network initiated detach even though UE has initiated a detach procedure with detach type set to EPS detach or combined EPSIMSI detach

pc_RequestIPv4HAAddress_DuringAttach,        BOOLEAN,       false   #-- @desc  Support for being configured to request the IPv4 address of the Home Agent during Attach procedure

pc_RequestIPv6HAAddress_DuringAttach,        BOOLEAN,       false   #-- @desc  Support for being configured to request the IPv6 address of the Home Agent during Attach procedure

pc_SCPTM,                                    BOOLEAN,       false   #-- @desc  The UE supports SC-PTM

pc_SIP_Based_UserConfiguration,              BOOLEAN,       false   #-- @desc  SIP based user configuration

pc_SIP_Digest,                               BOOLEAN,       false   #-- @desc  SIP Digest without TLS

pc_SI_Neighbour_UMTS_Autonomous_Gaps,        BOOLEAN,       false   #-- @desc  Upon configuration of si-RequestForHO by the network supports acquistion of relevant information from a neighbouring UMTS cell by reading the SI of the neighbouring cell using autonomous gaps and reporting

pc_SI_Neighbour_interFreq_Autonomous_Gaps,   BOOLEAN,       false   #-- @desc  Supports upon configuration of si-requestForHO by the network acquisition of relevant information from a neighbouring intrer-frequency cell by reading the SI of the neighouring cell using autonomous gaps and reporting

pc_SI_Neighbour_intraFreq_Autonomous_Gaps,   BOOLEAN,       false   #-- @desc  Supports upon configuration of si-requestForHO by the network acquisition of relevant information from a neighbouring intra-frequency cell by reading the SI of the neighouring cell using autonomous gaps and reporting

pc_SMS_IP_MO,                                BOOLEAN,       false   #-- @desc  UE supports SM-over-IP sender

pc_SMS_IP_MT,                                BOOLEAN,       false   #-- @desc  UE supports SM-over-IP receiver

pc_SMS_SGs,                                  BOOLEAN,       false   #-- @desc  The UE supports SMS over SGs and is configured for SMS over SGs.  If true at least one of pc_SMS_SGs_MT and pc_SMS_SGs_MO is true. If it is set to true pc_combined_attach shall be set to true

pc_SMS_SGs_MO,                               BOOLEAN,       TRUE    #-- @desc  Support of Short Message Service (SMS) MO over SGs

pc_SMS_SGs_MT,                               BOOLEAN,       TRUE    #-- @desc  Support of Short Message Service (SMS) MT over SGs

pc_SMS_SGs_Multi_MO,                         BOOLEAN,       TRUE    #-- @desc  Support of sending concatenated multiple short message over SGs

pc_SRS_switching,                            BOOLEAN,       false   #-- @desc  Support of SRS switching between a band pair

pc_SRVCC_GERAN_UTRAN,                        BOOLEAN,       TRUE    #-- @desc  Support for SRVCC from E-UTRAN to GERANUTRAN

pc_Semi_Persistence_Scheduling,              BOOLEAN,       TRUE    #-- @desc  Support of semi persistance scheduling

pc_ShortNameNetwork,                         BOOLEAN,       TRUE    #-- @desc  Support of storage of the network short name

pc_Speech,                                   BOOLEAN,       TRUE    #-- @desc  UE supports Speech

pc_Squal_based_CellReselection_between_E_UTRAN_and_GERAN,BOOLEAN,       TRUE    #-- @desc  Support of Squal based cell reselection to E-UTRAN from GERAN

pc_Squal_based_CellReselection_to_E_UTRAN_from_UTRAN,BOOLEAN,       TRUE    #-- @desc  Support of Squal based cell reselection to E-UTRAN from UTRAN

pc_Squal_based_CellReselection_to_UTRAN_from_E_UTRAN,BOOLEAN,       TRUE    #-- @desc  Support of Squal based cell reselection to UTRAN from E-UTRAN

pc_StandaloneGNSS_Location,                  BOOLEAN,       TRUE    #-- @desc  Support of standalone GNSS receiver to provide detailed location information in RRC measurement report and logged measurements in RRC_IDLE

pc_SupportOpModeA,                           BOOLEAN,       TRUE    #-- @desc  UE supports Operation Mode A

pc_SwitchOnOff,                              BOOLEAN,       TRUE    #-- @desc  switch onoff supported

pc_T3412Extended,                            BOOLEAN,       false   #-- @desc  Support of T3412 extended value IE

pc_TAU_connected_in_IMS,                     BOOLEAN,       false   #-- @desc  Support of TAU in connected mode. Applicable when configured to pc_voice_PS_1_CS_2 and pc_Attach

pc_TAU_idle_in_IMS,                          BOOLEAN,       false   #-- @desc  Support of TAU in idle mode. Applicable when configured to pc_voice_PS_1_CS_2 and pc_Attach

pc_TDD_HCR,                                  BOOLEAN,       false   #-- @desc  UE supports UTRA band as defined in TS 25.102

pc_TDD_LCR,                                  BOOLEAN,       false   #-- @desc  UE supports UTRA band as defined in TS 25.102

pc_TDD_SpecialSubframe,                      BOOLEAN,       false   #-- @desc  Support of TDD special subframe

pc_TDD_VHCR,                                 BOOLEAN,       false   #-- @desc  UE supports UTRA band as defined in TS 25.102

pc_TTI_Bundling,                             BOOLEAN,       TRUE    #-- @desc  Support of TTI Bundling

pc_TestModeforCSGproximity,                  BOOLEAN,       false   #-- @desc  Support of UE radio bearer test mode for CSG proximity testing

pc_UE_NoRegIMS_IMSVoPS_0,                    BOOLEAN,       false   #-- @desc  The UE does not request IMS PDN connection when IMS VoPS set to '0'

pc_UE_supports_user_initiated_PDN_disconnect,BOOLEAN,       false   #-- @desc  UE supports user initiated PDN disconnect

pc_UL_64QAM,                                 BOOLEAN,       false   #-- @desc  Support of uplink 64 QAM

pc_UL_CA,                                    BOOLEAN,       false   #-- @desc  Support of UL CA

pc_UL_CA_2Carriers,                          BOOLEAN,       false   #-- @desc  UL CA with 2 carriers

pc_UL_CA_3Carriers,                          BOOLEAN,       false   #-- @desc  UL CA with 3 carriers

pc_UL_CoMP,                                  BOOLEAN,       TRUE    #-- @desc  Support of UL co-ordinated multi-point operation

pc_UL_IntraBand_ContCaBWclassB,              BOOLEAN,       TRUE    #-- @desc  UL Intra-band contiguous CA BW class B

pc_UL_IntraBand_ContCaBWclassC,              BOOLEAN,       false   #-- @desc  UL Intra-band contiguous CA BW class C

pc_UL_MIMO,                                  BOOLEAN,       false   #-- @desc  Support of UL MIMO

pc_UL_SupportedInAllBandsInCAComb,           BOOLEAN,       false   #-- @desc  UL (Pcell) supported in each band of Inter-band CA combination under test

pc_UL_interBand_CaAA,                        BOOLEAN,       false   #-- @desc  Support of UL inter-band CA _ A-A

pc_UL_interBand_CaBwClassComb_AA,            BOOLEAN,       false   #-- @desc  UL Inter-band contiguous CA BW class A-A

pc_UL_intraBand_contCaTypeB,                 BOOLEAN,       false   #-- @desc  UL Intra-band contiguous CA Type B

pc_UL_intraBand_contCaTypeC,                 BOOLEAN,       false   #-- @desc  UL Intra-band contiguous CA Type C

pc_UL_intraBand_nonContCaAA,                 BOOLEAN,       false   #-- @desc  Support of UL intra-band non-contiguous CA _ A-A

pc_UL_intraBand_nonContCaBwClassComb_AA,     BOOLEAN,       false   #-- @desc  Support of UL intra-band non-contiguous CA BW Class Combination A-A

pc_UMI_ProcNeeded_DuringCSFB,                BOOLEAN,       TRUE    #-- @desc  Requiring UMI proceeding to paging response

pc_USIM_Removal,                             BOOLEAN,       TRUE    #-- @desc  USIM removable without power down supported

pc_UTRA,                                     BOOLEAN,       false   #-- @desc  UE supports UTRA

pc_UTRAN_ANR,                                BOOLEAN,       false   #-- @desc  Support of UTRAN ANR

pc_UTRAN_ProximityIndication,                BOOLEAN,       false   #-- @desc  Support of UTRAN Proximity Indication

pc_UTRA_FeatrGrp_1,                          BOOLEAN,       TRUE    #-- @desc  Support of UTRA CELL_PCH and URA_PCH to RRC_IDLE cell reselection

pc_UTRA_FeatrGrp_2,                          BOOLEAN,       TRUE    #-- @desc  Support of EUTRAN measurements and reporting in connected mode

pc_UTRA_FeatrGrp_3,                          BOOLEAN,       false   #-- @desc  Support of UTRA CELL_FACH absolute priority cell reselection for high priority layers

pc_UTRA_FeatrGrp_4,                          BOOLEAN,       false   #-- @desc  Support of UTRA CELL_FACH absolute priority cell reselection for all layers

pc_UeAssistedAgps,                           BOOLEAN,       false   #-- @desc  Support of UE assisted Network Assisted GPS L1 CA

pc_UeBasedAgps,                              BOOLEAN,       false   #-- @desc  Support of UE based Network Assisted GPS L1 CA

pc_UniversalAndLocalTimeZone,                BOOLEAN,       TRUE    #-- @desc  Support of storage of the universal time and local time zone

pc_UpdateUE_LocationInformation,             BOOLEAN,       TRUE    #-- @desc  Update UE Location Information

pc_Use_SMS_over_IP,                          BOOLEAN,       false   #-- @desc  The UE is configured to use SMS over IP

pc_UserInitiatedPLMN_Reselection,            BOOLEAN,       TRUE    #-- @desc  Support user initiated PLMN reselection in automatic mode

pc_User_Plane_CIoT_Optimisation,             BOOLEAN,       false   #-- @desc  Support of User Plane CIoT

pc_VideoCodecH264CBP,                        BOOLEAN,       TRUE    #-- @desc  MTSI media - Video codec H.264 CBP Level 1.2

pc_VoLTE,                                    BOOLEAN,       TRUE    #-- @desc  Support of VoLTE in GSMA PRD IR.92: "IMS profile for Voice and SMS"

pc_WLAN,                                     BOOLEAN,       false   #-- @desc  UE supports WLAN

pc_WLAN_voice,                               BOOLEAN,       false   #-- @desc  Support for IR.51

pc_XCAP_UsernameIsConfiguredInUE,            BOOLEAN,       false   #-- @desc  UE indicated OMA-TS-XDM_MO-V1_1-20080627-A.doc section 5.2.8 "Node: <X>AAUTHNAME" is configured

pc_XCAP_XUIisDefaultPublicUserId,            BOOLEAN,       false   #-- @desc  UE uses the default public user id received in P-Associated-URI header in 200 OK for REGISTER as XCAP User Identity (XUI)

pc_XCAP_only_APN,                            BOOLEAN,       false   #-- @desc  Configured with an APN for XCAP only usage

pc_XCAP_over_Internet_APN,                   BOOLEAN,       false   #-- @desc  Configured to use Internet APN for XCAP signalling

pc_ZUC,                                      BOOLEAN,       TRUE    #-- @desc  Support of ZUC algorithm

pc_am_WithShortSN,                           BOOLEAN,       false   #-- @desc  Support RLC AM with 12 bit length of RLC sequence number

pc_as_ReflectiveQoS,                         BOOLEAN,       false   #-- @desc  Support of reflective QoS

pc_configuredUL_GrantType1,                  BOOLEAN,       false   #-- @desc  Support Type 1 PUSCH transmissions with configured grant

pc_configuredUL_GrantType2,                  BOOLEAN,       false   #-- @desc  Support Type 2 PUSCH transmissions with configured grant

pc_csi_RSRP_AndRSRQ_MeasWithSSB,             BOOLEAN,       false   #-- @desc  Support CSI-RSRP and CSI-RSRQ measurement where CSI-RS resource is configured with an associated SSPBCH

pc_csi_RS_CFRA_ForHO,                        BOOLEAN,       false   #-- @desc  Support handover using a contention free random access on PRACH resources that are associated with CSI-RS resources of the target cell

pc_dataInactMon,                             BOOLEAN,       false   #-- @desc  Support of data inactivity monitoring

pc_downlinkSPS,                              BOOLEAN,       false   #-- @desc  Support PDSCH reception based on semi-persistent scheduling

pc_downlink_LAA,                             BOOLEAN,       false   #-- @desc  Supports downlink LAA operation

pc_dynamicSwitch_SUL,                        BOOLEAN,       false   #-- @desc  Support supplemental uplink with dynamic switch (DCI based selection of PUSCH carrier)

pc_eAttachWithIMSI,                          BOOLEAN,       false   #-- @desc  Support of Attach With IMSI

pc_eBand10_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 10

pc_eBand11_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 11

pc_eBand12_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 12

pc_eBand13_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 13

pc_eBand14_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 14

pc_eBand17_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 17

pc_eBand18_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 18

pc_eBand19_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 19

pc_eBand1_Supp,                              BOOLEAN,       TRUE    #-- @desc  Support of Band 1

pc_eBand20_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 20

pc_eBand21_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 21

pc_eBand22_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 22

pc_eBand23_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 23

pc_eBand24_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 24

pc_eBand25_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 25

pc_eBand26_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 26

pc_eBand27_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 27

pc_eBand28_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 28

pc_eBand29_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 29

pc_eBand2_Supp,                              BOOLEAN,       TRUE    #-- @desc  Support of Band 2

pc_eBand30_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 30

pc_eBand31_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 31

pc_eBand32_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 32

pc_eBand33_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 33

pc_eBand34_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 34

pc_eBand35_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 35

pc_eBand36_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 36

pc_eBand37_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 37

pc_eBand38_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 38

pc_eBand39_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 39

pc_eBand3_Supp,                              BOOLEAN,       TRUE    #-- @desc  Support of Band 3

pc_eBand40_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 40

pc_eBand41_Supp,                             BOOLEAN,       TRUE    #-- @desc  Support of Band 41

pc_eBand42_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 42

pc_eBand43_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 43

pc_eBand44_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 44

pc_eBand45_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 45

pc_eBand46_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 46

pc_eBand47_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 47

pc_eBand48_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 48

pc_eBand4_Supp,                              BOOLEAN,       TRUE    #-- @desc  Support of Band 4

pc_eBand5_Supp,                              BOOLEAN,       TRUE    #-- @desc  Support of Band 5

pc_eBand65_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 65

pc_eBand66_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 66

pc_eBand68_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 68

pc_eBand69_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 69

pc_eBand6_Supp,                              BOOLEAN,       false   #-- @desc  Support of Band 6

pc_eBand70_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 70

pc_eBand71_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 71

pc_eBand72_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 72

pc_eBand74_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 74

pc_eBand7_Supp,                              BOOLEAN,       TRUE    #-- @desc  Support of Band 7

pc_eBand8_Supp,                              BOOLEAN,       TRUE    #-- @desc  Support of Band 8

pc_eBand9_Supp,                              BOOLEAN,       false   #-- @desc  Support of Band 9

pc_eCall_Test_Call,                          BOOLEAN,       false   #-- @desc  Capability to trigger a Test eCall

pc_eCall_automatic_Initiated,                BOOLEAN,       false   #-- @desc  Capability to initiate Automatic eCall

pc_eCall_manual_Initiated,                   BOOLEAN,       false   #-- @desc  Capability to initiate a Manual eCall

pc_eFDD,                                     BOOLEAN,       TRUE    #-- @desc  UE supports EUTRA FDD

pc_eFDD_MultiBand,                           BOOLEAN,       TRUE    #-- @desc  Support of multiple E-UTRA FDD bands

pc_eHARQ_Pattern_for_TTI_bundling,           BOOLEAN,       false   #-- @desc  Support of enhanced HARQ pattern for TTI bundling operation for FDD

pc_eIMTA_TDD,                                BOOLEAN,       false   #-- @desc  Support of TDD ULDL reconfiguration for TDD serving cell(s) via monitoring PDCCH with eIMTA-RNTI on a TDD Pcell

pc_eMBMS,                                    BOOLEAN,       TRUE    #-- @desc  Support of eMBMS

pc_eMBMS_SC,                                 BOOLEAN,       TRUE    #-- @desc  Support of eMBMS service continuity

pc_eMinimumPeriodicSearchTimer,              BOOLEAN,       false   #-- @desc  Support of Minimum Periodic Search Timer

pc_ePDCCH,                                   BOOLEAN,       false   #-- @desc  Support of ePDCCH

pc_ePSM,                                     BOOLEAN,       false   #-- @desc  Support of Power Saving Mode (in EUTRA)

pc_eRedirectionUTRA,                         BOOLEAN,       TRUE    #-- @desc  Support of use of the UTRA system information provided by RRCConnectionRelease upon redirection

pc_eTDD,                                     BOOLEAN,       TRUE    #-- @desc  UE supports EUTRA TDD

pc_eTDD_MultiBand,                           BOOLEAN,       false   #-- @desc  Support of multiple E-UTRA TDD bands

pc_edrx,                                     BOOLEAN,       false   #-- @desc  Support of extended DRX

pc_eventA_MeasAndReport,                     BOOLEAN,       false   #-- @desc  Support NR measurements and events A triggered reporting

pc_extendedLongDRX,                          BOOLEAN,       false   #-- @desc  Support of extended Long DRX cycle

pc_fixed_broadband_XCAP,                     BOOLEAN,       false   #-- @desc  The UE uses XCAP in fixed broadband access

pc_freqBandPriorityAdjustment,               BOOLEAN,       false   #-- @desc  Support of prioritization of the frequency bands in multiBandInfoList over the band in freqBandIndicator as defined by freqBandIndicatorPriority-r12

pc_indepenedentGapConfig,                    BOOLEAN,       false   #-- @desc  Support two independent measurement gap configurations for FR1 and FR2

pc_intraAndInterF_MeasAndReport,             BOOLEAN,       false   #-- @desc  Support NR intra-freq and inter-freq measurements and at least periodical reporting

pc_intraFreq_CE_NeedForGaps,                 BOOLEAN,       false   #-- @desc  Require intra-frequency measurement gaps for operating in CE Mode A or CE Mode B

pc_longDRX_Cycle,                            BOOLEAN,       false   #-- @desc  Support long DRX cycle

pc_multipleTimingAdvance,                    BOOLEAN,       false   #-- @desc  Support of multiple timing advances

pc_multipleUplinkSPS,                        BOOLEAN,       false   #-- @desc  Support of multiple uplink SPS and reporting SPS assistance information

pc_nrBand1_Supp,                             BOOLEAN,       false   #-- @desc  NR Band 1

pc_nrBand20_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 20

pc_nrBand257_Supp,                           BOOLEAN,       false   #-- @desc  NR Band 257

pc_nrBand260_Supp,                           BOOLEAN,       false   #-- @desc  NR Band 260

pc_nrBand261_Supp,                           BOOLEAN,       false   #-- @desc  NR Band 261

pc_nrBand28_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 28

pc_nrBand2_Supp,                             BOOLEAN,       false   #-- @desc  NR Band 2

pc_nrBand38_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 38

pc_nrBand3_Supp,                             BOOLEAN,       false   #-- @desc  NR Band 3

pc_nrBand41_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 41

pc_nrBand5_Supp,                             BOOLEAN,       false   #-- @desc  NR Band 5

pc_nrBand66_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 66

pc_nrBand70_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 70

pc_nrBand77_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 77

pc_nrBand78_Supp,                            BOOLEAN,       false   #-- @desc  NR Band 78

pc_nrBand7_Supp,                             BOOLEAN,       false   #-- @desc  NR Band 7

pc_nrBand8_Supp,                             BOOLEAN,       false   #-- @desc  NR Band 8

pc_nrFDD,                                    BOOLEAN,       false   #-- @desc  NR FDD (Option 2)

pc_nrFDD_MultiBand,                          BOOLEAN,       false   #-- @desc  Support of multiple NR FDD bands

pc_nrTDD,                                    BOOLEAN,       TRUE    #-- @desc  NR TDD (Option 2)

pc_nrTDD_MultiBand,                          BOOLEAN,       false   #-- @desc  Support of multiple NR TDD bands

pc_pdsch_256QAM_FR1,                         BOOLEAN,       false   #-- @desc  Support 256QAM for PDSCH for FR1

pc_pdsch_256QAM_FR2,                         BOOLEAN,       false   #-- @desc  Support 256QAM for PDSCH for FR2

pc_pdsch_Mapping_TypeA,                      BOOLEAN,       false   #-- @desc  support receiving PDSCH using PDSCH mapping type A with less than seven symbols

pc_pdsch_Mapping_TypeB,                      BOOLEAN,       false   #-- @desc  support receiving PDSCH using PDSCH mapping type B with less than seven symbols

pc_pdsch_RepetitionMultiSlots,               BOOLEAN,       false   #-- @desc  Support PDSCH Reception when configured with higher layer parameter aggregationFactorDL>1

pc_pusch_256QAM_FR1,                         BOOLEAN,       false   #-- @desc  Support 256QAM for PUSCH for FR1

pc_qci1Indication_inRLF,                     BOOLEAN,       false   #-- @desc  Support of QCI1 indication in Radio Link Failure Report

pc_ra_Type0_PUSCH,                           BOOLEAN,       false   #-- @desc  Support resource allocation Type 0 for PUSCH

pc_reqFreqBands,                             BOOLEAN,       false   #-- @desc  Support of reception of requested Frequency Bands

pc_rssiAndChannelOccupancyReporting,         BOOLEAN,       false   #-- @desc  Supports measurement and reporting for RSSI and channel occupancy

pc_scalingFactor0dot75,                      BOOLEAN,       false   #-- @desc  Support scaling factor 0.75 is applied to the band in the max data rate calculation

pc_scptm_NonServingCell,                     BOOLEAN,       false   #-- @desc  Support of MBMS reception via SC-PTM on a cell that may be additionally configured as an Scell

pc_scptm_SCell,                              BOOLEAN,       false   #-- @desc  Support of MBMS reception via SC-PTM on configured SCell

pc_shortDRX_Cycle,                           BOOLEAN,       false   #-- @desc  Support short DRX cycle

pc_shortSN,                                  BOOLEAN,       false   #-- @desc  Support 12 bit length of PDCP sequence number

pc_shortSPS_intervalFDD,                     BOOLEAN,       false   #-- @desc  Support of SPS interval shorter than 10 subfranes in FDD mode

pc_shortSPS_intervalTDD,                     BOOLEAN,       false   #-- @desc  Support of SPS interval shorter than 10 subfranes in TDD mode

pc_skipUplinkDynamic,                        BOOLEAN,       false   #-- @desc  Support of skipping UL transmissions if no data is available

pc_skipUplinkSPS,                            BOOLEAN,       false   #-- @desc  Support of skipping SPS UL transmissions if no data is available

pc_skipUplinkTxDynamic,                      BOOLEAN,       false   #-- @desc  Support skipping of UL transmission for an uplink grant indicated on PDCCH if no data is available for transmission

pc_splitDRB_withUL_Both_MCG_SCG,             BOOLEAN,       false   #-- @desc  Support UL transmission via both MCG path and SCG path for the split DRB

pc_splitSRB_WithOneUL_Path,                  BOOLEAN,       false   #-- @desc  Support UL transmission via either MCG path or SCG path for the split SRB

pc_srb3,                                     BOOLEAN,       false   #-- @desc  Support direct SRB between the SN and the UE

pc_ss_CCH_Interference_Handling,             BOOLEAN,       false   #-- @desc  Support of Synchronisation signal and common channel interference handling

pc_tdd_FDD_CA_FDD_PCell,                     BOOLEAN,       false   #-- @desc  Support of tdd-FDD-CA-PCellDuplex-r12 with the second bit setting to 1

pc_tdd_FDD_CA_TDD_PCell,                     BOOLEAN,       false   #-- @desc  Support of tdd-FDD-CA-PCellDuplex-r12 with the first bit setting to 1

pc_ue_CategoryDL_0,                          BOOLEAN,       false   #-- @desc  UE Category DL 0

pc_ue_CategoryDL_10,                         BOOLEAN,       false   #-- @desc  UE Category DL 10

pc_ue_CategoryDL_11,                         BOOLEAN,       false   #-- @desc  UE Category DL 11

pc_ue_CategoryDL_12,                         BOOLEAN,       false   #-- @desc  UE Category DL 12

pc_ue_CategoryDL_13,                         BOOLEAN,       false   #-- @desc  UE Category DL 13

pc_ue_CategoryDL_14,                         BOOLEAN,       false   #-- @desc  UE Category DL 14

pc_ue_CategoryDL_15,                         BOOLEAN,       false   #-- @desc  UE Category DL 15

pc_ue_CategoryDL_16,                         BOOLEAN,       false   #-- @desc  UE Category DL 16

pc_ue_CategoryDL_17,                         BOOLEAN,       false   #-- @desc  UE Category DL 17

pc_ue_CategoryDL_18,                         BOOLEAN,       false   #-- @desc  UE Category DL 18

pc_ue_CategoryDL_19,                         BOOLEAN,       false   #-- @desc  UE Category DL 19

pc_ue_CategoryDL_1bis,                       BOOLEAN,       false   #-- @desc  Only in combination with Category UL 1bis and Category 1 UE

pc_ue_CategoryDL_20,                         BOOLEAN,       false   #-- @desc  UE Category DL 20

pc_ue_CategoryDL_21,                         BOOLEAN,       false   #-- @desc  UE Category DL 21

pc_ue_CategoryDL_22,                         BOOLEAN,       false   #-- @desc  UE Category DL 22

pc_ue_CategoryDL_23,                         BOOLEAN,       false   #-- @desc  UE Category DL 23

pc_ue_CategoryDL_24,                         BOOLEAN,       false   #-- @desc  UE Category DL 24

pc_ue_CategoryDL_25,                         BOOLEAN,       false   #-- @desc  UE Category DL 25

pc_ue_CategoryDL_26,                         BOOLEAN,       false   #-- @desc  UE Category DL 26

pc_ue_CategoryDL_4,                          BOOLEAN,       false   #-- @desc  UE Category DL 4

pc_ue_CategoryDL_6,                          BOOLEAN,       false   #-- @desc  UE Category DL 6

pc_ue_CategoryDL_7,                          BOOLEAN,       TRUE    #-- @desc  UE Category DL 7

pc_ue_CategoryDL_9,                          BOOLEAN,       false   #-- @desc  UE Category DL 9

pc_ue_CategoryDL_M1,                         BOOLEAN,       false   #-- @desc  Only in combination with Category UL M0

pc_ue_CategoryDL_M2,                         BOOLEAN,       false   #-- @desc  Only in combination with Category UL M2

pc_ue_CategoryUL_0,                          BOOLEAN,       false   #-- @desc  UE Category UL 0

pc_ue_CategoryUL_13,                         BOOLEAN,       TRUE    #-- @desc  UE Category UL 13

pc_ue_CategoryUL_14,                         BOOLEAN,       false   #-- @desc  UE Category UL 14

pc_ue_CategoryUL_15,                         BOOLEAN,       false   #-- @desc  UE Category UL 15

pc_ue_CategoryUL_16,                         BOOLEAN,       false   #-- @desc  UE Category UL 16

pc_ue_CategoryUL_17,                         BOOLEAN,       false   #-- @desc  UE Category UL 17

pc_ue_CategoryUL_18,                         BOOLEAN,       false   #-- @desc  UE Category UL 18

pc_ue_CategoryUL_19,                         BOOLEAN,       false   #-- @desc  UE Category UL 19

pc_ue_CategoryUL_1bis,                       BOOLEAN,       false   #-- @desc  Only in combination with Category DL 1bis

pc_ue_CategoryUL_20,                         BOOLEAN,       false   #-- @desc  UE Category UL 20

pc_ue_CategoryUL_21,                         BOOLEAN,       false   #-- @desc  UE Category UL 21

pc_ue_CategoryUL_22,                         BOOLEAN,       false   #-- @desc  UE Category UL 22

pc_ue_CategoryUL_23,                         BOOLEAN,       false   #-- @desc  UE Category UL 23

pc_ue_CategoryUL_24,                         BOOLEAN,       false   #-- @desc  UE Category UL 24

pc_ue_CategoryUL_25,                         BOOLEAN,       false   #-- @desc  UE Category UL 25

pc_ue_CategoryUL_26,                         BOOLEAN,       false   #-- @desc  UE Category UL 26

pc_ue_CategoryUL_3,                          BOOLEAN,       false   #-- @desc  UE Category UL 3

pc_ue_CategoryUL_5,                          BOOLEAN,       false   #-- @desc  UE Category UL 5

pc_ue_CategoryUL_7,                          BOOLEAN,       false   #-- @desc  UE Category UL 7

pc_ue_CategoryUL_8,                          BOOLEAN,       false   #-- @desc  UE Category UL 8

pc_ue_CategoryUL_M1,                         BOOLEAN,       false   #-- @desc  Only in combination with Category DL M1

pc_ue_CategoryUL_M2,                         BOOLEAN,       false   #-- @desc  Only in combination with Category DL M2

pc_ue_Category_1,                            BOOLEAN,       false   #-- @desc  UE Category 1

pc_ue_Category_10,                           BOOLEAN,       false   #-- @desc  UE Category 10

pc_ue_Category_11,                           BOOLEAN,       false   #-- @desc  UE Category 11

pc_ue_Category_12,                           BOOLEAN,       false   #-- @desc  UE Category 12

pc_ue_Category_2,                            BOOLEAN,       false   #-- @desc  UE Category 2

pc_ue_Category_3,                            BOOLEAN,       false   #-- @desc  UE Category 3

pc_ue_Category_4,                            BOOLEAN,       TRUE    #-- @desc  UE Category 4

pc_ue_Category_5,                            BOOLEAN,       false   #-- @desc  UE Category 5

pc_ue_Category_6,                            BOOLEAN,       TRUE    #-- @desc  UE Category 6

pc_ue_Category_7,                            BOOLEAN,       TRUE    #-- @desc  UE Category 7

pc_ue_Category_8,                            BOOLEAN,       false   #-- @desc  UE Category 8

pc_ue_Category_9,                            BOOLEAN,       false   #-- @desc  UE Category 9

pc_um_WithLongSN,                            BOOLEAN,       false   #-- @desc  Support RLC UM with 12 bit length of RLC sequence number

pc_um_WithShortSN,                           BOOLEAN,       false   #-- @desc  Support RLC UM with 6 bit length of RLC sequence number

pc_uplink_LAA,                               BOOLEAN,       false   #-- @desc  Supports uplink LAA operation

pc_v2xPartialSensing,                        BOOLEAN,       false   #-- @desc  Support of transmitting PSCCHPSSCH using UE autonomous resource selection mode with partial sensing

pc_voice_PS_1_CS_2,                          BOOLEAN,       TRUE    #-- @desc  Configured voice domain preference

px_AccessPointName,                          OCTETSTRING,   0361706E #-- @desc  Access Point Name

px_AquireGNSS_MaxTime,                       INTEGER,       60      #-- @desc  The maximume time (in seconds) taken for the UE to acquire GNSS and derive UTC time (and normally position) and then start to transit or receive as appropriate

px_AttachTypeTested,                         ENUM-EUTRA_ATTACH_TESTED_Type,COMBINED_ATTACH #-- @desc  Attach Type to be tested if UE supports both pc_Attach and pc_Combined_Attach

px_AuthAMF,                                  BITSTRING,     1001000100010001 #-- @desc  Authentication Management Field (16 bits). The value shall be different from '1111 1111 1111 111'B (AMFresynch).

px_AuthK,                                    BITSTRING,     00000000000000010000001000000011000001000000010100000110000001110000100000001001000010100000101100001100000011010000111000001111 #-- @desc  Authentication Key

px_CipherAlg,                                BITSTRING,     010     #-- Anritsu TTCN CR required px_CipherAlg type @desc  NAS Ciphering Algorithm Default value: (GEA2)

px_CipherKey,                                BITSTRING,     0101111001001010101100110101100010010001001101110101110100101010 #-- @desc  Cipher Key

px_CipherKey128,                             BITSTRING,     01011110010010101011001101011000100100010011011101011101001010100101111001001010101100110101100010010001001101110101110100101010 #-- @desc  Cipher key (128 bits) to be used e.g. for A54 and GEA4

px_DelayBeforeIntraCellHO,                   INTEGER,       300     #-- @desc  Temporary PIXIT used to define the delay before an intra cell handover

px_DigestPasswordForSIP,                     CHARSTRING,    SIP-Password #-- @desc  SIP password

px_DigestPasswordForXCAP,                    CHARSTRING,    XCAP-Password #-- @desc  XCAP password

px_ENDC_BandCombination,                     ENUM-ENDC_BandCombination_Type,DC_1A_n78A #-- @desc  Band combination for EN-DC test cases

px_EUTRA_CA_BandCombination,                 ENUM-CA_BandCombination_Type,CA_1C   #-- @desc  CA band combination applied in CA test cases

px_EUTRA_DC_BandCombination,                 ENUM-DC_BandCombination_Type,DC_1A_3A #-- @desc  DC band combination applied in DC test cases

px_EllipsoidPointWithAltitude,               OCTETSTRING,   1234560000000000 #-- @desc  Ellipsoid Point With Altitude value to be provided in Update UE location information (see 36.509 cl 6.12)

px_EmergencyCallNumber,                      CHARSTRING,    112     #-- @desc  Emergency Number used by UE to initiate an emergency call

px_FDD_OperationBand,                        INTEGER,       1       #-- @desc  The operation band under test as defined in 34.108 clause 5.1.1. Value 1 means Band 1 2 means Band 2 etc.This pixit shall be set in synchronisation with the values that are being set to 6 other Pixits viz: px_UARFCN_D_High px_UARFCN_D_Midpx_UARFCN_L_Mid

px_HorizontalVelocity,                       OCTETSTRING,   123456  #-- @desc  Horizontal Velocity to be provided in Update UE location information (see 36.509 cl 6.12)

px_IMEISV_Def,                               HEXSTRING,     35578102029156978 #-- @desc  Default IMEISV value.  No default can be proposed as this is a manufacturer defined value

px_IMEI_Def,                                 HEXSTRING,     355781020291569 #-- @desc  Default IMEI value transmitted by UE.  Digit 15 shall be set as a Spare Digit i.e. shall be set to '0' (see TS 23.003)

px_IMSI_Def,                                 HEXSTRING,     001010000000333 #-- @desc  Default IMSI

px_IMS_AssociatedTelUri,                     CHARSTRING,    tel:+4989364072 #-- @desc  Set as record 3 in EFIMPU as defined in TS 34.229-1[5]

px_IMS_CalleeContactUri,                     CHARSTRING,    sip:User-B-Contact@3gpp.org #-- @desc  URI provided by the remote side (i.e. by SS) to be used by the UE as contact address in further SIP signalling of the dialog

px_IMS_CalleeContactUri2,                    CHARSTRING,    sip:User-C-Contact@3gpp.org #-- @desc  URI provided by the remote side (i.e. by SS) to be used by the UE as contact address in further SIP signalling of the dialog

px_IMS_CalleeUri,                            CHARSTRING,    sip:User-B@3gpp.org #-- @desc  URI of Callee sent by the UE in INVITE (MO call establishment) to address the remote UE

px_IMS_CalleeUri2,                           CHARSTRING,    sip:User-C@3gpp.org #-- @desc  URI of Callee sent by the UE in INVITE (MO call establishment) to address the remote UE

px_IMS_CiphAlgo_Def,                         ENUM-IPsec_CipheringAlgorithm_Type,des_ede3_cbc #-- @desc  Ciphering Algorithm

px_IMS_HomeDomainName,                       CHARSTRING,    3gpp.org #-- @desc  Home Domain Name.

px_IMS_HomeDomainName_Refreshed,             CHARSTRING,    refreshed3gpp.org #-- @desc  Used in 8.15

px_IMS_IPSecAlgorithm,                       ENUM-IPsec_IntegrityAlgorithm_Type,hmac_sha_1_96 #-- @desc  Integrity Algorithm

px_IMS_MessageAccountIdentity,               CHARSTRING,    testaccountidentity #-- @desc  message accout identity configured at the UE as used for subscription to message-summary event package

px_IMS_Private_UserId,                       CHARSTRING,    privateuser@3gpp.org #-- @desc  Private User Identity.When usingan ISIM this is set to the same value as EFIMPI.When ISIM is not used just USIM the private user identity is derived from px_IMSI.

px_IMS_Private_UserId_Refreshed,             CHARSTRING,    privateuser@refreshed3gpp.org #-- @desc  Used in 8.15

px_IMS_PublicUserIdentity1,                  CHARSTRING,    sip:PublicId1@3gpp.org #-- @desc  Public User Identity. It is set to the same value as the first record in EFIMPU.

px_IMS_PublicUserIdentity1_Refreshed,        CHARSTRING,    sip:PublicId1@refreshed3gpp.org #-- @desc  Used in 8.15

px_IMS_PublicUserIdentity2,                  CHARSTRING,    sip:PublicId2@3gpp.org #-- @desc  Public User Identity. It is set to the same value as the second record in EFIMPU.

px_IMS_PublicUserIdentity3,                  CHARSTRING,    sip:PublicId3@3gpp.org #-- @desc  Public User Identity. It is set to the same value as the third record in EFIMPU.

px_IMS_SPI_ValidValueList_PDN1,              CHARSTRING,    256,258,264,266 #-- @desc  list of comma separated integer values that can be used as SPI values for IMS security on PDN1; each value shall be greater than or equal to 256

px_IMS_SPI_ValidValueList_PDN2,              CHARSTRING,    260,262,268,270 #-- @desc  list of comma separated integer values that can be used as SPI values for IMS security on PDN2; each value shall be greater than or equal to 256

px_IP_MTU_Size,                              INTEGER,       1300    #-- @desc  MTU size. This value is specific to the SS.

px_IPv4_Address,                             CHARSTRING,    192.168.0.1 #-- @desc  IPv4 Address

px_IPv4_Address1_NW,                         CHARSTRING,    192.168.0.3 #-- @desc  IPv4 Gateway Address in PDN1

px_IPv4_Address1_RemoteUE,                   CHARSTRING,    192.168.0.6 #-- @desc  IPv4 Address of remote UE connected to PDN1

px_IPv4_Address1_UE,                         CHARSTRING,    192.168.0.1 #-- @desc  IPv4 Address connected to PDN1

px_IPv4_Address2,                            CHARSTRING,    192.168.1.2 #-- @desc  2nd IPv4 Address @sic R5s110011 sic@

px_IPv4_Address2_NW,                         CHARSTRING,    192.168.1.4 #-- @desc  IPv4 Gateway Address in PDN2

px_IPv4_Address2_RemoteUE,                   CHARSTRING,    192.168.1.6 #-- @desc  IPv4 Address of remote UE connected to PDN2

px_IPv4_Address2_UE,                         CHARSTRING,    192.168.1.2 #-- @desc  IPv4 Address connected to PDN2

px_IPv4_Address2a_UE,                        CHARSTRING,    192.168.1.3 #-- @desc  IPv4 Address connected to PDN2a

px_IPv4_Address_HomeAgent,                   CHARSTRING,    192.168.0.5 #-- @desc  IPv4 Home Address Agent

px_IPv6_Address,                             CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:1111 #-- @desc  IPv6 Address

px_IPv6_Address1_NW,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:3333 #-- @desc  IPv6 Gateway Address in PDN1

px_IPv6_Address1_RemoteUE,                   CHARSTRING,    FD01:0000:0000:0000:0000:0000:0000:0006 #-- @desc  IPv6 Address of remote UE in PDN1

px_IPv6_Address1_UE,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:1111 #-- @desc  IPv6 Address in PDN1

px_IPv6_Address2,                            CHARSTRING,    1111:2222:3333:5555:5555:6666:7777:2222 #-- @desc  2nd IPv6 Address  @sic R5s110011 sic@

px_IPv6_Address2_NW,                         CHARSTRING,    1111:2222:3333:5555:5555:6666:7777:4444 #-- @desc  IPv6 Gateway Address in PDN2

px_IPv6_Address2_RemoteUE,                   CHARSTRING,    FD01:0000:0000:0000:0000:0000:0000:0006 #-- @desc  IPv6 Address of remote UE in PDN2

px_IPv6_Address2_UE,                         CHARSTRING,    1111:2222:3333:5555:5555:6666:7777:2222 #-- @desc  IPv6 Address in PDN2

px_IPv6_Address2a_UE,                        CHARSTRING,    0001:0002:0003:0004:0005:0006:0007:0008 #-- @desc  IPv6 Address in PDN2a

px_IPv6_Address_BSF,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:3333 #-- @desc  IPv6 BSF address

px_IPv6_Address_HomeAgent,                   CHARSTRING,    0001:0002:0003:0004:0005:0006:0007:5 #-- @desc  IPv6 Home Address Agent

px_MFBI_BandChannelBandwidth,                ENUM-Dl_Bandwidth_Type,n25     #-- @desc  MFBI E-UTRAN Channel Bandwidth

px_MFBI_FrequencyBand,                       INTEGER,       26      #-- @desc  a supported E-UTRA MFBI frequency band

px_MFBI_UTRAN_FrequencyBand,                 INTEGER,       1       #-- @desc  A supported UTRAN MFBI frequency band.

px_NAS_CipheringAlgorithm,                   BITSTRING,     001     #-- @desc  NAS Ciphering Algorithm (eea1)

px_NAS_IntegrityProtAlgorithm,               BITSTRING,     001     #-- @desc  NAS Integrity Algorithm (eia1)

px_NR_CipheringAlgorithm,                    ENUM-CipheringAlgorithm,nea2    #-- @desc  Ciphering Algorithm

px_NR_IntegrityProtAlgorithm,                ENUM-IntegrityProtAlgorithm,nia2    #-- @desc  Integrity Algorithm

px_NR_PrimaryBand,                           INTEGER,       78      #-- @desc  NR primary band

px_NR_SecondaryBand,                         INTEGER,       2       #-- @desc  NR secondary band

px_NoTDD_LCR_onLTE,                          BOOLEAN,       false   #-- @desc  Only applicable to UE supporting (at least) LTE and LCR TDD.  If set to true the UE is configured not to report support of LCR TDD (IE utraTDD128 in UECapabilityInformation) when being camped on an LTE cell with no detectable LCR TDD cell in the environment.

px_OverlappingNotSupportedFrequencyBand_MFBI,INTEGER,       27      #-- @desc  a not supported E-UTRA frequency band that is overlapping with a supported MFBI band

px_OverlappingSupportedFrequencyBand_MFBI,   INTEGER,       26      #-- @desc  a supported E-UTRA frequency band overlapping withpx_OverlappingNotSupportedFrequencyBand_MFBI applied to MFBI enhancement test case scenario.

px_PTMSI_Def,                                OCTETSTRING,   C2345678 #-- @desc  Default PTMSI

px_PTMSI_SigDef,                             OCTETSTRING,   AB1234  #-- @desc  Default PTMSI signature (3 octets 3GPP 24.008   10.5.5.8).

px_PWS_CB_DataCodingScheme,                  BITSTRING,     00000000000000010000001000000011000001000000010100000110000001110000100000001001000010100000101100001100000011010000111000001111 #-- @desc  CMAS or ETWS data coding scheme of the alphabetcodingand the applied language (see TS 23.401)

px_PWS_CB_DataPage1,                         CHARSTRING,    warning #-- @desc  ETWS or CMAS Page 1 warning data message

px_PWS_CB_DataPage2,                         CHARSTRING,    warning #-- @desc  ETWS or CMAS Page 2 warning data message

px_PWS_CB_DataPage3,                         CHARSTRING,    warning #-- @desc  CMAS or ETWS Page 3 warning data message

px_PWS_CB_DataPage4,                         CHARSTRING,    warning #-- @desc  CMAS or ETWS Page 4 warning data message

px_RATComb_Tested,                           ENUM-RATComb_Tested_Type,EUTRA_UTRA #-- @desc  This parameter represents the network RAT capabilitypreference and indicates which if any is supported RAT combination is to be tested

px_RRC_CipheringAlgorithm,                   CHARSTRING,    eea1    #-- @desc  Ciphering Algorithm

px_RRC_CipheringAlgorithm_r12,               ENUM-CipheringAlgorithm_r12,eea1    #-- @desc  Ciphering Algorithm

px_RRC_IntegrityProtAlgorithm,               ENUM-IntegrityProtAlgorithm_Type,eia1    #-- @desc  Integrity Algorithm

px_Release_check_in_eMBMS_TCs,               BOOLEAN,       true    #-- Anritsu TTCN WA for release check in MBMS

px_SMSTransport_CP_CIoT,                     BOOLEAN,       false   #-- @desc  NB-IoT UE configured to utilise the SMS service as transport mechanism for user data for Control Plane CIoT Optimisation

px_SMS_ChkMsgReceived,                       BOOLEAN,       true    #-- @desc  Whether the operator can check an MT Short Message received

px_SMS_IndexOffset,                          INTEGER,       0       #-- @desc  Memory location index at UE for SMS storage used in +CMSS command

px_SMS_MsgFrmt,                              CHARSTRING,    1       #-- @desc  SMS message format <mode> (see TS 27.005 cl.3.2.). NOTE: Default value is for text mode. Change value to 0 to execute tests with PDU mode

px_SMS_PrefMem1,                             CHARSTRING,    SM      #-- @desc  SMS Preferred Memory 1 <mem1> of TS 27.005 [31] clause 3.2.2

px_SMS_PrefMem2,                             CHARSTRING,    SM      #-- @desc  SMS Preferred Memory 2 <mem2> of TS 27.005 [31] clause 3.2.2

px_SMS_PrefMem3,                             CHARSTRING,    MT      #-- @desc  SMS Preferred Memory 3 <mem3> of TS 27.005 [31] clause 3.2.2

px_SMS_SMSC_InternationalNumber,             CHARSTRING,    112233445566778 #-- @desc  international number of the SMSC:

px_SMS_Service,                              CHARSTRING,    0       #-- @desc  SMS Service <service> of TS 27.005 [31] clause 3.2.1

px_SPI_pc,                                   INTEGER,       5000    #-- Anritsu TTCN WA for SPI

px_SPI_ps,                                   INTEGER,       1000    #-- Anritsu TTCN WA for SPI

px_SinglePLMN_Tested,                        ENUM-SinglePLMN_TestedType,MultiPLMN #-- @desc  This parameter represents the network capabilitypreference to support multi PLMNs on the same test Band and indicates the preference of multi PLMNs or single PLMN test environment. This PIXIT shall be set to SinglePLMN when only one frequency is defined for the test band

px_StartStop,                                BOOLEAN,       TRUE    #-- Anritsu TTCN WA for Automation EnableDisable

px_StartString,                              CHARSTRING,    StartTest: #-- Anritsu TTCN WA for Automation Starting test cases string e.g.: StartTest:TC_7_1_2_1

px_StopString,                               CHARSTRING,    EndTest: #-- Anritsu TTCN WA for Automation Stopping test cases string e.g.: StopTest:Passed

px_TMSI_Def,                                 OCTETSTRING,   11223344 #-- @desc  Default TMSI

px_TestLoopModeB_Delay,                      OCTETSTRING,   5A      #-- @desc  This parameter represents the IP PDU delay to be used for UE test loop mode B intest cases where long delay may be needed e.g. because of user interaction.

px_UE_CS_PS_UsageSetting_Tested,             ENUM-CS_PS_MODE,VOICE_CENTRIC #-- @desc  specifies which CSPS mode is under test @sic R5s120274 sic@

px_UE_PS_UsageSetting_Tested,                ENUM-PS_MODE,  VOICE_CENTRIC #-- @desc  specifies which PS mode is under test @sic R5s120274 sic@

px_UEwithISIM,                               BOOLEAN,       true    #-- @desc  true - UE has ISIM; false - UE has USIM only

px_UTRAN_ModeUnderTest,                      ENUM-UTRAN_FDD_TDD_Type,UTRAN_FDD #-- @desc  specifies which radio access technology is being tested in UTRAN

px_UTRAN_OverlappingNotSupportedFrequencyBandMFBI,INTEGER,       1       #-- @desc  A not supported UTRAN frequency band that is overlapping with a supported MFBI band (px_MFBI_UTRAN_FrequencyBand). This pixit shall be set also in accordance with the values of the 3 Pixits: px_UARFCN_D_High px_UARFCN_D_Midpx_UARFCN_L_Mid.

px_WLAN_PDN1_ToOffload,                      BOOLEAN,       true    #-- @desc  If set to true the first PDN connection is offloaded to WLAN. If set to false the second PDN connection is offloaded to WLAN.

px_XCAP_RootUri,                             CHARSTRING,    /XCAP.3gpp.org #-- @desc  XCAP Root URI

px_XCAP_TargetUri,                           CHARSTRING,    sip:user@domain.com #-- @desc  Target (SIP or TEL URI) where to forward to

px_XCAP_Username,                            CHARSTRING,    0       #-- @desc  username to be used for HTTP authentication in case of pc_XCAP_UsernameIsConfiguredInUE==true

px_eAuthRAND,                                BITSTRING,     10100011110111100000110001101101001101100011111000110000110000110110010010100100000001111000111100011011111110001101010101110111 #-- @desc  Random Challenge

px_eJapanMCC_Band6,                          HEXSTRING,     442     #-- @desc  Japan MCC code to be used for Band 6. The same value will be used for E-UTRAN and Inter-RAT cells. Type is different to that defined in 34.123-3.

px_eMaxNumberROHC_ContextSessions,           ENUM-MaxNumberROHC_ContextSessions_Type,cs16    #-- @desc  Maximum number of ROHC context sessions @sic R5s130329 sic@

px_ePrimaryBandChannelBandwidth,             ENUM-Dl_Bandwidth_Type,n25     #-- @desc  Channel bandwidth used on px_ePrimaryFrequencyBand

px_ePrimaryFrequencyBand,                    INTEGER,       1       #-- @desc  E-UTRAN primary frequency band

px_eSecondaryBandChannelBandwidth,           ENUM-Dl_Bandwidth_Type,n25     #-- @desc  Channel bandwidth used on px_eSecondaryFrequencyBand

px_eSecondaryFrequencyBand,                  INTEGER,       5       #-- @desc  E-UTRAN secondary frequency band

px_eTDDsubframeConfig,                       ENUM-TDD_SubframeAssignment_Type,sa1     #-- @desc  TDD uplink-downlink subframe configuration

px_nPrimaryFrequencyBand,                    INTEGER,       78      #-- @desc  NR primary frequency band

px_nonSMSTransport_CP_CIoT,                  BOOLEAN,       false   #-- @desc  NB-IoT UE configured to utilise non-SMS services as transport mechanism for user data for Control Plane CIoT Optimisation

