    Log Viewer 341.0.0.0
    Copyright © 2019, Keysight Technologies

    LogFile            : TC_7_1_3_2_2_20191127_102202_n41_PASS.alf
    Created            : 29/11/2019 16:46:55

| Details | Summary

    OperatorName = admin

    admin

    iutData = Manufacturer =
    Model =
    Hardware Version =
    Software Version =
    Serial Number =

    Manufacturer =
    Model =
    Hardware Version =
    Software Version =
    Serial Number =

    swName = Conformance Toolset (LTE)
    swVersion = Version 53.0 (0480)
    swDetails

    Conformance Toolset (LTE)

    swName = TTCN-3 Compiler
    swVersion = Version 5.3  p0, Compile Date 2019-08-20 16:23:42
    swDetails

    TTCN-3 Compiler

    swName = Anite IMS Enabler
    swVersion = Not Installed
    swDetails

    Anite IMS Enabler

    swName = Conformance Toolset (LTE): Common Library
    swVersion = Version 53.0 (0480), Compile Date: Nov 27 2019 09:58:08
    swDetails

    Conformance Toolset (LTE): Common Library

    swName = Conformance Toolset (LTE): Codec Library
    swVersion = Version 53.0 (0480), Compile Date: Nov 27 2019 09:57:45
    swDetails

    Conformance Toolset (LTE): Codec Library

    swName = Conformance Toolset (LTE): Logging Library
    swVersion = Version 53.0 (0480), Compile Date: Nov 27 2019 09:57:28
    swDetails

    Conformance Toolset (LTE): Logging Library

    swName = Conformance Toolset (LTE): Test Management Library
    swVersion = Version 53.0 (0480), Compile Date: Nov 27 2019 09:57:18
    swDetails

    Conformance Toolset (LTE): Test Management Library

    swName = Conformance Toolset (LTE): Platform Timer Library
    swVersion = Version 53.0 (0480), Compile Date: Nov 27 2019 09:57:44
    swDetails

    Conformance Toolset (LTE): Platform Timer Library

    swName = Conformance Toolset (LTE): System Adaptor Library
    swVersion = Version 53.0 (0480), Compile Date: Nov 27 2019 09:57:42
    swDetails

    Conformance Toolset (LTE): System Adaptor Library

    swName = Conformance Toolset (LTE): LTE Codec Library
    swVersion = Version 53.0 (0480), Compile Date: Nov 27 2019 09:57:10
    swDetails

    Conformance Toolset (LTE): LTE Codec Library

    swName = Conformance Toolset (LTE): LTE System Adaptor Library
    swVersion = Version 53.0 (0480), Compile Date: Nov 27 2019 09:57:14
    swDetails

    Conformance Toolset (LTE): LTE System Adaptor Library

    swName = Conformance Toolset (LTE): LTE External Function Library
    swVersion = Version 53.0 (0480), Compile Date: Nov 27 2019 09:56:10
    swDetails

    Conformance Toolset (LTE): LTE External Function Library

    recordType = 31
    fileName
    descriptionId
    lineNo = 0
    information = This log file was produced by a test case that is NOT validated and the test results are not verified to be suitable for certification testing.

    This log file was produced by a test case that is NOT validated and the test results are not verified to be suitable for certification testing.

    recordType = 22
    fileName
    descriptionId
    lineNo = 0
    information = TTCN-3 Ctrl File              : C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\NR5GC_Testsuite.ttcn

    TTCN-3 Ctrl File              : C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\NR5GC_Testsuite.ttcn

    recordType = 22
    fileName
    descriptionId
    lineNo = 0
    information = XML Parameter File            : C:\Keysight\CT\TestProjects\LJ_Halo\sa\2019-11-27 10.21.59\TC_7_1_3_2_2_20191127_102202_n41_%V.xml

    XML Parameter File            : C:\Keysight\CT\TestProjects\LJ_Halo\sa\2019-11-27 10.21.59\TC_7_1_3_2_2_20191127_102202_n41_%V.xml

    recordType = 22
    fileName
    descriptionId
    lineNo = 0
    information = Test Case Started By          : CT_PSCS.DLL v1,0,3324,823

    Test Case Started By          : CT_PSCS.DLL v1,0,3324,823

    recordType = 22
    fileName
    descriptionId
    lineNo = 0
    information = EMMI Automation               : AT Disabled, MMI Disabled

    EMMI Automation               : AT Disabled, MMI Disabled

    recordType = 22
    fileName = NR5GC_Testsuite
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 86
    text = ----------------------------------------------------------------------------------------------------

    ----------------------------------------------------------------------------------------------------

    recordType = 22
    fileName = NR5GC_Testsuite
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 87
    text = Test case started             : TC_7_1_3_2_2_NR5GC

    Test case started             : TC_7_1_3_2_2_NR5GC

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 72
    text = Mapping port "MTC_NR5GC:Ut" to port "SYSTEM_NR5GC:Ut"

    Mapping port "MTC_NR5GC:Ut" to port "SYSTEM_NR5GC:Ut"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\NR\NR_Component_Base.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 173
    text = Mapping port "NR5GC_PTC:SYS" to port "SYSTEM_NR5GC:NR_SYS"

    Mapping port "NR5GC_PTC:SYS" to port "SYSTEM_NR5GC:NR_SYS"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\NR\NR_Component_Base.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 174
    text = Mapping port "NR5GC_PTC:SYSIND" to port "SYSTEM_NR5GC:NR_SYSIND"

    Mapping port "NR5GC_PTC:SYSIND" to port "SYSTEM_NR5GC:NR_SYSIND"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\NR\NR_Component_Base.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 175
    text = Mapping port "NR5GC_PTC:DRB" to port "SYSTEM_NR5GC:NR_DRB"

    Mapping port "NR5GC_PTC:DRB" to port "SYSTEM_NR5GC:NR_DRB"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\NasEmulation\NasEmu5G_Component_NRNG.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 39
    text = Connecting port "NR5GC_PTC:NASCTRL" to port "NASEMU_NRNG_PTC:CTRL"

    Connecting port "NR5GC_PTC:NASCTRL" to port "NASEMU_NRNG_PTC:CTRL"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\NasEmulation\NasEmu5G_Component_NRNG.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 39
    text = Connecting port "NR5GC_PTC:SRB" to port "NASEMU_NRNG_PTC:TC_SRB"

    Connecting port "NR5GC_PTC:SRB" to port "NASEMU_NRNG_PTC:TC_SRB"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\NasEmulation\NasEmu5G_Component_NRNG.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 46
    text = Mapping port "NASEMU_NRNG_PTC:SYS_SRB" to port "SYSTEM_NR5GC:NR_SRB"

    Mapping port "NASEMU_NRNG_PTC:SYS_SRB" to port "SYSTEM_NR5GC:NR_SRB"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\IP_PTC\IP_PTC_Component.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 264
    text = Mapping port "IP_PTC:IP_CTRL" to port "SYSTEM_NR5GC:IP_CTRL"

    Mapping port "IP_PTC:IP_CTRL" to port "SYSTEM_NR5GC:IP_CTRL"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\IP_PTC\IP_PTC_Component.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 265
    text = Mapping port "IP_PTC:IPSEC_CTRL" to port "SYSTEM_NR5GC:IPSEC_CTRL"

    Mapping port "IP_PTC:IPSEC_CTRL" to port "SYSTEM_NR5GC:IPSEC_CTRL"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\IP_PTC\IP_PTC_Component.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 266
    text = Mapping port "IPMUX_PTC:IP_SOCK" to port "SYSTEM_NR5GC:IP_SOCK"

    Mapping port "IPMUX_PTC:IP_SOCK" to port "SYSTEM_NR5GC:IP_SOCK"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\IP_PTC\IP_PTC_Component.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 266
    text = Connecting port "IP_PTC:IP_SOCK_DATA" to port "IPMUX_PTC:IP_SOCK_DATA"

    Connecting port "IP_PTC:IP_SOCK_DATA" to port "IPMUX_PTC:IP_SOCK_DATA"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\IP_PTC\IP_PTC_Component.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 266
    text = Connecting port "IP_PTC:IP_SOCK_CTRL" to port "IPMUX_PTC:IP_SOCK_CTRL"

    Connecting port "IP_PTC:IP_SOCK_CTRL" to port "IPMUX_PTC:IP_SOCK_CTRL"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\NR5GC\Common\MTC_Main_NR5GC.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 61
    text = Connecting port "NR5GC_PTC:IP" to port "IP_PTC:NR_CTRL"

    Connecting port "NR5GC_PTC:IP" to port "IP_PTC:NR_CTRL"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\NR5GC\Common\MTC_Main_NR5GC.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 67
    text = Connecting port "IMS_PTC:IMS_CTRL" to port "IP_PTC:IMS_CTRL"

    Connecting port "IMS_PTC:IMS_CTRL" to port "IP_PTC:IMS_CTRL"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\NR5GC\Common\MTC_Main_NR5GC.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 67
    text = Connecting port "IMS_PTC:IMS_Server" to port "IP_PTC:IMS_Server"

    Connecting port "IMS_PTC:IMS_Server" to port "IP_PTC:IMS_Server"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\NR5GC\Common\MTC_Main_NR5GC.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 67
    text = Connecting port "IMS_PTC:IMS_Client" to port "IP_PTC:IMS_Client"

    Connecting port "IMS_PTC:IMS_Client" to port "IP_PTC:IMS_Client"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\NR5GC\Common\MTC_Main_NR5GC.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 67
    text = Connecting port "IMS_PTC:MMI" to port "MTC_NR5GC:PTC_Ut"

    Connecting port "IMS_PTC:MMI" to port "MTC_NR5GC:PTC_Ut"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\NR5GC\Common\MTC_Main_NR5GC.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 67
    text = Connecting port "IMS_PTC:IPCAN" to port "NR5GC_PTC:IMS"

    Connecting port "IMS_PTC:IPCAN" to port "NR5GC_PTC:IMS"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\NR5GC\Common\MTC_Main_NR5GC.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 82
    text = Connecting port "MTC_NR5GC:PTC_Ut" to port "NR5GC_PTC:UT"

    Connecting port "MTC_NR5GC:PTC_Ut" to port "NR5GC_PTC:UT"

    summary = Message Mismatch: IPCAN_RAN_Type
    MATCH_MISMATCH
    	Message Mismatch: IPCAN_RAN_Type
    		IPCAN_RAN_Type = FBBA (6)

    Message Mismatch: IPCAN_RAN_Type

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 2031
    text = Parameter: IMS_Component.vc_IMS_Global.Ctrl.TestBody = False

    Parameter: IMS_Component.vc_IMS_Global.Ctrl.TestBody = False

    UT_SYSTEM_REQ
    	Cmd
    		MMI
    			Cmd = 'POWER_OFF'
    			ParameterList = Omit
    	CnfRequired = CNF_REQUIRED (1)

    Sent from port: MTC_NR5GC:Ut

    UT_COMMON_CNF
    	Result = True
    	ResultString = ''

    Received on port: MTC_NR5GC:Ut

    timerEvent = 6
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\NR5GC_Testsuite.ttcn
    testName = TC_7_1_3_2_2_NR5GC
    lineNo = 1616
    outStr = Timer: t_GuardTimer, Duration: 300s, Started: 10:22:35

    Timer: t_GuardTimer, Duration: 300s, Started: 10:22:35

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\NR\NR_CellInfoInit.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 221
    text = Parameter: NR_Component_Base.vc_NR_Global.Ctrl.TestBody = False

    Parameter: NR_Component_Base.vc_NR_Global.Ctrl.TestBody = False

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 3

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 1

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 3

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 1

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 3

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 1

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 3

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 1

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 3

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 1

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 3

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 1

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 3

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 1

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 3

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 1

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 3

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 1

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 3

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 1

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 3

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 1

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 3

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 1

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 3

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 1

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 3

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 1

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 2
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 2
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 1

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 2
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 3

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 3

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 1

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: PDSCH_Config___6
    MATCH_MISMATCH
    	Message Mismatch: PDSCH_Config___6
    		PDSCH_Config___6 = resourceAllocationType0 (0)
    ConstraintMismatch::Expected:
    summary = Message Mismatch: PDSCH_Config___6
    MATCH_MISMATCH
    	Message Mismatch: PDSCH_Config___6
    		resourceAllocation = resourceAllocationType1 (1)

    Message Mismatch: PDSCH_Config___6

    ConstraintMismatch::Received:
    summary = Message Mismatch: PDSCH_Config___14
    MATCH_MISMATCH
    	Message Mismatch: PDSCH_Config___14
    		PDSCH_Config___14 = qam256 (0)
    ConstraintMismatch::Expected:
    summary = Message Mismatch: PDSCH_Config___14
    MATCH_MISMATCH
    	Message Mismatch: PDSCH_Config___14
    		mcs_Table = Omit

    Message Mismatch: PDSCH_Config___14

    ConstraintMismatch::Received:
    summary = Message Mismatch: PUSCH_Config___7
    MATCH_MISMATCH
    	Message Mismatch: PUSCH_Config___7
    		PUSCH_Config___7 = resourceAllocationType0 (0)
    ConstraintMismatch::Expected:
    summary = Message Mismatch: PUSCH_Config___7
    MATCH_MISMATCH
    	Message Mismatch: PUSCH_Config___7
    		resourceAllocation = resourceAllocationType1 (1)

    Message Mismatch: PUSCH_Config___7

    BCCH-BCH-Message
    	message = mib =
    		systemFrameNumber = 000000
    		subCarrierSpacingCommon = scs30or120
    		ssb-SubcarrierOffset = 10
    		dmrs-TypeA-Position = pos2
    		pdcch-ConfigSIB1
    			controlResourceSetZero = 1
    			searchSpaceZero = 0
    		cellBarred = notBarred
    		intraFreqReselection = allowed
    		spare = 0

    mib

    BCCH-DL-SCH-Message
    	message = c1 = systemInformationBlockType1 =
    		cellSelectionInfo
    			q-RxLevMin = -55
    		cellAccessRelatedInfo
    			plmn-IdentityList = SEQUENCE OF PLMN-IdentityInfo
    				PLMN-IdentityInfo(1)
    					plmn-IdentityList = SEQUENCE OF PLMN-Identity
    						PLMN-Identity(1)
    							mcc = SEQUENCE OF MCC-MNC-Digit
    								MCC-MNC-Digit(1) = 0
    								MCC-MNC-Digit(2) = 0
    								MCC-MNC-Digit(3) = 1
    							mnc = SEQUENCE OF MCC-MNC-Digit
    								MCC-MNC-Digit(1) = 0
    								MCC-MNC-Digit(2) = 1
    					trackingAreaCode = 000000000000000000000001
    					ranac = 1
    					cellIdentity = 000000000000000000000000010000000000
    					cellReservedForOperatorUse = notReserved
    		connEstFailureControl
    			connEstFailCount = n1
    			connEstFailOffsetValidity = s30
    			connEstFailOffset = 1
    		servingCellConfigCommon
    			downlinkConfigCommon
    				frequencyInfoDL
    					frequencyBandList = SEQUENCE OF NR-MultiBandInfo
    						NR-MultiBandInfo(1)
    							freqBandIndicatorNR = 41
    							nr-NS-PmaxList = SEQUENCE OF NR-NS-PmaxValue
    								NR-NS-PmaxValue(1)
    									additionalPmax = 20
    									additionalSpectrumEmission = 0
    					offsetToPointA = 2
    					scs-SpecificCarrierList = SEQUENCE OF SCS-SpecificCarrier
    						SCS-SpecificCarrier(1)
    							offsetToCarrier = 0
    							subcarrierSpacing = kHz30
    							carrierBandwidth = 162
    				initialDownlinkBWP
    					genericParameters
    						locationAndBandwidth = 31624
    						subcarrierSpacing = kHz30
    					pdcch-ConfigCommon = setup =
    						controlResourceSetZero = 1
    						commonControlResourceSet
    							controlResourceSetId = 1
    							frequencyDomainResources = 111100000000000000000000000000000000000000000
    							duration = 2
    							cce-REG-MappingType = nonInterleaved = NULL
    							precoderGranularity = sameAsREG-bundle
    						searchSpaceZero = 0
    						commonSearchSpaceList = SEQUENCE OF SearchSpace
    							SearchSpace(1)
    								searchSpaceId = 1
    								controlResourceSetId = 1
    								monitoringSlotPeriodicityAndOffset = sl1 = NULL
    								monitoringSymbolsWithinSlot = 10000000000000
    								nrofCandidates
    									aggregationLevel1 = n0
    									aggregationLevel2 = n4
    									aggregationLevel4 = n2
    									aggregationLevel8 = n2
    									aggregationLevel16 = n0
    								searchSpaceType = common =
    									dci-Format0-0-AndFormat1-0
    							SearchSpace(2)
    								searchSpaceId = 3
    								controlResourceSetId = 1
    								monitoringSlotPeriodicityAndOffset = sl10 = 5
    								duration = 2
    								monitoringSymbolsWithinSlot = 10000000000000
    								nrofCandidates
    									aggregationLevel1 = n0
    									aggregationLevel2 = n4
    									aggregationLevel4 = n2
    									aggregationLevel8 = n2
    									aggregationLevel16 = n0
    								searchSpaceType = common =
    									dci-Format0-0-AndFormat1-0
    						searchSpaceSIB1 = 0
    						searchSpaceOtherSystemInformation = 3
    						pagingSearchSpace = 0
    						ra-SearchSpace = 1
    					pdsch-ConfigCommon = setup =
    						pdsch-TimeDomainAllocationList = SEQUENCE OF PDSCH-TimeDomainResourceAllocation
    							PDSCH-TimeDomainResourceAllocation(1)
    								mappingType = typeA
    								startSymbolAndLength = 53
    							PDSCH-TimeDomainResourceAllocation(2)
    								mappingType = typeA
    								startSymbolAndLength = 72
    				bcch-Config
    					modificationPeriodCoeff = n4
    				pcch-Config
    					defaultPagingCycle = rf128
    					nAndPagingFrameOffset = halfT = 1
    					ns = one
    			uplinkConfigCommon
    				frequencyInfoUL
    					scs-SpecificCarrierList = SEQUENCE OF SCS-SpecificCarrier
    						SCS-SpecificCarrier(1)
    							offsetToCarrier = 0
    							subcarrierSpacing = kHz30
    							carrierBandwidth = 162
    					p-Max = 20
    				initialUplinkBWP
    					genericParameters
    						locationAndBandwidth = 31624
    						subcarrierSpacing = kHz30
    					rach-ConfigCommon = setup =
    						rach-ConfigGeneric
    							prach-ConfigurationIndex = 160
    							msg1-FDM = four
    							msg1-FrequencyStart = 0
    							zeroCorrelationZoneConfig = 15
    							preambleReceivedTargetPower = -118
    							preambleTransMax = n7
    							powerRampingStep = dB4
    							ra-ResponseWindow = sl20
    						ssb-perRACH-OccasionAndCB-PreamblesPerSSB = one = n8
    						ra-ContentionResolutionTimer = sf64
    						rsrp-ThresholdSSB = 0
    						prach-RootSequenceIndex = l139 = 0
    						msg1-SubcarrierSpacing = kHz30
    						restrictedSetConfig = unrestrictedSet
    					pusch-ConfigCommon = setup =
    						pusch-TimeDomainAllocationList = SEQUENCE OF PUSCH-TimeDomainResourceAllocation
    							PUSCH-TimeDomainResourceAllocation(1)
    								k2 = 4
    								mappingType = typeA
    								startSymbolAndLength = 27
    							PUSCH-TimeDomainResourceAllocation(2)
    								k2 = 6
    								mappingType = typeA
    								startSymbolAndLength = 27
    						msg3-DeltaPreamble = 1
    						p0-NominalWithGrant = -90
    					pucch-ConfigCommon = setup =
    						pucch-ResourceCommon = 0
    						pucch-GroupHopping = enable
    						p0-nominal = -90
    				timeAlignmentTimerCommon = infinity
    			ssb-PositionsInBurst
    				inOneGroup = 01000000
    			ssb-PeriodicityServingCell = ms20
    			tdd-UL-DL-ConfigurationCommon
    				referenceSubcarrierSpacing = kHz30
    				pattern1
    					dl-UL-TransmissionPeriodicity = ms5
    					nrofDownlinkSlots = 7
    					nrofDownlinkSymbols = 6
    					nrofUplinkSlots = 2
    					nrofUplinkSymbols = 4
    			ss-PBCH-BlockPower = 0
    		ue-TimersAndConstants
    			t300 = ms1000
    			t301 = ms1000
    			t310 = ms1000
    			n310 = n1
    			t311 = ms30000
    			n311 = n1
    			t319 = ms1000

    systemInformationBlockType1

    DL-CCCH-Message
    	message = c1 = rrcSetup =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcSetup =
    			radioBearerConfig
    				srb-ToAddModList = SEQUENCE OF SRB-ToAddMod
    					SRB-ToAddMod(1)
    						srb-Identity = 1
    			masterCellGroup = CONTAINING =
    				cellGroupId = 0
    				rlc-BearerToAddModList = SEQUENCE OF RLC-BearerConfig
    					RLC-BearerConfig(1)
    						logicalChannelIdentity = 1
    						servedRadioBearer = srb-Identity = 1
    						mac-LogicalChannelConfig
    							ul-SpecificParameters
    								priority = 1
    								prioritisedBitRate = infinity
    								bucketSizeDuration = ms50
    								logicalChannelGroup = 0
    								schedulingRequestID = 0
    								logicalChannelSR-Mask = FALSE
    								logicalChannelSR-DelayTimerApplied = FALSE
    				mac-CellGroupConfig
    					schedulingRequestConfig
    						schedulingRequestToAddModList = SEQUENCE OF SchedulingRequestToAddMod
    							SchedulingRequestToAddMod(1)
    								schedulingRequestId = 0
    								sr-TransMax = n16
    					bsr-Config
    						periodicBSR-Timer = infinity
    						retxBSR-Timer = sf10240
    					tag-Config
    						tag-ToAddModList = SEQUENCE OF TAG
    							TAG(1)
    								tag-Id = 0
    								timeAlignmentTimer = infinity
    					phr-Config = release = NULL
    					skipUplinkTxDynamic = FALSE
    				physicalCellGroupConfig
    					p-NR-FR1 = 20
    					pdsch-HARQ-ACK-Codebook = dynamic
    				spCellConfig
    					rlf-TimersAndConstants = setup =
    						t310 = ms1000
    						n310 = n1
    						n311 = n1
    					spCellConfigDedicated
    						initialDownlinkBWP
    							pdcch-Config = setup =
    								searchSpacesToAddModList = SEQUENCE OF SearchSpace
    									SearchSpace(1)
    										searchSpaceId = 2
    										controlResourceSetId = 1
    										monitoringSlotPeriodicityAndOffset = sl1 = NULL
    										monitoringSymbolsWithinSlot = 10000000000000
    										nrofCandidates
    											aggregationLevel1 = n0
    											aggregationLevel2 = n4
    											aggregationLevel4 = n2
    											aggregationLevel8 = n2
    											aggregationLevel16 = n0
    										searchSpaceType = ue-Specific =
    											dci-Formats = formats0-1-And-1-1
    							pdsch-Config = setup =
    								dataScramblingIdentityPDSCH = 0
    								dmrs-DownlinkForPDSCH-MappingTypeA = setup =
    									dmrs-AdditionalPosition = pos1
    								tci-StatesToAddModList = SEQUENCE OF TCI-State
    									TCI-State(1)
    										tci-StateId = 0
    										qcl-Type1
    											referenceSignal = ssb = 1
    											qcl-Type = typeD
    								resourceAllocation = resourceAllocationType1
    								rbg-Size = config1
    								prb-BundlingType = staticBundling =
    									bundleSize = wideband
    						firstActiveDownlinkBWP-Id = 0
    						defaultDownlinkBWP-Id = 0
    						uplinkConfig
    							initialUplinkBWP
    								pucch-Config = setup =
    									resourceSetToAddModList = SEQUENCE OF PUCCH-ResourceSet
    										PUCCH-ResourceSet(1)
    											pucch-ResourceSetId = 0
    											resourceList = SEQUENCE OF PUCCH-ResourceId
    												PUCCH-ResourceId(1) = 0
    												PUCCH-ResourceId(2) = 1
    												PUCCH-ResourceId(3) = 2
    												PUCCH-ResourceId(4) = 3
    												PUCCH-ResourceId(5) = 4
    												PUCCH-ResourceId(6) = 5
    												PUCCH-ResourceId(7) = 6
    												PUCCH-ResourceId(8) = 7
    										PUCCH-ResourceSet(2)
    											pucch-ResourceSetId = 1
    											resourceList = SEQUENCE OF PUCCH-ResourceId
    												PUCCH-ResourceId(1) = 8
    												PUCCH-ResourceId(2) = 9
    												PUCCH-ResourceId(3) = 10
    												PUCCH-ResourceId(4) = 11
    												PUCCH-ResourceId(5) = 12
    												PUCCH-ResourceId(6) = 13
    												PUCCH-ResourceId(7) = 14
    												PUCCH-ResourceId(8) = 15
    											maxPayloadMinus1 = 256
    										PUCCH-ResourceSet(3)
    											pucch-ResourceSetId = 2
    											resourceList = SEQUENCE OF PUCCH-ResourceId
    												PUCCH-ResourceId(1) = 8
    												PUCCH-ResourceId(2) = 9
    												PUCCH-ResourceId(3) = 10
    												PUCCH-ResourceId(4) = 11
    												PUCCH-ResourceId(5) = 12
    												PUCCH-ResourceId(6) = 13
    												PUCCH-ResourceId(7) = 14
    												PUCCH-ResourceId(8) = 15
    											maxPayloadMinus1 = 256
    										PUCCH-ResourceSet(4)
    											pucch-ResourceSetId = 3
    											resourceList = SEQUENCE OF PUCCH-ResourceId
    												PUCCH-ResourceId(1) = 8
    												PUCCH-ResourceId(2) = 9
    												PUCCH-ResourceId(3) = 10
    												PUCCH-ResourceId(4) = 11
    												PUCCH-ResourceId(5) = 12
    												PUCCH-ResourceId(6) = 13
    												PUCCH-ResourceId(7) = 14
    												PUCCH-ResourceId(8) = 15
    									resourceToAddModList = SEQUENCE OF PUCCH-Resource
    										PUCCH-Resource(1)
    											pucch-ResourceId = 0
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 0
    											format = format0 =
    												initialCyclicShift = 0
    												nrofSymbols = 2
    												startingSymbolIndex = 0
    										PUCCH-Resource(2)
    											pucch-ResourceId = 1
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 0
    											format = format0 =
    												initialCyclicShift = 0
    												nrofSymbols = 2
    												startingSymbolIndex = 2
    										PUCCH-Resource(3)
    											pucch-ResourceId = 2
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 0
    											format = format0 =
    												initialCyclicShift = 0
    												nrofSymbols = 2
    												startingSymbolIndex = 4
    										PUCCH-Resource(4)
    											pucch-ResourceId = 3
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 0
    											format = format0 =
    												initialCyclicShift = 0
    												nrofSymbols = 2
    												startingSymbolIndex = 6
    										PUCCH-Resource(5)
    											pucch-ResourceId = 4
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 0
    											format = format0 =
    												initialCyclicShift = 0
    												nrofSymbols = 2
    												startingSymbolIndex = 8
    										PUCCH-Resource(6)
    											pucch-ResourceId = 5
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 0
    											format = format0 =
    												initialCyclicShift = 0
    												nrofSymbols = 2
    												startingSymbolIndex = 10
    										PUCCH-Resource(7)
    											pucch-ResourceId = 6
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 0
    											format = format0 =
    												initialCyclicShift = 0
    												nrofSymbols = 2
    												startingSymbolIndex = 12
    										PUCCH-Resource(8)
    											pucch-ResourceId = 7
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 0
    											format = format1 =
    												initialCyclicShift = 0
    												nrofSymbols = 14
    												startingSymbolIndex = 0
    												timeDomainOCC = 0
    										PUCCH-Resource(9)
    											pucch-ResourceId = 8
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 0
    											format = format2 =
    												nrofPRBs = 6
    												nrofSymbols = 2
    												startingSymbolIndex = 0
    										PUCCH-Resource(10)
    											pucch-ResourceId = 9
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 0
    											format = format2 =
    												nrofPRBs = 6
    												nrofSymbols = 2
    												startingSymbolIndex = 2
    										PUCCH-Resource(11)
    											pucch-ResourceId = 10
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 0
    											format = format2 =
    												nrofPRBs = 6
    												nrofSymbols = 2
    												startingSymbolIndex = 4
    										PUCCH-Resource(12)
    											pucch-ResourceId = 11
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 0
    											format = format2 =
    												nrofPRBs = 6
    												nrofSymbols = 2
    												startingSymbolIndex = 6
    										PUCCH-Resource(13)
    											pucch-ResourceId = 12
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 0
    											format = format2 =
    												nrofPRBs = 6
    												nrofSymbols = 2
    												startingSymbolIndex = 8
    										PUCCH-Resource(14)
    											pucch-ResourceId = 13
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 0
    											format = format2 =
    												nrofPRBs = 6
    												nrofSymbols = 2
    												startingSymbolIndex = 10
    										PUCCH-Resource(15)
    											pucch-ResourceId = 14
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 0
    											format = format2 =
    												nrofPRBs = 6
    												nrofSymbols = 2
    												startingSymbolIndex = 12
    										PUCCH-Resource(16)
    											pucch-ResourceId = 15
    											startingPRB = 0
    											intraSlotFrequencyHopping = enabled
    											secondHopPRB = 0
    											format = format3 =
    												nrofPRBs = 1
    												nrofSymbols = 14
    												startingSymbolIndex = 0
    									format1 = setup =
    										interslotFrequencyHopping = enabled
    										additionalDMRS = true
    										maxCodeRate = zeroDot25
    										simultaneousHARQ-ACK-CSI = true
    									format2 = setup =
    										interslotFrequencyHopping = enabled
    										additionalDMRS = true
    										maxCodeRate = zeroDot25
    										simultaneousHARQ-ACK-CSI = true
    									format3 = setup =
    										interslotFrequencyHopping = enabled
    										additionalDMRS = true
    										maxCodeRate = zeroDot25
    										simultaneousHARQ-ACK-CSI = true
    									schedulingRequestResourceToAddModList = SEQUENCE OF SchedulingRequestResourceConfig
    										SchedulingRequestResourceConfig(1)
    											schedulingRequestResourceId = 1
    											schedulingRequestID = 0
    											periodicityAndOffset = sl20 = 9
    											resource = 0
    									dl-DataToUL-ACK = SEQUENCE OF INTEGER
    										INTEGER(1) = 2
    										INTEGER(2) = 3
    										INTEGER(3) = 4
    										INTEGER(4) = 5
    										INTEGER(5) = 6
    										INTEGER(6) = 7
    										INTEGER(7) = 8
    										INTEGER(8) = 9
    									pucch-PowerControl
    										deltaF-PUCCH-f0 = 0
    										deltaF-PUCCH-f1 = 0
    										deltaF-PUCCH-f2 = 0
    										deltaF-PUCCH-f3 = 0
    										deltaF-PUCCH-f4 = 0
    										pathlossReferenceRSs = SEQUENCE OF PUCCH-PathlossReferenceRS
    											PUCCH-PathlossReferenceRS(1)
    												pucch-PathlossReferenceRS-Id = 0
    												referenceSignal = ssb-Index = 1
    								pusch-Config = setup =
    									txConfig = codebook
    									dmrs-UplinkForPUSCH-MappingTypeA = setup =
    										dmrs-AdditionalPosition = pos1
    										transformPrecodingDisabled
    									pusch-PowerControl
    										msg3-Alpha = alpha08
    										p0-NominalWithoutGrant = -90
    										p0-AlphaSets = SEQUENCE OF P0-PUSCH-AlphaSet
    											P0-PUSCH-AlphaSet(1)
    												p0-PUSCH-AlphaSetId = 0
    												p0 = 0
    												alpha = alpha08
    										pathlossReferenceRSToAddModList = SEQUENCE OF PUSCH-PathlossReferenceRS
    											PUSCH-PathlossReferenceRS(1)
    												pusch-PathlossReferenceRS-Id = 0
    												referenceSignal = ssb-Index = 1
    										sri-PUSCH-MappingToAddModList = SEQUENCE OF SRI-PUSCH-PowerControl
    											SRI-PUSCH-PowerControl(1)
    												sri-PUSCH-PowerControlId = 0
    												sri-PUSCH-PathlossReferenceRS-Id = 0
    												sri-P0-PUSCH-AlphaSetId = 0
    												sri-PUSCH-ClosedLoopIndex = i0
    									resourceAllocation = resourceAllocationType1
    									codebookSubset = nonCoherent
    									maxRank = 1
    									uci-OnPUSCH = setup =
    										betaOffsets = semiStatic =
    											betaOffsetACK-Index1 = 9
    											betaOffsetACK-Index2 = 9
    											betaOffsetACK-Index3 = 9
    											betaOffsetCSI-Part1-Index1 = 6
    											betaOffsetCSI-Part1-Index2 = 6
    											betaOffsetCSI-Part2-Index1 = 6
    											betaOffsetCSI-Part2-Index2 = 6
    										scaling = f1
    								srs-Config = setup =
    									srs-ResourceSetToAddModList = SEQUENCE OF SRS-ResourceSet
    										SRS-ResourceSet(1)
    											srs-ResourceSetId = 0
    											srs-ResourceIdList = SEQUENCE OF SRS-ResourceId
    												SRS-ResourceId(1) = 0
    											resourceType = aperiodic =
    												aperiodicSRS-ResourceTrigger = 1
    												slotOffset = 7
    											usage = codebook
    											alpha = alpha0
    											p0 = 0
    											pathlossReferenceRS = ssb-Index = 1
    									srs-ResourceToAddModList = SEQUENCE OF SRS-Resource
    										SRS-Resource(1)
    											srs-ResourceId = 0
    											nrofSRS-Ports = port1
    											transmissionComb = n2 =
    												combOffset-n2 = 0
    												cyclicShift-n2 = 0
    											resourceMapping
    												startPosition = 0
    												nrofSymbols = n1
    												repetitionFactor = n1
    											freqDomainPosition = 0
    											freqDomainShift = 0
    											freqHopping
    												c-SRS = 63
    												b-SRS = 0
    												b-hop = 0
    											groupOrSequenceHopping = groupHopping
    											resourceType = aperiodic =
    											sequenceId = 0
    											spatialRelationInfo
    												referenceSignal = ssb-Index = 1
    							firstActiveUplinkBWP-Id = 0
    							pusch-ServingCellConfig = setup =
    						pdcch-ServingCellConfig = setup =
    						pdsch-ServingCellConfig = setup =
    							nrofHARQ-ProcessesForPDSCH = n16
    						tag-Id = 0

    rrcSetup

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		Cell
    			AddOrReconfigure
    				StaticResourceConfig
    					CellCapability = fullCell (2)
    					CarrierAggregation = None (3)
    				CellConfigCommon
    					C_RNTI = 4097
    					CellTimingInfo
    						TcOffset = 0
    						Tcell = 0
    						SfnOffset = 0
    						HsfnOffset = 0
    					InitialCellPower
    						MaxReferencePower = -88
    						Attenuation
    							Off = True
    				PhysicalLayer
    					Common
    						PhysicalCellId = 0
    						DuplexMode
    							TDD
    								Config
    									Common
    										R15
    											referenceSubcarrierSpacing = kHz30 (1)
    											pattern1
    												dl_UL_TransmissionPeriodicity = ms5 (6)
    												nrofDownlinkSlots = 7
    												nrofDownlinkSymbols = 6
    												nrofUplinkSlots = 2
    												nrofUplinkSymbols = 4
    												dl_UL_TransmissionPeriodicity_v1530 = Omit
    											pattern2 = Omit
    									Dedicated = Omit
    					Downlink
    						FrequencyInfoDL
    							R15
    								absoluteFrequencySSB = 500190
    								frequencyBandList
    									FreqBandIndicatorNR = 41
    								absoluteFrequencyPointA = 499368
    								scs_SpecificCarrierList
    									SCS_SpecificCarrier
    										offsetToCarrier = 0
    										subcarrierSpacing = kHz30 (1)
    										carrierBandwidth = 162
    										txDirectCurrentLocation_v1530 = Omit
    						SSPbchBlock
    							SubCarrierSpacing = kHz30 (1)
    							SubcarrierOffset = 10
    							Periodicity = ms20 (2)
    							HalfFrameOffset = 0
    							BurstConfig
    								BlockPattern = caseC (2)
    								Bitmap
    									mediumBitmap = 01000000'B
    								BeamArray = Omit
    							RelativeTxPower
    								Pbch = 0
    								Pss = 0
    								Sss = 0
    								Dmrs = 0
    						PdschCellLevelConfig
    							DMRS_TypeA_Position = pos2 (0)
    							RateMatchPattern
    								PatternList = Omit
    								PatternListLteCrs = Omit
    							ServingCellConfig
    								R15
    									codeBlockGroupTransmission = Omit
    									xOverhead = Omit
    									nrofHARQ_ProcessesForPDSCH = n16 (5)
    									pucch_Cell = Omit
    									maxMIMO_Layers = Omit
    									processingType2Enabled = Omit
    						BWPs
    							ActiveBWP = 0
    							BwpArray
    								NR_DownlinkBWP_Type
    									Id = 0
    									BWP
    										R15
    											locationAndBandwidth = 31624
    											subcarrierSpacing = kHz30 (1)
    											cyclicPrefix = Omit
    									Pdcch
    										SearchSpaceArray
    											NR_BWP_SearchSpaceConfig_Type
    												TypeAndPriorityList
    													NR_SearchSpaceTypeAndPriority_Type
    														NR_SearchSpaceType_Type = cssType0 (0)
    														IntegerType = 0
    													NR_SearchSpaceTypeAndPriority_Type
    														NR_SearchSpaceType_Type = cssType2 (3)
    														IntegerType = 3
    												AggregationLevel = AggregationLevel4 (2)
    												SearchSpaceConfigAtUE
    													R15
    														searchSpaceId = 0
    														controlResourceSetId = 0
    														monitoringSlotPeriodicityAndOffset
    															sl40 = 1
    														duration = 2
    														monitoringSymbolsWithinSlot = 10000000000000'B
    														nrofCandidates
    															aggregationLevel1 = n0 (0)
    															aggregationLevel2 = n0 (0)
    															aggregationLevel4 = n4 (4)
    															aggregationLevel8 = n2 (2)
    															aggregationLevel16 = n1 (1)
    														searchSpaceType
    															common
    																dci_Format0_0_AndFormat1_0
    																dci_Format2_0 = Omit
    																dci_Format2_1 = Omit
    																dci_Format2_2 = Omit
    																dci_Format2_3 = Omit
    											NR_BWP_SearchSpaceConfig_Type
    												TypeAndPriorityList
    													NR_SearchSpaceTypeAndPriority_Type
    														NR_SearchSpaceType_Type = cssType1 (2)
    														IntegerType = 2
    													NR_SearchSpaceTypeAndPriority_Type
    														NR_SearchSpaceType_Type = cssType3 (4)
    														IntegerType = 4
    												AggregationLevel = AggregationLevel4 (2)
    												SearchSpaceConfigAtUE
    													R15
    														searchSpaceId = 1
    														controlResourceSetId = 1
    														monitoringSlotPeriodicityAndOffset
    															sl1 = Null
    														duration = Omit
    														monitoringSymbolsWithinSlot = 10000000000000'B
    														nrofCandidates
    															aggregationLevel1 = n0 (0)
    															aggregationLevel2 = n4 (4)
    															aggregationLevel4 = n2 (2)
    															aggregationLevel8 = n2 (2)
    															aggregationLevel16 = n0 (0)
    														searchSpaceType
    															common
    																dci_Format0_0_AndFormat1_0
    																dci_Format2_0 = Omit
    																dci_Format2_1 = Omit
    																dci_Format2_2 = Omit
    																dci_Format2_3 = Omit
    											NR_BWP_SearchSpaceConfig_Type
    												TypeAndPriorityList
    													NR_SearchSpaceTypeAndPriority_Type
    														NR_SearchSpaceType_Type = ussDL (5)
    														IntegerType = 5
    													NR_SearchSpaceTypeAndPriority_Type
    														NR_SearchSpaceType_Type = ussUL (6)
    														IntegerType = 9
    												AggregationLevel = AggregationLevel4 (2)
    												SearchSpaceConfigAtUE
    													R15
    														searchSpaceId = 2
    														controlResourceSetId = 1
    														monitoringSlotPeriodicityAndOffset
    															sl1 = Null
    														duration = Omit
    														monitoringSymbolsWithinSlot = 10000000000000'B
    														nrofCandidates
    															aggregationLevel1 = n0 (0)
    															aggregationLevel2 = n4 (4)
    															aggregationLevel4 = n2 (2)
    															aggregationLevel8 = n2 (2)
    															aggregationLevel16 = n0 (0)
    														searchSpaceType
    															ue_Specific
    																dci_Formats = formats0_1_And_1_1 (1)
    											NR_BWP_SearchSpaceConfig_Type
    												TypeAndPriorityList
    													NR_SearchSpaceTypeAndPriority_Type
    														NR_SearchSpaceType_Type = cssType0A (1)
    														IntegerType = 1
    												AggregationLevel = AggregationLevel4 (2)
    												SearchSpaceConfigAtUE
    													R15
    														searchSpaceId = 3
    														controlResourceSetId = 1
    														monitoringSlotPeriodicityAndOffset
    															sl10 = 5
    														duration = 2
    														monitoringSymbolsWithinSlot = 10000000000000'B
    														nrofCandidates
    															aggregationLevel1 = n0 (0)
    															aggregationLevel2 = n4 (4)
    															aggregationLevel4 = n2 (2)
    															aggregationLevel8 = n2 (2)
    															aggregationLevel16 = n0 (0)
    														searchSpaceType
    															common
    																dci_Format0_0_AndFormat1_0
    																dci_Format2_0 = Omit
    																dci_Format2_1 = Omit
    																dci_Format2_2 = Omit
    																dci_Format2_3 = Omit
    										CoresetArray
    											NR_ASN1_ControlResourceSet_Type
    												R15
    													controlResourceSetId = 0
    													frequencyDomainResources = 111100000000000000000000000000000000000000000'B
    													duration = 2
    													cce_REG_MappingType
    														interleaved
    															reg_BundleSize = n6 (2)
    															interleaverSize = n2 (0)
    															shiftIndex = 0
    													precoderGranularity = sameAsREG_bundle (0)
    													tci_StatesPDCCH_ToAddList = Omit
    													tci_StatesPDCCH_ToReleaseList = Omit
    													tci_PresentInDCI = Omit
    													pdcch_DMRS_ScramblingID = Omit
    											NR_ASN1_ControlResourceSet_Type
    												R15
    													controlResourceSetId = 1
    													frequencyDomainResources = 111100000000000000000000000000000000000000000'B
    													duration = 2
    													cce_REG_MappingType
    														nonInterleaved = Null
    													precoderGranularity = sameAsREG_bundle (0)
    													tci_StatesPDCCH_ToAddList = Omit
    													tci_StatesPDCCH_ToReleaseList = Omit
    													tci_PresentInDCI = Omit
    													pdcch_DMRS_ScramblingID = Omit
    										RelativeTxPower
    											PdcchToCell = 0
    											PdcchToDmrs = 0
    									Pdsch
    										ConfigCommon
    											R15
    												pdsch_TimeDomainAllocationList
    													PDSCH_TimeDomainResourceAllocation
    														k0 = Omit
    														mappingType = typeA (0)
    														startSymbolAndLength = 53
    													PDSCH_TimeDomainResourceAllocation
    														k0 = Omit
    														mappingType = typeA (0)
    														startSymbolAndLength = 72
    										ConfigDedicated
    											R15
    												dataScramblingIdentityPDSCH = 0
    												dmrs_DownlinkForPDSCH_MappingTypeA
    													setup
    														dmrs_Type = Omit
    														dmrs_AdditionalPosition = pos1 (1)
    														maxLength = Omit
    														scramblingID0 = Omit
    														scramblingID1 = Omit
    														phaseTrackingRS = Omit
    												dmrs_DownlinkForPDSCH_MappingTypeB = Omit
    												tci_StatesToAddModList
    													TCI_State
    														tci_StateId = 0
    														qcl_Type1
    															cell = Omit
    															bwp_Id = Omit
    															referenceSignal
    																ssb = 1
    															qcl_Type = typeD (3)
    														qcl_Type2 = Omit
    												tci_StatesToReleaseList = Omit
    												vrb_ToPRB_Interleaver = Omit
    												resourceAllocation = resourceAllocationType1 (1)
    												pdsch_TimeDomainAllocationList = Omit
    												pdsch_AggregationFactor = Omit
    												rateMatchPatternToAddModList = Omit
    												rateMatchPatternToReleaseList = Omit
    												rateMatchPatternGroup1 = Omit
    												rateMatchPatternGroup2 = Omit
    												rbg_Size = config1 (0)
    												mcs_Table = Omit
    												maxNrofCodeWordsScheduledByDCI = Omit
    												prb_BundlingType
    													staticBundling
    														bundleSize = wideband (1)
    												zp_CSI_RS_ResourceToAddModList = Omit
    												zp_CSI_RS_ResourceToReleaseList = Omit
    												aperiodic_ZP_CSI_RS_ResourceSetsToAddModList = Omit
    												aperiodic_ZP_CSI_RS_ResourceSetsToReleaseList = Omit
    												sp_ZP_CSI_RS_ResourceSetsToAddModList = Omit
    												sp_ZP_CSI_RS_ResourceSetsToReleaseList = Omit
    												p_ZP_CSI_RS_ResourceSet = Omit
    										RelativeTxPower
    											PdschToCell = -3
    											PdschToDmrs = -3
    											PdschToPtrs = -3
    									Sps = Omit
    						CsiConfig
    							None = True
    					Uplink
    						Uplink
    							Config
    								FrequencyInfoUL
    									R15
    										frequencyBandList = Omit
    										absoluteFrequencyPointA = Omit
    										scs_SpecificCarrierList
    											SCS_SpecificCarrier
    												offsetToCarrier = 0
    												subcarrierSpacing = kHz30 (1)
    												carrierBandwidth = 162
    												txDirectCurrentLocation_v1530 = Omit
    										additionalSpectrumEmission = 0
    										p_Max = 20
    										frequencyShift7p5khz = Omit
    								BWPs
    									ActiveBWP
    										SameIdAsDL = True
    									BwpArray
    										NR_UplinkBWP_Type
    											Id = 0
    											Common
    												R15
    													genericParameters
    														locationAndBandwidth = 31624
    														subcarrierSpacing = kHz30 (1)
    														cyclicPrefix = Omit
    													rach_ConfigCommon
    														setup
    															rach_ConfigGeneric
    																prach_ConfigurationIndex = 160
    																msg1_FDM = four (2)
    																msg1_FrequencyStart = 0
    																zeroCorrelationZoneConfig = 15
    																preambleReceivedTargetPower = -118
    																preambleTransMax = n7 (4)
    																powerRampingStep = dB4 (2)
    																ra_ResponseWindow = sl20 (5)
    															totalNumberOfRA_Preambles = Omit
    															ssb_perRACH_OccasionAndCB_PreamblesPerSSB
    																one = n8 (1)
    															groupBconfigured = Omit
    															ra_ContentionResolutionTimer = sf64 (7)
    															rsrp_ThresholdSSB = 0
    															rsrp_ThresholdSSB_SUL = Omit
    															prach_RootSequenceIndex
    																l139 = 0
    															msg1_SubcarrierSpacing = kHz30 (1)
    															restrictedSetConfig = unrestrictedSet (0)
    															msg3_transformPrecoder = Omit
    													pusch_ConfigCommon
    														setup
    															groupHoppingEnabledTransformPrecoding = Omit
    															pusch_TimeDomainAllocationList
    																PUSCH_TimeDomainResourceAllocation
    																	k2 = 4
    																	mappingType = typeA (0)
    																	startSymbolAndLength = 27
    																PUSCH_TimeDomainResourceAllocation
    																	k2 = 6
    																	mappingType = typeA (0)
    																	startSymbolAndLength = 27
    															msg3_DeltaPreamble = 1
    															p0_NominalWithGrant = -90
    													pucch_ConfigCommon
    														setup
    															pucch_ResourceCommon = 0
    															pucch_GroupHopping = enable (1)
    															hoppingId = Omit
    															p0_nominal = -90
    											Dedicated
    												R15
    													pucch_Config
    														setup
    															resourceSetToAddModList
    																PUCCH_ResourceSet
    																	pucch_ResourceSetId = 0
    																	resourceList
    																		IntegerType = 0
    																		IntegerType = 1
    																		IntegerType = 2
    																		IntegerType = 3
    																		IntegerType = 4
    																		IntegerType = 5
    																		IntegerType = 6
    																		IntegerType = 7
    																	maxPayloadMinus1 = Omit
    																PUCCH_ResourceSet
    																	pucch_ResourceSetId = 1
    																	resourceList
    																		IntegerType = 8
    																		IntegerType = 9
    																		IntegerType = 10
    																		IntegerType = 11
    																		IntegerType = 12
    																		IntegerType = 13
    																		IntegerType = 14
    																		IntegerType = 15
    																	maxPayloadMinus1 = 256
    																PUCCH_ResourceSet
    																	pucch_ResourceSetId = 2
    																	resourceList
    																		IntegerType = 8
    																		IntegerType = 9
    																		IntegerType = 10
    																		IntegerType = 11
    																		IntegerType = 12
    																		IntegerType = 13
    																		IntegerType = 14
    																		IntegerType = 15
    																	maxPayloadMinus1 = 256
    																PUCCH_ResourceSet
    																	pucch_ResourceSetId = 3
    																	resourceList
    																		IntegerType = 8
    																		IntegerType = 9
    																		IntegerType = 10
    																		IntegerType = 11
    																		IntegerType = 12
    																		IntegerType = 13
    																		IntegerType = 14
    																		IntegerType = 15
    																	maxPayloadMinus1 = Omit
    															resourceSetToReleaseList = Omit
    															resourceToAddModList
    																PUCCH_Resource
    																	pucch_ResourceId = 0
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 0
    																PUCCH_Resource
    																	pucch_ResourceId = 1
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 2
    																PUCCH_Resource
    																	pucch_ResourceId = 2
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 4
    																PUCCH_Resource
    																	pucch_ResourceId = 3
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 6
    																PUCCH_Resource
    																	pucch_ResourceId = 4
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 8
    																PUCCH_Resource
    																	pucch_ResourceId = 5
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 10
    																PUCCH_Resource
    																	pucch_ResourceId = 6
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 12
    																PUCCH_Resource
    																	pucch_ResourceId = 7
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format1
    																			initialCyclicShift = 0
    																			nrofSymbols = 14
    																			startingSymbolIndex = 0
    																			timeDomainOCC = 0
    																PUCCH_Resource
    																	pucch_ResourceId = 8
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 0
    																PUCCH_Resource
    																	pucch_ResourceId = 9
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 2
    																PUCCH_Resource
    																	pucch_ResourceId = 10
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 4
    																PUCCH_Resource
    																	pucch_ResourceId = 11
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 6
    																PUCCH_Resource
    																	pucch_ResourceId = 12
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 8
    																PUCCH_Resource
    																	pucch_ResourceId = 13
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 10
    																PUCCH_Resource
    																	pucch_ResourceId = 14
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 12
    																PUCCH_Resource
    																	pucch_ResourceId = 15
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format3
    																			nrofPRBs = 1
    																			nrofSymbols = 14
    																			startingSymbolIndex = 0
    															resourceToReleaseList = Omit
    															format1
    																setup
    																	interslotFrequencyHopping = enabled (0)
    																	additionalDMRS = true_ (0)
    																	maxCodeRate = zeroDot25 (2)
    																	nrofSlots = Omit
    																	pi2BPSK = Omit
    																	simultaneousHARQ_ACK_CSI = true_ (0)
    															format2
    																setup
    																	interslotFrequencyHopping = enabled (0)
    																	additionalDMRS = true_ (0)
    																	maxCodeRate = zeroDot25 (2)
    																	nrofSlots = Omit
    																	pi2BPSK = Omit
    																	simultaneousHARQ_ACK_CSI = true_ (0)
    															format3
    																setup
    																	interslotFrequencyHopping = enabled (0)
    																	additionalDMRS = true_ (0)
    																	maxCodeRate = zeroDot25 (2)
    																	nrofSlots = Omit
    																	pi2BPSK = Omit
    																	simultaneousHARQ_ACK_CSI = true_ (0)
    															format4 = Omit
    															schedulingRequestResourceToAddModList
    																SchedulingRequestResourceConfig
    																	schedulingRequestResourceId = 1
    																	schedulingRequestID = 0
    																	periodicityAndOffset
    																		sl20 = 9
    																	resource = 0
    															schedulingRequestResourceToReleaseList = Omit
    															multi_CSI_PUCCH_ResourceList = Omit
    															dl_DataToUL_ACK
    																IntegerType = 2
    																IntegerType = 3
    																IntegerType = 4
    																IntegerType = 5
    																IntegerType = 6
    																IntegerType = 7
    																IntegerType = 8
    																IntegerType = 9
    															spatialRelationInfoToAddModList = Omit
    															spatialRelationInfoToReleaseList = Omit
    															pucch_PowerControl
    																deltaF_PUCCH_f0 = 0
    																deltaF_PUCCH_f1 = 0
    																deltaF_PUCCH_f2 = 0
    																deltaF_PUCCH_f3 = 0
    																deltaF_PUCCH_f4 = 0
    																p0_Set = Omit
    																pathlossReferenceRSs
    																	PUCCH_PathlossReferenceRS
    																		pucch_PathlossReferenceRS_Id = 0
    																		referenceSignal
    																			ssb_Index = 1
    																twoPUCCH_PC_AdjustmentStates = Omit
    													pusch_Config
    														setup
    															dataScramblingIdentityPUSCH = Omit
    															txConfig = codebook (0)
    															dmrs_UplinkForPUSCH_MappingTypeA
    																setup
    																	dmrs_Type = Omit
    																	dmrs_AdditionalPosition = pos1 (1)
    																	phaseTrackingRS = Omit
    																	maxLength = Omit
    																	transformPrecodingDisabled
    																		scramblingID0 = Omit
    																		scramblingID1 = Omit
    																	transformPrecodingEnabled = Omit
    															dmrs_UplinkForPUSCH_MappingTypeB = Omit
    															pusch_PowerControl
    																tpc_Accumulation = Omit
    																msg3_Alpha = alpha08 (5)
    																p0_NominalWithoutGrant = -90
    																p0_AlphaSets
    																	P0_PUSCH_AlphaSet
    																		p0_PUSCH_AlphaSetId = 0
    																		p0 = 0
    																		alpha = alpha08 (5)
    																pathlossReferenceRSToAddModList
    																	PUSCH_PathlossReferenceRS
    																		pusch_PathlossReferenceRS_Id = 0
    																		referenceSignal
    																			ssb_Index = 1
    																pathlossReferenceRSToReleaseList = Omit
    																twoPUSCH_PC_AdjustmentStates = Omit
    																deltaMCS = Omit
    																sri_PUSCH_MappingToAddModList
    																	SRI_PUSCH_PowerControl
    																		sri_PUSCH_PowerControlId = 0
    																		sri_PUSCH_PathlossReferenceRS_Id = 0
    																		sri_P0_PUSCH_AlphaSetId = 0
    																		sri_PUSCH_ClosedLoopIndex = i0 (0)
    																sri_PUSCH_MappingToReleaseList = Omit
    															frequencyHopping = Omit
    															frequencyHoppingOffsetLists = Omit
    															resourceAllocation = resourceAllocationType1 (1)
    															pusch_TimeDomainAllocationList = Omit
    															pusch_AggregationFactor = Omit
    															mcs_Table = Omit
    															mcs_TableTransformPrecoder = Omit
    															transformPrecoder = Omit
    															codebookSubset = nonCoherent (2)
    															maxRank = 1
    															rbg_Size = Omit
    															uci_OnPUSCH
    																setup
    																	betaOffsets
    																		semiStatic
    																			betaOffsetACK_Index1 = 9
    																			betaOffsetACK_Index2 = 9
    																			betaOffsetACK_Index3 = 9
    																			betaOffsetCSI_Part1_Index1 = 6
    																			betaOffsetCSI_Part1_Index2 = 6
    																			betaOffsetCSI_Part2_Index1 = 6
    																			betaOffsetCSI_Part2_Index2 = 6
    																	scaling = f1 (3)
    															tp_pi2BPSK = Omit
    													configuredGrantConfig = Omit
    													srs_Config
    														setup
    															srs_ResourceSetToReleaseList = Omit
    															srs_ResourceSetToAddModList
    																SRS_ResourceSet
    																	srs_ResourceSetId = 0
    																	srs_ResourceIdList
    																		IntegerType = 0
    																	resourceType
    																		aperiodic
    																			aperiodicSRS_ResourceTrigger = 1
    																			csi_RS = Omit
    																			slotOffset = 7
    																	usage = codebook (1)
    																	alpha = alpha0 (0)
    																	p0 = 0
    																	pathlossReferenceRS
    																		ssb_Index = 1
    																	srs_PowerControlAdjustmentStates = Omit
    															srs_ResourceToReleaseList = Omit
    															srs_ResourceToAddModList
    																SRS_Resource
    																	srs_ResourceId = 0
    																	nrofSRS_Ports = port1 (0)
    																	ptrs_PortIndex = Omit
    																	transmissionComb
    																		n2
    																			combOffset_n2 = 0
    																			cyclicShift_n2 = 0
    																	resourceMapping
    																		startPosition = 0
    																		nrofSymbols = n1 (0)
    																		repetitionFactor = n1 (0)
    																	freqDomainPosition = 0
    																	freqDomainShift = 0
    																	freqHopping
    																		c_SRS = 63
    																		b_SRS = 0
    																		b_hop = 0
    																	groupOrSequenceHopping = groupHopping (1)
    																	resourceType
    																		aperiodic
    																	sequenceId = 0
    																	spatialRelationInfo
    																		servingCellId = Omit
    																		referenceSignal
    																			ssb_Index = 1
    															tpc_Accumulation = Omit
    													beamFailureRecoveryConfig = Omit
    								RACH_ConfigDedicated = Omit
    								SI_RequestConfig = Omit
    						SupplementaryUplink = Omit
    						TimingAdvance
    							InitialValue = 0
    						PUSCH_ServingCellConfig
    							R15
    								codeBlockGroupTransmission = Omit
    								rateMatching = Omit
    								xOverhead = Omit
    								maxMIMO_Layers = Omit
    								processingType2Enabled = Omit
    				BcchConfig
    					Pbch = True
    					Pdsch
    						Sib1Schedul
    							SearchSpaceAndDci
    								AssignedBWPs
    									ActiveBWP = Omit
    									InitialBWP = True
    									DedicatedBWPs
    								SearchSpaceType = cssType0 (0)
    								DciInfo
    									ResoureAssignment
    										ResourceAllocationType = resourceAllocationType1 (1)
    										FreqDomain
    											Automatic
    												FirstRbIndex = 0
    												MaxRbCnt = 7
    										TimeDomain
    											Index = 0000'B
    										TransportBlockScheduling
    											Automatic
    												TransportBlock1 = qpsk (0)
    												TransportBlock2 = Omit
    												RedundancyVersionList
    													NR_RedundancyVersion_Type = 0
    										HarqProcessConfig
    											Broadcast = True
    									VrbPrbMapping
    										Index = 0'B
    									Format
    										Format_1_0_SI_RNTI
    											SystemInfoIndicator = 0'B
    							Periodicity = 20
    							SlotOffsetList
    								IntegerType = 1
    						SiSchedul = Omit
    					BcchInfo
    						MIB
    							message_
    								mib
    									systemFrameNumber = 000000'B
    									subCarrierSpacingCommon = scs30or120 (1)
    									ssb_SubcarrierOffset = 10
    									dmrs_TypeA_Position = pos2 (0)
    									pdcch_ConfigSIB1
    										controlResourceSetZero = 1
    										searchSpaceZero = 0
    									cellBarred = notBarred (1)
    									intraFreqReselection = allowed (0)
    									spare = 0'B
    						SIB1
    							message_
    								c1
    									systemInformationBlockType1
    										cellSelectionInfo
    											q_RxLevMin = -55
    											q_RxLevMinOffset = Omit
    											q_RxLevMinSUL = Omit
    											q_QualMin = Omit
    											q_QualMinOffset = Omit
    										cellAccessRelatedInfo
    											plmn_IdentityList
    												PLMN_IdentityInfo
    													plmn_IdentityList
    														PLMN_Identity
    															mcc
    																IntegerType = 0
    																IntegerType = 0
    																IntegerType = 1
    															mnc
    																IntegerType = 0
    																IntegerType = 1
    													trackingAreaCode = 000000000000000000000001'B
    													ranac = 1
    													cellIdentity = 000000000000000000000000010000000000'B
    													cellReservedForOperatorUse = notReserved (1)
    											cellReservedForOtherUse = Omit
    										connEstFailureControl
    											connEstFailCount = n1 (0)
    											connEstFailOffsetValidity = s30 (0)
    											connEstFailOffset = 1
    										si_SchedulingInfo = Omit
    										servingCellConfigCommon
    											downlinkConfigCommon
    												frequencyInfoDL
    													frequencyBandList
    														NR_MultiBandInfo
    															freqBandIndicatorNR = 41
    															nr_NS_PmaxList
    																NR_NS_PmaxValue
    																	additionalPmax = 20
    																	additionalSpectrumEmission = 0
    													offsetToPointA = 2
    													scs_SpecificCarrierList
    														SCS_SpecificCarrier
    															offsetToCarrier = 0
    															subcarrierSpacing = kHz30 (1)
    															carrierBandwidth = 162
    															txDirectCurrentLocation_v1530 = Omit
    												initialDownlinkBWP
    													genericParameters
    														locationAndBandwidth = 31624
    														subcarrierSpacing = kHz30 (1)
    														cyclicPrefix = Omit
    													pdcch_ConfigCommon
    														setup
    															controlResourceSetZero = 1
    															commonControlResourceSet
    																controlResourceSetId = 1
    																frequencyDomainResources = 111100000000000000000000000000000000000000000'B
    																duration = 2
    																cce_REG_MappingType
    																	nonInterleaved = Null
    																precoderGranularity = sameAsREG_bundle (0)
    																tci_StatesPDCCH_ToAddList = Omit
    																tci_StatesPDCCH_ToReleaseList = Omit
    																tci_PresentInDCI = Omit
    																pdcch_DMRS_ScramblingID = Omit
    															searchSpaceZero = 0
    															commonSearchSpaceList
    																SearchSpace
    																	searchSpaceId = 1
    																	controlResourceSetId = 1
    																	monitoringSlotPeriodicityAndOffset
    																		sl1 = Null
    																	duration = Omit
    																	monitoringSymbolsWithinSlot = 10000000000000'B
    																	nrofCandidates
    																		aggregationLevel1 = n0 (0)
    																		aggregationLevel2 = n4 (4)
    																		aggregationLevel4 = n2 (2)
    																		aggregationLevel8 = n2 (2)
    																		aggregationLevel16 = n0 (0)
    																	searchSpaceType
    																		common
    																			dci_Format0_0_AndFormat1_0
    																			dci_Format2_0 = Omit
    																			dci_Format2_1 = Omit
    																			dci_Format2_2 = Omit
    																			dci_Format2_3 = Omit
    																SearchSpace
    																	searchSpaceId = 3
    																	controlResourceSetId = 1
    																	monitoringSlotPeriodicityAndOffset
    																		sl10 = 5
    																	duration = 2
    																	monitoringSymbolsWithinSlot = 10000000000000'B
    																	nrofCandidates
    																		aggregationLevel1 = n0 (0)
    																		aggregationLevel2 = n4 (4)
    																		aggregationLevel4 = n2 (2)
    																		aggregationLevel8 = n2 (2)
    																		aggregationLevel16 = n0 (0)
    																	searchSpaceType
    																		common
    																			dci_Format0_0_AndFormat1_0
    																			dci_Format2_0 = Omit
    																			dci_Format2_1 = Omit
    																			dci_Format2_2 = Omit
    																			dci_Format2_3 = Omit
    															searchSpaceSIB1 = 0
    															searchSpaceOtherSystemInformation = 3
    															pagingSearchSpace = 0
    															ra_SearchSpace = 1
    															firstPDCCH_MonitoringOccasionOfPO = Omit
    													pdsch_ConfigCommon
    														setup
    															pdsch_TimeDomainAllocationList
    																PDSCH_TimeDomainResourceAllocation
    																	k0 = Omit
    																	mappingType = typeA (0)
    																	startSymbolAndLength = 53
    																PDSCH_TimeDomainResourceAllocation
    																	k0 = Omit
    																	mappingType = typeA (0)
    																	startSymbolAndLength = 72
    												bcch_Config
    													modificationPeriodCoeff = n4 (1)
    												pcch_Config
    													defaultPagingCycle = rf128 (2)
    													nAndPagingFrameOffset
    														halfT = 1
    													ns = one (2)
    													firstPDCCH_MonitoringOccasionOfPO = Omit
    											uplinkConfigCommon
    												frequencyInfoUL
    													frequencyBandList = Omit
    													absoluteFrequencyPointA = Omit
    													scs_SpecificCarrierList
    														SCS_SpecificCarrier
    															offsetToCarrier = 0
    															subcarrierSpacing = kHz30 (1)
    															carrierBandwidth = 162
    															txDirectCurrentLocation_v1530 = Omit
    													p_Max = 20
    													frequencyShift7p5khz = Omit
    												initialUplinkBWP
    													genericParameters
    														locationAndBandwidth = 31624
    														subcarrierSpacing = kHz30 (1)
    														cyclicPrefix = Omit
    													rach_ConfigCommon
    														setup
    															rach_ConfigGeneric
    																prach_ConfigurationIndex = 160
    																msg1_FDM = four (2)
    																msg1_FrequencyStart = 0
    																zeroCorrelationZoneConfig = 15
    																preambleReceivedTargetPower = -118
    																preambleTransMax = n7 (4)
    																powerRampingStep = dB4 (2)
    																ra_ResponseWindow = sl20 (5)
    															totalNumberOfRA_Preambles = Omit
    															ssb_perRACH_OccasionAndCB_PreamblesPerSSB
    																one = n8 (1)
    															groupBconfigured = Omit
    															ra_ContentionResolutionTimer = sf64 (7)
    															rsrp_ThresholdSSB = 0
    															rsrp_ThresholdSSB_SUL = Omit
    															prach_RootSequenceIndex
    																l139 = 0
    															msg1_SubcarrierSpacing = kHz30 (1)
    															restrictedSetConfig = unrestrictedSet (0)
    															msg3_transformPrecoder = Omit
    													pusch_ConfigCommon
    														setup
    															groupHoppingEnabledTransformPrecoding = Omit
    															pusch_TimeDomainAllocationList
    																PUSCH_TimeDomainResourceAllocation
    																	k2 = 4
    																	mappingType = typeA (0)
    																	startSymbolAndLength = 27
    																PUSCH_TimeDomainResourceAllocation
    																	k2 = 6
    																	mappingType = typeA (0)
    																	startSymbolAndLength = 27
    															msg3_DeltaPreamble = 1
    															p0_NominalWithGrant = -90
    													pucch_ConfigCommon
    														setup
    															pucch_ResourceCommon = 0
    															pucch_GroupHopping = enable (1)
    															hoppingId = Omit
    															p0_nominal = -90
    												timeAlignmentTimerCommon = infinity_ (7)
    											supplementaryUplink = Omit
    											n_TimingAdvanceOffset = Omit
    											ssb_PositionsInBurst
    												inOneGroup = 01000000'B
    												groupPresence = Omit
    											ssb_PeriodicityServingCell = ms20 (2)
    											tdd_UL_DL_ConfigurationCommon
    												referenceSubcarrierSpacing = kHz30 (1)
    												pattern1
    													dl_UL_TransmissionPeriodicity = ms5 (6)
    													nrofDownlinkSlots = 7
    													nrofDownlinkSymbols = 6
    													nrofUplinkSlots = 2
    													nrofUplinkSymbols = 4
    													dl_UL_TransmissionPeriodicity_v1530 = Omit
    												pattern2 = Omit
    											ss_PBCH_BlockPower = 0
    										ims_EmergencySupport = Omit
    										eCallOverIMS_Support = Omit
    										ue_TimersAndConstants
    											t300 = ms1000 (5)
    											t301 = ms1000 (5)
    											t310 = ms1000 (5)
    											n310 = n1 (0)
    											t311 = ms30000 (6)
    											n311 = n1 (0)
    											t319 = ms1000 (5)
    										uac_BarringInfo = Omit
    										useFullResumeID = Omit
    										lateNonCriticalExtension = Omit
    										nonCriticalExtension = Omit
    						SIs = Omit
    						SegmentedSIs = Omit
    				PcchConfig
    					SearchSpaceAndDci
    						AssignedBWPs
    							ActiveBWP = Omit
    							InitialBWP = True
    							DedicatedBWPs
    						SearchSpaceType = cssType2 (3)
    						DciInfo
    							ResoureAssignment
    								ResourceAllocationType = resourceAllocationType1 (1)
    								FreqDomain
    									Automatic
    										FirstRbIndex = 7
    										MaxRbCnt = 17
    								TimeDomain
    									Index = 0000'B
    								TransportBlockScheduling
    									Automatic
    										TransportBlock1 = qpsk (0)
    										TransportBlock2 = Omit
    										RedundancyVersionList
    								HarqProcessConfig
    									None = True
    							VrbPrbMapping
    								Index = 0'B
    							Format
    								Format_1_0_P_RNTI
    									ShortMessageIndicator = 01'B
    									ShortMessages = 00000000'B
    									TbScaling = 00'B
    				RachProcedureConfig
    					RachProcedureList
    						NR_RachProcedure_Type
    							RandomAccessResponse
    								SearchSpaceAndDci
    									AssignedBWPs
    										ActiveBWP = Omit
    										InitialBWP = True
    										DedicatedBWPs
    									SearchSpaceType = cssType1 (2)
    									DciInfo
    										ResoureAssignment
    											ResourceAllocationType = resourceAllocationType1 (1)
    											FreqDomain
    												Automatic
    													FirstRbIndex = 7
    													MaxRbCnt = 17
    											TimeDomain
    												Index = 0000'B
    											TransportBlockScheduling
    												Automatic
    													TransportBlock1 = qpsk (0)
    													TransportBlock2 = Omit
    													RedundancyVersionList
    											HarqProcessConfig
    												None = True
    										VrbPrbMapping
    											Index = 0'B
    										Format
    											Format_1_0_RA_RNTI
    												TbScaling = 00'B
    								MacPdu
    									SubPduList
    										NR_RAR_SubPdu_Type
    											RapIdAndPayload
    												RapId
    													Automatic = True
    												Payload
    													TimingAdvance = 0
    													UplinkGrant
    														HoppingFlag = 0'B
    														Msg3FrequencyResourceAllocation = 00001010001000'B
    														Msg3TimeResourceAllocation = 0001'B
    														MCS = 0010'B
    														TPC_Command = 011'B
    														CQI_Req = 0'B
    													TempC_RNTI
    														SameAsC_RNTI = True
    									CrcError = False
    							ContentionResolution
    								Msg4_Based
    									SearchSpaceAndDci
    										AssignedBWPs
    											ActiveBWP = Omit
    											InitialBWP = True
    											DedicatedBWPs
    										SearchSpaceType = cssType1 (2)
    										DciInfo
    											ResoureAssignment
    												ResourceAllocationType = resourceAllocationType1 (1)
    												FreqDomain
    													Automatic
    														FirstRbIndex = 7
    														MaxRbCnt = 17
    												TimeDomain
    													Index = 0000'B
    												TransportBlockScheduling
    													Automatic
    														TransportBlock1 = qam64 (2)
    														TransportBlock2 = Omit
    														RedundancyVersionList
    															NR_RedundancyVersion_Type = 0
    															NR_RedundancyVersion_Type = 2
    															NR_RedundancyVersion_Type = 3
    															NR_RedundancyVersion_Type = 1
    															NR_RedundancyVersion_Type = 0
    												HarqProcessConfig
    													AnyProcess = True
    											VrbPrbMapping
    												Index = 0'B
    											Format
    												Format_1_0
    													DAI
    														Index = 00'B
    													TpcCommandPucch
    														Value = 01'B
    													PucchResourceIndicator
    														Value = 000'B
    													PdschHarqTimingIndicator
    														Value = 100'B
    									ContentionResolutionId
    										XorMask = 000000000000000000000000000000000000000000000000'B
    									RrcPdu
    										RrcCcchMsg = '20400406C2E0048020C3CC00F8023E907041945D4001010025B0191006E10840002242DA00000024100001074C04CD55D270700041030814307A7102450B183470FFCC7102450B183470FFC67102450B183470F1F80000000430200000096080000014C18000002D84000000630A000000D618000001CC380000428062000004B0C4800009658A000012D316000025B63000004B8C6800009758E000012F31E000030A0F2BCAF28604A407234567897D421084000CD01A4921E2AE00C10A00400018FFD29498C637281E00002191940402000000001F82000008848A80'O
    									CrcError = False
    				CcchDcchDtchConfig
    					DL
    						SearchSpaceAndDci
    							AssignedBWPs
    								ActiveBWP = True
    								InitialBWP = Omit
    								DedicatedBWPs
    							SearchSpaceType = ussDL (5)
    							DciInfo
    								ResoureAssignment
    									ResourceAllocationType = resourceAllocationType1 (1)
    									FreqDomain
    										Automatic
    											FirstRbIndex = 7
    											MaxRbCnt = 17
    									TimeDomain
    										Index = 0'B
    									TransportBlockScheduling
    										Automatic
    											TransportBlock1 = qam64 (2)
    											TransportBlock2 = Omit
    											RedundancyVersionList
    												NR_RedundancyVersion_Type = 0
    												NR_RedundancyVersion_Type = 2
    												NR_RedundancyVersion_Type = 3
    												NR_RedundancyVersion_Type = 1
    												NR_RedundancyVersion_Type = 0
    									HarqProcessConfig
    										AnyProcess = True
    								VrbPrbMapping
    									Index = 0'B
    								Format
    									Format_1_1
    										CarrierIndicator
    											None = True
    										BWPIndicator
    											Index = 'B
    										PrbBundlingSizeIndicator
    											None = True
    										RateMatchingIndicator
    											Bitmap = 'B
    										ZP_CSI_RS_Trigger
    											Index = 'B
    										DAI
    											SingleServingCell = 00'B
    										TpcCommandPucch
    											Value = 01'B
    										PucchResourceIndicator
    											Value = 000'B
    										PdschHarqTimingIndicator
    											Value = 011'B
    										AntennaPorts
    											Index = 0000'B
    										TCI
    											None = True
    										SrsRequest
    											SingleUL = 00'B
    										CBGTI
    											Bitmap = 'B
    										CBGFI
    											None = True
    										DmrsSequenceInit
    											Value = 0'B
    					UL
    						SearchSpaceAndDci
    							AssignedBWPs
    								ActiveBWP = True
    								InitialBWP = Omit
    								DedicatedBWPs
    							SearchSpaceType = ussUL (6)
    							DciInfo
    								ResoureAssignment
    									ResourceAllocationType = resourceAllocationType1 (1)
    									FreqDomain
    										FirstRbIndex = 0
    										Nprb = 24
    									TimeDomain
    										Index = 0'B
    									TransportBlockScheduling
    										NR_TransportBlockSingleTransmission_Type
    											TimingOffset
    												None = True
    											ImcsValue = 9
    											RedundancyVersion = 0
    											ToggleNDI = True
    									HarqProcessConfig
    										AnyProcess = True
    								PuschHoppingCtrl
    									None = True
    								TpcCommandPusch
    									Value = 01'B
    								UL_SUL_Indicator
    									None = True
    								Format
    									Format_0_1
    										CarrierIndicator
    											None = True
    										BWPIndicator
    											Index = 'B
    										FirstDAI
    											SemiStaticCodebook = 0'B
    										SecondDAI
    											None = True
    										SrsResourceIndicator
    											CodeBook = 'B
    										PrecodingInfo
    											CodeBook = 'B
    										AntennaPorts
    											Index = 000'B
    										SrsRequest
    											SingleUL = 00'B
    										CsiRequest
    											Index = 'B
    										CBGTI
    											Index = 'B
    										PtrsDmrsAssociation
    											None = True
    										BetaOffsetIndicator
    											None = True
    										DmrsSequenceInit
    											Value = 0'B
    										UlschIndicator
    											Value = 1'B
    						PUCCH_Synch
    							None = True
    						GrantConfig
    							None = True
    					DrxCtrl
    						None = True
    					MeasGapCtrl
    						None = True
    				ServingCellConfig
    					SpCell
    						ServingCellIndex = 0
    						CellGroupConfig
    							CellGroupId = 0
    							SCellList
    							MAC_CellGroupConfig
    								R15
    									drx_Config = Omit
    									schedulingRequestConfig
    										schedulingRequestToAddModList
    											SchedulingRequestToAddMod
    												schedulingRequestId = 0
    												sr_ProhibitTimer = Omit
    												sr_TransMax = n16 (2)
    										schedulingRequestToReleaseList = Omit
    									bsr_Config
    										periodicBSR_Timer = infinity_ (15)
    										retxBSR_Timer = sf10240 (10)
    										logicalChannelSR_DelayTimer = Omit
    									tag_Config
    										tag_ToReleaseList = Omit
    										tag_ToAddModList
    											TAG
    												tag_Id = 0
    												timeAlignmentTimer = infinity_ (7)
    									phr_Config
    										release = Null
    									skipUplinkTxDynamic = False
    									csi_Mask = Omit
    									dataInactivityTimer = Omit
    							PhysicalCellGroupConfig
    								R15
    									harq_ACK_SpatialBundlingPUCCH = Omit
    									harq_ACK_SpatialBundlingPUSCH = Omit
    									p_NR_FR1 = 20
    									pdsch_HARQ_ACK_Codebook = dynamic (1)
    									tpc_SRS_RNTI = Omit
    									tpc_PUCCH_RNTI = Omit
    									tpc_PUSCH_RNTI = Omit
    									sp_CSI_RNTI = Omit
    									cs_RNTI = Omit
    									mcs_C_RNTI = Omit
    									p_UE_FR1 = Omit
    									xScale = Omit
    									pdcch_BlindDetection = Omit

    Sent from port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		Cell = True

    Received on port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		RadioBearerList
    			NR_RadioBearer_Type
    				Id
    					Srb = 0
    				Config
    					AddOrReconfigure
    						Sdap
    							None = True
    						Pdcp
    							None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										TM = True
    									TestMode
    										None = True
    								LogicalChannelId = Omit
    								Mac
    									LogicalChannel
    										Priority = 1
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit
    			NR_RadioBearer_Type
    				Id
    					Srb = 1
    				Config
    					AddOrReconfigure
    						Sdap
    							None = True
    						Pdcp
    							RBTerminating
    								RbConfig
    									Params
    										Rb
    											Srb = True
    								LinkToOtherCellGroup
    									None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										AM
    											Tx
    												R15
    													sn_FieldLength = size12 (0)
    													t_PollRetransmit = ms45 (8)
    													pollPDU = infinity_ (23)
    													pollByte = infinity_ (43)
    													maxRetxThreshold = t8 (5)
    											Rx
    												R15
    													sn_FieldLength = size12 (0)
    													t_Reassembly = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    									TestMode
    										None = True
    								LogicalChannelId = 1
    								Mac
    									LogicalChannel
    										Priority = 1
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit
    			NR_RadioBearer_Type
    				Id
    					Srb = 2
    				Config
    					AddOrReconfigure
    						Sdap
    							None = True
    						Pdcp
    							RBTerminating
    								RbConfig
    									Params
    										Rb
    											Srb = True
    								LinkToOtherCellGroup
    									None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										AM
    											Tx
    												R15
    													sn_FieldLength = size12 (0)
    													t_PollRetransmit = ms45 (8)
    													pollPDU = infinity_ (23)
    													pollByte = infinity_ (43)
    													maxRetxThreshold = t8 (5)
    											Rx
    												R15
    													sn_FieldLength = size12 (0)
    													t_Reassembly = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    									TestMode
    										None = True
    								LogicalChannelId = 2
    								Mac
    									LogicalChannel
    										Priority = 3
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit

    Sent from port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		RadioBearerList = True

    Received on port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		CellAttenuationList
    			NR_CellAttenuationConfig_Type
    				CellId = nr_Cell1 (1)
    				Attenuation
    					Value = 0
    				TimingInfo = Omit

    Sent from port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		CellAttenuationList = True

    Received on port: NR5GC_PTC:SYS

    ConstraintMismatch::Received:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = CNF_REQUIRED (1)
    ConstraintMismatch::Expected:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		CnfReq = NO_CNF_REQUIRED (0)

    Message Mismatch: Ut_CnfReq_Type

    UT_COMMON_CMD
    	Cmd = SWITCH_ON (115)
    	CnfReq = NO_CNF_REQUIRED (0)
    	ParameterList = Omit

    Inter-component message: PTC_Ut -> MTC_NR5GC:PTC_Ut

    ConstraintMismatch::Received:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = LOCAL_CNF_REQUIRED (2)
    ConstraintMismatch::Expected:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		CnfReq = NO_CNF_REQUIRED (0)

    Message Mismatch: Ut_CnfReq_Type

    ConstraintMismatch::Received:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = CNF_REQUIRED (1)
    ConstraintMismatch::Expected:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		CnfReq = NO_CNF_REQUIRED (0)

    Message Mismatch: Ut_CnfReq_Type

    IMS_IPCAN_Coordination_MSG
    	IPCAN_IMS_Control
    		Reset = True

    Inter-component message: IPCAN -> IMS_PTC:IPCAN

    ConstraintMismatch::Received:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = LOCAL_CNF_REQUIRED (2)
    ConstraintMismatch::Expected:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		CnfReq = NO_CNF_REQUIRED (0)

    Message Mismatch: Ut_CnfReq_Type

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		Cell
    			AddOrReconfigure
    				StaticResourceConfig = Omit
    				CellConfigCommon = Omit
    				PhysicalLayer = Omit
    				BcchConfig = Omit
    				PcchConfig = Omit
    				RachProcedureConfig = Omit
    				CcchDcchDtchConfig
    					DL = Omit
    					UL
    						SearchSpaceAndDci
    							AssignedBWPs = Omit
    							SearchSpaceType = Omit
    							DciInfo
    								ResoureAssignment
    									ResourceAllocationType = Omit
    									FreqDomain
    										FirstRbIndex = 0
    										Nprb = 24
    									TimeDomain = Omit
    									TransportBlockScheduling
    										NR_TransportBlockSingleTransmission_Type
    											TimingOffset
    												None = True
    											ImcsValue = 9
    											RedundancyVersion = 0
    											ToggleNDI = True
    									HarqProcessConfig = Omit
    								PuschHoppingCtrl = Omit
    								TpcCommandPusch = Omit
    								UL_SUL_Indicator = Omit
    								Format = Omit
    						PUCCH_Synch
    							None = True
    						GrantConfig
    							OnSR_Reception = True
    					DrxCtrl = Omit
    					MeasGapCtrl = Omit
    				ServingCellConfig = Omit

    Sent from port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		Cell = True

    Received on port: NR5GC_PTC:SYS

    UT_SYSTEM_REQ
    	Cmd
    		MMI
    			Cmd = 'SWITCH_ON'
    			ParameterList = Omit
    	CnfRequired = NO_CNF_REQUIRED (0)

    Sent from port: MTC_NR5GC:Ut

    UL-CCCH-Message
    	message = c1 = rrcSetupRequest =
    		rrcSetupRequest
    			ue-Identity = randomValue = 100111100011000110010100001001111111010
    			establishmentCause = mo-Signalling
    			spare = 0

    rrcSetupRequest

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 0
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 581
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Ccch
    			message_
    				c1
    					rrcSetupRequest
    						rrcSetupRequest
    							ue_Identity
    								randomValue = 100111100011000110010100001001111111010'B
    							establishmentCause = mo_Signalling (3)
    							spare = 0'B

    Received on port: NASEMU_NRNG_PTC:SYS_SRB

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 0
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 581
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Ccch
    				message_
    					c1
    						rrcSetupRequest
    							rrcSetupRequest
    								ue_Identity
    									randomValue = 100111100011000110010100001001111111010'B
    								establishmentCause = mo_Signalling (3)
    								spare = 0'B
    		Nas = Omit

    Inter-component message: SRB -> NR5GC_PTC:SRB

    REGISTRATION REQUEST
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Spare Half Octet [4 bits] = 0x0 [ 0 ]
    	reg_req_mt [8 bits] = 0x41 [ 65 ]
    	NAS key set identifierASME
    		Type of security context flag [1 bit] = 0x0 [ 0 ]
    		key sequence indicator [3 bits] = 0x0 [ 0 ]
    	s_reg_tp
    		for_f [1 bit] = 0x1 [ 1 ]
    		s_val [3 bits] = 0x1 [ 1 ]
    	s_mob_id
    		IE Length [16 bits] = 0xB [ 11 ]
    		id_dig [4 bits] = 0xF [ 15 ]
    		Spare Bits [1 bit] = 0x0 [ 0 ]
    		typ_id [3 bits] = 0x2 [ 2 ]
    		mcc_dig_2 [4 bits] = 0x0 [ 0 ]
    		mcc_dig_1 [4 bits] = 0x0 [ 0 ]
    		Mobile Network Code 3rd Digit [4 bits] = 0xF [ 15 ]
    		Mobile Country Code 3rd Digit [4 bits] = 0x1 [ 1 ]
    		mnc_dig_2 [4 bits] = 0x1 [ 1 ]
    		mnc_dig_1 [4 bits] = 0x0 [ 0 ]
    		amf_reg_id = 0xFE [ 254 ]
    		amf_set_id = 0x00 [ 0 ]
    		amf_set_id_conti [2 bits] = 0x1 [ 1 ]
    		amf_pntr [6 bits] = 0x1 [ 1 ]
    		fiveg_tmsi = 0xC2345678 [ 3258209912 ]
    	ue_sec_cap
    		IE Identifier [8 bits] = 0x2E [ 46 ]
    		IE Length [8 bits] = 0x2 [ 2 ]
    		ea0_128 [1 bit] = 0x1 [ 1 ]
    		ea1_128 [1 bit] = 0x1 [ 1 ]
    		ea2_128 [1 bit] = 0x1 [ 1 ]
    		ea3 [1 bit] = 0x1 [ 1 ]
    		ea4 [1 bit] = 0x0 [ 0 ]
    		ea5 [1 bit] = 0x0 [ 0 ]
    		ea6 [1 bit] = 0x0 [ 0 ]
    		ea7 [1 bit] = 0x0 [ 0 ]
    		ia0 [1 bit] = 0x1 [ 1 ]
    		ia1_128 [1 bit] = 0x1 [ 1 ]
    		ia2_128 [1 bit] = 0x1 [ 1 ]
    		ia3 [1 bit] = 0x1 [ 1 ]
    		ia4 [1 bit] = 0x0 [ 0 ]
    		ia5 [1 bit] = 0x0 [ 0 ]
    		ia6 [1 bit] = 0x0 [ 0 ]
    		ia7 [1 bit] = 0x0 [ 0 ]
    	nas_msg_container
    		IE Identifier [8 bits] = 0x71 [ 113 ]
    		IE Length [16 bits] = 0x2F [ 47 ]
    		container = 0xD50AE214749EE9C998C4D21A2C31BE77D340FA5CED99AA490379CD2CADCB2DB04189B67E0E380E34EC073156C5ED3A

    REGISTRATION REQUEST PDU

    UL-DCCH-Message
    	message = c1 = rrcSetupComplete =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcSetupComplete =
    			selectedPLMN-Identity = 1
    			registeredAMF
    				amf-Identifier = 111111100000000001000001
    			guami-Type = native
    			dedicatedNAS-Message = 7E01FDF12E97097E004109000BF200F110FE0041C23456782E02F0F071002FD50AE214749EE9C998C4D21A2C31BE77D340FA5CED99AA490379CD2CADCB2DB04189B67E0E380E34EC073156C5ED3A

    rrcSetupComplete

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 583
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcSetupComplete
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcSetupComplete
    								selectedPLMN_Identity = 1
    								registeredAMF
    									plmn_Identity = Omit
    									amf_Identifier = 111111100000000001000001'B
    								guami_Type = native (0)
    								s_NSSAI_List = Omit
    								dedicatedNAS_Message = '7E01FDF12E97097E004109000BF200F110FE0041C23456782E02F0F071002FD50AE214749EE9C998C4D21A2C31BE77D340FA5CED99AA490379CD2CADCB2DB04189B67E0E380E34EC073156C5ED3A'O
    								ng_5G_S_TMSI_Value = Omit
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Received on port: NASEMU_NRNG_PTC:SYS_SRB

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 583
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcSetupComplete
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcSetupComplete
    									selectedPLMN_Identity = 1
    									registeredAMF
    										plmn_Identity = Omit
    										amf_Identifier = 111111100000000001000001'B
    									guami_Type = native (0)
    									s_NSSAI_List = Omit
    									dedicatedNAS_Message = '7E01FDF12E97097E004109000BF200F110FE0041C23456782E02F0F071002FD50AE214749EE9C998C4D21A2C31BE77D340FA5CED99AA490379CD2CADCB2DB04189B67E0E380E34EC073156C5ED3A'O
    									ng_5G_S_TMSI_Value = Omit
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0001'B
    					NasCount = '00000009'O
    				Pdu
    					Msg
    						registration_Request
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01000001'B
    							ngNasKSI
    								iei = Omit
    								tsc = 0'B
    								nasKeySetId = 000'B
    							registrationType
    								fOR = 1'B
    								registrationType = 001'B
    							ngMobileId
    								iei = Omit
    								iel = '000B'O
    								idDigit1 = 1111'B
    								oddEvenInd = 0'B
    								typeOfId = 010'B
    								otherDigits = '00F110FE0041C2345678'O
    							nonCurrentNativeKSI = Omit
    							gmmCapability = Omit
    							ueSecurityCapability
    								iei = '2E'O
    								iel = '02'O
    								ngeaCap = 'F0'O
    								ngiaCap = 'F0'O
    								eeaCap = Omit
    								eiaCap = Omit
    								spare = Omit
    							requestedNSSAI = Omit
    							lastVisitedRegisteredTai = Omit
    							s1_UE_Capability = Omit
    							ulDataStatus = Omit
    							pduSessionStatus = Omit
    							micoInd = Omit
    							ueStatus = Omit
    							additionalGUTI = Omit
    							allowedPDUSessionStatus = Omit
    							ueUsageSetting = Omit
    							reqDRXParams = Omit
    							epsMessage = Omit
    							ladnInd = Omit
    							payloadContainerType = Omit
    							payload = Omit
    							networkSlicingInd = Omit
    							updateType = Omit
    							nasMsg
    								iei = '71'O
    								iel = '002F'O
    								replayedNASMsgContainerValue = 'D50AE214749EE9C998C4D21A2C31BE77D340FA5CED99AA490379CD2CADCB2DB04189B67E0E380E34EC073156C5ED3A'O
    							epsBearerContextStatus = Omit
    					PiggybackedPduList = Omit

    Inter-component message: SRB -> NR5GC_PTC:SRB

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		Cell
    			AddOrReconfigure
    				StaticResourceConfig = Omit
    				CellConfigCommon = Omit
    				PhysicalLayer = Omit
    				BcchConfig = Omit
    				PcchConfig = Omit
    				RachProcedureConfig = Omit
    				CcchDcchDtchConfig
    					DL = Omit
    					UL
    						SearchSpaceAndDci
    							AssignedBWPs = Omit
    							SearchSpaceType = Omit
    							DciInfo = Omit
    						PUCCH_Synch
    							Auto
    								TimingAdvance = 31
    								TA_Period = 600
    						GrantConfig = Omit
    					DrxCtrl = Omit
    					MeasGapCtrl = Omit
    				ServingCellConfig = Omit

    Sent from port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		Cell = True

    Received on port: NR5GC_PTC:SYS

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc = Omit
    		Nas
    			NG_NAS_MSG_Request_Type
    				SecurityProtection
    					Status = 0000'B
    					ForceMacError = False
    				Pdu
    					Msg
    						authentication_Request
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01010110'B
    							spareHalfOctet2 = '0'H
    							ngNasKeySetId
    								iei = Omit
    								tsc = 0'B
    								nasKeySetId = 001'B
    							abba
    								iei = Omit
    								iel = '02'O
    								abbaValue = '0000'O
    							rand
    								iei = '21'O
    								randValue = 10100011110111100000110001101101001101100011111000110000110000110110010010100100000001111000111100011011111110001101010101110111'B
    							autn
    								iei = '20'O
    								iel = '10'O
    								aUTN = 00100001011100110111000001100100111000110011000010000000000000001110001010011001010001010010000101110011011100001110010011100011'B
    							eapMessage = Omit
    					PiggybackedPduList = Omit

    Inter-component message: TC_SRB -> NASEMU_NRNG_PTC:TC_SRB

    Authentication Request
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	shoct1 [4 bits] = 0x0 [ 0 ]
    	auth_mt [8 bits] = 0x56 [ 86 ]
    	shoct2 [4 bits] = 0x0 [ 0 ]
    	NAS key set identifierASME
    		Type of security context flag [1 bit] = 0x0 [ 0 ]
    		key sequence indicator [3 bits] = 0x1 [ 1 ]
    	abba
    		IE Length [8 bits] = 0x2 [ 2 ]
    		abb = 0x0000 [ 0 ]
    	Authentication Parameter Rand
    		IE Identifier [8 bits] = 0x21 [ 33 ]
    		Authentication parameter random = 0xA3DE0C6D363E30C364A4078F1BF8D577
    	Authentication Parameter AUTN
    		IE Identifier [8 bits] = 0x20 [ 32 ]
    		IE Length [8 bits] = 0x10 [ 16 ]
    		value = 0x21737064E3308000E29945217370E4E3

    Authentication Request PDU

    DL-DCCH-Message
    	message = c1 = dlInformationTransfer =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = dlInformationTransfer =
    			dedicatedNAS-Message = 7E00560102000021A3DE0C6D363E30C364A4078F1BF8D577201021737064E3308000E29945217370E4E3

    dlInformationTransfer

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					dlInformationTransfer
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							dlInformationTransfer
    								dedicatedNAS_Message = '7E00560102000021A3DE0C6D363E30C364A4078F1BF8D577201021737064E3308000E29945217370E4E3'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Sent from port: NASEMU_NRNG_PTC:SYS_SRB

    Authentication Response
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Spare Half Octet [4 bits] = 0x0 [ 0 ]
    	Message Type [8 bits] = 0x57 - Authentication Response [ 87 ]
    	auth_res_param
    		IE Identifier [8 bits] = 0x2D [ 45 ]
    		IE Length [8 bits] = 0x10 [ 16 ]
    		Authentication response parameter information = 0x17530A83511B1D720BB31CB53FFB717C

    Authentication Response PDU

    UL-DCCH-Message
    	message = c1 = ulInformationTransfer =
    		criticalExtensions = ulInformationTransfer =
    			dedicatedNAS-Message = 7E0172126E1F0A7E00572D1017530A83511B1D720BB31CB53FFB717C

    ulInformationTransfer

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 592
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ulInformationTransfer
    						criticalExtensions
    							ulInformationTransfer
    								dedicatedNAS_Message = '7E0172126E1F0A7E00572D1017530A83511B1D720BB31CB53FFB717C'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Received on port: NASEMU_NRNG_PTC:SYS_SRB

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 592
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0001'B
    					NasCount = '0000000A'O
    				Pdu
    					Msg
    						authentication_Response
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01010111'B
    							authResponseParam
    								iei = '2D'O
    								iel = '10'O
    								res = 00010111010100110000101010000011010100010001101100011101011100100000101110110011000111001011010100111111111110110111000101111100'B
    							eapMessage = Omit
    					PiggybackedPduList = Omit

    Inter-component message: SRB -> NR5GC_PTC:SRB

    NG_NAS_CTRL_REQ
    	Common
    		ControlInfo
    			CnfFlag = True
    	Request
    		Security
    			StartRestart
    				Integrity
    					Algorithm = 0010'B
    					K_NAS = 01000101010001010001110011110011001111110110111101011011001000100100001011011001110000010101101110101111111110101001111110110001'B
    				Ciphering
    					Algorithm = 0010'B
    					K_NAS = 11010101000100100010100101101011110000000101100111110111110010010101110100011111110001110011111000010001000001100001101001111010'B
    				NasCountReset = True

    Inter-component message: CTRL -> NASEMU_NRNG_PTC:CTRL

    NG_NAS_CTRL_CNF
    	Common
    	Confirm
    		Security = True

    Inter-component message: NASCTRL -> NR5GC_PTC:NASCTRL

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc = Omit
    		Nas
    			NG_NAS_MSG_Request_Type
    				SecurityProtection
    					Status = 0011'B
    					ForceMacError = False
    				Pdu
    					Msg
    						security_Mode_Command
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01011101'B
    							nasSecurityAlgorithms
    								iei = Omit
    								cipheringType = 0010'B
    								integrityType = 0010'B
    							spareHalfOctet2 = '0'H
    							ngNasKSI
    								iei = Omit
    								tsc = 0'B
    								nasKeySetId = 001'B
    							ueSecurityCapability
    								iei = Omit
    								iel = '02'O
    								ngeaCap = 'F0'O
    								ngiaCap = 'F0'O
    								eeaCap = Omit
    								eiaCap = Omit
    								spare = Omit
    							imeisvRequest = Omit
    							epsSecurityAlgorithms = Omit
    							add5GSecurityInfo
    								iei = '36'O
    								iel = '03'O
    								spareBits = 000000'B
    								rinmr = 1'B
    								hdp = 0'B
    							eapMessage = Omit
    							abba = Omit
    							replayedUESecurityCap = Omit
    					PiggybackedPduList = Omit

    Inter-component message: TC_SRB -> NASEMU_NRNG_PTC:TC_SRB

    Security Mode Command
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Spare Half Octet [4 bits] = 0x0 [ 0 ]
    	Message Type [8 bits] = 0x5D - Security Mode Command [ 93 ]
    	sel_nas_secu_alg
    		Type of ciphering algorithm [4 bits] = 0x2 [ 2 ]
    		Type of integrity protection algorithm [4 bits] = 0x2 [ 2 ]
    	shoct1 [4 bits] = 0x0 [ 0 ]
    	ngksi
    		Type of security context flag [1 bit] = 0x0 [ 0 ]
    		key sequence indicator [3 bits] = 0x1 [ 1 ]
    	replay_ue_secu_cap
    		IE Length [8 bits] = 0x2 [ 2 ]
    		ea0_128 [1 bit] = 0x1 [ 1 ]
    		ea1_128 [1 bit] = 0x1 [ 1 ]
    		ea2_128 [1 bit] = 0x1 [ 1 ]
    		ea3 [1 bit] = 0x1 [ 1 ]
    		ea4 [1 bit] = 0x0 [ 0 ]
    		ea5 [1 bit] = 0x0 [ 0 ]
    		ea6 [1 bit] = 0x0 [ 0 ]
    		ea7 [1 bit] = 0x0 [ 0 ]
    		ia0 [1 bit] = 0x1 [ 1 ]
    		ia1_128 [1 bit] = 0x1 [ 1 ]
    		ia2_128 [1 bit] = 0x1 [ 1 ]
    		ia3 [1 bit] = 0x1 [ 1 ]
    		ia4 [1 bit] = 0x0 [ 0 ]
    		ia5 [1 bit] = 0x0 [ 0 ]
    		ia6 [1 bit] = 0x0 [ 0 ]
    		ia7 [1 bit] = 0x0 [ 0 ]
    	add_fiveg_secu_info
    		IE Identifier [8 bits] = 0x36 [ 54 ]
    		length_addfiveg [8 bits] = 0x3 [ 3 ]
    		Spare Bits [6 bits] = 0x0 [ 0 ]
    		rinm_r [1 bit] = 0x1 [ 1 ]
    		hdp [1 bit] = 0x0 [ 0 ]

    Security Mode Command PDU

    DL-DCCH-Message
    	message = c1 = dlInformationTransfer =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = dlInformationTransfer =
    			dedicatedNAS-Message = 7E03A5738177007E005D220102F0F0360302

    dlInformationTransfer

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					dlInformationTransfer
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							dlInformationTransfer
    								dedicatedNAS_Message = '7E03A5738177007E005D220102F0F0360302'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Sent from port: NASEMU_NRNG_PTC:SYS_SRB

    UL-DCCH-Message
    	message = c1 = ulInformationTransfer =
    		criticalExtensions = ulInformationTransfer =
    			dedicatedNAS-Message = 7E0411B0F536005BC7BA28FB8F2E2269489049F88C0FAF43A3E49B52AF862E92ECB2AC874CF5F5125915C55C6B5AB224B88944B3BA38FDD4EE0E343B

    ulInformationTransfer

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 595
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ulInformationTransfer
    						criticalExtensions
    							ulInformationTransfer
    								dedicatedNAS_Message = '7E0411B0F536005BC7BA28FB8F2E2269489049F88C0FAF43A3E49B52AF862E92ECB2AC874CF5F5125915C55C6B5AB224B88944B3BA38FDD4EE0E343B'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Received on port: NASEMU_NRNG_PTC:SYS_SRB

    Security Mode Complete
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Spare Half Octet [4 bits] = 0x0 [ 0 ]
    	Message Type [8 bits] = 0x5E - Security Mode Complete [ 94 ]
    	NAS message container
    		IE Identifier [8 bits] = 0x71 [ 113 ]
    		IE Length [16 bits] = 0x2F [ 47 ]
    		NAS message contents = 0x7E004109000BF200F110FE0041C23456781001032E02F0F02F0201015200F1100000011707F0F0C040018030180100

    Security Mode Complete PDU

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 595
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0100'B
    					NasCount = '00000000'O
    				Pdu
    					Msg
    						security_Mode_Complete
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01011110'B
    							imeisv = Omit
    							nasMsg
    								iei = '71'O
    								iel = '002F'O
    								replayedNASMsgContainerValue = '7E004109000BF200F110FE0041C23456781001032E02F0F02F0201015200F1100000011707F0F0C040018030180100'O
    					PiggybackedPduList
    						NG_NAS_UL_Pdu_Type
    							Msg
    								registration_Request
    									protocolDiscriminator = 01111110'B
    									spareHalfOctet = '0'H
    									securityHeaderType = 0000'B
    									messageType = 01000001'B
    									ngNasKSI
    										iei = Omit
    										tsc = 0'B
    										nasKeySetId = 000'B
    									registrationType
    										fOR = 1'B
    										registrationType = 001'B
    									ngMobileId
    										iei = Omit
    										iel = '000B'O
    										idDigit1 = 1111'B
    										oddEvenInd = 0'B
    										typeOfId = 010'B
    										otherDigits = '00F110FE0041C2345678'O
    									nonCurrentNativeKSI = Omit
    									gmmCapability
    										iei = '10'O
    										iel = '01'O
    										spareBits = 00000'B
    										lpp = 0'B
    										hoAttach = 1'B
    										s1Cap = 1'B
    										spare = Omit
    									ueSecurityCapability
    										iei = '2E'O
    										iel = '02'O
    										ngeaCap = 'F0'O
    										ngiaCap = 'F0'O
    										eeaCap = Omit
    										eiaCap = Omit
    										spare = Omit
    									requestedNSSAI
    										iei = '2F'O
    										iel = '02'O
    										s_nssai
    											S_NSSAI_Type
    												iei = Omit
    												iel = '01'O
    												sst = '01'O
    												sd = Omit
    												mappedSST = Omit
    												mappedSD = Omit
    									lastVisitedRegisteredTai
    										iei = '52'O
    										plmnId = '00F110'O
    										tac = '000001'O
    									s1_UE_Capability
    										iei = '17'O
    										iel = '07'O
    										eeaCap = 11110000'B
    										eiaCap = 11110000'B
    										ueaCap = 11000000'B
    										uiaCap = 01000000'B
    										srvcc_LPP_ProSeCap = 00000001'B
    										cIoT_proSeCap = 10000000'B
    										cIoT_V2X = 00110000'B
    										spare = Omit
    									ulDataStatus = Omit
    									pduSessionStatus = Omit
    									micoInd = Omit
    									ueStatus = Omit
    									additionalGUTI = Omit
    									allowedPDUSessionStatus = Omit
    									ueUsageSetting
    										iei = '18'O
    										iel = '01'O
    										spare = 0000000'B
    										ueUsageSetting = 0'B
    									reqDRXParams = Omit
    									epsMessage = Omit
    									ladnInd = Omit
    									payloadContainerType = Omit
    									payload = Omit
    									networkSlicingInd = Omit
    									updateType = Omit
    									nasMsg = Omit
    									epsBearerContextStatus = Omit
    							PiggybackedPduList = Omit

    Inter-component message: SRB -> NR5GC_PTC:SRB

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc = Omit
    		Nas
    			NG_NAS_MSG_Request_Type
    				SecurityProtection
    					Status = 0010'B
    					ForceMacError = False
    				Pdu
    					Msg
    						activate_Test_Mode
    							skipIndicator = 0000'B
    							protocolDiscriminator = 1111'B
    							messageType = 10000100'B
    							ueTestLoopMode = '00'O
    					PiggybackedPduList = Omit

    Inter-component message: TC_SRB -> NASEMU_NRNG_PTC:TC_SRB

    Activate Test Mode
    	Protocol Discriminator [4 bits] = 0x0 - Group Call Control [ 0 ]
    	Transaction Identifier or Skip Indicator [4 bits] = 0xF [ 15 ]
    	Message Type [8 bits] = 0x84 - Activate Test Mode [ 132 ]
    	ue_testloop_mode [8 bits] = 0x0 [ 0 ]

    Activate Test Mode PDU

    DL-DCCH-Message
    	message = c1 = dlInformationTransfer =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = dlInformationTransfer =
    			dedicatedNAS-Message = 7E0234CC3BAE012927FA

    dlInformationTransfer

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					dlInformationTransfer
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							dlInformationTransfer
    								dedicatedNAS_Message = '7E0234CC3BAE012927FA'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Sent from port: NASEMU_NRNG_PTC:SYS_SRB

    UL-DCCH-Message
    	message = c1 = ulInformationTransfer =
    		criticalExtensions = ulInformationTransfer =
    			dedicatedNAS-Message = 7E022DAFBC04011989

    ulInformationTransfer

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 598
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ulInformationTransfer
    						criticalExtensions
    							ulInformationTransfer
    								dedicatedNAS_Message = '7E022DAFBC04011989'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Received on port: NASEMU_NRNG_PTC:SYS_SRB

    Activate Test Mode Complete
    	Protocol Discriminator [4 bits] = 0x0 - Group Call Control [ 0 ]
    	Transaction Identifier or Skip Indicator [4 bits] = 0xF [ 15 ]
    	Message Type [8 bits] = 0x85 - Activate Test Mode Complete [ 133 ]

    Activate Test Mode Complete PDU

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 598
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0010'B
    					NasCount = '00000001'O
    				Pdu
    					Msg
    						activate_Test_Mode_Complete
    							skipIndicator = 0000'B
    							protocolDiscriminator = 1111'B
    							messageType = 10000101'B
    					PiggybackedPduList = Omit

    Inter-component message: SRB -> NR5GC_PTC:SRB

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		PdcpCount
    			Get
    				AllRBs = True

    Sent from port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		PdcpCount
    			Get
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 1
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000100'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000011'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 2
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B

    Received on port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		AS_Security
    			StartRestart
    				Integrity
    					Algorithm = nia2 (2)
    					KRRCint = 01111000000000111001000110110000011011000100010010001100011100101110100011110010011101110101010111111010000111001100011111111111'B
    					KUPint = 01001000000011110101001100110111100110001001100110011100011101100001010000111111001111111001001101101101000001001000100110011110'B
    					ActTimeList = Omit
    				Ciphering
    					Algorithm = nea2 (2)
    					KRRCenc = 11000000001001111111010101010010011111110001000110110000101111010111010010101010100110101010001110010110001101101111001000000101'B
    					KUPenc = 10100111000111010011000011010011001100000110010100010011111000110100110010100111001000001101100110100011011011100110110011100110'B
    					ActTimeList
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 1
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 5
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 4
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 2
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0

    Sent from port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		AS_Security = True

    Received on port: NR5GC_PTC:SYS

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						securityModeCommand
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								securityModeCommand
    									securityConfigSMC
    										securityAlgorithmConfig
    											cipheringAlgorithm = nea2 (2)
    											integrityProtAlgorithm = nia2 (2)
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: TC_SRB -> NASEMU_NRNG_PTC:TC_SRB

    DL-DCCH-Message
    	message = c1 = securityModeCommand =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = securityModeCommand =
    			securityConfigSMC
    				securityAlgorithmConfig
    					cipheringAlgorithm = nea2
    					integrityProtAlgorithm = nia2

    securityModeCommand

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					securityModeCommand
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							securityModeCommand
    								securityConfigSMC
    									securityAlgorithmConfig
    										cipheringAlgorithm = nea2 (2)
    										integrityProtAlgorithm = nia2 (2)
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Sent from port: NASEMU_NRNG_PTC:SYS_SRB

    UL-DCCH-Message
    	message = c1 = securityModeComplete =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = securityModeComplete =

    securityModeComplete

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 604
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					securityModeComplete
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							securityModeComplete
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Received on port: NASEMU_NRNG_PTC:SYS_SRB

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 604
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						securityModeComplete
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								securityModeComplete
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: SRB -> NR5GC_PTC:SRB

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						ueCapabilityEnquiry
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								ueCapabilityEnquiry
    									ue_CapabilityRAT_RequestList
    										UE_CapabilityRAT_Request
    											rat_Type = nr (0)
    											capabilityRequestFilter = Omit
    									lateNonCriticalExtension = Omit
    									ue_CapabilityEnquiryExt = Omit
    		Nas = Omit

    Inter-component message: TC_SRB -> NASEMU_NRNG_PTC:TC_SRB

    DL-DCCH-Message
    	message = c1 = ueCapabilityEnquiry =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = ueCapabilityEnquiry =
    			ue-CapabilityRAT-RequestList = SEQUENCE OF UE-CapabilityRAT-Request
    				UE-CapabilityRAT-Request(1)
    					rat-Type = nr

    ueCapabilityEnquiry

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ueCapabilityEnquiry
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							ueCapabilityEnquiry
    								ue_CapabilityRAT_RequestList
    									UE_CapabilityRAT_Request
    										rat_Type = nr (0)
    										capabilityRequestFilter = Omit
    								lateNonCriticalExtension = Omit
    								ue_CapabilityEnquiryExt = Omit

    Sent from port: NASEMU_NRNG_PTC:SYS_SRB

    UL-DCCH-Message
    	message = c1 = ueCapabilityInformation =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = ueCapabilityInformation =
    			ue-CapabilityRAT-ContainerList = SEQUENCE OF UE-CapabilityRAT-Container
    				UE-CapabilityRAT-Container(1)
    					rat-Type = nr
    					ue-CapabilityRAT-Container =

    ueCapabilityInformation

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 610
    				Subframe
    					Number = 4
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ueCapabilityInformation
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							ueCapabilityInformation
    								ue_CapabilityRAT_ContainerList
    									UE_CapabilityRAT_Container
    										rat_Type = nr (0)
    										ue_CapabilityRAT_Container = ' 'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Received on port: NASEMU_NRNG_PTC:SYS_SRB

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 610
    				Subframe
    					Number = 4
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						ueCapabilityInformation
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								ueCapabilityInformation
    									ue_CapabilityRAT_ContainerList
    										UE_CapabilityRAT_Container
    											rat_Type = nr (0)
    											ue_CapabilityRAT_Container = ' 'O
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: SRB -> NR5GC_PTC:SRB

    ConstraintMismatch::Received:
    summary = Message Mismatch: IntegerType
    MATCH_MISMATCH
    	Message Mismatch: IntegerType
    		bandNR = 3
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IntegerType
    MATCH_MISMATCH
    	Message Mismatch: IntegerType
    		IntegerType = 41

    Message Mismatch: IntegerType

    ConstraintMismatch::Received:
    summary = Message Mismatch: IntegerType
    MATCH_MISMATCH
    	Message Mismatch: IntegerType
    		bandNR = 28
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IntegerType
    MATCH_MISMATCH
    	Message Mismatch: IntegerType
    		IntegerType = 41

    Message Mismatch: IntegerType

    ConstraintMismatch::Received:
    summary = Message Mismatch: IntegerType
    MATCH_MISMATCH
    	Message Mismatch: IntegerType
    		bandNR = 38
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IntegerType
    MATCH_MISMATCH
    	Message Mismatch: IntegerType
    		IntegerType = 41

    Message Mismatch: IntegerType

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc = Omit
    		Nas
    			NG_NAS_MSG_Request_Type
    				SecurityProtection
    					Status = 0010'B
    					ForceMacError = False
    				Pdu
    					Msg
    						registration_Accept
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01000010'B
    							registrationResult
    								iel = '01'O
    								spare = 0000'B
    								smsAllowed = 0'B
    								resultValue = 001'B
    							guti
    								iei = '77'O
    								iel = '000B'O
    								idDigit1 = 1111'B
    								oddEvenInd = 0'B
    								typeOfId = 010'B
    								otherDigits = '00F110FE0041C2345678'O
    							equivalentPlmns = Omit
    							taiList
    								iei = '54'O
    								iel = '07'O
    								listOfPartialTais
    									NG_ListOfPartialTaiList
    										allowedType = 0'B
    										typeOfList = 00'B
    										numberOfElements = 00000'B
    										partialTaiList
    											type0List
    												NG_Type0Element
    													plmnId = '00F110'O
    													tacList
    														OctetStringType = '000001'O
    							allowedNSSAI
    								iei = '15'O
    								iel = '02'O
    								s_nssai
    									S_NSSAI_Type
    										iei = Omit
    										iel = '01'O
    										sst = '01'O
    										sd = Omit
    										mappedSST = Omit
    										mappedSD = Omit
    							rejectedNSSAI = Omit
    							configuredNSSAI = Omit
    							ngs_NetworkFeatureSupport
    								iei = '21'O
    								iel = '02'O
    								mpsi = 0'B
    								iwk_N26 = 0'B
    								emf = 00'B
    								emc = 00'B
    								imsVoPS_n3GPP = 0'B
    								imsVoPS_3GPP = 1'B
    								spareBits = 000000'B
    								mcsi = 0'B
    								emcn3 = 0'B
    								spare = Omit
    							pduSessionStatus = Omit
    							pduSessionReactivationResult = Omit
    							pduSessionReactResultError = Omit
    							ladnInfo = Omit
    							micoInd = Omit
    							networkSlicingInd = Omit
    							saiList = Omit
    							t3512Value
    								iei = '5E'O
    								iel = '01'O
    								unit = 111'B
    								gprsTimerValue = 00000'B
    							non3GPPDeregisterValue = Omit
    							t3502Value = Omit
    							emergencyNumberList = Omit
    							xtdEmergencyNumberList = Omit
    							sorTransparentContainer = Omit
    							eapMessage = Omit
    							inclusionModeNSSAI = Omit
    							operatorAccessCatDefs = Omit
    							negotiatedDRXParams = Omit
    							non3GPP_NW_ProvidedPolicies = Omit
    							epsBearerContextStatus = Omit
    					PiggybackedPduList = Omit

    Inter-component message: TC_SRB -> NASEMU_NRNG_PTC:TC_SRB

    REGISTRATION ACCEPT
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	shoct1 [4 bits] = 0x0 [ 0 ]
    	reg_acc_mt [8 bits] = 0x42 [ 66 ]
    	reg_res
    		IE Length [8 bits] = 0x1 [ 1 ]
    		Spare Bits [4 bits] = 0x0 [ 0 ]
    		sms_allowed [1 bit] = 0x0 [ 0 ]
    		val [3 bits] = 0x1 [ 1 ]
    	s_mob_id
    		IE Identifier [8 bits] = 0x77 [ 119 ]
    		IE Length [16 bits] = 0xB [ 11 ]
    		id_dig [4 bits] = 0xF [ 15 ]
    		Spare Bits [1 bit] = 0x0 [ 0 ]
    		typ_id [3 bits] = 0x2 [ 2 ]
    		mcc_dig_2 [4 bits] = 0x0 [ 0 ]
    		mcc_dig_1 [4 bits] = 0x0 [ 0 ]
    		Mobile Network Code 3rd Digit [4 bits] = 0xF [ 15 ]
    		Mobile Country Code 3rd Digit [4 bits] = 0x1 [ 1 ]
    		mnc_dig_2 [4 bits] = 0x1 [ 1 ]
    		mnc_dig_1 [4 bits] = 0x0 [ 0 ]
    		amf_reg_id = 0xFE [ 254 ]
    		amf_set_id = 0x00 [ 0 ]
    		amf_set_id_conti [2 bits] = 0x1 [ 1 ]
    		amf_pntr [6 bits] = 0x1 [ 1 ]
    		fiveg_tmsi = 0xC2345678 [ 3258209912 ]
    	Tracking area identity list
    		IE Identifier [8 bits] = 0x54 [ 84 ]
    		IE Length [8 bits] = 0x7 [ 7 ]
    		Spare Bits [1 bit] = 0x0 [ 0 ]
    		Type of list [2 bits] = 0x0 [ 0 ]
    		number of elements [5 bits] = 0x0 [ 0 ]
    		Mobile Country Code 1st and 2nd  Digits = 0x00 [ 0 ]
    		Mobile Network Code 3rd Digit = 0xF [ 15 ]
    		Mobile Country Code 3rd Digit = 0x1 [ 1 ]
    		Mobile Network Code 1st and 2nd  Digits = 0x10 [ 16 ]
    		Tracking area code 1 = 0x00 [ 0 ]
    		Tracking area code 1 continued = 0x0001 [ 1 ]
    	all_nssai
    		IE Identifier [8 bits] = 0x15 [ 21 ]
    		IE Length [8 bits] = 0x2 [ 2 ]
    		len_s_nssai [8 bits] = 0x1 [ 1 ]
    		sst = 0x01 [ 1 ]
    	nfs
    		IE Identifier [8 bits] = 0x21 [ 33 ]
    		IE Length [8 bits] = 0x2 [ 2 ]
    		mpsi [1 bit] = 0x0 [ 0 ]
    		iwk_n26 [1 bit] = 0x0 [ 0 ]
    		emf [2 bits] = 0x0 [ 0 ]
    		emc [2 bits] = 0x0 [ 0 ]
    		ims_vops_n [1 bit] = 0x0 [ 0 ]
    		IMS VoPS [1 bit] = 0x1 [ 1 ]
    		Spare Bits [6 bits] = 0x0 [ 0 ]
    		mcsi [1 bit] = 0x0 [ 0 ]
    		emcn [1 bit] = 0x0 [ 0 ]
    	t3512_val
    		IE Identifier [8 bits] = 0x5E [ 94 ]
    		IE Length [8 bits] = 0x1 [ 1 ]
    		Timer Value Unit [3 bits] = 0x7 - value indicates that the timer is deactivated [ 7 ]
    		Value [5 bits] = 0x0 [ 0 ]

    REGISTRATION ACCEPT PDU

    DL-DCCH-Message
    	message = c1 = dlInformationTransfer =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = dlInformationTransfer =
    			dedicatedNAS-Message = 7E024DA364690206F0C1B66387D383C8AA868DF92C7E43EB7C72B1D6350F0430B223864F74FB0248E2F5D961C817

    dlInformationTransfer

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					dlInformationTransfer
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							dlInformationTransfer
    								dedicatedNAS_Message = '7E024DA364690206F0C1B66387D383C8AA868DF92C7E43EB7C72B1D6350F0430B223864F74FB0248E2F5D961C817'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Sent from port: NASEMU_NRNG_PTC:SYS_SRB

    UL-DCCH-Message
    	message = c1 = ulInformationTransfer =
    		criticalExtensions = ulInformationTransfer =
    			dedicatedNAS-Message = 7E02EB7440CC02EC344A

    ulInformationTransfer

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 616
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ulInformationTransfer
    						criticalExtensions
    							ulInformationTransfer
    								dedicatedNAS_Message = '7E02EB7440CC02EC344A'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Received on port: NASEMU_NRNG_PTC:SYS_SRB

    REGISTRATION COMPLETE
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Spare Half Octet [4 bits] = 0x0 [ 0 ]
    	reg_comp_msg_id = 0x43 [ 67 ]

    REGISTRATION COMPLETE PDU

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 616
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0010'B
    					NasCount = '00000002'O
    				Pdu
    					Msg
    						registration_Complete
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01000011'B
    							sorTransparentContainer
    								iei = Omit
    								iel = Omit
    								header = Omit
    								mac = Omit
    								counter = Omit
    								data = Omit
    					PiggybackedPduList = Omit

    Inter-component message: SRB -> NR5GC_PTC:SRB

    UL-DCCH-Message
    	message = c1 = ulInformationTransfer =
    		criticalExtensions = ulInformationTransfer =
    			dedicatedNAS-Message = 7E02D873F81E03685E1800B9F77D78AF91D6777A840D49D9696088370AE5B1448FF4

    ulInformationTransfer

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 987
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ulInformationTransfer
    						criticalExtensions
    							ulInformationTransfer
    								dedicatedNAS_Message = '7E02D873F81E03685E1800B9F77D78AF91D6777A840D49D9696088370AE5B1448FF4'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Received on port: NASEMU_NRNG_PTC:SYS_SRB

    PDU SESSION ESTABLISHMENT REQUEST
    	Extended protocol discriminator = 0x2E [ 46 ]
    	pdu_sesn_id [8 bits] = 0x5 [ 5 ]
    	pti [8 bits] = 0xD [ 13 ]
    	pdu_sesn_est_req_msg_id [8 bits] = 0xC1 [ 193 ]
    	int_pro_max_dr
    		max_up = 0xFF [ 255 ]
    		max_dl = 0xFF [ 255 ]
    	pdu_sesn_typ
    		IE Identifier [4 bits] = 0x9 [ 9 ]
    		Spare Bits [1 bit] = 0x0 [ 0 ]
    		pdu_sesn_type [3 bits] = 0x1 [ 1 ]
    	ssc_mode
    		IE Identifier [4 bits] = 0xA [ 10 ]
    		Value [4 bits] = 0x1 [ 1 ]
    	extd_prt_config_opt
    		IE Identifier [8 bits] = 0x7B [ 123 ]
    		IE Length [16 bits] = 0x7 [ 7 ]
    		ex_contents = 0x80000A00000D00

    PDU SESSION ESTABLISHMENT REQUEST PDU

    UL NAS TRANSPORT
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Spare Half Octet [4 bits] = 0x0 [ 0 ]
    	Message Type [8 bits] = 0x67 - UL NAS TRANSPORT [ 103 ]
    	payload_typ
    		val [4 bits] = 0x0 [ 0 ]
    	shoct2 [4 bits] = 0x1 [ 1 ]
    	payload_cont
    		IE Length [16 bits] = 0x12 [ 18 ]
    		val = 0x2E050DC1FFFF91A17B000780000A00000D00
    	pdu_sess_id
    		IE Identifier [8 bits] = 0x12 [ 18 ]
    		val = 0x05 [ 5 ]
    	req_typ
    		IE Identifier [4 bits] = 0x8 [ 8 ]
    		Spare Bits [1 bit] = 0x0 [ 0 ]
    		val [3 bits] = 0x1 [ 1 ]

    UL NAS TRANSPORT PDU

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 987
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0010'B
    					NasCount = '00000003'O
    				Pdu
    					Msg
    						ul_Nas_Transport
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01100111'B
    							spareHalfOctet2 = '0'H
    							payloadContainerType
    								iei = Omit
    								container = 0001'B
    							payload
    								iei = Omit
    								iel = '0012'O
    								payload = '2E050DC1FFFF91A17B000780000A00000D00'O
    							pduSessionId
    								iei = '12'O
    								sessionId = '05'O
    							oldPDUSessionId
    								iei = Omit
    								sessionId = Omit
    							requestType
    								iei = '8'H
    								spare = 0'B
    								requestValue = 001'B
    							s_NSSAI
    								iei = Omit
    								iel = Omit
    								sst = Omit
    								sd = Omit
    								mappedSST = Omit
    								mappedSD = Omit
    							dnn
    								iei = Omit
    								iel = Omit
    								dnnValue = Omit
    							additionalInfo
    								iei = Omit
    								iel = Omit
    								additionalInfo = Omit
    					PiggybackedPduList
    						NG_NAS_UL_Pdu_Type
    							Msg
    								pdu_Session_Establishment_Request
    									protocolDiscriminator = 00101110'B
    									pduSessionId
    										iei = Omit
    										sessionId = '05'O
    									procedureTransactionIdentifier = '0D'O
    									messageType = 11000001'B
    									integrityProtMaxDataRate
    										iei = Omit
    										maxDataRateUL = 'FF'O
    										maxDataRateDL = 'FF'O
    									pduSessionType
    										iei = '9'H
    										spare = 0'B
    										typeValue = 001'B
    									sscMode
    										iei = 'A'H
    										spare = 0'B
    										sscModeValue = 001'B
    									smCapability
    										iei = Omit
    										iel = Omit
    										spareBits = Omit
    										mh6_PDU = Omit
    										rQoS = Omit
    										spare = Omit
    									maxNumPacketFilters
    										iei = Omit
    										numOfFilters = Omit
    										spareBits = Omit
    									alwaysOnPDUSessionReq = Omit
    									smPDU_RequestContainer
    										iei = Omit
    										iel = Omit
    										dnSpecificId = Omit
    									extdProtocolConfigurationOptions
    										iei = '7B'O
    										iel = '0007'O
    										ext = 1'B
    										spare = 0000'B
    										configProtocol = 000'B
    										pco
    											ProtocolContainer
    												protocolID = '000A'O
    												protocolLength = '00'O
    												content = '000D00'O
    							PiggybackedPduList = Omit

    Inter-component message: SRB -> NR5GC_PTC:SRB

    ConstraintMismatch::Received:
    summary = Message Mismatch: NG_NAS_UL_Message_Type.pdu_Session_Establishment_Request.procedureTransactionIdentifier
    MATCH_MISMATCH
    	Message Mismatch: NG_NAS_UL_Message_Type.pdu_Session_Establishment_Request.procedureTransactionIdentifier
    		dnnValue = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: NG_NAS_UL_Message_Type.pdu_Session_Establishment_Request.procedureTransactionIdentifier
    MATCH_MISMATCH
    	Message Mismatch: NG_NAS_UL_Message_Type.pdu_Session_Establishment_Request.procedureTransactionIdentifier
    		OctetStringType = '03494D53'O

    Message Mismatch: NG_NAS_UL_Message_Type.pdu_Session_Establishment_Request.procedureTransactionIdentifier

    IP_ConfigReq_Type
    	StartPDN
    		PdnId = PDN_Internet (3)
    		DrbInfo
    			Nr5GC
    				CellId = nr_Cell1 (1)
    				QosFlow
    					PDU_SessionId = 5
    					QFI = 1

    Inter-component message: NR_CTRL -> IP_PTC:NR_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.10'
    				Port = 53
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.10'
    				Port = 53
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Sent from port: IPMUX_PTC:IP_SOCK

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		CTRL
    			ConnectionId
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.10'
    					Port = 53
    				Remote
    					IpAddr = Omit
    					Port = Omit
    			Ind
    				UDP
    					SocketCnf = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		DATA
    			ConnectionId
    				Protocol
    				Local
    					IpAddr
    						V4
    							Addr
    					Port
    				Remote
    					IpAddr
    					Port
    			Ind
    				UDP
    					SocketCnf

    Message Mismatch: IP_SOCKET_IND

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.10'
    				Port = 53
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    Received on port: IPMUX_PTC:IP_SOCK

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.10'
    				Port = 53
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.10'
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 5
    						QFI = 1
    			DataMode = Omit

    Sent from port: IP_PTC:IP_CTRL

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    Received on port: IP_PTC:IP_CTRL

    ConstraintMismatch::Received:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		ICMPv6_ServerAddress = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    ConstraintMismatch::Expected:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = '[0-9]+[.][0-9]+[.][0-9]+[.][0-9]+'

    Message Mismatch: CharacterStringType

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = 53
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = 53
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Sent from port: IPMUX_PTC:IP_SOCK

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		CTRL
    			ConnectionId
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = 53
    				Remote
    					IpAddr = Omit
    					Port = Omit
    			Ind
    				UDP
    					SocketCnf = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		DATA
    			ConnectionId
    				Protocol
    				Local
    					IpAddr
    						V6
    							Addr
    							ScopeId
    					Port
    				Remote
    					IpAddr
    					Port
    			Ind
    				UDP
    					SocketCnf

    Message Mismatch: IP_SOCKET_IND

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = 53
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    Received on port: IPMUX_PTC:IP_SOCK

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = 53
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.10'

    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.10'

    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = 53
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.10'
    					ScopeId
    			Port = 53
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.10'
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 5
    						QFI = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 5
    						QFI = 1
    			DataMode = Omit

    Sent from port: IP_PTC:IP_CTRL

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    Received on port: IP_PTC:IP_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.10'
    				Port = 67
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.10'
    				Port = 67
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Sent from port: IPMUX_PTC:IP_SOCK

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		CTRL
    			ConnectionId
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.10'
    					Port = 67
    				Remote
    					IpAddr = Omit
    					Port = Omit
    			Ind
    				UDP
    					SocketCnf = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		DATA
    			ConnectionId
    				Protocol
    				Local
    					IpAddr
    						V4
    							Addr
    					Port
    				Remote
    					IpAddr
    					Port
    			Ind
    				UDP
    					SocketCnf

    Message Mismatch: IP_SOCKET_IND

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.10'
    				Port = 67
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    Received on port: IPMUX_PTC:IP_SOCK

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.10'
    				Port = 67
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.10'
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.10'
    			Port = 67
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.Port

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.10'
    					ScopeId
    			Port = 67
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.10'
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.10'
    			Port = 67
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.Port

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.10'
    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.10'
    			Port = 53
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.Port

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.10'
    					ScopeId
    			Port = 67
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.10'

    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = 53
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.10'
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 5
    						QFI = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 5
    						QFI = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.10'
    					Port = 67
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 5
    						QFI = 1
    			DataMode = Omit

    Sent from port: IP_PTC:IP_CTRL

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    Received on port: IP_PTC:IP_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    			Remote = Omit
    		Req
    			ICMP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    			Remote = Omit
    		Req
    			ICMP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Sent from port: IPMUX_PTC:IP_SOCK

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		CTRL
    			ConnectionId
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = Omit
    				Remote
    					IpAddr = Omit
    					Port = Omit
    			Ind
    				ICMP
    					SocketCnf = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		DATA
    			ConnectionId
    				Protocol
    				Local
    					IpAddr
    						V6
    							Addr
    							ScopeId
    					Port
    				Remote
    					IpAddr
    					Port
    			Ind
    				ICMP
    					SocketCnf

    Message Mismatch: IP_SOCKET_IND

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			ICMP
    				SocketCnf = True

    Received on port: IPMUX_PTC:IP_SOCK

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			ICMP
    				SocketCnf = True

    Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.10'

    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.10'

    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.10'

    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.10'
    					ScopeId
    			Port = 53
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = 53
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.10'

    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.10'
    					ScopeId
    			Port = 67
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.10'
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 5
    						QFI = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 5
    						QFI = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.10'
    					Port = 67
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 5
    						QFI = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 5
    						QFI = 1
    			DataMode = Omit

    Sent from port: IP_PTC:IP_CTRL

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    Received on port: IP_PTC:IP_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    			Remote = Omit
    		Req
    			ICMP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    			Remote = Omit
    		Req
    			ICMP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Sent from port: IPMUX_PTC:IP_SOCK

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		CTRL
    			ConnectionId
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = Omit
    				Remote
    					IpAddr = Omit
    					Port = Omit
    			Ind
    				ICMP
    					SocketCnf = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		DATA
    			ConnectionId
    				Protocol
    				Local
    					IpAddr
    						V6
    							Addr
    							ScopeId
    					Port
    				Remote
    					IpAddr
    					Port
    			Ind
    				ICMP
    					SocketCnf

    Message Mismatch: IP_SOCKET_IND

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			ICMP
    				SocketCnf = True

    Received on port: IPMUX_PTC:IP_SOCK

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			ICMP
    				SocketCnf = True

    Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.10'

    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.10'

    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.10'

    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.10'
    					ScopeId
    			Port = 53
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = 53
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.10'

    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.10'
    					ScopeId
    			Port = 67
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.10'
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 5
    						QFI = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 5
    						QFI = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.10'
    					Port = 67
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 5
    						QFI = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 5
    						QFI = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 5
    						QFI = 1
    			DataMode = Omit

    Sent from port: IP_PTC:IP_CTRL

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    Received on port: IP_PTC:IP_CTRL

    IP_Indication_Type
    	Cnf = True

    Inter-component message: IP -> NR5GC_PTC:IP

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		RadioBearerList
    			NR_RadioBearer_Type
    				Id
    					Drb = 2
    				Config
    					AddOrReconfigure
    						Sdap
    							Config
    								SdapConfig
    									Pdu_SessionId = 5
    									Sdap_HeaderDL = Absent (1)
    									Sdap_HeaderUL = Present (0)
    									MappedQoS_Flows
    										IntegerType = 1
    						Pdcp
    							RBTerminating
    								RbConfig
    									Params
    										Rb
    											Drb
    												SN_SizeUL = PDCP_SNLength18 (1)
    												SN_SizeDL = PDCP_SNLength18 (1)
    												HeaderCompression
    													None = True
    												IntegrityProtectionEnabled = False
    								LinkToOtherCellGroup
    									None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										AM
    											Tx
    												R15
    													sn_FieldLength = size18 (1)
    													t_PollRetransmit = ms80 (15)
    													pollPDU = p32768 (18)
    													pollByte = kB750 (14)
    													maxRetxThreshold = t8 (5)
    											Rx
    												R15
    													sn_FieldLength = size18 (1)
    													t_Reassembly = ms80 (16)
    													t_StatusProhibit = ms30 (6)
    									TestMode = Omit
    								LogicalChannelId = 5
    								Mac
    									LogicalChannel
    										Priority = 1
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit

    Sent from port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		RadioBearerList = True

    Received on port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		PdcpCount
    			Get
    				AllRBs = True

    Sent from port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		PdcpCount
    			Get
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 1
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000001000'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000110'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 2
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Drb = 2
    					UL
    						Format = PdcpCount_DrbSQN18 (2)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_DrbSQN18 (2)
    						Value = 00000000000000000000000000000000'B

    Received on port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		AS_Security
    			StartRestart
    				Integrity
    					Algorithm = nia2 (2)
    					KRRCint = 01111000000000111001000110110000011011000100010010001100011100101110100011110010011101110101010111111010000111001100011111111111'B
    					KUPint = 01001000000011110101001100110111100110001001100110011100011101100001010000111111001111111001001101101101000001001000100110011110'B
    					ActTimeList = Omit
    				Ciphering
    					Algorithm = nea2 (2)
    					KRRCenc = 11000000001001111111010101010010011111110001000110110000101111010111010010101010100110101010001110010110001101101111001000000101'B
    					KUPenc = 10100111000111010011000011010011001100000110010100010011111000110100110010100111001000001101100110100011011011100110110011100110'B
    					ActTimeList
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 1
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 9
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 7
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 2
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Drb = 2
    							UL
    								SQN
    									Format = PdcpCount_DrbSQN18 (2)
    									Value = 0
    							DL
    								SQN
    									Format = PdcpCount_DrbSQN18 (2)
    									Value = 0

    Sent from port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		AS_Security = True

    Received on port: NR5GC_PTC:SYS

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcReconfiguration
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcReconfiguration
    									radioBearerConfig
    										srb_ToAddModList
    											SRB_ToAddMod
    												srb_Identity = 2
    												reestablishPDCP = Omit
    												discardOnPDCP = Omit
    												pdcp_Config = Omit
    										srb3_ToRelease = Omit
    										drb_ToAddModList
    											DRB_ToAddMod
    												cnAssociation
    													sdap_Config
    														pdu_Session = 5
    														sdap_HeaderDL = absent (1)
    														sdap_HeaderUL = present_ (0)
    														defaultDRB = True
    														mappedQoS_FlowsToAdd
    															IntegerType = 1
    														mappedQoS_FlowsToRelease = Omit
    												drb_Identity = 2
    												reestablishPDCP = Omit
    												recoverPDCP = Omit
    												pdcp_Config
    													drb
    														discardTimer = infinity_ (15)
    														pdcp_SN_SizeUL = len18bits (1)
    														pdcp_SN_SizeDL = len18bits (1)
    														headerCompression
    															notUsed = Null
    														integrityProtection = Omit
    														statusReportRequired = true_ (0)
    														outOfOrderDelivery = Omit
    													moreThanOneRLC = Omit
    													t_Reordering = Omit
    													cipheringDisabled = Omit
    										drb_ToReleaseList = Omit
    										securityConfig
    											securityAlgorithmConfig
    												cipheringAlgorithm = nea2 (2)
    												integrityProtAlgorithm = nia2 (2)
    											keyToUse = master (0)
    									secondaryCellGroup = Omit
    									measConfig = Omit
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension
    										masterCellGroup = '4002B24233E475E0320C3CC81212832F3000'O
    										fullConfig = Omit
    										dedicatedNAS_MessageList = Omit
    										masterKeyUpdate = Omit
    										dedicatedSIB1_Delivery = Omit
    										dedicatedSystemInformationDelivery = Omit
    										otherConfig = Omit
    										nonCriticalExtension = Omit
    		Nas
    			NG_NAS_MSG_Request_Type
    				SecurityProtection
    					Status = 0010'B
    					ForceMacError = False
    				Pdu
    					Msg
    						dl_Nas_Transport
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01101000'B
    							spareHalfOctet2 = '0'H
    							payloadContainerType
    								iei = Omit
    								container = 0001'B
    							payload
    								iei = Omit
    								iel = '0000'O
    								payload = ''O
    							pduSessionId
    								iei = '12'O
    								sessionId = '05'O
    							additionalInfo = Omit
    							gmmCause = Omit
    							backOffTimerValue = Omit
    					PiggybackedPduList
    						NG_NAS_DL_Pdu_Type
    							Msg
    								pdu_Session_Establishment_Accept
    									protocolDiscriminator = 00101110'B
    									pduSessionId
    										iei = Omit
    										sessionId = '05'O
    									procedureTransactionIdentifier = '0D'O
    									messageType = 11000010'B
    									sscMode
    										iei = Omit
    										spare = 0'B
    										sscModeValue = 001'B
    									pduSessionType
    										iei = Omit
    										spare = 0'B
    										typeValue = 001'B
    									authorizedQoSRules
    										iei = Omit
    										iel = '0009'O
    										listofQoSRules
    											QoS_Rule
    												identifier = '01'O
    												iel = '0006'O
    												ruleOperationCode = 001'B
    												dqrBit = 1'B
    												numOfPacketFilters = 0001'B
    												packetFilterList
    													new
    														NG_PacketFilter_Type2
    															spare = 00'B
    															direction = 11'B
    															packetFilterId = 0000'B
    															len = '01'O
    															contents = '01'O
    												precedence = '00'O
    												spare = 0'B
    												segregation = 0'B
    												flowIdentifier = 000001'B
    									sessionAMBR
    										iei = Omit
    										iel = '06'O
    										unitDL = '05'O
    										downlink = '0004'O
    										unitUL = '05'O
    										uplink = '0004'O
    									gsmCause = Omit
    									pduAddress
    										iei = '29'O
    										iel = '05'O
    										spare = 00000'B
    										typeValue = 001'B
    										adressInfo = 'C0A8001A'O
    									rqTimerValue = Omit
    									s_NSSAI
    										iei = '22'O
    										iel = '01'O
    										sst = '01'O
    										sd = Omit
    										mappedSST = Omit
    										mappedSD = Omit
    									alwaysOnPDUSessionInd = Omit
    									mappedEPSContexts
    										iei = '75'O
    										iel = '0010'O
    										mappedContextList
    											MappedEPSContext
    												epsBearerId = '0C'O
    												lenOfContext = '000D'O
    												operationCode = 01'B
    												spare = 0'B
    												eBit = 1'B
    												numOfParams = 0001'B
    												epsParamsList
    													EPSParameters
    														id = '01'O
    														lenOfContent = '0A'O
    														epsParam = '09094040404000000000'O
    									eapMessage = Omit
    									authorizedQoSFlowDescr
    										iei = '79'O
    										iel = '0009'O
    										listofFlows
    											QoS_Flow
    												spare2 = 00'B
    												qfi = 000001'B
    												operationCode = 001'B
    												spare6 = 000000'B
    												eBit = 1'B
    												numOfParameters = 000010'B
    												parameterList
    													QoSParameters
    														id = '01'O
    														lenOfContent = '01'O
    														qosParam = '09'O
    													QoSParameters
    														id = '07'O
    														lenOfContent = '01'O
    														qosParam = '0C'O
    									extdProtocolConfigurationOptions = Omit
    									dnn
    										iei = '25'O
    										iel = '04'O
    										dnnValue = '0361706E'O
    							PiggybackedPduList = Omit

    Inter-component message: TC_SRB -> NASEMU_NRNG_PTC:TC_SRB

    PDU SESSION ESTABLISHMENT ACCEPT
    	Extended protocol discriminator = 0x2E [ 46 ]
    	pdu_sesn_id [8 bits] = 0x5 [ 5 ]
    	pti [8 bits] = 0xD [ 13 ]
    	pdu_sesn_est_acpt_msg_id [8 bits] = 0xC2 [ 194 ]
    	sltd_ssc_mode
    		Spare Bits [1 bit] = 0x0 [ 0 ]
    		SSC mode value [3 bits] = 0x1 [ 1 ]
    	sltd_pdu_sesn_typ
    		Spare Bits [1 bit] = 0x0 [ 0 ]
    		PDU session type value [3 bits] = 0x1 [ 1 ]
    	autz_qos_rules
    		qriel [16 bits] = 0x9 [ 9 ]
    		qiei [8 bits] = 0x1 [ 1 ]
    		qiel [16 bits] = 0x6 [ 6 ]
    		rule_op_code [3 bits] = 0x1 [ 1 ]
    		dqr_bit [1 bit] = 0x1 [ 1 ]
    		numof_pack_flt [4 bits] = 0x1 [ 1 ]
    		spare2bits1 [2 bits] = 0x0 [ 0 ]
    		pkt_flt_dir1 [2 bits] = 0x3 [ 3 ]
    		pkt_flt_id1 [4 bits] = 0x0 [ 0 ]
    		len_pkt_flt_con1 [8 bits] = 0x1 [ 1 ]
    		pkt_flt_con1 = 0x01 [ 1 ]
    		qrs_rule_pre = 0x00 [ 0 ]
    		Spare Bits [1 bit] = 0x0 [ 0 ]
    		segregation [1 bit] = 0x0 [ 0 ]
    		qrs_flow_iden [6 bits] = 0x1 [ 1 ]
    	sesn_ambr
    		Length [8 bits] = 0x6 [ 6 ]
    		unit_sesn_ambr_downlink = 0x05 [ 5 ]
    		sesn_ambr_downlink = 0x0004 [ 4 ]
    		unit_sesn_ambr_uplink = 0x05 [ 5 ]
    		sesn_ambr_uplink = 0x0004 [ 4 ]
    	pdu_address
    		IE Identifier [8 bits] = 0x29 [ 41 ]
    		IE Length [8 bits] = 0x5 [ 5 ]
    		Spare Bits [5 bits] = 0x0 [ 0 ]
    		pdue_sesn_typ [3 bits] = 0x1 [ 1 ]
    		ipv4 = 0xC0A8001A [ 3232235546 ]
    	s_nssai
    		IE Identifier [8 bits] = 0x22 [ 34 ]
    		IE Length [8 bits] = 0x1 [ 1 ]
    		sst = 0x01 [ 1 ]
    	map_eps_bear_cntx
    		IE Identifier [8 bits] = 0x75 [ 117 ]
    		m_len [16 bits] = 0x10 [ 16 ]
    		mapp_eps_bear_ctxt1
    			opern_code [2 bits] = 0x0 [ 0 ]
    			deb_bit [1 bit] = 0x0 [ 0 ]
    			e_bit [1 bit] = 0x0 [ 0 ]
    			numof_eps_bear_param [4 bits] = 0xC [ 12 ]
    			eps_param_list
    				iei_i [8 bits] = 0x0 [ 0 ]
    				IE Length [8 bits] = 0xD [ 13 ]
    				content1 = 0x5101 [ 20737 ]
    				iei_1 [8 bits] = 0xA [ 10 ]
    				iel_1 [8 bits] = 0x9 [ 9 ]
    				content2 = 0x0940 [ 2368 ]
    		mapp_eps_bear_ctxt2
    			opern_code [2 bits] = 0x1 [ 1 ]
    			deb_bit [1 bit] = 0x0 [ 0 ]
    			e_bit [1 bit] = 0x0 [ 0 ]
    			numof_eps_bear_param [4 bits] = 0x0 [ 0 ]
    			eps_param_list
    				iei_i [8 bits] = 0x40 [ 64 ]
    				IE Length [8 bits] = 0x40 [ 64 ]
    				content1 = 0x0000 [ 0 ]
    				iei_1 [8 bits] = 0x0 [ 0 ]
    				iel_1 [8 bits] = 0x0 [ 0 ]
    				content2 = 0x7900 [ 30976 ]

    PDU SESSION ESTABLISHMENT ACCEPT PDU

    DL NAS TRANSPORT
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Spare Half Octet [4 bits] = 0x0 [ 0 ]
    	Message Type [8 bits] = 0x68 - DL NAS TRANSPORT [ 104 ]
    	sht2 [4 bits] = 0x0 [ 0 ]
    	payload_typ
    		val [4 bits] = 0x1 [ 1 ]
    	payload_cont
    		IE Length [16 bits] = 0x46 [ 70 ]
    		val = 0x2E050DC211000901000631300101000106050004050004290501C0A8001A2201017500100C000D51010A0909404040400000000079000901204201010907010C25040361706E
    	pdu_sess_id
    		IE Identifier [8 bits] = 0x12 [ 18 ]
    		val = 0x05 [ 5 ]

    DL NAS TRANSPORT PDU

    DL-DCCH-Message
    	message = c1 = rrcReconfiguration =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcReconfiguration =
    			radioBearerConfig
    				srb-ToAddModList = SEQUENCE OF SRB-ToAddMod
    					SRB-ToAddMod(1)
    						srb-Identity = 2
    				drb-ToAddModList = SEQUENCE OF DRB-ToAddMod
    					DRB-ToAddMod(1)
    						cnAssociation = sdap-Config =
    							pdu-Session = 5
    							sdap-HeaderDL = absent
    							sdap-HeaderUL = present
    							defaultDRB = TRUE
    							mappedQoS-FlowsToAdd = SEQUENCE OF QFI
    								QFI(1) = 1
    						drb-Identity = 2
    						pdcp-Config
    							drb
    								discardTimer = infinity
    								pdcp-SN-SizeUL = len18bits
    								pdcp-SN-SizeDL = len18bits
    								headerCompression = notUsed = NULL
    								statusReportRequired = true
    				securityConfig
    					securityAlgorithmConfig
    						cipheringAlgorithm = nea2
    						integrityProtAlgorithm = nia2
    					keyToUse = master
    			nonCriticalExtension
    				masterCellGroup = CONTAINING =
    					cellGroupId = 0
    					rlc-BearerToAddModList = SEQUENCE OF RLC-BearerConfig
    						RLC-BearerConfig(1)
    							logicalChannelIdentity = 5
    							servedRadioBearer = drb-Identity = 2
    							rlc-Config = am =
    								ul-AM-RLC
    									sn-FieldLength = size18
    									t-PollRetransmit = ms80
    									pollPDU = p32768
    									pollByte = kB750
    									maxRetxThreshold = t8
    								dl-AM-RLC
    									sn-FieldLength = size18
    									t-Reassembly = ms80
    									t-StatusProhibit = ms30
    							mac-LogicalChannelConfig
    								ul-SpecificParameters
    									priority = 1
    									prioritisedBitRate = infinity
    									bucketSizeDuration = ms50
    									logicalChannelGroup = 1
    									schedulingRequestID = 0
    									logicalChannelSR-Mask = FALSE
    									logicalChannelSR-DelayTimerApplied = FALSE
    						RLC-BearerConfig(2)
    							logicalChannelIdentity = 2
    							servedRadioBearer = srb-Identity = 2
    							mac-LogicalChannelConfig
    								ul-SpecificParameters
    									priority = 3
    									prioritisedBitRate = infinity
    									bucketSizeDuration = ms50
    									logicalChannelGroup = 0
    									schedulingRequestID = 0
    									logicalChannelSR-Mask = FALSE
    									logicalChannelSR-DelayTimerApplied = FALSE
    				dedicatedNAS-MessageList = SEQUENCE OF DedicatedNAS-Message
    					DedicatedNAS-Message(1) = 7E02CA241113038B5CB0E979D0B8ED1FE606E35EAF8ECA3A37CD608BAEBBF521AD1A5FB06C315C4ACE73CF300D75600A43AA2E52F866ECAE80FB29DD6F4F130C2BDC8A5DE1ED3BD49E46D10A1D94D7FC7DFD8200BE

    rrcReconfiguration

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcReconfiguration
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcReconfiguration
    								radioBearerConfig
    									srb_ToAddModList
    										SRB_ToAddMod
    											srb_Identity = 2
    											reestablishPDCP = Omit
    											discardOnPDCP = Omit
    											pdcp_Config = Omit
    									srb3_ToRelease = Omit
    									drb_ToAddModList
    										DRB_ToAddMod
    											cnAssociation
    												sdap_Config
    													pdu_Session = 5
    													sdap_HeaderDL = absent (1)
    													sdap_HeaderUL = present_ (0)
    													defaultDRB = True
    													mappedQoS_FlowsToAdd
    														IntegerType = 1
    													mappedQoS_FlowsToRelease = Omit
    											drb_Identity = 2
    											reestablishPDCP = Omit
    											recoverPDCP = Omit
    											pdcp_Config
    												drb
    													discardTimer = infinity_ (15)
    													pdcp_SN_SizeUL = len18bits (1)
    													pdcp_SN_SizeDL = len18bits (1)
    													headerCompression
    														notUsed = Null
    													integrityProtection = Omit
    													statusReportRequired = true_ (0)
    													outOfOrderDelivery = Omit
    												moreThanOneRLC = Omit
    												t_Reordering = Omit
    												cipheringDisabled = Omit
    									drb_ToReleaseList = Omit
    									securityConfig
    										securityAlgorithmConfig
    											cipheringAlgorithm = nea2 (2)
    											integrityProtAlgorithm = nia2 (2)
    										keyToUse = master (0)
    								secondaryCellGroup = Omit
    								measConfig = Omit
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension
    									masterCellGroup = '4002B24233E475E0320C3CC81212832F3000'O
    									fullConfig = Omit
    									dedicatedNAS_MessageList
    										NG_NAS_Message = '7E02CA241113038B5CB0E979D0B8ED1FE606E35EAF8ECA3A37CD608BAEBBF521AD1A5FB06C315C4ACE73CF300D75600A43AA2E52F866ECAE80FB29DD6F4F130C2BDC8A5DE1ED3BD49E46D10A1D94D7FC7DFD8200BE'O
    									masterKeyUpdate = Omit
    									dedicatedSIB1_Delivery = Omit
    									dedicatedSystemInformationDelivery = Omit
    									otherConfig = Omit
    									nonCriticalExtension = Omit

    Sent from port: NASEMU_NRNG_PTC:SYS_SRB

    UL-DCCH-Message
    	message = c1 = rrcReconfigurationComplete =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcReconfigurationComplete =

    rrcReconfigurationComplete

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 1014
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcReconfigurationComplete
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcReconfigurationComplete
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Received on port: NASEMU_NRNG_PTC:SYS_SRB

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 1014
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcReconfigurationComplete
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcReconfigurationComplete
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: SRB -> NR5GC_PTC:SRB

    IMS_IPCAN_Coordination_MSG
    	IPCAN_IMS_Control
    		NoRegistration = True

    Inter-component message: IPCAN -> IMS_PTC:IPCAN

    timerEvent = 6
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\IMS\IMS_PTC_CoordMsg.ttcn
    testName = TC_7_1_3_2_2_NR5GC
    lineNo = 413
    outStr = Timer: t_WaitForUPlaneSignalling, Duration: 1.2s, Started: 10:22:45

    Timer: t_WaitForUPlaneSignalling, Duration: 1.2s, Started: 10:22:45

    timerEvent = 9
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\IMS\IMS_PTC_CoordMsg.ttcn
    testName = TC_7_1_3_2_2_NR5GC
    lineNo = 415
    outStr = Timer: t_WaitForUPlaneSignalling, Expired: 10:22:46

    Timer: t_WaitForUPlaneSignalling, Expired: 10:22:46

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		EnquireTiming = True

    Sent from port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 112
    				Subframe
    					Number = 2
    				HSFN
    					Number = 78
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		Result
    			Success = True
    	Confirm
    		EnquireTiming = True

    Received on port: NR5GC_PTC:SYS

    timerEvent = 6
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\NR5GC\NR5GC_RRCSteps.ttcn
    testName = TC_7_1_3_2_2_NR5GC
    lineNo = 281
    outStr = Timer: t_Timer, Duration: 1.22s, Started: 10:22:46

    Timer: t_Timer, Duration: 1.22s, Started: 10:22:46

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 142
    				Subframe
    					Number = 2
    				HSFN
    					Number = 78
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcRelease
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcRelease
    									redirectedCarrierInfo = Omit
    									cellReselectionPriorities = Omit
    									suspendConfig = Omit
    									deprioritisationReq = Omit
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: TC_SRB -> NASEMU_NRNG_PTC:TC_SRB

    DL-DCCH-Message
    	message = c1 = rrcRelease =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcRelease =

    rrcRelease

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 142
    				Subframe
    					Number = 2
    				HSFN
    					Number = 78
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcRelease
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcRelease
    								redirectedCarrierInfo = Omit
    								cellReselectionPriorities = Omit
    								suspendConfig = Omit
    								deprioritisationReq = Omit
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Sent from port: NASEMU_NRNG_PTC:SYS_SRB

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		PdcpCount
    			Get
    				AllRBs = True

    Sent from port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		PdcpCount
    			Get
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 1
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000001001'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000001000'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 2
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Drb = 2
    					UL
    						Format = PdcpCount_DrbSQN18 (2)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_DrbSQN18 (2)
    						Value = 00000000000000000000000000000000'B

    Received on port: NR5GC_PTC:SYS

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 142
    			Subframe
    				Number = 2
    			HSFN
    				Number = 78
    			Slot
    				SlotOffset
    					Numerology1 = 0
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		Now
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				SlotOffset
    					Numerology1

    Message Mismatch: TimingInfo_Type

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 142
    				Subframe
    					Number = 2
    				HSFN
    					Number = 78
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		Cell
    			AddOrReconfigure
    				StaticResourceConfig = Omit
    				CellConfigCommon = Omit
    				PhysicalLayer = Omit
    				BcchConfig = Omit
    				PcchConfig = Omit
    				RachProcedureConfig = Omit
    				CcchDcchDtchConfig
    					DL = Omit
    					UL
    						SearchSpaceAndDci
    							AssignedBWPs = Omit
    							SearchSpaceType = Omit
    							DciInfo = Omit
    						PUCCH_Synch
    							None = True
    						GrantConfig
    							None = True
    					DrxCtrl = Omit
    					MeasGapCtrl = Omit
    				ServingCellConfig = Omit

    Sent from port: NR5GC_PTC:SYS

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 142
    			Subframe
    				Number = 7
    			HSFN
    				Number = 78
    			Slot
    				SlotOffset
    					Numerology1 = 0
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		Now
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				SlotOffset
    					Numerology1

    Message Mismatch: TimingInfo_Type

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 142
    				Subframe
    					Number = 7
    				HSFN
    					Number = 78
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		AS_Security
    			Release = True

    Sent from port: NR5GC_PTC:SYS

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 147
    			Subframe
    				Number = 7
    			HSFN
    				Number = 78
    			Slot
    				SlotOffset
    					Numerology1 = 0
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		Now
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				SlotOffset
    					Numerology1

    Message Mismatch: TimingInfo_Type

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 147
    				Subframe
    					Number = 7
    				HSFN
    					Number = 78
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		RadioBearerList
    			NR_RadioBearer_Type
    				Id
    					Srb = 1
    				Config
    					Release = True
    			NR_RadioBearer_Type
    				Id
    					Srb = 2
    				Config
    					Release = True
    			NR_RadioBearer_Type
    				Id
    					Drb = 2
    				Config
    					Release = True

    Sent from port: NR5GC_PTC:SYS

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 148
    			Subframe
    				Number = 2
    			HSFN
    				Number = 78
    			Slot
    				SlotOffset
    					Numerology1 = 0
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		Now
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				SlotOffset
    					Numerology1

    Message Mismatch: TimingInfo_Type

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 148
    				Subframe
    					Number = 2
    				HSFN
    					Number = 78
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		RadioBearerList
    			NR_RadioBearer_Type
    				Id
    					Srb = 1
    				Config
    					AddOrReconfigure
    						Sdap
    							None = True
    						Pdcp
    							RBTerminating
    								RbConfig
    									Params
    										Rb
    											Srb = True
    								LinkToOtherCellGroup
    									None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										AM
    											Tx
    												R15
    													sn_FieldLength = size12 (0)
    													t_PollRetransmit = ms45 (8)
    													pollPDU = infinity_ (23)
    													pollByte = infinity_ (43)
    													maxRetxThreshold = t8 (5)
    											Rx
    												R15
    													sn_FieldLength = size12 (0)
    													t_Reassembly = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    									TestMode
    										None = True
    								LogicalChannelId = 1
    								Mac
    									LogicalChannel
    										Priority = 1
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit
    			NR_RadioBearer_Type
    				Id
    					Srb = 2
    				Config
    					AddOrReconfigure
    						Sdap
    							None = True
    						Pdcp
    							RBTerminating
    								RbConfig
    									Params
    										Rb
    											Srb = True
    								LinkToOtherCellGroup
    									None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										AM
    											Tx
    												R15
    													sn_FieldLength = size12 (0)
    													t_PollRetransmit = ms45 (8)
    													pollPDU = infinity_ (23)
    													pollByte = infinity_ (43)
    													maxRetxThreshold = t8 (5)
    											Rx
    												R15
    													sn_FieldLength = size12 (0)
    													t_Reassembly = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    									TestMode
    										None = True
    								LogicalChannelId = 2
    								Mac
    									LogicalChannel
    										Priority = 3
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit

    Sent from port: NR5GC_PTC:SYS

    timerEvent = 9
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\NR5GC\NR5GC_RRCSteps.ttcn
    testName = TC_7_1_3_2_2_NR5GC
    lineNo = 289
    outStr = Timer: t_Timer, Expired: 10:22:47

    Timer: t_Timer, Expired: 10:22:47

    timerEvent = 6
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\Common\CommonDefs.ttcn
    testName = TC_7_1_3_2_2_NR5GC
    lineNo = 569
    outStr = Timer: t_Delay, Duration: 1s, Started: 10:22:47

    Timer: t_Delay, Duration: 1s, Started: 10:22:47

    timerEvent = 9
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\Common\CommonDefs.ttcn
    testName = TC_7_1_3_2_2_NR5GC
    lineNo = 570
    outStr = Timer: t_Delay, Expired: 10:22:48

    Timer: t_Delay, Expired: 10:22:48

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		EnquireTiming = True

    Sent from port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 338
    				Subframe
    					Number = 6
    				HSFN
    					Number = 78
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		Result
    			Success = True
    	Confirm
    		EnquireTiming = True

    Received on port: NR5GC_PTC:SYS

    PCCH-Message
    	message = c1 = paging =
    		pagingRecordList = SEQUENCE OF PagingRecord
    			PagingRecord(1)
    				ue-Identity = ng-5G-S-TMSI = 000000000100000111000010001101000101011001111000

    paging

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 367
    				Subframe
    					Number = 1
    				HSFN
    					Number = 78
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		Paging
    			Paging
    				message_
    					c1
    						paging
    							pagingRecordList
    								PagingRecord
    									ue_Identity
    										ng_5G_S_TMSI = 000000000100000111000010001101000101011001111000'B
    									accessType = Omit
    							lateNonCriticalExtension = Omit
    							nonCriticalExtension = Omit
    			SlotOffsetList = Omit

    Sent from port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		Cell
    			AddOrReconfigure
    				StaticResourceConfig = Omit
    				CellConfigCommon = Omit
    				PhysicalLayer = Omit
    				BcchConfig = Omit
    				PcchConfig = Omit
    				RachProcedureConfig = Omit
    				CcchDcchDtchConfig
    					DL = Omit
    					UL
    						SearchSpaceAndDci
    							AssignedBWPs = Omit
    							SearchSpaceType = Omit
    							DciInfo
    								ResoureAssignment
    									ResourceAllocationType = Omit
    									FreqDomain
    										FirstRbIndex = 0
    										Nprb = 24
    									TimeDomain = Omit
    									TransportBlockScheduling
    										NR_TransportBlockSingleTransmission_Type
    											TimingOffset
    												None = True
    											ImcsValue = 9
    											RedundancyVersion = 0
    											ToggleNDI = True
    									HarqProcessConfig = Omit
    								PuschHoppingCtrl = Omit
    								TpcCommandPusch = Omit
    								UL_SUL_Indicator = Omit
    								Format = Omit
    						PUCCH_Synch
    							None = True
    						GrantConfig
    							OnSR_Reception = True
    					DrxCtrl = Omit
    					MeasGapCtrl = Omit
    				ServingCellConfig = Omit

    Sent from port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		Cell = True

    Received on port: NR5GC_PTC:SYS

    UL-CCCH-Message
    	message = c1 = rrcSetupRequest =
    		rrcSetupRequest
    			ue-Identity = ng-5G-S-TMSI-Part1 = 100000111000010001101000101011001111000
    			establishmentCause = mt-Access
    			spare = 0

    rrcSetupRequest

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 0
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 370
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Ccch
    			message_
    				c1
    					rrcSetupRequest
    						rrcSetupRequest
    							ue_Identity
    								ng_5G_S_TMSI_Part1 = 100000111000010001101000101011001111000'B
    							establishmentCause = mt_Access (2)
    							spare = 0'B

    Received on port: NASEMU_NRNG_PTC:SYS_SRB

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 0
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 370
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Ccch
    				message_
    					c1
    						rrcSetupRequest
    							rrcSetupRequest
    								ue_Identity
    									ng_5G_S_TMSI_Part1 = 100000111000010001101000101011001111000'B
    								establishmentCause = mt_Access (2)
    								spare = 0'B
    		Nas = Omit

    Inter-component message: SRB -> NR5GC_PTC:SRB

    SERVICE REQUEST
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Spare Half Octet [4 bits] = 0x0 [ 0 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Message Type [8 bits] = 0x4C - SERVICE REQUEST [ 76 ]
    	ser_typ
    		Value [4 bits] = 0x2 [ 2 ]
    	sr_ngksi
    		Type of security context flag [1 bit] = 0x0 [ 0 ]
    		key sequence indicator [3 bits] = 0x1 [ 1 ]
    	fiveg_s_tmsi
    		Length [16 bits] = 0x7 [ 7 ]
    		id_dig [4 bits] = 0xF [ 15 ]
    		Spare Bits [1 bit] = 0x0 [ 0 ]
    		typ_id [3 bits] = 0x4 [ 4 ]
    		amf_set_id = 0x00 [ 0 ]
    		amf_set_id_cont [2 bits] = 0x1 [ 1 ]
    		amf_pntr [6 bits] = 0x1 [ 1 ]
    		fiveg_tmsi = 0xC234 [ 49716 ]

    SERVICE REQUEST PDU

    UL-DCCH-Message
    	message = c1 = rrcSetupComplete =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcSetupComplete =
    			selectedPLMN-Identity = 1
    			dedicatedNAS-Message = 7E01CA7714D2047E004C210007F40041C234567871001121833AF07B249994CC9679561A016592C0
    			ng-5G-S-TMSI-Value = ng-5G-S-TMSI-Part2 = 000000000

    rrcSetupComplete

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 372
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcSetupComplete
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcSetupComplete
    								selectedPLMN_Identity = 1
    								registeredAMF = Omit
    								guami_Type = Omit
    								s_NSSAI_List = Omit
    								dedicatedNAS_Message = '7E01CA7714D2047E004C210007F40041C234567871001121833AF07B249994CC9679561A016592C0'O
    								ng_5G_S_TMSI_Value
    									ng_5G_S_TMSI_Part2 = 000000000'B
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Received on port: NASEMU_NRNG_PTC:SYS_SRB

    SERVICE REQUEST
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Spare Half Octet [4 bits] = 0x0 [ 0 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Message Type [8 bits] = 0x4C - SERVICE REQUEST [ 76 ]
    	ser_typ
    		Value [4 bits] = 0x2 [ 2 ]
    	sr_ngksi
    		Type of security context flag [1 bit] = 0x0 [ 0 ]
    		key sequence indicator [3 bits] = 0x1 [ 1 ]
    	fiveg_s_tmsi
    		Length [16 bits] = 0x7 [ 7 ]
    		id_dig [4 bits] = 0xF [ 15 ]
    		Spare Bits [1 bit] = 0x0 [ 0 ]
    		typ_id [3 bits] = 0x4 [ 4 ]
    		amf_set_id = 0x00 [ 0 ]
    		amf_set_id_cont [2 bits] = 0x1 [ 1 ]
    		amf_pntr [6 bits] = 0x1 [ 1 ]
    		fiveg_tmsi = 0xC234 [ 49716 ]

    SERVICE REQUEST PDU

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 372
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcSetupComplete
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcSetupComplete
    									selectedPLMN_Identity = 1
    									registeredAMF = Omit
    									guami_Type = Omit
    									s_NSSAI_List = Omit
    									dedicatedNAS_Message = '7E01CA7714D2047E004C210007F40041C234567871001121833AF07B249994CC9679561A016592C0'O
    									ng_5G_S_TMSI_Value
    										ng_5G_S_TMSI_Part2 = 000000000'B
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0001'B
    					NasCount = '00000004'O
    				Pdu
    					Msg
    						service_Request
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01001100'B
    							serviceType = 0010'B
    							ngKSI
    								iei = Omit
    								tsc = 0'B
    								nasKeySetId = 001'B
    							s_TMSI
    								iei = Omit
    								iel = '0007'O
    								idDigit1 = 1111'B
    								oddEvenInd = 0'B
    								typeOfId = 100'B
    								otherDigits = '0041C2345678'O
    							ulDataStatus = Omit
    							pduSessionStatus = Omit
    							allowedPDUSessionStatus = Omit
    							nasMsg
    								iei = '71'O
    								iel = '0011'O
    								replayedNASMsgContainerValue = '21833AF07B249994CC9679561A016592C0'O
    					PiggybackedPduList
    						NG_NAS_UL_Pdu_Type
    							Msg
    								service_Request
    									protocolDiscriminator = 01111110'B
    									spareHalfOctet = '0'H
    									securityHeaderType = 0000'B
    									messageType = 01001100'B
    									serviceType = 0010'B
    									ngKSI
    										iei = Omit
    										tsc = 0'B
    										nasKeySetId = 001'B
    									s_TMSI
    										iei = Omit
    										iel = '0007'O
    										idDigit1 = 1111'B
    										oddEvenInd = 0'B
    										typeOfId = 100'B
    										otherDigits = '0041C2345678'O
    									ulDataStatus = Omit
    									pduSessionStatus
    										iei = '50'O
    										iel = '02'O
    										psi0_7 = 00100000'B
    										psi8_15 = 00000000'B
    										spare = Omit
    									allowedPDUSessionStatus = Omit
    									nasMsg = Omit
    							PiggybackedPduList = Omit

    Inter-component message: SRB -> NR5GC_PTC:SRB

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		Cell
    			AddOrReconfigure
    				StaticResourceConfig = Omit
    				CellConfigCommon = Omit
    				PhysicalLayer = Omit
    				BcchConfig = Omit
    				PcchConfig = Omit
    				RachProcedureConfig = Omit
    				CcchDcchDtchConfig
    					DL = Omit
    					UL
    						SearchSpaceAndDci
    							AssignedBWPs = Omit
    							SearchSpaceType = Omit
    							DciInfo = Omit
    						PUCCH_Synch
    							Auto
    								TimingAdvance = 31
    								TA_Period = 600
    						GrantConfig = Omit
    					DrxCtrl = Omit
    					MeasGapCtrl = Omit
    				ServingCellConfig = Omit

    Sent from port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		Cell = True

    Received on port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		PdcpCount
    			Get
    				AllRBs = True

    Sent from port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		PdcpCount
    			Get
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 1
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000001'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 2
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B

    Received on port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		AS_Security
    			StartRestart
    				Integrity
    					Algorithm = nia2 (2)
    					KRRCint = 10001010011111110110001011001000010100101010010100010110000010010011001000000101101100110110110001000010000101000110100111010001'B
    					KUPint = 01110111101100000101111010100100001000010011010001001010101100001001100000001001101010111001001000001000110111110100001111101110'B
    					ActTimeList = Omit
    				Ciphering
    					Algorithm = nea2 (2)
    					KRRCenc = 10101100100110010001010110011010010110011101001111011100100000010101100101010100110110000110100111000001111100101100000110011110'B
    					KUPenc = 00100101011111100111111000110011111100111110011101101110101001111110000100011110000111101100000100010110001011111110111100000111'B
    					ActTimeList
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 1
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 2
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 1
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 2
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0

    Sent from port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		AS_Security = True

    Received on port: NR5GC_PTC:SYS

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						securityModeCommand
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								securityModeCommand
    									securityConfigSMC
    										securityAlgorithmConfig
    											cipheringAlgorithm = nea2 (2)
    											integrityProtAlgorithm = nia2 (2)
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: TC_SRB -> NASEMU_NRNG_PTC:TC_SRB

    DL-DCCH-Message
    	message = c1 = securityModeCommand =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = securityModeCommand =
    			securityConfigSMC
    				securityAlgorithmConfig
    					cipheringAlgorithm = nea2
    					integrityProtAlgorithm = nia2

    securityModeCommand

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					securityModeCommand
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							securityModeCommand
    								securityConfigSMC
    									securityAlgorithmConfig
    										cipheringAlgorithm = nea2 (2)
    										integrityProtAlgorithm = nia2 (2)
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Sent from port: NASEMU_NRNG_PTC:SYS_SRB

    UL-DCCH-Message
    	message = c1 = securityModeComplete =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = securityModeComplete =

    securityModeComplete

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 379
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					securityModeComplete
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							securityModeComplete
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Received on port: NASEMU_NRNG_PTC:SYS_SRB

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 379
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						securityModeComplete
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								securityModeComplete
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: SRB -> NR5GC_PTC:SRB

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		RadioBearerList
    			NR_RadioBearer_Type
    				Id
    					Drb = 2
    				Config
    					AddOrReconfigure
    						Sdap
    							None = True
    						Pdcp
    							RBTerminating
    								RbConfig
    									Params
    										Rb
    											Drb
    												SN_SizeUL = PDCP_SNLength18 (1)
    												SN_SizeDL = PDCP_SNLength18 (1)
    												HeaderCompression
    													None = True
    												IntegrityProtectionEnabled = True
    								LinkToOtherCellGroup
    									None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										AM
    											Tx
    												R15
    													sn_FieldLength = size18 (1)
    													t_PollRetransmit = ms80 (15)
    													pollPDU = p32768 (18)
    													pollByte = kB750 (14)
    													maxRetxThreshold = t8 (5)
    											Rx
    												R15
    													sn_FieldLength = size18 (1)
    													t_Reassembly = ms80 (16)
    													t_StatusProhibit = ms30 (6)
    									TestMode = Omit
    								LogicalChannelId = 5
    								Mac
    									LogicalChannel
    										Priority = 1
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit

    Sent from port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		RadioBearerList = True

    Received on port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		PdcpCount
    			Get
    				AllRBs = True

    Sent from port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		PdcpCount
    			Get
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 1
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000010'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000001'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 2
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Drb = 2
    					UL
    						Format = PdcpCount_DrbSQN18 (2)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_DrbSQN18 (2)
    						Value = 00000000000000000000000000000000'B

    Received on port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		AS_Security
    			StartRestart
    				Integrity
    					Algorithm = nia2 (2)
    					KRRCint = 10001010011111110110001011001000010100101010010100010110000010010011001000000101101100110110110001000010000101000110100111010001'B
    					KUPint = 01110111101100000101111010100100001000010011010001001010101100001001100000001001101010111001001000001000110111110100001111101110'B
    					ActTimeList = Omit
    				Ciphering
    					Algorithm = nea2 (2)
    					KRRCenc = 10101100100110010001010110011010010110011101001111011100100000010101100101010100110110000110100111000001111100101100000110011110'B
    					KUPenc = 00100101011111100111111000110011111100111110011101101110101001111110000100011110000111101100000100010110001011111110111100000111'B
    					ActTimeList
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 1
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 3
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 2
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 2
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Drb = 2
    							UL
    								SQN
    									Format = PdcpCount_DrbSQN18 (2)
    									Value = 0
    							DL
    								SQN
    									Format = PdcpCount_DrbSQN18 (2)
    									Value = 0

    Sent from port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		AS_Security = True

    Received on port: NR5GC_PTC:SYS

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcReconfiguration
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcReconfiguration
    									radioBearerConfig
    										srb_ToAddModList
    											SRB_ToAddMod
    												srb_Identity = 2
    												reestablishPDCP = Omit
    												discardOnPDCP = Omit
    												pdcp_Config = Omit
    										srb3_ToRelease = Omit
    										drb_ToAddModList
    											DRB_ToAddMod
    												cnAssociation
    													sdap_Config
    														pdu_Session = 5
    														sdap_HeaderDL = absent (1)
    														sdap_HeaderUL = present_ (0)
    														defaultDRB = True
    														mappedQoS_FlowsToAdd
    															IntegerType = 1
    														mappedQoS_FlowsToRelease = Omit
    												drb_Identity = 2
    												reestablishPDCP = Omit
    												recoverPDCP = Omit
    												pdcp_Config
    													drb
    														discardTimer = infinity_ (15)
    														pdcp_SN_SizeUL = len18bits (1)
    														pdcp_SN_SizeDL = len18bits (1)
    														headerCompression
    															notUsed = Null
    														integrityProtection = enabled (0)
    														statusReportRequired = true_ (0)
    														outOfOrderDelivery = Omit
    													moreThanOneRLC = Omit
    													t_Reordering = Omit
    													cipheringDisabled = Omit
    										drb_ToReleaseList = Omit
    										securityConfig
    											securityAlgorithmConfig
    												cipheringAlgorithm = nea2 (2)
    												integrityProtAlgorithm = nia2 (2)
    											keyToUse = master (0)
    									secondaryCellGroup = Omit
    									measConfig = Omit
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension
    										masterCellGroup = '400290941979802C908CF91D780C830F3200'O
    										fullConfig = Omit
    										dedicatedNAS_MessageList = Omit
    										masterKeyUpdate = Omit
    										dedicatedSIB1_Delivery = Omit
    										dedicatedSystemInformationDelivery = Omit
    										otherConfig = Omit
    										nonCriticalExtension = Omit
    		Nas
    			NG_NAS_MSG_Request_Type
    				SecurityProtection
    					Status = 0010'B
    					ForceMacError = False
    				Pdu
    					Msg
    						service_Accept
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01001110'B
    							pduSessionStatus = Omit
    							pduSessionReactivationResult = Omit
    							pduSessionReactResultError = Omit
    							eapMessage = Omit
    					PiggybackedPduList = Omit

    Inter-component message: TC_SRB -> NASEMU_NRNG_PTC:TC_SRB

    SERVICE ACCEPT
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Spare Half Octet [4 bits] = 0x0 [ 0 ]
    	Message Type [8 bits] = 0x4E - SERVICE ACCEPT [ 78 ]

    SERVICE ACCEPT PDU

    DL-DCCH-Message
    	message = c1 = rrcReconfiguration =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcReconfiguration =
    			radioBearerConfig
    				srb-ToAddModList = SEQUENCE OF SRB-ToAddMod
    					SRB-ToAddMod(1)
    						srb-Identity = 2
    				drb-ToAddModList = SEQUENCE OF DRB-ToAddMod
    					DRB-ToAddMod(1)
    						cnAssociation = sdap-Config =
    							pdu-Session = 5
    							sdap-HeaderDL = absent
    							sdap-HeaderUL = present
    							defaultDRB = TRUE
    							mappedQoS-FlowsToAdd = SEQUENCE OF QFI
    								QFI(1) = 1
    						drb-Identity = 2
    						pdcp-Config
    							drb
    								discardTimer = infinity
    								pdcp-SN-SizeUL = len18bits
    								pdcp-SN-SizeDL = len18bits
    								headerCompression = notUsed = NULL
    								integrityProtection = enabled
    								statusReportRequired = true
    				securityConfig
    					securityAlgorithmConfig
    						cipheringAlgorithm = nea2
    						integrityProtAlgorithm = nia2
    					keyToUse = master
    			nonCriticalExtension
    				masterCellGroup = CONTAINING =
    					cellGroupId = 0
    					rlc-BearerToAddModList = SEQUENCE OF RLC-BearerConfig
    						RLC-BearerConfig(1)
    							logicalChannelIdentity = 2
    							servedRadioBearer = srb-Identity = 2
    							mac-LogicalChannelConfig
    								ul-SpecificParameters
    									priority = 3
    									prioritisedBitRate = infinity
    									bucketSizeDuration = ms50
    									logicalChannelGroup = 0
    									schedulingRequestID = 0
    									logicalChannelSR-Mask = FALSE
    									logicalChannelSR-DelayTimerApplied = FALSE
    						RLC-BearerConfig(2)
    							logicalChannelIdentity = 5
    							servedRadioBearer = drb-Identity = 2
    							rlc-Config = am =
    								ul-AM-RLC
    									sn-FieldLength = size18
    									t-PollRetransmit = ms80
    									pollPDU = p32768
    									pollByte = kB750
    									maxRetxThreshold = t8
    								dl-AM-RLC
    									sn-FieldLength = size18
    									t-Reassembly = ms80
    									t-StatusProhibit = ms30
    							mac-LogicalChannelConfig
    								ul-SpecificParameters
    									priority = 1
    									prioritisedBitRate = infinity
    									bucketSizeDuration = ms50
    									logicalChannelGroup = 1
    									schedulingRequestID = 0
    									logicalChannelSR-Mask = FALSE
    									logicalChannelSR-DelayTimerApplied = FALSE
    				dedicatedNAS-MessageList = SEQUENCE OF DedicatedNAS-Message
    					DedicatedNAS-Message(1) = 7E0241526DA504BBF56B

    rrcReconfiguration

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcReconfiguration
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcReconfiguration
    								radioBearerConfig
    									srb_ToAddModList
    										SRB_ToAddMod
    											srb_Identity = 2
    											reestablishPDCP = Omit
    											discardOnPDCP = Omit
    											pdcp_Config = Omit
    									srb3_ToRelease = Omit
    									drb_ToAddModList
    										DRB_ToAddMod
    											cnAssociation
    												sdap_Config
    													pdu_Session = 5
    													sdap_HeaderDL = absent (1)
    													sdap_HeaderUL = present_ (0)
    													defaultDRB = True
    													mappedQoS_FlowsToAdd
    														IntegerType = 1
    													mappedQoS_FlowsToRelease = Omit
    											drb_Identity = 2
    											reestablishPDCP = Omit
    											recoverPDCP = Omit
    											pdcp_Config
    												drb
    													discardTimer = infinity_ (15)
    													pdcp_SN_SizeUL = len18bits (1)
    													pdcp_SN_SizeDL = len18bits (1)
    													headerCompression
    														notUsed = Null
    													integrityProtection = enabled (0)
    													statusReportRequired = true_ (0)
    													outOfOrderDelivery = Omit
    												moreThanOneRLC = Omit
    												t_Reordering = Omit
    												cipheringDisabled = Omit
    									drb_ToReleaseList = Omit
    									securityConfig
    										securityAlgorithmConfig
    											cipheringAlgorithm = nea2 (2)
    											integrityProtAlgorithm = nia2 (2)
    										keyToUse = master (0)
    								secondaryCellGroup = Omit
    								measConfig = Omit
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension
    									masterCellGroup = '400290941979802C908CF91D780C830F3200'O
    									fullConfig = Omit
    									dedicatedNAS_MessageList
    										NG_NAS_Message = '7E0241526DA504BBF56B'O
    									masterKeyUpdate = Omit
    									dedicatedSIB1_Delivery = Omit
    									dedicatedSystemInformationDelivery = Omit
    									otherConfig = Omit
    									nonCriticalExtension = Omit

    Sent from port: NASEMU_NRNG_PTC:SYS_SRB

    UL-DCCH-Message
    	message = c1 = rrcReconfigurationComplete =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcReconfigurationComplete =

    rrcReconfigurationComplete

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 397
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcReconfigurationComplete
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcReconfigurationComplete
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Received on port: NASEMU_NRNG_PTC:SYS_SRB

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 397
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcReconfigurationComplete
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcReconfigurationComplete
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: SRB -> NR5GC_PTC:SRB

    IP_ConfigReq_Type
    	ChangeToRawmode = True

    Inter-component message: NR_CTRL -> IP_PTC:NR_CTRL

    DRBMUX_CONFIG_REQ
    	RoutingInfo

    Sent from port: IP_PTC:IP_CTRL

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    Received on port: IP_PTC:IP_CTRL

    IP_Indication_Type
    	Cnf = True

    Inter-component message: IP -> NR5GC_PTC:IP

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 2
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc = Omit
    		Nas
    			NG_NAS_MSG_Request_Type
    				SecurityProtection
    					Status = 0010'B
    					ForceMacError = False
    				Pdu
    					Msg
    						close_Ue_Test_Loop
    							skipIndicator = 0000'B
    							protocolDiscriminator = 1111'B
    							messageType = 10000000'B
    							ueTestLoopMode = '00'O
    							ueTestLoopModeA_LB_Setup
    								iel = '00'O
    								lbSetupDrbList = Omit
    							ueTestLoopModeB_LB_Setup = Omit
    					PiggybackedPduList = Omit

    Inter-component message: TC_SRB -> NASEMU_NRNG_PTC:TC_SRB

    Close UE Test Loop
    	Transaction Identifier or Skip Indicator [4 bits] = 0x0 [ 0 ]
    	Message Type [8 bits] = 0x80 [ 128 ]
    	UE Test Loop Mode [8 bits] = 0x0 [ 0 ]
    	modeA_lb_setup
    		Length [8 bits] = 0x0 [ 0 ]

    Close UE Test Loop PDU

    DL-DCCH-Message
    	message = c1 = dlInformationTransfer =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = dlInformationTransfer =
    			dedicatedNAS-Message = 7E0242996CC105A574ED62

    dlInformationTransfer

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 2
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					dlInformationTransfer
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							dlInformationTransfer
    								dedicatedNAS_Message = '7E0242996CC105A574ED62'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Sent from port: NASEMU_NRNG_PTC:SYS_SRB

    UL-DCCH-Message
    	message = c1 = ulInformationTransfer =
    		criticalExtensions = ulInformationTransfer =
    			dedicatedNAS-Message = 7E02741C29160520EB

    ulInformationTransfer

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 2
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 400
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ulInformationTransfer
    						criticalExtensions
    							ulInformationTransfer
    								dedicatedNAS_Message = '7E02741C29160520EB'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Received on port: NASEMU_NRNG_PTC:SYS_SRB

    Close UE Test Loop Complete
    	Protocol Discriminator [4 bits] = 0x0 - Group Call Control [ 0 ]
    	Transaction Identifier or Skip Indicator [4 bits] = 0xF [ 15 ]
    	Message Type [8 bits] = 0x81 - Close UE Test Loop Complete [ 129 ]

    Close UE Test Loop Complete PDU

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 2
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 400
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0010'B
    					NasCount = '00000005'O
    				Pdu
    					Msg
    						close_Ue_Test_Loop_Complete
    							skipIndicator = 0000'B
    							protocolDiscriminator = 1111'B
    							messageType = 10000001'B
    					PiggybackedPduList = Omit

    Inter-component message: SRB -> NR5GC_PTC:SRB

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\NR\NR_Component_Base.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 298
    text = Parameter: NR_Component_Base.vc_NR_Global.Ctrl.TestBody = True

    Parameter: NR_Component_Base.vc_NR_Global.Ctrl.TestBody = True

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\NR\NR_Component_Base.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 299
    text = Parameter: NR_Component_Base.vc_NR_Global.Ctrl.VerdictCtrl = normal
    File: NR_Component_Base.ttcn [Line: 299]

    Parameter: NR_Component_Base.vc_NR_Global.Ctrl.VerdictCtrl = normal
    File: NR_Component_Base.ttcn [Line: 299]

    recordType = 24
    summary = Preamble

    Preamble

    IntermediateVerdict = (Pass)
    summary = Intermediate verdict: (PASS)
    TTCN-3 message: initial preliminary pass

    Intermediate verdict: (PASS)
    TTCN-3 message: initial preliminary pass

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 120
    text = Parameter: CommonIP.v_Index = 0
    File: CommonIP.ttcn [Line: 120]

    Parameter: CommonIP.v_Index = 0
    File: CommonIP.ttcn [Line: 120]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 141
    text = Parameter: CommonIP.v_Index = 0
    File: CommonIP.ttcn [Line: 141]

    Parameter: CommonIP.v_Index = 0
    File: CommonIP.ttcn [Line: 141]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 399
    text = Parameter: LoopbackIP.v_DestAddr = ''
    File: LoopbackIP.ttcn [Line: 399]

    Parameter: LoopbackIP.v_DestAddr = ''
    File: LoopbackIP.ttcn [Line: 399]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 403
    text = Parameter: LoopbackIP.v_DestAddr = '192.168.0.26'
    File: LoopbackIP.ttcn [Line: 403]

    Parameter: LoopbackIP.v_DestAddr = '192.168.0.26'
    File: LoopbackIP.ttcn [Line: 403]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 160
    text = Parameter: CommonIP.v_Pattern = '[0-9]+[.][0-9]+[.][0-9]+[.][0-9]+'
    File: CommonIP.ttcn [Line: 160]

    Parameter: CommonIP.v_Pattern = '[0-9]+[.][0-9]+[.][0-9]+[.][0-9]+'
    File: CommonIP.ttcn [Line: 160]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 406
    text = Parameter: LoopbackIP.v_IcmpMsgType = 0
    File: LoopbackIP.ttcn [Line: 406]

    Parameter: LoopbackIP.v_IcmpMsgType = 0
    File: LoopbackIP.ttcn [Line: 406]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 363
    text = Parameter: LoopbackIP.v_IcmpSequenceNumber = '0001'O
    File: LoopbackIP.ttcn [Line: 363]

    Parameter: LoopbackIP.v_IcmpSequenceNumber = '0001'O
    File: LoopbackIP.ttcn [Line: 363]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 364
    text = Parameter: LoopbackIP.v_IcmpPayload = ''O
    File: LoopbackIP.ttcn [Line: 364]

    Parameter: LoopbackIP.v_IcmpPayload = ''O
    File: LoopbackIP.ttcn [Line: 364]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 369
    text = Parameter: LoopbackIP.i = 0
    File: LoopbackIP.ttcn [Line: 369]

    Parameter: LoopbackIP.i = 0
    File: LoopbackIP.ttcn [Line: 369]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 370
    text = Parameter: LoopbackIP.v_IcmpPayload = '00112233445566778899AABBCCDDEEFF'O
    File: LoopbackIP.ttcn [Line: 370]

    Parameter: LoopbackIP.v_IcmpPayload = '00112233445566778899AABBCCDDEEFF'O
    File: LoopbackIP.ttcn [Line: 370]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 369
    text = Parameter: LoopbackIP.i = 1
    File: LoopbackIP.ttcn [Line: 369]

    Parameter: LoopbackIP.i = 1
    File: LoopbackIP.ttcn [Line: 369]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 334
    text = Parameter: LoopbackIP.v_ChecksumDummy = '0000'O
    File: LoopbackIP.ttcn [Line: 334]

    Parameter: LoopbackIP.v_ChecksumDummy = '0000'O
    File: LoopbackIP.ttcn [Line: 334]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 335
    text = Parameter: LoopbackIP.v_Id = '0001'O
    File: LoopbackIP.ttcn [Line: 335]

    Parameter: LoopbackIP.v_Id = '0001'O
    File: LoopbackIP.ttcn [Line: 335]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 336
    text = Parameter: LoopbackIP.v_OctetString = ''O
    File: LoopbackIP.ttcn [Line: 336]

    Parameter: LoopbackIP.v_OctetString = ''O
    File: LoopbackIP.ttcn [Line: 336]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 338
    text = Parameter: LoopbackIP.v_OctetString = '00'O
    File: LoopbackIP.ttcn [Line: 338]

    Parameter: LoopbackIP.v_OctetString = '00'O
    File: LoopbackIP.ttcn [Line: 338]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 339
    text = Parameter: LoopbackIP.v_OctetString = '0000'O
    File: LoopbackIP.ttcn [Line: 339]

    Parameter: LoopbackIP.v_OctetString = '0000'O
    File: LoopbackIP.ttcn [Line: 339]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 359
    text = Parameter: CommonIP.v_DataLength = 24
    File: CommonIP.ttcn [Line: 359]

    Parameter: CommonIP.v_DataLength = 24
    File: CommonIP.ttcn [Line: 359]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 360
    text = Parameter: CommonIP.v_Sum = 0
    File: CommonIP.ttcn [Line: 360]

    Parameter: CommonIP.v_Sum = 0
    File: CommonIP.ttcn [Line: 360]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 366
    text = Parameter: CommonIP.i = 0
    File: CommonIP.ttcn [Line: 366]

    Parameter: CommonIP.i = 0
    File: CommonIP.ttcn [Line: 366]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 367
    text = Parameter: CommonIP.v_Word = '0000'O
    File: CommonIP.ttcn [Line: 367]

    Parameter: CommonIP.v_Word = '0000'O
    File: CommonIP.ttcn [Line: 367]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 368
    text = Parameter: CommonIP.v_Sum = 0
    File: CommonIP.ttcn [Line: 368]

    Parameter: CommonIP.v_Sum = 0
    File: CommonIP.ttcn [Line: 368]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 366
    text = Parameter: CommonIP.i = 2
    File: CommonIP.ttcn [Line: 366]

    Parameter: CommonIP.i = 2
    File: CommonIP.ttcn [Line: 366]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 367
    text = Parameter: CommonIP.v_Word = '0000'O
    File: CommonIP.ttcn [Line: 367]

    Parameter: CommonIP.v_Word = '0000'O
    File: CommonIP.ttcn [Line: 367]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 368
    text = Parameter: CommonIP.v_Sum = 0
    File: CommonIP.ttcn [Line: 368]

    Parameter: CommonIP.v_Sum = 0
    File: CommonIP.ttcn [Line: 368]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 366
    text = Parameter: CommonIP.i = 4
    File: CommonIP.ttcn [Line: 366]

    Parameter: CommonIP.i = 4
    File: CommonIP.ttcn [Line: 366]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 367
    text = Parameter: CommonIP.v_Word = '0001'O
    File: CommonIP.ttcn [Line: 367]

    Parameter: CommonIP.v_Word = '0001'O
    File: CommonIP.ttcn [Line: 367]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 368
    text = Parameter: CommonIP.v_Sum = 1
    File: CommonIP.ttcn [Line: 368]

    Parameter: CommonIP.v_Sum = 1
    File: CommonIP.ttcn [Line: 368]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 366
    text = Parameter: CommonIP.i = 6
    File: CommonIP.ttcn [Line: 366]

    Parameter: CommonIP.i = 6
    File: CommonIP.ttcn [Line: 366]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 367
    text = Parameter: CommonIP.v_Word = '0001'O
    File: CommonIP.ttcn [Line: 367]

    Parameter: CommonIP.v_Word = '0001'O
    File: CommonIP.ttcn [Line: 367]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 368
    text = Parameter: CommonIP.v_Sum = 2
    File: CommonIP.ttcn [Line: 368]

    Parameter: CommonIP.v_Sum = 2
    File: CommonIP.ttcn [Line: 368]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 366
    text = Parameter: CommonIP.i = 8
    File: CommonIP.ttcn [Line: 366]

    Parameter: CommonIP.i = 8
    File: CommonIP.ttcn [Line: 366]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 367
    text = Parameter: CommonIP.v_Word = '0011'O
    File: CommonIP.ttcn [Line: 367]

    Parameter: CommonIP.v_Word = '0011'O
    File: CommonIP.ttcn [Line: 367]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 368
    text = Parameter: CommonIP.v_Sum = 19
    File: CommonIP.ttcn [Line: 368]

    Parameter: CommonIP.v_Sum = 19
    File: CommonIP.ttcn [Line: 368]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 366
    text = Parameter: CommonIP.i = 10
    File: CommonIP.ttcn [Line: 366]

    Parameter: CommonIP.i = 10
    File: CommonIP.ttcn [Line: 366]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 367
    text = Parameter: CommonIP.v_Word = '2233'O
    File: CommonIP.ttcn [Line: 367]

    Parameter: CommonIP.v_Word = '2233'O
    File: CommonIP.ttcn [Line: 367]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 368
    text = Parameter: CommonIP.v_Sum = 8774
    File: CommonIP.ttcn [Line: 368]

    Parameter: CommonIP.v_Sum = 8774
    File: CommonIP.ttcn [Line: 368]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 366
    text = Parameter: CommonIP.i = 12
    File: CommonIP.ttcn [Line: 366]

    Parameter: CommonIP.i = 12
    File: CommonIP.ttcn [Line: 366]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 367
    text = Parameter: CommonIP.v_Word = '4455'O
    File: CommonIP.ttcn [Line: 367]

    Parameter: CommonIP.v_Word = '4455'O
    File: CommonIP.ttcn [Line: 367]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 368
    text = Parameter: CommonIP.v_Sum = 26267
    File: CommonIP.ttcn [Line: 368]

    Parameter: CommonIP.v_Sum = 26267
    File: CommonIP.ttcn [Line: 368]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 366
    text = Parameter: CommonIP.i = 14
    File: CommonIP.ttcn [Line: 366]

    Parameter: CommonIP.i = 14
    File: CommonIP.ttcn [Line: 366]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 367
    text = Parameter: CommonIP.v_Word = '6677'O
    File: CommonIP.ttcn [Line: 367]

    Parameter: CommonIP.v_Word = '6677'O
    File: CommonIP.ttcn [Line: 367]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 368
    text = Parameter: CommonIP.v_Sum = 52498
    File: CommonIP.ttcn [Line: 368]

    Parameter: CommonIP.v_Sum = 52498
    File: CommonIP.ttcn [Line: 368]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 366
    text = Parameter: CommonIP.i = 16
    File: CommonIP.ttcn [Line: 366]

    Parameter: CommonIP.i = 16
    File: CommonIP.ttcn [Line: 366]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 367
    text = Parameter: CommonIP.v_Word = '8899'O
    File: CommonIP.ttcn [Line: 367]

    Parameter: CommonIP.v_Word = '8899'O
    File: CommonIP.ttcn [Line: 367]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 368
    text = Parameter: CommonIP.v_Sum = 87467
    File: CommonIP.ttcn [Line: 368]

    Parameter: CommonIP.v_Sum = 87467
    File: CommonIP.ttcn [Line: 368]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 366
    text = Parameter: CommonIP.i = 18
    File: CommonIP.ttcn [Line: 366]

    Parameter: CommonIP.i = 18
    File: CommonIP.ttcn [Line: 366]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 367
    text = Parameter: CommonIP.v_Word = 'AABB'O
    File: CommonIP.ttcn [Line: 367]

    Parameter: CommonIP.v_Word = 'AABB'O
    File: CommonIP.ttcn [Line: 367]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 368
    text = Parameter: CommonIP.v_Sum = 131174
    File: CommonIP.ttcn [Line: 368]

    Parameter: CommonIP.v_Sum = 131174
    File: CommonIP.ttcn [Line: 368]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 366
    text = Parameter: CommonIP.i = 20
    File: CommonIP.ttcn [Line: 366]

    Parameter: CommonIP.i = 20
    File: CommonIP.ttcn [Line: 366]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 367
    text = Parameter: CommonIP.v_Word = 'CCDD'O
    File: CommonIP.ttcn [Line: 367]

    Parameter: CommonIP.v_Word = 'CCDD'O
    File: CommonIP.ttcn [Line: 367]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 368
    text = Parameter: CommonIP.v_Sum = 183619
    File: CommonIP.ttcn [Line: 368]

    Parameter: CommonIP.v_Sum = 183619
    File: CommonIP.ttcn [Line: 368]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 366
    text = Parameter: CommonIP.i = 22
    File: CommonIP.ttcn [Line: 366]

    Parameter: CommonIP.i = 22
    File: CommonIP.ttcn [Line: 366]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 367
    text = Parameter: CommonIP.v_Word = 'EEFF'O
    File: CommonIP.ttcn [Line: 367]

    Parameter: CommonIP.v_Word = 'EEFF'O
    File: CommonIP.ttcn [Line: 367]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 368
    text = Parameter: CommonIP.v_Sum = 244802
    File: CommonIP.ttcn [Line: 368]

    Parameter: CommonIP.v_Sum = 244802
    File: CommonIP.ttcn [Line: 368]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 366
    text = Parameter: CommonIP.i = 24
    File: CommonIP.ttcn [Line: 366]

    Parameter: CommonIP.i = 24
    File: CommonIP.ttcn [Line: 366]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 372
    text = Parameter: CommonIP.v_Sum = 48197
    File: CommonIP.ttcn [Line: 372]

    Parameter: CommonIP.v_Sum = 48197
    File: CommonIP.ttcn [Line: 372]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 375
    text = Parameter: CommonIP.v_Sum = 17338
    File: CommonIP.ttcn [Line: 375]

    Parameter: CommonIP.v_Sum = 17338
    File: CommonIP.ttcn [Line: 375]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 340
    text = Parameter: LoopbackIP.v_OctetString = '000043BA'O
    File: LoopbackIP.ttcn [Line: 340]

    Parameter: LoopbackIP.v_OctetString = '000043BA'O
    File: LoopbackIP.ttcn [Line: 340]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 341
    text = Parameter: LoopbackIP.v_OctetString = '000043BA0001'O
    File: LoopbackIP.ttcn [Line: 341]

    Parameter: LoopbackIP.v_OctetString = '000043BA0001'O
    File: LoopbackIP.ttcn [Line: 341]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 342
    text = Parameter: LoopbackIP.v_OctetString = '000043BA00010001'O
    File: LoopbackIP.ttcn [Line: 342]

    Parameter: LoopbackIP.v_OctetString = '000043BA00010001'O
    File: LoopbackIP.ttcn [Line: 342]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 343
    text = Parameter: LoopbackIP.v_OctetString = '000043BA0001000100112233445566778899AABBCCDDEEFF'O
    File: LoopbackIP.ttcn [Line: 343]

    Parameter: LoopbackIP.v_OctetString = '000043BA0001000100112233445566778899AABBCCDDEEFF'O
    File: LoopbackIP.ttcn [Line: 343]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 372
    text = Parameter: LoopbackIP.v_Payload = '000043BA0001000100112233445566778899AABBCCDDEEFF'O
    File: LoopbackIP.ttcn [Line: 372]

    Parameter: LoopbackIP.v_Payload = '000043BA0001000100112233445566778899AABBCCDDEEFF'O
    File: LoopbackIP.ttcn [Line: 372]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 88
    text = Parameter: LoopbackIP.v_TotalLength = 44
    File: LoopbackIP.ttcn [Line: 88]

    Parameter: LoopbackIP.v_TotalLength = 44
    File: LoopbackIP.ttcn [Line: 88]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 206
    text = Parameter: CommonIP.v_IPv4AddrOct = ''O
    File: CommonIP.ttcn [Line: 206]

    Parameter: CommonIP.v_IPv4AddrOct = ''O
    File: CommonIP.ttcn [Line: 206]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 207
    text = Parameter: CommonIP.v_FieldCnt = 4
    File: CommonIP.ttcn [Line: 207]

    Parameter: CommonIP.v_FieldCnt = 4
    File: CommonIP.ttcn [Line: 207]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 214
    text = Parameter: CommonIP.i = 0
    File: CommonIP.ttcn [Line: 214]

    Parameter: CommonIP.i = 0
    File: CommonIP.ttcn [Line: 214]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 215
    text = Parameter: CommonIP.v_IntVal = 192
    File: CommonIP.ttcn [Line: 215]

    Parameter: CommonIP.v_IntVal = 192
    File: CommonIP.ttcn [Line: 215]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 216
    text = Parameter: CommonIP.v_IPv4AddrOct = 'C0'O
    File: CommonIP.ttcn [Line: 216]

    Parameter: CommonIP.v_IPv4AddrOct = 'C0'O
    File: CommonIP.ttcn [Line: 216]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 214
    text = Parameter: CommonIP.i = 1
    File: CommonIP.ttcn [Line: 214]

    Parameter: CommonIP.i = 1
    File: CommonIP.ttcn [Line: 214]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 215
    text = Parameter: CommonIP.v_IntVal = 168
    File: CommonIP.ttcn [Line: 215]

    Parameter: CommonIP.v_IntVal = 168
    File: CommonIP.ttcn [Line: 215]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 216
    text = Parameter: CommonIP.v_IPv4AddrOct = 'C0A8'O
    File: CommonIP.ttcn [Line: 216]

    Parameter: CommonIP.v_IPv4AddrOct = 'C0A8'O
    File: CommonIP.ttcn [Line: 216]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 214
    text = Parameter: CommonIP.i = 2
    File: CommonIP.ttcn [Line: 214]

    Parameter: CommonIP.i = 2
    File: CommonIP.ttcn [Line: 214]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 215
    text = Parameter: CommonIP.v_IntVal = 0
    File: CommonIP.ttcn [Line: 215]

    Parameter: CommonIP.v_IntVal = 0
    File: CommonIP.ttcn [Line: 215]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 216
    text = Parameter: CommonIP.v_IPv4AddrOct = 'C0A800'O
    File: CommonIP.ttcn [Line: 216]

    Parameter: CommonIP.v_IPv4AddrOct = 'C0A800'O
    File: CommonIP.ttcn [Line: 216]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 214
    text = Parameter: CommonIP.i = 3
    File: CommonIP.ttcn [Line: 214]

    Parameter: CommonIP.i = 3
    File: CommonIP.ttcn [Line: 214]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 215
    text = Parameter: CommonIP.v_IntVal = 26
    File: CommonIP.ttcn [Line: 215]

    Parameter: CommonIP.v_IntVal = 26
    File: CommonIP.ttcn [Line: 215]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 216
    text = Parameter: CommonIP.v_IPv4AddrOct = 'C0A8001A'O
    File: CommonIP.ttcn [Line: 216]

    Parameter: CommonIP.v_IPv4AddrOct = 'C0A8001A'O
    File: CommonIP.ttcn [Line: 216]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 214
    text = Parameter: CommonIP.i = 4
    File: CommonIP.ttcn [Line: 214]

    Parameter: CommonIP.i = 4
    File: CommonIP.ttcn [Line: 214]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 89
    text = Parameter: LoopbackIP.v_SourceAddrStr = 'C0A8001A'O
    File: LoopbackIP.ttcn [Line: 89]

    Parameter: LoopbackIP.v_SourceAddrStr = 'C0A8001A'O
    File: LoopbackIP.ttcn [Line: 89]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 206
    text = Parameter: CommonIP.v_IPv4AddrOct = ''O
    File: CommonIP.ttcn [Line: 206]

    Parameter: CommonIP.v_IPv4AddrOct = ''O
    File: CommonIP.ttcn [Line: 206]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 207
    text = Parameter: CommonIP.v_FieldCnt = 4
    File: CommonIP.ttcn [Line: 207]

    Parameter: CommonIP.v_FieldCnt = 4
    File: CommonIP.ttcn [Line: 207]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 214
    text = Parameter: CommonIP.i = 0
    File: CommonIP.ttcn [Line: 214]

    Parameter: CommonIP.i = 0
    File: CommonIP.ttcn [Line: 214]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 215
    text = Parameter: CommonIP.v_IntVal = 192
    File: CommonIP.ttcn [Line: 215]

    Parameter: CommonIP.v_IntVal = 192
    File: CommonIP.ttcn [Line: 215]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 216
    text = Parameter: CommonIP.v_IPv4AddrOct = 'C0'O
    File: CommonIP.ttcn [Line: 216]

    Parameter: CommonIP.v_IPv4AddrOct = 'C0'O
    File: CommonIP.ttcn [Line: 216]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 214
    text = Parameter: CommonIP.i = 1
    File: CommonIP.ttcn [Line: 214]

    Parameter: CommonIP.i = 1
    File: CommonIP.ttcn [Line: 214]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 215
    text = Parameter: CommonIP.v_IntVal = 168
    File: CommonIP.ttcn [Line: 215]

    Parameter: CommonIP.v_IntVal = 168
    File: CommonIP.ttcn [Line: 215]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 216
    text = Parameter: CommonIP.v_IPv4AddrOct = 'C0A8'O
    File: CommonIP.ttcn [Line: 216]

    Parameter: CommonIP.v_IPv4AddrOct = 'C0A8'O
    File: CommonIP.ttcn [Line: 216]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 214
    text = Parameter: CommonIP.i = 2
    File: CommonIP.ttcn [Line: 214]

    Parameter: CommonIP.i = 2
    File: CommonIP.ttcn [Line: 214]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 215
    text = Parameter: CommonIP.v_IntVal = 0
    File: CommonIP.ttcn [Line: 215]

    Parameter: CommonIP.v_IntVal = 0
    File: CommonIP.ttcn [Line: 215]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 216
    text = Parameter: CommonIP.v_IPv4AddrOct = 'C0A800'O
    File: CommonIP.ttcn [Line: 216]

    Parameter: CommonIP.v_IPv4AddrOct = 'C0A800'O
    File: CommonIP.ttcn [Line: 216]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 214
    text = Parameter: CommonIP.i = 3
    File: CommonIP.ttcn [Line: 214]

    Parameter: CommonIP.i = 3
    File: CommonIP.ttcn [Line: 214]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 215
    text = Parameter: CommonIP.v_IntVal = 26
    File: CommonIP.ttcn [Line: 215]

    Parameter: CommonIP.v_IntVal = 26
    File: CommonIP.ttcn [Line: 215]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 216
    text = Parameter: CommonIP.v_IPv4AddrOct = 'C0A8001A'O
    File: CommonIP.ttcn [Line: 216]

    Parameter: CommonIP.v_IPv4AddrOct = 'C0A8001A'O
    File: CommonIP.ttcn [Line: 216]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 214
    text = Parameter: CommonIP.i = 4
    File: CommonIP.ttcn [Line: 214]

    Parameter: CommonIP.i = 4
    File: CommonIP.ttcn [Line: 214]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 90
    text = Parameter: LoopbackIP.v_DestAddrStr = 'C0A8001A'O
    File: LoopbackIP.ttcn [Line: 90]

    Parameter: LoopbackIP.v_DestAddrStr = 'C0A8001A'O
    File: LoopbackIP.ttcn [Line: 90]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 94
    text = Parameter: LoopbackIP.v_OctetString = '45'O
    File: LoopbackIP.ttcn [Line: 94]

    Parameter: LoopbackIP.v_OctetString = '45'O
    File: LoopbackIP.ttcn [Line: 94]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 95
    text = Parameter: LoopbackIP.v_OctetString = '4500'O
    File: LoopbackIP.ttcn [Line: 95]

    Parameter: LoopbackIP.v_OctetString = '4500'O
    File: LoopbackIP.ttcn [Line: 95]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 96
    text = Parameter: LoopbackIP.v_OctetString = '4500002C'O
    File: LoopbackIP.ttcn [Line: 96]

    Parameter: LoopbackIP.v_OctetString = '4500002C'O
    File: LoopbackIP.ttcn [Line: 96]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 97
    text = Parameter: LoopbackIP.v_OctetString = '4500002C1001'O
    File: LoopbackIP.ttcn [Line: 97]

    Parameter: LoopbackIP.v_OctetString = '4500002C1001'O
    File: LoopbackIP.ttcn [Line: 97]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 98
    text = Parameter: LoopbackIP.v_OctetString = '4500002C10010000'O
    File: LoopbackIP.ttcn [Line: 98]

    Parameter: LoopbackIP.v_OctetString = '4500002C10010000'O
    File: LoopbackIP.ttcn [Line: 98]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 99
    text = Parameter: LoopbackIP.v_OctetString = '4500002C1001000080'O
    File: LoopbackIP.ttcn [Line: 99]

    Parameter: LoopbackIP.v_OctetString = '4500002C1001000080'O
    File: LoopbackIP.ttcn [Line: 99]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 100
    text = Parameter: LoopbackIP.v_OctetString = '4500002C100100008001'O
    File: LoopbackIP.ttcn [Line: 100]

    Parameter: LoopbackIP.v_OctetString = '4500002C100100008001'O
    File: LoopbackIP.ttcn [Line: 100]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 359
    text = Parameter: CommonIP.v_DataLength = 20
    File: CommonIP.ttcn [Line: 359]

    Parameter: CommonIP.v_DataLength = 20
    File: CommonIP.ttcn [Line: 359]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 360
    text = Parameter: CommonIP.v_Sum = 0
    File: CommonIP.ttcn [Line: 360]

    Parameter: CommonIP.v_Sum = 0
    File: CommonIP.ttcn [Line: 360]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 366
    text = Parameter: CommonIP.i = 0
    File: CommonIP.ttcn [Line: 366]

    Parameter: CommonIP.i = 0
    File: CommonIP.ttcn [Line: 366]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 367
    text = Parameter: CommonIP.v_Word = '4500'O
    File: CommonIP.ttcn [Line: 367]

    Parameter: CommonIP.v_Word = '4500'O
    File: CommonIP.ttcn [Line: 367]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 368
    text = Parameter: CommonIP.v_Sum = 17664
    File: CommonIP.ttcn [Line: 368]

    Parameter: CommonIP.v_Sum = 17664
    File: CommonIP.ttcn [Line: 368]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 366
    text = Parameter: CommonIP.i = 2
    File: CommonIP.ttcn [Line: 366]

    Parameter: CommonIP.i = 2
    File: CommonIP.ttcn [Line: 366]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 367
    text = Parameter: CommonIP.v_Word = '002C'O
    File: CommonIP.ttcn [Line: 367]

    Parameter: CommonIP.v_Word = '002C'O
    File: CommonIP.ttcn [Line: 367]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 368
    text = Parameter: CommonIP.v_Sum = 17708
    File: CommonIP.ttcn [Line: 368]

    Parameter: CommonIP.v_Sum = 17708
    File: CommonIP.ttcn [Line: 368]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 366
    text = Parameter: CommonIP.i = 4
    File: CommonIP.ttcn [Line: 366]

    Parameter: CommonIP.i = 4
    File: CommonIP.ttcn [Line: 366]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 367
    text = Parameter: CommonIP.v_Word = '1001'O
    File: CommonIP.ttcn [Line: 367]

    Parameter: CommonIP.v_Word = '1001'O
    File: CommonIP.ttcn [Line: 367]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 368
    text = Parameter: CommonIP.v_Sum = 21805
    File: CommonIP.ttcn [Line: 368]

    Parameter: CommonIP.v_Sum = 21805
    File: CommonIP.ttcn [Line: 368]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 366
    text = Parameter: CommonIP.i = 6
    File: CommonIP.ttcn [Line: 366]

    Parameter: CommonIP.i = 6
    File: CommonIP.ttcn [Line: 366]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 367
    text = Parameter: CommonIP.v_Word = '0000'O
    File: CommonIP.ttcn [Line: 367]

    Parameter: CommonIP.v_Word = '0000'O
    File: CommonIP.ttcn [Line: 367]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 368
    text = Parameter: CommonIP.v_Sum = 21805
    File: CommonIP.ttcn [Line: 368]

    Parameter: CommonIP.v_Sum = 21805
    File: CommonIP.ttcn [Line: 368]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 366
    text = Parameter: CommonIP.i = 8
    File: CommonIP.ttcn [Line: 366]

    Parameter: CommonIP.i = 8
    File: CommonIP.ttcn [Line: 366]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 367
    text = Parameter: CommonIP.v_Word = '8001'O
    File: CommonIP.ttcn [Line: 367]

    Parameter: CommonIP.v_Word = '8001'O
    File: CommonIP.ttcn [Line: 367]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 368
    text = Parameter: CommonIP.v_Sum = 54574
    File: CommonIP.ttcn [Line: 368]

    Parameter: CommonIP.v_Sum = 54574
    File: CommonIP.ttcn [Line: 368]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 366
    text = Parameter: CommonIP.i = 10
    File: CommonIP.ttcn [Line: 366]

    Parameter: CommonIP.i = 10
    File: CommonIP.ttcn [Line: 366]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 367
    text = Parameter: CommonIP.v_Word = '0000'O
    File: CommonIP.ttcn [Line: 367]

    Parameter: CommonIP.v_Word = '0000'O
    File: CommonIP.ttcn [Line: 367]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 368
    text = Parameter: CommonIP.v_Sum = 54574
    File: CommonIP.ttcn [Line: 368]

    Parameter: CommonIP.v_Sum = 54574
    File: CommonIP.ttcn [Line: 368]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 366
    text = Parameter: CommonIP.i = 12
    File: CommonIP.ttcn [Line: 366]

    Parameter: CommonIP.i = 12
    File: CommonIP.ttcn [Line: 366]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 367
    text = Parameter: CommonIP.v_Word = 'C0A8'O
    File: CommonIP.ttcn [Line: 367]

    Parameter: CommonIP.v_Word = 'C0A8'O
    File: CommonIP.ttcn [Line: 367]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 368
    text = Parameter: CommonIP.v_Sum = 103894
    File: CommonIP.ttcn [Line: 368]

    Parameter: CommonIP.v_Sum = 103894
    File: CommonIP.ttcn [Line: 368]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 366
    text = Parameter: CommonIP.i = 14
    File: CommonIP.ttcn [Line: 366]

    Parameter: CommonIP.i = 14
    File: CommonIP.ttcn [Line: 366]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 367
    text = Parameter: CommonIP.v_Word = '001A'O
    File: CommonIP.ttcn [Line: 367]

    Parameter: CommonIP.v_Word = '001A'O
    File: CommonIP.ttcn [Line: 367]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 368
    text = Parameter: CommonIP.v_Sum = 103920
    File: CommonIP.ttcn [Line: 368]

    Parameter: CommonIP.v_Sum = 103920
    File: CommonIP.ttcn [Line: 368]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 366
    text = Parameter: CommonIP.i = 16
    File: CommonIP.ttcn [Line: 366]

    Parameter: CommonIP.i = 16
    File: CommonIP.ttcn [Line: 366]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 367
    text = Parameter: CommonIP.v_Word = 'C0A8'O
    File: CommonIP.ttcn [Line: 367]

    Parameter: CommonIP.v_Word = 'C0A8'O
    File: CommonIP.ttcn [Line: 367]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 368
    text = Parameter: CommonIP.v_Sum = 153240
    File: CommonIP.ttcn [Line: 368]

    Parameter: CommonIP.v_Sum = 153240
    File: CommonIP.ttcn [Line: 368]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 366
    text = Parameter: CommonIP.i = 18
    File: CommonIP.ttcn [Line: 366]

    Parameter: CommonIP.i = 18
    File: CommonIP.ttcn [Line: 366]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 367
    text = Parameter: CommonIP.v_Word = '001A'O
    File: CommonIP.ttcn [Line: 367]

    Parameter: CommonIP.v_Word = '001A'O
    File: CommonIP.ttcn [Line: 367]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 368
    text = Parameter: CommonIP.v_Sum = 153266
    File: CommonIP.ttcn [Line: 368]

    Parameter: CommonIP.v_Sum = 153266
    File: CommonIP.ttcn [Line: 368]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 366
    text = Parameter: CommonIP.i = 20
    File: CommonIP.ttcn [Line: 366]

    Parameter: CommonIP.i = 20
    File: CommonIP.ttcn [Line: 366]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 372
    text = Parameter: CommonIP.v_Sum = 22196
    File: CommonIP.ttcn [Line: 372]

    Parameter: CommonIP.v_Sum = 22196
    File: CommonIP.ttcn [Line: 372]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 375
    text = Parameter: CommonIP.v_Sum = 43339
    File: CommonIP.ttcn [Line: 375]

    Parameter: CommonIP.v_Sum = 43339
    File: CommonIP.ttcn [Line: 375]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 101
    text = Parameter: LoopbackIP.v_OctetString = '4500002C100100008001A94B'O
    File: LoopbackIP.ttcn [Line: 101]

    Parameter: LoopbackIP.v_OctetString = '4500002C100100008001A94B'O
    File: LoopbackIP.ttcn [Line: 101]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 102
    text = Parameter: LoopbackIP.v_OctetString = '4500002C100100008001A94BC0A8001A'O
    File: LoopbackIP.ttcn [Line: 102]

    Parameter: LoopbackIP.v_OctetString = '4500002C100100008001A94BC0A8001A'O
    File: LoopbackIP.ttcn [Line: 102]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 103
    text = Parameter: LoopbackIP.v_OctetString = '4500002C100100008001A94BC0A8001AC0A8001A'O
    File: LoopbackIP.ttcn [Line: 103]

    Parameter: LoopbackIP.v_OctetString = '4500002C100100008001A94BC0A8001AC0A8001A'O
    File: LoopbackIP.ttcn [Line: 103]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 104
    text = Parameter: LoopbackIP.v_OctetString = '4500002C100100008001A94BC0A8001AC0A8001A000043BA0001000100112233445566778899AABBCCDDEEFF'O
    File: LoopbackIP.ttcn [Line: 104]

    Parameter: LoopbackIP.v_OctetString = '4500002C100100008001A94BC0A8001AC0A8001A000043BA0001000100112233445566778899AABBCCDDEEFF'O
    File: LoopbackIP.ttcn [Line: 104]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 376
    text = Parameter: LoopbackIP.v_IpPacket = '4500002C100100008001A94BC0A8001AC0A8001A000043BA0001000100112233445566778899AABBCCDDEEFF'O
    File: LoopbackIP.ttcn [Line: 376]

    Parameter: LoopbackIP.v_IpPacket = '4500002C100100008001A94BC0A8001AC0A8001A000043BA0001000100112233445566778899AABBCCDDEEFF'O
    File: LoopbackIP.ttcn [Line: 376]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\CommonIP\LoopbackIP.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 410
    text = Parameter: LoopbackIP.v_IpPacket = '4500002C100100008001A94BC0A8001AC0A8001A000043BA0001000100112233445566778899AABBCCDDEEFF'O
    File: LoopbackIP.ttcn [Line: 410]

    Parameter: LoopbackIP.v_IpPacket = '4500002C100100008001A94BC0A8001AC0A8001A000043BA0001000100112233445566778899AABBCCDDEEFF'O
    File: LoopbackIP.ttcn [Line: 410]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\NR_TC_Common\7_1_3\PDCP_TC_Common_NR.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 328
    text = Parameter: PDCP_TC_Common_NR.v_IPData = '4500002C100100008001A94BC0A8001AC0A8001A000043BA0001000100112233445566778899AABBCCDDEEFF'O
    File: PDCP_TC_Common_NR.ttcn [Line: 328]

    Parameter: PDCP_TC_Common_NR.v_IPData = '4500002C100100008001A94BC0A8001AC0A8001A000043BA0001000100112233445566778899AABBCCDDEEFF'O
    File: PDCP_TC_Common_NR.ttcn [Line: 328]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\NR_TC_Common\7_1_3\PDCP_TC_Common_NR.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 331
    text = Parameter: PDCP_TC_Common_NR.v_IntegrityAlg = nia2
    File: PDCP_TC_Common_NR.ttcn [Line: 331]

    Parameter: PDCP_TC_Common_NR.v_IntegrityAlg = nia2
    File: PDCP_TC_Common_NR.ttcn [Line: 331]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\NR_TC_Common\7_1_3\PDCP_TC_Common_NR.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 332
    text = Parameter: PDCP_TC_Common_NR.v_DontWaitForComplete = False
    File: PDCP_TC_Common_NR.ttcn [Line: 332]

    Parameter: PDCP_TC_Common_NR.v_DontWaitForComplete = False
    File: PDCP_TC_Common_NR.ttcn [Line: 332]

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\Common4G5G\Common4G5G_Templates.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 283
    text = Parameter: Common4G5G_Templates.v_CnfFlag = False
    File: Common4G5G_Templates.ttcn [Line: 283]

    Parameter: Common4G5G_Templates.v_CnfFlag = False
    File: Common4G5G_Templates.ttcn [Line: 283]

    IP PDU
    	IP Header
    		IP Version = IPv4
    		Internet Header Length = 5 (in 32-bit words)
    		Type of Service
    			Precedence = 0(Routine)
    			Delay = 0(Normal Delay)
    			Throughput = 0(Normal Throughput)
    			Reliability = 0(Normal Reliability)
    		Total Length = 44 (in Octets)
    		Identification = 0x1001
    		Flags
    			DF = 0(May Fragment)
    			MF = 0(Last Fragment)
    		Fragment Offset = 0 (in units of 8 octets)
    		Time to Live = 128 (in seconds)
    		Protocol = 1(Internet Control Message Protocol)
    		Header Checksum = 0xa94b
    		Source Address = 192.168.0.26
    		Destination Address = 192.168.0.26
    		Options =
    	Data Packet = 00,00,43,BA,00,01...

    Not available

    NR_DRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Drb = 2
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	U_Plane
    		SlotDataList
    			NR_DRB_DataPerSlot_DL_Type
    				SlotOffset = 0
    				HarqProcess
    					Automatic = True
    				PduSduList
    					PdcpSdu
    						OctetStringType = '4500002C100100008001A94BC0A8001AC0A8001A000043BA0001000100112233445566778899AABBCCDDEEFF'O
    	SuppressPdcchForC_RNTI = Omit

    Sent from port: NR5GC_PTC:DRB

    recordType = 24
    summary = Step 4a2

    Step 4a2

    IP PDU
    	IP Header
    		IP Version = IPv4
    		Internet Header Length = 5 (in 32-bit words)
    		Type of Service
    			Precedence = 0(Routine)
    			Delay = 0(Normal Delay)
    			Throughput = 0(Normal Throughput)
    			Reliability = 0(Normal Reliability)
    		Total Length = 44 (in Octets)
    		Identification = 0x1001
    		Flags
    			DF = 0(May Fragment)
    			MF = 0(Last Fragment)
    		Fragment Offset = 0 (in units of 8 octets)
    		Time to Live = 128 (in seconds)
    		Protocol = 1(Internet Control Message Protocol)
    		Header Checksum = 0xa94b
    		Source Address = 192.168.0.26
    		Destination Address = 192.168.0.26
    		Options =
    	Data Packet = 00,00,43,BA,00,01...

    Not available

    NR_DRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Drb = 2
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 403
    				Subframe
    					Number = 9
    				HSFN
    					Number = 78
    				Slot
    					Any = True
    		Status
    			Ok = True
    	U_Plane
    		SlotData
    			PduSduList
    				PdcpSdu
    					NR_PDCP_SDU_Type = '4500002C100100008001A94BC0A8001AC0A8001A000043BA0001000100112233445566778899AABBCCDDEEFF'O
    			NoOfTTIs = 1

    Received on port: NR5GC_PTC:DRB

    IntermediateVerdict = (Pass)
    summary = Intermediate verdict: (PASS)
    TTCN-3 message: Step 4a2

    Intermediate verdict: (PASS)
    TTCN-3 message: Step 4a2

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\NR\NR_Component_Base.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 298
    text = Parameter: NR_Component_Base.vc_NR_Global.Ctrl.TestBody = False

    Parameter: NR_Component_Base.vc_NR_Global.Ctrl.TestBody = False

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 2
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc = Omit
    		Nas
    			NG_NAS_MSG_Request_Type
    				SecurityProtection
    					Status = 0010'B
    					ForceMacError = False
    				Pdu
    					Msg
    						open_Ue_Test_Loop
    							skipIndicator = 0000'B
    							protocolDiscriminator = 1111'B
    							messageType = 10000010'B
    					PiggybackedPduList = Omit

    Inter-component message: TC_SRB -> NASEMU_NRNG_PTC:TC_SRB

    Open UE Test Loop
    	Protocol Discriminator [4 bits] = 0x0 - Group Call Control [ 0 ]
    	Transaction Identifier or Skip Indicator [4 bits] = 0xF [ 15 ]
    	Message Type [8 bits] = 0x82 - Open UE Test Loop [ 130 ]

    Open UE Test Loop PDU

    DL-DCCH-Message
    	message = c1 = dlInformationTransfer =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = dlInformationTransfer =
    			dedicatedNAS-Message = 7E02F1CD83C106716B

    dlInformationTransfer

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 2
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					dlInformationTransfer
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							dlInformationTransfer
    								dedicatedNAS_Message = '7E02F1CD83C106716B'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Sent from port: NASEMU_NRNG_PTC:SYS_SRB

    UL-DCCH-Message
    	message = c1 = ulInformationTransfer =
    		criticalExtensions = ulInformationTransfer =
    			dedicatedNAS-Message = 7E0249DE714706B0D9

    ulInformationTransfer

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 2
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 405
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ulInformationTransfer
    						criticalExtensions
    							ulInformationTransfer
    								dedicatedNAS_Message = '7E0249DE714706B0D9'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Received on port: NASEMU_NRNG_PTC:SYS_SRB

    Open UE Test Loop Complete
    	Protocol Discriminator [4 bits] = 0x0 - Group Call Control [ 0 ]
    	Transaction Identifier or Skip Indicator [4 bits] = 0xF [ 15 ]
    	Message Type [8 bits] = 0x83 - Open UE Test Loop Complete [ 131 ]

    Open UE Test Loop Complete PDU

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 2
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 405
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0010'B
    					NasCount = '00000006'O
    				Pdu
    					Msg
    						open_Ue_Test_Loop_Complete
    							skipIndicator = 0000'B
    							protocolDiscriminator = 1111'B
    							messageType = 10000011'B
    					PiggybackedPduList = Omit

    Inter-component message: SRB -> NR5GC_PTC:SRB

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 2
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc = Omit
    		Nas
    			NG_NAS_MSG_Request_Type
    				SecurityProtection
    					Status = 0010'B
    					ForceMacError = False
    				Pdu
    					Msg
    						deactivate_Test_Mode
    							skipIndicator = 0000'B
    							protocolDiscriminator = 1111'B
    							messageType = 10000110'B
    					PiggybackedPduList = Omit

    Inter-component message: TC_SRB -> NASEMU_NRNG_PTC:TC_SRB

    Deactivate Test Mode
    	Protocol Discriminator [4 bits] = 0x0 - Group Call Control [ 0 ]
    	Transaction Identifier or Skip Indicator [4 bits] = 0xF [ 15 ]
    	Message Type [8 bits] = 0x86 - Deactivate Test Mode [ 134 ]

    Deactivate Test Mode PDU

    DL-DCCH-Message
    	message = c1 = dlInformationTransfer =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = dlInformationTransfer =
    			dedicatedNAS-Message = 7E0218DD30BB07517C

    dlInformationTransfer

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 2
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					dlInformationTransfer
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							dlInformationTransfer
    								dedicatedNAS_Message = '7E0218DD30BB07517C'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Sent from port: NASEMU_NRNG_PTC:SYS_SRB

    UL-DCCH-Message
    	message = c1 = ulInformationTransfer =
    		criticalExtensions = ulInformationTransfer =
    			dedicatedNAS-Message = 7E0283513611071A42

    ulInformationTransfer

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 2
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 407
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ulInformationTransfer
    						criticalExtensions
    							ulInformationTransfer
    								dedicatedNAS_Message = '7E0283513611071A42'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Received on port: NASEMU_NRNG_PTC:SYS_SRB

    Deactivate Test Mode Complete
    	Protocol Discriminator [4 bits] = 0x0 - Group Call Control [ 0 ]
    	Transaction Identifier or Skip Indicator [4 bits] = 0xF [ 15 ]
    	Message Type [8 bits] = 0x87 - Deactivate Test Mode Complete [ 135 ]

    Deactivate Test Mode Complete

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 2
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 407
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0010'B
    					NasCount = '00000007'O
    				Pdu
    					Msg
    						deactivate_Test_Mode_Complete
    							skipIndicator = 0000'B
    							protocolDiscriminator = 1111'B
    							messageType = 10000111'B
    					PiggybackedPduList = Omit

    Inter-component message: SRB -> NR5GC_PTC:SRB

    UT_COMMON_CMD
    	Cmd = SWITCH_OFF (114)
    	CnfReq = NO_CNF_REQUIRED (0)
    	ParameterList = Omit

    Inter-component message: PTC_Ut -> MTC_NR5GC:PTC_Ut

    ConstraintMismatch::Received:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = CNF_REQUIRED (1)
    ConstraintMismatch::Expected:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		CnfReq = NO_CNF_REQUIRED (0)

    Message Mismatch: Ut_CnfReq_Type

    ConstraintMismatch::Received:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = CNF_REQUIRED (1)
    ConstraintMismatch::Expected:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		CnfReq = NO_CNF_REQUIRED (0)

    Message Mismatch: Ut_CnfReq_Type

    ConstraintMismatch::Received:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = LOCAL_CNF_REQUIRED (2)
    ConstraintMismatch::Expected:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		CnfReq = NO_CNF_REQUIRED (0)

    Message Mismatch: Ut_CnfReq_Type

    ConstraintMismatch::Received:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = LOCAL_CNF_REQUIRED (2)
    ConstraintMismatch::Expected:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		CnfReq = NO_CNF_REQUIRED (0)

    Message Mismatch: Ut_CnfReq_Type

    timerEvent = 6
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\NR5GC\NR5GC_NASSteps.ttcn
    testName = TC_7_1_3_2_2_NR5GC
    lineNo = 1418
    outStr = Timer: t_T3540, Duration: 9s, Started: 10:22:49

    Timer: t_T3540, Duration: 9s, Started: 10:22:49

    UT_SYSTEM_REQ
    	Cmd
    		MMI
    			Cmd = 'SWITCH_OFF'
    			ParameterList = Omit
    	CnfRequired = NO_CNF_REQUIRED (0)

    Sent from port: MTC_NR5GC:Ut

    UL-DCCH-Message
    	message = c1 = ulInformationTransfer =
    		criticalExtensions = ulInformationTransfer =
    			dedicatedNAS-Message = 7E0290CBAFBF08910F4805350EDF94A591E2A42844E588EE

    ulInformationTransfer

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 2
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 519
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ulInformationTransfer
    						criticalExtensions
    							ulInformationTransfer
    								dedicatedNAS_Message = '7E0290CBAFBF08910F4805350EDF94A591E2A42844E588EE'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Received on port: NASEMU_NRNG_PTC:SYS_SRB

    DEREGISTRATION REQUEST ORIGINATED
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Spare Half Octet [4 bits] = 0x0 [ 0 ]
    	dereg_req_mt [8 bits] = 0x45 [ 69 ]
    	de_reg_tp
    		switch_off [1 bit] = 0x0 [ 0 ]
    		re_reg_req [1 bit] = 0x0 [ 0 ]
    		Access_typ [2 bits] = 0x1 [ 1 ]
    	ngksi
    		Type of security context flag [1 bit] = 0x1 [ 1 ]
    		nas_key_set_identi [3 bits] = 0x1 [ 1 ]
    	fivegs_mob_id
    		IE Length [16 bits] = 0xB [ 11 ]
    		id_dig [4 bits] = 0xF [ 15 ]
    		Spare Bits [1 bit] = 0x0 [ 0 ]
    		typ_id [3 bits] = 0x2 [ 2 ]
    		mcc_dig_2 [4 bits] = 0x0 [ 0 ]
    		mcc_dig_1 [4 bits] = 0x0 [ 0 ]
    		Mobile Network Code 3rd Digit [4 bits] = 0xF [ 15 ]
    		Mobile Country Code 3rd Digit [4 bits] = 0x1 [ 1 ]
    		mnc_dig_2 [4 bits] = 0x1 [ 1 ]
    		mnc_dig_1 [4 bits] = 0x0 [ 0 ]
    		amf_reg_id = 0xFE [ 254 ]
    		amf_set_id = 0x00 [ 0 ]
    		amf_set_id_conti [2 bits] = 0x1 [ 1 ]
    		amf_pntr [6 bits] = 0x1 [ 1 ]
    		fiveg_tmsi = 0xC2345678 [ 3258209912 ]

    DEREGISTRATION REQUEST ORIGINATED PDU

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 2
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 519
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0010'B
    					NasCount = '00000008'O
    				Pdu
    					Msg
    						deregistration_RequestMO
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01000101'B
    							ngKSI
    								iei = Omit
    								tsc = 0'B
    								nasKeySetId = 001'B
    							deregistrationType
    								switchOff = 1'B
    								reRegistration = 0'B
    								accessType = 01'B
    							ngMobileId
    								iei = Omit
    								iel = '000B'O
    								idDigit1 = 1111'B
    								oddEvenInd = 0'B
    								typeOfId = 010'B
    								otherDigits = '00F110FE0041C2345678'O
    					PiggybackedPduList = Omit

    Inter-component message: SRB -> NR5GC_PTC:SRB

    timerEvent = 7
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\NR5GC\NR5GC_NASSteps.ttcn
    testName = TC_7_1_3_2_2_NR5GC
    lineNo = 1422
    outStr = Timer: t_T3540, Stopped: 10:22:50

    Timer: t_T3540, Stopped: 10:22:50

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		EnquireTiming = True

    Sent from port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 521
    				Subframe
    					Number = 4
    				HSFN
    					Number = 78
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		Result
    			Success = True
    	Confirm
    		EnquireTiming = True

    Received on port: NR5GC_PTC:SYS

    timerEvent = 6
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\NR5GC\NR5GC_RRCSteps.ttcn
    testName = TC_7_1_3_2_2_NR5GC
    lineNo = 281
    outStr = Timer: t_Timer, Duration: 1.22s, Started: 10:22:50

    Timer: t_Timer, Duration: 1.22s, Started: 10:22:50

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 551
    				Subframe
    					Number = 7
    				HSFN
    					Number = 78
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcRelease
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcRelease
    									redirectedCarrierInfo = Omit
    									cellReselectionPriorities = Omit
    									suspendConfig = Omit
    									deprioritisationReq = Omit
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: TC_SRB -> NASEMU_NRNG_PTC:TC_SRB

    DL-DCCH-Message
    	message = c1 = rrcRelease =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcRelease =

    rrcRelease

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 551
    				Subframe
    					Number = 7
    				HSFN
    					Number = 78
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcRelease
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcRelease
    								redirectedCarrierInfo = Omit
    								cellReselectionPriorities = Omit
    								suspendConfig = Omit
    								deprioritisationReq = Omit
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Sent from port: NASEMU_NRNG_PTC:SYS_SRB

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		PdcpCount
    			Get
    				AllRBs = True

    Sent from port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		PdcpCount
    			Get
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 1
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000011'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000011'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 2
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000100'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000011'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Drb = 2
    					UL
    						Format = PdcpCount_DrbSQN18 (2)
    						Value = 00000000000000000000000000000001'B
    					DL
    						Format = PdcpCount_DrbSQN18 (2)
    						Value = 00000000000000000000000000000001'B

    Received on port: NR5GC_PTC:SYS

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 551
    			Subframe
    				Number = 7
    			HSFN
    				Number = 78
    			Slot
    				SlotOffset
    					Numerology1 = 0
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		Now
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				SlotOffset
    					Numerology1

    Message Mismatch: TimingInfo_Type

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 551
    				Subframe
    					Number = 7
    				HSFN
    					Number = 78
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		Cell
    			AddOrReconfigure
    				StaticResourceConfig = Omit
    				CellConfigCommon = Omit
    				PhysicalLayer = Omit
    				BcchConfig = Omit
    				PcchConfig = Omit
    				RachProcedureConfig = Omit
    				CcchDcchDtchConfig
    					DL = Omit
    					UL
    						SearchSpaceAndDci
    							AssignedBWPs = Omit
    							SearchSpaceType = Omit
    							DciInfo = Omit
    						PUCCH_Synch
    							None = True
    						GrantConfig
    							None = True
    					DrxCtrl = Omit
    					MeasGapCtrl = Omit
    				ServingCellConfig = Omit

    Sent from port: NR5GC_PTC:SYS

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 552
    			Subframe
    				Number = 2
    			HSFN
    				Number = 78
    			Slot
    				SlotOffset
    					Numerology1 = 0
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		Now
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				SlotOffset
    					Numerology1

    Message Mismatch: TimingInfo_Type

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 552
    				Subframe
    					Number = 2
    				HSFN
    					Number = 78
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		AS_Security
    			Release = True

    Sent from port: NR5GC_PTC:SYS

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 557
    			Subframe
    				Number = 2
    			HSFN
    				Number = 78
    			Slot
    				SlotOffset
    					Numerology1 = 0
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		Now
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				SlotOffset
    					Numerology1

    Message Mismatch: TimingInfo_Type

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 557
    				Subframe
    					Number = 2
    				HSFN
    					Number = 78
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		RadioBearerList
    			NR_RadioBearer_Type
    				Id
    					Srb = 1
    				Config
    					Release = True
    			NR_RadioBearer_Type
    				Id
    					Srb = 2
    				Config
    					Release = True
    			NR_RadioBearer_Type
    				Id
    					Drb = 2
    				Config
    					Release = True

    Sent from port: NR5GC_PTC:SYS

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 557
    			Subframe
    				Number = 7
    			HSFN
    				Number = 78
    			Slot
    				SlotOffset
    					Numerology1 = 0
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		Now
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				SlotOffset
    					Numerology1

    Message Mismatch: TimingInfo_Type

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 557
    				Subframe
    					Number = 7
    				HSFN
    					Number = 78
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		RadioBearerList
    			NR_RadioBearer_Type
    				Id
    					Srb = 1
    				Config
    					AddOrReconfigure
    						Sdap
    							None = True
    						Pdcp
    							RBTerminating
    								RbConfig
    									Params
    										Rb
    											Srb = True
    								LinkToOtherCellGroup
    									None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										AM
    											Tx
    												R15
    													sn_FieldLength = size12 (0)
    													t_PollRetransmit = ms45 (8)
    													pollPDU = infinity_ (23)
    													pollByte = infinity_ (43)
    													maxRetxThreshold = t8 (5)
    											Rx
    												R15
    													sn_FieldLength = size12 (0)
    													t_Reassembly = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    									TestMode
    										None = True
    								LogicalChannelId = 1
    								Mac
    									LogicalChannel
    										Priority = 1
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit
    			NR_RadioBearer_Type
    				Id
    					Srb = 2
    				Config
    					AddOrReconfigure
    						Sdap
    							None = True
    						Pdcp
    							RBTerminating
    								RbConfig
    									Params
    										Rb
    											Srb = True
    								LinkToOtherCellGroup
    									None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										AM
    											Tx
    												R15
    													sn_FieldLength = size12 (0)
    													t_PollRetransmit = ms45 (8)
    													pollPDU = infinity_ (23)
    													pollByte = infinity_ (43)
    													maxRetxThreshold = t8 (5)
    											Rx
    												R15
    													sn_FieldLength = size12 (0)
    													t_Reassembly = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    									TestMode
    										None = True
    								LogicalChannelId = 2
    								Mac
    									LogicalChannel
    										Priority = 3
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit

    Sent from port: NR5GC_PTC:SYS

    timerEvent = 9
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\NR5GC\NR5GC_RRCSteps.ttcn
    testName = TC_7_1_3_2_2_NR5GC
    lineNo = 289
    outStr = Timer: t_Timer, Expired: 10:22:51

    Timer: t_Timer, Expired: 10:22:51

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		Cell
    			Release = True

    Sent from port: NR5GC_PTC:SYS

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		Cell
    			Release = True

    Sent from port: NR5GC_PTC:SYS

    recordType = 24
    summary = Postamble

    Postamble

    IntermediateVerdict = (Pass)
    summary = Intermediate verdict: (PASS)

    Intermediate verdict: (PASS)

    IntermediateVerdict = (Pass)
    summary = Intermediate verdict: (PASS)

    Intermediate verdict: (PASS)

    verdict = PASS
    summary = Test case ended: TC_7_1_3_2_2_NR5GC, Verdict: PASS

    Test case ended: TC_7_1_3_2_2_NR5GC, Verdict: PASS

    IntermediateVerdict = (None)
    summary = Intermediate verdict: (NONE)

    Intermediate verdict: (NONE)

    IntermediateVerdict = (None)
    summary = Intermediate verdict: (NONE)

    Intermediate verdict: (NONE)

    IntermediateVerdict = (None)
    summary = Intermediate verdict: (NONE)

    Intermediate verdict: (NONE)

    IntermediateVerdict = (None)
    summary = Intermediate verdict: (NONE)

    Intermediate verdict: (NONE)

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 148
    text = Unmapping port "MTC_NR5GC:Ut" from port "SYSTEM_NR5GC:Ut"

    Unmapping port "MTC_NR5GC:Ut" from port "SYSTEM_NR5GC:Ut"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 148
    text = Unmapping port "NR5GC_PTC:SYS" from port "SYSTEM_NR5GC:NR_SYS"

    Unmapping port "NR5GC_PTC:SYS" from port "SYSTEM_NR5GC:NR_SYS"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 148
    text = Unmapping port "NR5GC_PTC:SYSIND" from port "SYSTEM_NR5GC:NR_SYSIND"

    Unmapping port "NR5GC_PTC:SYSIND" from port "SYSTEM_NR5GC:NR_SYSIND"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 148
    text = Unmapping port "NR5GC_PTC:DRB" from port "SYSTEM_NR5GC:NR_DRB"

    Unmapping port "NR5GC_PTC:DRB" from port "SYSTEM_NR5GC:NR_DRB"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 148
    text = Unmapping port "NASEMU_NRNG_PTC:SYS_SRB" from port "SYSTEM_NR5GC:NR_SRB"

    Unmapping port "NASEMU_NRNG_PTC:SYS_SRB" from port "SYSTEM_NR5GC:NR_SRB"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 148
    text = Unmapping port "IP_PTC:IP_CTRL" from port "SYSTEM_NR5GC:IP_CTRL"

    Unmapping port "IP_PTC:IP_CTRL" from port "SYSTEM_NR5GC:IP_CTRL"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 148
    text = Unmapping port "IPMUX_PTC:IP_SOCK" from port "SYSTEM_NR5GC:IP_SOCK"

    Unmapping port "IPMUX_PTC:IP_SOCK" from port "SYSTEM_NR5GC:IP_SOCK"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 148
    text = Unmapping port "IP_PTC:IPSEC_CTRL" from port "SYSTEM_NR5GC:IPSEC_CTRL"

    Unmapping port "IP_PTC:IPSEC_CTRL" from port "SYSTEM_NR5GC:IPSEC_CTRL"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 148
    text = Disconnecting port "MTC_NR5GC:PTC_Ut" from port "IMS_PTC:MMI"

    Disconnecting port "MTC_NR5GC:PTC_Ut" from port "IMS_PTC:MMI"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 148
    text = Disconnecting port "MTC_NR5GC:PTC_Ut" from port "NR5GC_PTC:UT"

    Disconnecting port "MTC_NR5GC:PTC_Ut" from port "NR5GC_PTC:UT"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 148
    text = Disconnecting port "NR5GC_PTC:NASCTRL" from port "NASEMU_NRNG_PTC:CTRL"

    Disconnecting port "NR5GC_PTC:NASCTRL" from port "NASEMU_NRNG_PTC:CTRL"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 148
    text = Disconnecting port "NR5GC_PTC:SRB" from port "NASEMU_NRNG_PTC:TC_SRB"

    Disconnecting port "NR5GC_PTC:SRB" from port "NASEMU_NRNG_PTC:TC_SRB"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 148
    text = Disconnecting port "NR5GC_PTC:IMS" from port "IMS_PTC:IPCAN"

    Disconnecting port "NR5GC_PTC:IMS" from port "IMS_PTC:IPCAN"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 148
    text = Disconnecting port "NR5GC_PTC:IP" from port "IP_PTC:NR_CTRL"

    Disconnecting port "NR5GC_PTC:IP" from port "IP_PTC:NR_CTRL"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 148
    text = Disconnecting port "IP_PTC:IP_SOCK_DATA" from port "IPMUX_PTC:IP_SOCK_DATA"

    Disconnecting port "IP_PTC:IP_SOCK_DATA" from port "IPMUX_PTC:IP_SOCK_DATA"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 148
    text = Disconnecting port "IP_PTC:IP_SOCK_CTRL" from port "IPMUX_PTC:IP_SOCK_CTRL"

    Disconnecting port "IP_PTC:IP_SOCK_CTRL" from port "IPMUX_PTC:IP_SOCK_CTRL"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 148
    text = Disconnecting port "IP_PTC:IMS_CTRL" from port "IMS_PTC:IMS_CTRL"

    Disconnecting port "IP_PTC:IMS_CTRL" from port "IMS_PTC:IMS_CTRL"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 148
    text = Disconnecting port "IP_PTC:IMS_Client" from port "IMS_PTC:IMS_Client"

    Disconnecting port "IP_PTC:IMS_Client" from port "IMS_PTC:IMS_Client"

    recordType = 24
    fileName = C:\SourceCode\PCT_LJ\_TTCN\IWD_19wk38\IWD_19wk38_5G\NR5GC_IWD_19wk38\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 148
    text = Disconnecting port "IP_PTC:IMS_Server" from port "IMS_PTC:IMS_Server"

    Disconnecting port "IP_PTC:IMS_Server" from port "IMS_PTC:IMS_Server"

    recordType = 24
    fileName
    descriptionId = TC_7_1_3_2_2_NR5GC
    lineNo = 0
    text = Test Procedure: Final Verdict

    Test Procedure: Final Verdict

    recordType = 24
    summary = Final Verdict

    Final Verdict

    verdict = PASS
    summary = TEST CASE ENDED: TC_7_1_3_2_2_NR5GC

    TEST CASE ENDED: TC_7_1_3_2_2_NR5GC