MSG #72 2021-06-22 12:24:49.282
RRC

     DCCH: RRC Connection Reconfiguration
    {
      message c1: rrcConnectionReconfiguration: {
        rrc-TransactionIdentifier 0,
        criticalExtensions c1: rrcConnectionReconfiguration-r8: {
          dedicatedInfoNASList {
            '27522AF44702623FDD9AFDAF7FF79DCFA60D5A331AB2AA678F76808F9A4ABA47F42BA74B97213FFC65E56E167C127D03A17ABC2041F7DFB2DCB8E60EA1F9E8D7D36F967B7326CA3C948114890BD035A4B5FDB9D57BCA4A44E9DC0239B74D93EB8963CE89A1BBAD5A8FE693EE387B5752FC365A13E726E806E7EA92F0C1676A09E6C40D43855E717D'H
          },
          radioResourceConfigDedicated {
            srb-ToAddModList {
              {
                srb-Identity 2,
                rlc-Config explicitValue: am: {
                  ul-AM-RLC {
                    t-PollRetransmit ms60,
                    pollPDU pInfinity,
                    pollByte kBinfinity,
                    maxRetxThreshold t32
                  },
                  dl-AM-RLC {
                    t-Reordering ms45,
                    t-StatusProhibit ms0
                  }
                },
                logicalChannelConfig defaultValue: NULL
              }
            },
            drb-ToAddModList {
              {
                eps-BearerIdentity 5,
                drb-Identity 1,
                pdcp-Config {
                  discardTimer infinity,
                  rlc-AM {
                    statusReportRequired TRUE
                  },
                  headerCompression notUsed: NULL
                },
                rlc-Config am: {
                  ul-AM-RLC {
                    t-PollRetransmit ms80,
                    pollPDU p128,
                    pollByte kB125,
                    maxRetxThreshold t4
                  },
                  dl-AM-RLC {
                    t-Reordering ms80,
                    t-StatusProhibit ms60
                  }
                },
                logicalChannelIdentity 3,
                logicalChannelConfig {
                  ul-SpecificParameters {
                    priority 4,
                    prioritisedBitRate kBps8,
                    bucketSizeDuration ms100,
                    logicalChannelGroup 1
                  }
                }
              }
            },
            physicalConfigDedicated {
              cqi-ReportConfig {
                nomPDSCH-RS-EPRE-Offset 0,
                cqi-ReportPeriodic setup: {
                  cqi-PUCCH-ResourceIndex 0,
                  cqi-pmi-ConfigIndex 38,
                  cqi-FormatIndicatorPeriodic widebandCQI: NULL,
                  simultaneousAckNackAndCQI TRUE
                }
              }
            }
          }
        }
      }
    }