MSG #834 2021-06-22 12:27:11.912

NAS

     Message too short (len=9)
    0000:  27 12 1e fb e0 09 47 1b  1f                       '.....G..
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x2 (Integrity protected and ciphered)
    Auth code = 0x121efbe0
    Sequence number = 0x09
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x4 (Integrity protected and ciphered with new EPS security context)
    Message too short (len=9)
    0000:  27 12 1e fb e0 09 47 1b  1f                       '.....G..