ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 12:23:48.654 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 12:23:48.658 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 12:23:48.659 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 12:23:48.662 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 12:23:48.663 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 12:23:48.663 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:801: IMS UDP port 192.168.2.3:5060 configured
7 | 12:23:48.666 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:751: IMS TCP port 192.168.2.3:5060 configured!
8 | 12:23:48.669 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:772: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 12:23:48.670 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:783: IdM port 192.168.2.3:8080 configured!
10 | 12:23:48.674 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 12:23:49.875 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 12:23:49.875 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 12:23:53.984 |  | ←RRC BCCH SIB1 |  |  |
14 | 12:23:54.060 |  | ←RRC BCCH SIB |  |  |
15 | 12:23:54.065 |  | ←RRC BCCH SIB1 |  |  |
16 | 12:23:54.144 |  | ←RRC BCCH SIB1 |  |  |
17 | 12:23:54.219 |  | ←RRC BCCH SIB |  |  |
18 | 12:24:48.989 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 12:24:48.989 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 12:24:48.989 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 12:24:48.989 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 12:24:49.040 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 12:24:49.040 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 12:24:49.040 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 12:24:49.040 |  |  |  | →NAS EMM Attach request |  |
26 | 12:24:49.040 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 12:24:49.040 |  |  |  | NAS K-asme ca773e4954bb361f93d16d62e02d0b44... |  |
28 | 12:24:49.040 |  |  |  | NAS ← EMM Authentication request |  |
29 | 12:24:49.041 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 12:24:49.041 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 12:24:49.041 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 12:24:49.112 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 12:24:49.112 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 12:24:49.112 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 12:24:49.112 |  |  |  | →NAS EMM Authentication response |  |
36 | 12:24:49.112 |  |  |  | NAS UE auth OK |  |
37 | 12:24:49.112 |  |  |  | NAS K-nas-cip e368d897196198883e0a28320bd8e... |  |
38 | 12:24:49.112 |  |  |  | NAS K-nas-int df765a72c70910b5a4904e3575cce... |  |
39 | 12:24:49.112 |  |  |  | NAS ← EMM Security mode command |  |
40 | 12:24:49.112 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 12:24:49.112 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 12:24:49.113 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 12:24:49.152 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
44 | 12:24:49.152 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 12:24:49.152 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xd) |  |  |
46 | 12:24:49.152 |  |  |  | →NAS EMM Security mode complete |  |
47 | 12:24:49.152 |  |  |  | NAS ← ESM ESM information request |  |
48 | 12:24:49.153 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x5) |  |  |
49 | 12:24:49.153 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 12:24:49.154 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
51 | 12:24:49.161 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
52 | 12:24:49.200 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
53 | 12:24:49.200 |  | →RRC DCCH UL Information Transfer |  |  |
54 | 12:24:49.200 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x8) |  |  |
55 | 12:24:49.200 |  |  |  | →NAS ESM ESM information response |  |
56 | 12:24:49.200 |  |  |  | NAS ← EMM Attach accept |  |
57 | 12:24:49.200 |  |  |  | NAS K-enb 95a0a613080597b9b71a61461bee747be... |  |
58 | 12:24:49.201 |  | ←RRC DCCH Security Mode Command |  |  |
59 | 12:24:49.201 |  |  | RRC K-enb 95a0a613080597b9b71a61461bee747be... |  |  |
60 | 12:24:49.201 |  |  | RRC rrc-cip 301a3380b235e0eee0534308fd43740... |  |  |
61 | 12:24:49.201 |  |  | RRC rrc-int 3b496269e1d513551b07daffcc08f6c... |  |  |
62 | 12:24:49.201 |  |  | RRC up-cip 8c01e780a609586fc6b92f373e939805... |  |  |
63 | 12:24:49.201 |  |  | RRC up-int b2a6143d4197d132b239d5444f61e8af... |  |  |
64 | 12:24:49.202 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
65 | 12:24:49.232 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
66 | 12:24:49.232 |  | →RRC DCCH Security Mode Complete |  |  |
67 | 12:24:49.232 |  | ←RRC DCCH UE Capability Enquiry |  |  |
68 | 12:24:49.232 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
69 | 12:24:49.281 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
70 | 12:24:49.281 |  | →RRC DCCH UE Capability Information |  |  |
71 | 12:24:49.282 |  | [EMBEDDED NAS IN NEXT RRC] ESM Unknown message (type=0xdd) |  |  |
72 | 12:24:49.282 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
73 | 12:24:49.282 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration |  |  |
74 | 12:24:49.312 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
75 | 12:24:49.312 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
76 | 12:24:49.351 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
77 | 12:24:49.351 |  | →RRC DCCH UL Information Transfer |  |  |
78 | 12:24:49.351 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x9) |  |  |
79 | 12:24:49.352 |  |  |  | →NAS EMM Attach complete |  |
80 | 12:24:49.352 |  |  |  | NAS ← EMM EMM information |  |
81 | 12:24:49.353 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x3) |  |  |
82 | 12:24:49.353 |  | ←RRC DCCH DL Information Transfer |  |  |
83 | 12:24:49.354 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
84 | 12:24:52.116 |  | ←RRC DCCH RRC Connection Release |  |  |
85 | 12:24:52.117 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
86 | 12:24:55.299 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
87 | 12:24:55.299 |  | →RRC CCCH RRC Connection Request |  |  |
88 | 12:24:55.299 |  | ←RRC CCCH RRC Connection Setup |  |  |
89 | 12:24:55.299 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
90 | 12:24:55.352 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
91 | 12:24:55.352 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
92 | 12:24:55.352 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
93 | 12:24:55.352 |  |  |  | →NAS EMM Service request |  |
94 | 12:24:55.352 |  |  |  | NAS K-enb 9f2df9e51bb3464a4777e7edd574c3fea... |  |
95 | 12:24:55.353 |  | ←RRC DCCH Security Mode Command |  |  |
96 | 12:24:55.353 |  |  | RRC K-enb 9f2df9e51bb3464a4777e7edd574c3fea... |  |  |
97 | 12:24:55.353 |  |  | RRC rrc-cip 3aee3487cb715decf0fa38c193574a6... |  |  |
98 | 12:24:55.353 |  |  | RRC rrc-int e9a7dceaeaaf2d7ad918fa93ce98095... |  |  |
99 | 12:24:55.353 |  |  | RRC up-cip b9babf6798ca1dfd236ebc6fe7cb25bf... |  |  |
100 | 12:24:55.353 |  |  | RRC up-int 6308ea6587b35b3922d860389980782e... |  |  |
101 | 12:24:55.354 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
102 | 12:24:55.392 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
103 | 12:24:55.392 |  | →RRC DCCH Security Mode Complete |  |  |
104 | 12:24:55.392 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
105 | 12:24:55.392 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
106 | 12:24:55.432 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] ... |  |  |  |
107 | 12:24:55.432 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
108 | 12:25:12.752 | →enobeB PCAP frame→ TCP |  |  |  |
109 | 12:25:12.756 |  | ←enobeB PCAP frame← TCP |  |  |
110 | 12:25:12.792 | →enobeB PCAP frame→ TCP |  |  |  |
111 | 12:25:12.840 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
112 | 12:25:12.844 |  | ←enobeB PCAP frame← TCP |  |  |
113 | 12:25:12.849 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
114 | 12:25:12.872 | →enobeB PCAP frame→ TCP |  |  |  |
115 | 12:25:12.999 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
116 | 12:25:13.003 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:632: Client connected to Http Proxy port (id 17)
117 | 12:25:13.004 |  | ←enobeB PCAP frame← TCP |  |  |
118 | 12:25:13.005 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
119 | 12:25:13.032 | →enobeB PCAP frame→ TCP |  |  |  |
120 | 12:25:13.039 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
121 | 12:25:13.042 |  | ←enobeB PCAP frame← TCP |  |  |
122 | 12:25:13.042 |  |  |  |  | →HTTP GET | HTTP-Proxy
123 | 12:25:13.049 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:288: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
124 | 12:25:13.070 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
125 | 12:25:13.074 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
126 | 12:25:13.075 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
127 | 12:25:13.112 | →enobeB PCAP frame→ DNS |  |  |  |
128 | 12:25:13.152 | →enobeB PCAP frame→ TCP |  |  |  |
129 | 12:25:14.951 | →enobeB PCAP frame→ TCP |  |  |  |
130 | 12:25:14.954 |  | ←enobeB PCAP frame← TCP |  |  |
131 | 12:25:14.992 | →enobeB PCAP frame→ TCP |  |  |  |
132 | 12:25:15.000 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
133 | 12:25:15.003 |  | ←enobeB PCAP frame← TCP |  |  |
134 | 12:25:15.009 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
135 | 12:25:15.031 | →enobeB PCAP frame→ TCP |  |  |  |
136 | 12:25:15.279 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
137 | 12:25:15.283 |  | ←enobeB PCAP frame← TCP |  |  |
138 | 12:25:15.284 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:638: Client connected to IdM port (id 19)
139 | 12:25:15.285 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
140 | 12:25:15.312 | →enobeB PCAP frame→ TCP |  |  |  |
141 | 12:25:15.320 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
142 | 12:25:15.322 |  | ←enobeB PCAP frame← TCP |  |  |
143 | 12:25:15.323 |  |  |  |  | →HTTP GET | IDMS-Endpoint
144 | 12:25:15.324 |  | ←enobeB PCAP frame← TCP |  |  |
145 | 12:25:15.342 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
146 | 12:25:15.345 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
147 | 12:25:15.346 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:511: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
148 | 12:25:15.347 |  |  |  |  | MMICmd: Please provide user credentials: username and password
149 | 12:25:15.432 | →enobeB PCAP frame→ TCP |  |  |  |
150 | 12:25:21.760 | →enobeB PCAP frame→ HTTPS: POST /idms/userauth HTTP/1.1 |  |  |  |
151 | 12:25:21.764 |  | ←enobeB PCAP frame← TCP |  |  |
152 | 12:25:21.765 |  |  |  |  | →HTTP POST | IDMS-Endpoint
153 | 12:25:21.781 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
154 | 12:25:21.784 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
155 | 12:25:21.784 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:516: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
156 | 12:25:21.832 | →enobeB PCAP frame→ TCP |  |  |  |
157 | 12:25:21.840 | →enobeB PCAP frame→ TCP |  |  |  |
158 | 12:25:21.842 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:673: IdM port - Client closed the connection (id 19)
159 | 12:25:21.844 |  | ←enobeB PCAP frame← TCP |  |  |
160 | 12:25:21.871 | →enobeB PCAP frame→ TCP |  |  |  |
161 | 12:25:22.671 | →enobeB PCAP frame→ TCP |  |  |  |
162 | 12:25:22.676 |  | ←enobeB PCAP frame← TCP |  |  |
163 | 12:25:22.712 | →enobeB PCAP frame→ TCP |  |  |  |
164 | 12:25:22.720 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
165 | 12:25:22.724 |  | ←enobeB PCAP frame← TCP |  |  |
166 | 12:25:22.725 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
167 | 12:25:22.751 | →enobeB PCAP frame→ TCP |  |  |  |
168 | 12:25:22.840 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
169 | 12:25:22.843 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:638: Client connected to IdM port (id 19)
170 | 12:25:22.844 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
171 | 12:25:22.872 | →enobeB PCAP frame→ TCP |  |  |  |
172 | 12:25:22.880 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
173 | 12:25:22.883 |  |  |  |  | →HTTP POST | IDMS-Endpoint
174 | 12:25:22.884 |  | ←enobeB PCAP frame← TCP |  |  |
175 | 12:25:22.923 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
176 | 12:25:22.924 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:521: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
177 | 12:25:22.926 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
178 | 12:25:22.992 | →enobeB PCAP frame→ TCP |  |  |  |
179 | 12:25:23.272 | →enobeB PCAP frame→ TCP |  |  |  |
180 | 12:25:23.276 |  | ←enobeB PCAP frame← TCP |  |  |
181 | 12:25:23.311 | →enobeB PCAP frame→ TCP |  |  |  |
182 | 12:25:23.320 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
183 | 12:25:23.324 |  | ←enobeB PCAP frame← TCP |  |  |
184 | 12:25:23.327 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
185 | 12:25:23.352 | →enobeB PCAP frame→ TCP |  |  |  |
186 | 12:25:23.399 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
187 | 12:25:23.403 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:632: Client connected to Http Proxy port (id 20)
188 | 12:25:23.404 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
189 | 12:25:23.440 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
190 | 12:25:23.443 |  | ←enobeB PCAP frame← TCP |  |  |
191 | 12:25:23.444 |  |  |  |  | →HTTP POST | HTTP-Proxy
192 | 12:25:23.468 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:541: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
193 | 12:25:23.475 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
194 | 12:25:23.478 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
195 | 12:25:23.512 | →enobeB PCAP frame→ TCP |  |  |  |
196 | 12:25:23.552 | →enobeB PCAP frame→ TCP |  |  |  |
197 | 12:25:23.556 |  | ←enobeB PCAP frame← TCP |  |  |
198 | 12:25:23.592 | →enobeB PCAP frame→ TCP |  |  |  |
199 | 12:25:23.600 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
200 | 12:25:23.604 |  | ←enobeB PCAP frame← TCP |  |  |
201 | 12:25:23.607 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
202 | 12:25:23.631 | →enobeB PCAP frame→ TCP |  |  |  |
203 | 12:25:23.639 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
204 | 12:25:23.642 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:632: Client connected to Http Proxy port (id 21)
205 | 12:25:23.643 |  | ←enobeB PCAP frame← TCP |  |  |
206 | 12:25:23.644 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
207 | 12:25:23.680 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
208 | 12:25:23.684 |  | ←enobeB PCAP frame← TCP |  |  |
209 | 12:25:23.684 |  |  |  |  | →HTTP POST | HTTP-Proxy
210 | 12:25:23.746 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
211 | 12:25:23.746 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:545: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
212 | 12:25:23.749 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
213 | 12:25:23.749 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
214 | 12:25:23.792 | →enobeB PCAP frame→ TCP |  |  |  |
215 | 12:25:23.832 | →enobeB PCAP frame→ TCP |  |  |  |
216 | 12:25:23.839 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
217 | 12:25:23.844 |  |  |  |  | →SIP REGISTER | P-CSCF
218 | 12:25:23.867 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:810: IMS UDP_s port 192.168.2.3:5062 configured
219 | 12:25:23.896 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:761: IMS TCP_s port 192.168.2.3:5062 configured!
220 | 12:25:23.898 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:819: IMS UDP_c port 192.168.2.3:5061 configured
221 | 12:25:23.905 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
222 | 12:25:23.907 |  | ←enobeB PCAP frame← SIP -cleartext-: SIP/2.0 401 Unauthorized |  |  |
223 | 12:25:24.760 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
224 | 12:25:24.834 |  |  |  |  | →SIP REGISTER | P-CSCF
225 | 12:25:24.858 |  |  |  |  | ←SIP 200 OK | P-CSCF
226 | 12:25:24.861 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
227 | 12:25:25.240 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
228 | 12:25:25.241 | →enobeB PCAP frame→ SIP over IPSEC: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 |  |  |  |
229 | 12:25:25.255 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
230 | 12:25:25.315 |  |  |  |  | ←SIP 200 OK | P-CSCF
231 | 12:25:25.315 |  |  |  |  | MIKEY | Media-Server
232 | 12:25:25.316 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
233 | 12:25:25.536 |  |  |  |  | XML→ | Media-Server
234 | 12:25:25.537 |  |  |  |  | XML→ | Media-Server
235 | 12:25:25.540 |  |  |  |  | ←XML | Media-Server
236 | 12:25:25.543 |  |  |  |  | ←SIP NOTIFY | P-CSCF
237 | 12:25:25.547 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:43509;transp... |  |  |
238 | 12:25:25.600 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
239 | 12:25:25.602 |  |  |  |  | →SIP 200 OK | P-CSCF
240 | 12:25:25.911 | →enobeB PCAP frame→ TCP |  |  |  |
241 | 12:25:25.915 |  | ←enobeB PCAP frame← TCP |  |  |
242 | 12:25:25.951 | →enobeB PCAP frame→ TCP |  |  |  |
243 | 12:25:25.960 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
244 | 12:25:25.964 |  | ←enobeB PCAP frame← TCP |  |  |
245 | 12:25:25.966 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
246 | 12:25:25.992 | →enobeB PCAP frame→ TCP |  |  |  |
247 | 12:25:26.040 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
248 | 12:25:26.043 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:632: Client connected to Http Proxy port (id 26)
249 | 12:25:26.044 |  | ←enobeB PCAP frame← TCP |  |  |
250 | 12:25:26.045 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
251 | 12:25:26.120 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-co... |  |  |  |
252 | 12:25:26.123 |  |  |  |  | →HTTP GET | HTTP-Proxy
253 | 12:25:26.124 |  | ←enobeB PCAP frame← TCP |  |  |
254 | 12:25:26.132 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:642: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcptt-ue-configuration.xml
255 | 12:25:26.140 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
256 | 12:25:26.143 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
257 | 12:25:26.192 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
258 | 12:25:26.194 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:668: Http Proxy port - Client closed the connection (id 26)
259 | 12:25:26.196 |  | ←enobeB PCAP frame← TCP |  |  |
260 | 12:25:26.200 | →enobeB PCAP frame→ TCP |  |  |  |
261 | 12:25:26.202 |  | ←enobeB PCAP frame← TCP |  |  |
262 | 12:25:26.231 | →enobeB PCAP frame→ TCP |  |  |  |
263 | 12:25:26.352 | →enobeB PCAP frame→ TCP |  |  |  |
264 | 12:25:26.356 |  | ←enobeB PCAP frame← TCP |  |  |
265 | 12:25:26.392 | →enobeB PCAP frame→ TCP |  |  |  |
266 | 12:25:26.400 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
267 | 12:25:26.404 |  | ←enobeB PCAP frame← TCP |  |  |
268 | 12:25:26.406 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
269 | 12:25:26.432 | →enobeB PCAP frame→ TCP |  |  |  |
270 | 12:25:26.520 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
271 | 12:25:26.523 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:632: Client connected to Http Proxy port (id 26)
272 | 12:25:26.524 |  | ←enobeB PCAP frame← TCP |  |  |
273 | 12:25:26.525 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
274 | 12:25:26.551 | →enobeB PCAP frame→ TCP |  |  |  |
275 | 12:25:26.560 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-... |  |  |  |
276 | 12:25:26.563 |  |  |  |  | →HTTP GET | HTTP-Proxy
277 | 12:25:26.564 |  | ←enobeB PCAP frame← TCP |  |  |
278 | 12:25:26.571 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:647: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcptt-user-profile-49.xml
279 | 12:25:26.601 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
280 | 12:25:26.608 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
281 | 12:25:26.609 |  | ←enobeB PCAP frame← TCP |  |  |
282 | 12:25:26.609 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
283 | 12:25:26.632 | →enobeB PCAP frame→ TCP |  |  |  |
284 | 12:25:26.640 | →enobeB PCAP frame→ TCP |  |  |  |
285 | 12:25:26.648 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
286 | 12:25:26.650 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:668: Http Proxy port - Client closed the connection (id 26)
287 | 12:25:26.652 |  | ←enobeB PCAP frame← TCP |  |  |
288 | 12:25:26.672 | →enobeB PCAP frame→ TCP |  |  |  |
289 | 12:25:27.280 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
290 | 12:25:27.281 | →enobeB PCAP frame→ SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
291 | 12:25:27.299 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
292 | 12:25:27.317 |  |  |  |  | MIKEY | Media-Server
293 | 12:25:27.317 |  |  |  |  | ←SIP 200 OK | P-CSCF
294 | 12:25:27.319 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
295 | 12:25:27.391 | →enobeB PCAP frame→ TCP |  |  |  |
296 | 12:25:27.395 |  | ←enobeB PCAP frame← TCP |  |  |
297 | 12:25:27.432 | →enobeB PCAP frame→ TCP |  |  |  |
298 | 12:25:27.440 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
299 | 12:25:27.443 |  | ←enobeB PCAP frame← TCP |  |  |
300 | 12:25:27.443 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
301 | 12:25:27.471 | →enobeB PCAP frame→ TCP |  |  |  |
302 | 12:25:27.520 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
303 | 12:25:27.522 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:632: Client connected to Http Proxy port (id 26)
304 | 12:25:27.523 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
305 | 12:25:27.531 |  |  |  |  | XML→ | Media-Server
306 | 12:25:27.532 |  |  |  |  | XML→ | Media-Server
307 | 12:25:27.535 |  |  |  |  | ←XML | Media-Server
308 | 12:25:27.538 |  |  |  |  | ←SIP NOTIFY | P-CSCF
309 | 12:25:27.539 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:43509;transp... |  |  |
310 | 12:25:27.600 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.servi... |  |  |  |
311 | 12:25:27.602 |  | ←enobeB PCAP frame← TCP |  |  |
312 | 12:25:27.602 |  |  |  |  | →SIP 200 OK | P-CSCF
313 | 12:25:27.602 |  |  |  |  | →HTTP GET | HTTP-Proxy
314 | 12:25:27.607 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:652: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
315 | 12:25:27.619 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
316 | 12:25:27.624 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
317 | 12:25:27.625 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
318 | 12:25:27.672 | →enobeB PCAP frame→ TCP |  |  |  |
319 | 12:25:27.680 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
320 | 12:25:27.682 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:668: Http Proxy port - Client closed the connection (id 26)
321 | 12:25:27.684 |  | ←enobeB PCAP frame← TCP |  |  |
322 | 12:25:27.711 | →enobeB PCAP frame→ TCP |  |  |  |
323 | 12:25:27.751 | →enobeB PCAP frame→ TCP |  |  |  |
324 | 12:25:27.754 |  | ←enobeB PCAP frame← TCP |  |  |
325 | 12:25:27.791 | →enobeB PCAP frame→ TCP |  |  |  |
326 | 12:25:27.800 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
327 | 12:25:27.803 |  | ←enobeB PCAP frame← TCP |  |  |
328 | 12:25:27.806 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
329 | 12:25:27.832 | →enobeB PCAP frame→ TCP |  |  |  |
330 | 12:25:27.880 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
331 | 12:25:27.882 |  | ←enobeB PCAP frame← TCP |  |  |
332 | 12:25:27.882 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:632: Client connected to Http Proxy port (id 26)
333 | 12:25:27.884 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
334 | 12:25:27.911 | →enobeB PCAP frame→ TCP |  |  |  |
335 | 12:25:27.920 | →enobeB PCAP frame→ HTTPS: GET /xcap.gms.mcstaasting.com/org.openmobileallian... |  |  |  |
336 | 12:25:27.922 |  | ←enobeB PCAP frame← TCP |  |  |
337 | 12:25:27.923 |  |  |  |  | →HTTP GET | HTTP-Proxy
338 | 12:25:27.935 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:657: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at /xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
339 | 12:25:27.956 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
340 | 12:25:27.960 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
341 | 12:25:27.962 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
342 | 12:25:27.992 | →enobeB PCAP frame→ TCP |  |  |  |
343 | 12:25:28.000 | →enobeB PCAP frame→ TCP |  |  |  |
344 | 12:25:28.007 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
345 | 12:25:28.010 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:668: Http Proxy port - Client closed the connection (id 26)
346 | 12:25:28.011 |  | ←enobeB PCAP frame← TCP |  |  |
347 | 12:25:28.015 | →enobeB PCAP frame→ TCP |  |  |  |
348 | 12:25:28.018 |  | ←enobeB PCAP frame← TCP |  |  |
349 | 12:25:28.031 | →enobeB PCAP frame→ TCP |  |  |  |
350 | 12:25:28.160 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
351 | 12:25:28.161 | →enobeB PCAP frame→ SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
352 | 12:25:28.175 |  |  |  |  | →SIP PUBLISH | P-CSCF
353 | 12:25:28.222 |  |  |  |  | MIKEY | Media-Server
354 | 12:25:28.280 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
355 | 12:25:28.281 | →enobeB PCAP frame→ SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
356 | 12:25:28.285 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
357 | 12:25:28.449 |  |  |  |  | XML→ | Media-Server
358 | 12:25:28.452 |  |  |  |  | ←SIP 200 OK | P-CSCF
359 | 12:25:28.454 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
360 | 12:25:28.455 |  |  |  |  | ←SIP 200 OK | P-CSCF
361 | 12:25:28.455 |  |  |  |  | MIKEY | Media-Server
362 | 12:25:28.458 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
363 | 12:25:28.665 |  |  |  |  | XML→ | Media-Server
364 | 12:25:28.666 |  |  |  |  | XML→ | Media-Server
365 | 12:25:28.701 |  |  |  |  | ←XML | Media-Server
366 | 12:25:28.705 |  |  |  |  | ←SIP NOTIFY | P-CSCF
367 | 12:25:28.709 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:43509;transp... |  |  |
368 | 12:25:28.760 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
369 | 12:25:28.762 |  |  |  |  | →SIP 200 OK | P-CSCF
370 | 12:25:28.766 |  |  |  |  | ←XML | Media-Server
371 | 12:25:28.777 |  |  |  |  | ←SIP MESSAGE | P-CSCF
372 | 12:25:28.781 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
373 | 12:25:28.781 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
374 | 12:25:29.560 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
375 | 12:25:29.562 |  |  |  |  | →SIP 200 OK | P-CSCF
376 | 12:25:29.566 |  |  |  |  | Info: MCX_IMS_CommonProcedures.ttcn:155: MESSAGE/200OK Table 5.3.2.3-2 Steps 7-8 Done
377 | 12:25:29.569 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
378 | 12:25:29.591 | →enobeB PCAP frame→ TCP |  |  |  |
379 | 12:25:29.632 | →enobeB PCAP frame→ TCP |  |  |  |
380 | 12:25:31.568 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
381 | 12:25:31.605 |  | ←RRC DCCH RRC Connection Release |  |  |
382 | 12:25:31.605 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
383 | 12:25:31.626 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
384 | 12:25:31.628 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
385 | 12:25:31.628 |  |  |  |  | MMICmd: Make the MCPTT User request the establishment of an MCPTT on-demand pre-arranged group call using Group A, automatic commencement mode, with implicit floor control
386 | 12:25:34.649 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
387 | 12:25:34.649 |  | →RRC CCCH RRC Connection Request |  |  |
388 | 12:25:34.649 |  | ←RRC CCCH RRC Connection Setup |  |  |
389 | 12:25:34.649 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
390 | 12:25:34.672 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
391 | 12:25:34.672 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
392 | 12:25:34.672 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
393 | 12:25:34.672 |  |  |  | →NAS EMM Service request |  |
394 | 12:25:34.672 |  |  |  | NAS K-enb 4b8f80876b37ffe2310f63360c828f85f... |  |
395 | 12:25:34.673 |  | ←RRC DCCH Security Mode Command |  |  |
396 | 12:25:34.673 |  |  | RRC K-enb 4b8f80876b37ffe2310f63360c828f85f... |  |  |
397 | 12:25:34.673 |  |  | RRC rrc-cip 37536014e237556790e4239ccc9b43f... |  |  |
398 | 12:25:34.673 |  |  | RRC rrc-int 4b5f58d990f2accde2b83a6d214b031... |  |  |
399 | 12:25:34.673 |  |  | RRC up-cip 2173107500a308ef4216f7632772269d... |  |  |
400 | 12:25:34.673 |  |  | RRC up-int d6a27a09e34ed7163577d9f1034082af... |  |  |
401 | 12:25:34.674 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
402 | 12:25:34.712 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
403 | 12:25:34.712 |  | →RRC DCCH Security Mode Complete |  |  |
404 | 12:25:34.712 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
405 | 12:25:34.712 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
406 | 12:25:34.752 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
407 | 12:25:34.752 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
408 | 12:25:34.760 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
409 | 12:25:34.761 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
410 | 12:25:34.770 |  |  |  |  | →SIP INVITE | P-CSCF
411 | 12:25:34.814 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:731: SRTP config: Master Key: D87B9960A497882FD4A27700712198D0, Master Salt: 6AD6E57573DAE6505F0FB11A, MKI: 2CF7F71A
412 | 12:25:34.814 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
413 | 12:25:34.820 |  |  |  |  | XML→ | Media-Server
414 | 12:25:34.822 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
415 | 12:25:34.823 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1102: INVITE Verdict: Pass
416 | 12:25:34.824 |  |  |  |  | ←SIP 100 Trying | P-CSCF
417 | 12:25:34.827 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
418 | 12:25:34.827 |  |  |  |  | ←SIP 200 OK | P-CSCF
419 | 12:25:34.832 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
420 | 12:25:34.832 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x0) |  |  |
421 | 12:25:34.832 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
422 | 12:25:34.833 |  | ←enobeB PCAP frame← SIP/SDP/NAS-EPS RRCConnectionReconfiguration Ciphered message [1050-bytes] Activate dedicated EPS bearer context request SIP over IPSEC: SIP/2.0 200 OK |  |  |
423 | 12:25:34.872 | →enobeB PCAP frame→ RLC-LTE/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
424 | 12:25:34.872 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
425 | 12:25:34.872 |  | →RRC DCCH UL Information Transfer |  |  |
426 | 12:25:34.872 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x5) |  |  |
427 | 12:25:34.872 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
428 | 12:25:34.959 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
429 | 12:25:35.720 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
430 | 12:25:35.723 |  |  |  |  | →SIP ACK | P-CSCF
431 | 12:25:35.732 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1105: ACK Verdict: Pass
432 | 12:25:35.733 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:53: Step 2 Verdict: Pass
433 | 12:25:36.352 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
434 | 12:25:36.360 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
435 | 12:25:36.368 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
436 | 12:25:36.392 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
437 | 12:25:36.432 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
438 | 12:25:36.483 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:58: Step 7 Verdict: Pass
439 | 12:25:36.585 |  |  |  |  | MMICmd: Release PTT token
440 | 12:25:40.200 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
441 | 12:25:40.202 |  |  |  |  | Floor Release→ | Media-Server
442 | 12:25:40.204 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
443 | 12:25:40.205 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
444 | 12:25:40.206 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:65: Step 9 Verdict: Pass
445 | 12:25:40.208 |  |  |  |  | ←Floor Idle | Media-Server
446 | 12:25:40.211 |  | ←enobeB PCAP frame← |  |  |
447 | 12:25:40.307 |  |  |  |  | MMICmd: Request PTT token
448 | 12:25:41.512 | →enobeB PCAP frame→ |  |  |  |
449 | 12:25:41.514 |  |  |  |  | Floor Request→ | Media-Server
450 | 12:25:41.517 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Request Verdict: Pass
451 | 12:25:41.520 |  |  |  |  | ←Floor Granted | Media-Server
452 | 12:25:41.523 |  | ←enobeB PCAP frame← |  |  |
453 | 12:25:41.552 | →enobeB PCAP frame→ |  |  |  |
454 | 12:25:41.554 |  |  |  |  | Floor ACK→ | Media-Server
455 | 12:25:41.555 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
456 | 12:25:41.555 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:74: Step 13 Verdict: Pass
457 | 12:25:41.557 |  |  |  |  | ←Floor Revoke | Media-Server
458 | 12:25:41.559 |  | ←enobeB PCAP frame← |  |  |
459 | 12:25:41.592 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
460 | 12:25:41.596 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
461 | 12:25:41.600 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
462 | 12:25:41.601 |  |  |  |  | Floor Release→ | Media-Server
463 | 12:25:41.602 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
464 | 12:25:41.603 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
465 | 12:25:41.603 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:87: Step 19 Verdict: Pass
466 | 12:25:41.604 |  |  |  |  | ←Floor Taken | Media-Server
467 | 12:25:41.607 |  | ←enobeB PCAP frame← |  |  |
468 | 12:25:42.353 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:90: Table 6.1.1.1.3.2-2: Parallel Behaviour Verdict: Pass
469 | 12:25:42.455 |  |  |  |  | MMICmd: Request PTT token
470 | 12:25:43.752 | →enobeB PCAP frame→ |  |  |  |
471 | 12:25:43.754 |  |  |  |  | Floor Request→ | Media-Server
472 | 12:25:43.757 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Request Verdict: Pass
473 | 12:25:43.758 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:101: Step 22 Verdict: Pass
474 | 12:25:43.761 |  |  |  |  | ←Floor Deny | Media-Server
475 | 12:25:43.764 |  | ←enobeB PCAP frame← |  |  |
476 | 12:25:43.860 |  |  |  |  | MMICmd: Request PTT token
477 | 12:25:46.192 | →enobeB PCAP frame→ |  |  |  |
478 | 12:25:46.194 |  |  |  |  | Floor Request→ | Media-Server
479 | 12:25:46.196 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Request Verdict: Pass
480 | 12:25:46.196 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:111: Step 26 Verdict: Pass
481 | 12:25:46.198 |  |  |  |  | ←Floor Queue Position Info | Media-Server
482 | 12:25:46.201 |  | ←enobeB PCAP frame← |  |  |
483 | 12:25:46.947 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:116: Step 28 Verdict: Pass
484 | 12:25:46.948 |  |  |  |  | MMICmd: Make the MCPTT User request the current position in the queue
485 | 12:25:48.992 | →enobeB PCAP frame→ |  |  |  |
486 | 12:25:48.994 |  |  |  |  | Floor Queue Position Request→ | Media-Server
487 | 12:25:48.997 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Position Request Verdict: Pass
488 | 12:25:48.998 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:123: Step 30 Verdict: Pass
489 | 12:25:49.000 |  |  |  |  | ←Floor Queue Position Info | Media-Server
490 | 12:25:49.003 |  | ←enobeB PCAP frame← |  |  |
491 | 12:25:49.748 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:126: Step 30A Verdict: Pass
492 | 12:25:49.850 |  |  |  |  | MMICmd: Release PTT token
493 | 12:25:54.832 | →enobeB PCAP frame→ |  |  |  |
494 | 12:25:54.834 |  |  |  |  | Floor Release→ | Media-Server
495 | 12:25:54.837 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
496 | 12:25:54.838 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:135: Step 33 Verdict: Pass
497 | 12:25:54.841 |  |  |  |  | ←Floor Taken | Media-Server
498 | 12:25:54.844 |  | ←enobeB PCAP frame← |  |  |
499 | 12:25:54.940 |  |  |  |  | MMICmd: Request PTT token
500 | 12:25:57.312 | →enobeB PCAP frame→ |  |  |  |
501 | 12:25:57.314 |  |  |  |  | Floor Request→ | Media-Server
502 | 12:25:57.318 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Request Verdict: Pass
503 | 12:25:57.319 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:144: Step 36 Verdict: Pass
504 | 12:25:57.322 |  |  |  |  | ←Floor Queue Position Info | Media-Server
505 | 12:25:57.324 |  | ←enobeB PCAP frame← |  |  |
506 | 12:25:58.069 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:149: Step 38 Verdict: Pass
507 | 12:25:58.071 |  |  |  |  | ←Floor Granted | Media-Server
508 | 12:25:58.073 |  | ←enobeB PCAP frame← |  |  |
509 | 12:25:58.152 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
510 | 12:25:58.156 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
511 | 12:25:58.160 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
512 | 12:25:58.164 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
513 | 12:25:58.168 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
514 | 12:25:58.820 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:155: Step 40 Verdict: Pass
515 | 12:25:58.921 |  |  |  |  | MMICmd: Release PTT token
516 | 12:26:02.610 |  |  |  |  | Floor Release→ | Media-Server
517 | 12:26:02.613 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
518 | 12:26:02.614 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:162: Step 42 Verdict: Pass
519 | 12:26:02.617 |  |  |  |  | ←Floor Idle | Media-Server
520 | 12:26:02.619 |  | ←enobeB PCAP frame← |  |  |
521 | 12:26:02.623 |  |  |  |  | ←SIP BYE | P-CSCF
522 | 12:26:02.626 |  | ←enobeB PCAP frame← SIP over IPSEC: BYE sip:PublicUserId-A@192.168.3.2:43509;transport... |  |  |
523 | 12:26:02.680 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
524 | 12:26:02.683 |  |  |  |  | →SIP 200 OK | P-CSCF
525 | 12:26:03.432 | →enobeB PCAP frame→ |  |  |  |
526 | 12:26:04.692 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
527 | 12:26:04.712 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
528 | 12:26:04.713 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x4) |  |  |
529 | 12:26:04.713 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
530 | 12:26:04.714 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
531 | 12:26:04.752 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
532 | 12:26:04.752 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
533 | 12:26:04.752 |  | →RRC DCCH UL Information Transfer |  |  |
534 | 12:26:04.752 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xc) |  |  |
535 | 12:26:04.752 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
536 | 12:26:04.834 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
537 | 12:26:04.835 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
538 | 12:26:05.056 |  | ←RRC DCCH RRC Connection Release |  |  |
539 | 12:26:05.057 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
540 | 12:26:05.066 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
541 | 12:26:05.067 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:168: Step 45 Verdict: Pass
542 | 12:26:05.069 |  |  |  |  | MMICmd: Make the MCPTT User request the establishment of an MCPTT on-demand pre-arranged group call, automatic commencement mode, with implicit floor control
543 | 12:26:05.069 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
544 | 12:26:05.739 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
545 | 12:26:05.739 |  | →RRC CCCH RRC Connection Request |  |  |
546 | 12:26:05.739 |  | ←RRC CCCH RRC Connection Setup |  |  |
547 | 12:26:05.739 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
548 | 12:26:05.792 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
549 | 12:26:05.792 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
550 | 12:26:05.792 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
551 | 12:26:05.792 |  |  |  | →NAS EMM Service request |  |
552 | 12:26:05.792 |  |  |  | NAS K-enb cb114291eab88b38e4f6ab42f99444209... |  |
553 | 12:26:05.793 |  | ←RRC DCCH Security Mode Command |  |  |
554 | 12:26:05.793 |  |  | RRC K-enb cb114291eab88b38e4f6ab42f99444209... |  |  |
555 | 12:26:05.793 |  |  | RRC rrc-cip 46eacf33af31d8b968f78739effe31d... |  |  |
556 | 12:26:05.793 |  |  | RRC rrc-int e377cfccbd4fa4f48b26c298ee134da... |  |  |
557 | 12:26:05.793 |  |  | RRC up-cip 597559d43bca318f4899ae93efa61371... |  |  |
558 | 12:26:05.793 |  |  | RRC up-int 04099a0a671ada2d994e1956ce9446e9... |  |  |
559 | 12:26:05.794 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
560 | 12:26:05.832 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
561 | 12:26:05.832 |  | →RRC DCCH Security Mode Complete |  |  |
562 | 12:26:05.832 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
563 | 12:26:05.832 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
564 | 12:26:05.872 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
565 | 12:26:05.872 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
566 | 12:26:08.160 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
567 | 12:26:08.161 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
568 | 12:26:08.174 |  |  |  |  | →SIP INVITE | P-CSCF
569 | 12:26:08.225 |  |  |  |  | XML→ | Media-Server
570 | 12:26:08.226 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
571 | 12:26:08.228 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1102: INVITE Verdict: Pass
572 | 12:26:08.230 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
573 | 12:26:08.230 |  |  |  |  | ←SIP 100 Trying | P-CSCF
574 | 12:26:08.231 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xd) |  |  |
575 | 12:26:08.231 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
576 | 12:26:08.232 |  | ←enobeB PCAP frame← SIP/NAS-EPS RRCConnectionReconfiguration Ciphered message [362-bytes] Activate dedicated EPS bearer context request SIP over IPSEC: SIP/2.0 100 Trying |  |  |
577 | 12:26:08.233 |  |  |  |  | ←SIP 200 OK | P-CSCF
578 | 12:26:08.236 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
579 | 12:26:08.272 | →enobeB PCAP frame→ RLC-LTE/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
580 | 12:26:08.272 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
581 | 12:26:08.272 |  | →RRC DCCH UL Information Transfer |  |  |
582 | 12:26:08.272 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x8) |  |  |
583 | 12:26:08.272 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
584 | 12:26:08.366 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
585 | 12:26:08.840 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
586 | 12:26:08.843 |  |  |  |  | →SIP ACK | P-CSCF
587 | 12:26:08.852 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1105: ACK Verdict: Pass
588 | 12:26:08.853 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:178: Step 48 Verdict: Pass
589 | 12:26:09.312 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
590 | 12:26:09.316 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
591 | 12:26:09.320 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
592 | 12:26:09.324 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
593 | 12:26:09.328 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
594 | 12:26:09.603 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:183: Step 53 Verdict: Pass
595 | 12:26:09.705 |  |  |  |  | MMICmd: Release PTT token
596 | 12:26:12.888 | →enobeB PCAP frame→ |  |  |  |
597 | 12:26:12.890 |  |  |  |  | Floor Release→ | Media-Server
598 | 12:26:12.893 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
599 | 12:26:12.894 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:190: Step 55 Verdict: Pass
600 | 12:26:12.895 |  |  |  |  | MMICmd: Make the MCPTT User request upgrade of the ongoing On-Demand Pre-arranged Group Call to MCPTT Emergency Group Call with implicit floor control
601 | 12:26:12.896 |  |  |  |  | ←Floor Idle | Media-Server
602 | 12:26:12.899 |  | ←enobeB PCAP frame← |  |  |
603 | 12:26:17.680 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
604 | 12:26:17.681 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 SRTP frame: |  |  |  |
605 | 12:26:17.685 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
606 | 12:26:17.694 |  |  |  |  | →SIP INVITE | P-CSCF
607 | 12:26:17.696 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
608 | 12:26:17.712 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
609 | 12:26:17.715 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
610 | 12:26:17.734 |  |  |  |  | XML→ | Media-Server
611 | 12:26:17.737 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1171: re-INVITE Verdict: Pass
612 | 12:26:17.739 |  |  |  |  | ←SIP 100 Trying | P-CSCF
613 | 12:26:17.741 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
614 | 12:26:17.741 |  |  |  |  | ←SIP 200 OK | P-CSCF
615 | 12:26:17.744 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
616 | 12:26:17.752 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
617 | 12:26:17.755 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
618 | 12:26:17.760 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
619 | 12:26:17.764 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
620 | 12:26:17.800 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:mcptt-server-A@mcstaasting.com SIP/2.0 SRTP frame: |  |  |  |
621 | 12:26:17.802 |  |  |  |  | →SIP ACK | P-CSCF
622 | 12:26:17.806 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1176: ACK Verdict: Pass
623 | 12:26:17.808 |  |  |  |  | ←Floor Granted | Media-Server
624 | 12:26:17.810 |  | ←enobeB PCAP frame← |  |  |
625 | 12:26:17.832 | →enobeB PCAP frame→ |  |  |  |
626 | 12:26:17.834 |  |  |  |  | Floor ACK→ | Media-Server
627 | 12:26:17.835 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
628 | 12:26:17.835 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:200: Step 60 Verdict: Pass
629 | 12:26:17.912 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
630 | 12:26:17.919 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
631 | 12:26:17.920 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
632 | 12:26:17.925 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
633 | 12:26:17.952 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
634 | 12:26:18.585 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:205: Step 61D Verdict: Pass
635 | 12:26:18.686 |  |  |  |  | MMICmd: Release PTT token
636 | 12:26:21.440 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
637 | 12:26:21.442 |  |  |  |  | Floor Release→ | Media-Server
638 | 12:26:21.444 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
639 | 12:26:21.445 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
640 | 12:26:21.446 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:212: Step 63 Verdict: Pass
641 | 12:26:21.449 |  |  |  |  | ←Floor Idle | Media-Server
642 | 12:26:21.452 |  | ←enobeB PCAP frame← |  |  |
643 | 12:26:21.548 |  |  |  |  | MMICmd: Request PTT token
644 | 12:26:24.672 | →enobeB PCAP frame→ |  |  |  |
645 | 12:26:24.674 |  |  |  |  | Floor Request→ | Media-Server
646 | 12:26:24.678 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Request Verdict: Pass
647 | 12:26:24.681 |  |  |  |  | ←Floor Granted | Media-Server
648 | 12:26:24.684 |  | ←enobeB PCAP frame← |  |  |
649 | 12:26:24.712 | →enobeB PCAP frame→ |  |  |  |
650 | 12:26:24.714 |  |  |  |  | Floor ACK→ | Media-Server
651 | 12:26:24.717 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
652 | 12:26:24.717 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:221: Step 67 Verdict: Pass
653 | 12:26:24.752 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
654 | 12:26:24.756 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
655 | 12:26:24.760 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
656 | 12:26:24.764 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
657 | 12:26:24.792 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
658 | 12:26:24.819 |  |  |  |  | MMICmd: Release PTT token
659 | 12:26:29.288 | →enobeB PCAP frame→ |  |  |  |
660 | 12:26:29.290 |  |  |  |  | Floor Release→ | Media-Server
661 | 12:26:29.293 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
662 | 12:26:29.294 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:230: Step 72 Verdict: Pass
663 | 12:26:29.295 |  |  |  |  | MMICmd: Make the MCPTT User cancel the Emergency State.
664 | 12:26:29.297 |  |  |  |  | ←Floor Idle | Media-Server
665 | 12:26:29.299 |  | ←enobeB PCAP frame← |  |  |
666 | 12:26:29.312 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
667 | 12:26:29.316 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
668 | 12:26:33.880 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
669 | 12:26:33.881 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 SRTP frame: |  |  |  |
670 | 12:26:33.886 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
671 | 12:26:33.895 |  |  |  |  | →SIP INVITE | P-CSCF
672 | 12:26:33.897 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
673 | 12:26:33.912 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
674 | 12:26:33.916 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
675 | 12:26:33.957 |  |  |  |  | XML→ | Media-Server
676 | 12:26:33.961 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1171: re-INVITE Verdict: Pass
677 | 12:26:33.966 |  |  |  |  | ←SIP 100 Trying | P-CSCF
678 | 12:26:33.969 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
679 | 12:26:33.969 |  |  |  |  | ←SIP 200 OK | P-CSCF
680 | 12:26:33.971 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
681 | 12:26:33.992 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
682 | 12:26:33.996 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
683 | 12:26:34.000 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
684 | 12:26:34.005 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
685 | 12:26:34.040 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
686 | 12:26:34.042 |  |  |  |  | →SIP ACK | P-CSCF
687 | 12:26:34.044 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1176: ACK Verdict: Pass
688 | 12:26:34.044 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:239: Step 76 Verdict: Pass
689 | 12:26:34.045 |  |  |  |  | ←Floor Idle | Media-Server
690 | 12:26:34.047 |  | ←enobeB PCAP frame← |  |  |
691 | 12:26:34.145 |  |  |  |  | MMICmd: Request PTT token
692 | 12:26:38.512 | →enobeB PCAP frame→ |  |  |  |
693 | 12:26:38.514 |  |  |  |  | Floor Request→ | Media-Server
694 | 12:26:38.517 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Request Verdict: Pass
695 | 12:26:38.521 |  |  |  |  | ←Floor Granted | Media-Server
696 | 12:26:38.523 |  | ←enobeB PCAP frame← |  |  |
697 | 12:26:38.552 | →enobeB PCAP frame→ |  |  |  |
698 | 12:26:38.554 |  |  |  |  | Floor ACK→ | Media-Server
699 | 12:26:38.556 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
700 | 12:26:38.556 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:246: Step 77A Verdict: Pass
701 | 12:26:38.592 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
702 | 12:26:38.596 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
703 | 12:26:38.600 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
704 | 12:26:38.603 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
705 | 12:26:38.632 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
706 | 12:26:38.657 |  |  |  |  | MMICmd: Release PTT token
707 | 12:26:41.432 | →enobeB PCAP frame→ |  |  |  |
708 | 12:26:41.434 |  |  |  |  | Floor Release→ | Media-Server
709 | 12:26:41.437 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
710 | 12:26:41.438 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:255: Step 79 Verdict: Pass
711 | 12:26:41.439 |  |  |  |  | MMICmd: Make the MCPTT User request upgrade of the ongoing On-Demand Pre-arranged Group Call to MCPTT Imminent Peril Group Call with explcit request for floor control (implicit floor control)
712 | 12:26:41.440 |  |  |  |  | ←Floor Idle | Media-Server
713 | 12:26:41.443 |  | ←enobeB PCAP frame← |  |  |
714 | 12:26:46.560 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
715 | 12:26:46.561 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 SRTP frame: |  |  |  |
716 | 12:26:46.570 |  |  |  |  | →SIP INVITE | P-CSCF
717 | 12:26:46.573 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
718 | 12:26:46.592 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
719 | 12:26:46.595 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
720 | 12:26:46.600 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
721 | 12:26:46.611 |  |  |  |  | XML→ | Media-Server
722 | 12:26:46.613 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1171: re-INVITE Verdict: Pass
723 | 12:26:46.616 |  |  |  |  | ←SIP 100 Trying | P-CSCF
724 | 12:26:46.618 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
725 | 12:26:46.619 |  |  |  |  | ←SIP 200 OK | P-CSCF
726 | 12:26:46.621 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
727 | 12:26:46.640 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
728 | 12:26:46.643 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
729 | 12:26:46.644 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
730 | 12:26:46.680 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:mcptt-server-A@mcstaasting.com SIP/2.0 SRTP frame: |  |  |  |
731 | 12:26:46.681 |  |  |  |  | →SIP ACK | P-CSCF
732 | 12:26:46.683 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1176: ACK Verdict: Pass
733 | 12:26:46.684 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
734 | 12:26:46.684 |  |  |  |  | ←Floor Granted | Media-Server
735 | 12:26:46.687 |  | ←enobeB PCAP frame← |  |  |
736 | 12:26:46.712 | →enobeB PCAP frame→ |  |  |  |
737 | 12:26:46.713 |  |  |  |  | Floor ACK→ | Media-Server
738 | 12:26:46.714 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
739 | 12:26:46.714 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:265: Step 83 Verdict: Pass
740 | 12:26:46.752 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
741 | 12:26:46.756 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
742 | 12:26:46.760 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
743 | 12:26:46.764 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
744 | 12:26:46.792 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
745 | 12:26:47.464 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:270: Step 84D Verdict: Pass
746 | 12:26:47.566 |  |  |  |  | MMICmd: Release PTT token
747 | 12:26:49.880 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
748 | 12:26:49.882 |  |  |  |  | Floor Release→ | Media-Server
749 | 12:26:49.884 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
750 | 12:26:49.885 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
751 | 12:26:49.886 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:277: Step 86 Verdict: Pass
752 | 12:26:49.889 |  |  |  |  | ←Floor Idle | Media-Server
753 | 12:26:49.892 |  | ←enobeB PCAP frame← |  |  |
754 | 12:26:49.987 |  |  |  |  | MMICmd: Request PTT token
755 | 12:26:52.792 | →enobeB PCAP frame→ |  |  |  |
756 | 12:26:52.794 |  |  |  |  | Floor Request→ | Media-Server
757 | 12:26:52.797 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Request Verdict: Pass
758 | 12:26:52.801 |  |  |  |  | ←Floor Granted | Media-Server
759 | 12:26:52.803 |  | ←enobeB PCAP frame← |  |  |
760 | 12:26:52.832 | →enobeB PCAP frame→ |  |  |  |
761 | 12:26:52.834 |  |  |  |  | Floor ACK→ | Media-Server
762 | 12:26:52.837 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
763 | 12:26:52.837 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:286: Step 90 Verdict: Pass
764 | 12:26:52.872 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
765 | 12:26:52.876 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
766 | 12:26:52.880 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
767 | 12:26:52.883 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
768 | 12:26:52.912 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
769 | 12:26:52.939 |  |  |  |  | MMICmd: Release PTT token
770 | 12:26:55.501 |  |  |  |  | Floor Release→ | Media-Server
771 | 12:26:55.504 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
772 | 12:26:55.505 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:295: Step 95 Verdict: Pass
773 | 12:26:55.506 |  |  |  |  | MMICmd: Make the MCPTT User cancel the Imminent Peril State
774 | 12:26:55.508 |  |  |  |  | ←Floor Idle | Media-Server
775 | 12:26:55.510 |  | ←enobeB PCAP frame← |  |  |
776 | 12:26:59.960 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
777 | 12:26:59.961 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 SRTP frame: |  |  |  |
778 | 12:26:59.965 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
779 | 12:26:59.974 |  |  |  |  | →SIP INVITE | P-CSCF
780 | 12:26:59.977 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
781 | 12:26:59.978 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
782 | 12:26:59.992 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
783 | 12:27:00.027 |  |  |  |  | XML→ | Media-Server
784 | 12:27:00.030 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1171: re-INVITE Verdict: Pass
785 | 12:27:00.033 |  |  |  |  | ←SIP 100 Trying | P-CSCF
786 | 12:27:00.036 |  |  |  |  | ←SIP 200 OK | P-CSCF
787 | 12:27:00.039 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
788 | 12:27:00.040 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
789 | 12:27:00.044 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
790 | 12:27:00.080 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
791 | 12:27:00.084 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
792 | 12:27:00.120 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:mcptt-server-A@mcstaasting.com SIP/2.0 SRTP frame: |  |  |  |
793 | 12:27:00.122 |  |  |  |  | →SIP ACK | P-CSCF
794 | 12:27:00.124 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1176: ACK Verdict: Pass
795 | 12:27:00.124 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:304: Step 99 Verdict: Pass
796 | 12:27:00.125 |  |  |  |  | ←Floor Idle | Media-Server
797 | 12:27:00.128 |  | ←enobeB PCAP frame← |  |  |
798 | 12:27:00.225 |  |  |  |  | MMICmd: Request PTT token
799 | 12:27:03.440 | →enobeB PCAP frame→ |  |  |  |
800 | 12:27:03.442 |  |  |  |  | Floor Request→ | Media-Server
801 | 12:27:03.446 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Request Verdict: Pass
802 | 12:27:03.449 |  |  |  |  | ←Floor Granted | Media-Server
803 | 12:27:03.452 |  | ←enobeB PCAP frame← |  |  |
804 | 12:27:03.472 | →enobeB PCAP frame→ |  |  |  |
805 | 12:27:03.474 |  |  |  |  | Floor ACK→ | Media-Server
806 | 12:27:03.477 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
807 | 12:27:03.477 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:311: Step 100A Verdict: Pass
808 | 12:27:03.512 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
809 | 12:27:03.516 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
810 | 12:27:03.560 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
811 | 12:27:03.563 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
812 | 12:27:03.579 |  |  |  |  | MMICmd: Release PTT token
813 | 12:27:03.592 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
814 | 12:27:06.760 | →enobeB PCAP frame→ |  |  |  |
815 | 12:27:06.762 |  |  |  |  | Floor Release→ | Media-Server
816 | 12:27:06.765 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
817 | 12:27:06.765 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:320: Step 102 Verdict: Pass
818 | 12:27:06.768 |  |  |  |  | ←Floor Idle | Media-Server
819 | 12:27:06.771 |  | ←enobeB PCAP frame← |  |  |
820 | 12:27:06.870 |  |  |  |  | MMICmd: Release call (hang up the call)
821 | 12:27:09.800 | →enobeB PCAP frame→ SIP over IPSEC: BYE sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
822 | 12:27:09.804 |  |  |  |  | →SIP BYE | P-CSCF
823 | 12:27:09.823 |  |  |  |  | ←SIP 200 OK | P-CSCF
824 | 12:27:09.826 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
825 | 12:27:10.072 | →enobeB PCAP frame→ |  |  |  |
826 | 12:27:11.823 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
827 | 12:27:11.852 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
828 | 12:27:11.853 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x9) |  |  |
829 | 12:27:11.853 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
830 | 12:27:11.854 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
831 | 12:27:11.912 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
832 | 12:27:11.912 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
833 | 12:27:11.912 |  | →RRC DCCH UL Information Transfer |  |  |
834 | 12:27:11.912 |  | [EMBEDDED NAS IN PREV RRC] Message too short (len=9) |  |  |
835 | 12:27:11.912 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
836 | 12:27:11.980 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
837 | 12:27:11.981 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
838 | 12:27:12.018 |  | ←RRC DCCH RRC Connection Release |  |  |
839 | 12:27:12.019 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
840 | 12:27:12.039 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
841 | 12:27:12.039 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:326: Step 106 Verdict: Pass
842 | 12:27:12.040 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
843 | 12:27:12.042 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
844 | 12:27:12.791 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.