ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 12:35:22.384 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 12:35:22.385 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 12:35:22.385 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 12:35:22.386 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 12:35:22.387 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 12:35:22.387 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:801: IMS UDP port 192.168.2.3:5060 configured
7 | 12:35:22.390 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:751: IMS TCP port 192.168.2.3:5060 configured!
8 | 12:35:22.392 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:772: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 12:35:22.393 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:783: IdM port 192.168.2.3:8080 configured!
10 | 12:35:22.396 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 12:35:23.660 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 12:35:23.660 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 12:35:52.164 |  | ←RRC BCCH SIB |  |  |
14 | 12:35:52.169 |  | ←RRC BCCH SIB1 |  |  |
15 | 12:35:52.249 |  | ←RRC BCCH SIB1 |  |  |
16 | 12:35:52.324 |  | ←RRC BCCH SIB |  |  |
17 | 12:35:52.329 |  | ←RRC BCCH SIB1 |  |  |
18 | 12:37:03.843 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 12:37:03.844 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 12:37:03.844 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 12:37:03.844 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 12:37:03.904 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 12:37:03.904 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 12:37:03.904 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 12:37:03.904 |  |  |  | →NAS EMM Attach request |  |
26 | 12:37:03.904 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 12:37:03.905 |  |  |  | NAS K-asme f7ebed47ac5fab7b791bc18f57097530... |  |
28 | 12:37:03.905 |  |  |  | NAS ← EMM Authentication request |  |
29 | 12:37:03.905 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 12:37:03.905 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 12:37:03.907 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 12:37:03.976 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 12:37:03.976 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 12:37:03.976 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 12:37:03.977 |  |  |  | →NAS EMM Authentication response |  |
36 | 12:37:03.977 |  |  |  | NAS UE auth OK |  |
37 | 12:37:03.977 |  |  |  | NAS K-nas-cip 9cec8c7ef51bf66c92f4db44c3f09... |  |
38 | 12:37:03.977 |  |  |  | NAS K-nas-int 8d8f3e28285a328cda4ab7bb90ed4... |  |
39 | 12:37:03.977 |  |  |  | NAS ← EMM Security mode command |  |
40 | 12:37:03.977 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 12:37:03.977 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 12:37:03.979 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 12:37:04.016 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
44 | 12:37:04.016 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 12:37:04.016 |  | [EMBEDDED NAS IN PREV RRC] TP Unknown message (type=0xa7) |  |  |
46 | 12:37:04.016 |  |  |  | →NAS EMM Security mode complete |  |
47 | 12:37:04.017 |  |  |  | NAS ← ESM ESM information request |  |
48 | 12:37:04.017 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x0) |  |  |
49 | 12:37:04.017 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 12:37:04.018 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
51 | 12:37:04.026 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
52 | 12:37:04.064 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
53 | 12:37:04.064 |  | →RRC DCCH UL Information Transfer |  |  |
54 | 12:37:04.064 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x0) |  |  |
55 | 12:37:04.065 |  |  |  | →NAS ESM ESM information response |  |
56 | 12:37:04.065 |  |  |  | NAS ← EMM Attach accept |  |
57 | 12:37:04.065 |  |  |  | NAS K-enb d2ac3a4b0d3c5830a193e07207d8f50e7... |  |
58 | 12:37:04.065 |  |  | RRC K-enb d2ac3a4b0d3c5830a193e07207d8f50e7... |  |  |
59 | 12:37:04.065 |  |  | RRC rrc-cip b06d05a4978b9277aa592cde8ea6d65... |  |  |
60 | 12:37:04.065 |  |  | RRC rrc-int d4b2f6f70ea5bea09cb6bcbcfa7d29b... |  |  |
61 | 12:37:04.065 |  |  | RRC up-cip 323b0aa289bf324d3221e333e86c3fc3... |  |  |
62 | 12:37:04.065 |  |  | RRC up-int 61b8fe63b581547bf2d96aebbc00c94d... |  |  |
63 | 12:37:04.065 |  | ←RRC DCCH Security Mode Command |  |  |
64 | 12:37:04.067 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
65 | 12:37:04.096 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
66 | 12:37:04.096 |  | →RRC DCCH Security Mode Complete |  |  |
67 | 12:37:04.096 |  | ←RRC DCCH UE Capability Enquiry |  |  |
68 | 12:37:04.096 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
69 | 12:37:04.146 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
70 | 12:37:04.146 |  | →RRC DCCH UE Capability Information |  |  |
71 | 12:37:04.147 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x0) |  |  |
72 | 12:37:04.147 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
73 | 12:37:04.147 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
74 | 12:37:04.176 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
75 | 12:37:04.176 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
76 | 12:37:04.216 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
77 | 12:37:04.217 |  | →RRC DCCH UL Information Transfer |  |  |
78 | 12:37:04.217 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x5) |  |  |
79 | 12:37:04.217 |  |  |  | →NAS EMM Attach complete |  |
80 | 12:37:04.217 |  |  |  | NAS ← EMM EMM information |  |
81 | 12:37:04.217 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x6) |  |  |
82 | 12:37:04.217 |  | ←RRC DCCH DL Information Transfer |  |  |
83 | 12:37:04.218 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
84 | 12:37:11.138 |  | ←RRC DCCH RRC Connection Release |  |  |
85 | 12:37:11.139 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
86 | 12:37:11.273 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
87 | 12:37:11.273 |  | →RRC CCCH RRC Connection Request |  |  |
88 | 12:37:11.273 |  | ←RRC CCCH RRC Connection Setup |  |  |
89 | 12:37:11.273 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
90 | 12:37:11.296 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
91 | 12:37:11.296 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
92 | 12:37:11.296 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
93 | 12:37:11.296 |  |  |  | →NAS EMM Service request |  |
94 | 12:37:11.296 |  |  |  | NAS K-enb 2028ededa9305b072a7b80950bde2ca47... |  |
95 | 12:37:11.297 |  |  | RRC K-enb 2028ededa9305b072a7b80950bde2ca47... |  |  |
96 | 12:37:11.298 |  |  | RRC rrc-cip 9860f02dc6076aa218fff9c1398dea9... |  |  |
97 | 12:37:11.298 |  |  | RRC rrc-int 259c8726fa34f6a93edb2baa00fb2dc... |  |  |
98 | 12:37:11.298 |  |  | RRC up-cip de4cd6511174e1cc9aff3b324669370f... |  |  |
99 | 12:37:11.298 |  |  | RRC up-int ae9fa9dabde49e98e367d10ce966fbc7... |  |  |
100 | 12:37:11.298 |  | ←RRC DCCH Security Mode Command |  |  |
101 | 12:37:11.298 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
102 | 12:37:11.336 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
103 | 12:37:11.336 |  | →RRC DCCH Security Mode Complete |  |  |
104 | 12:37:11.337 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
105 | 12:37:11.337 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
106 | 12:37:11.377 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
107 | 12:37:11.377 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
108 | 12:37:25.977 | →enobeB PCAP frame→ TCP |  |  |  |
109 | 12:37:25.981 |  | ←enobeB PCAP frame← TCP |  |  |
110 | 12:37:26.016 | →enobeB PCAP frame→ TCP |  |  |  |
111 | 12:37:26.104 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
112 | 12:37:26.108 |  | ←enobeB PCAP frame← TCP |  |  |
113 | 12:37:26.113 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
114 | 12:37:26.137 | →enobeB PCAP frame→ TCP |  |  |  |
115 | 12:37:26.304 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
116 | 12:37:26.308 |  | ←enobeB PCAP frame← TCP |  |  |
117 | 12:37:26.308 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:632: Client connected to Http Proxy port (id 17)
118 | 12:37:26.309 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
119 | 12:37:26.336 | →enobeB PCAP frame→ TCP |  |  |  |
120 | 12:37:26.344 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
121 | 12:37:26.347 |  | ←enobeB PCAP frame← TCP |  |  |
122 | 12:37:26.347 |  |  |  |  | →HTTP GET | HTTP-Proxy
123 | 12:37:26.354 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:248: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
124 | 12:37:26.376 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
125 | 12:37:26.380 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
126 | 12:37:26.416 | →enobeB PCAP frame→ TCP |  |  |  |
127 | 12:37:28.416 | →enobeB PCAP frame→ TCP |  |  |  |
128 | 12:37:28.421 |  | ←enobeB PCAP frame← TCP |  |  |
129 | 12:37:28.456 | →enobeB PCAP frame→ TCP |  |  |  |
130 | 12:37:28.464 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
131 | 12:37:28.468 |  | ←enobeB PCAP frame← TCP |  |  |
132 | 12:37:28.473 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
133 | 12:37:28.496 | →enobeB PCAP frame→ TCP |  |  |  |
134 | 12:37:28.744 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
135 | 12:37:28.748 |  | ←enobeB PCAP frame← TCP |  |  |
136 | 12:37:28.748 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:638: Client connected to IdM port (id 19)
137 | 12:37:28.749 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
138 | 12:37:28.777 | →enobeB PCAP frame→ TCP |  |  |  |
139 | 12:37:28.784 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
140 | 12:37:28.788 |  | ←enobeB PCAP frame← TCP |  |  |
141 | 12:37:28.788 |  |  |  |  | →HTTP GET | IDMS-Endpoint
142 | 12:37:28.819 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
143 | 12:37:28.821 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
144 | 12:37:28.823 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:453: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
145 | 12:37:28.824 |  |  |  |  | MMICmd: Please provide user credentials: username and password
146 | 12:37:28.897 | →enobeB PCAP frame→ TCP |  |  |  |
147 | 12:37:35.504 | →enobeB PCAP frame→ HTTPS: POST /idms/userauth HTTP/1.1 |  |  |  |
148 | 12:37:35.508 |  | ←enobeB PCAP frame← TCP |  |  |
149 | 12:37:35.509 |  |  |  |  | →HTTP POST | IDMS-Endpoint
150 | 12:37:35.524 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
151 | 12:37:35.526 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
152 | 12:37:35.526 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:458: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
153 | 12:37:35.576 | →enobeB PCAP frame→ TCP |  |  |  |
154 | 12:37:35.578 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:673: IdM port - Client closed the connection (id 19)
155 | 12:37:35.580 |  | ←enobeB PCAP frame← TCP |  |  |
156 | 12:37:35.616 | →enobeB PCAP frame→ TCP |  |  |  |
157 | 12:37:35.976 | →enobeB PCAP frame→ TCP |  |  |  |
158 | 12:37:35.980 |  | ←enobeB PCAP frame← TCP |  |  |
159 | 12:37:36.016 | →enobeB PCAP frame→ TCP |  |  |  |
160 | 12:37:36.064 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
161 | 12:37:36.068 |  | ←enobeB PCAP frame← TCP |  |  |
162 | 12:37:36.069 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
163 | 12:37:36.096 | →enobeB PCAP frame→ TCP |  |  |  |
164 | 12:37:36.184 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
165 | 12:37:36.187 |  | ←enobeB PCAP frame← TCP |  |  |
166 | 12:37:36.187 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:638: Client connected to IdM port (id 19)
167 | 12:37:36.188 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
168 | 12:37:36.216 | →enobeB PCAP frame→ TCP |  |  |  |
169 | 12:37:36.264 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
170 | 12:37:36.267 |  |  |  |  | →HTTP POST | IDMS-Endpoint
171 | 12:37:36.268 |  | ←enobeB PCAP frame← TCP |  |  |
172 | 12:37:36.281 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
173 | 12:37:36.283 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
174 | 12:37:36.284 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:463: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
175 | 12:37:36.285 |  |  |  |  | Verdict PASS: MCPTT_ClientConfiguration_MCX_HTTP.ttcn:36: Step 3-12 Verdict: Pass
176 | 12:37:36.377 | →enobeB PCAP frame→ TCP |  |  |  |
177 | 12:37:36.657 | →enobeB PCAP frame→ TCP |  |  |  |
178 | 12:37:36.660 |  | ←enobeB PCAP frame← TCP |  |  |
179 | 12:37:36.696 | →enobeB PCAP frame→ TCP |  |  |  |
180 | 12:37:36.704 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
181 | 12:37:36.707 |  | ←enobeB PCAP frame← TCP |  |  |
182 | 12:37:36.708 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
183 | 12:37:36.736 | →enobeB PCAP frame→ TCP |  |  |  |
184 | 12:37:36.744 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
185 | 12:37:36.747 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:632: Client connected to Http Proxy port (id 20)
186 | 12:37:36.748 |  | ←enobeB PCAP frame← TCP |  |  |
187 | 12:37:36.748 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
188 | 12:37:36.784 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
189 | 12:37:36.788 |  | ←enobeB PCAP frame← TCP |  |  |
190 | 12:37:36.788 |  |  |  |  | →HTTP POST | HTTP-Proxy
191 | 12:37:36.811 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:481: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
192 | 12:37:36.818 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
193 | 12:37:36.821 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
194 | 12:37:36.857 | →enobeB PCAP frame→ TCP |  |  |  |
195 | 12:37:36.896 | →enobeB PCAP frame→ TCP |  |  |  |
196 | 12:37:36.900 |  | ←enobeB PCAP frame← TCP |  |  |
197 | 12:37:36.936 | →enobeB PCAP frame→ TCP |  |  |  |
198 | 12:37:36.944 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
199 | 12:37:36.949 |  | ←enobeB PCAP frame← TCP |  |  |
200 | 12:37:36.952 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
201 | 12:37:36.977 | →enobeB PCAP frame→ TCP |  |  |  |
202 | 12:37:36.984 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
203 | 12:37:36.988 |  | ←enobeB PCAP frame← TCP |  |  |
204 | 12:37:36.988 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:632: Client connected to Http Proxy port (id 21)
205 | 12:37:36.991 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
206 | 12:37:37.025 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
207 | 12:37:37.028 |  | ←enobeB PCAP frame← TCP |  |  |
208 | 12:37:37.030 |  |  |  |  | →HTTP POST | HTTP-Proxy
209 | 12:37:37.089 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
210 | 12:37:37.089 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:485: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
211 | 12:37:37.089 |  |  |  |  | Verdict PASS: MCPTT_ClientConfiguration_MCX_HTTP.ttcn:40: Step 13-16 Verdict: Pass
212 | 12:37:37.091 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
213 | 12:37:37.137 | →enobeB PCAP frame→ TCP |  |  |  |
214 | 12:37:37.176 | →enobeB PCAP frame→ TCP |  |  |  |
215 | 12:37:37.184 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
216 | 12:37:37.190 |  |  |  |  | →SIP REGISTER | P-CSCF
217 | 12:37:37.214 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:810: IMS UDP_s port 192.168.2.3:5062 configured
218 | 12:37:37.242 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:761: IMS TCP_s port 192.168.2.3:5062 configured!
219 | 12:37:37.245 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:819: IMS UDP_c port 192.168.2.3:5061 configured
220 | 12:37:37.254 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
221 | 12:37:37.256 |  | ←enobeB PCAP frame← SIP -cleartext-: SIP/2.0 401 Unauthorized |  |  |
222 | 12:37:37.984 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
223 | 12:37:37.990 |  |  |  |  | →SIP REGISTER | P-CSCF
224 | 12:37:38.015 |  |  |  |  | ←SIP 200 OK | P-CSCF
225 | 12:37:38.017 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
226 | 12:37:38.344 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
227 | 12:37:38.345 | →enobeB PCAP frame→ SIP over IPSEC: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 |  |  |  |
228 | 12:37:38.361 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
229 | 12:37:38.408 |  |  |  |  | ←SIP 200 OK | P-CSCF
230 | 12:37:38.408 |  |  |  |  | MIKEY | Media-Server
231 | 12:37:38.410 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
232 | 12:37:38.622 |  |  |  |  | XML→ | Media-Server
233 | 12:37:38.623 |  |  |  |  | XML→ | Media-Server
234 | 12:37:38.626 |  |  |  |  | ←XML | Media-Server
235 | 12:37:38.632 |  |  |  |  | ←SIP NOTIFY | P-CSCF
236 | 12:37:38.634 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:43206;transp... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
237 | 12:37:38.664 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK TLS: Mix Info |  |  |  |
238 | 12:37:38.666 |  |  |  |  | →SIP 200 OK | P-CSCF
239 | 12:37:39.024 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
240 | 12:37:39.028 |  | ←enobeB PCAP frame← TCP |  |  |
241 | 12:37:39.056 | →enobeB PCAP frame→ TCP |  |  |  |
242 | 12:37:39.064 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
243 | 12:37:39.070 |  | ←enobeB PCAP frame← TCP |  |  |
244 | 12:37:39.073 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
245 | 12:37:39.096 | →enobeB PCAP frame→ TCP |  |  |  |
246 | 12:37:39.184 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
247 | 12:37:39.187 |  | ←enobeB PCAP frame← TCP |  |  |
248 | 12:37:39.187 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:632: Client connected to Http Proxy port (id 26)
249 | 12:37:39.188 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
250 | 12:37:39.216 | →enobeB PCAP frame→ TCP |  |  |  |
251 | 12:37:39.224 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-co... |  |  |  |
252 | 12:37:39.227 |  | ←enobeB PCAP frame← TCP |  |  |
253 | 12:37:39.228 |  |  |  |  | →HTTP GET | HTTP-Proxy
254 | 12:37:39.239 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:568: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcptt-ue-configuration.xml
255 | 12:37:39.249 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
256 | 12:37:39.251 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
257 | 12:37:39.296 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
258 | 12:37:39.299 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:668: Http Proxy port - Client closed the connection (id 26)
259 | 12:37:39.300 |  | ←enobeB PCAP frame← TCP |  |  |
260 | 12:37:39.304 | →enobeB PCAP frame→ TCP |  |  |  |
261 | 12:37:39.307 |  | ←enobeB PCAP frame← TCP |  |  |
262 | 12:37:39.336 | →enobeB PCAP frame→ TCP |  |  |  |
263 | 12:37:39.456 | →enobeB PCAP frame→ TCP |  |  |  |
264 | 12:37:39.461 |  | ←enobeB PCAP frame← TCP |  |  |
265 | 12:37:39.496 | →enobeB PCAP frame→ TCP |  |  |  |
266 | 12:37:39.504 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
267 | 12:37:39.508 |  | ←enobeB PCAP frame← TCP |  |  |
268 | 12:37:39.511 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
269 | 12:37:39.536 | →enobeB PCAP frame→ TCP |  |  |  |
270 | 12:37:39.624 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
271 | 12:37:39.627 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:632: Client connected to Http Proxy port (id 26)
272 | 12:37:39.628 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
273 | 12:37:39.656 | →enobeB PCAP frame→ TCP |  |  |  |
274 | 12:37:39.664 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-... |  |  |  |
275 | 12:37:39.668 |  | ←enobeB PCAP frame← TCP |  |  |
276 | 12:37:39.668 |  |  |  |  | →HTTP GET | HTTP-Proxy
277 | 12:37:39.680 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:573: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcptt-user-profile-49.xml
278 | 12:37:39.714 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
279 | 12:37:39.719 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
280 | 12:37:39.719 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
281 | 12:37:39.737 | →enobeB PCAP frame→ TCP |  |  |  |
282 | 12:37:39.744 | →enobeB PCAP frame→ TCP |  |  |  |
283 | 12:37:39.776 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
284 | 12:37:39.779 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:668: Http Proxy port - Client closed the connection (id 26)
285 | 12:37:39.780 |  | ←enobeB PCAP frame← TCP |  |  |
286 | 12:37:39.784 | →enobeB PCAP frame→ TCP |  |  |  |
287 | 12:37:39.789 |  | ←enobeB PCAP frame← TCP |  |  |
288 | 12:37:39.816 | →enobeB PCAP frame→ TCP |  |  |  |
289 | 12:37:40.344 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
290 | 12:37:40.345 | →enobeB PCAP frame→ SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
291 | 12:37:40.407 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
292 | 12:37:40.426 |  |  |  |  | MIKEY | Media-Server
293 | 12:37:40.426 |  |  |  |  | ←SIP 200 OK | P-CSCF
294 | 12:37:40.427 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
295 | 12:37:40.496 | →enobeB PCAP frame→ TCP |  |  |  |
296 | 12:37:40.499 |  | ←enobeB PCAP frame← TCP |  |  |
297 | 12:37:40.536 | →enobeB PCAP frame→ TCP |  |  |  |
298 | 12:37:40.544 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
299 | 12:37:40.547 |  | ←enobeB PCAP frame← TCP |  |  |
300 | 12:37:40.548 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
301 | 12:37:40.576 | →enobeB PCAP frame→ TCP |  |  |  |
302 | 12:37:40.625 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
303 | 12:37:40.626 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:632: Client connected to Http Proxy port (id 26)
304 | 12:37:40.628 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
305 | 12:37:40.640 |  |  |  |  | XML→ | Media-Server
306 | 12:37:40.641 |  |  |  |  | XML→ | Media-Server
307 | 12:37:40.644 |  |  |  |  | ←XML | Media-Server
308 | 12:37:40.648 |  |  |  |  | ←SIP NOTIFY | P-CSCF
309 | 12:37:40.651 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:43206;transp... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
310 | 12:37:40.656 | →enobeB PCAP frame→ TCP |  |  |  |
311 | 12:37:40.664 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.servi... |  |  |  |
312 | 12:37:40.666 |  |  |  |  | →HTTP GET | HTTP-Proxy
313 | 12:37:40.667 |  | ←enobeB PCAP frame← TCP |  |  |
314 | 12:37:40.669 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:578: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
315 | 12:37:40.674 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
316 | 12:37:40.677 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
317 | 12:37:40.696 | →enobeB PCAP frame→ TCP |  |  |  |
318 | 12:37:40.704 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
319 | 12:37:40.707 |  |  |  |  | →SIP 200 OK | P-CSCF
320 | 12:37:40.736 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
321 | 12:37:40.739 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:668: Http Proxy port - Client closed the connection (id 26)
322 | 12:37:40.740 |  | ←enobeB PCAP frame← TCP |  |  |
323 | 12:37:40.745 | →enobeB PCAP frame→ TCP |  |  |  |
324 | 12:37:40.749 |  | ←enobeB PCAP frame← TCP |  |  |
325 | 12:37:40.776 | →enobeB PCAP frame→ TCP |  |  |  |
326 | 12:37:40.784 | →enobeB PCAP frame→ TCP |  |  |  |
327 | 12:37:40.788 |  | ←enobeB PCAP frame← TCP |  |  |
328 | 12:37:40.816 | →enobeB PCAP frame→ TCP |  |  |  |
329 | 12:37:40.824 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
330 | 12:37:40.828 |  | ←enobeB PCAP frame← TCP |  |  |
331 | 12:37:40.831 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
332 | 12:37:40.856 | →enobeB PCAP frame→ TCP |  |  |  |
333 | 12:37:40.944 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
334 | 12:37:40.947 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:632: Client connected to Http Proxy port (id 26)
335 | 12:37:40.948 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
336 | 12:37:40.976 | →enobeB PCAP frame→ TCP |  |  |  |
337 | 12:37:40.984 | →enobeB PCAP frame→ HTTPS: GET /xcap.gms.mcstaasting.com/org.openmobileallian... |  |  |  |
338 | 12:37:40.987 |  | ←enobeB PCAP frame← TCP |  |  |
339 | 12:37:40.988 |  |  |  |  | →HTTP GET | HTTP-Proxy
340 | 12:37:40.998 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:583: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at /xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
341 | 12:37:40.998 |  |  |  |  | Verdict PASS: MCPTT_ClientConfiguration_MCX_HTTP.ttcn:47: Parallel behaviour Verdict: Pass
342 | 12:37:41.019 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
343 | 12:37:41.022 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
344 | 12:37:41.023 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
345 | 12:37:41.057 | →enobeB PCAP frame→ TCP |  |  |  |
346 | 12:37:41.064 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
347 | 12:37:41.067 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:668: Http Proxy port - Client closed the connection (id 26)
348 | 12:37:41.068 |  | ←enobeB PCAP frame← TCP |  |  |
349 | 12:37:41.096 | →enobeB PCAP frame→ TCP |  |  |  |
350 | 12:37:41.464 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
351 | 12:37:41.465 | →enobeB PCAP frame→ SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
352 | 12:37:41.470 |  |  |  |  | →SIP PUBLISH | P-CSCF
353 | 12:37:41.481 |  |  |  |  | MIKEY | Media-Server
354 | 12:37:41.545 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
355 | 12:37:41.545 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
356 | 12:37:41.546 | →enobeB PCAP frame→ SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
357 | 12:37:41.551 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
358 | 12:37:41.696 |  |  |  |  | XML→ | Media-Server
359 | 12:37:41.699 |  |  |  |  | ←SIP 200 OK | P-CSCF
360 | 12:37:41.700 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
361 | 12:37:41.702 |  |  |  |  | ←SIP 200 OK | P-CSCF
362 | 12:37:41.702 |  |  |  |  | MIKEY | Media-Server
363 | 12:37:41.704 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
364 | 12:37:41.914 |  |  |  |  | XML→ | Media-Server
365 | 12:37:41.915 |  |  |  |  | XML→ | Media-Server
366 | 12:37:41.951 |  |  |  |  | ←XML | Media-Server
367 | 12:37:41.958 |  |  |  |  | ←SIP NOTIFY | P-CSCF
368 | 12:37:41.961 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
369 | 12:37:41.962 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:43206;transp... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
370 | 12:37:42.024 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
371 | 12:37:42.026 |  |  |  |  | →SIP 200 OK | P-CSCF
372 | 12:37:42.029 |  |  |  |  | Verdict PASS: MCPTT_ClientConfiguration_MCX_IMS.ttcn:73: TS 36.579-2 Table 5.1.3.2-1 Step 17 Verdict: Pass
373 | 12:37:42.030 |  |  |  |  | ←XML | Media-Server
374 | 12:37:42.037 |  |  |  |  | ←SIP MESSAGE | P-CSCF
375 | 12:37:42.040 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
376 | 12:37:42.824 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
377 | 12:37:42.826 |  |  |  |  | →SIP 200 OK | P-CSCF
378 | 12:37:42.828 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:1089: IdMPort to be closed id: 19
379 | 12:37:42.831 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
380 | 12:37:42.857 | →enobeB PCAP frame→ TCP |  |  |  |
381 | 12:37:42.896 | →enobeB PCAP frame→ TCP |  |  |  |
382 | 12:37:44.831 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
383 | 12:37:44.893 |  | ←RRC DCCH RRC Connection Release |  |  |
384 | 12:37:44.893 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
385 | 12:37:44.903 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
386 | 12:37:44.906 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
387 | 12:37:44.907 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
388 | 12:37:45.655 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.