MSG #72 2021-09-02 16:08:08.040
RRC

     DCCH: RRC Connection Reconfiguration
    {
      message c1: rrcConnectionReconfiguration: {
        rrc-TransactionIdentifier 0,
        criticalExtensions c1: rrcConnectionReconfiguration-r8: {
          dedicatedInfoNASList {
            '279F684A8702CA0B5A984824B6AC696E2657D04145FF38F4F909AC79CF2DC3A960B8E2EACE1C19B3BBF6441966B868BA57269E25FB8F4EB7351FA09A8ABDBB48577441125CCD3D6C5DC8CF4C12409DB3067E02C90435FBFFC2CD6DF70EECA8A41B5608B766E8DB35C70CD2FB5EF9B2059B37B57BD781480384AA8B0D1A301603B5F01861D0E2DCB0'H
          },
          radioResourceConfigDedicated {
            srb-ToAddModList {
              {
                srb-Identity 2,
                rlc-Config explicitValue: am: {
                  ul-AM-RLC {
                    t-PollRetransmit ms60,
                    pollPDU pInfinity,
                    pollByte kBinfinity,
                    maxRetxThreshold t32
                  },
                  dl-AM-RLC {
                    t-Reordering ms45,
                    t-StatusProhibit ms0
                  }
                },
                logicalChannelConfig defaultValue: NULL
              }
            },
            drb-ToAddModList {
              {
                eps-BearerIdentity 5,
                drb-Identity 1,
                pdcp-Config {
                  discardTimer infinity,
                  rlc-AM {
                    statusReportRequired TRUE
                  },
                  headerCompression notUsed: NULL
                },
                rlc-Config am: {
                  ul-AM-RLC {
                    t-PollRetransmit ms80,
                    pollPDU p128,
                    pollByte kB125,
                    maxRetxThreshold t4
                  },
                  dl-AM-RLC {
                    t-Reordering ms80,
                    t-StatusProhibit ms60
                  }
                },
                logicalChannelIdentity 3,
                logicalChannelConfig {
                  ul-SpecificParameters {
                    priority 4,
                    prioritisedBitRate kBps8,
                    bucketSizeDuration ms100,
                    logicalChannelGroup 1
                  }
                }
              }
            },
            physicalConfigDedicated {
              cqi-ReportConfig {
                nomPDSCH-RS-EPRE-Offset 0,
                cqi-ReportPeriodic setup: {
                  cqi-PUCCH-ResourceIndex 0,
                  cqi-pmi-ConfigIndex 38,
                  cqi-FormatIndicatorPeriodic widebandCQI: NULL,
                  simultaneousAckNackAndCQI TRUE
                }
              }
            }
          }
        }
      }
    }