ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 16:07:43.028 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 16:07:43.031 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 16:07:43.032 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 16:07:43.033 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 16:07:43.034 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 16:07:43.035 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:805: IMS UDP port 192.168.2.3:5060 configured
7 | 16:07:43.037 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:755: IMS TCP port 192.168.2.3:5060 configured!
8 | 16:07:43.039 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:776: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 16:07:43.039 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:787: IdM port 192.168.2.3:8080 configured!
10 | 16:07:43.041 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 16:07:44.243 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 16:07:44.244 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 16:07:44.582 |  | ←RRC BCCH SIB1 |  |  |
14 | 16:07:44.657 |  | ←RRC BCCH SIB |  |  |
15 | 16:07:44.662 |  | ←RRC BCCH SIB1 |  |  |
16 | 16:07:44.677 |  | ←RRC BCCH SIB |  |  |
17 | 16:07:44.697 |  | ←RRC BCCH SIB |  |  |
18 | 16:08:07.746 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 16:08:07.746 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 16:08:07.746 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 16:08:07.746 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 16:08:07.797 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 16:08:07.797 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 16:08:07.797 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 16:08:07.797 |  |  |  | →NAS EMM Attach request |  |
26 | 16:08:07.797 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 16:08:07.797 |  |  |  | NAS K-asme 905d3101544f6854fcdded4f57c26697... |  |
28 | 16:08:07.797 |  |  |  | NAS ← EMM Authentication request |  |
29 | 16:08:07.798 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 16:08:07.798 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 16:08:07.799 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 16:08:07.869 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 16:08:07.869 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 16:08:07.869 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 16:08:07.869 |  |  |  | →NAS EMM Authentication response |  |
36 | 16:08:07.869 |  |  |  | NAS UE auth OK |  |
37 | 16:08:07.869 |  |  |  | NAS K-nas-cip b4ff756fd50e4f68311fd11f1a838... |  |
38 | 16:08:07.869 |  |  |  | NAS K-nas-int 7281af3c192c5ee0c7f5a2032f8c6... |  |
39 | 16:08:07.869 |  |  |  | NAS ← EMM Security mode command |  |
40 | 16:08:07.870 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 16:08:07.870 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 16:08:07.871 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 16:08:07.909 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
44 | 16:08:07.909 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 16:08:07.909 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xc) |  |  |
46 | 16:08:07.909 |  |  |  | →NAS EMM Security mode complete |  |
47 | 16:08:07.909 |  |  |  | NAS ← ESM ESM information request |  |
48 | 16:08:07.910 |  | [EMBEDDED NAS IN NEXT RRC] TP Unknown message (type=0xa9) |  |  |
49 | 16:08:07.910 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 16:08:07.911 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
51 | 16:08:07.957 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer |  |  |  |
52 | 16:08:07.957 |  | →RRC DCCH UL Information Transfer |  |  |
53 | 16:08:07.957 |  | [EMBEDDED NAS IN PREV RRC] ESM Unknown message (type=0xad) |  |  |
54 | 16:08:07.957 |  |  |  | →NAS ESM ESM information response |  |
55 | 16:08:07.957 |  |  |  | NAS K-enb 582b6461acef7528bbac35ed6d50b9d07... |  |
56 | 16:08:07.957 |  |  |  | NAS ← EMM Attach accept |  |
57 | 16:08:07.958 |  | ←RRC DCCH Security Mode Command |  |  |
58 | 16:08:07.958 |  |  | RRC K-enb 582b6461acef7528bbac35ed6d50b9d07... |  |  |
59 | 16:08:07.958 |  |  | RRC rrc-cip a1689f6c2d56be1dab5dba4208660bd... |  |  |
60 | 16:08:07.958 |  |  | RRC rrc-int effd66a36f37bdf59215f09b953aefb... |  |  |
61 | 16:08:07.958 |  |  | RRC up-cip 0240390b659b25b3c624d8d473e0798b... |  |  |
62 | 16:08:07.958 |  |  | RRC up-int a91adadd2214334c0b16350d18e6ef0d... |  |  |
63 | 16:08:07.959 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
64 | 16:08:07.967 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
65 | 16:08:07.989 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
66 | 16:08:07.989 |  | →RRC DCCH Security Mode Complete |  |  |
67 | 16:08:07.989 |  | ←RRC DCCH UE Capability Enquiry |  |  |
68 | 16:08:07.989 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
69 | 16:08:08.039 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
70 | 16:08:08.039 |  | →RRC DCCH UE Capability Information |  |  |
71 | 16:08:08.040 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xa) |  |  |
72 | 16:08:08.040 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
73 | 16:08:08.040 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
74 | 16:08:08.069 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
75 | 16:08:08.069 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
76 | 16:08:08.109 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
77 | 16:08:08.109 |  | →RRC DCCH UL Information Transfer |  |  |
78 | 16:08:08.109 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x4) |  |  |
79 | 16:08:08.109 |  |  |  | →NAS EMM Attach complete |  |
80 | 16:08:08.109 |  |  |  | NAS ← EMM EMM information |  |
81 | 16:08:08.110 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xc) |  |  |
82 | 16:08:08.110 |  | ←RRC DCCH DL Information Transfer |  |  |
83 | 16:08:08.111 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
84 | 16:08:11.321 |  | ←RRC DCCH RRC Connection Release |  |  |
85 | 16:08:11.322 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
86 | 16:08:13.676 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
87 | 16:08:13.676 |  | →RRC CCCH RRC Connection Request |  |  |
88 | 16:08:13.676 |  | ←RRC CCCH RRC Connection Setup |  |  |
89 | 16:08:13.676 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
90 | 16:08:13.709 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
91 | 16:08:13.709 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
92 | 16:08:13.709 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
93 | 16:08:13.709 |  |  |  | →NAS EMM Service request |  |
94 | 16:08:13.709 |  |  |  | NAS K-enb 0fb02e0ec78d34f9ff3502b087568ec21... |  |
95 | 16:08:13.710 |  |  | RRC K-enb 0fb02e0ec78d34f9ff3502b087568ec21... |  |  |
96 | 16:08:13.711 |  |  | RRC rrc-cip 5e2e528e9dc9d16688b7ef50a97829a... |  |  |
97 | 16:08:13.711 |  |  | RRC rrc-int beb07caac47adfc367374d0db660598... |  |  |
98 | 16:08:13.711 |  |  | RRC up-cip b66ebbe68f66e590cd66b5a97f7be379... |  |  |
99 | 16:08:13.711 |  |  | RRC up-int 0c526850d7b16266bb17f5b5b6933b3f... |  |  |
100 | 16:08:13.711 |  | ←RRC DCCH Security Mode Command |  |  |
101 | 16:08:13.711 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
102 | 16:08:13.749 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
103 | 16:08:13.749 |  | →RRC DCCH Security Mode Complete |  |  |
104 | 16:08:13.749 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
105 | 16:08:13.749 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
106 | 16:08:13.789 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
107 | 16:08:13.789 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
108 | 16:08:31.509 | →enobeB PCAP frame→ TCP |  |  |  |
109 | 16:08:31.512 |  | ←enobeB PCAP frame← TCP |  |  |
110 | 16:08:31.549 | →enobeB PCAP frame→ TCP |  |  |  |
111 | 16:08:31.637 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
112 | 16:08:31.640 |  | ←enobeB PCAP frame← TCP |  |  |
113 | 16:08:31.646 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
114 | 16:08:31.669 | →enobeB PCAP frame→ TCP |  |  |  |
115 | 16:08:31.797 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
116 | 16:08:31.799 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 16)
117 | 16:08:31.800 |  | ←enobeB PCAP frame← TCP |  |  |
118 | 16:08:31.801 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
119 | 16:08:31.829 | →enobeB PCAP frame→ TCP |  |  |  |
120 | 16:08:31.877 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
121 | 16:08:31.878 |  |  |  |  | →HTTP GET | HTTP-Proxy
122 | 16:08:31.880 |  | ←enobeB PCAP frame← TCP |  |  |
123 | 16:08:31.885 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:288: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
124 | 16:08:31.903 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
125 | 16:08:31.908 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
126 | 16:08:31.949 | →enobeB PCAP frame→ TCP |  |  |  |
127 | 16:08:33.749 | →enobeB PCAP frame→ TCP |  |  |  |
128 | 16:08:33.752 |  | ←enobeB PCAP frame← TCP |  |  |
129 | 16:08:33.789 | →enobeB PCAP frame→ TCP |  |  |  |
130 | 16:08:33.797 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
131 | 16:08:33.800 |  | ←enobeB PCAP frame← TCP |  |  |
132 | 16:08:33.805 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
133 | 16:08:33.829 | →enobeB PCAP frame→ TCP |  |  |  |
134 | 16:08:34.117 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
135 | 16:08:34.119 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:642: Client connected to IdM port (id 18)
136 | 16:08:34.120 |  | ←enobeB PCAP frame← TCP |  |  |
137 | 16:08:34.121 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
138 | 16:08:34.149 | →enobeB PCAP frame→ TCP |  |  |  |
139 | 16:08:34.157 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
140 | 16:08:34.159 |  |  |  |  | →HTTP GET | IDMS-Endpoint
141 | 16:08:34.160 |  | ←enobeB PCAP frame← TCP |  |  |
142 | 16:08:34.214 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
143 | 16:08:34.217 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:511: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
144 | 16:08:34.218 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
145 | 16:08:34.218 |  |  |  |  | MMICmd: Please provide user credentials: username and password
146 | 16:08:34.309 | →enobeB PCAP frame→ TCP |  |  |  |
147 | 16:08:38.837 | →enobeB PCAP frame→ HTTPS: POST /idms/userauth HTTP/1.1 |  |  |  |
148 | 16:08:38.840 |  | ←enobeB PCAP frame← TCP |  |  |
149 | 16:08:38.840 |  |  |  |  | →HTTP POST | IDMS-Endpoint
150 | 16:08:38.854 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
151 | 16:08:38.857 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
152 | 16:08:38.857 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:516: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
153 | 16:08:38.909 | →enobeB PCAP frame→ TCP |  |  |  |
154 | 16:08:38.917 | →enobeB PCAP frame→ TCP |  |  |  |
155 | 16:08:38.918 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:677: IdM port - Client closed the connection (id 18)
156 | 16:08:38.920 |  | ←enobeB PCAP frame← TCP |  |  |
157 | 16:08:38.949 | →enobeB PCAP frame→ TCP |  |  |  |
158 | 16:08:39.629 | →enobeB PCAP frame→ TCP |  |  |  |
159 | 16:08:39.632 |  | ←enobeB PCAP frame← TCP |  |  |
160 | 16:08:39.669 | →enobeB PCAP frame→ TCP |  |  |  |
161 | 16:08:39.757 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
162 | 16:08:39.760 |  | ←enobeB PCAP frame← TCP |  |  |
163 | 16:08:39.766 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
164 | 16:08:39.789 | →enobeB PCAP frame→ TCP |  |  |  |
165 | 16:08:39.837 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
166 | 16:08:39.839 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:642: Client connected to IdM port (id 18)
167 | 16:08:39.840 |  | ←enobeB PCAP frame← TCP |  |  |
168 | 16:08:39.841 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
169 | 16:08:39.869 | →enobeB PCAP frame→ TCP |  |  |  |
170 | 16:08:39.877 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
171 | 16:08:39.879 |  |  |  |  | →HTTP POST | IDMS-Endpoint
172 | 16:08:39.880 |  | ←enobeB PCAP frame← TCP |  |  |
173 | 16:08:39.907 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
174 | 16:08:39.909 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:521: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
175 | 16:08:39.910 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
176 | 16:08:39.989 | →enobeB PCAP frame→ TCP |  |  |  |
177 | 16:08:40.229 | →enobeB PCAP frame→ TCP |  |  |  |
178 | 16:08:40.232 |  | ←enobeB PCAP frame← TCP |  |  |
179 | 16:08:40.269 | →enobeB PCAP frame→ TCP |  |  |  |
180 | 16:08:40.277 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
181 | 16:08:40.280 |  | ←enobeB PCAP frame← TCP |  |  |
182 | 16:08:40.283 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
183 | 16:08:40.309 | →enobeB PCAP frame→ TCP |  |  |  |
184 | 16:08:40.317 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
185 | 16:08:40.319 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 19)
186 | 16:08:40.320 |  | ←enobeB PCAP frame← TCP |  |  |
187 | 16:08:40.321 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
188 | 16:08:40.357 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
189 | 16:08:40.360 |  | ←enobeB PCAP frame← TCP |  |  |
190 | 16:08:40.360 |  |  |  |  | →HTTP POST | HTTP-Proxy
191 | 16:08:40.383 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:541: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
192 | 16:08:40.390 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
193 | 16:08:40.394 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
194 | 16:08:40.429 | →enobeB PCAP frame→ TCP |  |  |  |
195 | 16:08:40.469 | →enobeB PCAP frame→ TCP |  |  |  |
196 | 16:08:40.472 |  | ←enobeB PCAP frame← TCP |  |  |
197 | 16:08:40.509 | →enobeB PCAP frame→ TCP |  |  |  |
198 | 16:08:40.517 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
199 | 16:08:40.520 |  | ←enobeB PCAP frame← TCP |  |  |
200 | 16:08:40.524 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
201 | 16:08:40.589 | →enobeB PCAP frame→ TCP |  |  |  |
202 | 16:08:40.597 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
203 | 16:08:40.599 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 20)
204 | 16:08:40.600 |  | ←enobeB PCAP frame← TCP |  |  |
205 | 16:08:40.601 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
206 | 16:08:40.637 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
207 | 16:08:40.640 |  | ←enobeB PCAP frame← TCP |  |  |
208 | 16:08:40.640 |  |  |  |  | →HTTP POST | HTTP-Proxy
209 | 16:08:40.703 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
210 | 16:08:40.703 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:545: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
211 | 16:08:40.706 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
212 | 16:08:40.749 | →enobeB PCAP frame→ TCP |  |  |  |
213 | 16:08:40.797 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
214 | 16:08:40.801 |  |  |  |  | →SIP REGISTER | P-CSCF
215 | 16:08:40.822 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:814: IMS UDP_s port 192.168.2.3:5062 configured
216 | 16:08:40.837 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:765: IMS TCP_s port 192.168.2.3:5062 configured!
217 | 16:08:40.838 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:823: IMS UDP_c port 192.168.2.3:5061 configured
218 | 16:08:40.842 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
219 | 16:08:41.557 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
220 | 16:08:41.561 |  |  |  |  | →SIP REGISTER | P-CSCF
221 | 16:08:41.584 |  |  |  |  | ←SIP 200 OK | P-CSCF
222 | 16:08:41.588 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
223 | 16:08:41.917 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
224 | 16:08:41.918 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
225 | 16:08:41.919 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 SIP over IPSEC: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 |  |  |  |
226 | 16:08:41.932 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
227 | 16:08:41.990 |  |  |  |  | ←SIP 200 OK | P-CSCF
228 | 16:08:41.990 |  |  |  |  | MIKEY | Media-Server
229 | 16:08:41.993 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
230 | 16:08:42.222 |  |  |  |  | XML→ | Media-Server
231 | 16:08:42.288 |  |  |  |  | XML→ | Media-Server
232 | 16:08:42.301 |  |  |  |  | ←XML | Media-Server
233 | 16:08:42.314 |  |  |  |  | ←SIP NOTIFY | P-CSCF
234 | 16:08:42.318 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:43009;transp... |  |  |
235 | 16:08:42.357 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
236 | 16:08:42.359 |  |  |  |  | →SIP 200 OK | P-CSCF
237 | 16:08:42.589 | →enobeB PCAP frame→ TCP |  |  |  |
238 | 16:08:42.592 |  | ←enobeB PCAP frame← TCP |  |  |
239 | 16:08:42.629 | →enobeB PCAP frame→ TCP |  |  |  |
240 | 16:08:42.637 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
241 | 16:08:42.640 |  | ←enobeB PCAP frame← TCP |  |  |
242 | 16:08:42.644 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
243 | 16:08:42.669 | →enobeB PCAP frame→ TCP |  |  |  |
244 | 16:08:42.757 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
245 | 16:08:42.758 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
246 | 16:08:42.760 |  | ←enobeB PCAP frame← TCP |  |  |
247 | 16:08:42.761 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
248 | 16:08:42.789 | →enobeB PCAP frame→ TCP |  |  |  |
249 | 16:08:42.797 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-co... |  |  |  |
250 | 16:08:42.799 |  |  |  |  | →HTTP GET | HTTP-Proxy
251 | 16:08:42.800 |  | ←enobeB PCAP frame← TCP |  |  |
252 | 16:08:42.807 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:642: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcptt-ue-configuration.xml
253 | 16:08:42.815 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
254 | 16:08:42.819 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
255 | 16:08:42.869 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
256 | 16:08:42.870 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
257 | 16:08:42.872 |  | ←enobeB PCAP frame← TCP |  |  |
258 | 16:08:42.877 | →enobeB PCAP frame→ TCP |  |  |  |
259 | 16:08:42.880 |  | ←enobeB PCAP frame← TCP |  |  |
260 | 16:08:42.909 | →enobeB PCAP frame→ TCP |  |  |  |
261 | 16:08:43.029 | →enobeB PCAP frame→ TCP |  |  |  |
262 | 16:08:43.032 |  | ←enobeB PCAP frame← TCP |  |  |
263 | 16:08:43.069 | →enobeB PCAP frame→ TCP |  |  |  |
264 | 16:08:43.077 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
265 | 16:08:43.080 |  | ←enobeB PCAP frame← TCP |  |  |
266 | 16:08:43.086 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
267 | 16:08:43.109 | →enobeB PCAP frame→ TCP |  |  |  |
268 | 16:08:43.157 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
269 | 16:08:43.158 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
270 | 16:08:43.160 |  | ←enobeB PCAP frame← TCP |  |  |
271 | 16:08:43.161 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
272 | 16:08:43.237 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-... |  |  |  |
273 | 16:08:43.239 |  |  |  |  | →HTTP GET | HTTP-Proxy
274 | 16:08:43.240 |  | ←enobeB PCAP frame← TCP |  |  |
275 | 16:08:43.253 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:647: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcptt-user-profile-49.xml
276 | 16:08:43.292 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
277 | 16:08:43.300 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
278 | 16:08:43.301 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
279 | 16:08:43.349 | →enobeB PCAP frame→ TCP |  |  |  |
280 | 16:08:43.357 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
281 | 16:08:43.358 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
282 | 16:08:43.360 |  | ←enobeB PCAP frame← TCP |  |  |
283 | 16:08:43.389 | →enobeB PCAP frame→ TCP |  |  |  |
284 | 16:08:43.997 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
285 | 16:08:43.998 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
286 | 16:08:44.006 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
287 | 16:08:44.058 |  |  |  |  | ←SIP 200 OK | P-CSCF
288 | 16:08:44.058 |  |  |  |  | MIKEY | Media-Server
289 | 16:08:44.061 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
290 | 16:08:44.109 | →enobeB PCAP frame→ TCP |  |  |  |
291 | 16:08:44.112 |  | ←enobeB PCAP frame← TCP |  |  |
292 | 16:08:44.149 | →enobeB PCAP frame→ TCP |  |  |  |
293 | 16:08:44.157 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
294 | 16:08:44.160 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
295 | 16:08:44.189 | →enobeB PCAP frame→ TCP |  |  |  |
296 | 16:08:44.277 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
297 | 16:08:44.277 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
298 | 16:08:44.280 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
299 | 16:08:44.288 |  |  |  |  | XML→ | Media-Server
300 | 16:08:44.289 |  |  |  |  | XML→ | Media-Server
301 | 16:08:44.292 |  |  |  |  | ←XML | Media-Server
302 | 16:08:44.295 |  |  |  |  | ←SIP NOTIFY | P-CSCF
303 | 16:08:44.298 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:43009;transp... |  |  |
304 | 16:08:44.309 | →enobeB PCAP frame→ TCP |  |  |  |
305 | 16:08:44.317 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.servi... |  |  |  |
306 | 16:08:44.318 |  |  |  |  | →HTTP GET | HTTP-Proxy
307 | 16:08:44.320 |  | ←enobeB PCAP frame← TCP |  |  |
308 | 16:08:44.324 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:652: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
309 | 16:08:44.338 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
310 | 16:08:44.341 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
311 | 16:08:44.342 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
312 | 16:08:44.342 |  |  |  |  | →SIP 200 OK | P-CSCF
313 | 16:08:44.343 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
314 | 16:08:44.389 | →enobeB PCAP frame→ TCP |  |  |  |
315 | 16:08:44.397 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
316 | 16:08:44.398 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
317 | 16:08:44.400 |  | ←enobeB PCAP frame← TCP |  |  |
318 | 16:08:44.429 | →enobeB PCAP frame→ TCP |  |  |  |
319 | 16:08:44.469 | →enobeB PCAP frame→ TCP |  |  |  |
320 | 16:08:44.472 |  | ←enobeB PCAP frame← TCP |  |  |
321 | 16:08:44.509 | →enobeB PCAP frame→ TCP |  |  |  |
322 | 16:08:44.517 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
323 | 16:08:44.520 |  | ←enobeB PCAP frame← TCP |  |  |
324 | 16:08:44.523 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
325 | 16:08:44.549 | →enobeB PCAP frame→ TCP |  |  |  |
326 | 16:08:44.637 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
327 | 16:08:44.639 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
328 | 16:08:44.640 |  | ←enobeB PCAP frame← TCP |  |  |
329 | 16:08:44.641 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
330 | 16:08:44.669 | →enobeB PCAP frame→ TCP |  |  |  |
331 | 16:08:44.677 | →enobeB PCAP frame→ HTTPS: GET /xcap.gms.mcstaasting.com/org.openmobileallian... |  |  |  |
332 | 16:08:44.679 |  |  |  |  | →HTTP GET | HTTP-Proxy
333 | 16:08:44.680 |  | ←enobeB PCAP frame← TCP |  |  |
334 | 16:08:44.688 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:657: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at /xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
335 | 16:08:44.705 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
336 | 16:08:44.709 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
337 | 16:08:44.749 | →enobeB PCAP frame→ TCP |  |  |  |
338 | 16:08:44.789 | →enobeB PCAP frame→ TCP |  |  |  |
339 | 16:08:44.797 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
340 | 16:08:44.798 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
341 | 16:08:44.800 |  | ←enobeB PCAP frame← TCP |  |  |
342 | 16:08:44.829 | →enobeB PCAP frame→ TCP |  |  |  |
343 | 16:08:44.997 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
344 | 16:08:44.998 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
345 | 16:08:44.999 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
346 | 16:08:45.002 |  |  |  |  | →SIP PUBLISH | P-CSCF
347 | 16:08:45.013 |  |  |  |  | MIKEY | Media-Server
348 | 16:08:45.077 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
349 | 16:08:45.078 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
350 | 16:08:45.079 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
351 | 16:08:45.082 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
352 | 16:08:45.236 |  |  |  |  | XML→ | Media-Server
353 | 16:08:45.240 |  |  |  |  | ←SIP 200 OK | P-CSCF
354 | 16:08:45.243 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
355 | 16:08:45.243 |  |  |  |  | ←SIP 200 OK | P-CSCF
356 | 16:08:45.243 |  |  |  |  | MIKEY | Media-Server
357 | 16:08:45.246 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
358 | 16:08:45.464 |  |  |  |  | XML→ | Media-Server
359 | 16:08:45.465 |  |  |  |  | XML→ | Media-Server
360 | 16:08:45.502 |  |  |  |  | ←XML | Media-Server
361 | 16:08:45.506 |  |  |  |  | ←SIP NOTIFY | P-CSCF
362 | 16:08:45.526 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:43009;transp... |  |  |
363 | 16:08:45.557 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
364 | 16:08:45.558 |  |  |  |  | →SIP 200 OK | P-CSCF
365 | 16:08:45.560 |  |  |  |  | ←XML | Media-Server
366 | 16:08:45.567 |  |  |  |  | ←SIP MESSAGE | P-CSCF
367 | 16:08:45.571 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
368 | 16:08:46.397 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
369 | 16:08:46.399 |  |  |  |  | →SIP 200 OK | P-CSCF
370 | 16:08:46.408 |  |  |  |  | Info: MCX_IMS_CommonProcedures.ttcn:155: MESSAGE/200OK Table 5.3.2.3-2 Steps 7-8 Done
371 | 16:08:46.412 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
372 | 16:08:46.429 | →enobeB PCAP frame→ TCP |  |  |  |
373 | 16:08:46.509 | →enobeB PCAP frame→ TCP |  |  |  |
374 | 16:08:48.410 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
375 | 16:08:48.455 |  | ←RRC DCCH RRC Connection Release |  |  |
376 | 16:08:48.456 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
377 | 16:08:48.474 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
378 | 16:08:48.480 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:735: SRTP config: Master Key: 5E546436466B561881B1F75C1A12021E, Master Salt: 1B5ECBE52896392C212C2334, MKI: 2E9AC63D
379 | 16:08:48.480 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
380 | 16:08:48.482 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
381 | 16:08:48.484 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
382 | 16:08:48.497 |  |  |  |  | ←XML | Media-Server
383 | 16:08:48.497 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
384 | 16:08:48.526 |  |  |  |  | ←SIP INVITE | P-CSCF
385 | 16:08:49.196 |  | ←enobeB PCAP frame← LTE RRC PCCH Paging (1 PagingRecord) |  |  |
386 | 16:08:49.196 |  | ←RRC PCCH Paging |  |  |
387 | 16:08:49.236 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
388 | 16:08:49.236 |  | →RRC CCCH RRC Connection Request |  |  |
389 | 16:08:49.236 |  | ←RRC CCCH RRC Connection Setup |  |  |
390 | 16:08:49.236 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
391 | 16:08:49.269 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
392 | 16:08:49.269 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
393 | 16:08:49.269 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
394 | 16:08:49.269 |  |  |  | →NAS EMM Service request |  |
395 | 16:08:49.269 |  |  |  | NAS K-enb bc59b74456d77c9e226fd9c60b0f164e0... |  |
396 | 16:08:49.270 |  |  | RRC K-enb bc59b74456d77c9e226fd9c60b0f164e0... |  |  |
397 | 16:08:49.270 |  |  | RRC rrc-cip 0e85843dc7a2d5fd49509800fdc51e0... |  |  |
398 | 16:08:49.270 |  |  | RRC rrc-int 17a7e61443748a1c94734241de85d03... |  |  |
399 | 16:08:49.270 |  |  | RRC up-cip bb0175365b588c8706c7a43382b442d5... |  |  |
400 | 16:08:49.270 |  |  | RRC up-int 264692a4ab7c90a03ae5becba5ce70a0... |  |  |
401 | 16:08:49.270 |  | ←RRC DCCH Security Mode Command |  |  |
402 | 16:08:49.270 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
403 | 16:08:49.309 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
404 | 16:08:49.309 |  | →RRC DCCH Security Mode Complete |  |  |
405 | 16:08:49.309 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
406 | 16:08:49.309 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
407 | 16:08:49.349 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
408 | 16:08:49.349 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
409 | 16:08:49.351 |  | ←enobeB PCAP frame← SIP over IPSEC: INVITE sip:PublicUserId-A@192.168.3.2:43009;transp... |  |  |
410 | 16:08:49.397 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 100 Trying |  |  |  |
411 | 16:08:49.399 |  |  |  |  | →SIP 100 Trying | P-CSCF
412 | 16:08:49.437 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
413 | 16:08:49.440 |  |  |  |  | →SIP 200 OK | P-CSCF
414 | 16:08:49.451 |  |  |  |  | XML→ | Media-Server
415 | 16:08:49.454 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:612: 200 OK Verdict: Pass
416 | 16:08:49.454 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:47: Step 1 Verdict: Pass
417 | 16:08:49.455 |  |  |  |  | ←SIP ACK | P-CSCF
418 | 16:08:49.458 |  | ←enobeB PCAP frame← SIP over IPSEC: ACK sip:PublicUserId-A@192.168.3.2:43009;transport... |  |  |
419 | 16:08:49.555 |  |  |  |  | MMICmd: Request PTT token
420 | 16:08:49.802 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
421 | 16:08:49.803 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x6) |  |  |
422 | 16:08:49.803 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
423 | 16:08:49.804 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
424 | 16:08:49.829 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
425 | 16:08:49.829 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
426 | 16:08:49.869 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
427 | 16:08:49.869 |  | →RRC DCCH UL Information Transfer |  |  |
428 | 16:08:49.869 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x4) |  |  |
429 | 16:08:49.869 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
430 | 16:08:49.924 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
431 | 16:08:51.149 | →enobeB PCAP frame→ |  |  |  |
432 | 16:08:51.149 |  |  |  |  | Floor Request→ | Media-Server
433 | 16:08:51.151 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Request Verdict: Pass
434 | 16:08:51.152 |  |  |  |  | ←Floor Granted | Media-Server
435 | 16:08:51.189 | →enobeB PCAP frame→ |  |  |  |
436 | 16:08:51.189 |  |  |  |  | Floor ACK→ | Media-Server
437 | 16:08:51.191 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
438 | 16:08:51.191 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:56: Step 11 Verdict: Pass
439 | 16:08:51.192 |  |  |  |  | ←Floor Revoke | Media-Server
440 | 16:08:51.229 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
441 | 16:08:51.237 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
442 | 16:08:51.245 | →enobeB PCAP frame→ |  |  |  |
443 | 16:08:51.245 |  |  |  |  | Floor Release→ | Media-Server
444 | 16:08:51.247 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
445 | 16:08:51.247 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:67: Step 17 Verdict: Pass
446 | 16:08:51.248 |  |  |  |  | ←Floor Taken | Media-Server
447 | 16:08:51.997 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:70: Table 6.1.1.2.3.2-2: Parallel Behaviour Verdict: Pass
448 | 16:08:52.099 |  |  |  |  | MMICmd: Request PTT token
449 | 16:08:53.749 | →enobeB PCAP frame→ |  |  |  |
450 | 16:08:53.750 |  |  |  |  | Floor Request→ | Media-Server
451 | 16:08:53.753 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Request Verdict: Pass
452 | 16:08:53.754 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:81: Step 20 Verdict: Pass
453 | 16:08:53.757 |  |  |  |  | ←Floor Deny | Media-Server
454 | 16:08:53.856 |  |  |  |  | MMICmd: Request PTT token
455 | 16:08:55.709 | →enobeB PCAP frame→ |  |  |  |
456 | 16:08:55.710 |  |  |  |  | Floor Request→ | Media-Server
457 | 16:08:55.712 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Request Verdict: Pass
458 | 16:08:55.713 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:90: Step 24 Verdict: Pass
459 | 16:08:55.715 |  |  |  |  | ←Floor Queue Position Info | Media-Server
460 | 16:08:56.463 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:95: Step 26 Verdict: Pass
461 | 16:08:56.464 |  |  |  |  | MMICmd: Make the MCPTT User request the current position in the queue
462 | 16:08:59.029 | →enobeB PCAP frame→ |  |  |  |
463 | 16:08:59.029 |  |  |  |  | Floor Queue Position Request→ | Media-Server
464 | 16:08:59.031 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Position Request Verdict: Pass
465 | 16:08:59.031 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:102: Step 28 Verdict: Pass
466 | 16:08:59.032 |  |  |  |  | ←Floor Queue Position Info | Media-Server
467 | 16:08:59.781 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:105: Step 28A Verdict: Pass
468 | 16:08:59.882 |  |  |  |  | MMICmd: Release PTT token
469 | 16:09:02.469 | →enobeB PCAP frame→ |  |  |  |
470 | 16:09:02.469 |  |  |  |  | Floor Release→ | Media-Server
471 | 16:09:02.471 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
472 | 16:09:02.472 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:114: Step 31 Verdict: Pass
473 | 16:09:02.473 |  |  |  |  | ←Floor Taken | Media-Server
474 | 16:09:02.573 |  |  |  |  | MMICmd: Request PTT token
475 | 16:09:03.829 | →enobeB PCAP frame→ |  |  |  |
476 | 16:09:03.830 |  |  |  |  | Floor Request→ | Media-Server
477 | 16:09:03.833 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Request Verdict: Pass
478 | 16:09:03.834 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:123: Step 34 Verdict: Pass
479 | 16:09:03.837 |  |  |  |  | ←Floor Queue Position Info | Media-Server
480 | 16:09:04.584 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:128: Step 36 Verdict: Pass
481 | 16:09:04.588 |  |  |  |  | ←Floor Granted | Media-Server
482 | 16:09:04.629 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
483 | 16:09:04.669 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
484 | 16:09:04.677 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
485 | 16:09:04.709 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
486 | 16:09:04.717 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
487 | 16:09:05.335 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:134: Step 38 Verdict: Pass
488 | 16:09:05.437 |  |  |  |  | MMICmd: Release PTT token
489 | 16:09:07.069 | →enobeB PCAP frame→ |  |  |  |
490 | 16:09:07.070 |  |  |  |  | Floor Release→ | Media-Server
491 | 16:09:07.072 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
492 | 16:09:07.073 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:141: Step 40 Verdict: Pass
493 | 16:09:07.076 |  |  |  |  | ←Floor Idle | Media-Server
494 | 16:09:07.077 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
495 | 16:09:07.080 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
496 | 16:09:07.178 |  |  |  |  | MMICmd: Release call (hang up the call)
497 | 16:09:10.397 | →enobeB PCAP frame→ SIP over IPSEC: BYE sip:mcptt-server-A@mcstaasting.com:6543 SIP/2.... |  |  |  |
498 | 16:09:10.401 |  |  |  |  | →SIP BYE | P-CSCF
499 | 16:09:10.420 |  |  |  |  | ←SIP 200 OK | P-CSCF
500 | 16:09:10.423 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
501 | 16:09:10.669 | →enobeB PCAP frame→ |  |  |  |
502 | 16:09:12.418 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
503 | 16:09:12.423 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
504 | 16:09:12.423 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x1) |  |  |
505 | 16:09:12.423 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
506 | 16:09:12.424 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
507 | 16:09:12.469 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
508 | 16:09:12.469 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
509 | 16:09:12.469 |  | →RRC DCCH UL Information Transfer |  |  |
510 | 16:09:12.469 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xb) |  |  |
511 | 16:09:12.469 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
512 | 16:09:12.542 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
513 | 16:09:12.543 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
514 | 16:09:12.592 |  | ←RRC DCCH RRC Connection Release |  |  |
515 | 16:09:12.593 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
516 | 16:09:12.601 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
517 | 16:09:12.602 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:148: Step 44 Verdict: Pass
518 | 16:09:12.606 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
519 | 16:09:12.608 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
520 | 16:09:12.622 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
521 | 16:09:12.623 |  |  |  |  | ←XML | Media-Server
522 | 16:09:12.658 |  |  |  |  | ←SIP INVITE | P-CSCF
523 | 16:09:13.516 |  | ←enobeB PCAP frame← LTE RRC PCCH Paging (1 PagingRecord) |  |  |
524 | 16:09:13.516 |  | ←RRC PCCH Paging |  |  |
525 | 16:09:13.546 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
526 | 16:09:13.546 |  | →RRC CCCH RRC Connection Request |  |  |
527 | 16:09:13.546 |  | ←RRC CCCH RRC Connection Setup |  |  |
528 | 16:09:13.546 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
529 | 16:09:13.589 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
530 | 16:09:13.589 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
531 | 16:09:13.589 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
532 | 16:09:13.589 |  |  |  | →NAS EMM Service request |  |
533 | 16:09:13.589 |  |  |  | NAS K-enb 454d94bfa10ce65c4da9ccc8d720a0324... |  |
534 | 16:09:13.590 |  |  | RRC K-enb 454d94bfa10ce65c4da9ccc8d720a0324... |  |  |
535 | 16:09:13.591 |  |  | RRC rrc-cip c734545ef76d7abb20ba58fd3778d3b... |  |  |
536 | 16:09:13.591 |  |  | RRC rrc-int 872a8b4f361424653586e2eef8e392f... |  |  |
537 | 16:09:13.591 |  |  | RRC up-cip 061fac018da67b731b89bd3fc1bd291b... |  |  |
538 | 16:09:13.591 |  |  | RRC up-int a9f024db5f17b3e3e50e2d50cc195b54... |  |  |
539 | 16:09:13.591 |  | ←RRC DCCH Security Mode Command |  |  |
540 | 16:09:13.591 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
541 | 16:09:13.629 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
542 | 16:09:13.629 |  | →RRC DCCH Security Mode Complete |  |  |
543 | 16:09:13.629 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
544 | 16:09:13.629 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
545 | 16:09:13.669 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
546 | 16:09:13.669 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
547 | 16:09:13.671 |  | ←enobeB PCAP frame← SIP over IPSEC: INVITE sip:PublicUserId-A@192.168.3.2:43009;transp... |  |  |
548 | 16:09:13.717 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 100 Trying |  |  |  |
549 | 16:09:13.719 |  |  |  |  | →SIP 100 Trying | P-CSCF
550 | 16:09:13.757 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
551 | 16:09:13.764 |  |  |  |  | →SIP 200 OK | P-CSCF
552 | 16:09:13.795 |  |  |  |  | XML→ | Media-Server
553 | 16:09:13.803 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:612: 200 OK Verdict: Pass
554 | 16:09:13.803 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:154: Step 46 Verdict: Pass
555 | 16:09:13.806 |  |  |  |  | ←XML | Media-Server
556 | 16:09:13.808 |  |  |  |  | ←SIP ACK | P-CSCF
557 | 16:09:13.809 |  |  |  |  | ←Floor Taken | Media-Server
558 | 16:09:13.812 |  | ←enobeB PCAP frame← SIP over IPSEC: ACK sip:PublicUserId-A@192.168.3.2:43009;transport... |  |  |
559 | 16:09:13.830 |  |  |  |  | ←SIP INVITE | P-CSCF
560 | 16:09:13.834 |  | ←enobeB PCAP frame← SIP over IPSEC: INVITE sip:PublicUserId-A@192.168.3.2:43009;transp... |  |  |
561 | 16:09:14.088 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
562 | 16:09:14.089 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x5) |  |  |
563 | 16:09:14.089 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
564 | 16:09:14.090 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
565 | 16:09:14.109 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
566 | 16:09:14.109 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
567 | 16:09:14.149 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
568 | 16:09:14.149 |  | →RRC DCCH UL Information Transfer |  |  |
569 | 16:09:14.149 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x4) |  |  |
570 | 16:09:14.149 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
571 | 16:09:14.216 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
572 | 16:09:14.237 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
573 | 16:09:14.239 |  |  |  |  | →SIP 100 Trying | P-CSCF
574 | 16:09:14.246 |  |  |  |  | →SIP 200 OK | P-CSCF
575 | 16:09:14.279 |  |  |  |  | XML→ | Media-Server
576 | 16:09:14.287 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:685: 200 OK Verdict: Pass
577 | 16:09:14.287 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:163: Step 53 Verdict: Pass
578 | 16:09:14.291 |  |  |  |  | ←SIP ACK | P-CSCF
579 | 16:09:14.292 |  |  |  |  | ←Floor Taken | Media-Server
580 | 16:09:14.293 |  |  |  |  | ←Floor Idle | Media-Server
581 | 16:09:14.294 |  | ←enobeB PCAP frame← SIP over IPSEC: ACK sip:PublicUserId-A@192.168.3.2:43009;transport... |  |  |
582 | 16:09:14.389 |  |  |  |  | MMICmd: Request PTT token
583 | 16:09:16.149 | →enobeB PCAP frame→ |  |  |  |
584 | 16:09:16.150 |  |  |  |  | Floor Request→ | Media-Server
585 | 16:09:16.152 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Request Verdict: Pass
586 | 16:09:16.155 |  |  |  |  | ←Floor Granted | Media-Server
587 | 16:09:16.189 | →enobeB PCAP frame→ |  |  |  |
588 | 16:09:16.190 |  |  |  |  | Floor ACK→ | Media-Server
589 | 16:09:16.192 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
590 | 16:09:16.192 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:178: Step 57 Verdict: Pass
591 | 16:09:16.229 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
592 | 16:09:16.232 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
593 | 16:09:16.237 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
594 | 16:09:16.241 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
595 | 16:09:16.269 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
596 | 16:09:16.294 |  |  |  |  | MMICmd: Release PTT token
597 | 16:09:18.229 | →enobeB PCAP frame→ |  |  |  |
598 | 16:09:18.230 |  |  |  |  | Floor Release→ | Media-Server
599 | 16:09:18.233 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
600 | 16:09:18.233 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:187: Step 62 Verdict: Pass
601 | 16:09:18.235 |  |  |  |  | ←XML | Media-Server
602 | 16:09:18.237 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
603 | 16:09:18.237 |  |  |  |  | ←Floor Idle | Media-Server
604 | 16:09:18.240 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
605 | 16:09:18.273 |  |  |  |  | ←SIP INVITE | P-CSCF
606 | 16:09:18.276 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
607 | 16:09:18.277 |  | ←enobeB PCAP frame← SIP over IPSEC: INVITE sip:PublicUserId-A@192.168.3.2:43009;transp... |  |  |
608 | 16:09:18.357 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 100 Trying |  |  |  |
609 | 16:09:18.358 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
610 | 16:09:18.359 |  |  |  |  | →SIP 100 Trying | P-CSCF
611 | 16:09:18.364 |  |  |  |  | →SIP 200 OK | P-CSCF
612 | 16:09:18.378 |  |  |  |  | XML→ | Media-Server
613 | 16:09:18.381 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:685: 200 OK Verdict: Pass
614 | 16:09:18.381 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:193: Step 65 Verdict: Pass
615 | 16:09:18.382 |  |  |  |  | ←SIP ACK | P-CSCF
616 | 16:09:18.383 |  |  |  |  | ←Floor Taken | Media-Server
617 | 16:09:18.383 |  |  |  |  | ←Floor Idle | Media-Server
618 | 16:09:18.386 |  | ←enobeB PCAP frame← SIP over IPSEC: ACK sip:PublicUserId-A@192.168.3.2:43009;transport... |  |  |
619 | 16:09:18.482 |  |  |  |  | MMICmd: Request PTT token
620 | 16:09:20.149 | →enobeB PCAP frame→ |  |  |  |
621 | 16:09:20.150 |  |  |  |  | Floor Request→ | Media-Server
622 | 16:09:20.153 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Request Verdict: Pass
623 | 16:09:20.156 |  |  |  |  | ←Floor Granted | Media-Server
624 | 16:09:20.189 | →enobeB PCAP frame→ |  |  |  |
625 | 16:09:20.190 |  |  |  |  | Floor ACK→ | Media-Server
626 | 16:09:20.193 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
627 | 16:09:20.193 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:208: Step 70 Verdict: Pass
628 | 16:09:20.269 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
629 | 16:09:20.272 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
630 | 16:09:20.277 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
631 | 16:09:20.280 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
632 | 16:09:20.295 |  |  |  |  | MMICmd: Release PTT token
633 | 16:09:20.309 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
634 | 16:09:21.798 |  |  |  |  | Floor Release→ | Media-Server
635 | 16:09:21.801 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
636 | 16:09:21.802 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:217: Step 75 Verdict: Pass
637 | 16:09:21.804 |  |  |  |  | ←XML | Media-Server
638 | 16:09:21.805 |  |  |  |  | ←Floor Idle | Media-Server
639 | 16:09:21.842 |  |  |  |  | ←SIP INVITE | P-CSCF
640 | 16:09:21.846 |  | ←enobeB PCAP frame← SIP over IPSEC: INVITE sip:PublicUserId-A@192.168.3.2:43009;transp... |  |  |
641 | 16:09:21.877 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 100 Trying |  |  |  |
642 | 16:09:21.878 |  |  |  |  | →SIP 100 Trying | P-CSCF
643 | 16:09:21.917 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
644 | 16:09:21.924 |  |  |  |  | →SIP 200 OK | P-CSCF
645 | 16:09:21.960 |  |  |  |  | XML→ | Media-Server
646 | 16:09:21.968 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:685: 200 OK Verdict: Pass
647 | 16:09:21.968 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:223: Step 78 Verdict: Pass
648 | 16:09:21.970 |  |  |  |  | ←SIP ACK | P-CSCF
649 | 16:09:21.971 |  |  |  |  | ←Floor Idle | Media-Server
650 | 16:09:21.973 |  | ←enobeB PCAP frame← SIP over IPSEC: ACK sip:PublicUserId-A@192.168.3.2:43009;transport... |  |  |
651 | 16:09:22.069 |  |  |  |  | MMICmd: Request PTT token
652 | 16:09:23.709 | →enobeB PCAP frame→ |  |  |  |
653 | 16:09:23.712 |  |  |  |  | Floor Request→ | Media-Server
654 | 16:09:23.715 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Request Verdict: Pass
655 | 16:09:23.719 |  |  |  |  | ←Floor Granted | Media-Server
656 | 16:09:23.749 | →enobeB PCAP frame→ |  |  |  |
657 | 16:09:23.750 |  |  |  |  | Floor ACK→ | Media-Server
658 | 16:09:23.753 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
659 | 16:09:23.753 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:235: Step 82 Verdict: Pass
660 | 16:09:23.789 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
661 | 16:09:23.792 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
662 | 16:09:23.797 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
663 | 16:09:23.800 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
664 | 16:09:23.829 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
665 | 16:09:23.855 |  |  |  |  | MMICmd: Release PTT token
666 | 16:09:25.358 |  |  |  |  | Floor Release→ | Media-Server
667 | 16:09:25.361 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
668 | 16:09:25.362 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:244: Step 87 Verdict: Pass
669 | 16:09:25.364 |  |  |  |  | ←XML | Media-Server
670 | 16:09:25.364 |  |  |  |  | ←Floor Idle | Media-Server
671 | 16:09:25.402 |  |  |  |  | ←SIP INVITE | P-CSCF
672 | 16:09:25.407 |  | ←enobeB PCAP frame← SIP over IPSEC: INVITE sip:PublicUserId-A@192.168.3.2:43009;transp... |  |  |
673 | 16:09:25.477 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 100 Trying |  |  |  |
674 | 16:09:25.478 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
675 | 16:09:25.478 |  |  |  |  | →SIP 100 Trying | P-CSCF
676 | 16:09:25.480 |  |  |  |  | →SIP 200 OK | P-CSCF
677 | 16:09:25.491 |  |  |  |  | XML→ | Media-Server
678 | 16:09:25.494 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:685: 200 OK Verdict: Pass
679 | 16:09:25.494 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:250: Step 90 Verdict: Pass
680 | 16:09:25.496 |  |  |  |  | ←SIP ACK | P-CSCF
681 | 16:09:25.496 |  |  |  |  | ←Floor Taken | Media-Server
682 | 16:09:25.496 |  |  |  |  | ←Floor Idle | Media-Server
683 | 16:09:25.498 |  | ←enobeB PCAP frame← SIP over IPSEC: ACK sip:PublicUserId-A@192.168.3.2:43009;transport... |  |  |
684 | 16:09:25.595 |  |  |  |  | MMICmd: Request PTT token
685 | 16:09:27.189 | →enobeB PCAP frame→ |  |  |  |
686 | 16:09:27.190 |  |  |  |  | Floor Request→ | Media-Server
687 | 16:09:27.192 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Request Verdict: Pass
688 | 16:09:27.194 |  |  |  |  | ←Floor Granted | Media-Server
689 | 16:09:27.229 | →enobeB PCAP frame→ |  |  |  |
690 | 16:09:27.229 |  |  |  |  | Floor ACK→ | Media-Server
691 | 16:09:27.231 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
692 | 16:09:27.231 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:265: Step 95 Verdict: Pass
693 | 16:09:27.269 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
694 | 16:09:27.271 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
695 | 16:09:27.277 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
696 | 16:09:27.280 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
697 | 16:09:27.309 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
698 | 16:09:27.332 |  |  |  |  | MMICmd: Release PTT token
699 | 16:09:29.077 | →enobeB PCAP frame→ |  |  |  |
700 | 16:09:29.078 |  |  |  |  | Floor Release→ | Media-Server
701 | 16:09:29.081 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
702 | 16:09:29.081 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:274: Step 100 Verdict: Pass
703 | 16:09:29.083 |  |  |  |  | ←Floor Idle | Media-Server
704 | 16:09:29.088 |  |  |  |  | ←SIP BYE | P-CSCF
705 | 16:09:29.091 |  | ←enobeB PCAP frame← SIP over IPSEC: BYE sip:PublicUserId-A@192.168.3.2:43009;transport... |  |  |
706 | 16:09:29.157 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
707 | 16:09:29.159 |  |  |  |  | →SIP 200 OK | P-CSCF
708 | 16:09:29.669 | →enobeB PCAP frame→ |  |  |  |
709 | 16:09:31.169 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
710 | 16:09:31.173 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
711 | 16:09:31.174 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x8) |  |  |
712 | 16:09:31.174 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
713 | 16:09:31.175 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
714 | 16:09:31.229 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
715 | 16:09:31.229 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
716 | 16:09:31.229 |  | →RRC DCCH UL Information Transfer |  |  |
717 | 16:09:31.229 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xa) |  |  |
718 | 16:09:31.229 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
719 | 16:09:31.294 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
720 | 16:09:31.295 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
721 | 16:09:31.341 |  | ←RRC DCCH RRC Connection Release |  |  |
722 | 16:09:31.342 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
723 | 16:09:31.360 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
724 | 16:09:31.361 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:280: Step 103 Verdict: Pass
725 | 16:09:31.362 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
726 | 16:09:31.365 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
727 | 16:09:32.112 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.