ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 08:43:05.478 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 08:43:05.480 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 08:43:05.480 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 08:43:05.482 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 08:43:05.482 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 08:43:05.483 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:805: IMS UDP port 192.168.2.3:5060 configured
7 | 08:43:05.484 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:755: IMS TCP port 192.168.2.3:5060 configured!
8 | 08:43:05.486 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:776: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 08:43:05.487 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:787: IdM port 192.168.2.3:8080 configured!
10 | 08:43:05.488 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 08:43:06.690 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 08:43:06.692 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 08:43:09.862 |  | ←RRC BCCH SIB |  |  |
14 | 08:43:09.867 |  | ←RRC BCCH SIB1 |  |  |
15 | 08:43:09.947 |  | ←RRC BCCH SIB1 |  |  |
16 | 08:43:10.022 |  | ←RRC BCCH SIB |  |  |
17 | 08:43:10.027 |  | ←RRC BCCH SIB1 |  |  |
18 | 08:44:30.691 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 08:44:30.691 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 08:44:30.691 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 08:44:30.691 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 08:44:30.722 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 08:44:30.722 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 08:44:30.722 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 08:44:30.722 |  |  |  | →NAS EMM Attach request |  |
26 | 08:44:30.722 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 08:44:30.722 |  |  |  | NAS K-asme 39f81b718792b190b50d078805c2586b... |  |
28 | 08:44:30.722 |  |  |  | NAS ← EMM Authentication request |  |
29 | 08:44:30.723 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 08:44:30.723 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 08:44:30.724 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 08:44:30.834 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 08:44:30.834 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 08:44:30.834 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 08:44:30.834 |  |  |  | →NAS EMM Authentication response |  |
36 | 08:44:30.834 |  |  |  | NAS UE auth OK |  |
37 | 08:44:30.834 |  |  |  | NAS K-nas-cip 0cf24f04a388bd2601710c4bbd45f... |  |
38 | 08:44:30.834 |  |  |  | NAS K-nas-int c25ed452c369ee01caeeee086b919... |  |
39 | 08:44:30.834 |  |  |  | NAS ← EMM Security mode command |  |
40 | 08:44:30.835 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 08:44:30.835 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 08:44:30.836 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 08:44:30.844 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
44 | 08:44:30.874 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
45 | 08:44:30.874 |  | →RRC DCCH UL Information Transfer |  |  |
46 | 08:44:30.874 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xd) |  |  |
47 | 08:44:30.874 |  |  |  | →NAS EMM Security mode complete |  |
48 | 08:44:30.874 |  |  |  | NAS ← ESM ESM information request |  |
49 | 08:44:30.875 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x0) |  |  |
50 | 08:44:30.875 |  | ←RRC DCCH DL Information Transfer |  |  |
51 | 08:44:30.876 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
52 | 08:44:30.884 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
53 | 08:44:30.922 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
54 | 08:44:30.922 |  | →RRC DCCH UL Information Transfer |  |  |
55 | 08:44:30.922 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x3) |  |  |
56 | 08:44:30.922 |  |  |  | →NAS ESM ESM information response |  |
57 | 08:44:30.922 |  |  |  | NAS ← EMM Attach accept |  |
58 | 08:44:30.922 |  |  |  | NAS K-enb 232abe5c8f49ea8ddd658986355b9c732... |  |
59 | 08:44:30.923 |  | ←RRC DCCH Security Mode Command |  |  |
60 | 08:44:30.923 |  |  | RRC K-enb 232abe5c8f49ea8ddd658986355b9c732... |  |  |
61 | 08:44:30.923 |  |  | RRC rrc-cip 09d9a4a0ecfd27869ab928f93c51f08... |  |  |
62 | 08:44:30.923 |  |  | RRC rrc-int c1684b17656eba462302db0a3e97cbc... |  |  |
63 | 08:44:30.923 |  |  | RRC up-cip 7cc79e34f25f72f6ffd660faf3889024... |  |  |
64 | 08:44:30.923 |  |  | RRC up-int 5fa7bd86aef71fa7f31efd214f223f6f... |  |  |
65 | 08:44:30.924 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
66 | 08:44:30.932 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
67 | 08:44:30.954 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
68 | 08:44:30.954 |  | →RRC DCCH Security Mode Complete |  |  |
69 | 08:44:30.954 |  | ←RRC DCCH UE Capability Enquiry |  |  |
70 | 08:44:30.954 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
71 | 08:44:31.004 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
72 | 08:44:31.004 |  | →RRC DCCH UE Capability Information |  |  |
73 | 08:44:31.004 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xb) |  |  |
74 | 08:44:31.004 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
75 | 08:44:31.004 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
76 | 08:44:31.034 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
77 | 08:44:31.034 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
78 | 08:44:31.074 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
79 | 08:44:31.074 |  | →RRC DCCH UL Information Transfer |  |  |
80 | 08:44:31.074 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xb) |  |  |
81 | 08:44:31.074 |  |  |  | →NAS EMM Attach complete |  |
82 | 08:44:31.074 |  |  |  | NAS ← EMM EMM information |  |
83 | 08:44:31.075 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x8) |  |  |
84 | 08:44:31.075 |  | ←RRC DCCH DL Information Transfer |  |  |
85 | 08:44:31.076 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
86 | 08:44:33.936 |  | ←RRC DCCH RRC Connection Release |  |  |
87 | 08:44:33.937 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
88 | 08:44:36.131 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
89 | 08:44:36.131 |  | →RRC CCCH RRC Connection Request |  |  |
90 | 08:44:36.131 |  | ←RRC CCCH RRC Connection Setup |  |  |
91 | 08:44:36.131 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
92 | 08:44:36.194 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
93 | 08:44:36.194 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
94 | 08:44:36.194 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
95 | 08:44:36.194 |  |  |  | →NAS EMM Service request |  |
96 | 08:44:36.194 |  |  |  | NAS K-enb a35c026d0df04e3837e8b7a6d1e23b86a... |  |
97 | 08:44:36.195 |  | ←RRC DCCH Security Mode Command |  |  |
98 | 08:44:36.195 |  |  | RRC K-enb a35c026d0df04e3837e8b7a6d1e23b86a... |  |  |
99 | 08:44:36.195 |  |  | RRC rrc-cip 82a068b8899dc8dca201cf7ac0249ba... |  |  |
100 | 08:44:36.195 |  |  | RRC rrc-int 54bacafa4a8b03f0e5ad07cfba3a25b... |  |  |
101 | 08:44:36.195 |  |  | RRC up-cip e3535072cdd2251d54bdfcdd6dd48f4b... |  |  |
102 | 08:44:36.195 |  |  | RRC up-int e1703a18d68170af83683ad9582e5a95... |  |  |
103 | 08:44:36.196 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
104 | 08:44:36.234 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
105 | 08:44:36.234 |  | →RRC DCCH Security Mode Complete |  |  |
106 | 08:44:36.234 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
107 | 08:44:36.234 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
108 | 08:44:36.274 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
109 | 08:44:36.274 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
110 | 08:44:58.034 | →enobeB PCAP frame→ TCP |  |  |  |
111 | 08:44:58.037 |  | ←enobeB PCAP frame← TCP |  |  |
112 | 08:44:58.074 | →enobeB PCAP frame→ TCP |  |  |  |
113 | 08:44:58.162 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
114 | 08:44:58.165 |  | ←enobeB PCAP frame← TCP |  |  |
115 | 08:44:58.171 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
116 | 08:44:58.194 | →enobeB PCAP frame→ TCP |  |  |  |
117 | 08:44:58.285 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 16)
118 | 08:44:58.290 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
119 | 08:44:58.293 |  | ←enobeB PCAP frame← TCP |  |  |
120 | 08:44:58.294 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
121 | 08:44:58.314 | →enobeB PCAP frame→ TCP |  |  |  |
122 | 08:44:58.357 |  |  |  |  | →HTTP GET | HTTP-Proxy
123 | 08:44:58.362 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
124 | 08:44:58.363 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:288: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
125 | 08:44:58.365 |  | ←enobeB PCAP frame← TCP |  |  |
126 | 08:44:58.383 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
127 | 08:44:58.395 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
128 | 08:44:58.434 | →enobeB PCAP frame→ TCP |  |  |  |
129 | 08:44:58.474 | →enobeB PCAP frame→ TCP |  |  |  |
130 | 08:45:00.194 | →enobeB PCAP frame→ TCP |  |  |  |
131 | 08:45:00.197 |  | ←enobeB PCAP frame← TCP |  |  |
132 | 08:45:00.234 | →enobeB PCAP frame→ TCP |  |  |  |
133 | 08:45:00.242 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
134 | 08:45:00.245 |  | ←enobeB PCAP frame← TCP |  |  |
135 | 08:45:00.251 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
136 | 08:45:00.314 | →enobeB PCAP frame→ TCP |  |  |  |
137 | 08:45:00.517 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:642: Client connected to IdM port (id 18)
138 | 08:45:00.522 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
139 | 08:45:00.525 |  | ←enobeB PCAP frame← TCP |  |  |
140 | 08:45:00.526 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
141 | 08:45:00.554 | →enobeB PCAP frame→ TCP |  |  |  |
142 | 08:45:00.558 |  |  |  |  | →HTTP GET | IDMS-Endpoint
143 | 08:45:00.562 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
144 | 08:45:00.565 |  | ←enobeB PCAP frame← TCP |  |  |
145 | 08:45:00.600 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
146 | 08:45:00.603 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:511: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
147 | 08:45:00.604 |  |  |  |  | MMICmd: Please provide user credentials: username and password
148 | 08:45:00.609 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
149 | 08:45:00.674 | →enobeB PCAP frame→ TCP |  |  |  |
150 | 08:45:05.479 |  |  |  |  | →HTTP POST | IDMS-Endpoint
151 | 08:45:05.482 | →enobeB PCAP frame→ HTTPS: POST /idms/userauth HTTP/1.1 |  |  |  |
152 | 08:45:05.485 |  | ←enobeB PCAP frame← TCP |  |  |
153 | 08:45:05.493 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
154 | 08:45:05.495 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:516: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
155 | 08:45:05.502 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
156 | 08:45:05.554 | →enobeB PCAP frame→ TCP |  |  |  |
157 | 08:45:05.556 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:677: IdM port - Client closed the connection (id 18)
158 | 08:45:05.562 | →enobeB PCAP frame→ TCP |  |  |  |
159 | 08:45:05.565 |  | ←enobeB PCAP frame← TCP |  |  |
160 | 08:45:05.594 | →enobeB PCAP frame→ TCP |  |  |  |
161 | 08:45:05.994 | →enobeB PCAP frame→ TCP |  |  |  |
162 | 08:45:06.000 |  | ←enobeB PCAP frame← TCP |  |  |
163 | 08:45:06.034 | →enobeB PCAP frame→ TCP |  |  |  |
164 | 08:45:06.042 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
165 | 08:45:06.045 |  | ←enobeB PCAP frame← TCP |  |  |
166 | 08:45:06.046 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
167 | 08:45:06.074 | →enobeB PCAP frame→ TCP |  |  |  |
168 | 08:45:06.156 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:642: Client connected to IdM port (id 18)
169 | 08:45:06.162 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
170 | 08:45:06.165 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
171 | 08:45:06.194 | →enobeB PCAP frame→ TCP |  |  |  |
172 | 08:45:06.196 |  |  |  |  | →HTTP POST | IDMS-Endpoint
173 | 08:45:06.202 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
174 | 08:45:06.205 |  | ←enobeB PCAP frame← TCP |  |  |
175 | 08:45:06.206 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
176 | 08:45:06.209 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:521: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
177 | 08:45:06.215 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
178 | 08:45:06.274 | →enobeB PCAP frame→ TCP |  |  |  |
179 | 08:45:06.554 | →enobeB PCAP frame→ TCP |  |  |  |
180 | 08:45:06.557 |  | ←enobeB PCAP frame← TCP |  |  |
181 | 08:45:06.594 | →enobeB PCAP frame→ TCP |  |  |  |
182 | 08:45:06.602 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
183 | 08:45:06.605 |  | ←enobeB PCAP frame← TCP |  |  |
184 | 08:45:06.608 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
185 | 08:45:06.634 | →enobeB PCAP frame→ TCP |  |  |  |
186 | 08:45:06.677 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 19)
187 | 08:45:06.682 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
188 | 08:45:06.685 |  | ←enobeB PCAP frame← TCP |  |  |
189 | 08:45:06.686 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
190 | 08:45:06.718 |  |  |  |  | →HTTP POST | HTTP-Proxy
191 | 08:45:06.722 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
192 | 08:45:06.725 |  | ←enobeB PCAP frame← TCP |  |  |
193 | 08:45:06.744 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:541: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
194 | 08:45:06.751 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
195 | 08:45:06.761 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
196 | 08:45:06.794 | →enobeB PCAP frame→ TCP |  |  |  |
197 | 08:45:06.834 | →enobeB PCAP frame→ TCP |  |  |  |
198 | 08:45:06.837 |  | ←enobeB PCAP frame← TCP |  |  |
199 | 08:45:06.874 | →enobeB PCAP frame→ TCP |  |  |  |
200 | 08:45:06.882 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
201 | 08:45:06.885 |  | ←enobeB PCAP frame← TCP |  |  |
202 | 08:45:06.888 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
203 | 08:45:06.914 | →enobeB PCAP frame→ TCP |  |  |  |
204 | 08:45:06.917 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 20)
205 | 08:45:06.922 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
206 | 08:45:06.925 |  | ←enobeB PCAP frame← TCP |  |  |
207 | 08:45:06.926 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
208 | 08:45:06.958 |  |  |  |  | →HTTP POST | HTTP-Proxy
209 | 08:45:06.962 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
210 | 08:45:06.965 |  | ←enobeB PCAP frame← TCP |  |  |
211 | 08:45:07.021 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
212 | 08:45:07.021 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:545: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
213 | 08:45:07.031 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
214 | 08:45:07.074 | →enobeB PCAP frame→ TCP |  |  |  |
215 | 08:45:07.118 |  |  |  |  | →SIP REGISTER | P-CSCF
216 | 08:45:07.122 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
217 | 08:45:07.141 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:814: IMS UDP_s port 192.168.2.3:5062 configured
218 | 08:45:07.168 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:765: IMS TCP_s port 192.168.2.3:5062 configured!
219 | 08:45:07.171 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:823: IMS UDP_c port 192.168.2.3:5061 configured
220 | 08:45:07.182 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
221 | 08:45:07.962 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
222 | 08:45:08.027 |  |  |  |  | →SIP REGISTER | P-CSCF
223 | 08:45:08.043 |  |  |  |  | ←SIP 200 OK | P-CSCF
224 | 08:45:08.053 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
225 | 08:45:08.362 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
226 | 08:45:08.363 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 SIP over IPSEC: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 |  |  |  |
227 | 08:45:08.364 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
228 | 08:45:08.377 |  |  |  |  | ←SIP 200 OK | P-CSCF
229 | 08:45:08.377 |  |  |  |  | MIKEY | Media-Server
230 | 08:45:08.386 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
231 | 08:45:08.580 |  |  |  |  | XML→ | Media-Server
232 | 08:45:08.581 |  |  |  |  | XML→ | Media-Server
233 | 08:45:08.584 |  |  |  |  | ←XML | Media-Server
234 | 08:45:08.587 |  |  |  |  | ←SIP NOTIFY | P-CSCF
235 | 08:45:08.597 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:46895;transp... |  |  |
236 | 08:45:08.636 |  |  |  |  | →SIP 200 OK | P-CSCF
237 | 08:45:08.642 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
238 | 08:45:08.914 | →enobeB PCAP frame→ TCP |  |  |  |
239 | 08:45:08.917 |  | ←enobeB PCAP frame← TCP |  |  |
240 | 08:45:08.954 | →enobeB PCAP frame→ TCP |  |  |  |
241 | 08:45:08.962 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
242 | 08:45:08.965 |  | ←enobeB PCAP frame← TCP |  |  |
243 | 08:45:08.969 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
244 | 08:45:08.994 | →enobeB PCAP frame→ TCP |  |  |  |
245 | 08:45:09.082 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
246 | 08:45:09.085 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
247 | 08:45:09.114 | →enobeB PCAP frame→ TCP |  |  |  |
248 | 08:45:09.122 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-co... |  |  |  |
249 | 08:45:09.125 |  | ←enobeB PCAP frame← TCP |  |  |
250 | 08:45:09.138 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
251 | 08:45:09.140 |  |  |  |  | →HTTP GET | HTTP-Proxy
252 | 08:45:09.149 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:642: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcptt-ue-configuration.xml
253 | 08:45:09.158 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
254 | 08:45:09.169 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
255 | 08:45:09.228 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
256 | 08:45:09.234 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
257 | 08:45:09.237 |  | ←enobeB PCAP frame← TCP |  |  |
258 | 08:45:09.242 | →enobeB PCAP frame→ TCP |  |  |  |
259 | 08:45:09.245 |  | ←enobeB PCAP frame← TCP |  |  |
260 | 08:45:09.274 | →enobeB PCAP frame→ TCP |  |  |  |
261 | 08:45:09.394 | →enobeB PCAP frame→ TCP |  |  |  |
262 | 08:45:09.397 |  | ←enobeB PCAP frame← TCP |  |  |
263 | 08:45:09.434 | →enobeB PCAP frame→ TCP |  |  |  |
264 | 08:45:09.442 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
265 | 08:45:09.445 |  | ←enobeB PCAP frame← TCP |  |  |
266 | 08:45:09.448 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
267 | 08:45:09.474 | →enobeB PCAP frame→ TCP |  |  |  |
268 | 08:45:09.556 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
269 | 08:45:09.562 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
270 | 08:45:09.565 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
271 | 08:45:09.594 | →enobeB PCAP frame→ TCP |  |  |  |
272 | 08:45:09.597 |  |  |  |  | →HTTP GET | HTTP-Proxy
273 | 08:45:09.602 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-... |  |  |  |
274 | 08:45:09.605 |  | ←enobeB PCAP frame← TCP |  |  |
275 | 08:45:09.608 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:647: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcptt-user-profile-49.xml
276 | 08:45:09.647 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
277 | 08:45:09.661 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
278 | 08:45:09.662 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
279 | 08:45:09.674 | →enobeB PCAP frame→ TCP |  |  |  |
280 | 08:45:09.682 | →enobeB PCAP frame→ TCP |  |  |  |
281 | 08:45:09.708 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
282 | 08:45:09.714 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
283 | 08:45:09.717 |  | ←enobeB PCAP frame← TCP |  |  |
284 | 08:45:09.722 | →enobeB PCAP frame→ TCP |  |  |  |
285 | 08:45:09.725 |  | ←enobeB PCAP frame← TCP |  |  |
286 | 08:45:09.754 | →enobeB PCAP frame→ TCP |  |  |  |
287 | 08:45:10.322 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
288 | 08:45:10.323 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
289 | 08:45:10.324 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
290 | 08:45:10.330 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
291 | 08:45:10.347 |  |  |  |  | ←SIP 200 OK | P-CSCF
292 | 08:45:10.347 |  |  |  |  | MIKEY | Media-Server
293 | 08:45:10.356 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
294 | 08:45:10.394 | →enobeB PCAP frame→ TCP |  |  |  |
295 | 08:45:10.397 |  | ←enobeB PCAP frame← TCP |  |  |
296 | 08:45:10.434 | →enobeB PCAP frame→ TCP |  |  |  |
297 | 08:45:10.442 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
298 | 08:45:10.445 |  | ←enobeB PCAP frame← TCP |  |  |
299 | 08:45:10.446 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
300 | 08:45:10.474 | →enobeB PCAP frame→ TCP |  |  |  |
301 | 08:45:10.551 |  |  |  |  | XML→ | Media-Server
302 | 08:45:10.552 |  |  |  |  | XML→ | Media-Server
303 | 08:45:10.555 |  |  |  |  | ←XML | Media-Server
304 | 08:45:10.596 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
305 | 08:45:10.596 |  |  |  |  | ←SIP NOTIFY | P-CSCF
306 | 08:45:10.602 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
307 | 08:45:10.605 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
308 | 08:45:10.606 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:46895;transp... |  |  |
309 | 08:45:10.634 | →enobeB PCAP frame→ TCP |  |  |  |
310 | 08:45:10.636 |  |  |  |  | →HTTP GET | HTTP-Proxy
311 | 08:45:10.637 |  |  |  |  | →SIP 200 OK | P-CSCF
312 | 08:45:10.638 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:652: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
313 | 08:45:10.642 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.servi... |  |  |  |
314 | 08:45:10.644 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
315 | 08:45:10.645 |  | ←enobeB PCAP frame← TCP |  |  |
316 | 08:45:10.655 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
317 | 08:45:10.656 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
318 | 08:45:10.674 | →enobeB PCAP frame→ TCP |  |  |  |
319 | 08:45:10.682 | →enobeB PCAP frame→ TCP |  |  |  |
320 | 08:45:10.684 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
321 | 08:45:10.690 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
322 | 08:45:10.694 |  | ←enobeB PCAP frame← TCP |  |  |
323 | 08:45:10.714 | →enobeB PCAP frame→ TCP |  |  |  |
324 | 08:45:10.754 | →enobeB PCAP frame→ TCP |  |  |  |
325 | 08:45:10.757 |  | ←enobeB PCAP frame← TCP |  |  |
326 | 08:45:10.794 | →enobeB PCAP frame→ TCP |  |  |  |
327 | 08:45:10.802 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
328 | 08:45:10.805 |  | ←enobeB PCAP frame← TCP |  |  |
329 | 08:45:10.808 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
330 | 08:45:10.834 | →enobeB PCAP frame→ TCP |  |  |  |
331 | 08:45:10.917 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
332 | 08:45:10.922 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
333 | 08:45:10.925 |  | ←enobeB PCAP frame← TCP |  |  |
334 | 08:45:10.926 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
335 | 08:45:10.954 | →enobeB PCAP frame→ TCP |  |  |  |
336 | 08:45:10.957 |  |  |  |  | →HTTP GET | HTTP-Proxy
337 | 08:45:10.962 | →enobeB PCAP frame→ HTTPS: GET /xcap.gms.mcstaasting.com/org.openmobileallian... |  |  |  |
338 | 08:45:10.965 |  | ←enobeB PCAP frame← TCP |  |  |
339 | 08:45:10.967 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:657: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at /xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
340 | 08:45:10.991 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
341 | 08:45:11.004 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
342 | 08:45:11.034 | →enobeB PCAP frame→ TCP |  |  |  |
343 | 08:45:11.042 | →enobeB PCAP frame→ TCP |  |  |  |
344 | 08:45:11.068 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
345 | 08:45:11.074 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
346 | 08:45:11.077 |  | ←enobeB PCAP frame← TCP |  |  |
347 | 08:45:11.082 | →enobeB PCAP frame→ TCP |  |  |  |
348 | 08:45:11.086 |  | ←enobeB PCAP frame← TCP |  |  |
349 | 08:45:11.114 | →enobeB PCAP frame→ TCP |  |  |  |
350 | 08:45:11.322 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
351 | 08:45:11.323 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
352 | 08:45:11.329 |  |  |  |  | →SIP PUBLISH | P-CSCF
353 | 08:45:11.374 |  |  |  |  | MIKEY | Media-Server
354 | 08:45:11.399 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
355 | 08:45:11.402 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
356 | 08:45:11.403 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
357 | 08:45:11.583 |  |  |  |  | XML→ | Media-Server
358 | 08:45:11.586 |  |  |  |  | ←SIP 200 OK | P-CSCF
359 | 08:45:11.590 |  |  |  |  | ←SIP 200 OK | P-CSCF
360 | 08:45:11.590 |  |  |  |  | MIKEY | Media-Server
361 | 08:45:11.596 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
362 | 08:45:11.599 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
363 | 08:45:11.792 |  |  |  |  | XML→ | Media-Server
364 | 08:45:11.793 |  |  |  |  | XML→ | Media-Server
365 | 08:45:11.827 |  |  |  |  | ←XML | Media-Server
366 | 08:45:11.831 |  |  |  |  | ←SIP NOTIFY | P-CSCF
367 | 08:45:11.841 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:46895;transp... |  |  |
368 | 08:45:11.876 |  |  |  |  | →SIP 200 OK | P-CSCF
369 | 08:45:11.879 |  |  |  |  | ←XML | Media-Server
370 | 08:45:11.882 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
371 | 08:45:11.908 |  |  |  |  | ←SIP MESSAGE | P-CSCF
372 | 08:45:11.919 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
373 | 08:45:11.920 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
374 | 08:45:12.717 |  |  |  |  | →SIP 200 OK | P-CSCF
375 | 08:45:12.722 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
376 | 08:45:12.724 |  |  |  |  | Info: MCX_IMS_CommonProcedures.ttcn:155: MESSAGE/200OK Table 5.3.2.3-2 Steps 7-8 Done
377 | 08:45:12.735 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
378 | 08:45:12.794 | →enobeB PCAP frame→ TCP |  |  |  |
379 | 08:45:12.802 | →enobeB PCAP frame→ TCP |  |  |  |
380 | 08:45:14.726 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
381 | 08:45:14.769 |  | ←RRC DCCH RRC Connection Release |  |  |
382 | 08:45:14.770 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
383 | 08:45:14.782 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
384 | 08:45:14.784 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
385 | 08:45:14.784 |  |  |  |  | MMICmd: Make the MCPTT User request the establishment of an MCPTT on-demand pre-arranged group call, manual commencement mode, with explicit request for floor control (implicit floor control)
386 | 08:45:20.371 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
387 | 08:45:20.371 |  | →RRC CCCH RRC Connection Request |  |  |
388 | 08:45:20.371 |  | ←RRC CCCH RRC Connection Setup |  |  |
389 | 08:45:20.371 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
390 | 08:45:20.434 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
391 | 08:45:20.434 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
392 | 08:45:20.434 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
393 | 08:45:20.434 |  |  |  | →NAS EMM Service request |  |
394 | 08:45:20.434 |  |  |  | NAS K-enb e2fd89acfff4e5552989c242bf7cb8e8a... |  |
395 | 08:45:20.435 |  | ←RRC DCCH Security Mode Command |  |  |
396 | 08:45:20.435 |  |  | RRC K-enb e2fd89acfff4e5552989c242bf7cb8e8a... |  |  |
397 | 08:45:20.435 |  |  | RRC rrc-cip 92731f42cd72fcf8bc52b71a2f9515e... |  |  |
398 | 08:45:20.435 |  |  | RRC rrc-int f4816db0e2c4dad2140be7e1f9e4e96... |  |  |
399 | 08:45:20.435 |  |  | RRC up-cip 680625f706adb989b097c7c9eb9d3455... |  |  |
400 | 08:45:20.435 |  |  | RRC up-int 889dc475f97c0b39d164af9bcead30a2... |  |  |
401 | 08:45:20.436 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
402 | 08:45:20.474 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
403 | 08:45:20.474 |  | →RRC DCCH Security Mode Complete |  |  |
404 | 08:45:20.474 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
405 | 08:45:20.474 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
406 | 08:45:20.514 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
407 | 08:45:20.514 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
408 | 08:45:20.519 |  |  |  |  | →SIP INVITE | P-CSCF
409 | 08:45:20.522 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
410 | 08:45:20.523 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
411 | 08:45:20.600 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:735: SRTP config: Master Key: 1C9F80CF2D013C0902A72BAD1BDBC33E, Master Salt: B1BF55A91E0D35D075E9D2DE, MKI: 29B658B6
412 | 08:45:20.600 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
413 | 08:45:20.606 |  |  |  |  | XML→ | Media-Server
414 | 08:45:20.607 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
415 | 08:45:20.608 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1205: INVITE Verdict: Pass
416 | 08:45:20.610 |  |  |  |  | ←SIP 100 Trying | P-CSCF
417 | 08:45:20.613 |  |  |  |  | ←SIP 200 OK | P-CSCF
418 | 08:45:20.619 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
419 | 08:45:20.626 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
420 | 08:45:21.255 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
421 | 08:45:21.256 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xc) |  |  |
422 | 08:45:21.256 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
423 | 08:45:21.257 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
424 | 08:45:21.274 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
425 | 08:45:21.274 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
426 | 08:45:21.314 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
427 | 08:45:21.314 |  | →RRC DCCH UL Information Transfer |  |  |
428 | 08:45:21.314 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xc) |  |  |
429 | 08:45:21.314 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
430 | 08:45:21.381 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
431 | 08:45:21.557 |  |  |  |  | →SIP ACK | P-CSCF
432 | 08:45:21.562 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
433 | 08:45:21.566 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1208: ACK Verdict: Pass
434 | 08:45:21.567 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:352: Step 2 Verdict: Pass
435 | 08:45:21.570 |  |  |  |  | ←Floor Granted | Media-Server
436 | 08:45:22.074 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
437 | 08:45:22.082 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
438 | 08:45:22.114 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
439 | 08:45:22.122 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
440 | 08:45:22.154 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
441 | 08:45:22.318 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:357: Step 6A Verdict: Pass
442 | 08:45:22.421 |  |  |  |  | MMICmd: Release PTT token
443 | 08:45:24.236 |  |  |  |  | Floor Release→ | Media-Server
444 | 08:45:24.239 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
445 | 08:45:24.239 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:364: Step 6C Verdict: Pass
446 | 08:45:24.242 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
447 | 08:45:24.242 |  |  |  |  | ←Floor Idle | Media-Server
448 | 08:45:24.246 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
449 | 08:45:24.344 |  |  |  |  | MMICmd: Release call (hang up the call)
450 | 08:45:26.439 |  |  |  |  | →SIP BYE | P-CSCF
451 | 08:45:26.442 | →enobeB PCAP frame→ SIP over IPSEC: BYE sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
452 | 08:45:26.462 |  |  |  |  | ←SIP 200 OK | P-CSCF
453 | 08:45:26.472 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
454 | 08:45:26.754 | →enobeB PCAP frame→ |  |  |  |
455 | 08:45:28.460 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
456 | 08:45:28.484 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
457 | 08:45:28.485 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xc) |  |  |
458 | 08:45:28.485 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
459 | 08:45:28.486 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
460 | 08:45:28.514 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
461 | 08:45:28.514 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
462 | 08:45:28.514 |  | →RRC DCCH UL Information Transfer |  |  |
463 | 08:45:28.514 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xd) |  |  |
464 | 08:45:28.514 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
465 | 08:45:28.594 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
466 | 08:45:28.596 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
467 | 08:45:28.638 |  | ←RRC DCCH RRC Connection Release |  |  |
468 | 08:45:28.639 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
469 | 08:45:28.650 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
470 | 08:45:28.653 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
471 | 08:45:28.654 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
472 | 08:45:29.402 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.