MSG #314 2021-09-17 09:08:21.533

HTTP 200 OK message at 09:08:21.533

    HTTP/1.1 200 OK
    Content-Type: application/vnd.3gpp.mcptt-service-config+xml
    Cache-Control: no-store
    Pragma: no-cache
    Content-Length: 5780

    <mcpttsc:service-configuration-info-Type xmlns:mcpttsc='urn:3gpp:ns:mcpttServiceConfig:1.0'>
    	<mcpttsc:service-configuration-params domain='mcstaasting.com'>
    		<mcpttsc:common>
    			<mcpttsc:min-length-alias>2</mcpttsc:min-length-alias>
    			<mcpttsc:broadcast-group>
    				<mcpttsc:num-levels-group-hierarchy>1</mcpttsc:num-levels-group-hierarchy>
    				<mcpttsc:num-levels-user-hierarchy>1</mcpttsc:num-levels-user-hierarchy>
    			</mcpttsc:broadcast-group>
    		</mcpttsc:common>
    		<mcpttsc:on-network>
    			<mcpttsc:emergency-call>
    				<mcpttsc:private-cancel-timeout>PT30M</mcpttsc:private-cancel-timeout>
    				<mcpttsc:group-time-limit>PT20M</mcpttsc:group-time-limit>
    			</mcpttsc:emergency-call>
    			<mcpttsc:private-call>
    				<mcpttsc:hang-time>PT30S</mcpttsc:hang-time>
    				<mcpttsc:max-duration-with-floor-control>PT30S</mcpttsc:max-duration-with-floor-control>
    				<mcpttsc:max-duration-without-floor-control>PT20M</mcpttsc:max-duration-without-floor-control>
    			</mcpttsc:private-call>
    			<mcpttsc:num-levels-priority-hierarchy>10</mcpttsc:num-levels-priority-hierarchy>
    			<mcpttsc:transmit-time>
    				<mcpttsc:time-limit>PT30S</mcpttsc:time-limit>
    				<mcpttsc:time-warning>PT20M</mcpttsc:time-warning>
    			</mcpttsc:transmit-time>
    			<mcpttsc:hang-time-warning>PT20M</mcpttsc:hang-time-warning>
    			<mcpttsc:floor-control-queue>
    				<mcpttsc:depth>5</mcpttsc:depth>
    				<mcpttsc:max-user-request-time>PT20M</mcpttsc:max-user-request-time>
    			</mcpttsc:floor-control-queue>
    			<mcpttsc:fc-timers-counters>
    				<mcpttsc:T1-end-of-rtp-media>PT4S</mcpttsc:T1-end-of-rtp-media>
    				<mcpttsc:T3-stop-talking-grace>PT3S</mcpttsc:T3-stop-talking-grace>
    				<mcpttsc:T7-floor-idle>PT2S</mcpttsc:T7-floor-idle>
    				<mcpttsc:T8-floor-revoke>PT1S</mcpttsc:T8-floor-revoke>
    				<mcpttsc:T11-end-of-RTP-dual>PT4S</mcpttsc:T11-end-of-RTP-dual>
    				<mcpttsc:T12-stop-talking-dual>PT30S</mcpttsc:T12-stop-talking-dual>
    				<mcpttsc:T15-conversation>PT30S</mcpttsc:T15-conversation>
    				<mcpttsc:T16-map-group-to-bearer>PT0.5S</mcpttsc:T16-map-group-to-bearer>
    				<mcpttsc:T17-unmap-group-to-bearer>PT0.5S</mcpttsc:T17-unmap-group-to-bearer>
    				<mcpttsc:T20-floor-granted>PT1S</mcpttsc:T20-floor-granted>
    				<mcpttsc:T55-connect>PT2S</mcpttsc:T55-connect>
    				<mcpttsc:T56-disconnect>PT2S</mcpttsc:T56-disconnect>
    				<mcpttsc:C7-floor-idle>10</mcpttsc:C7-floor-idle>
    				<mcpttsc:C17-unmap-group-to-bearer>3</mcpttsc:C17-unmap-group-to-bearer>
    				<mcpttsc:C20-floor-granted>3</mcpttsc:C20-floor-granted>
    				<mcpttsc:C55-connect>3</mcpttsc:C55-connect>
    				<mcpttsc:C56-disconnect>3</mcpttsc:C56-disconnect>
    			</mcpttsc:fc-timers-counters>
    			<mcpttsc:signalling-protection>
    				<mcpttsc:confidentiality-protection>true</mcpttsc:confidentiality-protection>
    				<mcpttsc:integrity-protection>true</mcpttsc:integrity-protection>
    			</mcpttsc:signalling-protection>
    			<mcpttsc:protection-between-mcptt-servers>
    				<mcpttsc:allow-signalling-protection>true</mcpttsc:allow-signalling-protection>
    				<mcpttsc:allow-floor-control-protection>true</mcpttsc:allow-floor-control-protection>
    			</mcpttsc:protection-between-mcptt-servers>
    			<mcpttsc:emergency-resource-priority>
    				<mcpttsc:resource-priority-namespace>mcpttp</mcpttsc:resource-priority-namespace>
    				<mcpttsc:resource-priority-priority>8</mcpttsc:resource-priority-priority>
    			</mcpttsc:emergency-resource-priority>
    			<mcpttsc:imminent-peril-resource-priority>
    				<mcpttsc:resource-priority-namespace>mcpttp</mcpttsc:resource-priority-namespace>
    				<mcpttsc:resource-priority-priority>5</mcpttsc:resource-priority-priority>
    			</mcpttsc:imminent-peril-resource-priority>
    			<mcpttsc:normal-resource-priority>
    				<mcpttsc:resource-priority-namespace>mcpttp</mcpttsc:resource-priority-namespace>
    				<mcpttsc:resource-priority-priority>1</mcpttsc:resource-priority-priority>
    			</mcpttsc:normal-resource-priority>
    			<mcpttsc:anyExt>
    				<mcpttsc:functional-aliasType xmlns:mcpttsc='urn:3gpp:ns:mcpttServiceConfig:1.0'>
    	<mcpttsc:functional-alias>mcptt-FA-A-id@ mcptt-op.gov</mcpttsc:functional-alias>
    	<mcpttsc:max-simultaneous-activations>1</mcpttsc:max-simultaneous-activations>
    	<mcpttsc:allow-takeover>true</mcpttsc:allow-takeover>
    	<mcpttsc:mcptt-user-list>
    		<mcpttsc:entry>
    			<mcpttsc:uri-entry>mcptt-userA-id@mcstaasting.com</mcpttsc:uri-entry>
    		</mcpttsc:entry>
    	</mcpttsc:mcptt-user-list>
    </mcpttsc:functional-aliasType>

    			</mcpttsc:anyExt>
    		</mcpttsc:on-network>
    		<mcpttsc:off-network>
    			<mcpttsc:emergency-call>
    				<mcpttsc:private-cancel-timeout>PT5S</mcpttsc:private-cancel-timeout>
    				<mcpttsc:group-time-limit>PT5S</mcpttsc:group-time-limit>
    			</mcpttsc:emergency-call>
    			<mcpttsc:private-call>
    				<mcpttsc:hang-time>PT5S</mcpttsc:hang-time>
    				<mcpttsc:max-duration-with-floor-control>PT60S</mcpttsc:max-duration-with-floor-control>
    			</mcpttsc:private-call>
    			<mcpttsc:num-levels-priority-hierarchy>4</mcpttsc:num-levels-priority-hierarchy>
    			<mcpttsc:transmit-time>
    				<mcpttsc:time-limit>PT60S</mcpttsc:time-limit>
    				<mcpttsc:time-warning>PT50S</mcpttsc:time-warning>
    			</mcpttsc:transmit-time>
    			<mcpttsc:hang-time-warning>PT4S</mcpttsc:hang-time-warning>
    			<mcpttsc:default-prose-per-packet-priority>
    				<mcpttsc:mcptt-private-call-signalling>1</mcpttsc:mcptt-private-call-signalling>
    				<mcpttsc:mcptt-private-call-media>1</mcpttsc:mcptt-private-call-media>
    				<mcpttsc:mcptt-emergency-private-call-signalling>8</mcpttsc:mcptt-emergency-private-call-signalling>
    				<mcpttsc:mcptt-emergency-private-call-media>8</mcpttsc:mcptt-emergency-private-call-media>
    			</mcpttsc:default-prose-per-packet-priority>
    			<mcpttsc:allow-log-metadata>true</mcpttsc:allow-log-metadata>
    		</mcpttsc:off-network>
    	</mcpttsc:service-configuration-params>
    </mcpttsc:service-configuration-info-Type>