ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 09:06:52.011 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 09:06:52.015 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 09:06:52.015 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 09:06:52.017 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 09:06:52.018 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 09:06:52.018 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:807: IMS UDP port 192.168.2.3:5060 configured
7 | 09:06:52.020 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:757: IMS TCP port 192.168.2.3:5060 configured!
8 | 09:06:52.021 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:778: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 09:06:52.022 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:789: IdM port 192.168.2.3:8080 configured!
10 | 09:06:52.024 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 09:06:53.225 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 09:06:53.227 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 09:06:55.039 |  | ←RRC BCCH SIB |  |  |
14 | 09:06:55.044 |  | ←RRC BCCH SIB1 |  |  |
15 | 09:06:55.124 |  | ←RRC BCCH SIB1 |  |  |
16 | 09:06:55.199 |  | ←RRC BCCH SIB |  |  |
17 | 09:06:55.204 |  | ←RRC BCCH SIB1 |  |  |
18 | 09:07:47.728 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 09:07:47.728 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 09:07:47.728 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 09:07:47.728 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 09:07:47.779 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 09:07:47.779 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 09:07:47.779 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 09:07:47.779 |  |  |  | →NAS EMM Attach request |  |
26 | 09:07:47.779 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 09:07:47.779 |  |  |  | NAS K-asme 7edb926e729bfc38db12e7413d2a3f9f... |  |
28 | 09:07:47.779 |  |  |  | NAS ← EMM Authentication request |  |
29 | 09:07:47.780 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 09:07:47.780 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 09:07:47.781 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 09:07:47.851 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 09:07:47.851 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 09:07:47.851 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 09:07:47.851 |  |  |  | →NAS EMM Authentication response |  |
36 | 09:07:47.851 |  |  |  | NAS UE auth OK |  |
37 | 09:07:47.851 |  |  |  | NAS K-nas-cip dbc13dce2c0a3f66324725b7f7289... |  |
38 | 09:07:47.851 |  |  |  | NAS K-nas-int 2ec0e4af978f30cdbe20470725dd2... |  |
39 | 09:07:47.851 |  |  |  | NAS ← EMM Security mode command |  |
40 | 09:07:47.852 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 09:07:47.852 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 09:07:47.853 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 09:07:47.891 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
44 | 09:07:47.891 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 09:07:47.891 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x1e) |  |  |
46 | 09:07:47.891 |  |  |  | →NAS EMM Security mode complete |  |
47 | 09:07:47.891 |  |  |  | NAS ← ESM ESM information request |  |
48 | 09:07:47.892 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xc) |  |  |
49 | 09:07:47.892 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 09:07:47.893 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
51 | 09:07:47.939 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
52 | 09:07:47.939 |  | →RRC DCCH UL Information Transfer |  |  |
53 | 09:07:47.939 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xc) |  |  |
54 | 09:07:47.939 |  |  |  | →NAS ESM ESM information response |  |
55 | 09:07:47.939 |  |  |  | NAS ← EMM Attach accept |  |
56 | 09:07:47.939 |  |  |  | NAS K-enb 41a98ac1b46bfae199d26fd6f3b0ccde4... |  |
57 | 09:07:47.940 |  | ←RRC DCCH Security Mode Command |  |  |
58 | 09:07:47.940 |  |  | RRC K-enb 41a98ac1b46bfae199d26fd6f3b0ccde4... |  |  |
59 | 09:07:47.940 |  |  | RRC rrc-cip f97e420f46f637dacc049371e346222... |  |  |
60 | 09:07:47.940 |  |  | RRC rrc-int 25a8ef471b27fc975f11841d1a66c0d... |  |  |
61 | 09:07:47.940 |  |  | RRC up-cip 7a154d9e1ea29582ad10a99b8182bc27... |  |  |
62 | 09:07:47.940 |  |  | RRC up-int aa89137fa7415235f98a93bb6611c7a0... |  |  |
63 | 09:07:47.941 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
64 | 09:07:47.971 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
65 | 09:07:47.971 |  | →RRC DCCH Security Mode Complete |  |  |
66 | 09:07:47.971 |  | ←RRC DCCH UE Capability Enquiry |  |  |
67 | 09:07:47.971 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
68 | 09:07:48.021 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
69 | 09:07:48.021 |  | →RRC DCCH UE Capability Information |  |  |
70 | 09:07:48.022 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x8) |  |  |
71 | 09:07:48.022 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
72 | 09:07:48.022 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
73 | 09:07:48.051 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
74 | 09:07:48.051 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
75 | 09:07:48.091 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
76 | 09:07:48.091 |  | →RRC DCCH UL Information Transfer |  |  |
77 | 09:07:48.091 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x4e) |  |  |
78 | 09:07:48.091 |  |  |  | →NAS EMM Attach complete |  |
79 | 09:07:48.091 |  |  |  | NAS ← EMM EMM information |  |
80 | 09:07:48.092 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x6) |  |  |
81 | 09:07:48.092 |  | ←RRC DCCH DL Information Transfer |  |  |
82 | 09:07:48.093 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
83 | 09:07:55.351 |  | ←RRC DCCH RRC Connection Release |  |  |
84 | 09:07:55.352 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
85 | 09:07:57.238 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
86 | 09:07:57.238 |  | →RRC CCCH RRC Connection Request |  |  |
87 | 09:07:57.238 |  | ←RRC CCCH RRC Connection Setup |  |  |
88 | 09:07:57.238 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
89 | 09:07:57.291 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
90 | 09:07:57.291 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
91 | 09:07:57.291 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
92 | 09:07:57.291 |  |  |  | →NAS EMM Service request |  |
93 | 09:07:57.291 |  |  |  | NAS K-enb a3a8f74c36a18df7d223d2143ced03c08... |  |
94 | 09:07:57.292 |  |  | RRC K-enb a3a8f74c36a18df7d223d2143ced03c08... |  |  |
95 | 09:07:57.293 |  |  | RRC rrc-cip b97cd7aa117ef95002e2258e299f509... |  |  |
96 | 09:07:57.293 |  |  | RRC rrc-int 2647d51dfb015d8a2b91a07e6d666db... |  |  |
97 | 09:07:57.293 |  |  | RRC up-cip 469a67806161ec4e86a962e3c4613ede... |  |  |
98 | 09:07:57.293 |  |  | RRC up-int 2f2f16a0a88df8b8130d44412cb750a5... |  |  |
99 | 09:07:57.293 |  | ←RRC DCCH Security Mode Command |  |  |
100 | 09:07:57.293 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
101 | 09:07:57.331 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
102 | 09:07:57.331 |  | →RRC DCCH Security Mode Complete |  |  |
103 | 09:07:57.331 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
104 | 09:07:57.331 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
105 | 09:07:57.371 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
106 | 09:07:57.371 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
107 | 09:08:08.291 | →enobeB PCAP frame→ TCP |  |  |  |
108 | 09:08:08.294 |  | ←enobeB PCAP frame← TCP |  |  |
109 | 09:08:08.331 | →enobeB PCAP frame→ TCP |  |  |  |
110 | 09:08:08.419 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
111 | 09:08:08.422 |  | ←enobeB PCAP frame← TCP |  |  |
112 | 09:08:08.428 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
113 | 09:08:08.451 | →enobeB PCAP frame→ TCP |  |  |  |
114 | 09:08:08.585 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 16)
115 | 09:08:08.587 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
116 | 09:08:08.591 |  | ←enobeB PCAP frame← TCP |  |  |
117 | 09:08:08.592 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
118 | 09:08:08.611 | →enobeB PCAP frame→ TCP |  |  |  |
119 | 09:08:08.657 |  |  |  |  | →HTTP GET | HTTP-Proxy
120 | 09:08:08.659 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
121 | 09:08:08.662 |  | ←enobeB PCAP frame← TCP |  |  |
122 | 09:08:08.664 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:288: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
123 | 09:08:08.685 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
124 | 09:08:08.694 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
125 | 09:08:08.731 | →enobeB PCAP frame→ TCP |  |  |  |
126 | 09:08:10.731 | →enobeB PCAP frame→ DNS |  |  |  |
127 | 09:08:10.734 |  | ←enobeB PCAP frame← TCP |  |  |
128 | 09:08:10.771 | →enobeB PCAP frame→ TCP |  |  |  |
129 | 09:08:10.779 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
130 | 09:08:10.782 |  | ←enobeB PCAP frame← TCP |  |  |
131 | 09:08:10.788 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
132 | 09:08:10.811 | →enobeB PCAP frame→ TCP |  |  |  |
133 | 09:08:11.137 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:643: Client connected to IdM port (id 18)
134 | 09:08:11.139 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
135 | 09:08:11.142 |  | ←enobeB PCAP frame← TCP |  |  |
136 | 09:08:11.143 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
137 | 09:08:11.171 | →enobeB PCAP frame→ TCP |  |  |  |
138 | 09:08:11.177 |  |  |  |  | →HTTP GET | IDMS-Endpoint
139 | 09:08:11.179 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
140 | 09:08:11.182 |  | ←enobeB PCAP frame← TCP |  |  |
141 | 09:08:11.212 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
142 | 09:08:11.216 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:511: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
143 | 09:08:11.216 |  |  |  |  | MMICmd: Please provide user credentials: username and password
144 | 09:08:11.219 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
145 | 09:08:11.291 | →enobeB PCAP frame→ TCP |  |  |  |
146 | 09:08:15.898 |  |  |  |  | →HTTP POST | IDMS-Endpoint
147 | 09:08:15.899 | →enobeB PCAP frame→ HTTPS: POST /idms/userauth HTTP/1.1 |  |  |  |
148 | 09:08:15.902 |  | ←enobeB PCAP frame← TCP |  |  |
149 | 09:08:15.913 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
150 | 09:08:15.915 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:516: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
151 | 09:08:15.919 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
152 | 09:08:15.971 | →enobeB PCAP frame→ TCP |  |  |  |
153 | 09:08:15.976 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:679: IdM port - Client closed the connection (id 18)
154 | 09:08:15.979 | →enobeB PCAP frame→ TCP |  |  |  |
155 | 09:08:15.982 |  | ←enobeB PCAP frame← TCP |  |  |
156 | 09:08:16.011 | →enobeB PCAP frame→ TCP |  |  |  |
157 | 09:08:16.651 | →enobeB PCAP frame→ TCP |  |  |  |
158 | 09:08:16.654 |  | ←enobeB PCAP frame← TCP |  |  |
159 | 09:08:16.691 | →enobeB PCAP frame→ TCP |  |  |  |
160 | 09:08:16.739 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
161 | 09:08:16.742 |  | ←enobeB PCAP frame← TCP |  |  |
162 | 09:08:16.745 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
163 | 09:08:16.771 | →enobeB PCAP frame→ TCP |  |  |  |
164 | 09:08:16.856 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:643: Client connected to IdM port (id 18)
165 | 09:08:16.859 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
166 | 09:08:16.862 |  | ←enobeB PCAP frame← TCP |  |  |
167 | 09:08:16.863 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
168 | 09:08:16.891 | →enobeB PCAP frame→ TCP |  |  |  |
169 | 09:08:16.897 |  |  |  |  | →HTTP POST | IDMS-Endpoint
170 | 09:08:16.899 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
171 | 09:08:16.902 |  | ←enobeB PCAP frame← TCP |  |  |
172 | 09:08:16.937 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
173 | 09:08:16.939 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:521: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
174 | 09:08:16.944 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
175 | 09:08:17.011 | →enobeB PCAP frame→ TCP |  |  |  |
176 | 09:08:17.211 | →enobeB PCAP frame→ TCP |  |  |  |
177 | 09:08:17.214 |  | ←enobeB PCAP frame← TCP |  |  |
178 | 09:08:17.251 | →enobeB PCAP frame→ TCP |  |  |  |
179 | 09:08:17.259 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
180 | 09:08:17.263 |  | ←enobeB PCAP frame← TCP |  |  |
181 | 09:08:17.266 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
182 | 09:08:17.331 | →enobeB PCAP frame→ TCP |  |  |  |
183 | 09:08:17.337 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 19)
184 | 09:08:17.339 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
185 | 09:08:17.342 |  | ←enobeB PCAP frame← TCP |  |  |
186 | 09:08:17.343 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
187 | 09:08:17.378 |  |  |  |  | →HTTP POST | HTTP-Proxy
188 | 09:08:17.379 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
189 | 09:08:17.382 |  | ←enobeB PCAP frame← TCP |  |  |
190 | 09:08:17.404 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:541: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
191 | 09:08:17.410 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
192 | 09:08:17.418 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
193 | 09:08:17.451 | →enobeB PCAP frame→ TCP |  |  |  |
194 | 09:08:17.491 | →enobeB PCAP frame→ TCP |  |  |  |
195 | 09:08:17.494 |  | ←enobeB PCAP frame← TCP |  |  |
196 | 09:08:17.531 | →enobeB PCAP frame→ TCP |  |  |  |
197 | 09:08:17.539 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
198 | 09:08:17.542 |  | ←enobeB PCAP frame← TCP |  |  |
199 | 09:08:17.545 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
200 | 09:08:17.571 | →enobeB PCAP frame→ TCP |  |  |  |
201 | 09:08:17.577 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 20)
202 | 09:08:17.579 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
203 | 09:08:17.582 |  | ←enobeB PCAP frame← TCP |  |  |
204 | 09:08:17.583 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
205 | 09:08:17.658 |  |  |  |  | →HTTP POST | HTTP-Proxy
206 | 09:08:17.659 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
207 | 09:08:17.662 |  | ←enobeB PCAP frame← TCP |  |  |
208 | 09:08:17.724 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
209 | 09:08:17.724 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:545: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
210 | 09:08:17.731 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
211 | 09:08:17.771 | →enobeB PCAP frame→ TCP |  |  |  |
212 | 09:08:17.818 |  |  |  |  | →SIP REGISTER | P-CSCF
213 | 09:08:17.819 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
214 | 09:08:17.842 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:816: IMS UDP_s port 192.168.2.3:5062 configured
215 | 09:08:17.870 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:767: IMS TCP_s port 192.168.2.3:5062 configured!
216 | 09:08:17.873 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:825: IMS UDP_c port 192.168.2.3:5061 configured
217 | 09:08:17.881 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
218 | 09:08:18.579 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
219 | 09:08:18.667 |  |  |  |  | →SIP REGISTER | P-CSCF
220 | 09:08:18.692 |  |  |  |  | ←SIP 200 OK | P-CSCF
221 | 09:08:18.699 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
222 | 09:08:19.019 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
223 | 09:08:19.020 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 SIP over IPSEC: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 |  |  |  |
224 | 09:08:19.030 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
225 | 09:08:19.090 |  |  |  |  | ←SIP 200 OK | P-CSCF
226 | 09:08:19.090 |  |  |  |  | MIKEY | Media-Server
227 | 09:08:19.097 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
228 | 09:08:19.310 |  |  |  |  | XML→ | Media-Server
229 | 09:08:19.312 |  |  |  |  | XML→ | Media-Server
230 | 09:08:19.315 |  |  |  |  | ←XML | Media-Server
231 | 09:08:19.318 |  |  |  |  | ←SIP NOTIFY | P-CSCF
232 | 09:08:19.325 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:37019;transp... |  |  |
233 | 09:08:19.376 |  |  |  |  | →SIP 200 OK | P-CSCF
234 | 09:08:19.379 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
235 | 09:08:19.771 | →enobeB PCAP frame→ TCP |  |  |  |
236 | 09:08:19.774 |  | ←enobeB PCAP frame← TCP |  |  |
237 | 09:08:19.811 | →enobeB PCAP frame→ TCP |  |  |  |
238 | 09:08:19.819 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
239 | 09:08:19.822 |  | ←enobeB PCAP frame← TCP |  |  |
240 | 09:08:19.826 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
241 | 09:08:19.851 | →enobeB PCAP frame→ TCP |  |  |  |
242 | 09:08:19.936 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
243 | 09:08:19.939 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
244 | 09:08:19.942 |  | ←enobeB PCAP frame← TCP |  |  |
245 | 09:08:19.943 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
246 | 09:08:19.971 | →enobeB PCAP frame→ TCP |  |  |  |
247 | 09:08:19.977 |  |  |  |  | →HTTP GET | HTTP-Proxy
248 | 09:08:19.979 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-co... |  |  |  |
249 | 09:08:19.982 |  | ←enobeB PCAP frame← TCP |  |  |
250 | 09:08:19.986 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:642: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcptt-ue-configuration.xml
251 | 09:08:19.995 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
252 | 09:08:20.002 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
253 | 09:08:20.051 | →enobeB PCAP frame→ TCP |  |  |  |
254 | 09:08:20.088 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:674: Http Proxy port - Client closed the connection (id 25)
255 | 09:08:20.091 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
256 | 09:08:20.094 |  | ←enobeB PCAP frame← TCP |  |  |
257 | 09:08:20.131 | →enobeB PCAP frame→ TCP |  |  |  |
258 | 09:08:20.211 | →enobeB PCAP frame→ TCP |  |  |  |
259 | 09:08:20.214 |  | ←enobeB PCAP frame← TCP |  |  |
260 | 09:08:20.251 | →enobeB PCAP frame→ TCP |  |  |  |
261 | 09:08:20.259 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
262 | 09:08:20.262 |  | ←enobeB PCAP frame← TCP |  |  |
263 | 09:08:20.265 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
264 | 09:08:20.291 | →enobeB PCAP frame→ TCP |  |  |  |
265 | 09:08:20.376 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
266 | 09:08:20.379 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
267 | 09:08:20.382 |  | ←enobeB PCAP frame← TCP |  |  |
268 | 09:08:20.383 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
269 | 09:08:20.411 | →enobeB PCAP frame→ TCP |  |  |  |
270 | 09:08:20.417 |  |  |  |  | →HTTP GET | HTTP-Proxy
271 | 09:08:20.419 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-... |  |  |  |
272 | 09:08:20.422 |  | ←enobeB PCAP frame← TCP |  |  |
273 | 09:08:20.428 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:647: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcptt-user-profile-49.xml
274 | 09:08:20.460 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
275 | 09:08:20.470 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
276 | 09:08:20.471 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
277 | 09:08:20.491 | →enobeB PCAP frame→ TCP |  |  |  |
278 | 09:08:20.499 | →enobeB PCAP frame→ TCP |  |  |  |
279 | 09:08:20.504 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:674: Http Proxy port - Client closed the connection (id 25)
280 | 09:08:20.507 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
281 | 09:08:20.510 |  | ←enobeB PCAP frame← TCP |  |  |
282 | 09:08:20.511 |  | ←enobeB PCAP frame← TCP |  |  |
283 | 09:08:20.515 | →enobeB PCAP frame→ TCP |  |  |  |
284 | 09:08:20.518 |  | ←enobeB PCAP frame← TCP |  |  |
285 | 09:08:20.571 | →enobeB PCAP frame→ TCP |  |  |  |
286 | 09:08:21.219 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
287 | 09:08:21.220 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
288 | 09:08:21.224 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
289 | 09:08:21.237 |  |  |  |  | ←SIP 200 OK | P-CSCF
290 | 09:08:21.237 |  |  |  |  | MIKEY | Media-Server
291 | 09:08:21.244 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
292 | 09:08:21.331 | →enobeB PCAP frame→ TCP |  |  |  |
293 | 09:08:21.334 |  | ←enobeB PCAP frame← TCP |  |  |
294 | 09:08:21.371 | →enobeB PCAP frame→ TCP |  |  |  |
295 | 09:08:21.379 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
296 | 09:08:21.382 |  | ←enobeB PCAP frame← TCP |  |  |
297 | 09:08:21.383 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
298 | 09:08:21.411 | →enobeB PCAP frame→ TCP |  |  |  |
299 | 09:08:21.444 |  |  |  |  | XML→ | Media-Server
300 | 09:08:21.445 |  |  |  |  | XML→ | Media-Server
301 | 09:08:21.448 |  |  |  |  | ←XML | Media-Server
302 | 09:08:21.456 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
303 | 09:08:21.456 |  |  |  |  | ←SIP NOTIFY | P-CSCF
304 | 09:08:21.459 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
305 | 09:08:21.462 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
306 | 09:08:21.463 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:37019;transp... |  |  |
307 | 09:08:21.491 | →enobeB PCAP frame→ TCP |  |  |  |
308 | 09:08:21.496 |  |  |  |  | →SIP 200 OK | P-CSCF
309 | 09:08:21.499 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
310 | 09:08:21.520 |  |  |  |  | →HTTP GET | HTTP-Proxy
311 | 09:08:21.523 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.servi... |  |  |  |
312 | 09:08:21.525 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:652: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
313 | 09:08:21.526 |  | ←enobeB PCAP frame← TCP |  |  |
314 | 09:08:21.533 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
315 | 09:08:21.541 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
316 | 09:08:21.571 | →enobeB PCAP frame→ TCP |  |  |  |
317 | 09:08:21.579 | →enobeB PCAP frame→ TCP |  |  |  |
318 | 09:08:21.608 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:674: Http Proxy port - Client closed the connection (id 25)
319 | 09:08:21.611 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
320 | 09:08:21.614 |  | ←enobeB PCAP frame← TCP |  |  |
321 | 09:08:21.619 | →enobeB PCAP frame→ TCP |  |  |  |
322 | 09:08:21.622 |  | ←enobeB PCAP frame← TCP |  |  |
323 | 09:08:21.651 | →enobeB PCAP frame→ TCP |  |  |  |
324 | 09:08:21.731 | →enobeB PCAP frame→ TCP |  |  |  |
325 | 09:08:21.734 |  | ←enobeB PCAP frame← TCP |  |  |
326 | 09:08:21.771 | →enobeB PCAP frame→ TCP |  |  |  |
327 | 09:08:21.779 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
328 | 09:08:21.782 |  | ←enobeB PCAP frame← TCP |  |  |
329 | 09:08:21.784 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
330 | 09:08:21.811 | →enobeB PCAP frame→ TCP |  |  |  |
331 | 09:08:21.896 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
332 | 09:08:21.899 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
333 | 09:08:21.902 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
334 | 09:08:21.931 | →enobeB PCAP frame→ TCP |  |  |  |
335 | 09:08:21.936 |  |  |  |  | →HTTP GET | HTTP-Proxy
336 | 09:08:21.938 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:657: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at /xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
337 | 09:08:21.939 | →enobeB PCAP frame→ HTTPS: GET /xcap.gms.mcstaasting.com/org.openmobileallian... |  |  |  |
338 | 09:08:21.942 |  | ←enobeB PCAP frame← TCP |  |  |
339 | 09:08:21.943 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
340 | 09:08:21.950 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
341 | 09:08:21.951 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
342 | 09:08:21.971 | →enobeB PCAP frame→ TCP |  |  |  |
343 | 09:08:21.979 | →enobeB PCAP frame→ TCP |  |  |  |
344 | 09:08:22.048 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:674: Http Proxy port - Client closed the connection (id 25)
345 | 09:08:22.051 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
346 | 09:08:22.055 |  | ←enobeB PCAP frame← TCP |  |  |
347 | 09:08:22.091 | →enobeB PCAP frame→ TCP |  |  |  |
348 | 09:08:22.299 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
349 | 09:08:22.300 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
350 | 09:08:22.308 |  |  |  |  | →SIP PUBLISH | P-CSCF
351 | 09:08:22.351 |  |  |  |  | MIKEY | Media-Server
352 | 09:08:22.379 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
353 | 09:08:22.380 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
354 | 09:08:22.381 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
355 | 09:08:22.579 |  |  |  |  | XML→ | Media-Server
356 | 09:08:22.583 |  |  |  |  | ←SIP 200 OK | P-CSCF
357 | 09:08:22.586 |  |  |  |  | ←SIP 200 OK | P-CSCF
358 | 09:08:22.586 |  |  |  |  | MIKEY | Media-Server
359 | 09:08:22.590 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
360 | 09:08:22.593 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
361 | 09:08:22.791 |  |  |  |  | XML→ | Media-Server
362 | 09:08:22.793 |  |  |  |  | XML→ | Media-Server
363 | 09:08:22.831 |  |  |  |  | ←XML | Media-Server
364 | 09:08:22.836 |  |  |  |  | ←SIP NOTIFY | P-CSCF
365 | 09:08:22.843 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:37019;transp... |  |  |
366 | 09:08:22.899 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
367 | 09:08:22.900 |  |  |  |  | →SIP 200 OK | P-CSCF
368 | 09:08:22.911 |  |  |  |  | ←XML | Media-Server
369 | 09:08:22.929 |  |  |  |  | ←SIP MESSAGE | P-CSCF
370 | 09:08:22.936 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
371 | 09:08:23.737 |  |  |  |  | →SIP 200 OK | P-CSCF
372 | 09:08:23.739 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
373 | 09:08:23.744 |  |  |  |  | Info: MCX_IMS_CommonProcedures.ttcn:155: MESSAGE/200OK Table 5.3.2.3-2 Steps 7-8 Done
374 | 09:08:23.753 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
375 | 09:08:23.771 | →enobeB PCAP frame→ TCP |  |  |  |
376 | 09:08:23.811 | →enobeB PCAP frame→ TCP |  |  |  |
377 | 09:08:25.746 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
378 | 09:08:25.777 |  | ←RRC DCCH RRC Connection Release |  |  |
379 | 09:08:25.778 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
380 | 09:08:25.793 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
381 | 09:08:25.807 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:737: SRTP config: Master Key: 47532719411470D04BDE9195CBA4EC9A, Master Salt: 5B61012BFBD272B60479124B, MKI: 2439E618
382 | 09:08:25.807 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
383 | 09:08:25.810 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
384 | 09:08:25.811 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
385 | 09:08:25.826 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
386 | 09:08:25.826 |  |  |  |  | ←XML | Media-Server
387 | 09:08:25.849 |  |  |  |  | ←SIP INVITE | P-CSCF
388 | 09:08:26.298 |  | ←enobeB PCAP frame← LTE RRC PCCH Paging (1 PagingRecord) |  |  |
389 | 09:08:26.298 |  | ←RRC PCCH Paging |  |  |
390 | 09:08:26.328 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
391 | 09:08:26.328 |  | →RRC CCCH RRC Connection Request |  |  |
392 | 09:08:26.328 |  | ←RRC CCCH RRC Connection Setup |  |  |
393 | 09:08:26.328 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
394 | 09:08:26.371 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
395 | 09:08:26.371 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
396 | 09:08:26.371 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
397 | 09:08:26.371 |  |  |  | →NAS EMM Service request |  |
398 | 09:08:26.371 |  |  |  | NAS K-enb a6cbd36aa06d89f3edb6671f0810d8e19... |  |
399 | 09:08:26.372 |  |  | RRC K-enb a6cbd36aa06d89f3edb6671f0810d8e19... |  |  |
400 | 09:08:26.373 |  |  | RRC rrc-cip 0d0083302da28ae9fe259d60f6ba25f... |  |  |
401 | 09:08:26.373 |  |  | RRC rrc-int 26b8c893882a8ff2201feb4cbac867b... |  |  |
402 | 09:08:26.373 |  |  | RRC up-cip 70ee20d38a91fc60a056962cb68085c4... |  |  |
403 | 09:08:26.373 |  |  | RRC up-int 55084dbbae4aa6d609ae0a6371fd8883... |  |  |
404 | 09:08:26.373 |  | ←RRC DCCH Security Mode Command |  |  |
405 | 09:08:26.373 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
406 | 09:08:26.411 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
407 | 09:08:26.411 |  | →RRC DCCH Security Mode Complete |  |  |
408 | 09:08:26.411 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
409 | 09:08:26.411 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
410 | 09:08:26.451 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
411 | 09:08:26.451 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
412 | 09:08:26.453 |  | ←enobeB PCAP frame← SIP over IPSEC: INVITE sip:PublicUserId-A@192.168.3.2:37019;transp... |  |  |
413 | 09:08:26.497 |  |  |  |  | →SIP 100 Trying | P-CSCF
414 | 09:08:26.499 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 100 Trying |  |  |  |
415 | 09:08:26.538 |  |  |  |  | →SIP 183 Session Progress | P-CSCF
416 | 09:08:26.539 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 183 Session Progress |  |  |  |
417 | 09:08:26.559 |  |  |  |  | ←SIP PRACK | P-CSCF
418 | 09:08:26.567 |  | ←enobeB PCAP frame← SIP over IPSEC: PRACK sip:PublicUserId-A@192.168.3.2:37019;transpo... |  |  |
419 | 09:08:26.617 |  |  |  |  | →SIP 200 OK | P-CSCF
420 | 09:08:26.619 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
421 | 09:08:26.869 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
422 | 09:08:26.869 |  | [EMBEDDED NAS IN NEXT RRC] TP Unknown message (type=0x3f) |  |  |
423 | 09:08:26.869 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
424 | 09:08:26.870 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
425 | 09:08:26.931 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
426 | 09:08:26.931 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
427 | 09:08:26.931 |  | →RRC DCCH UL Information Transfer |  |  |
428 | 09:08:26.931 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x0) |  |  |
429 | 09:08:26.931 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
430 | 09:08:26.996 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
431 | 09:08:27.376 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:648: Verdict: Pass
432 | 09:08:27.478 |  |  |  |  | MMICmd: Please Accept the Call
433 | 09:08:34.859 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
434 | 09:08:34.860 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
435 | 09:08:34.862 |  |  |  |  | →SIP 200 OK | P-CSCF
436 | 09:08:34.869 |  |  |  |  | XML→ | Media-Server
437 | 09:08:34.871 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:657: 200 OK Verdict: Pass
438 | 09:08:34.871 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:307: Step 1 Verdict: Pass
439 | 09:08:34.872 |  |  |  |  | ←SIP ACK | P-CSCF
440 | 09:08:34.873 |  |  |  |  | ←SIP BYE | P-CSCF
441 | 09:08:34.879 |  | ←enobeB PCAP frame← SIP over IPSEC: ACK sip:PublicUserId-A@192.168.3.2:37019;transport... |  |  |
442 | 09:08:34.880 |  | ←enobeB PCAP frame← SIP over IPSEC: BYE sip:PublicUserId-A@192.168.3.2:37019;transport... |  |  |
443 | 09:08:35.897 |  |  |  |  | →SIP 200 OK | P-CSCF
444 | 09:08:35.899 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
445 | 09:08:36.571 | →enobeB PCAP frame→ |  |  |  |
446 | 09:08:37.906 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
447 | 09:08:37.932 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
448 | 09:08:37.932 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xa) |  |  |
449 | 09:08:37.932 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
450 | 09:08:37.933 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
451 | 09:08:37.971 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
452 | 09:08:37.971 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
453 | 09:08:37.971 |  | →RRC DCCH UL Information Transfer |  |  |
454 | 09:08:37.971 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x8) |  |  |
455 | 09:08:37.971 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
456 | 09:08:38.048 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
457 | 09:08:38.049 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
458 | 09:08:38.103 |  | ←RRC DCCH RRC Connection Release |  |  |
459 | 09:08:38.104 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
460 | 09:08:38.112 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
461 | 09:08:38.113 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:313: Step 8 Verdict: Pass
462 | 09:08:38.117 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
463 | 09:08:38.120 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
464 | 09:08:38.135 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
465 | 09:08:38.135 |  |  |  |  | ←XML | Media-Server
466 | 09:08:38.170 |  |  |  |  | ←SIP INVITE | P-CSCF
467 | 09:08:39.098 |  | ←enobeB PCAP frame← LTE RRC PCCH Paging (1 PagingRecord) |  |  |
468 | 09:08:39.098 |  | ←RRC PCCH Paging |  |  |
469 | 09:08:39.128 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
470 | 09:08:39.128 |  | →RRC CCCH RRC Connection Request |  |  |
471 | 09:08:39.128 |  | ←RRC CCCH RRC Connection Setup |  |  |
472 | 09:08:39.128 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
473 | 09:08:39.171 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
474 | 09:08:39.171 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
475 | 09:08:39.171 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
476 | 09:08:39.172 |  |  | RRC K-enb 249052ae886df891c787e78718a3d5574... |  |  |
477 | 09:08:39.172 |  |  |  | →NAS EMM Service request |  |
478 | 09:08:39.172 |  |  |  | NAS K-enb 249052ae886df891c787e78718a3d5574... |  |
479 | 09:08:39.173 |  |  | RRC rrc-cip a1f4f64000f5c6565ce221679e73e78... |  |  |
480 | 09:08:39.173 |  |  | RRC rrc-int 43262c8a2812db6dd68ace106ca8cc1... |  |  |
481 | 09:08:39.173 |  |  | RRC up-cip 2338ff6cad08ff17b080043133af4949... |  |  |
482 | 09:08:39.173 |  |  | RRC up-int b9738fd090d12cde8e95127cd8c8d9c1... |  |  |
483 | 09:08:39.173 |  | ←RRC DCCH Security Mode Command |  |  |
484 | 09:08:39.173 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
485 | 09:08:39.211 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
486 | 09:08:39.211 |  | →RRC DCCH Security Mode Complete |  |  |
487 | 09:08:39.211 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
488 | 09:08:39.211 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
489 | 09:08:39.251 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
490 | 09:08:39.251 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
491 | 09:08:39.253 |  | ←enobeB PCAP frame← SIP over IPSEC: INVITE sip:PublicUserId-A@192.168.3.2:37019;transp... |  |  |
492 | 09:08:39.297 |  |  |  |  | →SIP 100 Trying | P-CSCF
493 | 09:08:39.299 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 100 Trying |  |  |  |
494 | 09:08:39.338 |  |  |  |  | →SIP 183 Session Progress | P-CSCF
495 | 09:08:39.339 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 183 Session Progress |  |  |  |
496 | 09:08:39.357 |  |  |  |  | ←SIP PRACK | P-CSCF
497 | 09:08:39.365 |  | ←enobeB PCAP frame← SIP over IPSEC: PRACK sip:PublicUserId-A@192.168.3.2:37019;transpo... |  |  |
498 | 09:08:39.417 |  |  |  |  | →SIP 200 OK | P-CSCF
499 | 09:08:39.419 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
500 | 09:08:39.426 |  |  |  |  | MMICmd: Make the MCPTT User decline the call
501 | 09:08:39.660 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
502 | 09:08:39.661 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x9) |  |  |
503 | 09:08:39.661 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
504 | 09:08:39.662 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
505 | 09:08:39.691 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
506 | 09:08:39.691 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
507 | 09:08:39.691 |  | →RRC DCCH UL Information Transfer |  |  |
508 | 09:08:39.691 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
509 | 09:08:39.691 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
510 | 09:08:39.779 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
511 | 09:08:42.065 |  |  |  |  | →SIP 480 Temporarily Unavailable | P-CSCF
512 | 09:08:42.075 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:329: Step 15 Verdict: Pass
513 | 09:08:42.083 |  |  |  |  | ←SIP ACK | P-CSCF
514 | 09:08:42.090 |  | ←enobeB PCAP frame← SIP over IPSEC: ACK sip:PublicUserId-A@192.168.3.2:37019;transport... |  |  |
515 | 09:08:44.081 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
516 | 09:08:44.092 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
517 | 09:08:44.093 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x5) |  |  |
518 | 09:08:44.093 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
519 | 09:08:44.094 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
520 | 09:08:44.131 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
521 | 09:08:44.131 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
522 | 09:08:44.131 |  | →RRC DCCH UL Information Transfer |  |  |
523 | 09:08:44.131 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x9) |  |  |
524 | 09:08:44.131 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
525 | 09:08:44.205 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
526 | 09:08:44.207 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
527 | 09:08:44.246 |  | ←RRC DCCH RRC Connection Release |  |  |
528 | 09:08:44.247 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
529 | 09:08:44.251 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
530 | 09:08:44.253 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
531 | 09:08:44.255 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
532 | 09:08:45.004 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.