MSG #89 2021-09-06 12:46:01.117
RRC

     CCCH: RRC Connection Setup
    {
      message c1: rrcConnectionSetup: {
        rrc-TransactionIdentifier 0,
        criticalExtensions c1: rrcConnectionSetup-r8: {
          radioResourceConfigDedicated {
            srb-ToAddModList {
              {
                srb-Identity 1,
                rlc-Config explicitValue: am: {
                  ul-AM-RLC {
                    t-PollRetransmit ms60,
                    pollPDU pInfinity,
                    pollByte kBinfinity,
                    maxRetxThreshold t32
                  },
                  dl-AM-RLC {
                    t-Reordering ms45,
                    t-StatusProhibit ms0
                  }
                },
                logicalChannelConfig defaultValue: NULL
              }
            },
            mac-MainConfig explicitValue: {
              ul-SCH-Config {
                maxHARQ-Tx n5,
                periodicBSR-Timer sf20,
                retxBSR-Timer sf320,
                ttiBundling FALSE
              },
              drx-Config release: NULL,
              timeAlignmentTimerDedicated infinity,
              phr-Config setup: {
                periodicPHR-Timer sf500,
                prohibitPHR-Timer sf200,
                dl-PathlossChange dB3
              }
            },
            physicalConfigDedicated {
              pdsch-ConfigDedicated {
                p-a dB0
              },
              pucch-ConfigDedicated {
                ackNackRepetition release: NULL
              },
              pusch-ConfigDedicated {
                betaOffset-ACK-Index 9,
                betaOffset-RI-Index 6,
                betaOffset-CQI-Index 6
              },
              uplinkPowerControlDedicated {
                p0-UE-PUSCH 0,
                deltaMCS-Enabled en0,
                accumulationEnabled TRUE,
                p0-UE-PUCCH 0,
                pSRS-Offset 3
              },
              cqi-ReportConfig {
                nomPDSCH-RS-EPRE-Offset 0,
                cqi-ReportPeriodic setup: {
                  cqi-PUCCH-ResourceIndex 0,
                  cqi-pmi-ConfigIndex 38,
                  cqi-FormatIndicatorPeriodic widebandCQI: NULL,
                  simultaneousAckNackAndCQI FALSE
                }
              },
              soundingRS-UL-ConfigDedicated setup: {
                srs-Bandwidth bw1,
                srs-HoppingBandwidth hbw0,
                freqDomainPosition 0,
                duration TRUE,
                srs-ConfigIndex 37,
                transmissionComb 0,
                cyclicShift cs0
              },
              schedulingRequestConfig setup: {
                sr-PUCCH-ResourceIndex 0,
                sr-ConfigIndex 35,
                dsr-TransMax n64
              }
            }
          }
        }
      }
    }