MSG #22 2021-09-06 12:45:54.678

    enobeB PCAP frame

    {
      "layers": {
        "frame": {
          "frame.encap_type": "45",
          "frame.time": "Sep  6, 2021 12:45:54.678239000 CEST",
          "frame.offset_shift": "0.000000000",
          "frame.time_epoch": "1630925154.678239000",
          "frame.time_delta": "0.007908000",
          "frame.time_delta_displayed": "0.060917000",
          "frame.time_relative": "93.555108000",
          "frame.number": "8191",
          "frame.len": "76",
          "frame.cap_len": "76",
          "frame.marked": "0",
          "frame.ignored": "0",
          "frame.protocols": "user_dlt:mac-lte-framed:mac-lte:rlc-lte:pdcp-lte:lte_rrc:nas-eps"
        },
        "user_dlt": "DLT: 147, Payload: mac-lte-framed (mac-lte-framed)",
        "mac-lte": {
          "mac-lte.context": "",
          "mac-lte.context_tree": {
            "mac-lte.radio-type": "1",
            "mac-lte.direction": "0",
            "mac-lte.ueid": "540",
            "mac-lte.sfn": "981",
            "mac-lte.subframe": "6",
            "mac-lte.rnti": "600",
            "mac-lte.rnti-type": "3",
            "mac-lte.is-predefined-frame": "0",
            "mac-lte.length": "51",
            "mac-lte.ul-grant-size": "51",
            "mac-lte.crc-status": "1",
            "mac-lte.carrier-id": "0",
            "mac-lte.ul-tti-count": "1"
          },
          "mac-lte.ul-phy": "",
          "mac-lte.ul-phy_tree": {
            "mac-lte.ul-phy.modulation-type": "4",
            "mac-lte.ul-phy.tbs-index": "19",
            "mac-lte.ul-phy.resource-block-length": "1",
            "mac-lte.ul-phy.resource-block-start": "7",
            "mac-lte.ul-phy.harq-id": "0",
            "mac-lte.ul-phy.ndi": "0"
          },
          "mac-lte.ulsch.header": "",
          "mac-lte.ulsch.header_tree": {
            "mac-lte.sch.subheader": "",
            "mac-lte.sch.subheader_tree": {
              "mac-lte.sch.reserved": "0x00000000",
              "mac-lte.sch.format2": "0",
              "mac-lte.sch.extended": "0x00000000",
              "mac-lte.ulsch.lcid": "0x0000001f"
            }
          },
          "mac-lte.control.bsr": "",
          "mac-lte.control.bsr_tree": {
            "mac-lte.control.bsr.buffer-size-0": "0",
            "mac-lte.control.bsr.buffer-size-1": "0",
            "mac-lte.control.bsr.buffer-size-2": "0",
            "mac-lte.control.bsr.buffer-size-3": "0"
          },
          "mac-lte.sch.header-only": "0",
          "mac-lte.sch.sdu": "b0:01:00:60:00:00:00:00",
          "rlc-lte": {
            "rlc-lte.context": "",
            "rlc-lte.context_tree": {
              "rlc-lte.direction": "0",
              "rlc-lte.mode": "4",
              "rlc-lte.ueid": "540",
              "rlc-lte.channel-type": "4",
              "rlc-lte.channel-id": "1",
              "rlc-lte.pdu-length": "8",
              "rlc-lte.am-seqnum-length": "10"
            },
            "rlc-lte.am": "",
            "rlc-lte.am.header": "",
            "rlc-lte.am.header_tree": {
              "rlc-lte.am.frame-type": "0x00000001",
              "rlc-lte.am.rf": "0x00000000",
              "rlc-lte.am.p": "0x00000001",
              "rlc-lte.am.fi": "0x00000002",
              "rlc-lte.am.fixed.e": "0x00000000",
              "rlc-lte.am.fixed.sn": "1"
            },
            "rlc-lte.sequence-analysis": "",
            "rlc-lte.sequence-analysis_tree": {
              "rlc-lte.sequence-analysis.previous-frame": "8190",
              "rlc-lte.sequence-analysis.ok": "1"
            },
            "rlc-lte.am.data": "00:60:00:00:00:00",
            "rlc-lte.reassembly-info": "",
            "rlc-lte.reassembly-info_tree": {
              "rlc-lte.reassembly-info.number-of-segments": "2",
              "rlc-lte.reassembly-info.total-length": "104",
              "rlc-lte.reassembly-info.segment": {
                "rlc-lte.reassembly-info.segment.sn": "1",
                "rlc-lte.reassembly-info.segment.frame": "8191",
                "rlc-lte.reassembly-info.segment.length": "6"
              }
            },
            "pdcp-lte": {
              "pdcp-lte.configuration": "",
              "pdcp-lte.configuration_tree": {
                "pdcp-lte.direction": "0",
                "pdcp-lte.plane": "1",
                "pdcp-lte.ueid": "540",
                "pdcp-lte.channel-type": "1",
                "pdcp-lte.channel-id": "1",
                "pdcp-lte.rohc.compression": "0"
              },
              "pdcp-lte.reserved": "0",
              "pdcp-lte.seq-num": "0",
              "pdcp-lte.sequence-analysis": "",
              "pdcp-lte.sequence-analysis_tree": {
                "pdcp-lte.sequence-analysis.expected-sn": "0",
                "pdcp-lte.sequence-analysis.ok": "1"
              },
              "lte_rrc": {
                "lte_rrc": "LTE Radio Resource Control (RRC) protocol",
                "lte-rrc.UL_DCCH_Message_element": {
                  "per.choice_index": "0",
                  "lte-rrc.message": "0",
                  "lte-rrc.message_tree": {
                    "per.choice_index": "4",
                    "lte-rrc.c1": "4",
                    "lte-rrc.c1_tree": {
                      "lte-rrc.rrcConnectionSetupComplete_element": {
                        "lte-rrc.rrc_TransactionIdentifier": "0",
                        "per.choice_index": "0",
                        "lte-rrc.criticalExtensions": "0",
                        "lte-rrc.criticalExtensions_tree": {
                          "per.choice_index": "0",
                          "lte-rrc.c1": "0",
                          "lte-rrc.c1_tree": {
                            "lte-rrc.rrcConnectionSetupComplete_r8_element": {
                              "per.optional_field_bit": "1",
                              "lte-rrc.selectedPLMN_Identity": "1",
                              "lte-rrc.registeredMME_element": {
                                "per.optional_field_bit": "0",
                                "lte-rrc.mmegi": "80:01",
                                "lte-rrc.mmec": "01"
                              },
                              "per.octet_string_length": "92",
                              "lte-rrc.dedicatedInfoNAS": "17:69:66:1a:23:05:07:41:32:0b:f6:00:f1:10:80:01:01:fc:09:8d:d9:05:f0:70:c0:40:19:00:05:02:01:d0:31:d1:52:00:f1:10:00:01:5c:0a:00:31:03:e5:e0:3e:13:00:f1:10:00:01:11:03:57:58:a6:20:0c:60:14:04:e2:91:81:0f:12:1e:50:00:00:40:08:04:02:60:04:00:02:1f:02:5d:01:03:e0:c1:10:02:1a:00",
                              "lte-rrc.dedicatedInfoNAS_tree": {
                                "nas-eps": {
                                  "nas_eps.security_header_type": "0",
                                  "gsm_a.L3_protocol_discriminator": "0x00000007",
                                  "nas_eps.msg_auth_code": "0x69661a23",
                                  "nas_eps.seq_no": "5",
                                  "nas_eps.nas_msg_emm_type": "65",
                                  "nas_eps.emm.tsc": "0",
                                  "nas_eps.emm.nas_key_set_id": "3",
                                  "nas_eps.spare_bits": "0x00000000",
                                  "nas_eps.emm.eps_att_type": "2",
                                  "EPS mobile identity": {
                                    "gsm_a.len": "11",
                                    "nas_eps.emm.odd_even": "0",
                                    "nas_eps.emm.type_of_id": "6",
                                    "e212.mcc": "1",
                                    "e212.mnc": "1",
                                    "nas_eps.emm.mme_grp_id": "32769",
                                    "nas_eps.emm.mme_code": "1",
                                    "nas_eps.emm.m_tmsi": "4228484569",
                                    "3gpp.tmsi": "4228484569"
                                  },
                                  "UE network capability": {
                                    "gsm_a.len": "5",
                                    "nas_eps.emm.eea0": "1",
                                    "nas_eps.emm.128eea1": "1",
                                    "nas_eps.emm.128eea2": "1",
                                    "nas_eps.emm.eea3": "1",
                                    "nas_eps.emm.eea4": "0",
                                    "nas_eps.emm.eea5": "0",
                                    "nas_eps.emm.eea6": "0",
                                    "nas_eps.emm.eea7": "0",
                                    "nas_eps.emm.eia0": "0",
                                    "nas_eps.emm.128eia1": "1",
                                    "nas_eps.emm.128eia2": "1",
                                    "nas_eps.emm.eia3": "1",
                                    "nas_eps.emm.eia4": "0",
                                    "nas_eps.emm.eia5": "0",
                                    "nas_eps.emm.eia6": "0",
                                    "nas_eps.emm.eia7": "0",
                                    "nas_eps.emm.uea0": "1",
                                    "nas_eps.emm.uea1": "1",
                                    "nas_eps.emm.uea2": "0",
                                    "nas_eps.emm.uea3": "0",
                                    "nas_eps.emm.uea4": "0",
                                    "nas_eps.emm.uea5": "0",
                                    "nas_eps.emm.uea6": "0",
                                    "nas_eps.emm.uea7": "0",
                                    "nas_eps.emm.emm_ucs2_supp": "0",
                                    "nas_eps.emm.uia1": "1",
                                    "nas_eps.emm.uia2": "0",
                                    "nas_eps.emm.uia3": "0",
                                    "nas_eps.emm.uia4": "0",
                                    "nas_eps.emm.uia5": "0",
                                    "nas_eps.emm.uia6": "0",
                                    "nas_eps.emm.uia7": "0",
                                    "nas_eps.emm.prose_dd_cap": "0",
                                    "nas_eps.emm.prose_cap": "0",
                                    "nas_eps.emm.h245_ash_cap": "0",
                                    "nas_eps.emm.acc_csfb_cap": "1",
                                    "nas_eps.emm.lpp_cap": "1",
                                    "nas_eps.emm.lcs_cap": "0",
                                    "nas_eps.emm.1xsrvcc_cap": "0",
                                    "nas_eps.emm.nf_cap": "1"
                                  },
                                  "ESM message container": {
                                    "gsm_a.len": "5",
                                    "nas_eps.emm.esm_msg_cont": "02:01:d0:31:d1",
                                    "nas_eps.emm.esm_msg_cont_tree": {
                                      "nas_eps.bearer_id": "0",
                                      "gsm_a.L3_protocol_discriminator": "0x00000002",
                                      "nas_eps.esm.proc_trans_id": "1",
                                      "nas_eps.nas_msg_esm_type": "208",
                                      "nas_eps.esm_pdn_type": "3",
                                      "nas_eps.esm_request_type": "1",
                                      "ESM information transfer flag": {
                                        "gsm_a.common.elem_id": "0x0000000d",
                                        "nas_eps.spare_bits": "0x00000000",
                                        "nas_eps.esm.eit": "1"
                                      }
                                    }
                                  },
                                  "Tracking area identity - Last visited registered TAI": {
                                    "nas_eps.emm.elem_id": "0x00000052",
                                    "e212.tai.mcc": "1",
                                    "e212.tai.mnc": "1",
                                    "nas_eps.emm.tai_tac": "1"
                                  },
                                  "DRX Parameter": {
                                    "gsm_a.gm.elem_id": "0x0000005c",
                                    "gsm_a.gm.gmm.split_pg_cycle_code": "10",
                                    "gsm_a.gm.gmm.cn_spec_drx_cycle_len_coef": "0",
                                    "gsm_a.gm.gmm.split_on_ccch": "0",
                                    "gsm_a.gm.gmm.non_drx_timer": "0"
                                  },
                                  "MS Network Capability": {
                                    "gsm_a.gm.elem_id": "0x00000031",
                                    "gsm_a.len": "3",
                                    "gsm_a.gm.gmm.net_cap.gea1": "1",
                                    "gsm_a.gm.gmm.net_cap.smdch": "1",
                                    "gsm_a.gm.gmm.net_cap.smgprs": "1",
                                    "gsm_a.gm.gmm.net_cap.ucs2": "0",
                                    "gsm_a.gm.gmm.net_cap.ss_scr_ind": "0x00000001",
                                    "gsm_a.gm.gmm.net_cap.solsa": "0",
                                    "gsm_a.gm.gmm.net_cap.rev": "1",
                                    "gsm_a.gm.gmm.net_cap.pfc": "1",
                                    "gsm_a.gm.gmm.net_cap.ext_gea_bits": "0x00000030",
                                    "gsm_a.gm.gmm.net_cap.ext_gea_bits_tree": {
                                      "gsm_a.gm.gmm.net_cap.gea2": "1",
                                      "gsm_a.gm.gmm.net_cap.gea3": "1",
                                      "gsm_a.gm.gmm.net_cap.gea4": "0",
                                      "gsm_a.gm.gmm.net_cap.gea5": "0",
                                      "gsm_a.gm.gmm.net_cap.gea6": "0",
                                      "gsm_a.gm.gmm.net_cap.gea7": "0"
                                    },
                                    "gsm_a.gm.gmm.net_cap.lcs": "0",
                                    "gsm_a.gm.gmm.net_cap.ps_irat_iu": "0",
                                    "gsm_a.gm.gmm.net_cap.ps_irat_s1": "0",
                                    "gsm_a.gm.gmm.net_cap.comb_proc": "1",
                                    "gsm_a.gm.gmm.net_cap.isr": "1",
                                    "gsm_a.gm.gmm.net_cap.srvcc_to_geran": "1",
                                    "gsm_a.gm.gmm.net_cap.epc": "1",
                                    "gsm_a.gm.gmm.net_cap.nf": "1",
                                    "gsm_a.gm.gmm.net_cap.geran_net_sharing": "0"
                                  },
                                  "Location area identification - Old location area identification": {
                                    "nas_eps.common.elem_id": "0x00000013",
                                    "Location Area Identification (LAI) - 001/01/1": {
                                      "e212.lai.mcc": "1",
                                      "e212.lai.mnc": "1",
                                      "gsm_a.lac": "0x00000001"
                                    }
                                  },
                                  "Mobile station classmark 2": {
                                    "nas_eps.common.elem_id": "0x00000011",
                                    "gsm_a.len": "3",
                                    "gsm_a.spareb8": "0",
                                    "gsm_a.MSC_rev": "2",
                                    "gsm_a.ES_IND": "1",
                                    "gsm_a.A5_1_algorithm_sup": "0",
                                    "gsm_a.RF_power_capability": "7",
                                    "gsm_a.ps_sup_cap": "1",
                                    "gsm_a.SS_screening_indicator": "1",
                                    "gsm_a.SM_cap": "1",
                                    "gsm_a.VBS_notification_rec": "0",
                                    "gsm_a.VGCS_notification_rec": "0",
                                    "gsm_a.FC_frequency_cap": "0",
                                    "gsm_a.CM3": "1",
                                    "gsm_a.spareb7": "0",
                                    "gsm_a.LCS_VA_cap": "1",
                                    "gsm_a.UCS2_treatment": "0",
                                    "gsm_a.SoLSA": "0",
                                    "gsm_a.CMSP": "1",
                                    "gsm_a.A5_3_algorithm_sup": "1",
                                    "gsm_a.A5_2_algorithm_sup": "0"
                                  },
                                  "Mobile station classmark 3": {
                                    "nas_eps.common.elem_id": "0x00000020",
                                    "gsm_a.len": "12",
                                    "gsm_a.spare_bits": "0",
                                    "gsm_a.multi_bnd_sup_fields": "6",
                                    "gsm_a.multi_bnd_sup_fields_tree": {
                                      "gsm_a.classmark3.gsm1800Supported": "1",
                                      "gsm_a.classmark3.egsmSupported": "1",
                                      "gsm_a.classmark3.pgsmSupported": "0"
                                    },
                                    "gsm_a.classmark3.a5_bits": "0x00000000",
                                    "gsm_a.classmark3.a5_bits_tree": {
                                      "gsm_a.A5_7_algorithm_sup": "0",
                                      "gsm_a.A5_6_algorithm_sup": "0",
                                      "gsm_a.A5_5_algorithm_sup": "0",
                                      "gsm_a.A5_4_algorithm_sup": "0"
                                    },
                                    "gsm_a.classmark3.ass_radio_cap2": "1",
                                    "gsm_a.classmark3.ass_radio_cap1": "4",
                                    "gsm_a.classmark3.rsupport": "0",
                                    "gsm_a.classmark3.multislot_capabilities": "0",
                                    "gsm_a.UCS2_treatment": "0",
                                    "gsm_a.classmark3.ext_meas_cap": "0",
                                    "gsm_a.classmark3.ms_measurement_capability": "0",
                                    "gsm_a.classmark3.ms_pos_method_cap_present": "1",
                                    "gsm_a.classmark3.ms_pos_method": "0x00000007",
                                    "gsm_a.classmark3.ms_pos_method_tree": {
                                      "gsm_a.classmark3.ms_assisted_e_otd": "0",
                                      "gsm_a.classmark3.ms_based_e_otd": "0",
                                      "gsm_a.classmark3.ms_assisted_gps": "1",
                                      "gsm_a.classmark3.ms_based_gps": "1",
                                      "gsm_a.classmark3.ms_conventional_gps": "1"
                                    },
                                    "gsm_a.classmark3.ecsd_multi_slot_capability": "0",
                                    "gsm_a.classmark3.8_psk_struct_present": "0",
                                    "gsm_a.classmark3.gsm_400_band_info_present": "0",
                                    "gsm_a.classmark3.gsm_850_assoc_radio_cap_present": "1",
                                    "gsm_a.classmark3.gsm_850_assoc_radio_cap": "0x00000004",
                                    "gsm_a.classmark3.gsm_1900_assoc_radio_cap_present": "1",
                                    "gsm_a.classmark3.gsm_1900_assoc_radio_cap": "0x00000001",
                                    "gsm_a.classmark3.umts_fdd_rat_cap": "1",
                                    "gsm_a.classmark3.umts_384_mcps_tdd_rat_cap": "0",
                                    "gsm_a.classmark3.cdma_2000_rat_cap": "0",
                                    "gsm_a.classmark3.dtm_e_gprs_multi_slot_info_present": "0",
                                    "gsm_a.classmark3.single_band_support": "0",
                                    "gsm_a.classmark3.gsm_750_assoc_radio_cap_present": "0",
                                    "gsm_a.classmark3.umts_128_mcps_tdd_rat_cap": "0",
                                    "gsm_a.classmark3.geran_feature_package_1": "1",
                                    "gsm_a.classmark3.ext_dtm_e_gprs_info_present": "0",
                                    "gsm_a.classmark3.high_multislot_cap_present": "0",
                                    "gsm_a.classmark3.geran_iu_mode_support": "0",
                                    "gsm_a.classmark3.geran_feature_package_2": "0",
                                    "gsm_a.classmark3.gmsk_multislot_power_prof": "3",
                                    "gsm_a.classmark3.8_psk_multislot_power_prof": "3",
                                    "gsm_a.classmark3.t_gsm_900_assoc_radio_cap_present": "0",
                                    "gsm_a.classmark3.downlink_adv_receiver_perf": "1",
                                    "gsm_a.classmark3.dtm_enhancements_capability": "0",
                                    "gsm_a.classmark3.dtm_e_gprs_high_mutli_slot_info_present": "0",
                                    "gsm_a.classmark3.repeated_acch_cap": "1",
                                    "gsm_a.classmark3.gsm_710_assoc_radio_cap_present": "0",
                                    "gsm_a.classmark3.t_gsm_810_assoc_radio_cap_present": "0",
                                    "gsm_a.classmark3.ciphering_mode_setting_cap": "0",
                                    "gsm_a.classmark3.additional_positioning_caps": "0",
                                    "gsm_a.classmark3.e_utra_fdd_support": "1",
                                    "gsm_a.classmark3.e_utra_tdd_support": "1",
                                    "gsm_a.classmark3.e_utra_meas_and_report_support": "1",
                                    "gsm_a.classmark3.prio_based_resel_support": "1",
                                    "gsm_a.classmark3.utra_csg_cells_reporting": "0",
                                    "gsm_a.classmark3.vamos_level": "1",
                                    "gsm_a.classmark3.tighter_cap": "1",
                                    "gsm_a.classmark3.selective_ciph_down_sacch": "0",
                                    "gsm_a.classmark3.cs_to_ps_srvcc_geran_to_utra": "0",
                                    "gsm_a.classmark3.cs_to_ps_srvcc_geran_to_eutra": "0",
                                    "gsm_a.classmark3.geran_network_sharing_support": "0",
                                    "gsm_a.classmark3.eutra_wb_rsrq_support": "0",
                                    "gsm_a.classmark3.er_band_support": "0",
                                    "gsm_a.classmark3.utra_mfbi_support": "0",
                                    "gsm_a.classmark3.eutra_mfbi_support": "0",
                                    "gsm_a.classmark3.ext_tsc_set_cap_support": "0",
                                    "gsm_a.classmark3.ext_earfcn_value_range": "0",
                                    "Extraneous Data, dissector bug or later version spec(report to wireshark.org)": {
                                      "_ws.expert": {
                                        "gsm_a.extraneous_data": "",
                                        "_ws.expert.message": "Extraneous Data, dissector bug or later version spec(report to wireshark.org)",
                                        "_ws.expert.severity": "4194304",
                                        "_ws.expert.group": "150994944"
                                      }
                                    }
                                  },
                                  "Supported Codec List - Supported Codecs": {
                                    "gsm_a.dtap.elem_id": "0x00000040",
                                    "gsm_a.len": "8",
                                    "gsm_a.dtap.sysid": "0x00000000",
                                    "gsm_a.dtap.bitmap_length": "2",
                                    "Codec Bitmap for SysID 1": {
                                      "gsm_a.dtap.codec.tdma_efr": "0",
                                      "gsm_a.dtap.codec.umts_amr_2": "1",
                                      "gsm_a.dtap.codec.umts_amr": "1",
                                      "gsm_a.dtap.codec.hr_amr": "0",
                                      "gsm_a.dtap.codec.fr_amr": "0",
                                      "gsm_a.dtap.codec.gsm_efr": "0",
                                      "gsm_a.dtap.codec.gsm_hr": "0",
                                      "gsm_a.dtap.codec.gsm_fr": "0",
                                      "gsm_a.spare_bits": "0",
                                      "gsm_a.dtap.codec.umts_evs": "0",
                                      "gsm_a.dtap.codec.ohr_amr_wb": "0",
                                      "gsm_a.dtap.codec.ofr_amr_wb": "0",
                                      "gsm_a.dtap.codec.ohr_amr": "0",
                                      "gsm_a.dtap.codec.umts_amr_wb": "1",
                                      "gsm_a.dtap.codec.fr_amr_wb": "0",
                                      "gsm_a.dtap.codec.pdc_efr": "0"
                                    },
                                    "Codec Bitmap for SysID 2": {
                                      "gsm_a.dtap.codec.tdma_efr": "0",
                                      "gsm_a.dtap.codec.umts_amr_2": "0",
                                      "gsm_a.dtap.codec.umts_amr": "0",
                                      "gsm_a.dtap.codec.hr_amr": "1",
                                      "gsm_a.dtap.codec.fr_amr": "1",
                                      "gsm_a.dtap.codec.gsm_efr": "1",
                                      "gsm_a.dtap.codec.gsm_hr": "1",
                                      "gsm_a.dtap.codec.gsm_fr": "1",
                                      "gsm_a.spare_bits": "0",
                                      "gsm_a.dtap.codec.umts_evs": "0",
                                      "gsm_a.dtap.codec.ohr_amr_wb": "0",
                                      "gsm_a.dtap.codec.ofr_amr_wb": "0",
                                      "gsm_a.dtap.codec.ohr_amr": "0",
                                      "gsm_a.dtap.codec.umts_amr_wb": "0",
                                      "gsm_a.dtap.codec.fr_amr_wb": "1",
                                      "gsm_a.dtap.codec.pdc_efr": "0"
                                    }
                                  },
                                  "Voice Domain Preference and UE's Usage Setting": {
                                    "gsm_a.gm.elem_id": "0x0000005d",
                                    "gsm_a.len": "1",
                                    "gsm_a.spare_bits": "0",
                                    "gsm_a.gm.gmm.ue_usage_setting": "0",
                                    "gsm_a.gm.gmm.voice_domain_pref_for_eutran": "3"
                                  },
                                  "GUTI type - Old GUTI type": {
                                    "gsm_a.common.elem_id": "0x0000000e",
                                    "nas_eps.spare_bits": "0x00000000",
                                    "nas_eps.emm.guti_type": "0"
                                  },
                                  "MS network feature support": {
                                    "gsm_a.common.elem_id": "0x0000000c",
                                    "gsm_a.spare_bits": "0",
                                    "gsm_a.ext_periodic_timers": "1"
                                  },
                                  "Network Resource Identifier Container - TMSI based NRI container": {
                                    "gsm_a.gm.elem_id": "0x00000010",
                                    "gsm_a.len": "2",
                                    "gsm_a.gm.gmm.nri_cont_value": "0x00000068",
                                    "gsm_a.spare_bits": "0"
                                  }
                                }
                              },
                              "lte-rrc.nonCriticalExtension_element": {
                                "per.optional_field_bit": "1",
                                "lte-rrc.nonCriticalExtension_element": {
                                  "per.optional_field_bit": "0",
                                  "per.enum_index": "0",
                                  "lte-rrc.gummei_Type_r10": "0"
                                }
                              }
                            }
                          }
                        }
                      }
                    }
                  }
                }
              },
              "pdcp-lte.mac": "0x00000000"
            }
          },
          "mac-lte.padding-data": "00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00:00",
          "mac-lte.padding-length": "36"
        },
        "mac-lte.ulsch": "",
        "_ws.lua.fake": "",
        "_ws.col.Info": "RRCConnectionSetupComplete, Attach request, PDN connectivity request",
        "_ws.col.Protocol": "LTE RRC UL_DCCH/NAS-EPS"
      }
    }