ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 12:44:17.245 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 12:44:17.249 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 12:44:17.249 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 12:44:17.251 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 12:44:17.251 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 12:44:17.252 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:805: IMS UDP port 192.168.2.3:5060 configured
7 | 12:44:17.253 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:755: IMS TCP port 192.168.2.3:5060 configured!
8 | 12:44:17.255 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:776: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 12:44:17.256 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:787: IdM port 192.168.2.3:8080 configured!
10 | 12:44:17.257 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 12:44:18.460 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 12:44:18.462 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 12:44:21.103 |  | ←RRC BCCH SIB1 |  |  |
14 | 12:44:21.178 |  | ←RRC BCCH SIB |  |  |
15 | 12:44:21.183 |  | ←RRC BCCH SIB1 |  |  |
16 | 12:44:21.263 |  | ←RRC BCCH SIB1 |  |  |
17 | 12:44:21.338 |  | ←RRC BCCH SIB |  |  |
18 | 12:45:54.617 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 12:45:54.617 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 12:45:54.617 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 12:45:54.617 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 12:45:54.678 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 12:45:54.678 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 12:45:54.678 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 12:45:54.678 |  |  |  | →NAS EMM Attach request |  |
26 | 12:45:54.678 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 12:45:54.678 |  |  |  | NAS K-asme 8e491e136d0ddc74a9deb01e8e99ea1b... |  |
28 | 12:45:54.678 |  |  |  | NAS ← EMM Authentication request |  |
29 | 12:45:54.679 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 12:45:54.679 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 12:45:54.680 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 12:45:54.750 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 12:45:54.750 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 12:45:54.750 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 12:45:54.750 |  |  |  | →NAS EMM Authentication response |  |
36 | 12:45:54.750 |  |  |  | NAS UE auth OK |  |
37 | 12:45:54.750 |  |  |  | NAS K-nas-cip 45ca55c93b79940bff06992a2a5b1... |  |
38 | 12:45:54.750 |  |  |  | NAS K-nas-int 7751bc4847e09490ba11b63fab790... |  |
39 | 12:45:54.750 |  |  |  | NAS ← EMM Security mode command |  |
40 | 12:45:54.751 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 12:45:54.751 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 12:45:54.752 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 12:45:54.760 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
44 | 12:45:54.790 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
45 | 12:45:54.790 |  | →RRC DCCH UL Information Transfer |  |  |
46 | 12:45:54.790 |  | [EMBEDDED NAS IN PREV RRC] TP Unknown message (type=0x0e) |  |  |
47 | 12:45:54.790 |  |  |  | →NAS EMM Security mode complete |  |
48 | 12:45:54.790 |  |  |  | NAS ← ESM ESM information request |  |
49 | 12:45:54.791 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xd) |  |  |
50 | 12:45:54.791 |  | ←RRC DCCH DL Information Transfer |  |  |
51 | 12:45:54.792 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
52 | 12:45:54.838 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
53 | 12:45:54.838 |  | →RRC DCCH UL Information Transfer |  |  |
54 | 12:45:54.838 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x3e) |  |  |
55 | 12:45:54.838 |  |  |  | →NAS ESM ESM information response |  |
56 | 12:45:54.838 |  |  |  | NAS ← EMM Attach accept |  |
57 | 12:45:54.838 |  |  |  | NAS K-enb cde63290c6705514a1f8937de74b0e982... |  |
58 | 12:45:54.839 |  | ←RRC DCCH Security Mode Command |  |  |
59 | 12:45:54.839 |  |  | RRC K-enb cde63290c6705514a1f8937de74b0e982... |  |  |
60 | 12:45:54.839 |  |  | RRC rrc-cip b4884b4769403f886fb4fe211865b1d... |  |  |
61 | 12:45:54.839 |  |  | RRC rrc-int 9953279756de235595601e79030395c... |  |  |
62 | 12:45:54.839 |  |  | RRC up-cip 4cd78e3693cd8c1c7e0bf092f9dc7bf6... |  |  |
63 | 12:45:54.839 |  |  | RRC up-int 995d51329fcbaaf36718f933e1b642cc... |  |  |
64 | 12:45:54.840 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
65 | 12:45:54.848 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
66 | 12:45:54.870 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
67 | 12:45:54.870 |  | →RRC DCCH Security Mode Complete |  |  |
68 | 12:45:54.870 |  | ←RRC DCCH UE Capability Enquiry |  |  |
69 | 12:45:54.870 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
70 | 12:45:54.920 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
71 | 12:45:54.920 |  | →RRC DCCH UE Capability Information |  |  |
72 | 12:45:54.920 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x1) |  |  |
73 | 12:45:54.920 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
74 | 12:45:54.920 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
75 | 12:45:54.950 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
76 | 12:45:54.950 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
77 | 12:45:54.990 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
78 | 12:45:54.990 |  | →RRC DCCH UL Information Transfer |  |  |
79 | 12:45:54.990 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x4) |  |  |
80 | 12:45:54.990 |  |  |  | →NAS EMM Attach complete |  |
81 | 12:45:54.990 |  |  |  | NAS ← EMM EMM information |  |
82 | 12:45:54.991 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xfe) |  |  |
83 | 12:45:54.991 |  | ←RRC DCCH DL Information Transfer |  |  |
84 | 12:45:54.992 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
85 | 12:46:00.746 |  | ←RRC DCCH RRC Connection Release |  |  |
86 | 12:46:00.747 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
87 | 12:46:01.117 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
88 | 12:46:01.117 |  | →RRC CCCH RRC Connection Request |  |  |
89 | 12:46:01.117 |  | ←RRC CCCH RRC Connection Setup |  |  |
90 | 12:46:01.117 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
91 | 12:46:01.150 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
92 | 12:46:01.150 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
93 | 12:46:01.150 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
94 | 12:46:01.150 |  |  |  | →NAS EMM Service request |  |
95 | 12:46:01.150 |  |  |  | NAS K-enb 61dbdb241a8d487afd8472b972a9a05b0... |  |
96 | 12:46:01.151 |  | ←RRC DCCH Security Mode Command |  |  |
97 | 12:46:01.151 |  |  | RRC K-enb 61dbdb241a8d487afd8472b972a9a05b0... |  |  |
98 | 12:46:01.151 |  |  | RRC rrc-cip 9b3fac1f82ec69185c082878f46e224... |  |  |
99 | 12:46:01.151 |  |  | RRC rrc-int 7e2f65832f413f8ab14e330f1f160b8... |  |  |
100 | 12:46:01.151 |  |  | RRC up-cip f6822f1b0725d9baa6383846047fcb70... |  |  |
101 | 12:46:01.151 |  |  | RRC up-int 9ed631788d17badfbf8f4f36023541c1... |  |  |
102 | 12:46:01.152 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
103 | 12:46:01.190 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
104 | 12:46:01.190 |  | →RRC DCCH Security Mode Complete |  |  |
105 | 12:46:01.190 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
106 | 12:46:01.190 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
107 | 12:46:01.230 | →enobeB PCAP frame→ DNS RRCConnectionReconfigurationComplete [62-bytes] ... |  |  |  |
108 | 12:46:01.230 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
109 | 12:46:25.310 | →enobeB PCAP frame→ TCP |  |  |  |
110 | 12:46:25.313 |  | ←enobeB PCAP frame← TCP |  |  |
111 | 12:46:25.350 | →enobeB PCAP frame→ TCP |  |  |  |
112 | 12:46:25.398 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
113 | 12:46:25.401 |  | ←enobeB PCAP frame← TCP |  |  |
114 | 12:46:25.407 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
115 | 12:46:25.430 | →enobeB PCAP frame→ TCP |  |  |  |
116 | 12:46:25.558 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
117 | 12:46:25.561 |  | ←enobeB PCAP frame← TCP |  |  |
118 | 12:46:25.561 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 16)
119 | 12:46:25.562 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
120 | 12:46:25.590 | →enobeB PCAP frame→ TCP |  |  |  |
121 | 12:46:25.598 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
122 | 12:46:25.601 |  | ←enobeB PCAP frame← TCP |  |  |
123 | 12:46:25.601 |  |  |  |  | →HTTP GET | HTTP-Proxy
124 | 12:46:25.607 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:288: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
125 | 12:46:25.625 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
126 | 12:46:25.629 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
127 | 12:46:25.670 | →enobeB PCAP frame→ TCP |  |  |  |
128 | 12:46:27.630 | →enobeB PCAP frame→ TCP |  |  |  |
129 | 12:46:27.633 |  | ←enobeB PCAP frame← TCP |  |  |
130 | 12:46:27.670 | →enobeB PCAP frame→ TCP |  |  |  |
131 | 12:46:27.678 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
132 | 12:46:27.681 |  | ←enobeB PCAP frame← TCP |  |  |
133 | 12:46:27.687 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
134 | 12:46:27.710 | →enobeB PCAP frame→ TCP |  |  |  |
135 | 12:46:27.958 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
136 | 12:46:27.961 |  | ←enobeB PCAP frame← TCP |  |  |
137 | 12:46:27.961 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:642: Client connected to IdM port (id 18)
138 | 12:46:27.962 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
139 | 12:46:27.990 | →enobeB PCAP frame→ TCP |  |  |  |
140 | 12:46:27.998 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
141 | 12:46:28.001 |  | ←enobeB PCAP frame← TCP |  |  |
142 | 12:46:28.002 |  |  |  |  | →HTTP GET | IDMS-Endpoint
143 | 12:46:28.028 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
144 | 12:46:28.030 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
145 | 12:46:28.032 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:511: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
146 | 12:46:28.033 |  |  |  |  | MMICmd: Please provide user credentials: username and password
147 | 12:46:28.110 | →enobeB PCAP frame→ TCP |  |  |  |
148 | 12:46:33.849 |  | ←enobeB PCAP frame← TCP |  |  |
149 | 12:46:33.851 |  |  |  |  | →HTTP POST | IDMS-Endpoint
150 | 12:46:33.865 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
151 | 12:46:33.867 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
152 | 12:46:33.868 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:516: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
153 | 12:46:33.910 | →enobeB PCAP frame→ TCP |  |  |  |
154 | 12:46:33.912 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:677: IdM port - Client closed the connection (id 18)
155 | 12:46:33.913 |  | ←enobeB PCAP frame← TCP |  |  |
156 | 12:46:33.950 | →enobeB PCAP frame→ TCP |  |  |  |
157 | 12:46:34.350 | →enobeB PCAP frame→ TCP |  |  |  |
158 | 12:46:34.353 |  | ←enobeB PCAP frame← TCP |  |  |
159 | 12:46:34.390 | →enobeB PCAP frame→ TCP |  |  |  |
160 | 12:46:34.438 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
161 | 12:46:34.441 |  | ←enobeB PCAP frame← TCP |  |  |
162 | 12:46:34.443 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
163 | 12:46:34.470 | →enobeB PCAP frame→ TCP |  |  |  |
164 | 12:46:34.518 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
165 | 12:46:34.520 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:642: Client connected to IdM port (id 18)
166 | 12:46:34.521 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
167 | 12:46:34.550 | →enobeB PCAP frame→ TCP |  |  |  |
168 | 12:46:34.598 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
169 | 12:46:34.601 |  |  |  |  | →HTTP POST | IDMS-Endpoint
170 | 12:46:34.604 |  | ←enobeB PCAP frame← TCP |  |  |
171 | 12:46:34.616 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
172 | 12:46:34.617 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
173 | 12:46:34.619 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:521: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
174 | 12:46:34.710 | →enobeB PCAP frame→ TCP |  |  |  |
175 | 12:46:35.030 | →enobeB PCAP frame→ TCP |  |  |  |
176 | 12:46:35.033 |  | ←enobeB PCAP frame← TCP |  |  |
177 | 12:46:35.070 | →enobeB PCAP frame→ TCP |  |  |  |
178 | 12:46:35.078 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
179 | 12:46:35.081 |  | ←enobeB PCAP frame← TCP |  |  |
180 | 12:46:35.085 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
181 | 12:46:35.110 | →enobeB PCAP frame→ TCP |  |  |  |
182 | 12:46:35.158 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
183 | 12:46:35.161 |  | ←enobeB PCAP frame← TCP |  |  |
184 | 12:46:35.161 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 19)
185 | 12:46:35.162 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
186 | 12:46:35.238 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
187 | 12:46:35.241 |  | ←enobeB PCAP frame← TCP |  |  |
188 | 12:46:35.243 |  |  |  |  | →HTTP POST | HTTP-Proxy
189 | 12:46:35.269 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:541: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
190 | 12:46:35.276 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
191 | 12:46:35.279 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
192 | 12:46:35.310 | →enobeB PCAP frame→ TCP |  |  |  |
193 | 12:46:35.350 | →enobeB PCAP frame→ TCP |  |  |  |
194 | 12:46:35.353 |  | ←enobeB PCAP frame← TCP |  |  |
195 | 12:46:35.390 | →enobeB PCAP frame→ TCP |  |  |  |
196 | 12:46:35.398 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
197 | 12:46:35.401 |  | ←enobeB PCAP frame← TCP |  |  |
198 | 12:46:35.404 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
199 | 12:46:35.430 | →enobeB PCAP frame→ TCP |  |  |  |
200 | 12:46:35.478 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
201 | 12:46:35.481 |  | ←enobeB PCAP frame← TCP |  |  |
202 | 12:46:35.481 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 20)
203 | 12:46:35.482 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
204 | 12:46:35.518 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
205 | 12:46:35.521 |  | ←enobeB PCAP frame← TCP |  |  |
206 | 12:46:35.522 |  |  |  |  | →HTTP POST | HTTP-Proxy
207 | 12:46:35.575 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
208 | 12:46:35.575 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:545: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
209 | 12:46:35.577 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
210 | 12:46:35.630 | →enobeB PCAP frame→ TCP |  |  |  |
211 | 12:46:35.678 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
212 | 12:46:35.683 |  |  |  |  | →SIP REGISTER | P-CSCF
213 | 12:46:35.706 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:814: IMS UDP_s port 192.168.2.3:5062 configured
214 | 12:46:35.733 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:765: IMS TCP_s port 192.168.2.3:5062 configured!
215 | 12:46:35.736 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:823: IMS UDP_c port 192.168.2.3:5061 configured
216 | 12:46:35.741 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
217 | 12:46:36.278 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
218 | 12:46:36.283 |  |  |  |  | →SIP REGISTER | P-CSCF
219 | 12:46:36.309 |  |  |  |  | ←SIP 200 OK | P-CSCF
220 | 12:46:36.311 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
221 | 12:46:36.598 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
222 | 12:46:36.599 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
223 | 12:46:36.600 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 SIP over IPSEC: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 |  |  |  |
224 | 12:46:36.614 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
225 | 12:46:36.677 |  |  |  |  | ←SIP 200 OK | P-CSCF
226 | 12:46:36.677 |  |  |  |  | MIKEY | Media-Server
227 | 12:46:36.678 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
228 | 12:46:36.899 |  |  |  |  | XML→ | Media-Server
229 | 12:46:36.900 |  |  |  |  | XML→ | Media-Server
230 | 12:46:36.903 |  |  |  |  | ←XML | Media-Server
231 | 12:46:36.907 |  |  |  |  | ←SIP NOTIFY | P-CSCF
232 | 12:46:36.908 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:46253;transp... |  |  |
233 | 12:46:36.958 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
234 | 12:46:36.961 |  |  |  |  | →SIP 200 OK | P-CSCF
235 | 12:46:37.150 | →enobeB PCAP frame→ TCP |  |  |  |
236 | 12:46:37.153 |  | ←enobeB PCAP frame← TCP |  |  |
237 | 12:46:37.190 | →enobeB PCAP frame→ TCP |  |  |  |
238 | 12:46:37.198 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
239 | 12:46:37.201 |  | ←enobeB PCAP frame← TCP |  |  |
240 | 12:46:37.204 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
241 | 12:46:37.230 | →enobeB PCAP frame→ TCP |  |  |  |
242 | 12:46:37.318 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
243 | 12:46:37.321 |  | ←enobeB PCAP frame← TCP |  |  |
244 | 12:46:37.321 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
245 | 12:46:37.322 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
246 | 12:46:37.350 | →enobeB PCAP frame→ TCP |  |  |  |
247 | 12:46:37.398 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-co... |  |  |  |
248 | 12:46:37.401 |  | ←enobeB PCAP frame← TCP |  |  |
249 | 12:46:37.401 |  |  |  |  | →HTTP GET | HTTP-Proxy
250 | 12:46:37.410 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:642: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcptt-ue-configuration.xml
251 | 12:46:37.418 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
252 | 12:46:37.420 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
253 | 12:46:37.470 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
254 | 12:46:37.472 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
255 | 12:46:37.473 |  | ←enobeB PCAP frame← TCP |  |  |
256 | 12:46:37.478 | →enobeB PCAP frame→ TCP |  |  |  |
257 | 12:46:37.482 |  | ←enobeB PCAP frame← TCP |  |  |
258 | 12:46:37.510 | →enobeB PCAP frame→ TCP |  |  |  |
259 | 12:46:37.630 | →enobeB PCAP frame→ TCP |  |  |  |
260 | 12:46:37.633 |  | ←enobeB PCAP frame← TCP |  |  |
261 | 12:46:37.670 | →enobeB PCAP frame→ TCP |  |  |  |
262 | 12:46:37.678 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
263 | 12:46:37.681 |  | ←enobeB PCAP frame← TCP |  |  |
264 | 12:46:37.685 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
265 | 12:46:37.710 | →enobeB PCAP frame→ TCP |  |  |  |
266 | 12:46:37.758 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
267 | 12:46:37.761 |  | ←enobeB PCAP frame← TCP |  |  |
268 | 12:46:37.761 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
269 | 12:46:37.762 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
270 | 12:46:37.790 | →enobeB PCAP frame→ TCP |  |  |  |
271 | 12:46:37.798 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-... |  |  |  |
272 | 12:46:37.801 |  | ←enobeB PCAP frame← TCP |  |  |
273 | 12:46:37.802 |  |  |  |  | →HTTP GET | HTTP-Proxy
274 | 12:46:37.813 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:647: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcptt-user-profile-49.xml
275 | 12:46:37.856 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
276 | 12:46:37.862 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
277 | 12:46:37.863 |  | ←enobeB PCAP frame← TCP |  |  |
278 | 12:46:37.864 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
279 | 12:46:37.910 | →enobeB PCAP frame→ TCP |  |  |  |
280 | 12:46:37.918 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
281 | 12:46:37.921 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
282 | 12:46:37.922 |  | ←enobeB PCAP frame← TCP |  |  |
283 | 12:46:37.950 | →enobeB PCAP frame→ TCP |  |  |  |
284 | 12:46:38.478 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
285 | 12:46:38.479 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
286 | 12:46:38.480 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
287 | 12:46:38.494 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
288 | 12:46:38.550 | →enobeB PCAP frame→ TCP |  |  |  |
289 | 12:46:38.553 |  | ←enobeB PCAP frame← TCP |  |  |
290 | 12:46:38.554 |  |  |  |  | ←SIP 200 OK | P-CSCF
291 | 12:46:38.554 |  |  |  |  | MIKEY | Media-Server
292 | 12:46:38.556 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
293 | 12:46:38.590 | →enobeB PCAP frame→ TCP |  |  |  |
294 | 12:46:38.598 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
295 | 12:46:38.601 |  | ←enobeB PCAP frame← TCP |  |  |
296 | 12:46:38.602 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
297 | 12:46:38.630 | →enobeB PCAP frame→ TCP |  |  |  |
298 | 12:46:38.718 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
299 | 12:46:38.720 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
300 | 12:46:38.721 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
301 | 12:46:38.750 | →enobeB PCAP frame→ TCP |  |  |  |
302 | 12:46:38.758 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.servi... |  |  |  |
303 | 12:46:38.760 |  |  |  |  | →HTTP GET | HTTP-Proxy
304 | 12:46:38.761 |  | ←enobeB PCAP frame← TCP |  |  |
305 | 12:46:38.762 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:652: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
306 | 12:46:38.768 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
307 | 12:46:38.770 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
308 | 12:46:38.771 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
309 | 12:46:38.774 |  |  |  |  | XML→ | Media-Server
310 | 12:46:38.775 |  |  |  |  | XML→ | Media-Server
311 | 12:46:38.778 |  |  |  |  | ←XML | Media-Server
312 | 12:46:38.781 |  |  |  |  | ←SIP NOTIFY | P-CSCF
313 | 12:46:38.783 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:46253;transp... |  |  |
314 | 12:46:38.790 | →enobeB PCAP frame→ TCP |  |  |  |
315 | 12:46:38.798 | →enobeB PCAP frame→ TCP |  |  |  |
316 | 12:46:38.822 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
317 | 12:46:38.825 |  |  |  |  | →SIP 200 OK | P-CSCF
318 | 12:46:38.870 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
319 | 12:46:38.872 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
320 | 12:46:38.873 |  | ←enobeB PCAP frame← TCP |  |  |
321 | 12:46:38.878 | →enobeB PCAP frame→ TCP |  |  |  |
322 | 12:46:38.881 |  | ←enobeB PCAP frame← TCP |  |  |
323 | 12:46:38.910 | →enobeB PCAP frame→ TCP |  |  |  |
324 | 12:46:38.990 | →enobeB PCAP frame→ TCP |  |  |  |
325 | 12:46:38.993 |  | ←enobeB PCAP frame← TCP |  |  |
326 | 12:46:39.030 | →enobeB PCAP frame→ TCP |  |  |  |
327 | 12:46:39.038 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
328 | 12:46:39.041 |  | ←enobeB PCAP frame← TCP |  |  |
329 | 12:46:39.045 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
330 | 12:46:39.070 | →enobeB PCAP frame→ TCP |  |  |  |
331 | 12:46:39.118 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
332 | 12:46:39.121 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
333 | 12:46:39.121 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
334 | 12:46:39.198 | →enobeB PCAP frame→ HTTPS: GET /xcap.gms.mcstaasting.com/org.openmobileallian... |  |  |  |
335 | 12:46:39.201 |  | ←enobeB PCAP frame← TCP |  |  |
336 | 12:46:39.201 |  |  |  |  | →HTTP GET | HTTP-Proxy
337 | 12:46:39.213 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:657: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at /xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
338 | 12:46:39.236 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
339 | 12:46:39.241 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
340 | 12:46:39.242 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
341 | 12:46:39.270 | →enobeB PCAP frame→ TCP |  |  |  |
342 | 12:46:39.278 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
343 | 12:46:39.281 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
344 | 12:46:39.282 |  | ←enobeB PCAP frame← TCP |  |  |
345 | 12:46:39.310 | →enobeB PCAP frame→ TCP |  |  |  |
346 | 12:46:39.398 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
347 | 12:46:39.399 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
348 | 12:46:39.412 |  |  |  |  | →SIP PUBLISH | P-CSCF
349 | 12:46:39.460 |  |  |  |  | MIKEY | Media-Server
350 | 12:46:39.478 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
351 | 12:46:39.479 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
352 | 12:46:39.480 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
353 | 12:46:39.485 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
354 | 12:46:39.686 |  |  |  |  | XML→ | Media-Server
355 | 12:46:39.690 |  |  |  |  | ←SIP 200 OK | P-CSCF
356 | 12:46:39.691 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
357 | 12:46:39.693 |  |  |  |  | ←SIP 200 OK | P-CSCF
358 | 12:46:39.693 |  |  |  |  | MIKEY | Media-Server
359 | 12:46:39.695 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
360 | 12:46:39.907 |  |  |  |  | XML→ | Media-Server
361 | 12:46:39.908 |  |  |  |  | XML→ | Media-Server
362 | 12:46:39.943 |  |  |  |  | ←XML | Media-Server
363 | 12:46:39.948 |  |  |  |  | ←SIP NOTIFY | P-CSCF
364 | 12:46:39.950 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:46253;transp... |  |  |
365 | 12:46:39.998 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
366 | 12:46:40.000 |  |  |  |  | →SIP 200 OK | P-CSCF
367 | 12:46:40.004 |  |  |  |  | ←XML | Media-Server
368 | 12:46:40.014 |  |  |  |  | ←SIP MESSAGE | P-CSCF
369 | 12:46:40.016 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
370 | 12:46:40.017 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
371 | 12:46:40.838 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
372 | 12:46:40.841 |  |  |  |  | →SIP 200 OK | P-CSCF
373 | 12:46:40.849 |  |  |  |  | Info: MCX_IMS_CommonProcedures.ttcn:155: MESSAGE/200OK Table 5.3.2.3-2 Steps 7-8 Done
374 | 12:46:40.852 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
375 | 12:46:40.870 | →enobeB PCAP frame→ TCP |  |  |  |
376 | 12:46:40.910 | →enobeB PCAP frame→ TCP |  |  |  |
377 | 12:46:42.852 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
378 | 12:46:42.897 |  | ←RRC DCCH RRC Connection Release |  |  |
379 | 12:46:42.898 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
380 | 12:46:42.918 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
381 | 12:46:42.930 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:735: SRTP config: Master Key: 7C895CA92C5371B45BFDB8F580B8F1DE, Master Salt: 7F36E1D8638D68CDBA464E29, MKI: 20CAE407
382 | 12:46:42.930 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
383 | 12:46:42.933 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
384 | 12:46:42.935 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
385 | 12:46:42.949 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
386 | 12:46:42.949 |  |  |  |  | ←XML | Media-Server
387 | 12:46:42.985 |  |  |  |  | ←SIP INVITE | P-CSCF
388 | 12:46:43.957 |  | ←enobeB PCAP frame← LTE RRC PCCH Paging (1 PagingRecord) |  |  |
389 | 12:46:43.957 |  | ←RRC PCCH Paging |  |  |
390 | 12:46:43.997 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
391 | 12:46:43.997 |  | →RRC CCCH RRC Connection Request |  |  |
392 | 12:46:43.997 |  | ←RRC CCCH RRC Connection Setup |  |  |
393 | 12:46:43.997 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
394 | 12:46:44.030 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
395 | 12:46:44.030 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
396 | 12:46:44.030 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
397 | 12:46:44.030 |  |  |  | →NAS EMM Service request |  |
398 | 12:46:44.030 |  |  |  | NAS K-enb 0e726b3f18638563d7aa1efcc40f8ea07... |  |
399 | 12:46:44.031 |  | ←RRC DCCH Security Mode Command |  |  |
400 | 12:46:44.031 |  |  | RRC K-enb 0e726b3f18638563d7aa1efcc40f8ea07... |  |  |
401 | 12:46:44.031 |  |  | RRC rrc-cip 284394c61fdeae909eabbdc37e988b2... |  |  |
402 | 12:46:44.031 |  |  | RRC rrc-int eab0ff0d1bb67214c061f66b54aca97... |  |  |
403 | 12:46:44.031 |  |  | RRC up-cip 31c471530b4fd1a9209b4fe1f0965f8d... |  |  |
404 | 12:46:44.031 |  |  | RRC up-int 1f9194fbddbe4f8cfe3de29b549ebbfa... |  |  |
405 | 12:46:44.032 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
406 | 12:46:44.070 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
407 | 12:46:44.070 |  | →RRC DCCH Security Mode Complete |  |  |
408 | 12:46:44.070 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
409 | 12:46:44.070 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
410 | 12:46:44.110 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
411 | 12:46:44.110 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
412 | 12:46:44.112 |  | ←enobeB PCAP frame← SIP over IPSEC: INVITE sip:PublicUserId-A@192.168.3.2:46253;transp... |  |  |
413 | 12:46:44.158 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 100 Trying |  |  |  |
414 | 12:46:44.161 |  |  |  |  | →SIP 100 Trying | P-CSCF
415 | 12:46:44.198 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 183 Session Progress |  |  |  |
416 | 12:46:44.202 |  |  |  |  | →SIP 183 Session Progress | P-CSCF
417 | 12:46:44.222 |  |  |  |  | ←SIP PRACK | P-CSCF
418 | 12:46:44.224 |  | ←enobeB PCAP frame← SIP over IPSEC: PRACK sip:PublicUserId-A@192.168.3.2:46253;transpo... |  |  |
419 | 12:46:44.278 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
420 | 12:46:44.281 |  |  |  |  | →SIP 200 OK | P-CSCF
421 | 12:46:44.539 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
422 | 12:46:44.540 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x6) |  |  |
423 | 12:46:44.540 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
424 | 12:46:44.541 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
425 | 12:46:44.590 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
426 | 12:46:44.590 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
427 | 12:46:44.590 |  | →RRC DCCH UL Information Transfer |  |  |
428 | 12:46:44.590 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x6) |  |  |
429 | 12:46:44.590 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
430 | 12:46:44.666 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
431 | 12:46:45.042 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:648: Verdict: Pass
432 | 12:46:45.144 |  |  |  |  | MMICmd: Please Accept the Call
433 | 12:47:04.358 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
434 | 12:47:04.359 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
435 | 12:47:04.453 |  |  |  |  | →SIP 200 OK | P-CSCF
436 | 12:47:04.483 |  |  |  |  | XML→ | Media-Server
437 | 12:47:04.488 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:657: 200 OK Verdict: Pass
438 | 12:47:04.488 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:354: Step 1 Verdict: Pass
439 | 12:47:04.490 |  |  |  |  | ←SIP ACK | P-CSCF
440 | 12:47:04.491 |  | ←enobeB PCAP frame← SIP over IPSEC: ACK sip:PublicUserId-A@192.168.3.2:46253;transport... |  |  |
441 | 12:47:04.492 |  |  |  |  | ←SIP BYE | P-CSCF
442 | 12:47:04.493 |  | ←enobeB PCAP frame← SIP over IPSEC: BYE sip:PublicUserId-A@192.168.3.2:46253;transport... |  |  |
443 | 12:47:05.198 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
444 | 12:47:05.201 |  |  |  |  | →SIP 200 OK | P-CSCF
445 | 12:47:05.910 | →enobeB PCAP frame→ |  |  |  |
446 | 12:47:07.210 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
447 | 12:47:07.230 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
448 | 12:47:07.231 |  | [EMBEDDED NAS IN NEXT RRC] ESM Unknown message (type=0xa7) |  |  |
449 | 12:47:07.231 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
450 | 12:47:07.232 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration |  |  |
451 | 12:47:07.270 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
452 | 12:47:07.270 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
453 | 12:47:07.270 |  | →RRC DCCH UL Information Transfer |  |  |
454 | 12:47:07.270 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xc) |  |  |
455 | 12:47:07.270 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
456 | 12:47:07.344 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
457 | 12:47:07.345 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
458 | 12:47:07.379 |  | ←RRC DCCH RRC Connection Release |  |  |
459 | 12:47:07.380 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
460 | 12:47:07.400 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
461 | 12:47:07.402 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
462 | 12:47:07.404 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
463 | 12:47:08.152 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.