ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 08:57:31.436 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 08:57:31.439 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 08:57:31.439 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 08:57:31.441 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 08:57:31.442 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 08:57:31.443 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:805: IMS UDP port 192.168.2.3:5060 configured
7 | 08:57:31.447 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:755: IMS TCP port 192.168.2.3:5060 configured!
8 | 08:57:31.451 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:776: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 08:57:31.452 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:787: IdM port 192.168.2.3:8080 configured!
10 | 08:57:31.455 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 08:57:32.657 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 08:57:32.659 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 08:57:35.302 |  | ←RRC BCCH SIB |  |  |
14 | 08:57:35.307 |  | ←RRC BCCH SIB1 |  |  |
15 | 08:57:35.322 |  | ←RRC BCCH SIB |  |  |
16 | 08:57:35.342 |  | ←RRC BCCH SIB |  |  |
17 | 08:57:35.387 |  | ←RRC BCCH SIB1 |  |  |
18 | 08:58:58.981 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 08:58:58.981 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 08:58:58.981 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 08:58:58.981 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 08:58:59.042 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 08:58:59.042 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 08:58:59.042 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 08:58:59.042 |  |  |  | →NAS EMM Attach request |  |
26 | 08:58:59.042 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 08:58:59.042 |  |  |  | NAS K-asme a239733ce2b4c226ddd54b171f93dfdd... |  |
28 | 08:58:59.042 |  |  |  | NAS ← EMM Authentication request |  |
29 | 08:58:59.043 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 08:58:59.043 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 08:58:59.044 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 08:58:59.114 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 08:58:59.114 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 08:58:59.114 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 08:58:59.114 |  |  |  | →NAS EMM Authentication response |  |
36 | 08:58:59.114 |  |  |  | NAS UE auth OK |  |
37 | 08:58:59.114 |  |  |  | NAS K-nas-cip 153e5b1eadcebdae59dadf099eb40... |  |
38 | 08:58:59.114 |  |  |  | NAS K-nas-int e073193eef719a516f04051a64819... |  |
39 | 08:58:59.114 |  |  |  | NAS ← EMM Security mode command |  |
40 | 08:58:59.115 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 08:58:59.115 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 08:58:59.116 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 08:58:59.154 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
44 | 08:58:59.154 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 08:58:59.154 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x6) |  |  |
46 | 08:58:59.154 |  |  |  | →NAS EMM Security mode complete |  |
47 | 08:58:59.154 |  |  |  | NAS ← ESM ESM information request |  |
48 | 08:58:59.155 |  | [EMBEDDED NAS IN NEXT RRC] TP Unknown message (type=0x35) |  |  |
49 | 08:58:59.155 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 08:58:59.156 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
51 | 08:58:59.202 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
52 | 08:58:59.202 |  | →RRC DCCH UL Information Transfer |  |  |
53 | 08:58:59.202 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xd) |  |  |
54 | 08:58:59.202 |  |  |  | →NAS ESM ESM information response |  |
55 | 08:58:59.202 |  |  |  | NAS ← EMM Attach accept |  |
56 | 08:58:59.202 |  |  |  | NAS K-enb 2d5e0b84a87b965ab3106f351deac211c... |  |
57 | 08:58:59.203 |  | ←RRC DCCH Security Mode Command |  |  |
58 | 08:58:59.203 |  |  | RRC K-enb 2d5e0b84a87b965ab3106f351deac211c... |  |  |
59 | 08:58:59.203 |  |  | RRC rrc-cip 0ab0c7e008661b7829a1cb8bbbda75f... |  |  |
60 | 08:58:59.203 |  |  | RRC rrc-int fddb37bf10f5ca45fb80ebb442b0a72... |  |  |
61 | 08:58:59.203 |  |  | RRC up-cip adf7d0d9d8ed7b4e1d4708c667ba51dd... |  |  |
62 | 08:58:59.203 |  |  | RRC up-int b057a163ecdac27fb49b400978bf6230... |  |  |
63 | 08:58:59.204 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
64 | 08:58:59.234 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
65 | 08:58:59.234 |  | →RRC DCCH Security Mode Complete |  |  |
66 | 08:58:59.234 |  | ←RRC DCCH UE Capability Enquiry |  |  |
67 | 08:58:59.234 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
68 | 08:58:59.284 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
69 | 08:58:59.284 |  | →RRC DCCH UE Capability Information |  |  |
70 | 08:58:59.284 |  | [EMBEDDED NAS IN NEXT RRC] ESM Unknown message (type=0x30) |  |  |
71 | 08:58:59.284 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
72 | 08:58:59.284 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration |  |  |
73 | 08:58:59.314 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
74 | 08:58:59.314 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
75 | 08:58:59.354 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
76 | 08:58:59.354 |  | →RRC DCCH UL Information Transfer |  |  |
77 | 08:58:59.354 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x3) |  |  |
78 | 08:58:59.354 |  |  |  | →NAS EMM Attach complete |  |
79 | 08:58:59.354 |  |  |  | NAS ← EMM EMM information |  |
80 | 08:58:59.355 |  | [EMBEDDED NAS IN NEXT RRC] EMM Service request |  |  |
81 | 08:58:59.355 |  | ←RRC DCCH DL Information Transfer |  |  |
82 | 08:58:59.356 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
83 | 08:59:04.899 |  | ←RRC DCCH RRC Connection Release |  |  |
84 | 08:59:04.900 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
85 | 08:59:05.381 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
86 | 08:59:05.381 |  | →RRC CCCH RRC Connection Request |  |  |
87 | 08:59:05.381 |  | ←RRC CCCH RRC Connection Setup |  |  |
88 | 08:59:05.381 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
89 | 08:59:05.434 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
90 | 08:59:05.434 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
91 | 08:59:05.434 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
92 | 08:59:05.434 |  |  |  | →NAS EMM Service request |  |
93 | 08:59:05.434 |  |  |  | NAS K-enb 9665c708c1745259538ad917489497747... |  |
94 | 08:59:05.435 |  |  | RRC K-enb 9665c708c1745259538ad917489497747... |  |  |
95 | 08:59:05.436 |  |  | RRC rrc-cip 5e2706f9eb6d29ba7cef3094da0921f... |  |  |
96 | 08:59:05.436 |  |  | RRC rrc-int e36a5f34ccecbf8683cd673c44d4ce3... |  |  |
97 | 08:59:05.436 |  |  | RRC up-cip e93eb407e7aac8f6bae519790ac130ed... |  |  |
98 | 08:59:05.436 |  |  | RRC up-int 2ae5c01cf9fe4ba864f5866ceb20a024... |  |  |
99 | 08:59:05.436 |  | ←RRC DCCH Security Mode Command |  |  |
100 | 08:59:05.436 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
101 | 08:59:05.474 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
102 | 08:59:05.474 |  | →RRC DCCH Security Mode Complete |  |  |
103 | 08:59:05.474 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
104 | 08:59:05.474 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
105 | 08:59:05.514 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
106 | 08:59:05.514 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
107 | 08:59:20.034 | →enobeB PCAP frame→ TCP |  |  |  |
108 | 08:59:20.037 |  | ←enobeB PCAP frame← TCP |  |  |
109 | 08:59:20.074 | →enobeB PCAP frame→ TCP |  |  |  |
110 | 08:59:20.162 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
111 | 08:59:20.165 |  | ←enobeB PCAP frame← TCP |  |  |
112 | 08:59:20.170 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
113 | 08:59:20.194 | →enobeB PCAP frame→ TCP |  |  |  |
114 | 08:59:20.314 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 16)
115 | 08:59:20.322 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
116 | 08:59:20.325 |  | ←enobeB PCAP frame← TCP |  |  |
117 | 08:59:20.326 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
118 | 08:59:20.354 | →enobeB PCAP frame→ TCP |  |  |  |
119 | 08:59:20.394 |  |  |  |  | →HTTP GET | HTTP-Proxy
120 | 08:59:20.400 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:288: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
121 | 08:59:20.402 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
122 | 08:59:20.405 |  | ←enobeB PCAP frame← TCP |  |  |
123 | 08:59:20.419 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
124 | 08:59:20.433 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
125 | 08:59:20.434 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
126 | 08:59:20.474 | →enobeB PCAP frame→ TCP |  |  |  |
127 | 08:59:20.514 | →enobeB PCAP frame→ TCP |  |  |  |
128 | 08:59:22.434 | →enobeB PCAP frame→ TCP |  |  |  |
129 | 08:59:22.438 |  | ←enobeB PCAP frame← TCP |  |  |
130 | 08:59:22.474 | →enobeB PCAP frame→ TCP |  |  |  |
131 | 08:59:22.482 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
132 | 08:59:22.485 |  | ←enobeB PCAP frame← TCP |  |  |
133 | 08:59:22.490 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
134 | 08:59:22.514 | →enobeB PCAP frame→ TCP |  |  |  |
135 | 08:59:22.834 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:642: Client connected to IdM port (id 18)
136 | 08:59:22.842 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
137 | 08:59:22.845 |  | ←enobeB PCAP frame← TCP |  |  |
138 | 08:59:22.846 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
139 | 08:59:22.873 |  |  |  |  | →HTTP GET | IDMS-Endpoint
140 | 08:59:22.874 | →enobeB PCAP frame→ TCP |  |  |  |
141 | 08:59:22.882 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
142 | 08:59:22.885 |  | ←enobeB PCAP frame← TCP |  |  |
143 | 08:59:22.885 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
144 | 08:59:22.889 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:511: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
145 | 08:59:22.889 |  |  |  |  | MMICmd: Please provide user credentials: username and password
146 | 08:59:22.897 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
147 | 08:59:22.954 | →enobeB PCAP frame→ TCP |  |  |  |
148 | 08:59:27.436 |  |  |  |  | →HTTP POST | IDMS-Endpoint
149 | 08:59:27.442 | →enobeB PCAP frame→ HTTPS: POST /idms/userauth HTTP/1.1 |  |  |  |
150 | 08:59:27.446 |  | ←enobeB PCAP frame← TCP |  |  |
151 | 08:59:27.450 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
152 | 08:59:27.453 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:516: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
153 | 08:59:27.463 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
154 | 08:59:27.513 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:677: IdM port - Client closed the connection (id 18)
155 | 08:59:27.514 | →enobeB PCAP frame→ TCP |  |  |  |
156 | 08:59:27.522 | →enobeB PCAP frame→ DNS |  |  |  |
157 | 08:59:27.525 |  | ←enobeB PCAP frame← TCP |  |  |
158 | 08:59:27.554 | →enobeB PCAP frame→ TCP |  |  |  |
159 | 08:59:28.194 | →enobeB PCAP frame→ TCP |  |  |  |
160 | 08:59:28.198 |  | ←enobeB PCAP frame← TCP |  |  |
161 | 08:59:28.234 | →enobeB PCAP frame→ TCP |  |  |  |
162 | 08:59:28.242 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
163 | 08:59:28.245 |  | ←enobeB PCAP frame← TCP |  |  |
164 | 08:59:28.246 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
165 | 08:59:28.274 | →enobeB PCAP frame→ TCP |  |  |  |
166 | 08:59:28.314 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:642: Client connected to IdM port (id 18)
167 | 08:59:28.322 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
168 | 08:59:28.325 |  | ←enobeB PCAP frame← TCP |  |  |
169 | 08:59:28.326 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
170 | 08:59:28.354 | →enobeB PCAP frame→ TCP |  |  |  |
171 | 08:59:28.355 |  |  |  |  | →HTTP POST | IDMS-Endpoint
172 | 08:59:28.362 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
173 | 08:59:28.365 |  | ←enobeB PCAP frame← TCP |  |  |
174 | 08:59:28.374 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
175 | 08:59:28.377 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:521: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
176 | 08:59:28.386 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
177 | 08:59:28.474 | →enobeB PCAP frame→ TCP |  |  |  |
178 | 08:59:28.714 | →enobeB PCAP frame→ TCP |  |  |  |
179 | 08:59:28.717 |  | ←enobeB PCAP frame← TCP |  |  |
180 | 08:59:28.754 | →enobeB PCAP frame→ TCP |  |  |  |
181 | 08:59:28.762 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
182 | 08:59:28.765 |  | ←enobeB PCAP frame← TCP |  |  |
183 | 08:59:28.768 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
184 | 08:59:28.794 | →enobeB PCAP frame→ TCP |  |  |  |
185 | 08:59:28.795 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 19)
186 | 08:59:28.802 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
187 | 08:59:28.805 |  | ←enobeB PCAP frame← TCP |  |  |
188 | 08:59:28.806 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
189 | 08:59:28.835 |  |  |  |  | →HTTP POST | HTTP-Proxy
190 | 08:59:28.842 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
191 | 08:59:28.845 |  | ←enobeB PCAP frame← TCP |  |  |
192 | 08:59:28.860 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:541: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
193 | 08:59:28.867 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
194 | 08:59:28.881 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
195 | 08:59:28.914 | →enobeB PCAP frame→ TCP |  |  |  |
196 | 08:59:28.954 | →enobeB PCAP frame→ TCP |  |  |  |
197 | 08:59:28.957 |  | ←enobeB PCAP frame← TCP |  |  |
198 | 08:59:28.994 | →enobeB PCAP frame→ TCP |  |  |  |
199 | 08:59:29.002 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
200 | 08:59:29.005 |  | ←enobeB PCAP frame← TCP |  |  |
201 | 08:59:29.009 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
202 | 08:59:29.034 | →enobeB PCAP frame→ TCP |  |  |  |
203 | 08:59:29.034 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 20)
204 | 08:59:29.042 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
205 | 08:59:29.045 |  | ←enobeB PCAP frame← TCP |  |  |
206 | 08:59:29.046 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
207 | 08:59:29.075 |  |  |  |  | →HTTP POST | HTTP-Proxy
208 | 08:59:29.082 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
209 | 08:59:29.085 |  | ←enobeB PCAP frame← TCP |  |  |
210 | 08:59:29.140 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
211 | 08:59:29.140 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:545: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
212 | 08:59:29.153 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
213 | 08:59:29.194 | →enobeB PCAP frame→ TCP |  |  |  |
214 | 08:59:29.235 |  |  |  |  | →SIP REGISTER | P-CSCF
215 | 08:59:29.242 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
216 | 08:59:29.258 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:814: IMS UDP_s port 192.168.2.3:5062 configured
217 | 08:59:29.286 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:765: IMS TCP_s port 192.168.2.3:5062 configured!
218 | 08:59:29.288 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:823: IMS UDP_c port 192.168.2.3:5061 configured
219 | 08:59:29.294 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
220 | 08:59:29.996 |  |  |  |  | →SIP REGISTER | P-CSCF
221 | 08:59:30.002 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
222 | 08:59:30.017 |  |  |  |  | ←SIP 200 OK | P-CSCF
223 | 08:59:30.030 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
224 | 08:59:30.322 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
225 | 08:59:30.322 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
226 | 08:59:30.323 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
227 | 08:59:30.324 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 SIP over IPSEC: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 |  |  |  |
228 | 08:59:30.336 |  |  |  |  | ←SIP 200 OK | P-CSCF
229 | 08:59:30.336 |  |  |  |  | MIKEY | Media-Server
230 | 08:59:30.348 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
231 | 08:59:30.543 |  |  |  |  | XML→ | Media-Server
232 | 08:59:30.544 |  |  |  |  | XML→ | Media-Server
233 | 08:59:30.547 |  |  |  |  | ←XML | Media-Server
234 | 08:59:30.551 |  |  |  |  | ←SIP NOTIFY | P-CSCF
235 | 08:59:30.563 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:41447;transp... |  |  |
236 | 08:59:30.593 |  |  |  |  | →SIP 200 OK | P-CSCF
237 | 08:59:30.602 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
238 | 08:59:30.834 | →enobeB PCAP frame→ TCP |  |  |  |
239 | 08:59:30.837 |  | ←enobeB PCAP frame← TCP |  |  |
240 | 08:59:30.874 | →enobeB PCAP frame→ TCP |  |  |  |
241 | 08:59:30.882 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
242 | 08:59:30.885 |  | ←enobeB PCAP frame← TCP |  |  |
243 | 08:59:30.889 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
244 | 08:59:30.914 | →enobeB PCAP frame→ TCP |  |  |  |
245 | 08:59:30.954 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
246 | 08:59:30.962 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
247 | 08:59:30.965 |  | ←enobeB PCAP frame← TCP |  |  |
248 | 08:59:30.966 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
249 | 08:59:30.994 | →enobeB PCAP frame→ TCP |  |  |  |
250 | 08:59:30.994 |  |  |  |  | →HTTP GET | HTTP-Proxy
251 | 08:59:31.002 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-co... |  |  |  |
252 | 08:59:31.003 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:642: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcptt-ue-configuration.xml
253 | 08:59:31.005 |  | ←enobeB PCAP frame← TCP |  |  |
254 | 08:59:31.011 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
255 | 08:59:31.024 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
256 | 08:59:31.066 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
257 | 08:59:31.074 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
258 | 08:59:31.077 |  | ←enobeB PCAP frame← TCP |  |  |
259 | 08:59:31.082 | →enobeB PCAP frame→ TCP |  |  |  |
260 | 08:59:31.085 |  | ←enobeB PCAP frame← TCP |  |  |
261 | 08:59:31.114 | →enobeB PCAP frame→ TCP |  |  |  |
262 | 08:59:31.274 | →enobeB PCAP frame→ TCP |  |  |  |
263 | 08:59:31.277 |  | ←enobeB PCAP frame← TCP |  |  |
264 | 08:59:31.314 | →enobeB PCAP frame→ TCP |  |  |  |
265 | 08:59:31.322 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
266 | 08:59:31.325 |  | ←enobeB PCAP frame← TCP |  |  |
267 | 08:59:31.328 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
268 | 08:59:31.354 | →enobeB PCAP frame→ TCP |  |  |  |
269 | 08:59:31.434 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
270 | 08:59:31.442 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
271 | 08:59:31.445 |  | ←enobeB PCAP frame← TCP |  |  |
272 | 08:59:31.446 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
273 | 08:59:31.474 | →enobeB PCAP frame→ TCP |  |  |  |
274 | 08:59:31.514 |  |  |  |  | →HTTP GET | HTTP-Proxy
275 | 08:59:31.522 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-... |  |  |  |
276 | 08:59:31.525 |  | ←enobeB PCAP frame← TCP |  |  |
277 | 08:59:31.527 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:647: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcptt-user-profile-49.xml
278 | 08:59:31.567 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
279 | 08:59:31.584 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
280 | 08:59:31.585 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
281 | 08:59:31.634 | →enobeB PCAP frame→ TCP |  |  |  |
282 | 08:59:31.634 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
283 | 08:59:31.642 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
284 | 08:59:31.645 |  | ←enobeB PCAP frame← TCP |  |  |
285 | 08:59:31.674 | →enobeB PCAP frame→ TCP |  |  |  |
286 | 08:59:32.242 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
287 | 08:59:32.242 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
288 | 08:59:32.243 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
289 | 08:59:32.255 |  |  |  |  | ←SIP 200 OK | P-CSCF
290 | 08:59:32.255 |  |  |  |  | MIKEY | Media-Server
291 | 08:59:32.267 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
292 | 08:59:32.314 | →enobeB PCAP frame→ TCP |  |  |  |
293 | 08:59:32.317 |  | ←enobeB PCAP frame← TCP |  |  |
294 | 08:59:32.354 | →enobeB PCAP frame→ TCP |  |  |  |
295 | 08:59:32.362 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
296 | 08:59:32.365 |  | ←enobeB PCAP frame← TCP |  |  |
297 | 08:59:32.366 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
298 | 08:59:32.394 | →enobeB PCAP frame→ TCP |  |  |  |
299 | 08:59:32.462 |  |  |  |  | XML→ | Media-Server
300 | 08:59:32.463 |  |  |  |  | XML→ | Media-Server
301 | 08:59:32.466 |  |  |  |  | ←XML | Media-Server
302 | 08:59:32.473 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
303 | 08:59:32.474 |  |  |  |  | ←SIP NOTIFY | P-CSCF
304 | 08:59:32.482 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
305 | 08:59:32.485 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
306 | 08:59:32.486 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:41447;transp... |  |  |
307 | 08:59:32.514 | →enobeB PCAP frame→ TCP |  |  |  |
308 | 08:59:32.515 |  |  |  |  | →SIP 200 OK | P-CSCF
309 | 08:59:32.515 |  |  |  |  | →HTTP GET | HTTP-Proxy
310 | 08:59:32.522 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.servi... |  |  |  |
311 | 08:59:32.523 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:652: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
312 | 08:59:32.525 |  | ←enobeB PCAP frame← TCP |  |  |
313 | 08:59:32.528 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
314 | 08:59:32.541 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
315 | 08:59:32.542 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
316 | 08:59:32.593 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
317 | 08:59:32.594 | →enobeB PCAP frame→ TCP |  |  |  |
318 | 08:59:32.602 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
319 | 08:59:32.605 |  | ←enobeB PCAP frame← TCP |  |  |
320 | 08:59:32.634 | →enobeB PCAP frame→ TCP |  |  |  |
321 | 08:59:32.714 | →enobeB PCAP frame→ TCP |  |  |  |
322 | 08:59:32.717 |  | ←enobeB PCAP frame← TCP |  |  |
323 | 08:59:32.754 | →enobeB PCAP frame→ TCP |  |  |  |
324 | 08:59:32.762 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
325 | 08:59:32.765 |  | ←enobeB PCAP frame← TCP |  |  |
326 | 08:59:32.768 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
327 | 08:59:32.794 | →enobeB PCAP frame→ TCP |  |  |  |
328 | 08:59:32.874 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
329 | 08:59:32.882 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
330 | 08:59:32.885 |  | ←enobeB PCAP frame← TCP |  |  |
331 | 08:59:32.886 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
332 | 08:59:32.914 | →enobeB PCAP frame→ TCP |  |  |  |
333 | 08:59:32.914 |  |  |  |  | →HTTP GET | HTTP-Proxy
334 | 08:59:32.922 | →enobeB PCAP frame→ HTTPS: GET /xcap.gms.mcstaasting.com/org.openmobileallian... |  |  |  |
335 | 08:59:32.925 |  | ←enobeB PCAP frame← TCP |  |  |
336 | 08:59:32.925 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:657: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at /xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
337 | 08:59:32.949 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
338 | 08:59:32.964 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
339 | 08:59:32.993 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
340 | 08:59:32.994 | →enobeB PCAP frame→ TCP |  |  |  |
341 | 08:59:33.002 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
342 | 08:59:33.006 |  | ←enobeB PCAP frame← TCP |  |  |
343 | 08:59:33.034 | →enobeB PCAP frame→ TCP |  |  |  |
344 | 08:59:33.242 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
345 | 08:59:33.243 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
346 | 08:59:33.246 |  |  |  |  | →SIP PUBLISH | P-CSCF
347 | 08:59:33.293 |  |  |  |  | MIKEY | Media-Server
348 | 08:59:33.357 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
349 | 08:59:33.362 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
350 | 08:59:33.363 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
351 | 08:59:33.518 |  |  |  |  | XML→ | Media-Server
352 | 08:59:33.521 |  |  |  |  | ←SIP 200 OK | P-CSCF
353 | 08:59:33.524 |  |  |  |  | ←SIP 200 OK | P-CSCF
354 | 08:59:33.524 |  |  |  |  | MIKEY | Media-Server
355 | 08:59:33.533 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
356 | 08:59:33.536 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
357 | 08:59:33.726 |  |  |  |  | XML→ | Media-Server
358 | 08:59:33.727 |  |  |  |  | XML→ | Media-Server
359 | 08:59:33.761 |  |  |  |  | ←XML | Media-Server
360 | 08:59:33.765 |  |  |  |  | ←SIP NOTIFY | P-CSCF
361 | 08:59:33.778 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:41447;transp... |  |  |
362 | 08:59:33.833 |  |  |  |  | →SIP 200 OK | P-CSCF
363 | 08:59:33.838 |  |  |  |  | ←XML | Media-Server
364 | 08:59:33.842 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
365 | 08:59:33.851 |  |  |  |  | ←SIP MESSAGE | P-CSCF
366 | 08:59:33.864 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
367 | 08:59:34.674 |  |  |  |  | →SIP 200 OK | P-CSCF
368 | 08:59:34.681 |  |  |  |  | Info: MCX_IMS_CommonProcedures.ttcn:155: MESSAGE/200OK Table 5.3.2.3-2 Steps 7-8 Done
369 | 08:59:34.682 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
370 | 08:59:34.695 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
371 | 08:59:34.714 | →enobeB PCAP frame→ TCP |  |  |  |
372 | 08:59:34.754 | →enobeB PCAP frame→ TCP |  |  |  |
373 | 08:59:36.746 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
374 | 08:59:36.790 |  | ←RRC DCCH RRC Connection Release |  |  |
375 | 08:59:36.791 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
376 | 08:59:36.801 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
377 | 08:59:36.803 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
378 | 08:59:36.803 |  |  |  |  | MMICmd: Make the MCPTT User requesting the establishment of an MCPTT On-demand pre-arranged emergency group call for the selected MCPTT emergency group GROUP A, with explicit floor control
379 | 08:59:41.271 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
380 | 08:59:41.271 |  | →RRC CCCH RRC Connection Request |  |  |
381 | 08:59:41.271 |  | ←RRC CCCH RRC Connection Setup |  |  |
382 | 08:59:41.271 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
383 | 08:59:41.314 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
384 | 08:59:41.314 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
385 | 08:59:41.314 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
386 | 08:59:41.314 |  |  |  | →NAS EMM Service request |  |
387 | 08:59:41.314 |  |  |  | NAS K-enb 145efd88f95bf5fa5037fd1fc3a22d64a... |  |
388 | 08:59:41.315 |  | ←RRC DCCH Security Mode Command |  |  |
389 | 08:59:41.315 |  |  | RRC K-enb 145efd88f95bf5fa5037fd1fc3a22d64a... |  |  |
390 | 08:59:41.315 |  |  | RRC rrc-cip 2fd146b6a3d452e5cb063657173f996... |  |  |
391 | 08:59:41.315 |  |  | RRC rrc-int f5b56bf8fd99a98e776ba08bd12a5bd... |  |  |
392 | 08:59:41.315 |  |  | RRC up-cip cefb77238f66ed9e497298c02154b796... |  |  |
393 | 08:59:41.315 |  |  | RRC up-int 03ab22cf40ebee9478db533afb089b99... |  |  |
394 | 08:59:41.316 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
395 | 08:59:41.354 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
396 | 08:59:41.354 |  | →RRC DCCH Security Mode Complete |  |  |
397 | 08:59:41.354 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
398 | 08:59:41.354 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
399 | 08:59:41.394 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
400 | 08:59:41.394 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
401 | 08:59:41.402 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
402 | 08:59:41.403 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
403 | 08:59:41.405 |  |  |  |  | →SIP INVITE | P-CSCF
404 | 08:59:41.428 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:735: SRTP config: Master Key: ABAA68F0FDDD36AF8E8C387CE9FF379F, Master Salt: C280E35181446FEAF7AE6B04, MKI: 2B08696A
405 | 08:59:41.428 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
406 | 08:59:41.431 |  |  |  |  | XML→ | Media-Server
407 | 08:59:41.432 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
408 | 08:59:41.433 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1205: INVITE Verdict: Pass
409 | 08:59:41.434 |  |  |  |  | ←SIP 100 Trying | P-CSCF
410 | 08:59:41.436 |  |  |  |  | ←SIP 200 OK | P-CSCF
411 | 08:59:41.446 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
412 | 08:59:41.448 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
413 | 08:59:42.093 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
414 | 08:59:42.093 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x3) |  |  |
415 | 08:59:42.093 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
416 | 08:59:42.094 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
417 | 08:59:42.114 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
418 | 08:59:42.114 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
419 | 08:59:42.154 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
420 | 08:59:42.154 |  | →RRC DCCH UL Information Transfer |  |  |
421 | 08:59:42.154 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x8) |  |  |
422 | 08:59:42.154 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
423 | 08:59:42.227 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
424 | 08:59:42.315 |  |  |  |  | →SIP ACK | P-CSCF
425 | 08:59:42.322 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
426 | 08:59:42.324 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1208: ACK Verdict: Pass
427 | 08:59:42.324 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:451: Step 2 Verdict: Pass
428 | 08:59:42.874 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
429 | 08:59:42.882 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
430 | 08:59:42.914 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
431 | 08:59:42.922 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
432 | 08:59:42.954 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
433 | 08:59:43.075 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:456: Step 5A Verdict: Pass
434 | 08:59:43.083 |  |  |  |  | ←SIP BYE | P-CSCF
435 | 08:59:43.096 |  | ←enobeB PCAP frame← SIP over IPSEC: BYE sip:PublicUserId-A@192.168.3.2:41447;transport... |  |  |
436 | 08:59:43.114 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
437 | 08:59:43.122 |  |  |  |  | →SIP 200 OK | P-CSCF
438 | 08:59:43.130 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK SRTP frame: |  |  |  |
439 | 08:59:43.138 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
440 | 08:59:43.594 | →enobeB PCAP frame→ |  |  |  |
441 | 08:59:45.130 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
442 | 08:59:45.147 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
443 | 08:59:45.148 |  | [EMBEDDED NAS IN NEXT RRC] TP Unknown message (type=0x32) |  |  |
444 | 08:59:45.148 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
445 | 08:59:45.149 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
446 | 08:59:45.194 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
447 | 08:59:45.194 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
448 | 08:59:45.194 |  | →RRC DCCH UL Information Transfer |  |  |
449 | 08:59:45.194 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xc) |  |  |
450 | 08:59:45.194 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
451 | 08:59:45.255 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
452 | 08:59:45.256 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
453 | 08:59:45.300 |  | ←RRC DCCH RRC Connection Release |  |  |
454 | 08:59:45.301 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
455 | 08:59:45.311 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
456 | 08:59:45.313 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
457 | 08:59:45.315 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
458 | 08:59:46.063 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.