MSG #80 2021-09-07 08:58:59.355
NAS

     EMM: Service request
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x2 (Integrity protected and ciphered)
    Auth code = 0xd880d48f
    Sequence number = 0x03
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0xd (?)
    NAS key set identifier = 2
    Sequence number = 0x1b
    Auth code = 0xdd27
    Remaining bytes:
      95 a8 0a f6 1b c6 16 b5 a7 13 0d 75 e0 2d 53 03
      7f 71 d4 f8 fd f2 83 90 ba 82 75 63 56 36 d4 c3
      1e 28 d9