MSG #35 2021-09-07 08:58:59.114
NAS

     EMM: Authentication response
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x1 (Integrity protected)
    Auth code = 0xed49cb22
    Sequence number = 0x0b
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x0 (Plain NAS message, not security protected)
    Message type = 0x53 (Authentication response)
    Authentication response parameter:
      Length = 8
      Data = 61 11 c0 e4 a4 a9 d0 0c