ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 12:53:52.818 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 12:53:52.824 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 12:53:52.824 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 12:53:52.826 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 12:53:52.826 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 12:53:52.827 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:805: IMS UDP port 192.168.2.3:5060 configured
7 | 12:53:52.829 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:755: IMS TCP port 192.168.2.3:5060 configured!
8 | 12:53:52.830 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:776: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 12:53:52.831 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:787: IdM port 192.168.2.3:8080 configured!
10 | 12:53:52.832 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 12:53:54.033 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 12:53:54.033 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 12:53:55.663 |  | ←RRC BCCH SIB1 |  |  |
14 | 12:53:55.738 |  | ←RRC BCCH SIB |  |  |
15 | 12:53:55.743 |  | ←RRC BCCH SIB1 |  |  |
16 | 12:53:55.758 |  | ←RRC BCCH SIB |  |  |
17 | 12:53:55.778 |  | ←RRC BCCH SIB |  |  |
18 | 12:55:35.007 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 12:55:35.007 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 12:55:35.007 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 12:55:35.007 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 12:55:35.038 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 12:55:35.038 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 12:55:35.038 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 12:55:35.038 |  |  |  | →NAS EMM Attach request |  |
26 | 12:55:35.038 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 12:55:35.039 |  |  |  | NAS K-asme 219865e35b065c869a5fa6e2bd4db440... |  |
28 | 12:55:35.039 |  |  |  | NAS ← EMM Authentication request |  |
29 | 12:55:35.039 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 12:55:35.039 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 12:55:35.040 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 12:55:35.110 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 12:55:35.110 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 12:55:35.110 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 12:55:35.110 |  |  |  | →NAS EMM Authentication response |  |
36 | 12:55:35.110 |  |  |  | NAS UE auth OK |  |
37 | 12:55:35.110 |  |  |  | NAS K-nas-cip ea55a0746e14c1a543b3ff9a8ad16... |  |
38 | 12:55:35.110 |  |  |  | NAS K-nas-int 01ef9bc4c6fd98b20b7e3e01c4959... |  |
39 | 12:55:35.110 |  |  |  | NAS ← EMM Security mode command |  |
40 | 12:55:35.111 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 12:55:35.111 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 12:55:35.112 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 12:55:35.150 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
44 | 12:55:35.150 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 12:55:35.150 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x1) |  |  |
46 | 12:55:35.150 |  |  |  | →NAS EMM Security mode complete |  |
47 | 12:55:35.151 |  |  |  | NAS ← ESM ESM information request |  |
48 | 12:55:35.151 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xc) |  |  |
49 | 12:55:35.151 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 12:55:35.152 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
51 | 12:55:35.198 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
52 | 12:55:35.198 |  | →RRC DCCH UL Information Transfer |  |  |
53 | 12:55:35.198 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x3) |  |  |
54 | 12:55:35.198 |  |  |  | →NAS ESM ESM information response |  |
55 | 12:55:35.198 |  |  |  | NAS ← EMM Attach accept |  |
56 | 12:55:35.198 |  |  |  | NAS K-enb baa113f29e7ab3648af22e6af064ebf54... |  |
57 | 12:55:35.199 |  | ←RRC DCCH Security Mode Command |  |  |
58 | 12:55:35.199 |  |  | RRC K-enb baa113f29e7ab3648af22e6af064ebf54... |  |  |
59 | 12:55:35.199 |  |  | RRC rrc-cip dbe10422cfe8549f7470e7626fc05a3... |  |  |
60 | 12:55:35.199 |  |  | RRC rrc-int 779f15d9612489346719a24a58c4d2b... |  |  |
61 | 12:55:35.199 |  |  | RRC up-cip 8af193769cd894c3ac926775bca3b4b1... |  |  |
62 | 12:55:35.199 |  |  | RRC up-int 59c191780a426f3e25ca64faf685ece0... |  |  |
63 | 12:55:35.200 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
64 | 12:55:35.208 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
65 | 12:55:35.230 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
66 | 12:55:35.230 |  | →RRC DCCH Security Mode Complete |  |  |
67 | 12:55:35.230 |  | ←RRC DCCH UE Capability Enquiry |  |  |
68 | 12:55:35.230 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
69 | 12:55:35.280 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
70 | 12:55:35.280 |  | →RRC DCCH UE Capability Information |  |  |
71 | 12:55:35.281 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x0) |  |  |
72 | 12:55:35.281 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
73 | 12:55:35.281 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
74 | 12:55:35.310 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
75 | 12:55:35.310 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
76 | 12:55:35.350 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
77 | 12:55:35.350 |  | →RRC DCCH UL Information Transfer |  |  |
78 | 12:55:35.350 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x4) |  |  |
79 | 12:55:35.350 |  |  |  | →NAS EMM Attach complete |  |
80 | 12:55:35.351 |  |  |  | NAS ← EMM EMM information |  |
81 | 12:55:35.351 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x4) |  |  |
82 | 12:55:35.351 |  | ←RRC DCCH DL Information Transfer |  |  |
83 | 12:55:35.352 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
84 | 12:55:41.435 |  | ←RRC DCCH RRC Connection Release |  |  |
85 | 12:55:41.436 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
86 | 12:55:42.107 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
87 | 12:55:42.107 |  | →RRC CCCH RRC Connection Request |  |  |
88 | 12:55:42.107 |  | ←RRC CCCH RRC Connection Setup |  |  |
89 | 12:55:42.107 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
90 | 12:55:42.150 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
91 | 12:55:42.150 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
92 | 12:55:42.150 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
93 | 12:55:42.150 |  |  |  | →NAS EMM Service request |  |
94 | 12:55:42.150 |  |  |  | NAS K-enb 0cbf023bf89913cc5e0b08ce62bb3cd86... |  |
95 | 12:55:42.151 |  |  | RRC K-enb 0cbf023bf89913cc5e0b08ce62bb3cd86... |  |  |
96 | 12:55:42.152 |  |  | RRC rrc-cip 6261846929fa697fc0c4912cf46623f... |  |  |
97 | 12:55:42.152 |  |  | RRC rrc-int 56a046b695e6f436a25afd401edb19a... |  |  |
98 | 12:55:42.152 |  |  | RRC up-cip b5af9e1fec3612e0c90087d60fc85fa3... |  |  |
99 | 12:55:42.152 |  |  | RRC up-int c960f46251674089ce861a50cf95de45... |  |  |
100 | 12:55:42.152 |  | ←RRC DCCH Security Mode Command |  |  |
101 | 12:55:42.152 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
102 | 12:55:42.190 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
103 | 12:55:42.190 |  | →RRC DCCH Security Mode Complete |  |  |
104 | 12:55:42.190 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
105 | 12:55:42.190 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
106 | 12:55:42.230 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
107 | 12:55:42.230 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
108 | 12:56:09.110 | →enobeB PCAP frame→ TCP |  |  |  |
109 | 12:56:09.113 |  | ←enobeB PCAP frame← TCP |  |  |
110 | 12:56:09.150 | →enobeB PCAP frame→ TCP |  |  |  |
111 | 12:56:09.238 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
112 | 12:56:09.241 |  | ←enobeB PCAP frame← TCP |  |  |
113 | 12:56:09.242 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
114 | 12:56:09.270 | →enobeB PCAP frame→ TCP |  |  |  |
115 | 12:56:09.398 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
116 | 12:56:09.400 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 16)
117 | 12:56:09.401 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
118 | 12:56:09.430 | →enobeB PCAP frame→ TCP |  |  |  |
119 | 12:56:09.478 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
120 | 12:56:09.480 |  |  |  |  | →HTTP GET | HTTP-Proxy
121 | 12:56:09.481 |  | ←enobeB PCAP frame← TCP |  |  |
122 | 12:56:09.482 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:288: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
123 | 12:56:09.486 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
124 | 12:56:09.487 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
125 | 12:56:09.510 | →enobeB PCAP frame→ TCP |  |  |  |
126 | 12:56:11.670 | →enobeB PCAP frame→ TCP |  |  |  |
127 | 12:56:11.673 |  | ←enobeB PCAP frame← TCP |  |  |
128 | 12:56:11.710 | →enobeB PCAP frame→ TCP |  |  |  |
129 | 12:56:11.718 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
130 | 12:56:11.721 |  | ←enobeB PCAP frame← TCP |  |  |
131 | 12:56:11.722 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
132 | 12:56:11.750 | →enobeB PCAP frame→ TCP |  |  |  |
133 | 12:56:12.038 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
134 | 12:56:12.040 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:642: Client connected to IdM port (id 18)
135 | 12:56:12.041 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
136 | 12:56:12.070 | →enobeB PCAP frame→ TCP |  |  |  |
137 | 12:56:12.078 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
138 | 12:56:12.080 |  |  |  |  | →HTTP GET | IDMS-Endpoint
139 | 12:56:12.082 |  | ←enobeB PCAP frame← TCP |  |  |
140 | 12:56:12.091 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
141 | 12:56:12.092 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
142 | 12:56:12.095 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:511: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
143 | 12:56:12.096 |  |  |  |  | MMICmd: Please provide user credentials: username and password
144 | 12:56:18.438 | →enobeB PCAP frame→ TCP |  |  |  |
145 | 12:56:18.441 |  | ←enobeB PCAP frame← TCP |  |  |
146 | 12:56:18.441 |  |  |  |  | →HTTP POST | IDMS-Endpoint
147 | 12:56:18.444 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
148 | 12:56:18.445 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
149 | 12:56:18.448 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:516: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
150 | 12:56:18.470 | →enobeB PCAP frame→ TCP |  |  |  |
151 | 12:56:18.478 | →enobeB PCAP frame→ TCP |  |  |  |
152 | 12:56:18.480 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:677: IdM port - Client closed the connection (id 18)
153 | 12:56:18.481 |  | ←enobeB PCAP frame← TCP |  |  |
154 | 12:56:18.510 | →enobeB PCAP frame→ TCP |  |  |  |
155 | 12:56:18.910 | →enobeB PCAP frame→ TCP |  |  |  |
156 | 12:56:18.913 |  | ←enobeB PCAP frame← TCP |  |  |
157 | 12:56:18.950 | →enobeB PCAP frame→ TCP |  |  |  |
158 | 12:56:18.958 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
159 | 12:56:18.961 |  | ←enobeB PCAP frame← TCP |  |  |
160 | 12:56:18.962 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
161 | 12:56:18.990 | →enobeB PCAP frame→ TCP |  |  |  |
162 | 12:56:19.078 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
163 | 12:56:19.080 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:642: Client connected to IdM port (id 18)
164 | 12:56:19.081 |  | ←enobeB PCAP frame← TCP |  |  |
165 | 12:56:19.082 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
166 | 12:56:19.110 | →enobeB PCAP frame→ TCP |  |  |  |
167 | 12:56:19.158 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
168 | 12:56:19.160 |  |  |  |  | →HTTP POST | IDMS-Endpoint
169 | 12:56:19.161 |  | ←enobeB PCAP frame← TCP |  |  |
170 | 12:56:19.170 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
171 | 12:56:19.172 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
172 | 12:56:19.174 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:521: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
173 | 12:56:19.230 | →enobeB PCAP frame→ TCP |  |  |  |
174 | 12:56:19.470 | →enobeB PCAP frame→ TCP |  |  |  |
175 | 12:56:19.473 |  | ←enobeB PCAP frame← TCP |  |  |
176 | 12:56:19.510 | →enobeB PCAP frame→ TCP |  |  |  |
177 | 12:56:19.518 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
178 | 12:56:19.521 |  | ←enobeB PCAP frame← TCP |  |  |
179 | 12:56:19.522 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
180 | 12:56:19.550 | →enobeB PCAP frame→ TCP |  |  |  |
181 | 12:56:19.598 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
182 | 12:56:19.600 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 19)
183 | 12:56:19.601 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
184 | 12:56:19.638 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
185 | 12:56:19.641 |  | ←enobeB PCAP frame← TCP |  |  |
186 | 12:56:19.641 |  |  |  |  | →HTTP POST | HTTP-Proxy
187 | 12:56:19.647 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
188 | 12:56:19.649 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
189 | 12:56:19.650 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:541: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
190 | 12:56:19.670 | →enobeB PCAP frame→ TCP |  |  |  |
191 | 12:56:19.750 | →enobeB PCAP frame→ TCP |  |  |  |
192 | 12:56:19.753 |  | ←enobeB PCAP frame← TCP |  |  |
193 | 12:56:19.790 | →enobeB PCAP frame→ TCP |  |  |  |
194 | 12:56:19.798 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
195 | 12:56:19.801 |  | ←enobeB PCAP frame← TCP |  |  |
196 | 12:56:19.802 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
197 | 12:56:19.830 | →enobeB PCAP frame→ TCP |  |  |  |
198 | 12:56:19.838 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
199 | 12:56:19.840 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 20)
200 | 12:56:19.841 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
201 | 12:56:19.878 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
202 | 12:56:19.880 |  |  |  |  | →HTTP POST | HTTP-Proxy
203 | 12:56:19.881 |  | ←enobeB PCAP frame← TCP |  |  |
204 | 12:56:19.902 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
205 | 12:56:19.904 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
206 | 12:56:19.904 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:545: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
207 | 12:56:19.950 | →enobeB PCAP frame→ TCP |  |  |  |
208 | 12:56:19.998 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
209 | 12:56:20.001 |  |  |  |  | →SIP REGISTER | P-CSCF
210 | 12:56:20.006 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:814: IMS UDP_s port 192.168.2.3:5062 configured
211 | 12:56:20.013 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:765: IMS TCP_s port 192.168.2.3:5062 configured!
212 | 12:56:20.013 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:823: IMS UDP_c port 192.168.2.3:5061 configured
213 | 12:56:20.016 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
214 | 12:56:20.638 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
215 | 12:56:20.641 |  |  |  |  | →SIP REGISTER | P-CSCF
216 | 12:56:20.647 |  |  |  |  | ←SIP 200 OK | P-CSCF
217 | 12:56:20.648 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
218 | 12:56:20.998 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
219 | 12:56:20.999 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
220 | 12:56:21.000 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 SIP over IPSEC: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 |  |  |  |
221 | 12:56:21.005 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
222 | 12:56:21.018 |  |  |  |  | ←SIP 200 OK | P-CSCF
223 | 12:56:21.018 |  |  |  |  | MIKEY | Media-Server
224 | 12:56:21.020 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
225 | 12:56:21.247 |  |  |  |  | XML→ | Media-Server
226 | 12:56:21.248 |  |  |  |  | XML→ | Media-Server
227 | 12:56:21.251 |  |  |  |  | ←XML | Media-Server
228 | 12:56:21.255 |  |  |  |  | ←SIP NOTIFY | P-CSCF
229 | 12:56:21.256 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:38862;transp... |  |  |
230 | 12:56:21.318 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
231 | 12:56:21.320 |  |  |  |  | →SIP 200 OK | P-CSCF
232 | 12:56:21.590 | →enobeB PCAP frame→ TCP |  |  |  |
233 | 12:56:21.593 |  | ←enobeB PCAP frame← TCP |  |  |
234 | 12:56:21.630 | →enobeB PCAP frame→ TCP |  |  |  |
235 | 12:56:21.638 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
236 | 12:56:21.641 |  | ←enobeB PCAP frame← TCP |  |  |
237 | 12:56:21.642 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
238 | 12:56:21.670 | →enobeB PCAP frame→ TCP |  |  |  |
239 | 12:56:21.718 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
240 | 12:56:21.720 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
241 | 12:56:21.721 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
242 | 12:56:21.750 | →enobeB PCAP frame→ TCP |  |  |  |
243 | 12:56:21.798 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-co... |  |  |  |
244 | 12:56:21.800 |  |  |  |  | →HTTP GET | HTTP-Proxy
245 | 12:56:21.801 |  | ←enobeB PCAP frame← TCP |  |  |
246 | 12:56:21.803 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:642: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcptt-ue-configuration.xml
247 | 12:56:21.805 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
248 | 12:56:21.806 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
249 | 12:56:21.870 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
250 | 12:56:21.872 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
251 | 12:56:21.873 |  | ←enobeB PCAP frame← TCP |  |  |
252 | 12:56:21.878 | →enobeB PCAP frame→ TCP |  |  |  |
253 | 12:56:21.881 |  | ←enobeB PCAP frame← TCP |  |  |
254 | 12:56:21.910 | →enobeB PCAP frame→ TCP |  |  |  |
255 | 12:56:21.990 | →enobeB PCAP frame→ TCP |  |  |  |
256 | 12:56:21.993 |  | ←enobeB PCAP frame← TCP |  |  |
257 | 12:56:22.030 | →enobeB PCAP frame→ TCP |  |  |  |
258 | 12:56:22.038 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
259 | 12:56:22.041 |  | ←enobeB PCAP frame← TCP |  |  |
260 | 12:56:22.042 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
261 | 12:56:22.070 | →enobeB PCAP frame→ TCP |  |  |  |
262 | 12:56:22.118 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
263 | 12:56:22.120 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
264 | 12:56:22.121 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
265 | 12:56:22.150 | →enobeB PCAP frame→ TCP |  |  |  |
266 | 12:56:22.158 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-... |  |  |  |
267 | 12:56:22.160 |  |  |  |  | →HTTP GET | HTTP-Proxy
268 | 12:56:22.161 |  | ←enobeB PCAP frame← TCP |  |  |
269 | 12:56:22.163 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:647: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcptt-user-profile-49.xml
270 | 12:56:22.174 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
271 | 12:56:22.176 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
272 | 12:56:22.177 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
273 | 12:56:22.190 | →enobeB PCAP frame→ TCP |  |  |  |
274 | 12:56:22.198 | →enobeB PCAP frame→ TCP |  |  |  |
275 | 12:56:22.230 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
276 | 12:56:22.232 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
277 | 12:56:22.233 |  | ←enobeB PCAP frame← TCP |  |  |
278 | 12:56:22.238 | →enobeB PCAP frame→ TCP |  |  |  |
279 | 12:56:22.241 |  | ←enobeB PCAP frame← TCP |  |  |
280 | 12:56:22.270 | →enobeB PCAP frame→ TCP |  |  |  |
281 | 12:56:22.798 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
282 | 12:56:22.799 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
283 | 12:56:22.836 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
284 | 12:56:22.850 |  |  |  |  | ←SIP 200 OK | P-CSCF
285 | 12:56:22.850 |  |  |  |  | MIKEY | Media-Server
286 | 12:56:22.851 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
287 | 12:56:22.870 | →enobeB PCAP frame→ TCP |  |  |  |
288 | 12:56:22.873 |  | ←enobeB PCAP frame← TCP |  |  |
289 | 12:56:22.910 | →enobeB PCAP frame→ TCP |  |  |  |
290 | 12:56:22.918 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
291 | 12:56:22.921 |  | ←enobeB PCAP frame← TCP |  |  |
292 | 12:56:22.922 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
293 | 12:56:22.950 | →enobeB PCAP frame→ TCP |  |  |  |
294 | 12:56:23.038 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
295 | 12:56:23.040 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
296 | 12:56:23.041 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
297 | 12:56:23.070 | →enobeB PCAP frame→ TCP |  |  |  |
298 | 12:56:23.078 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.servi... |  |  |  |
299 | 12:56:23.081 |  | ←enobeB PCAP frame← TCP |  |  |
300 | 12:56:23.081 |  |  |  |  | →HTTP GET | HTTP-Proxy
301 | 12:56:23.083 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:652: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
302 | 12:56:23.085 |  |  |  |  | XML→ | Media-Server
303 | 12:56:23.087 |  |  |  |  | XML→ | Media-Server
304 | 12:56:23.091 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
305 | 12:56:23.091 |  |  |  |  | ←XML | Media-Server
306 | 12:56:23.093 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
307 | 12:56:23.094 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
308 | 12:56:23.095 |  |  |  |  | ←SIP NOTIFY | P-CSCF
309 | 12:56:23.096 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:38862;transp... |  |  |
310 | 12:56:23.150 | →enobeB PCAP frame→ TCP |  |  |  |
311 | 12:56:23.158 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK TLS: Mix Info |  |  |  |
312 | 12:56:23.160 |  |  |  |  | →SIP 200 OK | P-CSCF
313 | 12:56:23.160 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
314 | 12:56:23.161 |  | ←enobeB PCAP frame← TCP |  |  |
315 | 12:56:23.190 | →enobeB PCAP frame→ TCP |  |  |  |
316 | 12:56:23.270 | →enobeB PCAP frame→ TCP |  |  |  |
317 | 12:56:23.273 |  | ←enobeB PCAP frame← TCP |  |  |
318 | 12:56:23.310 | →enobeB PCAP frame→ TCP |  |  |  |
319 | 12:56:23.318 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
320 | 12:56:23.321 |  | ←enobeB PCAP frame← TCP |  |  |
321 | 12:56:23.322 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
322 | 12:56:23.350 | →enobeB PCAP frame→ TCP |  |  |  |
323 | 12:56:23.398 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
324 | 12:56:23.400 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
325 | 12:56:23.401 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
326 | 12:56:23.448 |  |  |  |  | →HTTP GET | HTTP-Proxy
327 | 12:56:23.449 |  | ←enobeB PCAP frame← TCP |  |  |
328 | 12:56:23.451 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:657: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at /xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
329 | 12:56:23.456 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
330 | 12:56:23.458 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
331 | 12:56:23.478 | →enobeB PCAP frame→ TCP |  |  |  |
332 | 12:56:23.510 | →enobeB PCAP frame→ TCP |  |  |  |
333 | 12:56:23.512 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
334 | 12:56:23.513 |  | ←enobeB PCAP frame← TCP |  |  |
335 | 12:56:23.518 | →enobeB PCAP frame→ TCP |  |  |  |
336 | 12:56:23.522 |  | ←enobeB PCAP frame← TCP |  |  |
337 | 12:56:23.550 | →enobeB PCAP frame→ TCP |  |  |  |
338 | 12:56:23.718 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
339 | 12:56:23.719 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
340 | 12:56:23.724 |  |  |  |  | →SIP PUBLISH | P-CSCF
341 | 12:56:23.735 |  |  |  |  | MIKEY | Media-Server
342 | 12:56:23.798 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
343 | 12:56:23.799 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
344 | 12:56:23.804 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
345 | 12:56:23.968 |  |  |  |  | XML→ | Media-Server
346 | 12:56:23.972 |  |  |  |  | ←SIP 200 OK | P-CSCF
347 | 12:56:23.973 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
348 | 12:56:23.975 |  |  |  |  | ←SIP 200 OK | P-CSCF
349 | 12:56:23.975 |  |  |  |  | MIKEY | Media-Server
350 | 12:56:23.977 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
351 | 12:56:24.215 |  |  |  |  | XML→ | Media-Server
352 | 12:56:24.216 |  |  |  |  | XML→ | Media-Server
353 | 12:56:24.255 |  |  |  |  | ←XML | Media-Server
354 | 12:56:24.260 |  |  |  |  | ←SIP NOTIFY | P-CSCF
355 | 12:56:24.262 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:38862;transp... |  |  |
356 | 12:56:24.318 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
357 | 12:56:24.320 |  |  |  |  | →SIP 200 OK | P-CSCF
358 | 12:56:24.323 |  |  |  |  | ←XML | Media-Server
359 | 12:56:24.330 |  |  |  |  | ←SIP MESSAGE | P-CSCF
360 | 12:56:24.333 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
361 | 12:56:25.198 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
362 | 12:56:25.200 |  |  |  |  | →SIP 200 OK | P-CSCF
363 | 12:56:25.202 |  |  |  |  | Info: MCX_IMS_CommonProcedures.ttcn:155: MESSAGE/200OK Table 5.3.2.3-2 Steps 7-8 Done
364 | 12:56:25.203 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
365 | 12:56:25.204 |  | ←enobeB PCAP frame← TCP |  |  |
366 | 12:56:25.230 | →enobeB PCAP frame→ TCP |  |  |  |
367 | 12:56:25.270 | →enobeB PCAP frame→ TCP |  |  |  |
368 | 12:56:27.203 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
369 | 12:56:27.239 |  | ←RRC DCCH RRC Connection Release |  |  |
370 | 12:56:27.240 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
371 | 12:56:27.259 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
372 | 12:56:27.262 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:735: SRTP config: Master Key: E84045DBB79C657996458315508169AF, Master Salt: D9F1F70D86757A663B4C66B0, MKI: 263602C4
373 | 12:56:27.262 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
374 | 12:56:27.262 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
375 | 12:56:27.264 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
376 | 12:56:27.267 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
377 | 12:56:27.268 |  |  |  |  | ←XML | Media-Server
378 | 12:56:27.279 |  |  |  |  | ←SIP INVITE | P-CSCF
379 | 12:56:27.637 |  | ←enobeB PCAP frame← LTE RRC PCCH Paging (1 PagingRecord) |  |  |
380 | 12:56:27.637 |  | ←RRC PCCH Paging |  |  |
381 | 12:56:27.677 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
382 | 12:56:27.677 |  | →RRC CCCH RRC Connection Request |  |  |
383 | 12:56:27.677 |  | ←RRC CCCH RRC Connection Setup |  |  |
384 | 12:56:27.677 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
385 | 12:56:27.710 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
386 | 12:56:27.710 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
387 | 12:56:27.710 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
388 | 12:56:27.710 |  |  |  | →NAS EMM Service request |  |
389 | 12:56:27.710 |  |  |  | NAS K-enb 2337fdcd1fbefcc6665f493835f2d592b... |  |
390 | 12:56:27.711 |  |  | RRC K-enb 2337fdcd1fbefcc6665f493835f2d592b... |  |  |
391 | 12:56:27.712 |  |  | RRC rrc-cip 4fe3265397ce9ce284baf91a278af96... |  |  |
392 | 12:56:27.712 |  |  | RRC rrc-int aa0569449f43a464be1e7a75839c09a... |  |  |
393 | 12:56:27.712 |  |  | RRC up-cip cedb71c18ea3b8fadd7a0a06edce1238... |  |  |
394 | 12:56:27.712 |  |  | RRC up-int 35a597b1d894ae7e79a38c0bd1c4a607... |  |  |
395 | 12:56:27.712 |  | ←RRC DCCH Security Mode Command |  |  |
396 | 12:56:27.712 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
397 | 12:56:27.750 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
398 | 12:56:27.750 |  | →RRC DCCH Security Mode Complete |  |  |
399 | 12:56:27.750 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
400 | 12:56:27.750 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
401 | 12:56:27.790 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
402 | 12:56:27.790 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
403 | 12:56:27.792 |  | ←enobeB PCAP frame← SIP over IPSEC: INVITE sip:PublicUserId-A@192.168.3.2:38862;transp... |  |  |
404 | 12:56:27.838 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 100 Trying |  |  |  |
405 | 12:56:27.840 |  |  |  |  | →SIP 100 Trying | P-CSCF
406 | 12:56:27.878 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 183 Session Progress |  |  |  |
407 | 12:56:27.880 |  |  |  |  | →SIP 183 Session Progress | P-CSCF
408 | 12:56:27.886 |  |  |  |  | ←SIP PRACK | P-CSCF
409 | 12:56:27.887 |  | ←enobeB PCAP frame← SIP over IPSEC: PRACK sip:PublicUserId-A@192.168.3.2:38862;transpo... |  |  |
410 | 12:56:27.918 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
411 | 12:56:27.920 |  |  |  |  | →SIP 200 OK | P-CSCF
412 | 12:56:28.312 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
413 | 12:56:28.312 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xb) |  |  |
414 | 12:56:28.312 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
415 | 12:56:28.313 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
416 | 12:56:28.350 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
417 | 12:56:28.350 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
418 | 12:56:28.350 |  | →RRC DCCH UL Information Transfer |  |  |
419 | 12:56:28.350 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x3) |  |  |
420 | 12:56:28.350 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
421 | 12:56:28.444 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
422 | 12:56:28.672 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:648: Verdict: Pass
423 | 12:56:28.773 |  |  |  |  | MMICmd: Please Accept the Call
424 | 12:56:39.998 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
425 | 12:56:39.999 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
426 | 12:56:40.003 |  |  |  |  | →SIP 200 OK | P-CSCF
427 | 12:56:40.010 |  |  |  |  | XML→ | Media-Server
428 | 12:56:40.012 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:657: 200 OK Verdict: Pass
429 | 12:56:40.012 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:378: Step 1 Verdict: Pass
430 | 12:56:40.013 |  |  |  |  | ←SIP ACK | P-CSCF
431 | 12:56:40.014 |  | ←enobeB PCAP frame← SIP over IPSEC: ACK sip:PublicUserId-A@192.168.3.2:38862;transport... |  |  |
432 | 12:56:40.762 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:383: Step 7B Verdict: Pass
433 | 12:56:40.764 |  |  |  |  | ←SIP BYE | P-CSCF
434 | 12:56:40.766 |  | ←enobeB PCAP frame← SIP over IPSEC: BYE sip:PublicUserId-A@192.168.3.2:38862;transport... |  |  |
435 | 12:56:40.878 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
436 | 12:56:40.880 |  |  |  |  | →SIP 200 OK | P-CSCF
437 | 12:56:41.990 | →enobeB PCAP frame→ |  |  |  |
438 | 12:56:42.883 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
439 | 12:56:42.894 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
440 | 12:56:42.894 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x9) |  |  |
441 | 12:56:42.894 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
442 | 12:56:42.895 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
443 | 12:56:42.950 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
444 | 12:56:42.950 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
445 | 12:56:42.950 |  | →RRC DCCH UL Information Transfer |  |  |
446 | 12:56:42.950 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x4) |  |  |
447 | 12:56:42.950 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
448 | 12:56:43.007 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
449 | 12:56:43.008 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
450 | 12:56:43.052 |  | ←RRC DCCH RRC Connection Release |  |  |
451 | 12:56:43.053 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
452 | 12:56:43.072 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
453 | 12:56:43.073 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
454 | 12:56:43.075 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
455 | 12:56:43.823 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.