MSG #420 2021-09-06 12:56:28.350
NAS

     ESM: Activate dedicated EPS bearer context accept
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x2 (Integrity protected and ciphered)
    Auth code = 0x0dc8b54b
    Sequence number = 0x05
    Protocol discriminator = 0x2 (EPS Session Management)
    EPS bearer identity = 6
    Procedure transaction identity = 0
    Message type = 0xc6 (Activate dedicated EPS bearer context accept)