ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 09:01:42.489 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 09:01:42.494 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 09:01:42.494 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 09:01:42.496 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 09:01:42.497 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 09:01:42.497 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:805: IMS UDP port 192.168.2.3:5060 configured
7 | 09:01:42.500 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:755: IMS TCP port 192.168.2.3:5060 configured!
8 | 09:01:42.502 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:776: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 09:01:42.503 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:787: IdM port 192.168.2.3:8080 configured!
10 | 09:01:42.505 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 09:01:43.705 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 09:01:43.706 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 09:01:45.542 |  | ←RRC BCCH SIB |  |  |
14 | 09:01:45.547 |  | ←RRC BCCH SIB1 |  |  |
15 | 09:01:45.562 |  | ←RRC BCCH SIB |  |  |
16 | 09:01:45.582 |  | ←RRC BCCH SIB |  |  |
17 | 09:01:45.627 |  | ←RRC BCCH SIB1 |  |  |
18 | 09:02:30.071 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 09:02:30.071 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 09:02:30.071 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 09:02:30.071 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 09:02:30.122 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 09:02:30.122 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 09:02:30.122 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 09:02:30.122 |  |  |  | →NAS EMM Attach request |  |
26 | 09:02:30.122 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 09:02:30.122 |  |  |  | NAS K-asme 08e5fbec217481597a9755f596d14570... |  |
28 | 09:02:30.122 |  |  |  | NAS ← EMM Authentication request |  |
29 | 09:02:30.123 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 09:02:30.123 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 09:02:30.124 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 09:02:30.194 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 09:02:30.194 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 09:02:30.194 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 09:02:30.194 |  |  |  | →NAS EMM Authentication response |  |
36 | 09:02:30.194 |  |  |  | NAS UE auth OK |  |
37 | 09:02:30.194 |  |  |  | NAS K-nas-cip 2829e5e47cc6d56709720b3b208ea... |  |
38 | 09:02:30.194 |  |  |  | NAS K-nas-int 42e88dfe6e14e6d906211107cd54a... |  |
39 | 09:02:30.194 |  |  |  | NAS ← EMM Security mode command |  |
40 | 09:02:30.195 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 09:02:30.195 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 09:02:30.196 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 09:02:30.234 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
44 | 09:02:30.234 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 09:02:30.234 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x6) |  |  |
46 | 09:02:30.234 |  |  |  | →NAS EMM Security mode complete |  |
47 | 09:02:30.234 |  |  |  | NAS ← ESM ESM information request |  |
48 | 09:02:30.235 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x7) |  |  |
49 | 09:02:30.235 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 09:02:30.236 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
51 | 09:02:30.282 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
52 | 09:02:30.282 |  | →RRC DCCH UL Information Transfer |  |  |
53 | 09:02:30.282 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x4) |  |  |
54 | 09:02:30.282 |  |  |  | →NAS ESM ESM information response |  |
55 | 09:02:30.282 |  |  |  | NAS ← EMM Attach accept |  |
56 | 09:02:30.282 |  |  |  | NAS K-enb 1b45a69caff5362780ed5cc0e2dad9841... |  |
57 | 09:02:30.283 |  | ←RRC DCCH Security Mode Command |  |  |
58 | 09:02:30.283 |  |  | RRC K-enb 1b45a69caff5362780ed5cc0e2dad9841... |  |  |
59 | 09:02:30.283 |  |  | RRC rrc-cip 4856ec5bdbbb350944c64f02bfa8e19... |  |  |
60 | 09:02:30.283 |  |  | RRC rrc-int 4d8b29853ce90c1bf2d368f831e4060... |  |  |
61 | 09:02:30.283 |  |  | RRC up-cip 2abe9d8ebdcf7a89016186ef865b696d... |  |  |
62 | 09:02:30.283 |  |  | RRC up-int 9f159cc938d440b2c4a3303b880bf9de... |  |  |
63 | 09:02:30.284 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
64 | 09:02:30.314 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
65 | 09:02:30.314 |  | →RRC DCCH Security Mode Complete |  |  |
66 | 09:02:30.314 |  | ←RRC DCCH UE Capability Enquiry |  |  |
67 | 09:02:30.314 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
68 | 09:02:30.364 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
69 | 09:02:30.364 |  | →RRC DCCH UE Capability Information |  |  |
70 | 09:02:30.364 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x8) |  |  |
71 | 09:02:30.364 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
72 | 09:02:30.364 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
73 | 09:02:30.394 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
74 | 09:02:30.394 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
75 | 09:02:30.434 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
76 | 09:02:30.434 |  | →RRC DCCH UL Information Transfer |  |  |
77 | 09:02:30.434 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xc) |  |  |
78 | 09:02:30.434 |  |  |  | →NAS EMM Attach complete |  |
79 | 09:02:30.434 |  |  |  | NAS ← EMM EMM information |  |
80 | 09:02:30.435 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x6) |  |  |
81 | 09:02:30.435 |  | ←RRC DCCH DL Information Transfer |  |  |
82 | 09:02:30.436 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
83 | 09:02:35.807 |  | ←RRC DCCH RRC Connection Release |  |  |
84 | 09:02:35.808 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
85 | 09:02:36.821 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
86 | 09:02:36.821 |  | →RRC CCCH RRC Connection Request |  |  |
87 | 09:02:36.821 |  | ←RRC CCCH RRC Connection Setup |  |  |
88 | 09:02:36.821 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
89 | 09:02:36.874 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
90 | 09:02:36.874 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
91 | 09:02:36.874 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
92 | 09:02:36.874 |  |  |  | →NAS EMM Service request |  |
93 | 09:02:36.874 |  |  |  | NAS K-enb ebdac409232b1d1114b511fe304fb7ea2... |  |
94 | 09:02:36.875 |  |  | RRC K-enb ebdac409232b1d1114b511fe304fb7ea2... |  |  |
95 | 09:02:36.876 |  |  | RRC rrc-cip 8384b05b89e5b6b8b2583a1380793eb... |  |  |
96 | 09:02:36.876 |  |  | RRC rrc-int 57e5ad3d70c862d1adbdd2681c7202a... |  |  |
97 | 09:02:36.876 |  |  | RRC up-cip b75df1cca08d7518ab1c0baa59ddaa98... |  |  |
98 | 09:02:36.876 |  |  | RRC up-int bea0c0cec5c9944afe886af6a76ddc52... |  |  |
99 | 09:02:36.876 |  | ←RRC DCCH Security Mode Command |  |  |
100 | 09:02:36.876 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
101 | 09:02:36.914 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
102 | 09:02:36.914 |  | →RRC DCCH Security Mode Complete |  |  |
103 | 09:02:36.914 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
104 | 09:02:36.914 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
105 | 09:02:36.954 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
106 | 09:02:36.954 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
107 | 09:02:53.754 | →enobeB PCAP frame→ TCP |  |  |  |
108 | 09:02:53.757 |  | ←enobeB PCAP frame← TCP |  |  |
109 | 09:02:53.794 | →enobeB PCAP frame→ TCP |  |  |  |
110 | 09:02:53.882 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
111 | 09:02:53.885 |  | ←enobeB PCAP frame← TCP |  |  |
112 | 09:02:53.891 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
113 | 09:02:53.914 | →enobeB PCAP frame→ TCP |  |  |  |
114 | 09:02:54.035 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 16)
115 | 09:02:54.042 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
116 | 09:02:54.045 |  | ←enobeB PCAP frame← TCP |  |  |
117 | 09:02:54.046 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
118 | 09:02:54.074 | →enobeB PCAP frame→ TCP |  |  |  |
119 | 09:02:54.115 |  |  |  |  | →HTTP GET | HTTP-Proxy
120 | 09:02:54.122 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
121 | 09:02:54.122 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:288: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
122 | 09:02:54.125 |  | ←enobeB PCAP frame← TCP |  |  |
123 | 09:02:54.142 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
124 | 09:02:54.155 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
125 | 09:02:54.194 | →enobeB PCAP frame→ TCP |  |  |  |
126 | 09:02:55.794 | →enobeB PCAP frame→ TCP |  |  |  |
127 | 09:02:55.797 |  | ←enobeB PCAP frame← TCP |  |  |
128 | 09:02:55.834 | →enobeB PCAP frame→ TCP |  |  |  |
129 | 09:02:55.842 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
130 | 09:02:55.845 |  | ←enobeB PCAP frame← TCP |  |  |
131 | 09:02:55.851 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
132 | 09:02:55.874 | →enobeB PCAP frame→ TCP |  |  |  |
133 | 09:02:56.115 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:642: Client connected to IdM port (id 18)
134 | 09:02:56.122 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
135 | 09:02:56.125 |  | ←enobeB PCAP frame← TCP |  |  |
136 | 09:02:56.126 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
137 | 09:02:56.154 | →enobeB PCAP frame→ TCP |  |  |  |
138 | 09:02:56.156 |  |  |  |  | →HTTP GET | IDMS-Endpoint
139 | 09:02:56.162 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
140 | 09:02:56.165 |  | ←enobeB PCAP frame← TCP |  |  |
141 | 09:02:56.201 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
142 | 09:02:56.204 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:511: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
143 | 09:02:56.204 |  |  |  |  | MMICmd: Please provide user credentials: username and password
144 | 09:02:56.212 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
145 | 09:02:56.274 | →enobeB PCAP frame→ TCP |  |  |  |
146 | 09:03:00.637 |  |  |  |  | →HTTP POST | IDMS-Endpoint
147 | 09:03:00.642 | →enobeB PCAP frame→ HTTPS: POST /idms/userauth HTTP/1.1 |  |  |  |
148 | 09:03:00.645 |  | ←enobeB PCAP frame← TCP |  |  |
149 | 09:03:00.651 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
150 | 09:03:00.653 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:516: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
151 | 09:03:00.662 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
152 | 09:03:00.714 | →enobeB PCAP frame→ TCP |  |  |  |
153 | 09:03:00.714 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:677: IdM port - Client closed the connection (id 18)
154 | 09:03:00.722 | →enobeB PCAP frame→ TCP |  |  |  |
155 | 09:03:00.725 |  | ←enobeB PCAP frame← TCP |  |  |
156 | 09:03:00.754 | →enobeB PCAP frame→ TCP |  |  |  |
157 | 09:03:01.514 | →enobeB PCAP frame→ TCP |  |  |  |
158 | 09:03:01.517 |  | ←enobeB PCAP frame← TCP |  |  |
159 | 09:03:01.554 | →enobeB PCAP frame→ TCP |  |  |  |
160 | 09:03:01.602 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
161 | 09:03:01.712 |  | ←enobeB PCAP frame← TCP |  |  |
162 | 09:03:01.715 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
163 | 09:03:01.754 | →enobeB PCAP frame→ TCP |  |  |  |
164 | 09:03:01.802 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
165 | 09:03:01.854 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:642: Client connected to IdM port (id 18)
166 | 09:03:01.864 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
167 | 09:03:01.922 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
168 | 09:03:02.013 |  |  |  |  | →HTTP POST | IDMS-Endpoint
169 | 09:03:02.023 |  | ←enobeB PCAP frame← TCP |  |  |
170 | 09:03:02.026 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
171 | 09:03:02.030 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:521: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
172 | 09:03:02.038 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
173 | 09:03:02.114 | →enobeB PCAP frame→ TCP |  |  |  |
174 | 09:03:02.394 | →enobeB PCAP frame→ TCP |  |  |  |
175 | 09:03:02.397 |  | ←enobeB PCAP frame← TCP |  |  |
176 | 09:03:02.434 | →enobeB PCAP frame→ TCP |  |  |  |
177 | 09:03:02.442 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
178 | 09:03:02.445 |  | ←enobeB PCAP frame← TCP |  |  |
179 | 09:03:02.449 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
180 | 09:03:02.474 | →enobeB PCAP frame→ TCP |  |  |  |
181 | 09:03:02.515 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 19)
182 | 09:03:02.522 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
183 | 09:03:02.525 |  | ←enobeB PCAP frame← TCP |  |  |
184 | 09:03:02.526 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
185 | 09:03:02.556 |  |  |  |  | →HTTP POST | HTTP-Proxy
186 | 09:03:02.562 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
187 | 09:03:02.565 |  | ←enobeB PCAP frame← TCP |  |  |
188 | 09:03:02.638 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:541: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
189 | 09:03:02.648 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
190 | 09:03:02.660 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
191 | 09:03:02.714 | →enobeB PCAP frame→ TCP |  |  |  |
192 | 09:03:02.722 | →enobeB PCAP frame→ TCP |  |  |  |
193 | 09:03:02.725 |  | ←enobeB PCAP frame← TCP |  |  |
194 | 09:03:02.754 | →enobeB PCAP frame→ TCP |  |  |  |
195 | 09:03:02.762 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
196 | 09:03:02.765 |  | ←enobeB PCAP frame← TCP |  |  |
197 | 09:03:02.769 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
198 | 09:03:02.794 | →enobeB PCAP frame→ TCP |  |  |  |
199 | 09:03:02.795 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 20)
200 | 09:03:02.802 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
201 | 09:03:02.805 |  | ←enobeB PCAP frame← TCP |  |  |
202 | 09:03:02.806 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
203 | 09:03:02.837 |  |  |  |  | →HTTP POST | HTTP-Proxy
204 | 09:03:02.842 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
205 | 09:03:02.846 |  | ←enobeB PCAP frame← TCP |  |  |
206 | 09:03:02.919 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:545: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
207 | 09:03:02.920 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
208 | 09:03:02.932 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
209 | 09:03:02.954 | →enobeB PCAP frame→ TCP |  |  |  |
210 | 09:03:02.997 |  |  |  |  | →SIP REGISTER | P-CSCF
211 | 09:03:03.002 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
212 | 09:03:03.019 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:814: IMS UDP_s port 192.168.2.3:5062 configured
213 | 09:03:03.047 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:765: IMS TCP_s port 192.168.2.3:5062 configured!
214 | 09:03:03.049 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:823: IMS UDP_c port 192.168.2.3:5061 configured
215 | 09:03:03.057 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
216 | 09:03:03.758 |  |  |  |  | →SIP REGISTER | P-CSCF
217 | 09:03:03.762 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
218 | 09:03:03.775 |  |  |  |  | ←SIP 200 OK | P-CSCF
219 | 09:03:03.786 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
220 | 09:03:04.119 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
221 | 09:03:04.122 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
222 | 09:03:04.123 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
223 | 09:03:04.124 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 SIP over IPSEC: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 |  |  |  |
224 | 09:03:04.132 |  |  |  |  | ←SIP 200 OK | P-CSCF
225 | 09:03:04.132 |  |  |  |  | MIKEY | Media-Server
226 | 09:03:04.143 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
227 | 09:03:04.365 |  |  |  |  | XML→ | Media-Server
228 | 09:03:04.367 |  |  |  |  | XML→ | Media-Server
229 | 09:03:04.370 |  |  |  |  | ←XML | Media-Server
230 | 09:03:04.373 |  |  |  |  | ←SIP NOTIFY | P-CSCF
231 | 09:03:04.384 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:40605;transp... |  |  |
232 | 09:03:04.435 |  |  |  |  | →SIP 200 OK | P-CSCF
233 | 09:03:04.442 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
234 | 09:03:04.634 | →enobeB PCAP frame→ TCP |  |  |  |
235 | 09:03:04.637 |  | ←enobeB PCAP frame← TCP |  |  |
236 | 09:03:04.674 | →enobeB PCAP frame→ TCP |  |  |  |
237 | 09:03:04.682 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
238 | 09:03:04.685 |  | ←enobeB PCAP frame← TCP |  |  |
239 | 09:03:04.689 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
240 | 09:03:04.714 | →enobeB PCAP frame→ TCP |  |  |  |
241 | 09:03:04.795 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
242 | 09:03:04.802 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
243 | 09:03:04.805 |  | ←enobeB PCAP frame← TCP |  |  |
244 | 09:03:04.806 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
245 | 09:03:04.834 | →enobeB PCAP frame→ TCP |  |  |  |
246 | 09:03:04.875 |  |  |  |  | →HTTP GET | HTTP-Proxy
247 | 09:03:04.882 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-co... |  |  |  |
248 | 09:03:04.885 |  | ←enobeB PCAP frame← TCP |  |  |
249 | 09:03:04.885 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:642: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcptt-ue-configuration.xml
250 | 09:03:04.892 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
251 | 09:03:04.904 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
252 | 09:03:04.987 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
253 | 09:03:04.994 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
254 | 09:03:04.997 |  | ←enobeB PCAP frame← TCP |  |  |
255 | 09:03:05.002 | →enobeB PCAP frame→ TCP |  |  |  |
256 | 09:03:05.006 |  | ←enobeB PCAP frame← TCP |  |  |
257 | 09:03:05.034 | →enobeB PCAP frame→ TCP |  |  |  |
258 | 09:03:05.114 | →enobeB PCAP frame→ TCP |  |  |  |
259 | 09:03:05.117 |  | ←enobeB PCAP frame← TCP |  |  |
260 | 09:03:05.154 | →enobeB PCAP frame→ TCP |  |  |  |
261 | 09:03:05.162 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
262 | 09:03:05.165 |  | ←enobeB PCAP frame← TCP |  |  |
263 | 09:03:05.168 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
264 | 09:03:05.194 | →enobeB PCAP frame→ TCP |  |  |  |
265 | 09:03:05.235 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
266 | 09:03:05.242 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
267 | 09:03:05.245 |  | ←enobeB PCAP frame← TCP |  |  |
268 | 09:03:05.246 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
269 | 09:03:05.315 |  |  |  |  | →HTTP GET | HTTP-Proxy
270 | 09:03:05.322 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-... |  |  |  |
271 | 09:03:05.325 |  | ←enobeB PCAP frame← TCP |  |  |
272 | 09:03:05.328 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:647: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcptt-user-profile-49.xml
273 | 09:03:05.367 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
274 | 09:03:05.384 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
275 | 09:03:05.385 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
276 | 09:03:05.434 | →enobeB PCAP frame→ TCP |  |  |  |
277 | 09:03:05.435 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
278 | 09:03:05.442 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
279 | 09:03:05.445 |  | ←enobeB PCAP frame← TCP |  |  |
280 | 09:03:05.474 | →enobeB PCAP frame→ TCP |  |  |  |
281 | 09:03:06.122 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
282 | 09:03:06.122 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
283 | 09:03:06.123 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
284 | 09:03:06.136 |  |  |  |  | ←SIP 200 OK | P-CSCF
285 | 09:03:06.136 |  |  |  |  | MIKEY | Media-Server
286 | 09:03:06.147 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
287 | 09:03:06.274 | →enobeB PCAP frame→ TCP |  |  |  |
288 | 09:03:06.277 |  | ←enobeB PCAP frame← TCP |  |  |
289 | 09:03:06.314 | →enobeB PCAP frame→ TCP |  |  |  |
290 | 09:03:06.322 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
291 | 09:03:06.325 |  | ←enobeB PCAP frame← TCP |  |  |
292 | 09:03:06.326 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
293 | 09:03:06.344 |  |  |  |  | XML→ | Media-Server
294 | 09:03:06.345 |  |  |  |  | XML→ | Media-Server
295 | 09:03:06.348 |  |  |  |  | ←XML | Media-Server
296 | 09:03:06.354 | →enobeB PCAP frame→ TCP |  |  |  |
297 | 09:03:06.395 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
298 | 09:03:06.397 |  |  |  |  | ←SIP NOTIFY | P-CSCF
299 | 09:03:06.402 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
300 | 09:03:06.405 |  | ←enobeB PCAP frame← TCP |  |  |
301 | 09:03:06.406 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
302 | 09:03:06.409 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:40605;transp... |  |  |
303 | 09:03:06.434 | →enobeB PCAP frame→ TCP |  |  |  |
304 | 09:03:06.434 |  |  |  |  | →HTTP GET | HTTP-Proxy
305 | 09:03:06.435 |  |  |  |  | →SIP 200 OK | P-CSCF
306 | 09:03:06.437 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:652: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
307 | 09:03:06.442 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.servi... |  |  |  |
308 | 09:03:06.445 |  | ←enobeB PCAP frame← TCP |  |  |
309 | 09:03:06.446 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
310 | 09:03:06.458 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
311 | 09:03:06.474 | →enobeB PCAP frame→ TCP |  |  |  |
312 | 09:03:06.482 | →enobeB PCAP frame→ TCP |  |  |  |
313 | 09:03:06.506 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
314 | 09:03:06.514 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
315 | 09:03:06.517 |  | ←enobeB PCAP frame← TCP |  |  |
316 | 09:03:06.554 | →enobeB PCAP frame→ TCP |  |  |  |
317 | 09:03:06.594 | →enobeB PCAP frame→ TCP |  |  |  |
318 | 09:03:06.597 |  | ←enobeB PCAP frame← TCP |  |  |
319 | 09:03:06.634 | →enobeB PCAP frame→ TCP |  |  |  |
320 | 09:03:06.642 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
321 | 09:03:06.645 |  | ←enobeB PCAP frame← TCP |  |  |
322 | 09:03:06.648 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
323 | 09:03:06.674 | →enobeB PCAP frame→ TCP |  |  |  |
324 | 09:03:06.795 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
325 | 09:03:06.802 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
326 | 09:03:06.805 |  | ←enobeB PCAP frame← TCP |  |  |
327 | 09:03:06.806 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
328 | 09:03:06.834 | →enobeB PCAP frame→ TCP |  |  |  |
329 | 09:03:06.835 |  |  |  |  | →HTTP GET | HTTP-Proxy
330 | 09:03:06.842 | →enobeB PCAP frame→ HTTPS: GET /xcap.gms.mcstaasting.com/org.openmobileallian... |  |  |  |
331 | 09:03:06.845 |  | ←enobeB PCAP frame← TCP |  |  |
332 | 09:03:06.846 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:657: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at /xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
333 | 09:03:06.863 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
334 | 09:03:06.875 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
335 | 09:03:06.914 | →enobeB PCAP frame→ TCP |  |  |  |
336 | 09:03:06.914 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
337 | 09:03:06.922 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
338 | 09:03:06.925 |  | ←enobeB PCAP frame← TCP |  |  |
339 | 09:03:06.930 | →enobeB PCAP frame→ TCP |  |  |  |
340 | 09:03:06.934 |  | ←enobeB PCAP frame← TCP |  |  |
341 | 09:03:06.954 | →enobeB PCAP frame→ TCP |  |  |  |
342 | 09:03:07.082 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
343 | 09:03:07.083 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
344 | 09:03:07.087 |  |  |  |  | →SIP PUBLISH | P-CSCF
345 | 09:03:07.134 |  |  |  |  | MIKEY | Media-Server
346 | 09:03:07.159 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
347 | 09:03:07.162 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
348 | 09:03:07.163 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
349 | 09:03:07.356 |  |  |  |  | XML→ | Media-Server
350 | 09:03:07.359 |  |  |  |  | ←SIP 200 OK | P-CSCF
351 | 09:03:07.362 |  |  |  |  | ←SIP 200 OK | P-CSCF
352 | 09:03:07.362 |  |  |  |  | MIKEY | Media-Server
353 | 09:03:07.370 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
354 | 09:03:07.374 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
355 | 09:03:07.566 |  |  |  |  | XML→ | Media-Server
356 | 09:03:07.567 |  |  |  |  | XML→ | Media-Server
357 | 09:03:07.601 |  |  |  |  | ←XML | Media-Server
358 | 09:03:07.670 |  |  |  |  | ←SIP NOTIFY | P-CSCF
359 | 09:03:07.682 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:40605;transp... |  |  |
360 | 09:03:07.715 |  |  |  |  | →SIP 200 OK | P-CSCF
361 | 09:03:07.722 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
362 | 09:03:07.724 |  |  |  |  | ←XML | Media-Server
363 | 09:03:07.751 |  |  |  |  | ←SIP MESSAGE | P-CSCF
364 | 09:03:07.762 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
365 | 09:03:08.554 |  |  |  |  | →SIP 200 OK | P-CSCF
366 | 09:03:08.557 |  |  |  |  | Info: MCX_IMS_CommonProcedures.ttcn:155: MESSAGE/200OK Table 5.3.2.3-2 Steps 7-8 Done
367 | 09:03:08.562 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
368 | 09:03:08.568 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
369 | 09:03:08.594 | →enobeB PCAP frame→ TCP |  |  |  |
370 | 09:03:08.634 | →enobeB PCAP frame→ TCP |  |  |  |
371 | 09:03:10.558 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
372 | 09:03:10.603 |  | ←RRC DCCH RRC Connection Release |  |  |
373 | 09:03:10.604 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
374 | 09:03:10.613 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
375 | 09:03:10.615 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
376 | 09:03:10.615 |  |  |  |  | MMICmd: Make the MCPTT User requesting the establishment of an MCPTT On-demand pre-arranged imminent peril group call for the selected MCPTT imminent peril group GROUP A, with implicit floor control
377 | 09:03:15.191 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
378 | 09:03:15.191 |  | →RRC CCCH RRC Connection Request |  |  |
379 | 09:03:15.191 |  | ←RRC CCCH RRC Connection Setup |  |  |
380 | 09:03:15.191 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
381 | 09:03:15.234 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
382 | 09:03:15.234 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
383 | 09:03:15.234 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
384 | 09:03:15.234 |  |  |  | →NAS EMM Service request |  |
385 | 09:03:15.234 |  |  |  | NAS K-enb a23e1a4543cb65d9a1df467c82e861cbc... |  |
386 | 09:03:15.235 |  | ←RRC DCCH Security Mode Command |  |  |
387 | 09:03:15.235 |  |  | RRC K-enb a23e1a4543cb65d9a1df467c82e861cbc... |  |  |
388 | 09:03:15.235 |  |  | RRC rrc-cip 2648bfb42b6f4a4ed012fc6bd806898... |  |  |
389 | 09:03:15.235 |  |  | RRC rrc-int 94183dd18a37f2fa9154c39c5295a11... |  |  |
390 | 09:03:15.235 |  |  | RRC up-cip e4caafa49aff0d4834c0f0f9d4d4ddd3... |  |  |
391 | 09:03:15.235 |  |  | RRC up-int 88e82b7c1cfc2fce503dd2cb8f5f57e3... |  |  |
392 | 09:03:15.236 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
393 | 09:03:15.274 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
394 | 09:03:15.274 |  | →RRC DCCH Security Mode Complete |  |  |
395 | 09:03:15.274 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
396 | 09:03:15.274 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
397 | 09:03:15.314 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
398 | 09:03:15.314 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
399 | 09:03:15.317 |  |  |  |  | →SIP INVITE | P-CSCF
400 | 09:03:15.322 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
401 | 09:03:15.323 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
402 | 09:03:15.331 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:735: SRTP config: Master Key: D55113EBD106763E3DC69B913D55BF1B, Master Salt: 7B01A9AB2BB4B868FCFBF666, MKI: 252E16AC
403 | 09:03:15.331 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
404 | 09:03:15.336 |  |  |  |  | XML→ | Media-Server
405 | 09:03:15.337 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
406 | 09:03:15.338 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1205: INVITE Verdict: Pass
407 | 09:03:15.339 |  |  |  |  | ←SIP 100 Trying | P-CSCF
408 | 09:03:15.342 |  |  |  |  | ←SIP 200 OK | P-CSCF
409 | 09:03:15.351 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
410 | 09:03:15.354 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
411 | 09:03:15.983 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
412 | 09:03:15.984 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x5) |  |  |
413 | 09:03:15.984 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
414 | 09:03:15.985 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
415 | 09:03:16.034 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
416 | 09:03:16.034 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
417 | 09:03:16.034 |  | →RRC DCCH UL Information Transfer |  |  |
418 | 09:03:16.034 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x9) |  |  |
419 | 09:03:16.034 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
420 | 09:03:16.103 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
421 | 09:03:16.156 |  |  |  |  | →SIP ACK | P-CSCF
422 | 09:03:16.162 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
423 | 09:03:16.165 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1208: ACK Verdict: Pass
424 | 09:03:16.165 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:483: Step 2 Verdict: Pass
425 | 09:03:16.714 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
426 | 09:03:16.722 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
427 | 09:03:16.754 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
428 | 09:03:16.762 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
429 | 09:03:16.794 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
430 | 09:03:16.915 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:488: Step 5A Verdict: Pass
431 | 09:03:16.924 |  |  |  |  | ←SIP BYE | P-CSCF
432 | 09:03:16.935 |  | ←enobeB PCAP frame← SIP over IPSEC: BYE sip:PublicUserId-A@192.168.3.2:40605;transport... |  |  |
433 | 09:03:16.938 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
434 | 09:03:16.955 |  |  |  |  | →SIP 200 OK | P-CSCF
435 | 09:03:16.962 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK SRTP frame: |  |  |  |
436 | 09:03:16.994 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
437 | 09:03:17.234 | →enobeB PCAP frame→ |  |  |  |
438 | 09:03:18.964 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
439 | 09:03:18.993 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
440 | 09:03:18.993 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x4) |  |  |
441 | 09:03:18.993 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
442 | 09:03:18.994 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
443 | 09:03:19.034 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
444 | 09:03:19.034 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
445 | 09:03:19.034 |  | →RRC DCCH UL Information Transfer |  |  |
446 | 09:03:19.034 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x4) |  |  |
447 | 09:03:19.034 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
448 | 09:03:19.099 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
449 | 09:03:19.101 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
450 | 09:03:19.154 |  | ←RRC DCCH RRC Connection Release |  |  |
451 | 09:03:19.155 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
452 | 09:03:19.155 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
453 | 09:03:19.158 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
454 | 09:03:19.160 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
455 | 09:03:19.907 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.