ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 13:02:48.012 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 13:02:48.014 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 13:02:48.014 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 13:02:48.016 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 13:02:48.017 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 13:02:48.017 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:805: IMS UDP port 192.168.2.3:5060 configured
7 | 13:02:48.019 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:755: IMS TCP port 192.168.2.3:5060 configured!
8 | 13:02:48.021 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:776: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 13:02:48.022 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:787: IdM port 192.168.2.3:8080 configured!
10 | 13:02:48.023 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 13:02:49.225 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 13:02:49.227 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 13:02:50.779 |  | ←RRC BCCH SIB |  |  |
14 | 13:02:50.783 |  | ←RRC BCCH SIB1 |  |  |
15 | 13:02:50.799 |  | ←RRC BCCH SIB |  |  |
16 | 13:02:50.818 |  | ←RRC BCCH SIB |  |  |
17 | 13:02:50.863 |  | ←RRC BCCH SIB1 |  |  |
18 | 13:04:22.138 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 13:04:22.138 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 13:04:22.138 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 13:04:22.138 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 13:04:22.199 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 13:04:22.199 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 13:04:22.199 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 13:04:22.199 |  |  |  | →NAS EMM Attach request |  |
26 | 13:04:22.199 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 13:04:22.199 |  |  |  | NAS K-asme 2ba8c47a69ba623b67cdfcfca2a9b687... |  |
28 | 13:04:22.199 |  |  |  | NAS ← EMM Authentication request |  |
29 | 13:04:22.200 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 13:04:22.200 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 13:04:22.201 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 13:04:22.271 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 13:04:22.271 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 13:04:22.271 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 13:04:22.271 |  |  |  | →NAS EMM Authentication response |  |
36 | 13:04:22.271 |  |  |  | NAS UE auth OK |  |
37 | 13:04:22.271 |  |  |  | NAS K-nas-cip 1d391b87de49cd0407e764fc43a39... |  |
38 | 13:04:22.271 |  |  |  | NAS K-nas-int cce6c1a999e7be045c57942dda93b... |  |
39 | 13:04:22.271 |  |  |  | NAS ← EMM Security mode command |  |
40 | 13:04:22.272 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 13:04:22.272 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 13:04:22.273 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 13:04:22.281 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
44 | 13:04:22.311 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer |  |  |  |
45 | 13:04:22.311 |  | →RRC DCCH UL Information Transfer |  |  |
46 | 13:04:22.311 |  | [EMBEDDED NAS IN PREV RRC] ESM Unknown message (type=0x64) |  |  |
47 | 13:04:22.311 |  |  |  | →NAS EMM Security mode complete |  |
48 | 13:04:22.311 |  |  |  | NAS ← ESM ESM information request |  |
49 | 13:04:22.312 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xd) |  |  |
50 | 13:04:22.312 |  | ←RRC DCCH DL Information Transfer |  |  |
51 | 13:04:22.313 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
52 | 13:04:22.359 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
53 | 13:04:22.359 |  | →RRC DCCH UL Information Transfer |  |  |
54 | 13:04:22.359 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xa) |  |  |
55 | 13:04:22.359 |  |  |  | →NAS ESM ESM information response |  |
56 | 13:04:22.359 |  |  |  | NAS ← EMM Attach accept |  |
57 | 13:04:22.359 |  |  |  | NAS K-enb 78e962f85e4a8cc6e601dbf7c0a6f9995... |  |
58 | 13:04:22.360 |  | ←RRC DCCH Security Mode Command |  |  |
59 | 13:04:22.360 |  |  | RRC K-enb 78e962f85e4a8cc6e601dbf7c0a6f9995... |  |  |
60 | 13:04:22.360 |  |  | RRC rrc-cip fe937e507a3ee575a518a13d9f18485... |  |  |
61 | 13:04:22.360 |  |  | RRC rrc-int be25905755bc8100757ece8b3bcb281... |  |  |
62 | 13:04:22.360 |  |  | RRC up-cip e734521d3f52c78155c1c47faf34c2fc... |  |  |
63 | 13:04:22.360 |  |  | RRC up-int 135d7cb647523a3811226dad81bed2de... |  |  |
64 | 13:04:22.361 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
65 | 13:04:22.369 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
66 | 13:04:22.391 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
67 | 13:04:22.391 |  | →RRC DCCH Security Mode Complete |  |  |
68 | 13:04:22.391 |  | ←RRC DCCH UE Capability Enquiry |  |  |
69 | 13:04:22.391 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
70 | 13:04:22.441 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
71 | 13:04:22.441 |  | →RRC DCCH UE Capability Information |  |  |
72 | 13:04:22.441 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xa) |  |  |
73 | 13:04:22.441 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
74 | 13:04:22.441 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
75 | 13:04:22.471 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
76 | 13:04:22.471 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
77 | 13:04:22.511 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
78 | 13:04:22.511 |  | →RRC DCCH UL Information Transfer |  |  |
79 | 13:04:22.511 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x1) |  |  |
80 | 13:04:22.511 |  |  |  | →NAS EMM Attach complete |  |
81 | 13:04:22.511 |  |  |  | NAS ← EMM EMM information |  |
82 | 13:04:22.512 |  | [EMBEDDED NAS IN NEXT RRC] ESM Unknown message (type=0x8f) |  |  |
83 | 13:04:22.512 |  | ←RRC DCCH DL Information Transfer |  |  |
84 | 13:04:22.513 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer |  |  |
85 | 13:04:26.520 |  | ←RRC DCCH RRC Connection Release |  |  |
86 | 13:04:26.520 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
87 | 13:04:29.388 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
88 | 13:04:29.388 |  | →RRC CCCH RRC Connection Request |  |  |
89 | 13:04:29.388 |  | ←RRC CCCH RRC Connection Setup |  |  |
90 | 13:04:29.388 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
91 | 13:04:29.431 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
92 | 13:04:29.431 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
93 | 13:04:29.431 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
94 | 13:04:29.431 |  |  |  | →NAS EMM Service request |  |
95 | 13:04:29.431 |  |  |  | NAS K-enb cffe3b1f50f8e7acdc23b918de24b7283... |  |
96 | 13:04:29.432 |  | ←RRC DCCH Security Mode Command |  |  |
97 | 13:04:29.432 |  |  | RRC K-enb cffe3b1f50f8e7acdc23b918de24b7283... |  |  |
98 | 13:04:29.432 |  |  | RRC rrc-cip fa27cd53bb2bc0fa24843b8be2f69f8... |  |  |
99 | 13:04:29.432 |  |  | RRC rrc-int 31d7ec703c9548b0ca6fe2c657d5c50... |  |  |
100 | 13:04:29.432 |  |  | RRC up-cip 7e65242c60ddd4202d58c83ef968b9ab... |  |  |
101 | 13:04:29.432 |  |  | RRC up-int f79bc4347a8f5eb1c1ad9ef942b8e396... |  |  |
102 | 13:04:29.433 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
103 | 13:04:29.471 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
104 | 13:04:29.471 |  | →RRC DCCH Security Mode Complete |  |  |
105 | 13:04:29.471 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
106 | 13:04:29.471 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
107 | 13:04:29.511 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
108 | 13:04:29.511 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
109 | 13:04:43.442 |  | ←enobeB PCAP frame← TCP |  |  |
110 | 13:04:43.562 |  | ←enobeB PCAP frame← TCP |  |  |
111 | 13:04:43.567 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
112 | 13:04:43.591 | →enobeB PCAP frame→ TCP |  |  |  |
113 | 13:04:43.719 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
114 | 13:04:43.722 |  | ←enobeB PCAP frame← TCP |  |  |
115 | 13:04:43.722 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
116 | 13:04:43.722 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 16)
117 | 13:04:43.751 | →enobeB PCAP frame→ TCP |  |  |  |
118 | 13:04:43.759 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
119 | 13:04:43.761 |  |  |  |  | →HTTP GET | HTTP-Proxy
120 | 13:04:43.762 |  | ←enobeB PCAP frame← TCP |  |  |
121 | 13:04:43.768 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:288: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
122 | 13:04:43.786 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
123 | 13:04:43.790 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
124 | 13:04:43.831 | →enobeB PCAP frame→ TCP |  |  |  |
125 | 13:04:45.711 | →enobeB PCAP frame→ TCP |  |  |  |
126 | 13:04:45.714 |  | ←enobeB PCAP frame← TCP |  |  |
127 | 13:04:45.751 | →enobeB PCAP frame→ TCP |  |  |  |
128 | 13:04:45.759 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
129 | 13:04:45.762 |  | ←enobeB PCAP frame← TCP |  |  |
130 | 13:04:45.767 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
131 | 13:04:45.791 | →enobeB PCAP frame→ TCP |  |  |  |
132 | 13:04:46.039 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
133 | 13:04:46.041 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:642: Client connected to IdM port (id 18)
134 | 13:04:46.042 |  | ←enobeB PCAP frame← TCP |  |  |
135 | 13:04:46.043 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
136 | 13:04:46.071 | →enobeB PCAP frame→ TCP |  |  |  |
137 | 13:04:46.119 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
138 | 13:04:46.121 |  |  |  |  | →HTTP GET | IDMS-Endpoint
139 | 13:04:46.122 |  | ←enobeB PCAP frame← TCP |  |  |
140 | 13:04:46.132 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
141 | 13:04:46.134 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
142 | 13:04:46.136 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:511: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
143 | 13:04:46.136 |  |  |  |  | MMICmd: Please provide user credentials: username and password
144 | 13:04:46.191 | →enobeB PCAP frame→ TCP |  |  |  |
145 | 13:04:51.519 | →enobeB PCAP frame→ HTTPS: POST /idms/userauth HTTP/1.1 |  |  |  |
146 | 13:04:51.523 |  | ←enobeB PCAP frame← TCP |  |  |
147 | 13:04:51.523 |  |  |  |  | →HTTP POST | IDMS-Endpoint
148 | 13:04:51.539 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
149 | 13:04:51.541 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
150 | 13:04:51.541 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:516: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
151 | 13:04:51.591 | →enobeB PCAP frame→ TCP |  |  |  |
152 | 13:04:51.599 | →enobeB PCAP frame→ TCP |  |  |  |
153 | 13:04:51.600 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:677: IdM port - Client closed the connection (id 18)
154 | 13:04:51.602 |  | ←enobeB PCAP frame← TCP |  |  |
155 | 13:04:51.631 | →enobeB PCAP frame→ TCP |  |  |  |
156 | 13:04:52.351 | →enobeB PCAP frame→ TCP |  |  |  |
157 | 13:04:52.354 |  | ←enobeB PCAP frame← TCP |  |  |
158 | 13:04:52.391 | →enobeB PCAP frame→ TCP |  |  |  |
159 | 13:04:52.451 |  | ←enobeB PCAP frame← TCP |  |  |
160 | 13:04:52.453 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
161 | 13:04:52.559 | →enobeB PCAP frame→ TCP |  |  |  |
162 | 13:04:52.561 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:642: Client connected to IdM port (id 18)
163 | 13:04:52.562 |  | ←enobeB PCAP frame← TCP |  |  |
164 | 13:04:52.563 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
165 | 13:04:52.591 | →enobeB PCAP frame→ TCP |  |  |  |
166 | 13:04:52.599 | →enobeB PCAP frame→ TCP |  |  |  |
167 | 13:04:52.602 |  | ←enobeB PCAP frame← TCP |  |  |
168 | 13:04:52.602 |  |  |  |  | →HTTP POST | IDMS-Endpoint
169 | 13:04:52.645 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
170 | 13:04:52.645 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:521: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
171 | 13:04:52.648 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
172 | 13:04:52.711 | →enobeB PCAP frame→ TCP |  |  |  |
173 | 13:04:52.991 | →enobeB PCAP frame→ TCP |  |  |  |
174 | 13:04:52.997 |  | ←enobeB PCAP frame← TCP |  |  |
175 | 13:04:53.031 | →enobeB PCAP frame→ TCP |  |  |  |
176 | 13:04:53.039 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
177 | 13:04:53.045 |  | ←enobeB PCAP frame← TCP |  |  |
178 | 13:04:53.047 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
179 | 13:04:53.071 | →enobeB PCAP frame→ TCP |  |  |  |
180 | 13:04:53.079 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
181 | 13:04:53.084 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 19)
182 | 13:04:53.089 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
183 | 13:04:53.119 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
184 | 13:04:53.122 |  | ←enobeB PCAP frame← TCP |  |  |
185 | 13:04:53.122 |  |  |  |  | →HTTP POST | HTTP-Proxy
186 | 13:04:53.146 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:541: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
187 | 13:04:53.153 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
188 | 13:04:53.156 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
189 | 13:04:53.191 | →enobeB PCAP frame→ TCP |  |  |  |
190 | 13:04:53.199 | →enobeB PCAP frame→ TCP |  |  |  |
191 | 13:04:53.202 |  | ←enobeB PCAP frame← TCP |  |  |
192 | 13:04:53.231 | →enobeB PCAP frame→ TCP |  |  |  |
193 | 13:04:53.239 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
194 | 13:04:53.242 |  | ←enobeB PCAP frame← TCP |  |  |
195 | 13:04:53.243 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
196 | 13:04:53.271 | →enobeB PCAP frame→ TCP |  |  |  |
197 | 13:04:53.279 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
198 | 13:04:53.281 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 20)
199 | 13:04:53.282 |  | ←enobeB PCAP frame← TCP |  |  |
200 | 13:04:53.283 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
201 | 13:04:53.319 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
202 | 13:04:53.322 |  | ←enobeB PCAP frame← TCP |  |  |
203 | 13:04:53.322 |  |  |  |  | →HTTP POST | HTTP-Proxy
204 | 13:04:53.378 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
205 | 13:04:53.378 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:545: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
206 | 13:04:53.381 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
207 | 13:04:53.450 |  |  |  |  | →SIP REGISTER | P-CSCF
208 | 13:04:53.470 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:814: IMS UDP_s port 192.168.2.3:5062 configured
209 | 13:04:53.498 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:765: IMS TCP_s port 192.168.2.3:5062 configured!
210 | 13:04:53.501 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:823: IMS UDP_c port 192.168.2.3:5061 configured
211 | 13:04:53.507 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
212 | 13:04:54.279 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
213 | 13:04:54.281 |  |  |  |  | →SIP REGISTER | P-CSCF
214 | 13:04:54.286 |  |  |  |  | ←SIP 200 OK | P-CSCF
215 | 13:04:54.288 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
216 | 13:04:54.639 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
217 | 13:04:54.640 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
218 | 13:04:54.641 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 SIP over IPSEC: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 |  |  |  |
219 | 13:04:54.654 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
220 | 13:04:54.712 |  |  |  |  | ←SIP 200 OK | P-CSCF
221 | 13:04:54.712 |  |  |  |  | MIKEY | Media-Server
222 | 13:04:54.714 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
223 | 13:04:54.937 |  |  |  |  | XML→ | Media-Server
224 | 13:04:54.939 |  |  |  |  | XML→ | Media-Server
225 | 13:04:54.942 |  |  |  |  | ←XML | Media-Server
226 | 13:04:54.945 |  |  |  |  | ←SIP NOTIFY | P-CSCF
227 | 13:04:54.947 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:49729;transp... |  |  |
228 | 13:04:54.999 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
229 | 13:04:55.000 |  |  |  |  | →SIP 200 OK | P-CSCF
230 | 13:04:55.351 | →enobeB PCAP frame→ TCP |  |  |  |
231 | 13:04:55.354 |  | ←enobeB PCAP frame← TCP |  |  |
232 | 13:04:55.391 | →enobeB PCAP frame→ TCP |  |  |  |
233 | 13:04:55.399 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
234 | 13:04:55.402 |  | ←enobeB PCAP frame← TCP |  |  |
235 | 13:04:55.403 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
236 | 13:04:55.481 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
237 | 13:04:55.482 |  | ←enobeB PCAP frame← TCP |  |  |
238 | 13:04:55.483 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
239 | 13:04:55.519 | →enobeB PCAP frame→ TCP |  |  |  |
240 | 13:04:55.521 |  |  |  |  | →HTTP GET | HTTP-Proxy
241 | 13:04:55.522 |  | ←enobeB PCAP frame← TCP |  |  |
242 | 13:04:55.524 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:642: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcptt-ue-configuration.xml
243 | 13:04:55.527 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
244 | 13:04:55.529 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
245 | 13:04:55.591 | →enobeB PCAP frame→ TCP |  |  |  |
246 | 13:04:55.599 | →enobeB PCAP frame→ TCP |  |  |  |
247 | 13:04:55.601 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
248 | 13:04:55.602 |  | ←enobeB PCAP frame← TCP |  |  |
249 | 13:04:55.631 | →enobeB PCAP frame→ TCP |  |  |  |
250 | 13:04:55.791 | →enobeB PCAP frame→ TCP |  |  |  |
251 | 13:04:55.794 |  | ←enobeB PCAP frame← TCP |  |  |
252 | 13:04:55.831 | →enobeB PCAP frame→ TCP |  |  |  |
253 | 13:04:55.839 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
254 | 13:04:55.842 |  | ←enobeB PCAP frame← TCP |  |  |
255 | 13:04:55.845 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
256 | 13:04:55.871 | →enobeB PCAP frame→ TCP |  |  |  |
257 | 13:04:55.959 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
258 | 13:04:55.962 |  | ←enobeB PCAP frame← TCP |  |  |
259 | 13:04:55.962 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
260 | 13:04:55.963 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
261 | 13:04:55.990 | →enobeB PCAP frame→ TCP |  |  |  |
262 | 13:04:55.999 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-... |  |  |  |
263 | 13:04:56.001 |  | ←enobeB PCAP frame← TCP |  |  |
264 | 13:04:56.002 |  |  |  |  | →HTTP GET | HTTP-Proxy
265 | 13:04:56.014 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:647: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcptt-user-profile-49.xml
266 | 13:04:56.054 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
267 | 13:04:56.061 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
268 | 13:04:56.062 |  | ←enobeB PCAP frame← TCP |  |  |
269 | 13:04:56.063 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
270 | 13:04:56.111 | →enobeB PCAP frame→ TCP |  |  |  |
271 | 13:04:56.119 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
272 | 13:04:56.121 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
273 | 13:04:56.122 |  | ←enobeB PCAP frame← TCP |  |  |
274 | 13:04:56.123 |  | ←enobeB PCAP frame← TCP |  |  |
275 | 13:04:56.151 | →enobeB PCAP frame→ TCP |  |  |  |
276 | 13:04:56.759 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
277 | 13:04:56.760 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
278 | 13:04:56.761 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
279 | 13:04:56.776 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
280 | 13:04:56.836 |  |  |  |  | ←SIP 200 OK | P-CSCF
281 | 13:04:56.836 |  |  |  |  | MIKEY | Media-Server
282 | 13:04:56.838 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
283 | 13:04:56.871 | →enobeB PCAP frame→ TCP |  |  |  |
284 | 13:04:56.874 |  | ←enobeB PCAP frame← TCP |  |  |
285 | 13:04:56.911 | →enobeB PCAP frame→ TCP |  |  |  |
286 | 13:04:56.919 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
287 | 13:04:56.922 |  | ←enobeB PCAP frame← TCP |  |  |
288 | 13:04:56.923 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
289 | 13:04:56.951 | →enobeB PCAP frame→ TCP |  |  |  |
290 | 13:04:57.039 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
291 | 13:04:57.040 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
292 | 13:04:57.042 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
293 | 13:04:57.057 |  |  |  |  | XML→ | Media-Server
294 | 13:04:57.058 |  |  |  |  | XML→ | Media-Server
295 | 13:04:57.061 |  |  |  |  | ←XML | Media-Server
296 | 13:04:57.064 |  |  |  |  | ←SIP NOTIFY | P-CSCF
297 | 13:04:57.066 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:49729;transp... |  |  |
298 | 13:04:57.071 | →enobeB PCAP frame→ TCP |  |  |  |
299 | 13:04:57.079 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.servi... |  |  |  |
300 | 13:04:57.080 |  |  |  |  | →HTTP GET | HTTP-Proxy
301 | 13:04:57.082 |  | ←enobeB PCAP frame← TCP |  |  |
302 | 13:04:57.083 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:652: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
303 | 13:04:57.088 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
304 | 13:04:57.091 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
305 | 13:04:57.092 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
306 | 13:04:57.103 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
307 | 13:04:57.106 |  |  |  |  | →SIP 200 OK | P-CSCF
308 | 13:04:57.151 | →enobeB PCAP frame→ TCP |  |  |  |
309 | 13:04:57.159 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
310 | 13:04:57.161 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
311 | 13:04:57.162 |  | ←enobeB PCAP frame← TCP |  |  |
312 | 13:04:57.191 | →enobeB PCAP frame→ TCP |  |  |  |
313 | 13:04:57.271 | →enobeB PCAP frame→ TCP |  |  |  |
314 | 13:04:57.274 |  | ←enobeB PCAP frame← TCP |  |  |
315 | 13:04:57.311 | →enobeB PCAP frame→ TCP |  |  |  |
316 | 13:04:57.319 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
317 | 13:04:57.322 |  | ←enobeB PCAP frame← TCP |  |  |
318 | 13:04:57.325 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
319 | 13:04:57.351 | →enobeB PCAP frame→ TCP |  |  |  |
320 | 13:04:57.439 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
321 | 13:04:57.441 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
322 | 13:04:57.442 |  | ←enobeB PCAP frame← TCP |  |  |
323 | 13:04:57.443 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
324 | 13:04:57.471 | →enobeB PCAP frame→ TCP |  |  |  |
325 | 13:04:57.479 | →enobeB PCAP frame→ HTTPS: GET /xcap.gms.mcstaasting.com/org.openmobileallian... |  |  |  |
326 | 13:04:57.481 |  |  |  |  | →HTTP GET | HTTP-Proxy
327 | 13:04:57.482 |  | ←enobeB PCAP frame← TCP |  |  |
328 | 13:04:57.492 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:657: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at /xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
329 | 13:04:57.517 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
330 | 13:04:57.522 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
331 | 13:04:57.523 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
332 | 13:04:57.551 | →enobeB PCAP frame→ TCP |  |  |  |
333 | 13:04:57.559 | →enobeB PCAP frame→ TCP |  |  |  |
334 | 13:04:57.567 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
335 | 13:04:57.569 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
336 | 13:04:57.570 |  | ←enobeB PCAP frame← TCP |  |  |
337 | 13:04:57.591 | →enobeB PCAP frame→ TCP |  |  |  |
338 | 13:04:57.839 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
339 | 13:04:57.840 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
340 | 13:04:57.853 |  |  |  |  | →SIP PUBLISH | P-CSCF
341 | 13:04:57.900 |  |  |  |  | MIKEY | Media-Server
342 | 13:04:57.919 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
343 | 13:04:57.920 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
344 | 13:04:57.926 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
345 | 13:04:58.128 |  |  |  |  | XML→ | Media-Server
346 | 13:04:58.131 |  |  |  |  | ←SIP 200 OK | P-CSCF
347 | 13:04:58.133 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
348 | 13:04:58.134 |  |  |  |  | ←SIP 200 OK | P-CSCF
349 | 13:04:58.134 |  |  |  |  | MIKEY | Media-Server
350 | 13:04:58.136 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
351 | 13:04:58.341 |  |  |  |  | XML→ | Media-Server
352 | 13:04:58.342 |  |  |  |  | XML→ | Media-Server
353 | 13:04:58.377 |  |  |  |  | ←XML | Media-Server
354 | 13:04:58.381 |  |  |  |  | ←SIP NOTIFY | P-CSCF
355 | 13:04:58.384 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:49729;transp... |  |  |
356 | 13:04:58.449 |  |  |  |  | →SIP 200 OK | P-CSCF
357 | 13:04:58.460 |  |  |  |  | ←XML | Media-Server
358 | 13:04:58.471 |  |  |  |  | ←SIP MESSAGE | P-CSCF
359 | 13:04:58.474 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
360 | 13:04:58.475 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
361 | 13:04:59.242 |  |  |  |  | →SIP 200 OK | P-CSCF
362 | 13:04:59.249 |  |  |  |  | Info: MCX_IMS_CommonProcedures.ttcn:155: MESSAGE/200OK Table 5.3.2.3-2 Steps 7-8 Done
363 | 13:04:59.252 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
364 | 13:04:59.271 | →enobeB PCAP frame→ TCP |  |  |  |
365 | 13:04:59.351 | →enobeB PCAP frame→ TCP |  |  |  |
366 | 13:05:01.252 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
367 | 13:05:01.298 |  | ←RRC DCCH RRC Connection Release |  |  |
368 | 13:05:01.299 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
369 | 13:05:01.317 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
370 | 13:05:01.327 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:735: SRTP config: Master Key: 16FA289113506568A575D2FD7BE88CC0, Master Salt: F0A99FBFD73A7D1E1C39F30C, MKI: 2BBCCCAA
371 | 13:05:01.327 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
372 | 13:05:01.329 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
373 | 13:05:01.331 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
374 | 13:05:01.342 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
375 | 13:05:01.342 |  |  |  |  | ←XML | Media-Server
376 | 13:05:01.372 |  |  |  |  | ←SIP INVITE | P-CSCF
377 | 13:05:02.198 |  | ←enobeB PCAP frame← LTE RRC PCCH Paging (1 PagingRecord) |  |  |
378 | 13:05:02.198 |  | ←RRC PCCH Paging |  |  |
379 | 13:05:02.238 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
380 | 13:05:02.238 |  | →RRC CCCH RRC Connection Request |  |  |
381 | 13:05:02.238 |  | ←RRC CCCH RRC Connection Setup |  |  |
382 | 13:05:02.238 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
383 | 13:05:02.271 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
384 | 13:05:02.271 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
385 | 13:05:02.271 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
386 | 13:05:02.271 |  |  |  | →NAS EMM Service request |  |
387 | 13:05:02.271 |  |  |  | NAS K-enb 853569bcbd75a0c14ec42c27a7b769897... |  |
388 | 13:05:02.272 |  |  | RRC K-enb 853569bcbd75a0c14ec42c27a7b769897... |  |  |
389 | 13:05:02.273 |  |  | RRC rrc-cip 6531aa233bd6f78a9243a27f711ac06... |  |  |
390 | 13:05:02.273 |  |  | RRC rrc-int d049b2e5364f0cc3cc2879374917f32... |  |  |
391 | 13:05:02.273 |  |  | RRC up-cip de060603eb918270870f0d0e2e999857... |  |  |
392 | 13:05:02.273 |  |  | RRC up-int 776a4cfa9c66fa8f0ad7bfdd3811bea6... |  |  |
393 | 13:05:02.273 |  | ←RRC DCCH Security Mode Command |  |  |
394 | 13:05:02.273 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
395 | 13:05:02.311 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
396 | 13:05:02.311 |  | →RRC DCCH Security Mode Complete |  |  |
397 | 13:05:02.311 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
398 | 13:05:02.311 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
399 | 13:05:02.351 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
400 | 13:05:02.351 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
401 | 13:05:02.353 |  | ←enobeB PCAP frame← SIP over IPSEC: INVITE sip:PublicUserId-A@192.168.3.2:49729;transp... |  |  |
402 | 13:05:02.399 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 100 Trying |  |  |  |
403 | 13:05:02.406 |  |  |  |  | →SIP 100 Trying | P-CSCF
404 | 13:05:02.439 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 183 Session Progress |  |  |  |
405 | 13:05:02.444 |  |  |  |  | →SIP 183 Session Progress | P-CSCF
406 | 13:05:02.459 |  |  |  |  | ←SIP PRACK | P-CSCF
407 | 13:05:02.474 |  | ←enobeB PCAP frame← SIP over IPSEC: PRACK sip:PublicUserId-A@192.168.3.2:49729;transpo... |  |  |
408 | 13:05:02.519 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
409 | 13:05:02.522 |  |  |  |  | →SIP 200 OK | P-CSCF
410 | 13:05:02.808 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
411 | 13:05:02.809 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x4e) |  |  |
412 | 13:05:02.809 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
413 | 13:05:02.810 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
414 | 13:05:02.831 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
415 | 13:05:02.831 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
416 | 13:05:02.871 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
417 | 13:05:02.871 |  | →RRC DCCH UL Information Transfer |  |  |
418 | 13:05:02.871 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x8) |  |  |
419 | 13:05:02.871 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
420 | 13:05:02.937 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
421 | 13:05:03.279 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:648: Verdict: Pass
422 | 13:05:03.381 |  |  |  |  | MMICmd: Please Accept the Call
423 | 13:05:12.199 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
424 | 13:05:12.200 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
425 | 13:05:12.249 |  |  |  |  | →SIP 200 OK | P-CSCF
426 | 13:05:12.282 |  |  |  |  | XML→ | Media-Server
427 | 13:05:12.290 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:657: 200 OK Verdict: Pass
428 | 13:05:12.290 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:405: Step 1 Verdict: Pass
429 | 13:05:12.295 |  |  |  |  | ←SIP ACK | P-CSCF
430 | 13:05:12.298 |  | ←enobeB PCAP frame← SIP over IPSEC: ACK sip:PublicUserId-A@192.168.3.2:49729;transport... |  |  |
431 | 13:05:13.041 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:410: Step 7B Verdict: Pass
432 | 13:05:13.050 |  |  |  |  | ←SIP BYE | P-CSCF
433 | 13:05:13.054 |  | ←enobeB PCAP frame← SIP over IPSEC: BYE sip:PublicUserId-A@192.168.3.2:49729;transport... |  |  |
434 | 13:05:13.119 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
435 | 13:05:13.122 |  |  |  |  | →SIP 200 OK | P-CSCF
436 | 13:05:14.071 | →enobeB PCAP frame→ |  |  |  |
437 | 13:05:15.131 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
438 | 13:05:15.139 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
439 | 13:05:15.140 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x0) |  |  |
440 | 13:05:15.140 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
441 | 13:05:15.141 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
442 | 13:05:15.191 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
443 | 13:05:15.191 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
444 | 13:05:15.191 |  | →RRC DCCH UL Information Transfer |  |  |
445 | 13:05:15.191 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x4e) |  |  |
446 | 13:05:15.191 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
447 | 13:05:15.260 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
448 | 13:05:15.261 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
449 | 13:05:15.286 |  | ←RRC DCCH RRC Connection Release |  |  |
450 | 13:05:15.287 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
451 | 13:05:15.306 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
452 | 13:05:15.308 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
453 | 13:05:15.310 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
454 | 13:05:16.058 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.