ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 13:13:20.120 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 13:13:20.124 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 13:13:20.125 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 13:13:20.127 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 13:13:20.129 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 13:13:20.131 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:805: IMS UDP port 192.168.2.3:5060 configured
7 | 13:13:20.140 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:755: IMS TCP port 192.168.2.3:5060 configured!
8 | 13:13:20.147 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:776: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 13:13:20.149 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:787: IdM port 192.168.2.3:8080 configured!
10 | 13:13:20.156 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 13:13:21.356 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 13:13:21.359 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 13:13:23.259 |  | ←RRC BCCH SIB |  |  |
14 | 13:13:23.264 |  | ←RRC BCCH SIB1 |  |  |
15 | 13:13:23.344 |  | ←RRC BCCH SIB1 |  |  |
16 | 13:13:23.419 |  | ←RRC BCCH SIB |  |  |
17 | 13:13:23.424 |  | ←RRC BCCH SIB1 |  |  |
18 | 13:14:26.508 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 13:14:26.508 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 13:14:26.508 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 13:14:26.508 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 13:14:26.559 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 13:14:26.559 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 13:14:26.559 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 13:14:26.559 |  |  |  | →NAS EMM Attach request |  |
26 | 13:14:26.559 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 13:14:26.559 |  |  |  | NAS K-asme 3cfa4cd3e11289f7b2475fd540cd19e9... |  |
28 | 13:14:26.559 |  |  |  | NAS ← EMM Authentication request |  |
29 | 13:14:26.560 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 13:14:26.560 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 13:14:26.561 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 13:14:26.631 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 13:14:26.631 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 13:14:26.631 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 13:14:26.631 |  |  |  | →NAS EMM Authentication response |  |
36 | 13:14:26.631 |  |  |  | NAS UE auth OK |  |
37 | 13:14:26.631 |  |  |  | NAS K-nas-cip e1db8b76d04fabefd77b7a41c0b45... |  |
38 | 13:14:26.631 |  |  |  | NAS K-nas-int d8f641d7361e0d76400f13354fffc... |  |
39 | 13:14:26.631 |  |  |  | NAS ← EMM Security mode command |  |
40 | 13:14:26.632 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 13:14:26.632 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 13:14:26.633 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 13:14:26.671 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
44 | 13:14:26.671 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 13:14:26.671 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xd) |  |  |
46 | 13:14:26.671 |  |  |  | →NAS EMM Security mode complete |  |
47 | 13:14:26.671 |  |  |  | NAS ← ESM ESM information request |  |
48 | 13:14:26.672 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xc) |  |  |
49 | 13:14:26.672 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 13:14:26.673 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
51 | 13:14:26.719 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
52 | 13:14:26.719 |  | →RRC DCCH UL Information Transfer |  |  |
53 | 13:14:26.719 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xd) |  |  |
54 | 13:14:26.719 |  |  |  | →NAS ESM ESM information response |  |
55 | 13:14:26.719 |  |  |  | NAS ← EMM Attach accept |  |
56 | 13:14:26.719 |  |  |  | NAS K-enb 370523d256849b49c0bcd6e2794418537... |  |
57 | 13:14:26.720 |  | ←RRC DCCH Security Mode Command |  |  |
58 | 13:14:26.720 |  |  | RRC K-enb 370523d256849b49c0bcd6e2794418537... |  |  |
59 | 13:14:26.720 |  |  | RRC rrc-cip 266fc01cd566576e9348161b15ee9a7... |  |  |
60 | 13:14:26.720 |  |  | RRC rrc-int 284211738adfe0871fcd64984e5d1da... |  |  |
61 | 13:14:26.720 |  |  | RRC up-cip 1688c4a8f7a81653a941820546957929... |  |  |
62 | 13:14:26.720 |  |  | RRC up-int 80fac9ce7307b35982da2f62320607a5... |  |  |
63 | 13:14:26.721 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
64 | 13:14:26.751 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
65 | 13:14:26.751 |  | →RRC DCCH Security Mode Complete |  |  |
66 | 13:14:26.751 |  | ←RRC DCCH UE Capability Enquiry |  |  |
67 | 13:14:26.751 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
68 | 13:14:26.801 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
69 | 13:14:26.801 |  | →RRC DCCH UE Capability Information |  |  |
70 | 13:14:26.802 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xb) |  |  |
71 | 13:14:26.802 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
72 | 13:14:26.802 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
73 | 13:14:26.831 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
74 | 13:14:26.831 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
75 | 13:14:26.871 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
76 | 13:14:26.871 |  | →RRC DCCH UL Information Transfer |  |  |
77 | 13:14:26.871 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xd) |  |  |
78 | 13:14:26.871 |  |  |  | →NAS EMM Attach complete |  |
79 | 13:14:26.871 |  |  |  | NAS ← EMM EMM information |  |
80 | 13:14:26.872 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xc) |  |  |
81 | 13:14:26.872 |  | ←RRC DCCH DL Information Transfer |  |  |
82 | 13:14:26.873 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
83 | 13:14:33.541 |  | ←RRC DCCH RRC Connection Release |  |  |
84 | 13:14:33.542 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
85 | 13:14:34.768 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
86 | 13:14:34.768 |  | →RRC CCCH RRC Connection Request |  |  |
87 | 13:14:34.768 |  | ←RRC CCCH RRC Connection Setup |  |  |
88 | 13:14:34.768 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
89 | 13:14:34.831 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
90 | 13:14:34.831 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
91 | 13:14:34.831 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
92 | 13:14:34.831 |  |  |  | →NAS EMM Service request |  |
93 | 13:14:34.831 |  |  |  | NAS K-enb 12edce2db629c0cd09caf8136f74a322c... |  |
94 | 13:14:34.832 |  |  | RRC K-enb 12edce2db629c0cd09caf8136f74a322c... |  |  |
95 | 13:14:34.833 |  |  | RRC rrc-cip 07e443b6f43bf9c40e574bf6ffcebce... |  |  |
96 | 13:14:34.833 |  |  | RRC rrc-int 713c083f8472d162f40f97dd8bb4f0b... |  |  |
97 | 13:14:34.833 |  |  | RRC up-cip 2f82e40903f6d6c0d87be0bde3caae46... |  |  |
98 | 13:14:34.833 |  |  | RRC up-int 0f8caed81ea13538dd07934692dd0198... |  |  |
99 | 13:14:34.833 |  | ←RRC DCCH Security Mode Command |  |  |
100 | 13:14:34.833 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
101 | 13:14:34.871 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
102 | 13:14:34.871 |  | →RRC DCCH Security Mode Complete |  |  |
103 | 13:14:34.871 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
104 | 13:14:34.871 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
105 | 13:14:34.911 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
106 | 13:14:34.911 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
107 | 13:15:07.871 | →enobeB PCAP frame→ TCP |  |  |  |
108 | 13:15:07.874 |  | ←enobeB PCAP frame← TCP |  |  |
109 | 13:15:07.911 | →enobeB PCAP frame→ TCP |  |  |  |
110 | 13:15:07.999 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
111 | 13:15:08.002 |  | ←enobeB PCAP frame← TCP |  |  |
112 | 13:15:08.008 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
113 | 13:15:08.031 | →enobeB PCAP frame→ TCP |  |  |  |
114 | 13:15:08.159 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
115 | 13:15:08.162 |  | ←enobeB PCAP frame← TCP |  |  |
116 | 13:15:08.162 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 16)
117 | 13:15:08.163 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
118 | 13:15:08.191 | →enobeB PCAP frame→ TCP |  |  |  |
119 | 13:15:08.199 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
120 | 13:15:08.202 |  | ←enobeB PCAP frame← TCP |  |  |
121 | 13:15:08.202 |  |  |  |  | →HTTP GET | HTTP-Proxy
122 | 13:15:08.208 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:288: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
123 | 13:15:08.226 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
124 | 13:15:08.230 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
125 | 13:15:08.271 | →enobeB PCAP frame→ TCP |  |  |  |
126 | 13:15:10.111 | →enobeB PCAP frame→ TCP |  |  |  |
127 | 13:15:10.114 |  | ←enobeB PCAP frame← TCP |  |  |
128 | 13:15:10.151 | →enobeB PCAP frame→ TCP |  |  |  |
129 | 13:15:10.159 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
130 | 13:15:10.163 |  | ←enobeB PCAP frame← TCP |  |  |
131 | 13:15:10.168 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
132 | 13:15:10.191 | →enobeB PCAP frame→ TCP |  |  |  |
133 | 13:15:10.519 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
134 | 13:15:10.522 |  | ←enobeB PCAP frame← TCP |  |  |
135 | 13:15:10.522 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:642: Client connected to IdM port (id 18)
136 | 13:15:10.523 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
137 | 13:15:10.551 | →enobeB PCAP frame→ TCP |  |  |  |
138 | 13:15:10.559 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
139 | 13:15:10.562 |  | ←enobeB PCAP frame← TCP |  |  |
140 | 13:15:10.562 |  |  |  |  | →HTTP GET | IDMS-Endpoint
141 | 13:15:10.581 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
142 | 13:15:10.583 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
143 | 13:15:10.585 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:511: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
144 | 13:15:10.585 |  |  |  |  | MMICmd: Please provide user credentials: username and password
145 | 13:15:10.631 | →enobeB PCAP frame→ TCP |  |  |  |
146 | 13:15:15.239 | →enobeB PCAP frame→ HTTPS: POST /idms/userauth HTTP/1.1 |  |  |  |
147 | 13:15:15.242 |  | ←enobeB PCAP frame← TCP |  |  |
148 | 13:15:15.244 |  |  |  |  | →HTTP POST | IDMS-Endpoint
149 | 13:15:15.259 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
150 | 13:15:15.261 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:516: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
151 | 13:15:15.262 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
152 | 13:15:15.311 | →enobeB PCAP frame→ TCP |  |  |  |
153 | 13:15:15.319 | →enobeB PCAP frame→ TCP |  |  |  |
154 | 13:15:15.321 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:677: IdM port - Client closed the connection (id 18)
155 | 13:15:15.322 |  | ←enobeB PCAP frame← TCP |  |  |
156 | 13:15:15.351 | →enobeB PCAP frame→ TCP |  |  |  |
157 | 13:15:15.911 | →enobeB PCAP frame→ TCP |  |  |  |
158 | 13:15:15.914 |  | ←enobeB PCAP frame← TCP |  |  |
159 | 13:15:15.951 | →enobeB PCAP frame→ TCP |  |  |  |
160 | 13:15:15.959 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
161 | 13:15:15.962 |  | ←enobeB PCAP frame← TCP |  |  |
162 | 13:15:15.963 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
163 | 13:15:15.991 | →enobeB PCAP frame→ TCP |  |  |  |
164 | 13:15:16.039 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
165 | 13:15:16.042 |  | ←enobeB PCAP frame← TCP |  |  |
166 | 13:15:16.043 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
167 | 13:15:16.071 | →enobeB PCAP frame→ TCP |  |  |  |
168 | 13:15:16.079 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
169 | 13:15:16.082 |  | ←enobeB PCAP frame← TCP |  |  |
170 | 13:15:16.104 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:642: Client connected to IdM port (id 18)
171 | 13:15:16.106 |  |  |  |  | →HTTP POST | IDMS-Endpoint
172 | 13:15:16.150 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
173 | 13:15:16.150 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:521: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
174 | 13:15:16.152 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
175 | 13:15:16.231 | →enobeB PCAP frame→ TCP |  |  |  |
176 | 13:15:16.471 | →enobeB PCAP frame→ TCP |  |  |  |
177 | 13:15:16.474 |  | ←enobeB PCAP frame← TCP |  |  |
178 | 13:15:16.511 | →enobeB PCAP frame→ TCP |  |  |  |
179 | 13:15:16.519 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
180 | 13:15:16.522 |  | ←enobeB PCAP frame← TCP |  |  |
181 | 13:15:16.527 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
182 | 13:15:16.551 | →enobeB PCAP frame→ TCP |  |  |  |
183 | 13:15:16.559 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
184 | 13:15:16.562 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 19)
185 | 13:15:16.563 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
186 | 13:15:16.599 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
187 | 13:15:16.602 |  | ←enobeB PCAP frame← TCP |  |  |
188 | 13:15:16.604 |  |  |  |  | →HTTP POST | HTTP-Proxy
189 | 13:15:16.629 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:541: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
190 | 13:15:16.636 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
191 | 13:15:16.639 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
192 | 13:15:16.671 | →enobeB PCAP frame→ TCP |  |  |  |
193 | 13:15:16.711 | →enobeB PCAP frame→ TCP |  |  |  |
194 | 13:15:16.714 |  | ←enobeB PCAP frame← TCP |  |  |
195 | 13:15:16.751 | →enobeB PCAP frame→ TCP |  |  |  |
196 | 13:15:16.759 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
197 | 13:15:16.762 |  | ←enobeB PCAP frame← TCP |  |  |
198 | 13:15:16.767 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
199 | 13:15:16.791 | →enobeB PCAP frame→ TCP |  |  |  |
200 | 13:15:16.799 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
201 | 13:15:16.802 |  | ←enobeB PCAP frame← TCP |  |  |
202 | 13:15:16.802 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 20)
203 | 13:15:16.803 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
204 | 13:15:16.839 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
205 | 13:15:16.842 |  | ←enobeB PCAP frame← TCP |  |  |
206 | 13:15:16.843 |  |  |  |  | →HTTP POST | HTTP-Proxy
207 | 13:15:16.904 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
208 | 13:15:16.905 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:545: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
209 | 13:15:16.907 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
210 | 13:15:16.951 | →enobeB PCAP frame→ TCP |  |  |  |
211 | 13:15:17.039 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
212 | 13:15:17.043 |  |  |  |  | →SIP REGISTER | P-CSCF
213 | 13:15:17.068 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:814: IMS UDP_s port 192.168.2.3:5062 configured
214 | 13:15:17.097 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:765: IMS TCP_s port 192.168.2.3:5062 configured!
215 | 13:15:17.099 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:823: IMS UDP_c port 192.168.2.3:5061 configured
216 | 13:15:17.107 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
217 | 13:15:17.799 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
218 | 13:15:17.804 |  |  |  |  | →SIP REGISTER | P-CSCF
219 | 13:15:17.830 |  |  |  |  | ←SIP 200 OK | P-CSCF
220 | 13:15:17.832 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
221 | 13:15:18.199 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
222 | 13:15:18.200 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
223 | 13:15:18.201 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 SIP over IPSEC: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 |  |  |  |
224 | 13:15:18.216 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
225 | 13:15:18.275 |  |  |  |  | ←SIP 200 OK | P-CSCF
226 | 13:15:18.275 |  |  |  |  | MIKEY | Media-Server
227 | 13:15:18.277 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
228 | 13:15:18.504 |  |  |  |  | XML→ | Media-Server
229 | 13:15:18.506 |  |  |  |  | XML→ | Media-Server
230 | 13:15:18.509 |  |  |  |  | ←XML | Media-Server
231 | 13:15:18.512 |  |  |  |  | ←SIP NOTIFY | P-CSCF
232 | 13:15:18.515 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:44167;transp... |  |  |
233 | 13:15:18.559 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
234 | 13:15:18.561 |  |  |  |  | →SIP 200 OK | P-CSCF
235 | 13:15:18.751 | →enobeB PCAP frame→ TCP |  |  |  |
236 | 13:15:18.754 |  | ←enobeB PCAP frame← TCP |  |  |
237 | 13:15:18.791 | →enobeB PCAP frame→ TCP |  |  |  |
238 | 13:15:18.799 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
239 | 13:15:18.802 |  | ←enobeB PCAP frame← TCP |  |  |
240 | 13:15:18.806 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
241 | 13:15:18.831 | →enobeB PCAP frame→ TCP |  |  |  |
242 | 13:15:18.919 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
243 | 13:15:18.921 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
244 | 13:15:18.922 |  | ←enobeB PCAP frame← TCP |  |  |
245 | 13:15:18.923 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
246 | 13:15:18.951 | →enobeB PCAP frame→ TCP |  |  |  |
247 | 13:15:18.999 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-co... |  |  |  |
248 | 13:15:19.002 |  | ←enobeB PCAP frame← TCP |  |  |
249 | 13:15:19.002 |  |  |  |  | →HTTP GET | HTTP-Proxy
250 | 13:15:19.010 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:642: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcptt-ue-configuration.xml
251 | 13:15:19.018 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
252 | 13:15:19.020 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
253 | 13:15:19.071 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
254 | 13:15:19.073 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
255 | 13:15:19.074 |  | ←enobeB PCAP frame← TCP |  |  |
256 | 13:15:19.080 | →enobeB PCAP frame→ TCP |  |  |  |
257 | 13:15:19.082 |  | ←enobeB PCAP frame← TCP |  |  |
258 | 13:15:19.111 | →enobeB PCAP frame→ TCP |  |  |  |
259 | 13:15:19.231 | →enobeB PCAP frame→ TCP |  |  |  |
260 | 13:15:19.234 |  | ←enobeB PCAP frame← TCP |  |  |
261 | 13:15:19.271 | →enobeB PCAP frame→ TCP |  |  |  |
262 | 13:15:19.279 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
263 | 13:15:19.282 |  | ←enobeB PCAP frame← TCP |  |  |
264 | 13:15:19.285 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
265 | 13:15:19.311 | →enobeB PCAP frame→ TCP |  |  |  |
266 | 13:15:19.359 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
267 | 13:15:19.362 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
268 | 13:15:19.363 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
269 | 13:15:19.391 | →enobeB PCAP frame→ TCP |  |  |  |
270 | 13:15:19.399 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-... |  |  |  |
271 | 13:15:19.402 |  | ←enobeB PCAP frame← TCP |  |  |
272 | 13:15:19.402 |  |  |  |  | →HTTP GET | HTTP-Proxy
273 | 13:15:19.414 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:647: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcptt-user-profile-49.xml
274 | 13:15:19.454 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
275 | 13:15:19.461 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
276 | 13:15:19.462 |  | ←enobeB PCAP frame← TCP |  |  |
277 | 13:15:19.463 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
278 | 13:15:19.511 | →enobeB PCAP frame→ TCP |  |  |  |
279 | 13:15:19.519 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
280 | 13:15:19.521 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
281 | 13:15:19.522 |  | ←enobeB PCAP frame← TCP |  |  |
282 | 13:15:19.523 |  | ←enobeB PCAP frame← TCP |  |  |
283 | 13:15:19.551 | →enobeB PCAP frame→ TCP |  |  |  |
284 | 13:15:20.239 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
285 | 13:15:20.240 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
286 | 13:15:20.267 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
287 | 13:15:20.327 |  |  |  |  | ←SIP 200 OK | P-CSCF
288 | 13:15:20.327 |  |  |  |  | MIKEY | Media-Server
289 | 13:15:20.328 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
290 | 13:15:20.351 | →enobeB PCAP frame→ TCP |  |  |  |
291 | 13:15:20.354 |  | ←enobeB PCAP frame← TCP |  |  |
292 | 13:15:20.391 | →enobeB PCAP frame→ TCP |  |  |  |
293 | 13:15:20.399 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
294 | 13:15:20.402 |  | ←enobeB PCAP frame← TCP |  |  |
295 | 13:15:20.403 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
296 | 13:15:20.521 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
297 | 13:15:20.522 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
298 | 13:15:20.554 |  |  |  |  | XML→ | Media-Server
299 | 13:15:20.555 |  |  |  |  | XML→ | Media-Server
300 | 13:15:20.559 | →enobeB PCAP frame→ TCP |  |  |  |
301 | 13:15:20.559 |  |  |  |  | ←XML | Media-Server
302 | 13:15:20.561 |  |  |  |  | →HTTP GET | HTTP-Proxy
303 | 13:15:20.562 |  | ←enobeB PCAP frame← TCP |  |  |
304 | 13:15:20.562 |  |  |  |  | ←SIP NOTIFY | P-CSCF
305 | 13:15:20.564 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:44167;transp... |  |  |
306 | 13:15:20.564 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:652: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
307 | 13:15:20.569 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
308 | 13:15:20.572 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
309 | 13:15:20.573 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
310 | 13:15:20.591 | →enobeB PCAP frame→ TCP |  |  |  |
311 | 13:15:20.599 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
312 | 13:15:20.601 |  |  |  |  | →SIP 200 OK | P-CSCF
313 | 13:15:20.631 | →enobeB PCAP frame→ TCP |  |  |  |
314 | 13:15:20.633 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
315 | 13:15:20.634 |  | ←enobeB PCAP frame← TCP |  |  |
316 | 13:15:20.639 | →enobeB PCAP frame→ TCP |  |  |  |
317 | 13:15:20.643 |  | ←enobeB PCAP frame← TCP |  |  |
318 | 13:15:20.671 | →enobeB PCAP frame→ TCP |  |  |  |
319 | 13:15:20.711 | →enobeB PCAP frame→ TCP |  |  |  |
320 | 13:15:20.714 |  | ←enobeB PCAP frame← TCP |  |  |
321 | 13:15:20.751 | →enobeB PCAP frame→ TCP |  |  |  |
322 | 13:15:20.759 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
323 | 13:15:20.762 |  | ←enobeB PCAP frame← TCP |  |  |
324 | 13:15:20.765 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
325 | 13:15:20.791 | →enobeB PCAP frame→ TCP |  |  |  |
326 | 13:15:20.879 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
327 | 13:15:20.881 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
328 | 13:15:20.882 |  | ←enobeB PCAP frame← TCP |  |  |
329 | 13:15:20.883 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
330 | 13:15:20.911 | →enobeB PCAP frame→ TCP |  |  |  |
331 | 13:15:20.959 | →enobeB PCAP frame→ HTTPS: GET /xcap.gms.mcstaasting.com/org.openmobileallian... |  |  |  |
332 | 13:15:20.962 |  | ←enobeB PCAP frame← TCP |  |  |
333 | 13:15:20.962 |  |  |  |  | →HTTP GET | HTTP-Proxy
334 | 13:15:20.972 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:657: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at /xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
335 | 13:15:21.001 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
336 | 13:15:21.006 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
337 | 13:15:21.007 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
338 | 13:15:21.031 | →enobeB PCAP frame→ TCP |  |  |  |
339 | 13:15:21.039 | →enobeB PCAP frame→ TCP |  |  |  |
340 | 13:15:21.071 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
341 | 13:15:21.073 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
342 | 13:15:21.074 |  | ←enobeB PCAP frame← TCP |  |  |
343 | 13:15:21.079 | →enobeB PCAP frame→ TCP |  |  |  |
344 | 13:15:21.082 |  | ←enobeB PCAP frame← TCP |  |  |
345 | 13:15:21.111 | →enobeB PCAP frame→ TCP |  |  |  |
346 | 13:15:21.279 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
347 | 13:15:21.280 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
348 | 13:15:21.294 |  |  |  |  | →SIP PUBLISH | P-CSCF
349 | 13:15:21.344 |  |  |  |  | MIKEY | Media-Server
350 | 13:15:21.359 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
351 | 13:15:21.360 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
352 | 13:15:21.366 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
353 | 13:15:21.572 |  |  |  |  | XML→ | Media-Server
354 | 13:15:21.575 |  |  |  |  | ←SIP 200 OK | P-CSCF
355 | 13:15:21.577 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
356 | 13:15:21.578 |  |  |  |  | ←SIP 200 OK | P-CSCF
357 | 13:15:21.579 |  |  |  |  | MIKEY | Media-Server
358 | 13:15:21.580 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
359 | 13:15:21.787 |  |  |  |  | XML→ | Media-Server
360 | 13:15:21.788 |  |  |  |  | XML→ | Media-Server
361 | 13:15:21.822 |  |  |  |  | ←XML | Media-Server
362 | 13:15:21.827 |  |  |  |  | ←SIP NOTIFY | P-CSCF
363 | 13:15:21.830 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:44167;transp... |  |  |
364 | 13:15:21.879 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
365 | 13:15:21.882 |  |  |  |  | →SIP 200 OK | P-CSCF
366 | 13:15:21.893 |  |  |  |  | ←XML | Media-Server
367 | 13:15:21.924 |  |  |  |  | ←SIP MESSAGE | P-CSCF
368 | 13:15:21.928 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
369 | 13:15:22.799 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
370 | 13:15:22.802 |  |  |  |  | →SIP 200 OK | P-CSCF
371 | 13:15:22.809 |  |  |  |  | Info: MCX_IMS_CommonProcedures.ttcn:155: MESSAGE/200OK Table 5.3.2.3-2 Steps 7-8 Done
372 | 13:15:22.812 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
373 | 13:15:22.871 | →enobeB PCAP frame→ TCP |  |  |  |
374 | 13:15:22.879 | →enobeB PCAP frame→ TCP |  |  |  |
375 | 13:15:24.812 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
376 | 13:15:24.847 |  | ←RRC DCCH RRC Connection Release |  |  |
377 | 13:15:24.848 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
378 | 13:15:24.867 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
379 | 13:15:24.869 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
380 | 13:15:24.869 |  |  |  |  | MMICmd: Make the MCPTT User request the establishment of an MCPTT On-demand chat group emergency group call for the selected MCPTT chat group emergency group GROUP A, with implicit floor control
381 | 13:15:29.338 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
382 | 13:15:29.338 |  | →RRC CCCH RRC Connection Request |  |  |
383 | 13:15:29.338 |  | ←RRC CCCH RRC Connection Setup |  |  |
384 | 13:15:29.338 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
385 | 13:15:29.391 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
386 | 13:15:29.391 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
387 | 13:15:29.391 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
388 | 13:15:29.391 |  |  |  | →NAS EMM Service request |  |
389 | 13:15:29.391 |  |  |  | NAS K-enb 902076fdd21b8b0e62673e3474403263d... |  |
390 | 13:15:29.392 |  |  | RRC K-enb 902076fdd21b8b0e62673e3474403263d... |  |  |
391 | 13:15:29.393 |  |  | RRC rrc-cip c95a6b0d1aaeef1ea378379258f253d... |  |  |
392 | 13:15:29.393 |  |  | RRC rrc-int 05b70db7427a6df748f0aa6306b47bf... |  |  |
393 | 13:15:29.393 |  |  | RRC up-cip cceebf6d9a3a2f3ea0055298045ba160... |  |  |
394 | 13:15:29.393 |  |  | RRC up-int f4cec85549bfadc59598a83f4e1b1cb7... |  |  |
395 | 13:15:29.393 |  | ←RRC DCCH Security Mode Command |  |  |
396 | 13:15:29.393 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
397 | 13:15:29.431 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
398 | 13:15:29.431 |  | →RRC DCCH Security Mode Complete |  |  |
399 | 13:15:29.431 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
400 | 13:15:29.431 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
401 | 13:15:29.471 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
402 | 13:15:29.471 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
403 | 13:15:29.479 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
404 | 13:15:29.480 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
405 | 13:15:29.494 |  |  |  |  | →SIP INVITE | P-CSCF
406 | 13:15:29.521 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:735: SRTP config: Master Key: 8C60442ACC341B766553FB53F4529434, Master Salt: 52B16E244B61E057D92650E1, MKI: 21142DFD
407 | 13:15:29.521 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
408 | 13:15:29.525 |  |  |  |  | XML→ | Media-Server
409 | 13:15:29.527 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
410 | 13:15:29.527 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1205: INVITE Verdict: Pass
411 | 13:15:29.528 |  |  |  |  | ←SIP 100 Trying | P-CSCF
412 | 13:15:29.530 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
413 | 13:15:29.531 |  |  |  |  | ←SIP 200 OK | P-CSCF
414 | 13:15:29.533 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
415 | 13:15:30.162 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
416 | 13:15:30.163 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x5) |  |  |
417 | 13:15:30.163 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
418 | 13:15:30.164 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
419 | 13:15:30.191 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
420 | 13:15:30.191 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
421 | 13:15:30.191 |  | →RRC DCCH UL Information Transfer |  |  |
422 | 13:15:30.191 |  | [EMBEDDED NAS IN PREV RRC] TP Unknown message (type=0x33) |  |  |
423 | 13:15:30.191 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
424 | 13:15:30.300 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
425 | 13:15:30.439 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
426 | 13:15:30.443 |  |  |  |  | →SIP ACK | P-CSCF
427 | 13:15:30.452 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1208: ACK Verdict: Pass
428 | 13:15:30.453 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:566: Step 2 Verdict: Pass
429 | 13:15:30.456 |  |  |  |  | ←Floor Granted | Media-Server
430 | 13:15:30.951 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
431 | 13:15:30.959 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
432 | 13:15:30.967 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
433 | 13:15:30.991 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
434 | 13:15:30.999 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
435 | 13:15:31.203 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:571: Step 9 Verdict: Pass
436 | 13:15:31.308 |  |  |  |  | MMICmd: Release call (hang up the call)
437 | 13:15:34.283 |  |  |  |  | →SIP BYE | P-CSCF
438 | 13:15:34.303 |  |  |  |  | ←SIP 200 OK | P-CSCF
439 | 13:15:34.305 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
440 | 13:15:34.551 | →enobeB PCAP frame→ |  |  |  |
441 | 13:15:36.301 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
442 | 13:15:36.314 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
443 | 13:15:36.315 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x1) |  |  |
444 | 13:15:36.315 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
445 | 13:15:36.316 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
446 | 13:15:36.351 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
447 | 13:15:36.351 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
448 | 13:15:36.351 |  | →RRC DCCH UL Information Transfer |  |  |
449 | 13:15:36.351 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x4) |  |  |
450 | 13:15:36.351 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
451 | 13:15:36.436 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
452 | 13:15:36.437 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
453 | 13:15:36.482 |  | ←RRC DCCH RRC Connection Release |  |  |
454 | 13:15:36.483 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
455 | 13:15:36.503 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
456 | 13:15:36.505 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
457 | 13:15:36.507 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
458 | 13:15:37.256 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.