MSG #71 2021-09-17 08:57:10.261
RRC

     DCCH: RRC Connection Reconfiguration
    {
      message c1: rrcConnectionReconfiguration: {
        rrc-TransactionIdentifier 0,
        criticalExtensions c1: rrcConnectionReconfiguration-r8: {
          dedicatedInfoNASList {
            '277D39222C02CBB3D56B577BFDF4341DD5B6B06F24CC46105956A9CC841F07AACA624BB88AC3D182658AEE3642F75452F98D913E15B970BC6A5B99D8F8689B7DB73CEEA675F612DA40F08251C8CFD26FBF0594696121F69816EB82B99766D7A4BD1B96F52EECECAA2EB0BA7C4DD1A31420542ACEAB176E240B96DC0D2D0431818EE1FF0ACCF7CFFE'H
          },
          radioResourceConfigDedicated {
            srb-ToAddModList {
              {
                srb-Identity 2,
                rlc-Config explicitValue: am: {
                  ul-AM-RLC {
                    t-PollRetransmit ms60,
                    pollPDU pInfinity,
                    pollByte kBinfinity,
                    maxRetxThreshold t32
                  },
                  dl-AM-RLC {
                    t-Reordering ms45,
                    t-StatusProhibit ms0
                  }
                },
                logicalChannelConfig defaultValue: NULL
              }
            },
            drb-ToAddModList {
              {
                eps-BearerIdentity 5,
                drb-Identity 1,
                pdcp-Config {
                  discardTimer infinity,
                  rlc-AM {
                    statusReportRequired TRUE
                  },
                  headerCompression notUsed: NULL
                },
                rlc-Config am: {
                  ul-AM-RLC {
                    t-PollRetransmit ms80,
                    pollPDU p128,
                    pollByte kB125,
                    maxRetxThreshold t4
                  },
                  dl-AM-RLC {
                    t-Reordering ms80,
                    t-StatusProhibit ms60
                  }
                },
                logicalChannelIdentity 3,
                logicalChannelConfig {
                  ul-SpecificParameters {
                    priority 4,
                    prioritisedBitRate kBps8,
                    bucketSizeDuration ms100,
                    logicalChannelGroup 1
                  }
                }
              }
            },
            physicalConfigDedicated {
              cqi-ReportConfig {
                nomPDSCH-RS-EPRE-Offset 0,
                cqi-ReportPeriodic setup: {
                  cqi-PUCCH-ResourceIndex 0,
                  cqi-pmi-ConfigIndex 38,
                  cqi-FormatIndicatorPeriodic widebandCQI: NULL,
                  simultaneousAckNackAndCQI TRUE
                }
              }
            }
          }
        }
      }
    }