ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 08:55:42.376 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 08:55:42.379 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 08:55:42.379 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 08:55:42.381 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 08:55:42.381 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 08:55:42.382 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:807: IMS UDP port 192.168.2.3:5060 configured
7 | 08:55:42.384 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:757: IMS TCP port 192.168.2.3:5060 configured!
8 | 08:55:42.385 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:778: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 08:55:42.386 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:789: IdM port 192.168.2.3:8080 configured!
10 | 08:55:42.387 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 08:55:43.588 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 08:55:43.588 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 08:55:46.963 |  | ←RRC BCCH SIB1 |  |  |
14 | 08:55:47.038 |  | ←RRC BCCH SIB |  |  |
15 | 08:55:47.043 |  | ←RRC BCCH SIB1 |  |  |
16 | 08:55:47.058 |  | ←RRC BCCH SIB |  |  |
17 | 08:55:47.078 |  | ←RRC BCCH SIB |  |  |
18 | 08:57:09.967 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 08:57:09.967 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 08:57:09.967 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 08:57:09.967 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 08:57:10.018 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 08:57:10.018 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 08:57:10.018 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 08:57:10.018 |  |  |  | →NAS EMM Attach request |  |
26 | 08:57:10.018 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 08:57:10.018 |  |  |  | NAS K-asme 6f99f7843afe3cb75bf075d97ec00f42... |  |
28 | 08:57:10.018 |  |  |  | NAS ← EMM Authentication request |  |
29 | 08:57:10.019 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 08:57:10.019 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 08:57:10.020 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 08:57:10.090 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 08:57:10.090 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 08:57:10.090 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 08:57:10.090 |  |  |  | →NAS EMM Authentication response |  |
36 | 08:57:10.090 |  |  |  | NAS UE auth OK |  |
37 | 08:57:10.090 |  |  |  | NAS K-nas-cip c38e013f66549eb4d7b2a3ad9c8d8... |  |
38 | 08:57:10.090 |  |  |  | NAS K-nas-int f9d3343b35c05d32b050183802ffc... |  |
39 | 08:57:10.090 |  |  |  | NAS ← EMM Security mode command |  |
40 | 08:57:10.091 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 08:57:10.091 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 08:57:10.092 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 08:57:10.130 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
44 | 08:57:10.130 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 08:57:10.130 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x6) |  |  |
46 | 08:57:10.130 |  |  |  | →NAS EMM Security mode complete |  |
47 | 08:57:10.130 |  |  |  | NAS ← ESM ESM information request |  |
48 | 08:57:10.131 |  | [EMBEDDED NAS IN NEXT RRC] TP Activate test mode complete |  |  |
49 | 08:57:10.131 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 08:57:10.132 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
51 | 08:57:10.178 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
52 | 08:57:10.178 |  | →RRC DCCH UL Information Transfer |  |  |
53 | 08:57:10.178 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x6) |  |  |
54 | 08:57:10.178 |  |  |  | →NAS ESM ESM information response |  |
55 | 08:57:10.178 |  |  |  | NAS ← EMM Attach accept |  |
56 | 08:57:10.178 |  |  |  | NAS K-enb f01e0e5e753204025c39a1cd33bf6d85d... |  |
57 | 08:57:10.179 |  | ←RRC DCCH Security Mode Command |  |  |
58 | 08:57:10.179 |  |  | RRC K-enb f01e0e5e753204025c39a1cd33bf6d85d... |  |  |
59 | 08:57:10.179 |  |  | RRC rrc-cip dc2d5474d9b3ca639bcdbe5477b4708... |  |  |
60 | 08:57:10.179 |  |  | RRC rrc-int 41e7ea4bea10f78b93a732d1c9ab853... |  |  |
61 | 08:57:10.179 |  |  | RRC up-cip 3ade3edb89e491b61ff696702f0ac52c... |  |  |
62 | 08:57:10.179 |  |  | RRC up-int 89f53c9713e6973be8ebb39f4b31cfb9... |  |  |
63 | 08:57:10.180 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
64 | 08:57:10.210 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
65 | 08:57:10.210 |  | →RRC DCCH Security Mode Complete |  |  |
66 | 08:57:10.210 |  | ←RRC DCCH UE Capability Enquiry |  |  |
67 | 08:57:10.210 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
68 | 08:57:10.260 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
69 | 08:57:10.260 |  | →RRC DCCH UE Capability Information |  |  |
70 | 08:57:10.261 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xb) |  |  |
71 | 08:57:10.261 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
72 | 08:57:10.261 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
73 | 08:57:10.290 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
74 | 08:57:10.290 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
75 | 08:57:10.330 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
76 | 08:57:10.330 |  | →RRC DCCH UL Information Transfer |  |  |
77 | 08:57:10.330 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xc) |  |  |
78 | 08:57:10.330 |  |  |  | →NAS EMM Attach complete |  |
79 | 08:57:10.330 |  |  |  | NAS ← EMM EMM information |  |
80 | 08:57:10.331 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x8) |  |  |
81 | 08:57:10.331 |  | ←RRC DCCH DL Information Transfer |  |  |
82 | 08:57:10.332 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
83 | 08:57:15.887 |  | ←RRC DCCH RRC Connection Release |  |  |
84 | 08:57:15.888 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
85 | 08:57:17.137 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
86 | 08:57:17.137 |  | →RRC CCCH RRC Connection Request |  |  |
87 | 08:57:17.137 |  | ←RRC CCCH RRC Connection Setup |  |  |
88 | 08:57:17.137 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
89 | 08:57:17.170 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
90 | 08:57:17.170 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
91 | 08:57:17.170 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
92 | 08:57:17.170 |  |  |  | →NAS EMM Service request |  |
93 | 08:57:17.170 |  |  |  | NAS K-enb bec439ab1095fea43bf98252625da7045... |  |
94 | 08:57:17.171 |  |  | RRC K-enb bec439ab1095fea43bf98252625da7045... |  |  |
95 | 08:57:17.172 |  |  | RRC rrc-cip f8e68a7ed293f5df7f43ae92dbc67c8... |  |  |
96 | 08:57:17.172 |  |  | RRC rrc-int 2a94f7c5ea4b4b201f70269d9759c39... |  |  |
97 | 08:57:17.172 |  |  | RRC up-cip 98d8f7533fef2c5482b2ade9bc35db24... |  |  |
98 | 08:57:17.172 |  |  | RRC up-int a790735556e71deb1443f92621635b27... |  |  |
99 | 08:57:17.172 |  | ←RRC DCCH Security Mode Command |  |  |
100 | 08:57:17.172 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
101 | 08:57:17.210 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
102 | 08:57:17.210 |  | →RRC DCCH Security Mode Complete |  |  |
103 | 08:57:17.210 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
104 | 08:57:17.210 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
105 | 08:57:17.250 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
106 | 08:57:17.250 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
107 | 08:57:32.538 | →enobeB PCAP frame→ TCP |  |  |  |
108 | 08:57:32.541 |  | ←enobeB PCAP frame← TCP |  |  |
109 | 08:57:32.570 | →enobeB PCAP frame→ TCP |  |  |  |
110 | 08:57:32.658 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
111 | 08:57:32.661 |  | ←enobeB PCAP frame← TCP |  |  |
112 | 08:57:32.667 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
113 | 08:57:32.690 | →enobeB PCAP frame→ TCP |  |  |  |
114 | 08:57:32.857 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 16)
115 | 08:57:32.858 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
116 | 08:57:32.861 |  | ←enobeB PCAP frame← TCP |  |  |
117 | 08:57:32.862 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
118 | 08:57:32.890 | →enobeB PCAP frame→ TCP |  |  |  |
119 | 08:57:32.937 |  |  |  |  | →HTTP GET | HTTP-Proxy
120 | 08:57:32.938 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
121 | 08:57:32.941 |  | ←enobeB PCAP frame← TCP |  |  |
122 | 08:57:32.943 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:288: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
123 | 08:57:32.962 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
124 | 08:57:32.970 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
125 | 08:57:33.010 | →enobeB PCAP frame→ TCP |  |  |  |
126 | 08:57:34.650 | →enobeB PCAP frame→ TCP |  |  |  |
127 | 08:57:34.653 |  | ←enobeB PCAP frame← TCP |  |  |
128 | 08:57:34.690 | →enobeB PCAP frame→ TCP |  |  |  |
129 | 08:57:34.698 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
130 | 08:57:34.701 |  | ←enobeB PCAP frame← TCP |  |  |
131 | 08:57:34.706 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
132 | 08:57:34.730 | →enobeB PCAP frame→ TCP |  |  |  |
133 | 08:57:35.016 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:643: Client connected to IdM port (id 18)
134 | 08:57:35.018 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
135 | 08:57:35.021 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
136 | 08:57:35.050 | →enobeB PCAP frame→ TCP |  |  |  |
137 | 08:57:35.056 |  |  |  |  | →HTTP GET | IDMS-Endpoint
138 | 08:57:35.058 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
139 | 08:57:35.061 |  | ←enobeB PCAP frame← TCP |  |  |
140 | 08:57:35.067 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
141 | 08:57:35.071 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:511: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
142 | 08:57:35.072 |  |  |  |  | MMICmd: Please provide user credentials: username and password
143 | 08:57:35.073 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
144 | 08:57:35.130 | →enobeB PCAP frame→ TCP |  |  |  |
145 | 08:57:39.458 | →enobeB PCAP frame→ HTTPS: POST /idms/userauth HTTP/1.1 |  |  |  |
146 | 08:57:39.458 |  |  |  |  | →HTTP POST | IDMS-Endpoint
147 | 08:57:39.461 |  | ←enobeB PCAP frame← TCP |  |  |
148 | 08:57:39.472 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
149 | 08:57:39.475 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:516: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
150 | 08:57:39.479 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
151 | 08:57:39.530 | →enobeB PCAP frame→ TCP |  |  |  |
152 | 08:57:39.536 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:679: IdM port - Client closed the connection (id 18)
153 | 08:57:39.538 | →enobeB PCAP frame→ TCP |  |  |  |
154 | 08:57:39.541 |  | ←enobeB PCAP frame← TCP |  |  |
155 | 08:57:39.570 | →enobeB PCAP frame→ TCP |  |  |  |
156 | 08:57:40.330 | →enobeB PCAP frame→ TCP |  |  |  |
157 | 08:57:40.335 |  | ←enobeB PCAP frame← TCP |  |  |
158 | 08:57:40.370 | →enobeB PCAP frame→ TCP |  |  |  |
159 | 08:57:40.418 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
160 | 08:57:40.421 |  | ←enobeB PCAP frame← TCP |  |  |
161 | 08:57:40.422 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
162 | 08:57:40.450 | →enobeB PCAP frame→ TCP |  |  |  |
163 | 08:57:40.536 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:643: Client connected to IdM port (id 18)
164 | 08:57:40.538 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
165 | 08:57:40.541 |  | ←enobeB PCAP frame← TCP |  |  |
166 | 08:57:40.542 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
167 | 08:57:40.570 | →enobeB PCAP frame→ TCP |  |  |  |
168 | 08:57:40.577 |  |  |  |  | →HTTP POST | IDMS-Endpoint
169 | 08:57:40.578 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
170 | 08:57:40.581 |  | ←enobeB PCAP frame← TCP |  |  |
171 | 08:57:40.615 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
172 | 08:57:40.616 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:521: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
173 | 08:57:40.621 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
174 | 08:57:40.690 | →enobeB PCAP frame→ TCP |  |  |  |
175 | 08:57:40.930 | →enobeB PCAP frame→ TCP |  |  |  |
176 | 08:57:40.933 |  | ←enobeB PCAP frame← TCP |  |  |
177 | 08:57:40.970 | →enobeB PCAP frame→ TCP |  |  |  |
178 | 08:57:40.978 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
179 | 08:57:40.981 |  | ←enobeB PCAP frame← TCP |  |  |
180 | 08:57:40.984 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
181 | 08:57:41.010 | →enobeB PCAP frame→ TCP |  |  |  |
182 | 08:57:41.017 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 19)
183 | 08:57:41.018 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
184 | 08:57:41.021 |  | ←enobeB PCAP frame← TCP |  |  |
185 | 08:57:41.022 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
186 | 08:57:41.058 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
187 | 08:57:41.058 |  |  |  |  | →HTTP POST | HTTP-Proxy
188 | 08:57:41.062 |  | ←enobeB PCAP frame← TCP |  |  |
189 | 08:57:41.082 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:541: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
190 | 08:57:41.088 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
191 | 08:57:41.096 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
192 | 08:57:41.130 | →enobeB PCAP frame→ TCP |  |  |  |
193 | 08:57:41.133 |  | ←enobeB PCAP frame← TCP |  |  |
194 | 08:57:41.170 | →enobeB PCAP frame→ TCP |  |  |  |
195 | 08:57:41.178 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
196 | 08:57:41.181 |  | ←enobeB PCAP frame← TCP |  |  |
197 | 08:57:41.185 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
198 | 08:57:41.210 | →enobeB PCAP frame→ TCP |  |  |  |
199 | 08:57:41.216 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 20)
200 | 08:57:41.218 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
201 | 08:57:41.221 |  | ←enobeB PCAP frame← TCP |  |  |
202 | 08:57:41.222 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
203 | 08:57:41.258 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
204 | 08:57:41.258 |  |  |  |  | →HTTP POST | HTTP-Proxy
205 | 08:57:41.261 |  | ←enobeB PCAP frame← TCP |  |  |
206 | 08:57:41.262 |  | ←enobeB PCAP frame← TCP |  |  |
207 | 08:57:41.298 | →enobeB PCAP frame→ TCP |  |  |  |
208 | 08:57:41.301 |  | ←enobeB PCAP frame← TCP |  |  |
209 | 08:57:41.319 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
210 | 08:57:41.319 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:545: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
211 | 08:57:41.326 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
212 | 08:57:41.370 | →enobeB PCAP frame→ TCP |  |  |  |
213 | 08:57:41.418 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
214 | 08:57:41.418 |  |  |  |  | →SIP REGISTER | P-CSCF
215 | 08:57:41.442 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:816: IMS UDP_s port 192.168.2.3:5062 configured
216 | 08:57:41.464 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:767: IMS TCP_s port 192.168.2.3:5062 configured!
217 | 08:57:41.465 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:825: IMS UDP_c port 192.168.2.3:5061 configured
218 | 08:57:41.470 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
219 | 08:57:42.178 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
220 | 08:57:42.179 |  |  |  |  | →SIP REGISTER | P-CSCF
221 | 08:57:42.204 |  |  |  |  | ←SIP 200 OK | P-CSCF
222 | 08:57:42.211 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
223 | 08:57:42.538 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
224 | 08:57:42.539 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
225 | 08:57:42.540 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 SIP over IPSEC: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 |  |  |  |
226 | 08:57:42.550 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
227 | 08:57:42.606 |  |  |  |  | ←SIP 200 OK | P-CSCF
228 | 08:57:42.606 |  |  |  |  | MIKEY | Media-Server
229 | 08:57:42.612 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
230 | 08:57:42.830 |  |  |  |  | XML→ | Media-Server
231 | 08:57:42.831 |  |  |  |  | XML→ | Media-Server
232 | 08:57:42.835 |  |  |  |  | ←XML | Media-Server
233 | 08:57:42.838 |  |  |  |  | ←SIP NOTIFY | P-CSCF
234 | 08:57:42.845 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:47081;transp... |  |  |
235 | 08:57:42.895 |  |  |  |  | →SIP 200 OK | P-CSCF
236 | 08:57:42.898 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
237 | 08:57:43.170 | →enobeB PCAP frame→ TCP |  |  |  |
238 | 08:57:43.175 |  | ←enobeB PCAP frame← TCP |  |  |
239 | 08:57:43.210 | →enobeB PCAP frame→ TCP |  |  |  |
240 | 08:57:43.218 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
241 | 08:57:43.221 |  | ←enobeB PCAP frame← TCP |  |  |
242 | 08:57:43.225 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
243 | 08:57:43.250 | →enobeB PCAP frame→ TCP |  |  |  |
244 | 08:57:43.377 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
245 | 08:57:43.378 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
246 | 08:57:43.382 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
247 | 08:57:43.410 | →enobeB PCAP frame→ TCP |  |  |  |
248 | 08:57:43.417 |  |  |  |  | →HTTP GET | HTTP-Proxy
249 | 08:57:43.418 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-co... |  |  |  |
250 | 08:57:43.421 |  | ←enobeB PCAP frame← TCP |  |  |
251 | 08:57:43.426 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:642: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcptt-ue-configuration.xml
252 | 08:57:43.435 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
253 | 08:57:43.442 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
254 | 08:57:43.488 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:674: Http Proxy port - Client closed the connection (id 25)
255 | 08:57:43.490 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
256 | 08:57:43.493 |  | ←enobeB PCAP frame← TCP |  |  |
257 | 08:57:43.498 | →enobeB PCAP frame→ TCP |  |  |  |
258 | 08:57:43.502 |  | ←enobeB PCAP frame← TCP |  |  |
259 | 08:57:43.530 | →enobeB PCAP frame→ TCP |  |  |  |
260 | 08:57:43.690 | →enobeB PCAP frame→ TCP |  |  |  |
261 | 08:57:43.693 |  | ←enobeB PCAP frame← TCP |  |  |
262 | 08:57:43.730 | →enobeB PCAP frame→ TCP |  |  |  |
263 | 08:57:43.738 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
264 | 08:57:43.741 |  | ←enobeB PCAP frame← TCP |  |  |
265 | 08:57:43.744 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
266 | 08:57:43.770 | →enobeB PCAP frame→ TCP |  |  |  |
267 | 08:57:43.857 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
268 | 08:57:43.858 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
269 | 08:57:43.861 |  | ←enobeB PCAP frame← TCP |  |  |
270 | 08:57:43.862 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
271 | 08:57:43.890 | →enobeB PCAP frame→ TCP |  |  |  |
272 | 08:57:43.896 |  |  |  |  | →HTTP GET | HTTP-Proxy
273 | 08:57:43.898 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-... |  |  |  |
274 | 08:57:43.901 |  | ←enobeB PCAP frame← TCP |  |  |
275 | 08:57:43.908 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:647: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcptt-user-profile-49.xml
276 | 08:57:43.947 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
277 | 08:57:43.957 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
278 | 08:57:43.958 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
279 | 08:57:43.970 | →enobeB PCAP frame→ TCP |  |  |  |
280 | 08:57:43.978 | →enobeB PCAP frame→ TCP |  |  |  |
281 | 08:57:44.008 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:674: Http Proxy port - Client closed the connection (id 25)
282 | 08:57:44.010 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
283 | 08:57:44.013 |  | ←enobeB PCAP frame← TCP |  |  |
284 | 08:57:44.014 |  | ←enobeB PCAP frame← TCP |  |  |
285 | 08:57:44.018 | →enobeB PCAP frame→ TCP |  |  |  |
286 | 08:57:44.021 |  | ←enobeB PCAP frame← TCP |  |  |
287 | 08:57:44.050 | →enobeB PCAP frame→ TCP |  |  |  |
288 | 08:57:44.658 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
289 | 08:57:44.659 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
290 | 08:57:44.669 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
291 | 08:57:44.726 |  |  |  |  | ←SIP 200 OK | P-CSCF
292 | 08:57:44.727 |  |  |  |  | MIKEY | Media-Server
293 | 08:57:44.734 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
294 | 08:57:44.770 | →enobeB PCAP frame→ TCP |  |  |  |
295 | 08:57:44.773 |  | ←enobeB PCAP frame← TCP |  |  |
296 | 08:57:44.810 | →enobeB PCAP frame→ TCP |  |  |  |
297 | 08:57:44.818 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
298 | 08:57:44.821 |  | ←enobeB PCAP frame← TCP |  |  |
299 | 08:57:44.822 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
300 | 08:57:44.850 | →enobeB PCAP frame→ TCP |  |  |  |
301 | 08:57:44.935 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
302 | 08:57:44.938 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
303 | 08:57:44.941 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
304 | 08:57:44.954 |  |  |  |  | XML→ | Media-Server
305 | 08:57:44.955 |  |  |  |  | XML→ | Media-Server
306 | 08:57:44.958 |  |  |  |  | ←XML | Media-Server
307 | 08:57:44.961 |  |  |  |  | ←SIP NOTIFY | P-CSCF
308 | 08:57:44.967 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:47081;transp... |  |  |
309 | 08:57:44.970 | →enobeB PCAP frame→ TCP |  |  |  |
310 | 08:57:44.975 |  |  |  |  | →HTTP GET | HTTP-Proxy
311 | 08:57:44.978 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.servi... |  |  |  |
312 | 08:57:44.978 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:652: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
313 | 08:57:44.981 |  | ←enobeB PCAP frame← TCP |  |  |
314 | 08:57:44.983 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
315 | 08:57:44.990 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
316 | 08:57:45.010 | →enobeB PCAP frame→ TCP |  |  |  |
317 | 08:57:45.017 |  |  |  |  | →SIP 200 OK | P-CSCF
318 | 08:57:45.018 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
319 | 08:57:45.088 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:674: Http Proxy port - Client closed the connection (id 25)
320 | 08:57:45.090 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
321 | 08:57:45.093 |  | ←enobeB PCAP frame← TCP |  |  |
322 | 08:57:45.130 | →enobeB PCAP frame→ TCP |  |  |  |
323 | 08:57:45.138 | →enobeB PCAP frame→ TCP |  |  |  |
324 | 08:57:45.141 |  | ←enobeB PCAP frame← TCP |  |  |
325 | 08:57:45.170 | →enobeB PCAP frame→ TCP |  |  |  |
326 | 08:57:45.178 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
327 | 08:57:45.181 |  | ←enobeB PCAP frame← TCP |  |  |
328 | 08:57:45.185 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
329 | 08:57:45.210 | →enobeB PCAP frame→ TCP |  |  |  |
330 | 08:57:45.336 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
331 | 08:57:45.338 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
332 | 08:57:45.341 |  | ←enobeB PCAP frame← TCP |  |  |
333 | 08:57:45.342 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
334 | 08:57:45.370 | →enobeB PCAP frame→ TCP |  |  |  |
335 | 08:57:45.417 |  |  |  |  | →HTTP GET | HTTP-Proxy
336 | 08:57:45.418 | →enobeB PCAP frame→ HTTPS: GET /xcap.gms.mcstaasting.com/org.openmobileallian... |  |  |  |
337 | 08:57:45.421 |  | ←enobeB PCAP frame← TCP |  |  |
338 | 08:57:45.428 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:657: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at /xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
339 | 08:57:45.455 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
340 | 08:57:45.465 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
341 | 08:57:45.490 | →enobeB PCAP frame→ TCP |  |  |  |
342 | 08:57:45.498 | →enobeB PCAP frame→ TCP |  |  |  |
343 | 08:57:45.568 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:674: Http Proxy port - Client closed the connection (id 25)
344 | 08:57:45.570 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
345 | 08:57:45.573 |  | ←enobeB PCAP frame← TCP |  |  |
346 | 08:57:45.578 | →enobeB PCAP frame→ TCP |  |  |  |
347 | 08:57:45.581 |  | ←enobeB PCAP frame← TCP |  |  |
348 | 08:57:45.610 | →enobeB PCAP frame→ TCP |  |  |  |
349 | 08:57:45.698 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
350 | 08:57:45.699 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
351 | 08:57:45.708 |  |  |  |  | →SIP PUBLISH | P-CSCF
352 | 08:57:45.759 |  |  |  |  | MIKEY | Media-Server
353 | 08:57:45.778 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
354 | 08:57:45.779 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
355 | 08:57:45.780 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
356 | 08:57:45.782 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
357 | 08:57:45.991 |  |  |  |  | XML→ | Media-Server
358 | 08:57:45.994 |  |  |  |  | ←SIP 200 OK | P-CSCF
359 | 08:57:45.997 |  |  |  |  | ←SIP 200 OK | P-CSCF
360 | 08:57:45.998 |  |  |  |  | MIKEY | Media-Server
361 | 08:57:46.000 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
362 | 08:57:46.004 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
363 | 08:57:46.211 |  |  |  |  | XML→ | Media-Server
364 | 08:57:46.212 |  |  |  |  | XML→ | Media-Server
365 | 08:57:46.247 |  |  |  |  | ←XML | Media-Server
366 | 08:57:46.251 |  |  |  |  | ←SIP NOTIFY | P-CSCF
367 | 08:57:46.258 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:47081;transp... |  |  |
368 | 08:57:46.296 |  |  |  |  | →SIP 200 OK | P-CSCF
369 | 08:57:46.298 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
370 | 08:57:46.298 |  |  |  |  | ←XML | Media-Server
371 | 08:57:46.306 |  |  |  |  | ←SIP MESSAGE | P-CSCF
372 | 08:57:46.313 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
373 | 08:57:47.137 |  |  |  |  | →SIP 200 OK | P-CSCF
374 | 08:57:47.138 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
375 | 08:57:47.144 |  |  |  |  | Info: MCX_IMS_CommonProcedures.ttcn:155: MESSAGE/200OK Table 5.3.2.3-2 Steps 7-8 Done
376 | 08:57:47.151 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
377 | 08:57:47.170 | →enobeB PCAP frame→ TCP |  |  |  |
378 | 08:57:47.210 | →enobeB PCAP frame→ TCP |  |  |  |
379 | 08:57:49.147 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
380 | 08:57:49.186 |  | ←RRC DCCH RRC Connection Release |  |  |
381 | 08:57:49.187 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
382 | 08:57:49.202 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
383 | 08:57:49.215 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:737: SRTP config: Master Key: C5EBD6FFBDE153F13A767E6A7EFAE5DA, Master Salt: 51E389D645FFF5CC52191C71, MKI: 25D6E9E8
384 | 08:57:49.216 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
385 | 08:57:49.218 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
386 | 08:57:49.221 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
387 | 08:57:49.237 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
388 | 08:57:49.237 |  |  |  |  | ←XML | Media-Server
389 | 08:57:49.277 |  |  |  |  | ←SIP INVITE | P-CSCF
390 | 08:57:50.137 |  | ←enobeB PCAP frame← LTE RRC PCCH Paging (1 PagingRecord) |  |  |
391 | 08:57:50.137 |  | ←RRC PCCH Paging |  |  |
392 | 08:57:50.177 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
393 | 08:57:50.177 |  | →RRC CCCH RRC Connection Request |  |  |
394 | 08:57:50.177 |  | ←RRC CCCH RRC Connection Setup |  |  |
395 | 08:57:50.177 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
396 | 08:57:50.210 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
397 | 08:57:50.210 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
398 | 08:57:50.210 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
399 | 08:57:50.210 |  |  |  | →NAS EMM Service request |  |
400 | 08:57:50.210 |  |  |  | NAS K-enb 9d74f20afeaf1471814fdf682817141e2... |  |
401 | 08:57:50.211 |  |  | RRC K-enb 9d74f20afeaf1471814fdf682817141e2... |  |  |
402 | 08:57:50.212 |  |  | RRC rrc-cip 2e9c5c3b5469d2713fc3220e56c5f6a... |  |  |
403 | 08:57:50.212 |  |  | RRC rrc-int f3e8874779ef3d28391e384096e3388... |  |  |
404 | 08:57:50.212 |  |  | RRC up-cip c89d7481aafa16710669464a3d876ee3... |  |  |
405 | 08:57:50.212 |  |  | RRC up-int 9790d19a68d2dd6fb6479369283f3285... |  |  |
406 | 08:57:50.212 |  | ←RRC DCCH Security Mode Command |  |  |
407 | 08:57:50.212 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
408 | 08:57:50.250 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
409 | 08:57:50.250 |  | →RRC DCCH Security Mode Complete |  |  |
410 | 08:57:50.250 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
411 | 08:57:50.250 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
412 | 08:57:50.290 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
413 | 08:57:50.290 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
414 | 08:57:50.292 |  | ←enobeB PCAP frame← SIP over IPSEC: INVITE sip:PublicUserId-A@192.168.3.2:47081;transp... |  |  |
415 | 08:57:50.337 |  |  |  |  | →SIP 100 Trying | P-CSCF
416 | 08:57:50.338 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 100 Trying |  |  |  |
417 | 08:57:50.418 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
418 | 08:57:50.422 |  |  |  |  | →SIP 200 OK | P-CSCF
419 | 08:57:50.456 |  |  |  |  | XML→ | Media-Server
420 | 08:57:50.463 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:612: 200 OK Verdict: Pass
421 | 08:57:50.464 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:512: Step 1 Verdict: Pass
422 | 08:57:50.467 |  |  |  |  | ←SIP ACK | P-CSCF
423 | 08:57:50.468 |  |  |  |  | ←Floor Taken | Media-Server
424 | 08:57:50.473 |  | ←enobeB PCAP frame← SIP over IPSEC: ACK sip:PublicUserId-A@192.168.3.2:47081;transport... |  |  |
425 | 08:57:50.705 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
426 | 08:57:50.705 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x3) |  |  |
427 | 08:57:50.705 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
428 | 08:57:50.706 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
429 | 08:57:50.730 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
430 | 08:57:50.730 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
431 | 08:57:50.770 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
432 | 08:57:50.770 |  | →RRC DCCH UL Information Transfer |  |  |
433 | 08:57:50.770 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xc) |  |  |
434 | 08:57:50.770 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
435 | 08:57:50.808 |  |  |  |  | Floor ACK→ | Media-Server
436 | 08:57:50.810 | →enobeB PCAP frame→ |  |  |  |
437 | 08:57:50.811 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
438 | 08:57:50.819 |  |  |  |  | ←SIP BYE | P-CSCF
439 | 08:57:50.824 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
440 | 08:57:50.826 |  | ←enobeB PCAP frame← SIP over IPSEC: BYE sip:PublicUserId-A@192.168.3.2:47081;transport... |  |  |
441 | 08:57:50.858 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
442 | 08:57:50.858 |  |  |  |  | →SIP 200 OK | P-CSCF
443 | 08:57:52.010 | →enobeB PCAP frame→ |  |  |  |
444 | 08:57:52.866 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
445 | 08:57:52.881 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
446 | 08:57:52.882 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xb) |  |  |
447 | 08:57:52.882 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
448 | 08:57:52.883 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
449 | 08:57:52.930 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
450 | 08:57:52.930 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
451 | 08:57:52.930 |  | →RRC DCCH UL Information Transfer |  |  |
452 | 08:57:52.930 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xa) |  |  |
453 | 08:57:52.930 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
454 | 08:57:52.991 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
455 | 08:57:52.992 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
456 | 08:57:53.031 |  | ←RRC DCCH RRC Connection Release |  |  |
457 | 08:57:53.032 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
458 | 08:57:53.046 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
459 | 08:57:53.049 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
460 | 08:57:53.051 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
461 | 08:57:53.798 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.