ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 09:11:09.656 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 09:11:09.659 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 09:11:09.660 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 09:11:09.661 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 09:11:09.662 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 09:11:09.662 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:805: IMS UDP port 192.168.2.3:5060 configured
7 | 09:11:09.664 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:755: IMS TCP port 192.168.2.3:5060 configured!
8 | 09:11:09.665 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:776: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 09:11:09.666 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:787: IdM port 192.168.2.3:8080 configured!
10 | 09:11:09.667 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 09:11:10.869 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 09:11:10.871 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 09:11:13.062 |  | ←RRC BCCH SIB |  |  |
14 | 09:11:13.067 |  | ←RRC BCCH SIB1 |  |  |
15 | 09:11:13.147 |  | ←RRC BCCH SIB1 |  |  |
16 | 09:11:13.222 |  | ←RRC BCCH SIB |  |  |
17 | 09:11:13.227 |  | ←RRC BCCH SIB1 |  |  |
18 | 09:12:46.071 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 09:12:46.071 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 09:12:46.071 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 09:12:46.071 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 09:12:46.122 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 09:12:46.122 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 09:12:46.122 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 09:12:46.122 |  |  |  | →NAS EMM Attach request |  |
26 | 09:12:46.122 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 09:12:46.122 |  |  |  | NAS K-asme fe3ac53313e00eef68107a0ea5724302... |  |
28 | 09:12:46.122 |  |  |  | NAS ← EMM Authentication request |  |
29 | 09:12:46.123 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 09:12:46.123 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 09:12:46.124 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 09:12:46.194 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 09:12:46.194 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 09:12:46.194 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 09:12:46.194 |  |  |  | →NAS EMM Authentication response |  |
36 | 09:12:46.194 |  |  |  | NAS UE auth OK |  |
37 | 09:12:46.194 |  |  |  | NAS K-nas-cip e07b438126bc031abd45f6d75d94a... |  |
38 | 09:12:46.194 |  |  |  | NAS K-nas-int 1a8f328c72cb025a0d3eaf01fa119... |  |
39 | 09:12:46.194 |  |  |  | NAS ← EMM Security mode command |  |
40 | 09:12:46.195 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 09:12:46.195 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 09:12:46.196 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 09:12:46.234 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
44 | 09:12:46.234 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 09:12:46.234 |  | [EMBEDDED NAS IN PREV RRC] TP Unknown message (type=0x6b) |  |  |
46 | 09:12:46.234 |  |  |  | →NAS EMM Security mode complete |  |
47 | 09:12:46.234 |  |  |  | NAS ← ESM ESM information request |  |
48 | 09:12:46.235 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x8) |  |  |
49 | 09:12:46.235 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 09:12:46.236 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Ciphered message |  |  |
51 | 09:12:46.282 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
52 | 09:12:46.282 |  | →RRC DCCH UL Information Transfer |  |  |
53 | 09:12:46.282 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xc) |  |  |
54 | 09:12:46.282 |  |  |  | →NAS ESM ESM information response |  |
55 | 09:12:46.282 |  |  |  | NAS K-enb 4f3e5e6fd2a809f48d1b539e55cee3288... |  |
56 | 09:12:46.282 |  |  |  | NAS ← EMM Attach accept |  |
57 | 09:12:46.283 |  | ←RRC DCCH Security Mode Command |  |  |
58 | 09:12:46.283 |  |  | RRC K-enb 4f3e5e6fd2a809f48d1b539e55cee3288... |  |  |
59 | 09:12:46.283 |  |  | RRC rrc-cip 79f0527b98192523ed94534a8935133... |  |  |
60 | 09:12:46.283 |  |  | RRC rrc-int a36671d267804a01f36dfc190d65af7... |  |  |
61 | 09:12:46.283 |  |  | RRC up-cip e23ac75c58b8c6876ba6c491aca6b057... |  |  |
62 | 09:12:46.283 |  |  | RRC up-int 38e0b728b1696e8c74fff830fd56be39... |  |  |
63 | 09:12:46.284 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
64 | 09:12:46.314 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
65 | 09:12:46.314 |  | →RRC DCCH Security Mode Complete |  |  |
66 | 09:12:46.314 |  | ←RRC DCCH UE Capability Enquiry |  |  |
67 | 09:12:46.314 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
68 | 09:12:46.364 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
69 | 09:12:46.364 |  | →RRC DCCH UE Capability Information |  |  |
70 | 09:12:46.365 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xd) |  |  |
71 | 09:12:46.365 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
72 | 09:12:46.365 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
73 | 09:12:46.394 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
74 | 09:12:46.394 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
75 | 09:12:46.434 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
76 | 09:12:46.434 |  | →RRC DCCH UL Information Transfer |  |  |
77 | 09:12:46.434 |  | [EMBEDDED NAS IN PREV RRC] Message too short (len=13) |  |  |
78 | 09:12:46.434 |  |  |  | →NAS EMM Attach complete |  |
79 | 09:12:46.434 |  |  |  | NAS ← EMM EMM information |  |
80 | 09:12:46.435 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x6) |  |  |
81 | 09:12:46.435 |  | ←RRC DCCH DL Information Transfer |  |  |
82 | 09:12:46.436 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Ciphered message |  |  |
83 | 09:12:53.151 |  | ←RRC DCCH RRC Connection Release |  |  |
84 | 09:12:53.152 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
85 | 09:12:54.851 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
86 | 09:12:54.851 |  | →RRC CCCH RRC Connection Request |  |  |
87 | 09:12:54.851 |  | ←RRC CCCH RRC Connection Setup |  |  |
88 | 09:12:54.851 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
89 | 09:12:54.914 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
90 | 09:12:54.914 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
91 | 09:12:54.914 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
92 | 09:12:54.914 |  |  |  | →NAS EMM Service request |  |
93 | 09:12:54.914 |  |  |  | NAS K-enb 22f67ac472009ce1335cc70e2aa0387c4... |  |
94 | 09:12:54.915 |  |  | RRC K-enb 22f67ac472009ce1335cc70e2aa0387c4... |  |  |
95 | 09:12:54.916 |  |  | RRC rrc-cip b36f799e9647072391b45913c91aa4b... |  |  |
96 | 09:12:54.916 |  |  | RRC rrc-int 4c2cdd331d36ed1da5a61f7d7b0abf0... |  |  |
97 | 09:12:54.916 |  |  | RRC up-cip 698f0a74820c695860d7cdfe48a684e4... |  |  |
98 | 09:12:54.916 |  |  | RRC up-int 1fefd84bbeabb993b92b1f7d366bccda... |  |  |
99 | 09:12:54.916 |  | ←RRC DCCH Security Mode Command |  |  |
100 | 09:12:54.916 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
101 | 09:12:54.954 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
102 | 09:12:54.954 |  | →RRC DCCH Security Mode Complete |  |  |
103 | 09:12:54.954 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
104 | 09:12:54.954 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
105 | 09:12:54.994 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
106 | 09:12:54.994 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
107 | 09:13:09.114 | →enobeB PCAP frame→ TCP |  |  |  |
108 | 09:13:09.117 |  | ←enobeB PCAP frame← TCP |  |  |
109 | 09:13:09.154 | →enobeB PCAP frame→ TCP |  |  |  |
110 | 09:13:09.202 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
111 | 09:13:09.205 |  | ←enobeB PCAP frame← TCP |  |  |
112 | 09:13:09.210 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
113 | 09:13:09.234 | →enobeB PCAP frame→ TCP |  |  |  |
114 | 09:13:09.365 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 16)
115 | 09:13:09.370 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
116 | 09:13:09.373 |  | ←enobeB PCAP frame← TCP |  |  |
117 | 09:13:09.374 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
118 | 09:13:09.434 | →enobeB PCAP frame→ TCP |  |  |  |
119 | 09:13:09.438 |  |  |  |  | →HTTP GET | HTTP-Proxy
120 | 09:13:09.442 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
121 | 09:13:09.444 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:288: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
122 | 09:13:09.445 |  | ←enobeB PCAP frame← TCP |  |  |
123 | 09:13:09.463 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
124 | 09:13:09.474 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
125 | 09:13:09.514 | →enobeB PCAP frame→ TCP |  |  |  |
126 | 09:13:11.074 | →enobeB PCAP frame→ TCP |  |  |  |
127 | 09:13:11.077 |  | ←enobeB PCAP frame← TCP |  |  |
128 | 09:13:11.114 | →enobeB PCAP frame→ TCP |  |  |  |
129 | 09:13:11.122 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
130 | 09:13:11.125 |  | ←enobeB PCAP frame← TCP |  |  |
131 | 09:13:11.130 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
132 | 09:13:11.194 | →enobeB PCAP frame→ TCP |  |  |  |
133 | 09:13:11.437 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:642: Client connected to IdM port (id 18)
134 | 09:13:11.442 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
135 | 09:13:11.445 |  | ←enobeB PCAP frame← TCP |  |  |
136 | 09:13:11.446 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
137 | 09:13:11.474 | →enobeB PCAP frame→ TCP |  |  |  |
138 | 09:13:11.517 |  |  |  |  | →HTTP GET | IDMS-Endpoint
139 | 09:13:11.522 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
140 | 09:13:11.525 |  | ←enobeB PCAP frame← TCP |  |  |
141 | 09:13:11.529 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
142 | 09:13:11.533 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:511: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
143 | 09:13:11.533 |  |  |  |  | MMICmd: Please provide user credentials: username and password
144 | 09:13:11.537 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
145 | 09:13:11.562 | →enobeB PCAP frame→ TCP |  |  |  |
146 | 09:13:11.565 |  | ←enobeB PCAP frame← TCP |  |  |
147 | 09:13:11.634 | →enobeB PCAP frame→ TCP |  |  |  |
148 | 09:13:16.119 |  |  |  |  | →HTTP POST | IDMS-Endpoint
149 | 09:13:16.122 | →enobeB PCAP frame→ HTTPS: POST /idms/userauth HTTP/1.1 |  |  |  |
150 | 09:13:16.125 |  | ←enobeB PCAP frame← TCP |  |  |
151 | 09:13:16.134 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
152 | 09:13:16.136 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:516: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
153 | 09:13:16.143 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
154 | 09:13:16.194 | →enobeB PCAP frame→ TCP |  |  |  |
155 | 09:13:16.197 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:677: IdM port - Client closed the connection (id 18)
156 | 09:13:16.202 | →enobeB PCAP frame→ TCP |  |  |  |
157 | 09:13:16.205 |  | ←enobeB PCAP frame← TCP |  |  |
158 | 09:13:16.234 | →enobeB PCAP frame→ TCP |  |  |  |
159 | 09:13:16.925 |  | ←enobeB PCAP frame← TCP |  |  |
160 | 09:13:17.005 |  | ←enobeB PCAP frame← TCP |  |  |
161 | 09:13:17.008 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
162 | 09:13:17.034 | →enobeB PCAP frame→ TCP |  |  |  |
163 | 09:13:17.122 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
164 | 09:13:17.123 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:642: Client connected to IdM port (id 18)
165 | 09:13:17.125 |  | ←enobeB PCAP frame← TCP |  |  |
166 | 09:13:17.126 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
167 | 09:13:17.154 | →enobeB PCAP frame→ TCP |  |  |  |
168 | 09:13:17.197 |  |  |  |  | →HTTP POST | IDMS-Endpoint
169 | 09:13:17.202 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
170 | 09:13:17.205 |  | ←enobeB PCAP frame← TCP |  |  |
171 | 09:13:17.223 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
172 | 09:13:17.225 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:521: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
173 | 09:13:17.232 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
174 | 09:13:17.314 | →enobeB PCAP frame→ TCP |  |  |  |
175 | 09:13:17.554 | →enobeB PCAP frame→ TCP |  |  |  |
176 | 09:13:17.557 |  | ←enobeB PCAP frame← TCP |  |  |
177 | 09:13:17.594 | →enobeB PCAP frame→ TCP |  |  |  |
178 | 09:13:17.602 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
179 | 09:13:17.605 |  | ←enobeB PCAP frame← TCP |  |  |
180 | 09:13:17.609 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
181 | 09:13:17.634 | →enobeB PCAP frame→ TCP |  |  |  |
182 | 09:13:17.678 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 19)
183 | 09:13:17.682 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
184 | 09:13:17.685 |  | ←enobeB PCAP frame← TCP |  |  |
185 | 09:13:17.686 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
186 | 09:13:17.719 |  |  |  |  | →HTTP POST | HTTP-Proxy
187 | 09:13:17.722 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
188 | 09:13:17.725 |  | ←enobeB PCAP frame← TCP |  |  |
189 | 09:13:17.742 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:541: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
190 | 09:13:17.749 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
191 | 09:13:17.759 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
192 | 09:13:17.794 | →enobeB PCAP frame→ TCP |  |  |  |
193 | 09:13:17.834 | →enobeB PCAP frame→ TCP |  |  |  |
194 | 09:13:17.837 |  | ←enobeB PCAP frame← TCP |  |  |
195 | 09:13:17.874 | →enobeB PCAP frame→ TCP |  |  |  |
196 | 09:13:17.882 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
197 | 09:13:17.885 |  | ←enobeB PCAP frame← TCP |  |  |
198 | 09:13:17.888 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
199 | 09:13:17.926 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 20)
200 | 09:13:17.933 |  | ←enobeB PCAP frame← TCP |  |  |
201 | 09:13:17.934 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
202 | 09:13:17.999 |  |  |  |  | →HTTP POST | HTTP-Proxy
203 | 09:13:18.002 | →enobeB PCAP frame→ TCP |  |  |  |
204 | 09:13:18.005 |  | ←enobeB PCAP frame← TCP |  |  |
205 | 09:13:18.006 |  | ←enobeB PCAP frame← TCP |  |  |
206 | 09:13:18.065 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
207 | 09:13:18.065 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:545: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
208 | 09:13:18.074 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
209 | 09:13:18.114 | →enobeB PCAP frame→ TCP |  |  |  |
210 | 09:13:18.159 |  |  |  |  | →SIP REGISTER | P-CSCF
211 | 09:13:18.162 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
212 | 09:13:18.182 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:814: IMS UDP_s port 192.168.2.3:5062 configured
213 | 09:13:18.209 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:765: IMS TCP_s port 192.168.2.3:5062 configured!
214 | 09:13:18.212 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:823: IMS UDP_c port 192.168.2.3:5061 configured
215 | 09:13:18.222 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
216 | 09:13:18.961 |  |  |  |  | →SIP REGISTER | P-CSCF
217 | 09:13:18.973 |  |  |  |  | ←SIP 200 OK | P-CSCF
218 | 09:13:18.982 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
219 | 09:13:19.323 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
220 | 09:13:19.324 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
221 | 09:13:19.331 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
222 | 09:13:19.349 |  |  |  |  | ←SIP 200 OK | P-CSCF
223 | 09:13:19.349 |  |  |  |  | MIKEY | Media-Server
224 | 09:13:19.358 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
225 | 09:13:19.558 |  |  |  |  | XML→ | Media-Server
226 | 09:13:19.559 |  |  |  |  | XML→ | Media-Server
227 | 09:13:19.562 |  |  |  |  | ←XML | Media-Server
228 | 09:13:19.565 |  |  |  |  | ←SIP NOTIFY | P-CSCF
229 | 09:13:19.575 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:49154;transp... |  |  |
230 | 09:13:19.597 |  |  |  |  | →SIP 200 OK | P-CSCF
231 | 09:13:19.602 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
232 | 09:13:19.954 | →enobeB PCAP frame→ TCP |  |  |  |
233 | 09:13:19.957 |  | ←enobeB PCAP frame← TCP |  |  |
234 | 09:13:19.994 | →enobeB PCAP frame→ TCP |  |  |  |
235 | 09:13:20.002 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
236 | 09:13:20.005 |  | ←enobeB PCAP frame← TCP |  |  |
237 | 09:13:20.009 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
238 | 09:13:20.034 | →enobeB PCAP frame→ TCP |  |  |  |
239 | 09:13:20.078 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
240 | 09:13:20.082 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
241 | 09:13:20.085 |  | ←enobeB PCAP frame← TCP |  |  |
242 | 09:13:20.086 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
243 | 09:13:20.114 | →enobeB PCAP frame→ TCP |  |  |  |
244 | 09:13:20.118 |  |  |  |  | →HTTP GET | HTTP-Proxy
245 | 09:13:20.122 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-co... |  |  |  |
246 | 09:13:20.125 |  | ←enobeB PCAP frame← TCP |  |  |
247 | 09:13:20.126 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:642: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcptt-ue-configuration.xml
248 | 09:13:20.133 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
249 | 09:13:20.143 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
250 | 09:13:20.234 | →enobeB PCAP frame→ TCP |  |  |  |
251 | 09:13:20.237 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
252 | 09:13:20.242 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
253 | 09:13:20.245 |  | ←enobeB PCAP frame← TCP |  |  |
254 | 09:13:20.274 | →enobeB PCAP frame→ TCP |  |  |  |
255 | 09:13:20.394 | →enobeB PCAP frame→ TCP |  |  |  |
256 | 09:13:20.397 |  | ←enobeB PCAP frame← TCP |  |  |
257 | 09:13:20.434 | →enobeB PCAP frame→ TCP |  |  |  |
258 | 09:13:20.442 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
259 | 09:13:20.445 |  | ←enobeB PCAP frame← TCP |  |  |
260 | 09:13:20.448 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
261 | 09:13:20.474 | →enobeB PCAP frame→ TCP |  |  |  |
262 | 09:13:20.517 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
263 | 09:13:20.522 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
264 | 09:13:20.525 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
265 | 09:13:20.554 | →enobeB PCAP frame→ TCP |  |  |  |
266 | 09:13:20.557 |  |  |  |  | →HTTP GET | HTTP-Proxy
267 | 09:13:20.561 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:647: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcptt-user-profile-49.xml
268 | 09:13:20.562 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-... |  |  |  |
269 | 09:13:20.565 |  | ←enobeB PCAP frame← TCP |  |  |
270 | 09:13:20.578 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
271 | 09:13:20.589 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
272 | 09:13:20.590 |  | ←enobeB PCAP frame← TCP |  |  |
273 | 09:13:20.591 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
274 | 09:13:20.634 | →enobeB PCAP frame→ TCP |  |  |  |
275 | 09:13:20.637 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
276 | 09:13:20.642 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
277 | 09:13:20.645 |  | ←enobeB PCAP frame← TCP |  |  |
278 | 09:13:20.650 | →enobeB PCAP frame→ TCP |  |  |  |
279 | 09:13:20.653 |  | ←enobeB PCAP frame← TCP |  |  |
280 | 09:13:20.674 | →enobeB PCAP frame→ TCP |  |  |  |
281 | 09:13:21.322 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
282 | 09:13:21.323 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
283 | 09:13:21.428 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
284 | 09:13:21.434 | →enobeB PCAP frame→ TCP |  |  |  |
285 | 09:13:21.437 |  | ←enobeB PCAP frame← TCP |  |  |
286 | 09:13:21.454 |  |  |  |  | ←SIP 200 OK | P-CSCF
287 | 09:13:21.454 |  |  |  |  | MIKEY | Media-Server
288 | 09:13:21.462 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
289 | 09:13:21.474 | →enobeB PCAP frame→ TCP |  |  |  |
290 | 09:13:21.482 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
291 | 09:13:21.485 |  | ←enobeB PCAP frame← TCP |  |  |
292 | 09:13:21.486 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
293 | 09:13:21.514 | →enobeB PCAP frame→ TCP |  |  |  |
294 | 09:13:21.597 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
295 | 09:13:21.602 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
296 | 09:13:21.605 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
297 | 09:13:21.634 | →enobeB PCAP frame→ TCP |  |  |  |
298 | 09:13:21.637 |  |  |  |  | →HTTP GET | HTTP-Proxy
299 | 09:13:21.639 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:652: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
300 | 09:13:21.642 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.servi... |  |  |  |
301 | 09:13:21.645 |  | ←enobeB PCAP frame← TCP |  |  |
302 | 09:13:21.645 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
303 | 09:13:21.654 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
304 | 09:13:21.660 |  |  |  |  | XML→ | Media-Server
305 | 09:13:21.661 |  |  |  |  | XML→ | Media-Server
306 | 09:13:21.664 |  |  |  |  | ←XML | Media-Server
307 | 09:13:21.667 |  |  |  |  | ←SIP NOTIFY | P-CSCF
308 | 09:13:21.674 | →enobeB PCAP frame→ TCP |  |  |  |
309 | 09:13:21.676 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:49154;transp... |  |  |
310 | 09:13:21.682 | →enobeB PCAP frame→ TCP |  |  |  |
311 | 09:13:21.709 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
312 | 09:13:21.714 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
313 | 09:13:21.717 |  | ←enobeB PCAP frame← TCP |  |  |
314 | 09:13:21.717 |  |  |  |  | →SIP 200 OK | P-CSCF
315 | 09:13:21.722 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
316 | 09:13:21.726 |  | ←enobeB PCAP frame← TCP |  |  |
317 | 09:13:21.754 | →enobeB PCAP frame→ TCP |  |  |  |
318 | 09:13:21.794 | →enobeB PCAP frame→ TCP |  |  |  |
319 | 09:13:21.797 |  | ←enobeB PCAP frame← TCP |  |  |
320 | 09:13:21.834 | →enobeB PCAP frame→ TCP |  |  |  |
321 | 09:13:21.842 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
322 | 09:13:21.845 |  | ←enobeB PCAP frame← TCP |  |  |
323 | 09:13:21.848 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
324 | 09:13:21.874 | →enobeB PCAP frame→ TCP |  |  |  |
325 | 09:13:21.958 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
326 | 09:13:21.962 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
327 | 09:13:21.965 |  | ←enobeB PCAP frame← TCP |  |  |
328 | 09:13:21.966 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
329 | 09:13:21.994 | →enobeB PCAP frame→ TCP |  |  |  |
330 | 09:13:22.046 |  |  |  |  | →HTTP GET | HTTP-Proxy
331 | 09:13:22.053 |  | ←enobeB PCAP frame← TCP |  |  |
332 | 09:13:22.057 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:657: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at /xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
333 | 09:13:22.083 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
334 | 09:13:22.095 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
335 | 09:13:22.157 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
336 | 09:13:22.162 | →enobeB PCAP frame→ TCP |  |  |  |
337 | 09:13:22.165 |  | ←enobeB PCAP frame← TCP |  |  |
338 | 09:13:22.194 | →enobeB PCAP frame→ TCP |  |  |  |
339 | 09:13:22.322 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
340 | 09:13:22.323 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
341 | 09:13:22.329 |  |  |  |  | →SIP PUBLISH | P-CSCF
342 | 09:13:22.377 |  |  |  |  | MIKEY | Media-Server
343 | 09:13:22.402 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
344 | 09:13:22.402 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
345 | 09:13:22.403 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
346 | 09:13:22.404 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
347 | 09:13:22.607 |  |  |  |  | XML→ | Media-Server
348 | 09:13:22.611 |  |  |  |  | ←SIP 200 OK | P-CSCF
349 | 09:13:22.614 |  |  |  |  | ←SIP 200 OK | P-CSCF
350 | 09:13:22.614 |  |  |  |  | MIKEY | Media-Server
351 | 09:13:22.619 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
352 | 09:13:22.623 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
353 | 09:13:22.825 |  |  |  |  | XML→ | Media-Server
354 | 09:13:22.830 |  |  |  |  | XML→ | Media-Server
355 | 09:13:22.876 |  |  |  |  | ←XML | Media-Server
356 | 09:13:22.881 |  |  |  |  | ←SIP NOTIFY | P-CSCF
357 | 09:13:22.890 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:49154;transp... |  |  |
358 | 09:13:22.925 |  |  |  |  | →SIP 200 OK | P-CSCF
359 | 09:13:22.928 |  |  |  |  | ←XML | Media-Server
360 | 09:13:22.936 |  |  |  |  | ←SIP MESSAGE | P-CSCF
361 | 09:13:22.946 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
362 | 09:13:23.757 |  |  |  |  | →SIP 200 OK | P-CSCF
363 | 09:13:23.759 |  |  |  |  | Info: MCX_IMS_CommonProcedures.ttcn:155: MESSAGE/200OK Table 5.3.2.3-2 Steps 7-8 Done
364 | 09:13:23.768 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
365 | 09:13:23.794 | →enobeB PCAP frame→ TCP |  |  |  |
366 | 09:13:23.834 | →enobeB PCAP frame→ TCP |  |  |  |
367 | 09:13:25.761 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
368 | 09:13:25.803 |  | ←RRC DCCH RRC Connection Release |  |  |
369 | 09:13:25.804 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
370 | 09:13:25.816 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
371 | 09:13:25.818 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
372 | 09:13:25.819 |  |  |  |  | MMICmd: Make the MCPTT User request the establishment of an MCPTT On-demand imminent peril chat group call for the selected MCPTT imminent peril group GROUP A, with implicit floor control
373 | 09:13:32.241 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
374 | 09:13:32.241 |  | →RRC CCCH RRC Connection Request |  |  |
375 | 09:13:32.241 |  | ←RRC CCCH RRC Connection Setup |  |  |
376 | 09:13:32.241 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
377 | 09:13:32.274 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
378 | 09:13:32.274 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
379 | 09:13:32.274 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
380 | 09:13:32.274 |  |  |  | →NAS EMM Service request |  |
381 | 09:13:32.274 |  |  |  | NAS K-enb 3a703ce606a68457f0ff5360b03b7771b... |  |
382 | 09:13:32.275 |  |  | RRC K-enb 3a703ce606a68457f0ff5360b03b7771b... |  |  |
383 | 09:13:32.276 |  |  | RRC rrc-cip 999bac97383534854d95b15c88fca9f... |  |  |
384 | 09:13:32.276 |  |  | RRC rrc-int 6940f81ee610df6794beb65f53fbc9b... |  |  |
385 | 09:13:32.276 |  |  | RRC up-cip 259cfbf5851dc7f225c4afac715cb7a2... |  |  |
386 | 09:13:32.276 |  |  | RRC up-int 319f203ae96f330025d639019719f245... |  |  |
387 | 09:13:32.276 |  | ←RRC DCCH Security Mode Command |  |  |
388 | 09:13:32.276 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
389 | 09:13:32.314 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
390 | 09:13:32.314 |  | →RRC DCCH Security Mode Complete |  |  |
391 | 09:13:32.314 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
392 | 09:13:32.314 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
393 | 09:13:32.354 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
394 | 09:13:32.354 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
395 | 09:13:32.362 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
396 | 09:13:32.363 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
397 | 09:13:32.366 |  |  |  |  | →SIP INVITE | P-CSCF
398 | 09:13:32.388 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:735: SRTP config: Master Key: D148E42F0B0774DC139E2B5F3DEA9879, Master Salt: 104867C5D3706E002D795C85, MKI: 299D2D5F
399 | 09:13:32.388 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
400 | 09:13:32.392 |  |  |  |  | XML→ | Media-Server
401 | 09:13:32.393 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
402 | 09:13:32.394 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1205: INVITE Verdict: Pass
403 | 09:13:32.395 |  |  |  |  | ←SIP 100 Trying | P-CSCF
404 | 09:13:32.397 |  |  |  |  | ←SIP 200 OK | P-CSCF
405 | 09:13:32.404 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
406 | 09:13:32.406 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
407 | 09:13:33.055 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
408 | 09:13:33.056 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xae) |  |  |
409 | 09:13:33.056 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
410 | 09:13:33.057 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
411 | 09:13:33.074 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
412 | 09:13:33.074 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
413 | 09:13:33.114 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
414 | 09:13:33.114 |  | →RRC DCCH UL Information Transfer |  |  |
415 | 09:13:33.114 |  | [EMBEDDED NAS IN PREV RRC] TP Unknown message (type=0xd7) |  |  |
416 | 09:13:33.114 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
417 | 09:13:33.176 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
418 | 09:13:33.198 |  |  |  |  | →SIP ACK | P-CSCF
419 | 09:13:33.202 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
420 | 09:13:33.207 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1208: ACK Verdict: Pass
421 | 09:13:33.208 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:597: Step 2 Verdict: Pass
422 | 09:13:33.211 |  |  |  |  | ←Floor Granted | Media-Server
423 | 09:13:33.794 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
424 | 09:13:33.802 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
425 | 09:13:33.834 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
426 | 09:13:33.842 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
427 | 09:13:33.874 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
428 | 09:13:33.959 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCO_MCX_IMS.ttcn:602: Step 9 Verdict: Pass
429 | 09:13:34.063 |  |  |  |  | MMICmd: Release call (hang up the call)
430 | 09:13:36.319 |  |  |  |  | →SIP BYE | P-CSCF
431 | 09:13:36.330 |  |  |  |  | ←SIP 200 OK | P-CSCF
432 | 09:13:36.339 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
433 | 09:13:36.594 | →enobeB PCAP frame→ |  |  |  |
434 | 09:13:38.332 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
435 | 09:13:38.354 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
436 | 09:13:38.354 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x9) |  |  |
437 | 09:13:38.354 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
438 | 09:13:38.355 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
439 | 09:13:38.394 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
440 | 09:13:38.394 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
441 | 09:13:38.394 |  | →RRC DCCH UL Information Transfer |  |  |
442 | 09:13:38.394 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x4) |  |  |
443 | 09:13:38.394 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
444 | 09:13:38.471 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
445 | 09:13:38.472 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
446 | 09:13:38.546 |  | ←RRC DCCH RRC Connection Release |  |  |
447 | 09:13:38.547 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
448 | 09:13:38.550 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
449 | 09:13:38.553 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
450 | 09:13:38.554 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
451 | 09:13:39.302 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.