ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 13:44:27.482 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 13:44:27.486 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 13:44:27.486 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 13:44:27.488 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 13:44:27.489 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 13:44:27.490 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:824: IMS UDP port 192.168.2.3:5060 configured
7 | 13:44:27.495 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:774: IMS TCP port 192.168.2.3:5060 configured!
8 | 13:44:27.499 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:795: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 13:44:27.500 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:806: IdM port 192.168.2.3:8080 configured!
10 | 13:44:27.504 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 13:44:28.705 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 13:44:28.707 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 13:44:31.098 |  | ←RRC BCCH SIB1 |  |  |
14 | 13:44:31.173 |  | ←RRC BCCH SIB |  |  |
15 | 13:44:31.178 |  | ←RRC BCCH SIB1 |  |  |
16 | 13:44:31.193 |  | ←RRC BCCH SIB |  |  |
17 | 13:44:31.213 |  | ←RRC BCCH SIB |  |  |
18 | 13:45:48.042 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 13:45:48.042 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 13:45:48.042 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 13:45:48.042 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 13:45:48.073 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 13:45:48.073 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 13:45:48.073 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 13:45:48.073 |  |  |  | →NAS EMM Attach request |  |
26 | 13:45:48.073 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 13:45:48.074 |  |  |  | NAS K-asme ca0ee4f2c0a6488e691efcea246ad073... |  |
28 | 13:45:48.074 |  |  |  | NAS ← EMM Authentication request |  |
29 | 13:45:48.074 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 13:45:48.074 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 13:45:48.075 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 13:45:48.145 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 13:45:48.145 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 13:45:48.145 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 13:45:48.145 |  |  |  | →NAS EMM Authentication response |  |
36 | 13:45:48.145 |  |  |  | NAS UE auth OK |  |
37 | 13:45:48.145 |  |  |  | NAS K-nas-cip 6453ddb36fc9d3c0c760615042bc6... |  |
38 | 13:45:48.145 |  |  |  | NAS K-nas-int cfab8862e985586f4b0f4ad9db780... |  |
39 | 13:45:48.145 |  |  |  | NAS ← EMM Security mode command |  |
40 | 13:45:48.146 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 13:45:48.146 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 13:45:48.147 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 13:45:48.185 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
44 | 13:45:48.185 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 13:45:48.185 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x8) |  |  |
46 | 13:45:48.185 |  |  |  | →NAS EMM Security mode complete |  |
47 | 13:45:48.185 |  |  |  | NAS ← ESM ESM information request |  |
48 | 13:45:48.186 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xd) |  |  |
49 | 13:45:48.186 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 13:45:48.187 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
51 | 13:45:48.233 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
52 | 13:45:48.233 |  | →RRC DCCH UL Information Transfer |  |  |
53 | 13:45:48.233 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x1) |  |  |
54 | 13:45:48.233 |  |  |  | →NAS ESM ESM information response |  |
55 | 13:45:48.233 |  |  |  | NAS ← EMM Attach accept |  |
56 | 13:45:48.233 |  |  |  | NAS K-enb b60f7fceb6b73e0e69971202bb70283d1... |  |
57 | 13:45:48.234 |  | ←RRC DCCH Security Mode Command |  |  |
58 | 13:45:48.234 |  |  | RRC K-enb b60f7fceb6b73e0e69971202bb70283d1... |  |  |
59 | 13:45:48.234 |  |  | RRC rrc-cip c2c1cf2e870d55837aae029b8ecb050... |  |  |
60 | 13:45:48.234 |  |  | RRC rrc-int 124f2eb28f7361738d5077e2ce3b890... |  |  |
61 | 13:45:48.234 |  |  | RRC up-cip 2968a549003d0a049277f5d28233c762... |  |  |
62 | 13:45:48.234 |  |  | RRC up-int a21dfdb099395e2ffde5805f4f7906dd... |  |  |
63 | 13:45:48.235 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
64 | 13:45:48.265 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
65 | 13:45:48.265 |  | →RRC DCCH Security Mode Complete |  |  |
66 | 13:45:48.265 |  | ←RRC DCCH UE Capability Enquiry |  |  |
67 | 13:45:48.265 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
68 | 13:45:48.315 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
69 | 13:45:48.315 |  | →RRC DCCH UE Capability Information |  |  |
70 | 13:45:48.316 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x9) |  |  |
71 | 13:45:48.316 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
72 | 13:45:48.316 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
73 | 13:45:48.345 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
74 | 13:45:48.345 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
75 | 13:45:48.385 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
76 | 13:45:48.385 |  | →RRC DCCH UL Information Transfer |  |  |
77 | 13:45:48.385 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x5) |  |  |
78 | 13:45:48.385 |  |  |  | →NAS EMM Attach complete |  |
79 | 13:45:48.385 |  |  |  | NAS ← EMM EMM information |  |
80 | 13:45:48.386 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x5) |  |  |
81 | 13:45:48.386 |  | ←RRC DCCH DL Information Transfer |  |  |
82 | 13:45:48.387 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
83 | 13:45:55.869 |  | ←RRC DCCH RRC Connection Release |  |  |
84 | 13:45:55.870 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
85 | 13:45:57.372 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
86 | 13:45:57.372 |  | →RRC CCCH RRC Connection Request |  |  |
87 | 13:45:57.372 |  | ←RRC CCCH RRC Connection Setup |  |  |
88 | 13:45:57.372 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
89 | 13:45:57.425 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
90 | 13:45:57.425 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
91 | 13:45:57.425 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
92 | 13:45:57.425 |  |  |  | →NAS EMM Service request |  |
93 | 13:45:57.425 |  |  |  | NAS K-enb 3ccad6db9287dd4d83d717bfe2500887a... |  |
94 | 13:45:57.426 |  |  | RRC K-enb 3ccad6db9287dd4d83d717bfe2500887a... |  |  |
95 | 13:45:57.427 |  |  | RRC rrc-cip 0f4cf1b9de32fd2204ac45d15be4b5c... |  |  |
96 | 13:45:57.427 |  |  | RRC rrc-int 08c8e200a60fe7fb2616b86ce72cc0c... |  |  |
97 | 13:45:57.427 |  |  | RRC up-cip 8f659db94536f574c830eb27bd9d063d... |  |  |
98 | 13:45:57.427 |  |  | RRC up-int d541d1e7f5beefaa46fd217a4bc05ef6... |  |  |
99 | 13:45:57.427 |  | ←RRC DCCH Security Mode Command |  |  |
100 | 13:45:57.427 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
101 | 13:45:57.465 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
102 | 13:45:57.465 |  | →RRC DCCH Security Mode Complete |  |  |
103 | 13:45:57.465 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
104 | 13:45:57.465 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
105 | 13:45:57.505 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
106 | 13:45:57.505 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
107 | 13:46:47.585 | →enobeB PCAP frame→ TCP |  |  |  |
108 | 13:46:47.588 |  | ←enobeB PCAP frame← TCP |  |  |
109 | 13:46:47.625 | →enobeB PCAP frame→ TCP |  |  |  |
110 | 13:46:47.713 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
111 | 13:46:47.716 |  | ←enobeB PCAP frame← TCP |  |  |
112 | 13:46:47.722 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
113 | 13:46:47.745 | →enobeB PCAP frame→ TCP |  |  |  |
114 | 13:46:47.912 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 16)
115 | 13:46:47.913 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
116 | 13:46:47.916 |  | ←enobeB PCAP frame← TCP |  |  |
117 | 13:46:47.917 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
118 | 13:46:47.945 | →enobeB PCAP frame→ TCP |  |  |  |
119 | 13:46:47.952 |  |  |  |  | →HTTP GET | HTTP-Proxy
120 | 13:46:47.953 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
121 | 13:46:47.956 |  | ←enobeB PCAP frame← TCP |  |  |
122 | 13:46:47.958 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:301: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
123 | 13:46:47.977 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
124 | 13:46:47.986 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
125 | 13:46:48.025 | →enobeB PCAP frame→ TCP |  |  |  |
126 | 13:46:49.985 | →enobeB PCAP frame→ TCP |  |  |  |
127 | 13:46:49.988 |  | ←enobeB PCAP frame← TCP |  |  |
128 | 13:46:50.025 | →enobeB PCAP frame→ TCP |  |  |  |
129 | 13:46:50.033 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
130 | 13:46:50.036 |  | ←enobeB PCAP frame← TCP |  |  |
131 | 13:46:50.041 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
132 | 13:46:50.065 | →enobeB PCAP frame→ TCP |  |  |  |
133 | 13:46:50.351 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
134 | 13:46:50.353 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
135 | 13:46:50.356 |  | ←enobeB PCAP frame← TCP |  |  |
136 | 13:46:50.357 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
137 | 13:46:50.385 | →enobeB PCAP frame→ TCP |  |  |  |
138 | 13:46:50.392 |  |  |  |  | →HTTP GET | IDMS-Endpoint
139 | 13:46:50.393 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
140 | 13:46:50.396 |  | ←enobeB PCAP frame← TCP |  |  |
141 | 13:46:50.410 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
142 | 13:46:50.414 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:524: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
143 | 13:46:50.416 |  |  |  |  | MMICmd: Please provide user credentials: username and password
144 | 13:46:50.417 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
145 | 13:46:50.505 | →enobeB PCAP frame→ TCP |  |  |  |
146 | 13:46:56.873 | →enobeB PCAP frame→ HTTPS: POST /idms/userauth HTTP/1.1 |  |  |  |
147 | 13:46:56.874 |  |  |  |  | →HTTP POST | IDMS-Endpoint
148 | 13:46:56.877 |  | ←enobeB PCAP frame← TCP |  |  |
149 | 13:46:56.889 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
150 | 13:46:56.891 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:529: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
151 | 13:46:56.895 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
152 | 13:46:56.945 | →enobeB PCAP frame→ TCP |  |  |  |
153 | 13:46:56.951 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:693: IdM port - Client closed the connection (id 18)
154 | 13:46:56.953 | →enobeB PCAP frame→ TCP |  |  |  |
155 | 13:46:56.957 |  | ←enobeB PCAP frame← TCP |  |  |
156 | 13:46:56.985 | →enobeB PCAP frame→ TCP |  |  |  |
157 | 13:46:57.505 | →enobeB PCAP frame→ TCP |  |  |  |
158 | 13:46:57.508 |  | ←enobeB PCAP frame← TCP |  |  |
159 | 13:46:57.545 | →enobeB PCAP frame→ TCP |  |  |  |
160 | 13:46:57.593 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
161 | 13:46:57.596 |  | ←enobeB PCAP frame← TCP |  |  |
162 | 13:46:57.597 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
163 | 13:46:57.625 | →enobeB PCAP frame→ TCP |  |  |  |
164 | 13:46:57.710 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
165 | 13:46:57.713 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
166 | 13:46:57.716 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
167 | 13:46:57.745 | →enobeB PCAP frame→ TCP |  |  |  |
168 | 13:46:57.753 |  |  |  |  | →HTTP POST | IDMS-Endpoint
169 | 13:46:57.754 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
170 | 13:46:57.756 |  | ←enobeB PCAP frame← TCP |  |  |
171 | 13:46:57.791 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
172 | 13:46:57.792 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:534: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
173 | 13:46:57.798 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
174 | 13:46:57.865 | →enobeB PCAP frame→ TCP |  |  |  |
175 | 13:46:58.145 | →enobeB PCAP frame→ TCP |  |  |  |
176 | 13:46:58.148 |  | ←enobeB PCAP frame← TCP |  |  |
177 | 13:46:58.185 | →enobeB PCAP frame→ TCP |  |  |  |
178 | 13:46:58.193 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
179 | 13:46:58.196 |  | ←enobeB PCAP frame← TCP |  |  |
180 | 13:46:58.199 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
181 | 13:46:58.225 | →enobeB PCAP frame→ TCP |  |  |  |
182 | 13:46:58.231 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 19)
183 | 13:46:58.233 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
184 | 13:46:58.236 |  | ←enobeB PCAP frame← TCP |  |  |
185 | 13:46:58.237 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
186 | 13:46:58.272 |  |  |  |  | →HTTP POST | HTTP-Proxy
187 | 13:46:58.273 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
188 | 13:46:58.276 |  | ←enobeB PCAP frame← TCP |  |  |
189 | 13:46:58.296 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:554: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
190 | 13:46:58.303 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
191 | 13:46:58.311 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
192 | 13:46:58.345 | →enobeB PCAP frame→ TCP |  |  |  |
193 | 13:46:58.385 | →enobeB PCAP frame→ TCP |  |  |  |
194 | 13:46:58.388 |  | ←enobeB PCAP frame← TCP |  |  |
195 | 13:46:58.425 | →enobeB PCAP frame→ TCP |  |  |  |
196 | 13:46:58.433 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
197 | 13:46:58.436 |  | ←enobeB PCAP frame← TCP |  |  |
198 | 13:46:58.439 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
199 | 13:46:58.465 | →enobeB PCAP frame→ TCP |  |  |  |
200 | 13:46:58.472 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 20)
201 | 13:46:58.473 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
202 | 13:46:58.476 |  | ←enobeB PCAP frame← TCP |  |  |
203 | 13:46:58.477 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
204 | 13:46:58.513 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
205 | 13:46:58.513 |  |  |  |  | →HTTP POST | HTTP-Proxy
206 | 13:46:58.516 |  | ←enobeB PCAP frame← TCP |  |  |
207 | 13:46:58.574 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
208 | 13:46:58.575 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:558: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
209 | 13:46:58.581 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
210 | 13:46:58.625 | →enobeB PCAP frame→ TCP |  |  |  |
211 | 13:46:58.713 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
212 | 13:46:58.714 |  |  |  |  | →SIP REGISTER | P-CSCF
213 | 13:46:58.735 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:833: IMS UDP_s port 192.168.2.3:5062 configured
214 | 13:46:58.740 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:784: IMS TCP_s port 192.168.2.3:5062 configured!
215 | 13:46:58.742 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:842: IMS UDP_c port 192.168.2.3:5061 configured
216 | 13:46:58.753 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
217 | 13:46:59.513 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
218 | 13:46:59.514 |  |  |  |  | →SIP REGISTER | P-CSCF
219 | 13:46:59.539 |  |  |  |  | ←SIP 200 OK | P-CSCF
220 | 13:46:59.545 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
221 | 13:46:59.873 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
222 | 13:46:59.875 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 SIP over IPSEC: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 |  |  |  |
223 | 13:46:59.883 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
224 | 13:46:59.939 |  |  |  |  | ←SIP 200 OK | P-CSCF
225 | 13:46:59.939 |  |  |  |  | MIKEY | Media-Server
226 | 13:46:59.945 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
227 | 13:47:00.146 |  |  |  |  | XML→ | Media-Server
228 | 13:47:00.147 |  |  |  |  | XML→ | Media-Server
229 | 13:47:00.151 |  |  |  |  | ←XML | Media-Server
230 | 13:47:00.154 |  |  |  |  | ←SIP NOTIFY | P-CSCF
231 | 13:47:00.161 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:47467;transp... |  |  |
232 | 13:47:00.192 |  |  |  |  | →SIP 200 OK | P-CSCF
233 | 13:47:00.193 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
234 | 13:47:00.545 | →enobeB PCAP frame→ TCP |  |  |  |
235 | 13:47:00.548 |  | ←enobeB PCAP frame← TCP |  |  |
236 | 13:47:00.585 | →enobeB PCAP frame→ TCP |  |  |  |
237 | 13:47:00.593 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
238 | 13:47:00.596 |  | ←enobeB PCAP frame← TCP |  |  |
239 | 13:47:00.599 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
240 | 13:47:00.625 | →enobeB PCAP frame→ TCP |  |  |  |
241 | 13:47:00.672 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
242 | 13:47:00.673 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
243 | 13:47:00.676 |  | ←enobeB PCAP frame← TCP |  |  |
244 | 13:47:00.677 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
245 | 13:47:00.705 | →enobeB PCAP frame→ TCP |  |  |  |
246 | 13:47:00.711 |  |  |  |  | →HTTP GET | HTTP-Proxy
247 | 13:47:00.713 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
248 | 13:47:00.713 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:655: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcptt-ue-configuration.xml
249 | 13:47:00.715 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
250 | 13:47:00.716 |  | ←enobeB PCAP frame← TCP |  |  |
251 | 13:47:00.722 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
252 | 13:47:00.785 | →enobeB PCAP frame→ TCP |  |  |  |
253 | 13:47:00.791 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
254 | 13:47:00.793 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
255 | 13:47:00.796 |  | ←enobeB PCAP frame← TCP |  |  |
256 | 13:47:00.825 | →enobeB PCAP frame→ TCP |  |  |  |
257 | 13:47:01.025 | →enobeB PCAP frame→ TCP |  |  |  |
258 | 13:47:01.028 |  | ←enobeB PCAP frame← TCP |  |  |
259 | 13:47:01.065 | →enobeB PCAP frame→ TCP |  |  |  |
260 | 13:47:01.073 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
261 | 13:47:01.076 |  | ←enobeB PCAP frame← TCP |  |  |
262 | 13:47:01.079 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
263 | 13:47:01.105 | →enobeB PCAP frame→ TCP |  |  |  |
264 | 13:47:01.193 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
265 | 13:47:01.196 |  | ←enobeB PCAP frame← TCP |  |  |
266 | 13:47:01.213 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
267 | 13:47:01.219 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
268 | 13:47:01.265 | →enobeB PCAP frame→ TCP |  |  |  |
269 | 13:47:01.272 |  |  |  |  | →HTTP GET | HTTP-Proxy
270 | 13:47:01.273 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
271 | 13:47:01.276 |  | ←enobeB PCAP frame← TCP |  |  |
272 | 13:47:01.285 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:660: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcptt-user-profile-49.xml
273 | 13:47:01.326 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
274 | 13:47:01.336 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
275 | 13:47:01.337 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
276 | 13:47:01.385 | →enobeB PCAP frame→ TCP |  |  |  |
277 | 13:47:01.391 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
278 | 13:47:01.393 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
279 | 13:47:01.396 |  | ←enobeB PCAP frame← TCP |  |  |
280 | 13:47:01.397 |  | ←enobeB PCAP frame← TCP |  |  |
281 | 13:47:01.425 | →enobeB PCAP frame→ TCP |  |  |  |
282 | 13:47:02.114 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
283 | 13:47:02.114 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
284 | 13:47:02.124 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
285 | 13:47:02.175 |  |  |  |  | MIKEY | Media-Server
286 | 13:47:02.175 |  |  |  |  | ←SIP 200 OK | P-CSCF
287 | 13:47:02.182 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
288 | 13:47:02.225 | →enobeB PCAP frame→ TCP |  |  |  |
289 | 13:47:02.228 |  | ←enobeB PCAP frame← TCP |  |  |
290 | 13:47:02.265 | →enobeB PCAP frame→ TCP |  |  |  |
291 | 13:47:02.273 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
292 | 13:47:02.276 |  | ←enobeB PCAP frame← TCP |  |  |
293 | 13:47:02.277 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
294 | 13:47:02.305 | →enobeB PCAP frame→ TCP |  |  |  |
295 | 13:47:02.350 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
296 | 13:47:02.353 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
297 | 13:47:02.356 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
298 | 13:47:02.384 |  |  |  |  | XML→ | Media-Server
299 | 13:47:02.385 | →enobeB PCAP frame→ TCP |  |  |  |
300 | 13:47:02.386 |  |  |  |  | XML→ | Media-Server
301 | 13:47:02.389 |  |  |  |  | ←XML | Media-Server
302 | 13:47:02.391 |  |  |  |  | →HTTP GET | HTTP-Proxy
303 | 13:47:02.392 |  |  |  |  | ←SIP NOTIFY | P-CSCF
304 | 13:47:02.393 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
305 | 13:47:02.393 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:665: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
306 | 13:47:02.396 |  | ←enobeB PCAP frame← TCP |  |  |
307 | 13:47:02.398 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:47467;transp... |  |  |
308 | 13:47:02.399 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
309 | 13:47:02.405 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
310 | 13:47:02.407 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
311 | 13:47:02.425 | →enobeB PCAP frame→ TCP |  |  |  |
312 | 13:47:02.440 |  |  |  |  | →SIP 200 OK | P-CSCF
313 | 13:47:02.463 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
314 | 13:47:02.468 |  | ←enobeB PCAP frame← TCP |  |  |
315 | 13:47:02.478 |  | ←enobeB PCAP frame← TCP |  |  |
316 | 13:47:02.545 | →enobeB PCAP frame→ TCP |  |  |  |
317 | 13:47:02.548 |  | ←enobeB PCAP frame← TCP |  |  |
318 | 13:47:02.585 | →enobeB PCAP frame→ TCP |  |  |  |
319 | 13:47:02.594 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
320 | 13:47:02.596 |  | ←enobeB PCAP frame← TCP |  |  |
321 | 13:47:02.600 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
322 | 13:47:02.625 | →enobeB PCAP frame→ TCP |  |  |  |
323 | 13:47:02.712 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
324 | 13:47:02.713 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
325 | 13:47:02.716 |  | ←enobeB PCAP frame← TCP |  |  |
326 | 13:47:02.717 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
327 | 13:47:02.745 | →enobeB PCAP frame→ TCP |  |  |  |
328 | 13:47:02.752 |  |  |  |  | →HTTP GET | HTTP-Proxy
329 | 13:47:02.753 | →enobeB PCAP frame→ HTTPS: GET http://xcap.gms.mcstaasting.com/org.openmobile... |  |  |  |
330 | 13:47:02.756 |  | ←enobeB PCAP frame← TCP |  |  |
331 | 13:47:02.763 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:670: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at http://xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
332 | 13:47:02.789 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
333 | 13:47:02.799 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
334 | 13:47:02.801 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
335 | 13:47:02.825 | →enobeB PCAP frame→ TCP |  |  |  |
336 | 13:47:02.903 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
337 | 13:47:02.905 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
338 | 13:47:02.908 |  | ←enobeB PCAP frame← TCP |  |  |
339 | 13:47:02.913 | →enobeB PCAP frame→ TCP |  |  |  |
340 | 13:47:02.916 |  | ←enobeB PCAP frame← TCP |  |  |
341 | 13:47:02.945 | →enobeB PCAP frame→ TCP |  |  |  |
342 | 13:47:03.033 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
343 | 13:47:03.034 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
344 | 13:47:03.043 |  |  |  |  | →SIP PUBLISH | P-CSCF
345 | 13:47:03.090 |  |  |  |  | MIKEY | Media-Server
346 | 13:47:03.194 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
347 | 13:47:03.194 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
348 | 13:47:03.194 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
349 | 13:47:03.304 |  |  |  |  | XML→ | Media-Server
350 | 13:47:03.307 |  |  |  |  | ←SIP 200 OK | P-CSCF
351 | 13:47:03.310 |  |  |  |  | ←SIP 200 OK | P-CSCF
352 | 13:47:03.310 |  |  |  |  | MIKEY | Media-Server
353 | 13:47:03.313 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
354 | 13:47:03.316 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
355 | 13:47:03.511 |  |  |  |  | XML→ | Media-Server
356 | 13:47:03.512 |  |  |  |  | XML→ | Media-Server
357 | 13:47:03.550 |  |  |  |  | MIKEY | Media-Server
358 | 13:47:03.550 |  |  |  |  | ←XML | Media-Server
359 | 13:47:03.555 |  |  |  |  | ←SIP NOTIFY | P-CSCF
360 | 13:47:03.562 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:47467;transp... |  |  |
361 | 13:47:03.590 |  |  |  |  | →SIP 200 OK | P-CSCF
362 | 13:47:03.593 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
363 | 13:47:03.593 |  |  |  |  | ←XML | Media-Server
364 | 13:47:03.600 |  |  |  |  | ←SIP MESSAGE | P-CSCF
365 | 13:47:03.607 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
366 | 13:47:04.512 |  |  |  |  | →SIP 200 OK | P-CSCF
367 | 13:47:04.513 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
368 | 13:47:04.519 |  |  |  |  | Info: MCX_IMS_CommonProcedures.ttcn:228: MESSAGE/200OK Table 5.3.2.3-2 Steps 7-8 Done
369 | 13:47:06.522 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
370 | 13:47:06.574 |  | ←RRC DCCH RRC Connection Release |  |  |
371 | 13:47:06.575 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
372 | 13:47:06.590 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
373 | 13:47:06.593 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
374 | 13:47:06.593 |  |  |  |  | MMICmd: Make the UE (MCPTT User) request the establishment of an MCPTT private call, on-demand Automatic Commencement Mode, no Force of automatic commencement, without Floor Control
375 | 13:47:18.952 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
376 | 13:47:18.952 |  | →RRC CCCH RRC Connection Request |  |  |
377 | 13:47:18.952 |  | ←RRC CCCH RRC Connection Setup |  |  |
378 | 13:47:18.952 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
379 | 13:47:18.985 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
380 | 13:47:18.985 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
381 | 13:47:18.985 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
382 | 13:47:18.985 |  |  |  | →NAS EMM Service request |  |
383 | 13:47:18.985 |  |  |  | NAS K-enb 9e7909a9bec40ed9f78d07096806010e0... |  |
384 | 13:47:18.986 |  |  | RRC K-enb 9e7909a9bec40ed9f78d07096806010e0... |  |  |
385 | 13:47:18.987 |  |  | RRC rrc-cip 8045d80d7980e2feae2d3fae9519f41... |  |  |
386 | 13:47:18.987 |  |  | RRC rrc-int 64c450fc6e8f38fe13f65deb2b6f37b... |  |  |
387 | 13:47:18.987 |  |  | RRC up-cip f92b514092866fbbc5e38b550ade9d6d... |  |  |
388 | 13:47:18.987 |  |  | RRC up-int 9623f99f04d0a5535708fabbab87dc73... |  |  |
389 | 13:47:18.987 |  | ←RRC DCCH Security Mode Command |  |  |
390 | 13:47:18.987 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
391 | 13:47:19.025 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
392 | 13:47:19.025 |  | →RRC DCCH Security Mode Complete |  |  |
393 | 13:47:19.025 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
394 | 13:47:19.025 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
395 | 13:47:19.065 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
396 | 13:47:19.065 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
397 | 13:47:19.074 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
398 | 13:47:19.074 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |  |
399 | 13:47:19.084 |  |  |  |  | →SIP INVITE | P-CSCF
400 | 13:47:19.134 |  |  |  |  | MIKEY | Media-Server
401 | 13:47:19.345 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:754: SRTP config: Master Key: D20B6C6FEB316EAA3F4F30817D376ED2, Master Salt: E2F34531E43CE4FE2FCF3449, MKI: 2F034FAE
402 | 13:47:19.345 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
403 | 13:47:19.348 |  |  |  |  | XML→ | Media-Server
404 | 13:47:19.349 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
405 | 13:47:19.349 |  |  |  |  | XML→ | Media-Server
406 | 13:47:19.351 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1233: INVITE Verdict: Pass
407 | 13:47:19.352 |  |  |  |  | ←SIP 100 Trying | P-CSCF
408 | 13:47:19.354 |  |  |  |  | ←SIP 200 OK | P-CSCF
409 | 13:47:19.358 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
410 | 13:47:19.360 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
411 | 13:47:20.001 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
412 | 13:47:20.001 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x6) |  |  |
413 | 13:47:20.001 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
414 | 13:47:20.002 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
415 | 13:47:20.025 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
416 | 13:47:20.025 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
417 | 13:47:20.065 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
418 | 13:47:20.065 |  | →RRC DCCH UL Information Transfer |  |  |
419 | 13:47:20.065 |  | [EMBEDDED NAS IN PREV RRC] Message too short (len=9) |  |  |
420 | 13:47:20.065 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
421 | 13:47:20.123 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
422 | 13:47:20.352 |  |  |  |  | →SIP ACK | P-CSCF
423 | 13:47:20.353 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
424 | 13:47:20.361 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1236: ACK Verdict: Pass
425 | 13:47:20.362 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:349: Step 2 Verdict: Pass
426 | 13:47:20.865 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
427 | 13:47:20.906 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
428 | 13:47:20.913 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
429 | 13:47:20.921 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
430 | 13:47:20.945 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
431 | 13:47:21.112 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:354: Step 5 Verdict: Pass
432 | 13:47:21.217 |  |  |  |  | MMICmd: Release call (hang up the call)
433 | 13:47:23.162 |  |  |  |  | →SIP BYE | P-CSCF
434 | 13:47:23.181 |  |  |  |  | ←SIP 200 OK | P-CSCF
435 | 13:47:23.665 | →enobeB PCAP frame→ |  |  |  |
436 | 13:47:25.179 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
437 | 13:47:25.192 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
438 | 13:47:25.192 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x0) |  |  |
439 | 13:47:25.192 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
440 | 13:47:25.193 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
441 | 13:47:25.225 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
442 | 13:47:25.225 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
443 | 13:47:25.225 |  | →RRC DCCH UL Information Transfer |  |  |
444 | 13:47:25.225 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
445 | 13:47:25.226 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
446 | 13:47:25.304 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
447 | 13:47:25.305 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
448 | 13:47:25.356 |  | ←RRC DCCH RRC Connection Release |  |  |
449 | 13:47:25.357 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
450 | 13:47:25.371 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
451 | 13:47:25.374 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:360: Step 9 Verdict: Pass
452 | 13:47:25.376 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
453 | 13:47:25.377 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
454 | 13:47:26.125 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.