MSG #411 2021-09-28 13:47:20.001
NAS

     ESM: Activate dedicated EPS bearer context request
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x2 (Integrity protected and ciphered)
    Auth code = 0x02176fe7
    Sequence number = 0x04
    Protocol discriminator = 0x2 (EPS Session Management)
    EPS bearer identity = 6
    Procedure transaction identity = 0
    Message type = 0xc5 (Activate dedicated EPS bearer context request)
    Linked EPS bearer identity = 5
    EPS Qos:
      QCI = 65
      Maximum bit rate for uplink = 384000 bits
      Maximum bit rate for downlink = 384000 bits
      Guaranteed bit rate for uplink = 128000 bits
      Guaranteed bit rate for downlink = 128000 bits
    Traffic Flow Template:
      TFT operation code = 1 (create new TFT)
      E = 0 (parameters list is not included)
      Number of packet filters = 2
      Packet filter identifier = 6
        Packet filter direction = 3 (bidirectional)
        Packet filter evaluation precedence = 0
        IPv4 remote address = 192.168.2.3 mask 255.255.255.255
        Protocol identifier/Next header = 17
        Remote port range = [60350;60351]
      Packet filter identifier = 7
        Packet filter direction = 3 (bidirectional)
        Packet filter evaluation precedence = 1
        IPv4 remote address = 192.168.2.3 mask 255.255.255.255
        Protocol identifier/Next header = 17
        Single remote port = 60354