ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 13:32:25.765 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 13:32:25.767 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 13:32:25.767 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 13:32:25.769 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 13:32:25.769 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 13:32:25.770 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:824: IMS UDP port 192.168.2.3:5060 configured
7 | 13:32:25.773 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:774: IMS TCP port 192.168.2.3:5060 configured!
8 | 13:32:25.774 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:795: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 13:32:25.775 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:806: IdM port 192.168.2.3:8080 configured!
10 | 13:32:25.777 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 13:32:26.979 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 13:32:26.981 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 13:32:32.778 |  | ←RRC BCCH SIB1 |  |  |
14 | 13:32:32.793 |  | ←RRC BCCH SIB |  |  |
15 | 13:32:32.813 |  | ←RRC BCCH SIB |  |  |
16 | 13:32:32.858 |  | ←RRC BCCH SIB1 |  |  |
17 | 13:32:32.933 |  | ←RRC BCCH SIB |  |  |
18 | 13:33:42.692 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 13:33:42.692 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 13:33:42.692 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 13:33:42.692 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 13:33:42.753 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 13:33:42.753 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 13:33:42.753 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 13:33:42.753 |  |  |  | →NAS EMM Attach request |  |
26 | 13:33:42.753 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 13:33:42.753 |  |  |  | NAS K-asme 37467f314ca850b25528e7da6a979b32... |  |
28 | 13:33:42.753 |  |  |  | NAS ← EMM Authentication request |  |
29 | 13:33:42.754 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 13:33:42.754 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 13:33:42.755 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 13:33:42.825 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 13:33:42.825 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 13:33:42.825 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 13:33:42.825 |  |  |  | →NAS EMM Authentication response |  |
36 | 13:33:42.825 |  |  |  | NAS UE auth OK |  |
37 | 13:33:42.825 |  |  |  | NAS K-nas-cip 19b14d386c7c4549601549a0600b2... |  |
38 | 13:33:42.825 |  |  |  | NAS K-nas-int 85b2b237825b78377da82f9ebd4bd... |  |
39 | 13:33:42.825 |  |  |  | NAS ← EMM Security mode command |  |
40 | 13:33:42.826 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 13:33:42.826 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 13:33:42.827 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 13:33:42.865 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
44 | 13:33:42.865 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 13:33:42.865 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x5) |  |  |
46 | 13:33:42.865 |  |  |  | →NAS EMM Security mode complete |  |
47 | 13:33:42.865 |  |  |  | NAS ← ESM ESM information request |  |
48 | 13:33:42.866 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xc) |  |  |
49 | 13:33:42.866 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 13:33:42.867 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
51 | 13:33:42.913 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
52 | 13:33:42.913 |  | →RRC DCCH UL Information Transfer |  |  |
53 | 13:33:42.913 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x1) |  |  |
54 | 13:33:42.913 |  |  |  | →NAS ESM ESM information response |  |
55 | 13:33:42.913 |  |  |  | NAS ← EMM Attach accept |  |
56 | 13:33:42.913 |  |  |  | NAS K-enb 4bab103d05b84ef673069677a238f7ae6... |  |
57 | 13:33:42.914 |  | ←RRC DCCH Security Mode Command |  |  |
58 | 13:33:42.914 |  |  | RRC K-enb 4bab103d05b84ef673069677a238f7ae6... |  |  |
59 | 13:33:42.914 |  |  | RRC rrc-cip b8b6011eccecf3f974e8558b21fde75... |  |  |
60 | 13:33:42.914 |  |  | RRC rrc-int 9de220ba6e0a56a1fe423b4827390e0... |  |  |
61 | 13:33:42.914 |  |  | RRC up-cip 0712c34316a6de633c0be910fb3f4d20... |  |  |
62 | 13:33:42.914 |  |  | RRC up-int 8bc0919cd068672b1ee44517f72f2e12... |  |  |
63 | 13:33:42.915 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
64 | 13:33:42.945 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
65 | 13:33:42.945 |  | →RRC DCCH Security Mode Complete |  |  |
66 | 13:33:42.945 |  | ←RRC DCCH UE Capability Enquiry |  |  |
67 | 13:33:42.945 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
68 | 13:33:42.995 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
69 | 13:33:42.995 |  | →RRC DCCH UE Capability Information |  |  |
70 | 13:33:42.996 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xc) |  |  |
71 | 13:33:42.996 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
72 | 13:33:42.996 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
73 | 13:33:43.025 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
74 | 13:33:43.025 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
75 | 13:33:43.065 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
76 | 13:33:43.065 |  | →RRC DCCH UL Information Transfer |  |  |
77 | 13:33:43.065 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x4) |  |  |
78 | 13:33:43.065 |  |  |  | →NAS EMM Attach complete |  |
79 | 13:33:43.065 |  |  |  | NAS ← EMM EMM information |  |
80 | 13:33:43.066 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x9) |  |  |
81 | 13:33:43.066 |  | ←RRC DCCH DL Information Transfer |  |  |
82 | 13:33:43.067 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
83 | 13:33:49.200 |  | ←RRC DCCH RRC Connection Release |  |  |
84 | 13:33:49.201 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
85 | 13:33:49.452 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
86 | 13:33:49.452 |  | →RRC CCCH RRC Connection Request |  |  |
87 | 13:33:49.452 |  | ←RRC CCCH RRC Connection Setup |  |  |
88 | 13:33:49.452 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
89 | 13:33:49.505 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
90 | 13:33:49.505 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
91 | 13:33:49.505 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
92 | 13:33:49.505 |  |  |  | →NAS EMM Service request |  |
93 | 13:33:49.505 |  |  |  | NAS K-enb 36c109af340dcef2a6cfc52ab8858e9c4... |  |
94 | 13:33:49.506 |  |  | RRC K-enb 36c109af340dcef2a6cfc52ab8858e9c4... |  |  |
95 | 13:33:49.507 |  |  | RRC rrc-cip 909ad93fbb83e8db7ab59077199f3b8... |  |  |
96 | 13:33:49.507 |  |  | RRC rrc-int 21905daf58e8a1e03aae00deef5ad48... |  |  |
97 | 13:33:49.507 |  |  | RRC up-cip 7d5266027cca9dde0e585b7de47a22f1... |  |  |
98 | 13:33:49.507 |  |  | RRC up-int 072a5a11a3ca2d63705eb7e32c7f82fd... |  |  |
99 | 13:33:49.507 |  | ←RRC DCCH Security Mode Command |  |  |
100 | 13:33:49.507 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
101 | 13:33:49.545 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
102 | 13:33:49.545 |  | →RRC DCCH Security Mode Complete |  |  |
103 | 13:33:49.545 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
104 | 13:33:49.545 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
105 | 13:33:49.585 | →enobeB PCAP frame→ DNS RRCConnectionReconfigurationComplete [77-bytes] ... |  |  |  |
106 | 13:33:49.585 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
107 | 13:34:08.225 | →enobeB PCAP frame→ TCP |  |  |  |
108 | 13:34:08.228 |  | ←enobeB PCAP frame← TCP |  |  |
109 | 13:34:08.265 | →enobeB PCAP frame→ TCP |  |  |  |
110 | 13:34:08.353 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
111 | 13:34:08.356 |  | ←enobeB PCAP frame← TCP |  |  |
112 | 13:34:08.361 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
113 | 13:34:08.385 | →enobeB PCAP frame→ TCP |  |  |  |
114 | 13:34:08.551 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 16)
115 | 13:34:08.553 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
116 | 13:34:08.556 |  | ←enobeB PCAP frame← TCP |  |  |
117 | 13:34:08.557 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
118 | 13:34:08.585 | →enobeB PCAP frame→ TCP |  |  |  |
119 | 13:34:08.631 |  |  |  |  | →HTTP GET | HTTP-Proxy
120 | 13:34:08.633 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
121 | 13:34:08.636 |  | ←enobeB PCAP frame← TCP |  |  |
122 | 13:34:08.638 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:301: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
123 | 13:34:08.657 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
124 | 13:34:08.666 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
125 | 13:34:08.705 | →enobeB PCAP frame→ TCP |  |  |  |
126 | 13:34:10.593 | →enobeB PCAP frame→ TCP |  |  |  |
127 | 13:34:10.596 |  | ←enobeB PCAP frame← TCP |  |  |
128 | 13:34:10.625 | →enobeB PCAP frame→ TCP |  |  |  |
129 | 13:34:10.633 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
130 | 13:34:10.636 |  | ←enobeB PCAP frame← TCP |  |  |
131 | 13:34:10.642 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
132 | 13:34:10.665 | →enobeB PCAP frame→ TCP |  |  |  |
133 | 13:34:10.951 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
134 | 13:34:10.953 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
135 | 13:34:10.956 |  | ←enobeB PCAP frame← TCP |  |  |
136 | 13:34:10.957 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
137 | 13:34:10.985 | →enobeB PCAP frame→ TCP |  |  |  |
138 | 13:34:10.992 |  |  |  |  | →HTTP GET | IDMS-Endpoint
139 | 13:34:10.993 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
140 | 13:34:10.996 |  | ←enobeB PCAP frame← TCP |  |  |
141 | 13:34:11.033 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
142 | 13:34:11.036 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:524: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
143 | 13:34:11.037 |  |  |  |  | MMICmd: Please provide user credentials: username and password
144 | 13:34:11.040 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
145 | 13:34:11.105 | →enobeB PCAP frame→ TCP |  |  |  |
146 | 13:34:15.841 |  |  |  |  | →HTTP POST | IDMS-Endpoint
147 | 13:34:15.844 |  | ←enobeB PCAP frame← TCP |  |  |
148 | 13:34:15.855 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
149 | 13:34:15.857 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:529: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
150 | 13:34:15.862 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
151 | 13:34:15.902 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:693: IdM port - Client closed the connection (id 18)
152 | 13:34:15.908 |  | ←enobeB PCAP frame← TCP |  |  |
153 | 13:34:16.625 | →enobeB PCAP frame→ TCP |  |  |  |
154 | 13:34:16.629 |  | ←enobeB PCAP frame← TCP |  |  |
155 | 13:34:16.665 | →enobeB PCAP frame→ TCP |  |  |  |
156 | 13:34:16.753 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
157 | 13:34:16.756 |  | ←enobeB PCAP frame← TCP |  |  |
158 | 13:34:16.757 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
159 | 13:34:16.785 | →enobeB PCAP frame→ TCP |  |  |  |
160 | 13:34:16.871 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
161 | 13:34:16.873 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
162 | 13:34:16.876 |  | ←enobeB PCAP frame← TCP |  |  |
163 | 13:34:16.877 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
164 | 13:34:16.905 | →enobeB PCAP frame→ TCP |  |  |  |
165 | 13:34:16.911 |  |  |  |  | →HTTP POST | IDMS-Endpoint
166 | 13:34:16.913 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
167 | 13:34:16.916 |  | ←enobeB PCAP frame← TCP |  |  |
168 | 13:34:16.954 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
169 | 13:34:16.955 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:534: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
170 | 13:34:16.961 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
171 | 13:34:17.025 | →enobeB PCAP frame→ TCP |  |  |  |
172 | 13:34:17.225 | →enobeB PCAP frame→ TCP |  |  |  |
173 | 13:34:17.228 |  | ←enobeB PCAP frame← TCP |  |  |
174 | 13:34:17.265 | →enobeB PCAP frame→ TCP |  |  |  |
175 | 13:34:17.273 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
176 | 13:34:17.276 |  | ←enobeB PCAP frame← TCP |  |  |
177 | 13:34:17.280 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
178 | 13:34:17.305 | →enobeB PCAP frame→ TCP |  |  |  |
179 | 13:34:17.311 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 19)
180 | 13:34:17.313 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
181 | 13:34:17.316 |  | ←enobeB PCAP frame← TCP |  |  |
182 | 13:34:17.317 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
183 | 13:34:17.360 |  |  |  |  | →HTTP POST | HTTP-Proxy
184 | 13:34:17.364 |  | ←enobeB PCAP frame← TCP |  |  |
185 | 13:34:17.386 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:554: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
186 | 13:34:17.392 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
187 | 13:34:17.400 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
188 | 13:34:17.468 |  | ←enobeB PCAP frame← TCP |  |  |
189 | 13:34:17.505 | →enobeB PCAP frame→ TCP |  |  |  |
190 | 13:34:17.513 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
191 | 13:34:17.516 |  | ←enobeB PCAP frame← TCP |  |  |
192 | 13:34:17.520 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
193 | 13:34:17.545 | →enobeB PCAP frame→ TCP |  |  |  |
194 | 13:34:17.551 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 20)
195 | 13:34:17.553 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
196 | 13:34:17.556 |  | ←enobeB PCAP frame← TCP |  |  |
197 | 13:34:17.557 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
198 | 13:34:17.593 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
199 | 13:34:17.593 |  |  |  |  | →HTTP POST | HTTP-Proxy
200 | 13:34:17.596 |  | ←enobeB PCAP frame← TCP |  |  |
201 | 13:34:17.662 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
202 | 13:34:17.662 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:558: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
203 | 13:34:17.669 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
204 | 13:34:17.705 | →enobeB PCAP frame→ TCP |  |  |  |
205 | 13:34:17.752 |  |  |  |  | →SIP REGISTER | P-CSCF
206 | 13:34:17.753 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
207 | 13:34:17.764 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:833: IMS UDP_s port 192.168.2.3:5062 configured
208 | 13:34:17.766 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:784: IMS TCP_s port 192.168.2.3:5062 configured!
209 | 13:34:17.767 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:842: IMS UDP_c port 192.168.2.3:5061 configured
210 | 13:34:17.770 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
211 | 13:34:18.441 |  |  |  |  | →SIP REGISTER | P-CSCF
212 | 13:34:18.453 |  |  |  |  | ←SIP 200 OK | P-CSCF
213 | 13:34:18.461 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
214 | 13:34:18.754 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
215 | 13:34:18.819 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
216 | 13:34:18.832 |  |  |  |  | ←SIP 200 OK | P-CSCF
217 | 13:34:18.833 |  |  |  |  | MIKEY | Media-Server
218 | 13:34:18.839 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
219 | 13:34:19.032 |  |  |  |  | XML→ | Media-Server
220 | 13:34:19.033 |  |  |  |  | XML→ | Media-Server
221 | 13:34:19.036 |  |  |  |  | ←XML | Media-Server
222 | 13:34:19.040 |  |  |  |  | ←SIP NOTIFY | P-CSCF
223 | 13:34:19.047 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:47229;transp... |  |  |
224 | 13:34:19.070 |  |  |  |  | →SIP 200 OK | P-CSCF
225 | 13:34:19.073 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
226 | 13:34:19.385 | →enobeB PCAP frame→ TCP |  |  |  |
227 | 13:34:19.388 |  | ←enobeB PCAP frame← TCP |  |  |
228 | 13:34:19.425 | →enobeB PCAP frame→ TCP |  |  |  |
229 | 13:34:19.433 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
230 | 13:34:19.436 |  | ←enobeB PCAP frame← TCP |  |  |
231 | 13:34:19.439 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
232 | 13:34:19.465 | →enobeB PCAP frame→ TCP |  |  |  |
233 | 13:34:19.550 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
234 | 13:34:19.553 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
235 | 13:34:19.556 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
236 | 13:34:19.585 | →enobeB PCAP frame→ TCP |  |  |  |
237 | 13:34:19.591 |  |  |  |  | →HTTP GET | HTTP-Proxy
238 | 13:34:19.593 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
239 | 13:34:19.596 |  | ←enobeB PCAP frame← TCP |  |  |
240 | 13:34:19.600 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:655: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcptt-ue-configuration.xml
241 | 13:34:19.608 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
242 | 13:34:19.615 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
243 | 13:34:19.662 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
244 | 13:34:19.665 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
245 | 13:34:19.668 |  | ←enobeB PCAP frame← TCP |  |  |
246 | 13:34:19.673 | →enobeB PCAP frame→ TCP |  |  |  |
247 | 13:34:19.676 |  | ←enobeB PCAP frame← TCP |  |  |
248 | 13:34:19.705 | →enobeB PCAP frame→ TCP |  |  |  |
249 | 13:34:19.865 | →enobeB PCAP frame→ TCP |  |  |  |
250 | 13:34:19.868 |  | ←enobeB PCAP frame← TCP |  |  |
251 | 13:34:19.905 | →enobeB PCAP frame→ TCP |  |  |  |
252 | 13:34:19.913 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
253 | 13:34:19.916 |  | ←enobeB PCAP frame← TCP |  |  |
254 | 13:34:19.920 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
255 | 13:34:19.945 | →enobeB PCAP frame→ TCP |  |  |  |
256 | 13:34:20.030 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
257 | 13:34:20.033 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
258 | 13:34:20.036 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
259 | 13:34:20.065 | →enobeB PCAP frame→ TCP |  |  |  |
260 | 13:34:20.071 |  |  |  |  | →HTTP GET | HTTP-Proxy
261 | 13:34:20.073 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
262 | 13:34:20.076 |  | ←enobeB PCAP frame← TCP |  |  |
263 | 13:34:20.082 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:660: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcptt-user-profile-49.xml
264 | 13:34:20.091 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
265 | 13:34:20.099 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
266 | 13:34:20.100 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
267 | 13:34:20.145 | →enobeB PCAP frame→ TCP |  |  |  |
268 | 13:34:20.151 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
269 | 13:34:20.153 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
270 | 13:34:20.157 |  | ←enobeB PCAP frame← TCP |  |  |
271 | 13:34:20.185 | →enobeB PCAP frame→ TCP |  |  |  |
272 | 13:34:20.713 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
273 | 13:34:20.714 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
274 | 13:34:20.724 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
275 | 13:34:20.762 |  |  |  |  | ←SIP 200 OK | P-CSCF
276 | 13:34:20.762 |  |  |  |  | MIKEY | Media-Server
277 | 13:34:20.769 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
278 | 13:34:20.785 | →enobeB PCAP frame→ TCP |  |  |  |
279 | 13:34:20.788 |  | ←enobeB PCAP frame← TCP |  |  |
280 | 13:34:20.825 | →enobeB PCAP frame→ TCP |  |  |  |
281 | 13:34:20.833 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
282 | 13:34:20.836 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
283 | 13:34:20.865 | →enobeB PCAP frame→ TCP |  |  |  |
284 | 13:34:20.950 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
285 | 13:34:20.953 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
286 | 13:34:20.956 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
287 | 13:34:20.959 |  |  |  |  | XML→ | Media-Server
288 | 13:34:20.961 |  |  |  |  | XML→ | Media-Server
289 | 13:34:20.964 |  |  |  |  | ←XML | Media-Server
290 | 13:34:20.967 |  |  |  |  | ←SIP NOTIFY | P-CSCF
291 | 13:34:20.974 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:47229;transp... |  |  |
292 | 13:34:20.985 | →enobeB PCAP frame→ TCP |  |  |  |
293 | 13:34:20.991 |  |  |  |  | →HTTP GET | HTTP-Proxy
294 | 13:34:20.993 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
295 | 13:34:20.996 |  | ←enobeB PCAP frame← TCP |  |  |
296 | 13:34:21.002 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:665: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
297 | 13:34:21.009 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
298 | 13:34:21.015 |  |  |  |  | →SIP 200 OK | P-CSCF
299 | 13:34:21.016 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
300 | 13:34:21.017 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
301 | 13:34:21.018 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
302 | 13:34:21.065 | →enobeB PCAP frame→ TCP |  |  |  |
303 | 13:34:21.071 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
304 | 13:34:21.073 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
305 | 13:34:21.077 |  | ←enobeB PCAP frame← TCP |  |  |
306 | 13:34:21.105 | →enobeB PCAP frame→ TCP |  |  |  |
307 | 13:34:21.145 | →enobeB PCAP frame→ TCP |  |  |  |
308 | 13:34:21.148 |  | ←enobeB PCAP frame← TCP |  |  |
309 | 13:34:21.185 | →enobeB PCAP frame→ TCP |  |  |  |
310 | 13:34:21.193 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
311 | 13:34:21.196 |  | ←enobeB PCAP frame← TCP |  |  |
312 | 13:34:21.198 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
313 | 13:34:21.225 | →enobeB PCAP frame→ TCP |  |  |  |
314 | 13:34:21.271 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
315 | 13:34:21.273 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
316 | 13:34:21.276 |  | ←enobeB PCAP frame← TCP |  |  |
317 | 13:34:21.277 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
318 | 13:34:21.311 |  |  |  |  | →HTTP GET | HTTP-Proxy
319 | 13:34:21.313 | →enobeB PCAP frame→ HTTPS: GET http://xcap.gms.mcstaasting.com/org.openmobile... |  |  |  |
320 | 13:34:21.316 |  | ←enobeB PCAP frame← TCP |  |  |
321 | 13:34:21.324 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:670: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at http://xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
322 | 13:34:21.350 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
323 | 13:34:21.360 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
324 | 13:34:21.385 | →enobeB PCAP frame→ TCP |  |  |  |
325 | 13:34:21.423 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
326 | 13:34:21.425 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
327 | 13:34:21.428 |  | ←enobeB PCAP frame← TCP |  |  |
328 | 13:34:21.429 |  | ←enobeB PCAP frame← TCP |  |  |
329 | 13:34:21.433 | →enobeB PCAP frame→ TCP |  |  |  |
330 | 13:34:21.436 |  | ←enobeB PCAP frame← TCP |  |  |
331 | 13:34:21.465 | →enobeB PCAP frame→ TCP |  |  |  |
332 | 13:34:21.593 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
333 | 13:34:21.594 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
334 | 13:34:21.606 |  |  |  |  | →SIP PUBLISH | P-CSCF
335 | 13:34:21.654 |  |  |  |  | MIKEY | Media-Server
336 | 13:34:21.673 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
337 | 13:34:21.674 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
338 | 13:34:21.676 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
339 | 13:34:21.868 |  |  |  |  | XML→ | Media-Server
340 | 13:34:21.872 |  |  |  |  | ←SIP 200 OK | P-CSCF
341 | 13:34:21.875 |  |  |  |  | ←SIP 200 OK | P-CSCF
342 | 13:34:21.875 |  |  |  |  | MIKEY | Media-Server
343 | 13:34:21.879 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
344 | 13:34:21.882 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
345 | 13:34:22.070 |  |  |  |  | XML→ | Media-Server
346 | 13:34:22.071 |  |  |  |  | XML→ | Media-Server
347 | 13:34:22.105 |  |  |  |  | MIKEY | Media-Server
348 | 13:34:22.105 |  |  |  |  | ←XML | Media-Server
349 | 13:34:22.111 |  |  |  |  | ←SIP NOTIFY | P-CSCF
350 | 13:34:22.119 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:47229;transp... |  |  |
351 | 13:34:22.151 |  |  |  |  | →SIP 200 OK | P-CSCF
352 | 13:34:22.153 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
353 | 13:34:22.161 |  |  |  |  | ←XML | Media-Server
354 | 13:34:22.181 |  |  |  |  | ←SIP MESSAGE | P-CSCF
355 | 13:34:22.188 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
356 | 13:34:23.031 |  |  |  |  | →SIP 200 OK | P-CSCF
357 | 13:34:23.033 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
358 | 13:34:23.038 |  |  |  |  | Info: MCX_IMS_CommonProcedures.ttcn:228: MESSAGE/200OK Table 5.3.2.3-2 Steps 7-8 Done
359 | 13:34:25.041 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
360 | 13:34:25.081 |  | ←RRC DCCH RRC Connection Release |  |  |
361 | 13:34:25.082 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
362 | 13:34:25.096 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
363 | 13:34:25.172 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:754: SRTP config: Master Key: 7CBE7C5516F2B091DFFFF3B606877528, Master Salt: F0D980059F54B1845536ACAC, MKI: 20AEA9DD
364 | 13:34:25.172 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
365 | 13:34:25.173 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
366 | 13:34:25.175 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
367 | 13:34:25.179 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
368 | 13:34:25.179 |  |  |  |  | ←XML | Media-Server
369 | 13:34:25.188 |  |  |  |  | ←SIP INVITE | P-CSCF
370 | 13:34:25.952 |  | ←enobeB PCAP frame← LTE RRC PCCH Paging (1 PagingRecord) |  |  |
371 | 13:34:25.952 |  | ←RRC PCCH Paging |  |  |
372 | 13:34:25.992 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
373 | 13:34:25.992 |  | →RRC CCCH RRC Connection Request |  |  |
374 | 13:34:25.992 |  | ←RRC CCCH RRC Connection Setup |  |  |
375 | 13:34:25.992 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
376 | 13:34:26.025 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
377 | 13:34:26.025 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
378 | 13:34:26.025 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
379 | 13:34:26.025 |  |  |  | →NAS EMM Service request |  |
380 | 13:34:26.025 |  |  |  | NAS K-enb cbece23434dce10e9e0d79e170d4dfe35... |  |
381 | 13:34:26.026 |  |  | RRC K-enb cbece23434dce10e9e0d79e170d4dfe35... |  |  |
382 | 13:34:26.027 |  |  | RRC rrc-cip 99c485f0e9d2a4f9cc6e02af12382e5... |  |  |
383 | 13:34:26.027 |  |  | RRC rrc-int 6b2c50187f4d10347020a98555c8b73... |  |  |
384 | 13:34:26.027 |  |  | RRC up-cip 4b761c01824b3cccd009263d8f5c6acf... |  |  |
385 | 13:34:26.027 |  |  | RRC up-int 5063f0e9b19e69c7aa696e39b995f991... |  |  |
386 | 13:34:26.027 |  | ←RRC DCCH Security Mode Command |  |  |
387 | 13:34:26.027 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
388 | 13:34:26.065 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
389 | 13:34:26.065 |  | →RRC DCCH Security Mode Complete |  |  |
390 | 13:34:26.065 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
391 | 13:34:26.065 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
392 | 13:34:26.105 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
393 | 13:34:26.105 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
394 | 13:34:26.107 |  | ←enobeB PCAP frame← SIP over IPSEC: INVITE sip:PublicUserId-A@192.168.3.2:47229;transp... |  |  |
395 | 13:34:26.151 |  |  |  |  | →SIP 100 Trying | P-CSCF
396 | 13:34:26.153 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 100 Trying |  |  |  |
397 | 13:34:26.353 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
398 | 13:34:26.358 |  |  |  |  | →SIP 200 OK | P-CSCF
399 | 13:34:26.395 |  |  |  |  | XML→ | Media-Server
400 | 13:34:26.403 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:591: 200 OK Verdict: Pass
401 | 13:34:26.403 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:379: Step 1 Verdict: Pass
402 | 13:34:26.408 |  |  |  |  | ←SIP ACK | P-CSCF
403 | 13:34:26.411 |  |  |  |  | ←SIP BYE | P-CSCF
404 | 13:34:26.415 |  | ←enobeB PCAP frame← SIP over IPSEC: ACK sip:PublicUserId-A@192.168.3.2:47229;transport... |  |  |
405 | 13:34:26.418 |  | ←enobeB PCAP frame← SIP over IPSEC: BYE sip:PublicUserId-A@192.168.3.2:47229;transport... |  |  |
406 | 13:34:26.536 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
407 | 13:34:26.537 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x3) |  |  |
408 | 13:34:26.537 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
409 | 13:34:26.538 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
410 | 13:34:26.585 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
411 | 13:34:26.585 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
412 | 13:34:26.585 |  | →RRC DCCH UL Information Transfer |  |  |
413 | 13:34:26.585 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x8) |  |  |
414 | 13:34:26.585 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
415 | 13:34:26.656 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
416 | 13:34:26.831 |  |  |  |  | →SIP 200 OK | P-CSCF
417 | 13:34:26.833 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
418 | 13:34:27.625 | →enobeB PCAP frame→ |  |  |  |
419 | 13:34:28.840 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
420 | 13:34:28.866 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
421 | 13:34:28.867 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xa) |  |  |
422 | 13:34:28.867 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
423 | 13:34:28.868 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
424 | 13:34:28.905 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
425 | 13:34:28.905 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
426 | 13:34:28.905 |  | →RRC DCCH UL Information Transfer |  |  |
427 | 13:34:28.905 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xa) |  |  |
428 | 13:34:28.905 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
429 | 13:34:28.976 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
430 | 13:34:28.977 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
431 | 13:34:29.016 |  | ←RRC DCCH RRC Connection Release |  |  |
432 | 13:34:29.017 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
433 | 13:34:29.031 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
434 | 13:34:29.032 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:385: Step 5 Verdict: Pass
435 | 13:34:29.034 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
436 | 13:34:29.036 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
437 | 13:34:29.784 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.