MSG #34 2021-09-28 13:33:42.825

NAS

     EMM: Authentication response
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x1 (Integrity protected)
    Auth code = 0x4523823e
    Sequence number = 0x0a
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x0 (Plain NAS message, not security protected)
    Message type = 0x53 (Authentication response)
    Authentication response parameter:
      Length = 8
      Data = e9 bb 02 36 aa b7 b9 96