MSG #428 2021-09-28 13:34:28.905
NAS

     ESM: Deactivate EPS bearer context accept
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x2 (Integrity protected and ciphered)
    Auth code = 0xd947b28e
    Sequence number = 0x06
    Protocol discriminator = 0x2 (EPS Session Management)
    EPS bearer identity = 6
    Procedure transaction identity = 0
    Message type = 0xce (Deactivate EPS bearer context accept)