ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 13:50:14.777 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 13:50:14.781 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 13:50:14.781 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 13:50:14.783 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 13:50:14.784 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 13:50:14.785 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:824: IMS UDP port 192.168.2.3:5060 configured
7 | 13:50:14.787 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:774: IMS TCP port 192.168.2.3:5060 configured!
8 | 13:50:14.789 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:795: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 13:50:14.789 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:806: IdM port 192.168.2.3:8080 configured!
10 | 13:50:14.791 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 13:50:15.992 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 13:50:15.994 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 13:50:26.213 |  | ←RRC BCCH SIB |  |  |
14 | 13:50:26.218 |  | ←RRC BCCH SIB1 |  |  |
15 | 13:50:26.298 |  | ←RRC BCCH SIB1 |  |  |
16 | 13:50:26.373 |  | ←RRC BCCH SIB |  |  |
17 | 13:50:26.378 |  | ←RRC BCCH SIB1 |  |  |
18 | 13:51:37.252 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 13:51:37.252 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 13:51:37.252 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 13:51:37.252 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 13:51:37.314 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 13:51:37.314 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 13:51:37.314 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 13:51:37.314 |  |  |  | →NAS EMM Attach request |  |
26 | 13:51:37.314 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 13:51:37.314 |  |  |  | NAS K-asme f5d7ade570e94e3e877c9e06242dc008... |  |
28 | 13:51:37.314 |  |  |  | NAS ← EMM Authentication request |  |
29 | 13:51:37.314 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 13:51:37.314 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 13:51:37.316 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 13:51:37.385 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 13:51:37.385 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 13:51:37.385 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 13:51:37.386 |  |  |  | →NAS EMM Authentication response |  |
36 | 13:51:37.386 |  |  |  | NAS UE auth OK |  |
37 | 13:51:37.386 |  |  |  | NAS K-nas-cip 85ee06b29184ac55cf58054910526... |  |
38 | 13:51:37.386 |  |  |  | NAS K-nas-int 78b768a3afb34d141cf2eca130207... |  |
39 | 13:51:37.386 |  |  |  | NAS ← EMM Security mode command |  |
40 | 13:51:37.386 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 13:51:37.386 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 13:51:37.388 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 13:51:37.426 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
44 | 13:51:37.426 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 13:51:37.426 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xa) |  |  |
46 | 13:51:37.426 |  |  |  | →NAS EMM Security mode complete |  |
47 | 13:51:37.426 |  |  |  | NAS ← ESM ESM information request |  |
48 | 13:51:37.426 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x9) |  |  |
49 | 13:51:37.426 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 13:51:37.427 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
51 | 13:51:37.473 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
52 | 13:51:37.473 |  | →RRC DCCH UL Information Transfer |  |  |
53 | 13:51:37.473 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x8) |  |  |
54 | 13:51:37.474 |  |  |  | →NAS ESM ESM information response |  |
55 | 13:51:37.474 |  |  |  | NAS ← EMM Attach accept |  |
56 | 13:51:37.474 |  |  |  | NAS K-enb 53dad7fccd09ca5d4d0bd61a0a65f0526... |  |
57 | 13:51:37.474 |  |  | RRC K-enb 53dad7fccd09ca5d4d0bd61a0a65f0526... |  |  |
58 | 13:51:37.474 |  |  | RRC rrc-cip 85beec36c375dad5c16eb43f7ec893f... |  |  |
59 | 13:51:37.474 |  |  | RRC rrc-int 2dbda56bef507cf7608a959790b7183... |  |  |
60 | 13:51:37.474 |  |  | RRC up-cip 26d6824d6b0b526ddc55aaf6db42b13f... |  |  |
61 | 13:51:37.474 |  |  | RRC up-int bd1451f02fd610921cc746ddfa803df7... |  |  |
62 | 13:51:37.474 |  | ←RRC DCCH Security Mode Command |  |  |
63 | 13:51:37.475 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
64 | 13:51:37.505 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
65 | 13:51:37.505 |  | →RRC DCCH Security Mode Complete |  |  |
66 | 13:51:37.505 |  | ←RRC DCCH UE Capability Enquiry |  |  |
67 | 13:51:37.505 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
68 | 13:51:37.555 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
69 | 13:51:37.555 |  | →RRC DCCH UE Capability Information |  |  |
70 | 13:51:37.556 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xa) |  |  |
71 | 13:51:37.556 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
72 | 13:51:37.556 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
73 | 13:51:37.586 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
74 | 13:51:37.586 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
75 | 13:51:37.625 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
76 | 13:51:37.625 |  | →RRC DCCH UL Information Transfer |  |  |
77 | 13:51:37.625 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x8) |  |  |
78 | 13:51:37.626 |  |  |  | →NAS EMM Attach complete |  |
79 | 13:51:37.626 |  |  |  | NAS ← EMM EMM information |  |
80 | 13:51:37.627 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xa) |  |  |
81 | 13:51:37.627 |  | ←RRC DCCH DL Information Transfer |  |  |
82 | 13:51:37.627 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
83 | 13:51:43.215 |  | ←RRC DCCH RRC Connection Release |  |  |
84 | 13:51:43.217 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
85 | 13:51:44.543 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
86 | 13:51:44.543 |  | →RRC CCCH RRC Connection Request |  |  |
87 | 13:51:44.543 |  | ←RRC CCCH RRC Connection Setup |  |  |
88 | 13:51:44.543 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
89 | 13:51:44.585 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
90 | 13:51:44.585 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
91 | 13:51:44.585 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
92 | 13:51:44.585 |  |  |  | →NAS EMM Service request |  |
93 | 13:51:44.585 |  |  |  | NAS K-enb b5dd8006d834be2ffe7fd952b17e8ec8d... |  |
94 | 13:51:44.587 |  |  | RRC K-enb b5dd8006d834be2ffe7fd952b17e8ec8d... |  |  |
95 | 13:51:44.587 |  |  | RRC rrc-cip 02e05eaade088d0f79932bf6e8725c5... |  |  |
96 | 13:51:44.587 |  |  | RRC rrc-int d2b3531c482035f72c351a23f501ab9... |  |  |
97 | 13:51:44.587 |  |  | RRC up-cip a6a9d1eddbdf4aef55b010e670f5afbd... |  |  |
98 | 13:51:44.587 |  |  | RRC up-int eebcaec7f6968890b17ae5d1547117e2... |  |  |
99 | 13:51:44.587 |  | ←RRC DCCH Security Mode Command |  |  |
100 | 13:51:44.587 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
101 | 13:51:44.625 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
102 | 13:51:44.625 |  | →RRC DCCH Security Mode Complete |  |  |
103 | 13:51:44.625 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
104 | 13:51:44.625 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
105 | 13:51:44.665 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
106 | 13:51:44.665 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
107 | 13:52:03.426 | →enobeB PCAP frame→ TCP |  |  |  |
108 | 13:52:03.429 |  | ←enobeB PCAP frame← TCP |  |  |
109 | 13:52:03.465 | →enobeB PCAP frame→ TCP |  |  |  |
110 | 13:52:03.553 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
111 | 13:52:03.556 |  | ←enobeB PCAP frame← TCP |  |  |
112 | 13:52:03.562 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
113 | 13:52:03.585 | →enobeB PCAP frame→ TCP |  |  |  |
114 | 13:52:03.712 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 16)
115 | 13:52:03.714 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
116 | 13:52:03.716 |  | ←enobeB PCAP frame← TCP |  |  |
117 | 13:52:03.717 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
118 | 13:52:03.746 | →enobeB PCAP frame→ TCP |  |  |  |
119 | 13:52:03.752 |  |  |  |  | →HTTP GET | HTTP-Proxy
120 | 13:52:03.754 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
121 | 13:52:03.757 |  | ←enobeB PCAP frame← TCP |  |  |
122 | 13:52:03.759 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:301: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
123 | 13:52:03.777 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
124 | 13:52:03.786 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
125 | 13:52:03.825 | →enobeB PCAP frame→ TCP |  |  |  |
126 | 13:52:05.666 | →enobeB PCAP frame→ TCP |  |  |  |
127 | 13:52:05.669 |  | ←enobeB PCAP frame← TCP |  |  |
128 | 13:52:05.705 | →enobeB PCAP frame→ TCP |  |  |  |
129 | 13:52:05.714 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
130 | 13:52:05.717 |  | ←enobeB PCAP frame← TCP |  |  |
131 | 13:52:05.726 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
132 | 13:52:05.745 | →enobeB PCAP frame→ TCP |  |  |  |
133 | 13:52:05.992 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
134 | 13:52:05.994 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
135 | 13:52:05.997 |  | ←enobeB PCAP frame← TCP |  |  |
136 | 13:52:05.997 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
137 | 13:52:06.025 | →enobeB PCAP frame→ TCP |  |  |  |
138 | 13:52:06.032 |  |  |  |  | →HTTP GET | IDMS-Endpoint
139 | 13:52:06.033 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
140 | 13:52:06.036 |  | ←enobeB PCAP frame← TCP |  |  |
141 | 13:52:06.060 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
142 | 13:52:06.064 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:524: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
143 | 13:52:06.064 |  |  |  |  | MMICmd: Please provide user credentials: username and password
144 | 13:52:06.068 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
145 | 13:52:06.145 | →enobeB PCAP frame→ TCP |  |  |  |
146 | 13:52:10.353 | →enobeB PCAP frame→ HTTPS: POST /idms/userauth HTTP/1.1 |  |  |  |
147 | 13:52:10.353 |  |  |  |  | →HTTP POST | IDMS-Endpoint
148 | 13:52:10.356 |  | ←enobeB PCAP frame← TCP |  |  |
149 | 13:52:10.368 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
150 | 13:52:10.371 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:529: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
151 | 13:52:10.375 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
152 | 13:52:10.423 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:693: IdM port - Client closed the connection (id 18)
153 | 13:52:10.425 | →enobeB PCAP frame→ TCP |  |  |  |
154 | 13:52:10.428 |  | ←enobeB PCAP frame← TCP |  |  |
155 | 13:52:10.465 | →enobeB PCAP frame→ TCP |  |  |  |
156 | 13:52:11.226 | →enobeB PCAP frame→ TCP |  |  |  |
157 | 13:52:11.228 |  | ←enobeB PCAP frame← TCP |  |  |
158 | 13:52:11.266 | →enobeB PCAP frame→ TCP |  |  |  |
159 | 13:52:11.354 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
160 | 13:52:11.356 |  | ←enobeB PCAP frame← TCP |  |  |
161 | 13:52:11.357 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
162 | 13:52:11.386 | →enobeB PCAP frame→ TCP |  |  |  |
163 | 13:52:11.471 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
164 | 13:52:11.473 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
165 | 13:52:11.476 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
166 | 13:52:11.505 | →enobeB PCAP frame→ TCP |  |  |  |
167 | 13:52:11.520 |  |  |  |  | →HTTP POST | IDMS-Endpoint
168 | 13:52:11.524 |  | ←enobeB PCAP frame← TCP |  |  |
169 | 13:52:11.559 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
170 | 13:52:11.561 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:534: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
171 | 13:52:11.566 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
172 | 13:52:11.908 |  | ←enobeB PCAP frame← TCP |  |  |
173 | 13:52:11.945 | →enobeB PCAP frame→ TCP |  |  |  |
174 | 13:52:11.953 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
175 | 13:52:11.956 |  | ←enobeB PCAP frame← TCP |  |  |
176 | 13:52:11.959 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
177 | 13:52:11.985 | →enobeB PCAP frame→ TCP |  |  |  |
178 | 13:52:11.992 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 19)
179 | 13:52:11.994 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
180 | 13:52:11.996 |  | ←enobeB PCAP frame← TCP |  |  |
181 | 13:52:11.997 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
182 | 13:52:12.034 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
183 | 13:52:12.034 |  |  |  |  | →HTTP POST | HTTP-Proxy
184 | 13:52:12.036 |  | ←enobeB PCAP frame← TCP |  |  |
185 | 13:52:12.061 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:554: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
186 | 13:52:12.067 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
187 | 13:52:12.075 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
188 | 13:52:12.075 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
189 | 13:52:12.105 | →enobeB PCAP frame→ TCP |  |  |  |
190 | 13:52:12.145 | →enobeB PCAP frame→ TCP |  |  |  |
191 | 13:52:12.148 |  | ←enobeB PCAP frame← TCP |  |  |
192 | 13:52:12.185 | →enobeB PCAP frame→ TCP |  |  |  |
193 | 13:52:12.193 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
194 | 13:52:12.197 |  | ←enobeB PCAP frame← TCP |  |  |
195 | 13:52:12.199 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
196 | 13:52:12.226 | →enobeB PCAP frame→ TCP |  |  |  |
197 | 13:52:12.232 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 20)
198 | 13:52:12.234 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
199 | 13:52:12.236 |  | ←enobeB PCAP frame← TCP |  |  |
200 | 13:52:12.237 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
201 | 13:52:12.273 |  |  |  |  | →HTTP POST | HTTP-Proxy
202 | 13:52:12.274 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
203 | 13:52:12.276 |  | ←enobeB PCAP frame← TCP |  |  |
204 | 13:52:12.334 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
205 | 13:52:12.334 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:558: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
206 | 13:52:12.340 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
207 | 13:52:12.385 | →enobeB PCAP frame→ TCP |  |  |  |
208 | 13:52:12.441 |  |  |  |  | →SIP REGISTER | P-CSCF
209 | 13:52:12.464 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:833: IMS UDP_s port 192.168.2.3:5062 configured
210 | 13:52:12.468 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:784: IMS TCP_s port 192.168.2.3:5062 configured!
211 | 13:52:12.471 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:842: IMS UDP_c port 192.168.2.3:5061 configured
212 | 13:52:12.482 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
213 | 13:52:13.242 |  |  |  |  | →SIP REGISTER | P-CSCF
214 | 13:52:13.267 |  |  |  |  | ←SIP 200 OK | P-CSCF
215 | 13:52:13.274 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
216 | 13:52:13.635 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
217 | 13:52:13.644 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
218 | 13:52:13.695 |  |  |  |  | MIKEY | Media-Server
219 | 13:52:13.696 |  |  |  |  | ←SIP 200 OK | P-CSCF
220 | 13:52:13.702 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
221 | 13:52:13.903 |  |  |  |  | XML→ | Media-Server
222 | 13:52:13.905 |  |  |  |  | XML→ | Media-Server
223 | 13:52:13.908 |  |  |  |  | ←XML | Media-Server
224 | 13:52:13.911 |  |  |  |  | ←SIP NOTIFY | P-CSCF
225 | 13:52:13.919 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:39408;transp... |  |  |
226 | 13:52:13.951 |  |  |  |  | →SIP 200 OK | P-CSCF
227 | 13:52:13.954 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
228 | 13:52:14.266 | →enobeB PCAP frame→ TCP |  |  |  |
229 | 13:52:14.268 |  | ←enobeB PCAP frame← TCP |  |  |
230 | 13:52:14.305 | →enobeB PCAP frame→ TCP |  |  |  |
231 | 13:52:14.314 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
232 | 13:52:14.317 |  | ←enobeB PCAP frame← TCP |  |  |
233 | 13:52:14.322 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
234 | 13:52:14.345 | →enobeB PCAP frame→ TCP |  |  |  |
235 | 13:52:14.392 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
236 | 13:52:14.394 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
237 | 13:52:14.396 |  | ←enobeB PCAP frame← TCP |  |  |
238 | 13:52:14.397 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
239 | 13:52:14.425 | →enobeB PCAP frame→ TCP |  |  |  |
240 | 13:52:14.432 |  |  |  |  | →HTTP GET | HTTP-Proxy
241 | 13:52:14.433 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
242 | 13:52:14.437 |  | ←enobeB PCAP frame← TCP |  |  |
243 | 13:52:14.441 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:655: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcptt-ue-configuration.xml
244 | 13:52:14.449 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
245 | 13:52:14.456 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
246 | 13:52:14.545 | →enobeB PCAP frame→ TCP |  |  |  |
247 | 13:52:14.551 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
248 | 13:52:14.553 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
249 | 13:52:14.556 |  | ←enobeB PCAP frame← TCP |  |  |
250 | 13:52:14.586 | →enobeB PCAP frame→ TCP |  |  |  |
251 | 13:52:14.705 | →enobeB PCAP frame→ TCP |  |  |  |
252 | 13:52:14.708 |  | ←enobeB PCAP frame← TCP |  |  |
253 | 13:52:14.745 | →enobeB PCAP frame→ TCP |  |  |  |
254 | 13:52:14.754 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
255 | 13:52:14.757 |  | ←enobeB PCAP frame← TCP |  |  |
256 | 13:52:14.760 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
257 | 13:52:14.785 | →enobeB PCAP frame→ TCP |  |  |  |
258 | 13:52:14.872 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
259 | 13:52:14.874 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
260 | 13:52:14.877 |  | ←enobeB PCAP frame← TCP |  |  |
261 | 13:52:14.877 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
262 | 13:52:14.905 | →enobeB PCAP frame→ TCP |  |  |  |
263 | 13:52:14.952 |  |  |  |  | →HTTP GET | HTTP-Proxy
264 | 13:52:14.953 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
265 | 13:52:14.956 |  | ←enobeB PCAP frame← TCP |  |  |
266 | 13:52:14.966 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:660: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcptt-user-profile-49.xml
267 | 13:52:15.008 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
268 | 13:52:15.019 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
269 | 13:52:15.020 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
270 | 13:52:15.065 | →enobeB PCAP frame→ TCP |  |  |  |
271 | 13:52:15.071 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
272 | 13:52:15.073 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
273 | 13:52:15.076 |  | ←enobeB PCAP frame← TCP |  |  |
274 | 13:52:15.105 | →enobeB PCAP frame→ TCP |  |  |  |
275 | 13:52:15.713 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
276 | 13:52:15.715 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
277 | 13:52:15.719 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
278 | 13:52:15.733 |  |  |  |  | ←SIP 200 OK | P-CSCF
279 | 13:52:15.733 |  |  |  |  | MIKEY | Media-Server
280 | 13:52:15.739 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
281 | 13:52:15.865 | →enobeB PCAP frame→ TCP |  |  |  |
282 | 13:52:15.868 |  | ←enobeB PCAP frame← TCP |  |  |
283 | 13:52:15.906 | →enobeB PCAP frame→ TCP |  |  |  |
284 | 13:52:15.914 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
285 | 13:52:15.916 |  | ←enobeB PCAP frame← TCP |  |  |
286 | 13:52:15.918 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
287 | 13:52:15.938 |  |  |  |  | XML→ | Media-Server
288 | 13:52:15.940 |  |  |  |  | XML→ | Media-Server
289 | 13:52:15.944 |  |  |  |  | ←XML | Media-Server
290 | 13:52:15.945 | →enobeB PCAP frame→ TCP |  |  |  |
291 | 13:52:15.991 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
292 | 13:52:15.991 |  |  |  |  | ←SIP NOTIFY | P-CSCF
293 | 13:52:15.994 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
294 | 13:52:15.997 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
295 | 13:52:15.997 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:39408;transp... |  |  |
296 | 13:52:16.033 |  |  |  |  | →SIP 200 OK | P-CSCF
297 | 13:52:16.033 |  |  |  |  | →HTTP GET | HTTP-Proxy
298 | 13:52:16.034 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
299 | 13:52:16.037 |  | ←enobeB PCAP frame← TCP |  |  |
300 | 13:52:16.041 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:665: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
301 | 13:52:16.047 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
302 | 13:52:16.055 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
303 | 13:52:16.065 | →enobeB PCAP frame→ TCP |  |  |  |
304 | 13:52:16.103 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
305 | 13:52:16.106 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
306 | 13:52:16.109 |  | ←enobeB PCAP frame← TCP |  |  |
307 | 13:52:16.145 | →enobeB PCAP frame→ TCP |  |  |  |
308 | 13:52:16.225 | →enobeB PCAP frame→ TCP |  |  |  |
309 | 13:52:16.229 |  | ←enobeB PCAP frame← TCP |  |  |
310 | 13:52:16.265 | →enobeB PCAP frame→ TCP |  |  |  |
311 | 13:52:16.274 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
312 | 13:52:16.276 |  | ←enobeB PCAP frame← TCP |  |  |
313 | 13:52:16.281 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
314 | 13:52:16.305 | →enobeB PCAP frame→ TCP |  |  |  |
315 | 13:52:16.391 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
316 | 13:52:16.393 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
317 | 13:52:16.397 |  | ←enobeB PCAP frame← TCP |  |  |
318 | 13:52:16.397 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
319 | 13:52:16.425 | →enobeB PCAP frame→ TCP |  |  |  |
320 | 13:52:16.472 |  |  |  |  | →HTTP GET | HTTP-Proxy
321 | 13:52:16.474 | →enobeB PCAP frame→ HTTPS: GET http://xcap.gms.mcstaasting.com/org.openmobile... |  |  |  |
322 | 13:52:16.476 |  | ←enobeB PCAP frame← TCP |  |  |
323 | 13:52:16.484 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:670: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at http://xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
324 | 13:52:16.510 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
325 | 13:52:16.519 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
326 | 13:52:16.521 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
327 | 13:52:16.546 | →enobeB PCAP frame→ TCP |  |  |  |
328 | 13:52:16.551 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
329 | 13:52:16.554 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
330 | 13:52:16.557 |  | ←enobeB PCAP frame← TCP |  |  |
331 | 13:52:16.585 | →enobeB PCAP frame→ TCP |  |  |  |
332 | 13:52:16.674 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
333 | 13:52:16.675 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
334 | 13:52:16.684 |  |  |  |  | →SIP PUBLISH | P-CSCF
335 | 13:52:16.730 |  |  |  |  | MIKEY | Media-Server
336 | 13:52:16.754 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
337 | 13:52:16.755 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
338 | 13:52:16.756 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
339 | 13:52:16.945 |  |  |  |  | XML→ | Media-Server
340 | 13:52:16.949 |  |  |  |  | ←SIP 200 OK | P-CSCF
341 | 13:52:16.952 |  |  |  |  | ←SIP 200 OK | P-CSCF
342 | 13:52:16.952 |  |  |  |  | MIKEY | Media-Server
343 | 13:52:16.954 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
344 | 13:52:16.958 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
345 | 13:52:17.146 |  |  |  |  | XML→ | Media-Server
346 | 13:52:17.147 |  |  |  |  | XML→ | Media-Server
347 | 13:52:17.181 |  |  |  |  | MIKEY | Media-Server
348 | 13:52:17.182 |  |  |  |  | ←XML | Media-Server
349 | 13:52:17.187 |  |  |  |  | ←SIP NOTIFY | P-CSCF
350 | 13:52:17.193 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:39408;transp... |  |  |
351 | 13:52:17.232 |  |  |  |  | →SIP 200 OK | P-CSCF
352 | 13:52:17.234 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
353 | 13:52:17.242 |  |  |  |  | ←XML | Media-Server
354 | 13:52:17.262 |  |  |  |  | ←SIP MESSAGE | P-CSCF
355 | 13:52:17.269 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
356 | 13:52:18.040 |  |  |  |  | →SIP 200 OK | P-CSCF
357 | 13:52:18.047 |  |  |  |  | Info: MCX_IMS_CommonProcedures.ttcn:228: MESSAGE/200OK Table 5.3.2.3-2 Steps 7-8 Done
358 | 13:52:20.050 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
359 | 13:52:20.099 |  | ←RRC DCCH RRC Connection Release |  |  |
360 | 13:52:20.100 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
361 | 13:52:20.115 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
362 | 13:52:20.116 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
363 | 13:52:20.116 |  |  |  |  | MMICmd: Make the UE (MCPTT User) request the establishment of an MCPTT private emergency call, force of automatic commencement mode, without Floor Control
364 | 13:52:28.322 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
365 | 13:52:28.322 |  | →RRC CCCH RRC Connection Request |  |  |
366 | 13:52:28.322 |  | ←RRC CCCH RRC Connection Setup |  |  |
367 | 13:52:28.322 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
368 | 13:52:28.385 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
369 | 13:52:28.385 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
370 | 13:52:28.385 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
371 | 13:52:28.386 |  |  |  | →NAS EMM Service request |  |
372 | 13:52:28.386 |  |  |  | NAS K-enb 2800936143b293cd7af42f9923f922acf... |  |
373 | 13:52:28.387 |  |  | RRC K-enb 2800936143b293cd7af42f9923f922acf... |  |  |
374 | 13:52:28.387 |  |  | RRC rrc-cip ec67a38af646c1db738737741bd61b5... |  |  |
375 | 13:52:28.387 |  |  | RRC rrc-int dbca5cd6fe2ed51231f19c2f2cc8960... |  |  |
376 | 13:52:28.387 |  |  | RRC up-cip 21199434df532ec1fac209580d4bd380... |  |  |
377 | 13:52:28.387 |  |  | RRC up-int 35cc98fedcc2c1270f7aaf86db3594ba... |  |  |
378 | 13:52:28.387 |  | ←RRC DCCH Security Mode Command |  |  |
379 | 13:52:28.387 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
380 | 13:52:28.426 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
381 | 13:52:28.426 |  | →RRC DCCH Security Mode Complete |  |  |
382 | 13:52:28.426 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
383 | 13:52:28.426 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
384 | 13:52:28.466 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
385 | 13:52:28.466 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
386 | 13:52:28.474 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
387 | 13:52:28.475 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |  |
388 | 13:52:28.476 |  |  |  |  | →SIP INVITE | P-CSCF
389 | 13:52:28.490 |  |  |  |  | MIKEY | Media-Server
390 | 13:52:28.690 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:754: SRTP config: Master Key: CD7F26B065C50ECA1DFDC94566FD3659, Master Salt: D038496754D5A3DADF0EA3A9, MKI: 2B49DEBC
391 | 13:52:28.690 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
392 | 13:52:28.694 |  |  |  |  | XML→ | Media-Server
393 | 13:52:28.694 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
394 | 13:52:28.695 |  |  |  |  | XML→ | Media-Server
395 | 13:52:28.698 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1233: INVITE Verdict: Pass
396 | 13:52:28.699 |  |  |  |  | ←SIP 100 Trying | P-CSCF
397 | 13:52:28.701 |  |  |  |  | ←SIP 200 OK | P-CSCF
398 | 13:52:28.704 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
399 | 13:52:28.706 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
400 | 13:52:29.327 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
401 | 13:52:29.329 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x9) |  |  |
402 | 13:52:29.329 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
403 | 13:52:29.329 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
404 | 13:52:29.386 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
405 | 13:52:29.386 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
406 | 13:52:29.386 |  | →RRC DCCH UL Information Transfer |  |  |
407 | 13:52:29.386 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x8) |  |  |
408 | 13:52:29.386 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
409 | 13:52:29.448 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
410 | 13:52:29.672 |  |  |  |  | →SIP ACK | P-CSCF
411 | 13:52:29.673 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
412 | 13:52:29.682 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1236: ACK Verdict: Pass
413 | 13:52:29.682 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:409: Step 2 Verdict: Pass
414 | 13:52:30.225 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
415 | 13:52:30.233 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
416 | 13:52:30.265 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
417 | 13:52:30.274 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
418 | 13:52:30.305 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
419 | 13:52:30.433 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:414: Step 5 Verdict: Pass
420 | 13:52:30.538 |  |  |  |  | MMICmd: Release call (hang up the call)
421 | 13:52:32.473 |  |  |  |  | →SIP BYE | P-CSCF
422 | 13:52:32.493 |  |  |  |  | ←SIP 200 OK | P-CSCF
423 | 13:52:32.499 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
424 | 13:52:33.065 | →enobeB PCAP frame→ |  |  |  |
425 | 13:52:34.491 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
426 | 13:52:34.512 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
427 | 13:52:34.512 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xb) |  |  |
428 | 13:52:34.512 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
429 | 13:52:34.514 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
430 | 13:52:34.545 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
431 | 13:52:34.545 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
432 | 13:52:34.545 |  | →RRC DCCH UL Information Transfer |  |  |
433 | 13:52:34.545 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x3) |  |  |
434 | 13:52:34.546 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
435 | 13:52:34.628 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
436 | 13:52:34.629 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
437 | 13:52:34.679 |  | ←RRC DCCH RRC Connection Release |  |  |
438 | 13:52:34.680 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
439 | 13:52:34.694 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
440 | 13:52:34.696 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:420: Step 9 Verdict: Pass
441 | 13:52:34.697 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
442 | 13:52:34.699 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
443 | 13:52:35.447 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.