MSG #403 2021-09-28 13:52:29.329

    enobeB PCAP frame

    {
      "layers": {
        "frame": {
          "frame.encap_type": "45",
          "frame.time": "Sep 28, 2021 13:52:29.329992000 CEST",
          "frame.offset_shift": "0.000000000",
          "frame.time_epoch": "1632829949.329992000",
          "frame.time_delta": "0.010938000",
          "frame.time_delta_displayed": "0.623097000",
          "frame.time_relative": "123.111079000",
          "frame.number": "11302",
          "frame.len": "102",
          "frame.cap_len": "102",
          "frame.marked": "0",
          "frame.ignored": "0",
          "frame.protocols": "user_dlt:mac-lte-framed:mac-lte:rlc-lte:pdcp-lte:lte_rrc:nas-eps"
        },
        "user_dlt": "DLT: 147, Payload: mac-lte-framed (mac-lte-framed)",
        "mac-lte": {
          "mac-lte.context": "",
          "mac-lte.context_tree": {
            "mac-lte.radio-type": "1",
            "mac-lte.direction": "1",
            "mac-lte.ueid": "2952",
            "mac-lte.sfn": "967",
            "mac-lte.subframe": "6",
            "mac-lte.rnti": "3012",
            "mac-lte.rnti-type": "3",
            "mac-lte.is-predefined-frame": "0",
            "mac-lte.length": "77",
            "mac-lte.carrier-id": "0",
            "mac-lte.dl-tti-count": "1"
          },
          "mac-lte.dl-phy": "",
          "mac-lte.dl-phy_tree": {
            "mac-lte.dl-phy.dci-format": "2",
            "mac-lte.dl-phy.resource-allocation-type": "2",
            "mac-lte.dl-phy.aggregation-level": "0",
            "mac-lte.dl-phy.mcs-index": "27",
            "mac-lte.dl-phy.rv-index": "0",
            "mac-lte.dl-phy.dl-retx": "0",
            "mac-lte.dl-phy.rb-length": "1",
            "mac-lte.dl-phy.harq-id": "0",
            "mac-lte.dl-phy.ndi": "0",
            "mac-lte.dl-phy.tb": "0"
          },
          "mac-lte.dlsch.header": "",
          "mac-lte.dlsch.header_tree": {
            "mac-lte.sch.subheader": "",
            "mac-lte.sch.subheader_tree": {
              "mac-lte.sch.reserved": "0x00000000",
              "mac-lte.sch.format2": "0",
              "mac-lte.sch.extended": "0x00000000",
              "mac-lte.dlsch.lcid": "0x0000001f"
            }
          },
          "mac-lte.sch.header-only": "0",
          "mac-lte.sch.sdu": "a0:02:02:37:e8:53:89:ae:e1:9c:c1:11:ae:01:f7:e6:4a:2b:18:48:7f:eb:6c:19:d6:68:e0:d8:9f:50:de:86:b3:47:95:c7:6c:59:c0:d8:28:26:8b:41:09:f0:7d:9c:40:35:01:ae:37:67:7b:9f:9b:35:73:d7:07:e2:49:85:98:68:88:fd:0d:8d:83:96:8c",
          "rlc-lte": {
            "rlc-lte.context": "",
            "rlc-lte.context_tree": {
              "rlc-lte.direction": "1",
              "rlc-lte.mode": "4",
              "rlc-lte.ueid": "2952",
              "rlc-lte.channel-type": "4",
              "rlc-lte.channel-id": "1",
              "rlc-lte.pdu-length": "73",
              "rlc-lte.am-seqnum-length": "10"
            },
            "rlc-lte.am": "",
            "rlc-lte.am.header": "",
            "rlc-lte.am.header_tree": {
              "rlc-lte.am.frame-type": "0x00000001",
              "rlc-lte.am.rf": "0x00000000",
              "rlc-lte.am.p": "0x00000001",
              "rlc-lte.am.fi": "0x00000000",
              "rlc-lte.am.fixed.e": "0x00000000",
              "rlc-lte.am.fixed.sn": "2"
            },
            "rlc-lte.sequence-analysis": "",
            "rlc-lte.sequence-analysis_tree": {
              "rlc-lte.sequence-analysis.previous-frame": "11211",
              "rlc-lte.sequence-analysis.ok": "1"
            },
            "rlc-lte.am.data": "02:37:e8:53:89:ae:e1:9c:c1:11:ae:01:f7:e6:4a:2b:18:48:7f:eb:6c:19:d6:68:e0:d8:9f:50:de:86:b3:47:95:c7:6c:59:c0:d8:28:26:8b:41:09:f0:7d:9c:40:35:01:ae:37:67:7b:9f:9b:35:73:d7:07:e2:49:85:98:68:88:fd:0d:8d:83:96:8c",
            "pdcp-lte": {
              "pdcp-lte.configuration": "",
              "pdcp-lte.configuration_tree": {
                "pdcp-lte.direction": "1",
                "pdcp-lte.plane": "1",
                "pdcp-lte.ueid": "2952",
                "pdcp-lte.channel-type": "1",
                "pdcp-lte.channel-id": "1",
                "pdcp-lte.rohc.compression": "0"
              },
              "pdcp-lte.security-config": "",
              "pdcp-lte.security-config_tree": {
                "pdcp-lte.security-config.setup-frame": "11207",
                "pdcp-lte.security-config.ciphering": "2",
                "pdcp-lte.security-config.integrity": "2",
                "pdcp-lte.security-config.bearer": "0",
                "pdcp-lte.security-config.direction": "1",
                "pdcp-lte.security-config.count": "2",
                "pdcp-lte.security-config.cipher-key": "ec67a38af646c1db738737741bd61b52",
                "pdcp-lte.security-config.integrity-key": "dbca5cd6fe2ed51231f19c2f2cc89609"
              },
              "pdcp-lte.reserved": "0",
              "pdcp-lte.seq-num": "2",
              "pdcp-lte.sequence-analysis": "",
              "pdcp-lte.sequence-analysis_tree": {
                "pdcp-lte.sequence-analysis.previous-frame": "11211",
                "pdcp-lte.sequence-analysis.expected-sn": "2",
                "pdcp-lte.sequence-analysis.ok": "1"
              },
              "lte_rrc": {
                "lte_rrc": "LTE Radio Resource Control (RRC) protocol",
                "lte-rrc.DL_DCCH_Message_element": {
                  "per.choice_index": "0",
                  "lte-rrc.message": "0",
                  "lte-rrc.message_tree": {
                    "per.choice_index": "4",
                    "lte-rrc.c1": "4",
                    "lte-rrc.c1_tree": {
                      "lte_rrc": "LTE Radio Resource Control (RRC) protocol",
                      "lte-rrc.rrcConnectionReconfiguration_element": {
                        "lte-rrc.rrc_TransactionIdentifier": "0",
                        "per.choice_index": "0",
                        "lte-rrc.criticalExtensions": "0",
                        "lte-rrc.criticalExtensions_tree": {
                          "per.choice_index": "0",
                          "lte-rrc.c1": "0",
                          "lte-rrc.c1_tree": {
                            "lte-rrc.rrcConnectionReconfiguration_r8_element": {
                              "per.optional_field_bit": "0",
                              "per.sequence_of_length": "1",
                              "lte-rrc.dedicatedInfoNASList": "1",
                              "lte-rrc.dedicatedInfoNASList_tree": {
                                "Item 0": {
                                  "per.octet_string_length": "54",
                                  "lte-rrc.DedicatedInfoNAS": "27:0d:7e:d5:cb:04:97:c8:a8:08:ea:90:04:31:a5:42:2f:4f:78:fa:9d:15:d8:d6:c3:42:38:5d:9e:c0:de:f0:ad:77:ad:24:5a:5f:08:7e:a1:a2:a1:15:95:39:61:3e:ab:65:1b:59:51:c9",
                                  "lte-rrc.DedicatedInfoNAS_tree": {
                                    "nas-eps": {
                                      "nas_eps.security_header_type": "2",
                                      "gsm_a.L3_protocol_discriminator": "0x00000007",
                                      "nas_eps.msg_auth_code": "0x0d7ed5cb",
                                      "nas_eps.seq_no": "4",
                                      "nas_eps.ciphered_msg": "97:c8:a8:08:ea:90:04:31:a5:42:2f:4f:78:fa:9d:15:d8:d6:c3:42:38:5d:9e:c0:de:f0:ad:77:ad:24:5a:5f:08:7e:a1:a2:a1:15:95:39:61:3e:ab:65:1b:59:51:c9"
                                    }
                                  }
                                }
                              },
                              "lte-rrc.radioResourceConfigDedicated_element": {
                                "per.extension_bit": "0",
                                "per.optional_field_bit": "0",
                                "per.sequence_of_length": "1",
                                "lte-rrc.drb_ToAddModList": "1",
                                "lte-rrc.drb_ToAddModList_tree": {
                                  "Item 0": {
                                    "lte-rrc.DRB_ToAddMod_element": {
                                      "per.extension_bit": "0",
                                      "per.optional_field_bit": "1",
                                      "lte-rrc.eps_BearerIdentity": "6",
                                      "lte-rrc.drb_Identity": "2",
                                      "lte-rrc.pdcp_Config_element": {
                                        "per.extension_bit": "0",
                                        "per.optional_field_bit": "1",
                                        "per.enum_index": "1",
                                        "lte-rrc.discardTimer": "1",
                                        "lte-rrc.rlc_UM_element": {
                                          "per.enum_index": "1",
                                          "lte-rrc.pdcp_SN_Size": "1"
                                        },
                                        "per.choice_index": "0",
                                        "lte-rrc.headerCompression": "0",
                                        "lte-rrc.headerCompression_tree": {
                                          "lte-rrc.notUsed_element": ""
                                        }
                                      },
                                      "per.choice_index": "1",
                                      "lte-rrc.rlc_Config": "1",
                                      "lte-rrc.rlc_Config_tree": {
                                        "lte-rrc.um_Bi_Directional_element": {
                                          "lte-rrc.ul_UM_RLC_element": {
                                            "per.enum_index": "1",
                                            "lte-rrc.sn_FieldLength": "1"
                                          },
                                          "lte-rrc.dl_UM_RLC_element": {
                                            "per.enum_index": "10",
                                            "lte-rrc.sn_FieldLength": "1",
                                            "lte-rrc.t_Reordering": "10"
                                          }
                                        }
                                      },
                                      "lte-rrc.logicalChannelIdentity": "4",
                                      "lte-rrc.logicalChannelConfig_element": {
                                        "per.extension_bit": "0",
                                        "per.optional_field_bit": "1",
                                        "lte-rrc.ul_SpecificParameters_element": {
                                          "per.optional_field_bit": "1",
                                          "lte-rrc.priority": "5",
                                          "per.enum_index": "1",
                                          "lte-rrc.prioritisedBitRate": "0",
                                          "lte-rrc.bucketSizeDuration": "1",
                                          "lte-rrc.logicalChannelGroup": "1"
                                        }
                                      }
                                    }
                                  }
                                }
                              }
                            }
                          }
                        }
                      }
                    }
                  }
                }
              },
              "pdcp-lte.mac": "0x997b0444"
            }
          },
          "mac-lte.padding-data": "00",
          "mac-lte.padding-length": "1"
        },
        "mac-lte.dlsch": "",
        "_ws.lua.fake": "",
        "nas_eea2": {
          "nas-eps": {
            "nas_eps.security_header_type": "2",
            "gsm_a.L3_protocol_discriminator": "0x00000002",
            "nas_eps.msg_auth_code": "0x0d7ed5cb",
            "nas_eps.seq_no": "4",
            "nas_eps.bearer_id": "6",
            "nas_eps.esm.proc_trans_id": "0",
            "nas_eps.nas_msg_esm_type": "197",
            "nas_eps.emm.spare_half_octet": "0",
            "nas_eps.esm.linked_bearer_id": "5",
            "EPS quality of service": {
              "gsm_a.len": "5",
              "nas_eps.esm.qci": "65",
              "nas_eps.esm.mbr_ul": "104",
              "nas_eps.esm.mbr_dl": "104",
              "nas_eps.esm.gbr_ul": "72",
              "nas_eps.esm.gbr_dl": "72"
            },
            "Traffic Flow Template": {
              "gsm_a.len": "37",
              "gsm_a.gm.sm.tft.op_code": "1",
              "gsm_a.gm.sm.tft.e_bit": "0",
              "gsm_a.gm.sm.tft.pkt_flt": "2",
              "gsm_a.gm.sm.tft.packet_filter": "1",
              "gsm_a.gm.sm.tft.packet_filter_tree": {
                "gsm_a.spare_bits": "0",
                "gsm_a.gm.sm.tft.pkt_flt_dir": "3",
                "gsm_a.gm.sm.tft.pkt_flt_id": "7",
                "gsm_a.gm.sm.tft.packet_evaluation_precedence": "0x00000001",
                "gsm_a.gm.sm.tft.packet_filter_length": "0x0000000e",
                "gsm_a.gm.sm.tft.packet_filter_component_type_id": "80",
                "gsm_a.gm.sm.tft.packet_filter_component_type_id_tree": {
                  "gsm_a.gm.sm.tft.port": "60354"
                }
              }
            }
          }
        },
        "_ws.col.Info": "RRCConnectionReconfiguration, Ciphered message",
        "_ws.col.Protocol": "LTE RRC DL_DCCH/NAS-EPS/NAS-EPS"
      }
    }