ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 13:57:55.621 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 13:57:55.627 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 13:57:55.628 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 13:57:55.631 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 13:57:55.633 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 13:57:55.635 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:824: IMS UDP port 192.168.2.3:5060 configured
7 | 13:57:55.643 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:774: IMS TCP port 192.168.2.3:5060 configured!
8 | 13:57:55.649 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:795: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 13:57:55.652 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:806: IdM port 192.168.2.3:8080 configured!
10 | 13:57:55.658 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 13:57:56.859 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 13:57:56.861 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 13:57:58.459 |  | ←RRC BCCH SIB1 |  |  |
14 | 13:57:58.533 |  | ←RRC BCCH SIB |  |  |
15 | 13:57:58.538 |  | ←RRC BCCH SIB1 |  |  |
16 | 13:57:58.554 |  | ←RRC BCCH SIB |  |  |
17 | 13:57:58.574 |  | ←RRC BCCH SIB |  |  |
18 | 13:59:21.463 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 13:59:21.463 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 13:59:21.463 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 13:59:21.463 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 13:59:21.514 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 13:59:21.514 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 13:59:21.514 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 13:59:21.514 |  |  |  | →NAS EMM Attach request |  |
26 | 13:59:21.514 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 13:59:21.514 |  |  |  | NAS K-asme 6cb7ced3dd92cb664bb104da1b778720... |  |
28 | 13:59:21.514 |  |  |  | NAS ← EMM Authentication request |  |
29 | 13:59:21.515 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 13:59:21.515 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 13:59:21.516 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 13:59:21.586 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 13:59:21.586 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 13:59:21.586 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 13:59:21.586 |  |  |  | →NAS EMM Authentication response |  |
36 | 13:59:21.586 |  |  |  | NAS UE auth OK |  |
37 | 13:59:21.586 |  |  |  | NAS K-nas-cip ec04245977ef0ee82f224ee4c9d51... |  |
38 | 13:59:21.586 |  |  |  | NAS K-nas-int f4eb6dee9311760a11754a97555fa... |  |
39 | 13:59:21.586 |  |  |  | NAS ← EMM Security mode command |  |
40 | 13:59:21.587 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 13:59:21.587 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 13:59:21.588 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 13:59:21.626 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
44 | 13:59:21.626 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 13:59:21.626 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xa) |  |  |
46 | 13:59:21.626 |  |  |  | →NAS EMM Security mode complete |  |
47 | 13:59:21.626 |  |  |  | NAS ← ESM ESM information request |  |
48 | 13:59:21.626 |  | [EMBEDDED NAS IN NEXT RRC] ESM Unknown message (type=0xec) |  |  |
49 | 13:59:21.626 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 13:59:21.628 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer |  |  |
51 | 13:59:21.674 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
52 | 13:59:21.674 |  | →RRC DCCH UL Information Transfer |  |  |
53 | 13:59:21.674 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x1) |  |  |
54 | 13:59:21.674 |  |  |  | →NAS ESM ESM information response |  |
55 | 13:59:21.674 |  |  |  | NAS ← EMM Attach accept |  |
56 | 13:59:21.674 |  |  |  | NAS K-enb c95b714f14da1fdab8318deea944db9a6... |  |
57 | 13:59:21.675 |  |  | RRC K-enb c95b714f14da1fdab8318deea944db9a6... |  |  |
58 | 13:59:21.675 |  |  | RRC rrc-cip d89dbc065c8013d5adf11e12f316a19... |  |  |
59 | 13:59:21.675 |  |  | RRC rrc-int 5482bb7c0f748b147b140b12c9d740c... |  |  |
60 | 13:59:21.675 |  |  | RRC up-cip 1fc6bdbe5ce0c3d8e89a222b3ed37f49... |  |  |
61 | 13:59:21.675 |  |  | RRC up-int 5cfe376454996988181eed91f8ceeebe... |  |  |
62 | 13:59:21.675 |  | ←RRC DCCH Security Mode Command |  |  |
63 | 13:59:21.675 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
64 | 13:59:21.706 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
65 | 13:59:21.706 |  | →RRC DCCH Security Mode Complete |  |  |
66 | 13:59:21.706 |  | ←RRC DCCH UE Capability Enquiry |  |  |
67 | 13:59:21.706 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
68 | 13:59:21.756 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
69 | 13:59:21.756 |  | →RRC DCCH UE Capability Information |  |  |
70 | 13:59:21.756 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xd) |  |  |
71 | 13:59:21.756 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
72 | 13:59:21.756 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
73 | 13:59:21.786 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
74 | 13:59:21.786 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
75 | 13:59:21.826 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer |  |  |  |
76 | 13:59:21.826 |  | →RRC DCCH UL Information Transfer |  |  |
77 | 13:59:21.826 |  | [EMBEDDED NAS IN PREV RRC] ESM Unknown message (type=0xbc) |  |  |
78 | 13:59:21.826 |  |  |  | →NAS EMM Attach complete |  |
79 | 13:59:21.826 |  |  |  | NAS ← EMM EMM information |  |
80 | 13:59:21.827 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x6e) |  |  |
81 | 13:59:21.827 |  | ←RRC DCCH DL Information Transfer |  |  |
82 | 13:59:21.828 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
83 | 13:59:29.115 |  | ←RRC DCCH RRC Connection Release |  |  |
84 | 13:59:29.115 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
85 | 13:59:30.763 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
86 | 13:59:30.763 |  | →RRC CCCH RRC Connection Request |  |  |
87 | 13:59:30.763 |  | ←RRC CCCH RRC Connection Setup |  |  |
88 | 13:59:30.763 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
89 | 13:59:30.826 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
90 | 13:59:30.826 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
91 | 13:59:30.826 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
92 | 13:59:30.826 |  |  |  | →NAS EMM Service request |  |
93 | 13:59:30.826 |  |  |  | NAS K-enb e874cc17cd970e2bf15923132fa561e65... |  |
94 | 13:59:30.827 |  |  | RRC K-enb e874cc17cd970e2bf15923132fa561e65... |  |  |
95 | 13:59:30.827 |  |  | RRC rrc-cip 52b6ba386b02b5f6902f4df601499f2... |  |  |
96 | 13:59:30.827 |  |  | RRC rrc-int 420bb7ce3bedb78ff30941292b4ff86... |  |  |
97 | 13:59:30.827 |  |  | RRC up-cip 3fb58b07e0f1eec7782e30ea32b28d30... |  |  |
98 | 13:59:30.827 |  |  | RRC up-int 99b522e2a8762b0b8b2d8a0afd622fd7... |  |  |
99 | 13:59:30.827 |  | ←RRC DCCH Security Mode Command |  |  |
100 | 13:59:30.827 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
101 | 13:59:30.866 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
102 | 13:59:30.866 |  | →RRC DCCH Security Mode Complete |  |  |
103 | 13:59:30.866 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
104 | 13:59:30.866 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
105 | 13:59:30.906 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
106 | 13:59:30.906 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
107 | 13:59:43.074 | →enobeB PCAP frame→ DNS |  |  |  |
108 | 13:59:43.077 |  | ←enobeB PCAP frame← TCP |  |  |
109 | 13:59:43.106 | →enobeB PCAP frame→ TCP |  |  |  |
110 | 13:59:43.193 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
111 | 13:59:43.197 |  | ←enobeB PCAP frame← TCP |  |  |
112 | 13:59:43.202 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
113 | 13:59:43.226 | →enobeB PCAP frame→ TCP |  |  |  |
114 | 13:59:43.392 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 16)
115 | 13:59:43.393 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
116 | 13:59:43.397 |  | ←enobeB PCAP frame← TCP |  |  |
117 | 13:59:43.398 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
118 | 13:59:43.425 | →enobeB PCAP frame→ TCP |  |  |  |
119 | 13:59:43.432 |  |  |  |  | →HTTP GET | HTTP-Proxy
120 | 13:59:43.434 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
121 | 13:59:43.437 |  | ←enobeB PCAP frame← TCP |  |  |
122 | 13:59:43.439 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:301: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
123 | 13:59:43.457 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
124 | 13:59:43.465 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
125 | 13:59:43.506 | →enobeB PCAP frame→ TCP |  |  |  |
126 | 13:59:45.386 | →enobeB PCAP frame→ TCP |  |  |  |
127 | 13:59:45.389 |  | ←enobeB PCAP frame← TCP |  |  |
128 | 13:59:45.426 | →enobeB PCAP frame→ TCP |  |  |  |
129 | 13:59:45.434 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
130 | 13:59:45.437 |  | ←enobeB PCAP frame← TCP |  |  |
131 | 13:59:45.440 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
132 | 13:59:45.466 | →enobeB PCAP frame→ TCP |  |  |  |
133 | 13:59:45.752 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
134 | 13:59:45.754 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
135 | 13:59:45.757 |  | ←enobeB PCAP frame← TCP |  |  |
136 | 13:59:45.758 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
137 | 13:59:45.786 | →enobeB PCAP frame→ TCP |  |  |  |
138 | 13:59:45.792 |  |  |  |  | →HTTP GET | IDMS-Endpoint
139 | 13:59:45.794 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
140 | 13:59:45.798 |  | ←enobeB PCAP frame← TCP |  |  |
141 | 13:59:45.802 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
142 | 13:59:45.806 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:524: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
143 | 13:59:45.807 |  |  |  |  | MMICmd: Please provide user credentials: username and password
144 | 13:59:45.809 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
145 | 13:59:45.866 | →enobeB PCAP frame→ TCP |  |  |  |
146 | 13:59:50.443 |  |  |  |  | →HTTP POST | IDMS-Endpoint
147 | 13:59:50.446 |  | ←enobeB PCAP frame← TCP |  |  |
148 | 13:59:50.459 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
149 | 13:59:50.461 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:529: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
150 | 13:59:50.465 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
151 | 13:59:50.503 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:693: IdM port - Client closed the connection (id 18)
152 | 13:59:50.508 |  | ←enobeB PCAP frame← TCP |  |  |
153 | 13:59:51.266 | →enobeB PCAP frame→ TCP |  |  |  |
154 | 13:59:51.269 |  | ←enobeB PCAP frame← TCP |  |  |
155 | 13:59:51.306 | →enobeB PCAP frame→ TCP |  |  |  |
156 | 13:59:51.434 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
157 | 13:59:51.437 |  | ←enobeB PCAP frame← TCP |  |  |
158 | 13:59:51.440 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
159 | 13:59:51.466 | →enobeB PCAP frame→ TCP |  |  |  |
160 | 13:59:51.592 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
161 | 13:59:51.594 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
162 | 13:59:51.596 |  | ←enobeB PCAP frame← TCP |  |  |
163 | 13:59:51.598 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
164 | 13:59:51.626 | →enobeB PCAP frame→ TCP |  |  |  |
165 | 13:59:51.632 |  |  |  |  | →HTTP POST | IDMS-Endpoint
166 | 13:59:51.634 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
167 | 13:59:51.637 |  | ←enobeB PCAP frame← TCP |  |  |
168 | 13:59:51.670 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
169 | 13:59:51.672 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:534: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
170 | 13:59:51.676 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
171 | 13:59:51.746 | →enobeB PCAP frame→ TCP |  |  |  |
172 | 13:59:51.986 | →enobeB PCAP frame→ TCP |  |  |  |
173 | 13:59:51.989 |  | ←enobeB PCAP frame← TCP |  |  |
174 | 13:59:52.025 | →enobeB PCAP frame→ TCP |  |  |  |
175 | 13:59:52.034 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
176 | 13:59:52.037 |  | ←enobeB PCAP frame← TCP |  |  |
177 | 13:59:52.041 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
178 | 13:59:52.066 | →enobeB PCAP frame→ TCP |  |  |  |
179 | 13:59:52.072 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 19)
180 | 13:59:52.073 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
181 | 13:59:52.076 |  | ←enobeB PCAP frame← TCP |  |  |
182 | 13:59:52.078 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
183 | 13:59:52.113 |  |  |  |  | →HTTP POST | HTTP-Proxy
184 | 13:59:52.114 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
185 | 13:59:52.116 |  | ←enobeB PCAP frame← TCP |  |  |
186 | 13:59:52.137 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:554: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
187 | 13:59:52.144 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
188 | 13:59:52.152 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
189 | 13:59:52.186 | →enobeB PCAP frame→ TCP |  |  |  |
190 | 13:59:52.226 | →enobeB PCAP frame→ TCP |  |  |  |
191 | 13:59:52.229 |  | ←enobeB PCAP frame← TCP |  |  |
192 | 13:59:52.266 | →enobeB PCAP frame→ TCP |  |  |  |
193 | 13:59:52.274 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
194 | 13:59:52.277 |  | ←enobeB PCAP frame← TCP |  |  |
195 | 13:59:52.280 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
196 | 13:59:52.306 | →enobeB PCAP frame→ TCP |  |  |  |
197 | 13:59:52.312 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 20)
198 | 13:59:52.314 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
199 | 13:59:52.316 |  | ←enobeB PCAP frame← TCP |  |  |
200 | 13:59:52.318 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
201 | 13:59:52.361 |  |  |  |  | →HTTP POST | HTTP-Proxy
202 | 13:59:52.365 |  | ←enobeB PCAP frame← TCP |  |  |
203 | 13:59:52.417 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
204 | 13:59:52.417 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:558: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
205 | 13:59:52.422 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
206 | 13:59:52.515 |  |  |  |  | →SIP REGISTER | P-CSCF
207 | 13:59:52.538 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:833: IMS UDP_s port 192.168.2.3:5062 configured
208 | 13:59:52.543 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:784: IMS TCP_s port 192.168.2.3:5062 configured!
209 | 13:59:52.546 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:842: IMS UDP_c port 192.168.2.3:5061 configured
210 | 13:59:52.557 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
211 | 13:59:53.314 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
212 | 13:59:53.346 |  |  |  |  | →SIP REGISTER | P-CSCF
213 | 13:59:53.358 |  |  |  |  | ←SIP 200 OK | P-CSCF
214 | 13:59:53.364 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
215 | 13:59:53.714 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
216 | 13:59:53.733 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
217 | 13:59:53.750 |  |  |  |  | ←SIP 200 OK | P-CSCF
218 | 13:59:53.750 |  |  |  |  | MIKEY | Media-Server
219 | 13:59:53.757 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
220 | 13:59:53.947 |  |  |  |  | XML→ | Media-Server
221 | 13:59:53.949 |  |  |  |  | XML→ | Media-Server
222 | 13:59:53.952 |  |  |  |  | ←XML | Media-Server
223 | 13:59:53.956 |  |  |  |  | ←SIP NOTIFY | P-CSCF
224 | 13:59:53.962 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:48431;transp... |  |  |
225 | 13:59:53.991 |  |  |  |  | →SIP 200 OK | P-CSCF
226 | 13:59:54.269 |  | ←enobeB PCAP frame← TCP |  |  |
227 | 13:59:54.306 | →enobeB PCAP frame→ TCP |  |  |  |
228 | 13:59:54.314 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
229 | 13:59:54.317 |  | ←enobeB PCAP frame← TCP |  |  |
230 | 13:59:54.320 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
231 | 13:59:54.346 | →enobeB PCAP frame→ TCP |  |  |  |
232 | 13:59:54.431 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
233 | 13:59:54.434 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
234 | 13:59:54.437 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
235 | 13:59:54.465 | →enobeB PCAP frame→ TCP |  |  |  |
236 | 13:59:54.473 |  |  |  |  | →HTTP GET | HTTP-Proxy
237 | 13:59:54.474 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
238 | 13:59:54.477 |  | ←enobeB PCAP frame← TCP |  |  |
239 | 13:59:54.481 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:655: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcptt-ue-configuration.xml
240 | 13:59:54.488 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
241 | 13:59:54.496 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
242 | 13:59:54.543 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
243 | 13:59:54.545 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
244 | 13:59:54.549 |  | ←enobeB PCAP frame← TCP |  |  |
245 | 13:59:54.554 | →enobeB PCAP frame→ TCP |  |  |  |
246 | 13:59:54.557 |  | ←enobeB PCAP frame← TCP |  |  |
247 | 13:59:54.586 | →enobeB PCAP frame→ TCP |  |  |  |
248 | 13:59:54.745 | →enobeB PCAP frame→ TCP |  |  |  |
249 | 13:59:54.748 |  | ←enobeB PCAP frame← TCP |  |  |
250 | 13:59:54.786 | →enobeB PCAP frame→ TCP |  |  |  |
251 | 13:59:54.794 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
252 | 13:59:54.798 |  | ←enobeB PCAP frame← TCP |  |  |
253 | 13:59:54.801 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
254 | 13:59:54.826 | →enobeB PCAP frame→ TCP |  |  |  |
255 | 13:59:54.872 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
256 | 13:59:54.874 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
257 | 13:59:54.877 |  | ←enobeB PCAP frame← TCP |  |  |
258 | 13:59:54.878 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
259 | 13:59:54.906 | →enobeB PCAP frame→ TCP |  |  |  |
260 | 13:59:54.912 |  |  |  |  | →HTTP GET | HTTP-Proxy
261 | 13:59:54.914 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
262 | 13:59:54.916 |  | ←enobeB PCAP frame← TCP |  |  |
263 | 13:59:54.924 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:660: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcptt-user-profile-49.xml
264 | 13:59:54.968 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
265 | 13:59:54.981 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
266 | 13:59:54.981 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
267 | 13:59:55.026 | →enobeB PCAP frame→ TCP |  |  |  |
268 | 13:59:55.032 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
269 | 13:59:55.034 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
270 | 13:59:55.037 |  | ←enobeB PCAP frame← TCP |  |  |
271 | 13:59:55.066 | →enobeB PCAP frame→ TCP |  |  |  |
272 | 13:59:55.634 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
273 | 13:59:55.635 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
274 | 13:59:55.646 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
275 | 13:59:55.663 |  |  |  |  | ←SIP 200 OK | P-CSCF
276 | 13:59:55.663 |  |  |  |  | MIKEY | Media-Server
277 | 13:59:55.670 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
278 | 13:59:55.706 | →enobeB PCAP frame→ TCP |  |  |  |
279 | 13:59:55.709 |  | ←enobeB PCAP frame← TCP |  |  |
280 | 13:59:55.746 | →enobeB PCAP frame→ TCP |  |  |  |
281 | 13:59:55.754 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
282 | 13:59:55.757 |  | ←enobeB PCAP frame← TCP |  |  |
283 | 13:59:55.758 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
284 | 13:59:55.786 | →enobeB PCAP frame→ TCP |  |  |  |
285 | 13:59:55.864 |  |  |  |  | XML→ | Media-Server
286 | 13:59:55.866 |  |  |  |  | XML→ | Media-Server
287 | 13:59:55.869 |  |  |  |  | ←XML | Media-Server
288 | 13:59:55.871 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
289 | 13:59:55.872 |  |  |  |  | ←SIP NOTIFY | P-CSCF
290 | 13:59:55.873 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
291 | 13:59:55.877 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
292 | 13:59:55.878 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:48431;transp... |  |  |
293 | 13:59:55.906 | →enobeB PCAP frame→ TCP |  |  |  |
294 | 13:59:55.912 |  |  |  |  | →SIP 200 OK | P-CSCF
295 | 13:59:55.912 |  |  |  |  | →HTTP GET | HTTP-Proxy
296 | 13:59:55.914 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
297 | 13:59:55.915 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:665: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
298 | 13:59:55.917 |  | ←enobeB PCAP frame← TCP |  |  |
299 | 13:59:55.921 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
300 | 13:59:55.928 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
301 | 13:59:55.928 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
302 | 13:59:55.986 | →enobeB PCAP frame→ TCP |  |  |  |
303 | 13:59:55.991 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
304 | 13:59:55.994 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
305 | 13:59:55.997 |  | ←enobeB PCAP frame← TCP |  |  |
306 | 13:59:56.025 | →enobeB PCAP frame→ TCP |  |  |  |
307 | 13:59:56.066 | →enobeB PCAP frame→ TCP |  |  |  |
308 | 13:59:56.070 |  | ←enobeB PCAP frame← TCP |  |  |
309 | 13:59:56.106 | →enobeB PCAP frame→ TCP |  |  |  |
310 | 13:59:56.113 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
311 | 13:59:56.117 |  | ←enobeB PCAP frame← TCP |  |  |
312 | 13:59:56.119 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
313 | 13:59:56.146 | →enobeB PCAP frame→ TCP |  |  |  |
314 | 13:59:56.192 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
315 | 13:59:56.194 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
316 | 13:59:56.197 |  | ←enobeB PCAP frame← TCP |  |  |
317 | 13:59:56.198 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
318 | 13:59:56.226 | →enobeB PCAP frame→ TCP |  |  |  |
319 | 13:59:56.240 |  |  |  |  | →HTTP GET | HTTP-Proxy
320 | 13:59:56.245 |  | ←enobeB PCAP frame← TCP |  |  |
321 | 13:59:56.251 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:670: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at http://xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
322 | 13:59:56.277 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
323 | 13:59:56.287 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
324 | 13:59:56.288 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
325 | 13:59:56.346 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
326 | 13:59:56.350 |  | ←enobeB PCAP frame← TCP |  |  |
327 | 13:59:56.352 |  | ←enobeB PCAP frame← TCP |  |  |
328 | 13:59:56.354 | →enobeB PCAP frame→ TCP |  |  |  |
329 | 13:59:56.357 |  | ←enobeB PCAP frame← TCP |  |  |
330 | 13:59:56.386 | →enobeB PCAP frame→ TCP |  |  |  |
331 | 13:59:56.514 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
332 | 13:59:56.515 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
333 | 13:59:56.524 |  |  |  |  | →SIP PUBLISH | P-CSCF
334 | 13:59:56.571 |  |  |  |  | MIKEY | Media-Server
335 | 13:59:56.634 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
336 | 13:59:56.635 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
337 | 13:59:56.635 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
338 | 13:59:56.793 |  |  |  |  | XML→ | Media-Server
339 | 13:59:56.796 |  |  |  |  | ←SIP 200 OK | P-CSCF
340 | 13:59:56.799 |  |  |  |  | ←SIP 200 OK | P-CSCF
341 | 13:59:56.799 |  |  |  |  | MIKEY | Media-Server
342 | 13:59:56.801 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
343 | 13:59:56.805 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
344 | 13:59:57.000 |  |  |  |  | XML→ | Media-Server
345 | 13:59:57.002 |  |  |  |  | XML→ | Media-Server
346 | 13:59:57.037 |  |  |  |  | MIKEY | Media-Server
347 | 13:59:57.037 |  |  |  |  | ←XML | Media-Server
348 | 13:59:57.042 |  |  |  |  | ←SIP NOTIFY | P-CSCF
349 | 13:59:57.048 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:48431;transp... |  |  |
350 | 13:59:57.111 |  |  |  |  | →SIP 200 OK | P-CSCF
351 | 13:59:57.114 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
352 | 13:59:57.116 |  |  |  |  | ←XML | Media-Server
353 | 13:59:57.133 |  |  |  |  | ←SIP MESSAGE | P-CSCF
354 | 13:59:57.141 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
355 | 13:59:57.952 |  |  |  |  | →SIP 200 OK | P-CSCF
356 | 13:59:57.954 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
357 | 13:59:57.960 |  |  |  |  | Info: MCX_IMS_CommonProcedures.ttcn:228: MESSAGE/200OK Table 5.3.2.3-2 Steps 7-8 Done
358 | 13:59:59.963 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
359 | 13:59:59.992 |  | ←RRC DCCH RRC Connection Release |  |  |
360 | 13:59:59.992 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
361 | 14:00:00.007 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
362 | 14:00:00.083 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:754: SRTP config: Master Key: 613ECE54392AABD843AF711A30B4CD9F, Master Salt: 8066C8B459A404FB06FADF10, MKI: 28F3EB6E
363 | 14:00:00.083 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
364 | 14:00:00.084 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
365 | 14:00:00.086 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
366 | 14:00:00.089 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
367 | 14:00:00.089 |  |  |  |  | ←XML | Media-Server
368 | 14:00:00.100 |  |  |  |  | ←SIP INVITE | P-CSCF
369 | 14:00:00.673 |  | ←enobeB PCAP frame← LTE RRC PCCH Paging (1 PagingRecord) |  |  |
370 | 14:00:00.673 |  | ←RRC PCCH Paging |  |  |
371 | 14:00:00.713 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
372 | 14:00:00.713 |  | →RRC CCCH RRC Connection Request |  |  |
373 | 14:00:00.713 |  | ←RRC CCCH RRC Connection Setup |  |  |
374 | 14:00:00.713 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
375 | 14:00:00.746 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
376 | 14:00:00.746 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
377 | 14:00:00.746 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
378 | 14:00:00.746 |  |  |  | →NAS EMM Service request |  |
379 | 14:00:00.746 |  |  |  | NAS K-enb 75510fba290f4bcf222b68a296837c366... |  |
380 | 14:00:00.747 |  | ←RRC DCCH Security Mode Command |  |  |
381 | 14:00:00.747 |  |  | RRC K-enb 75510fba290f4bcf222b68a296837c366... |  |  |
382 | 14:00:00.747 |  |  | RRC rrc-cip a2096a3ad24d3a512bdb5a9a30162c5... |  |  |
383 | 14:00:00.747 |  |  | RRC rrc-int 3accb17a110150a7b7e44b5a8432638... |  |  |
384 | 14:00:00.747 |  |  | RRC up-cip 2dfca8f543781a09ae5cbddab17f30ac... |  |  |
385 | 14:00:00.747 |  |  | RRC up-int 69354e89fa0646f790a2ce2d426ce2ea... |  |  |
386 | 14:00:00.748 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
387 | 14:00:00.786 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
388 | 14:00:00.786 |  | →RRC DCCH Security Mode Complete |  |  |
389 | 14:00:00.786 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
390 | 14:00:00.786 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
391 | 14:00:00.826 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
392 | 14:00:00.826 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
393 | 14:00:00.828 |  | ←enobeB PCAP frame← SIP over IPSEC: INVITE sip:PublicUserId-A@192.168.3.2:48431;transp... |  |  |
394 | 14:00:00.872 |  |  |  |  | →SIP 100 Trying | P-CSCF
395 | 14:00:00.874 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 100 Trying |  |  |  |
396 | 14:00:01.114 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
397 | 14:00:01.119 |  |  |  |  | →SIP 200 OK | P-CSCF
398 | 14:00:01.157 |  |  |  |  | XML→ | Media-Server
399 | 14:00:01.165 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:591: 200 OK Verdict: Pass
400 | 14:00:01.165 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:439: Step 1 Verdict: Pass
401 | 14:00:01.169 |  |  |  |  | ←SIP ACK | P-CSCF
402 | 14:00:01.171 |  |  |  |  | ←SIP BYE | P-CSCF
403 | 14:00:01.174 |  | ←enobeB PCAP frame← SIP over IPSEC: ACK sip:PublicUserId-A@192.168.3.2:48431;transport... |  |  |
404 | 14:00:01.178 |  | ←enobeB PCAP frame← SIP over IPSEC: BYE sip:PublicUserId-A@192.168.3.2:48431;transport... |  |  |
405 | 14:00:01.256 |  | [EMBEDDED NAS IN NEXT RRC] TP Unknown message (type=0x27) |  |  |
406 | 14:00:01.256 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
407 | 14:00:01.257 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
408 | 14:00:01.258 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
409 | 14:00:01.306 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
410 | 14:00:01.306 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
411 | 14:00:01.306 |  | →RRC DCCH UL Information Transfer |  |  |
412 | 14:00:01.306 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x6e) |  |  |
413 | 14:00:01.306 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
414 | 14:00:01.376 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
415 | 14:00:01.631 |  |  |  |  | →SIP 200 OK | P-CSCF
416 | 14:00:01.634 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
417 | 14:00:02.505 | →enobeB PCAP frame→ |  |  |  |
418 | 14:00:03.636 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
419 | 14:00:03.650 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
420 | 14:00:03.650 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x3) |  |  |
421 | 14:00:03.650 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
422 | 14:00:03.651 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
423 | 14:00:03.706 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
424 | 14:00:03.706 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
425 | 14:00:03.706 |  | →RRC DCCH UL Information Transfer |  |  |
426 | 14:00:03.706 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x8) |  |  |
427 | 14:00:03.706 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
428 | 14:00:03.762 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
429 | 14:00:03.763 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
430 | 14:00:03.811 |  | ←RRC DCCH RRC Connection Release |  |  |
431 | 14:00:03.813 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
432 | 14:00:03.828 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
433 | 14:00:03.829 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:452: Step 6 Verdict: Pass
434 | 14:00:03.831 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
435 | 14:00:03.833 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
436 | 14:00:04.580 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.