MSG #407 2021-09-28 14:00:01.257
RRC

     DCCH: RRC Connection Reconfiguration
    {
      message c1: rrcConnectionReconfiguration: {
        rrc-TransactionIdentifier 0,
        criticalExtensions c1: rrcConnectionReconfiguration-r8: {
          dedicatedInfoNASList {
            '27C8F8339F044F2713D6249421E3876DB768C036F63B99BC4DB6CD0CFC43D5A98022E70A44932291CE4D4C281FB30E881078663F8FBA'H
          },
          radioResourceConfigDedicated {
            drb-ToAddModList {
              {
                eps-BearerIdentity 6,
                drb-Identity 2,
                pdcp-Config {
                  discardTimer ms100,
                  rlc-UM {
                    pdcp-SN-Size len12bits
                  },
                  headerCompression notUsed: NULL
                },
                rlc-Config um-Bi-Directional: {
                  ul-UM-RLC {
                    sn-FieldLength size10
                  },
                  dl-UM-RLC {
                    sn-FieldLength size10,
                    t-Reordering ms50
                  }
                },
                logicalChannelIdentity 4,
                logicalChannelConfig {
                  ul-SpecificParameters {
                    priority 5,
                    prioritisedBitRate kBps0,
                    bucketSizeDuration ms100,
                    logicalChannelGroup 1
                  }
                }
              }
            }
          }
        }
      }
    }