ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 14:01:36.144 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 14:01:36.147 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 14:01:36.148 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 14:01:36.149 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 14:01:36.150 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 14:01:36.150 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:824: IMS UDP port 192.168.2.3:5060 configured
7 | 14:01:36.152 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:774: IMS TCP port 192.168.2.3:5060 configured!
8 | 14:01:36.154 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:795: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 14:01:36.154 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:806: IdM port 192.168.2.3:8080 configured!
10 | 14:01:36.155 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 14:01:37.358 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 14:01:37.360 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 14:01:40.453 |  | ←RRC BCCH SIB |  |  |
14 | 14:01:40.459 |  | ←RRC BCCH SIB1 |  |  |
15 | 14:01:40.539 |  | ←RRC BCCH SIB1 |  |  |
16 | 14:01:40.614 |  | ←RRC BCCH SIB |  |  |
17 | 14:01:40.619 |  | ←RRC BCCH SIB1 |  |  |
18 | 14:02:58.743 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 14:02:58.743 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 14:02:58.743 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 14:02:58.743 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 14:02:58.794 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 14:02:58.794 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 14:02:58.794 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 14:02:58.794 |  |  |  | →NAS EMM Attach request |  |
26 | 14:02:58.794 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 14:02:58.796 |  |  |  | NAS K-asme 767ba9fd6e5490ac2cdcd5fd28fa17c0... |  |
28 | 14:02:58.796 |  |  |  | NAS ← EMM Authentication request |  |
29 | 14:02:58.797 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 14:02:58.797 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 14:02:58.798 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 14:02:58.866 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 14:02:58.866 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 14:02:58.866 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 14:02:58.866 |  |  |  | →NAS EMM Authentication response |  |
36 | 14:02:58.866 |  |  |  | NAS UE auth OK |  |
37 | 14:02:58.866 |  |  |  | NAS K-nas-cip e0f6d74972e0987bad3ec90e13439... |  |
38 | 14:02:58.866 |  |  |  | NAS K-nas-int 009ab3ebf7fa1b8d27b19b2a1c315... |  |
39 | 14:02:58.866 |  |  |  | NAS ← EMM Security mode command |  |
40 | 14:02:58.867 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 14:02:58.867 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 14:02:58.868 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 14:02:58.906 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
44 | 14:02:58.906 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 14:02:58.906 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x1) |  |  |
46 | 14:02:58.906 |  |  |  | →NAS EMM Security mode complete |  |
47 | 14:02:58.906 |  |  |  | NAS ← ESM ESM information request |  |
48 | 14:02:58.907 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xd) |  |  |
49 | 14:02:58.907 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 14:02:58.908 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
51 | 14:02:58.954 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
52 | 14:02:58.954 |  | →RRC DCCH UL Information Transfer |  |  |
53 | 14:02:58.954 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x5) |  |  |
54 | 14:02:58.954 |  |  |  | →NAS ESM ESM information response |  |
55 | 14:02:58.954 |  |  |  | NAS ← EMM Attach accept |  |
56 | 14:02:58.954 |  |  |  | NAS K-enb 14fa5a65edd257cb4b8c5c0478d571740... |  |
57 | 14:02:58.955 |  | ←RRC DCCH Security Mode Command |  |  |
58 | 14:02:58.955 |  |  | RRC K-enb 14fa5a65edd257cb4b8c5c0478d571740... |  |  |
59 | 14:02:58.955 |  |  | RRC rrc-cip 22c06b62552ff53dd36df10e1bf00f1... |  |  |
60 | 14:02:58.955 |  |  | RRC rrc-int c639c35f3d3da066462207e5eb24d43... |  |  |
61 | 14:02:58.955 |  |  | RRC up-cip e18212fa9e8ff8c1bb213ae7f91b8ba8... |  |  |
62 | 14:02:58.955 |  |  | RRC up-int e19433f01d461b671444d1783211d086... |  |  |
63 | 14:02:58.956 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
64 | 14:02:58.986 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
65 | 14:02:58.986 |  | →RRC DCCH Security Mode Complete |  |  |
66 | 14:02:58.986 |  | ←RRC DCCH UE Capability Enquiry |  |  |
67 | 14:02:58.986 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
68 | 14:02:59.036 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
69 | 14:02:59.036 |  | →RRC DCCH UE Capability Information |  |  |
70 | 14:02:59.036 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xb) |  |  |
71 | 14:02:59.036 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
72 | 14:02:59.036 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
73 | 14:02:59.066 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
74 | 14:02:59.066 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
75 | 14:02:59.106 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
76 | 14:02:59.106 |  | →RRC DCCH UL Information Transfer |  |  |
77 | 14:02:59.106 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xb) |  |  |
78 | 14:02:59.106 |  |  |  | →NAS EMM Attach complete |  |
79 | 14:02:59.106 |  |  |  | NAS ← EMM EMM information |  |
80 | 14:02:59.107 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x9) |  |  |
81 | 14:02:59.107 |  | ←RRC DCCH DL Information Transfer |  |  |
82 | 14:02:59.108 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
83 | 14:03:04.581 |  | ←RRC DCCH RRC Connection Release |  |  |
84 | 14:03:04.582 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
85 | 14:03:04.923 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
86 | 14:03:04.923 |  | →RRC CCCH RRC Connection Request |  |  |
87 | 14:03:04.923 |  | ←RRC CCCH RRC Connection Setup |  |  |
88 | 14:03:04.923 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
89 | 14:03:04.946 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
90 | 14:03:04.946 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
91 | 14:03:04.946 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
92 | 14:03:04.946 |  |  |  | →NAS EMM Service request |  |
93 | 14:03:04.946 |  |  |  | NAS K-enb b94da01d2d3663bfb086cff53d349f66d... |  |
94 | 14:03:04.947 |  | ←RRC DCCH Security Mode Command |  |  |
95 | 14:03:04.947 |  |  | RRC K-enb b94da01d2d3663bfb086cff53d349f66d... |  |  |
96 | 14:03:04.947 |  |  | RRC rrc-cip 6eea2b25fe586bb848819faeeceb6c1... |  |  |
97 | 14:03:04.947 |  |  | RRC rrc-int 88df5f598c7fde18a5ae255b6224344... |  |  |
98 | 14:03:04.947 |  |  | RRC up-cip f6367c64f60388ee458dc89e004cf37a... |  |  |
99 | 14:03:04.947 |  |  | RRC up-int c77ad246a1ff621d3f4ab010f71ae5a8... |  |  |
100 | 14:03:04.948 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
101 | 14:03:04.986 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
102 | 14:03:04.986 |  | →RRC DCCH Security Mode Complete |  |  |
103 | 14:03:04.986 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
104 | 14:03:04.986 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
105 | 14:03:05.026 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
106 | 14:03:05.026 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
107 | 14:03:45.106 | →enobeB PCAP frame→ TCP |  |  |  |
108 | 14:03:45.109 |  | ←enobeB PCAP frame← TCP |  |  |
109 | 14:03:45.146 | →enobeB PCAP frame→ TCP |  |  |  |
110 | 14:03:45.194 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
111 | 14:03:45.197 |  | ←enobeB PCAP frame← TCP |  |  |
112 | 14:03:45.203 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
113 | 14:03:45.226 | →enobeB PCAP frame→ TCP |  |  |  |
114 | 14:03:45.352 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 16)
115 | 14:03:45.354 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
116 | 14:03:45.357 |  | ←enobeB PCAP frame← TCP |  |  |
117 | 14:03:45.358 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
118 | 14:03:45.386 | →enobeB PCAP frame→ TCP |  |  |  |
119 | 14:03:45.392 |  |  |  |  | →HTTP GET | HTTP-Proxy
120 | 14:03:45.394 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
121 | 14:03:45.397 |  | ←enobeB PCAP frame← TCP |  |  |
122 | 14:03:45.398 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:301: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
123 | 14:03:45.417 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
124 | 14:03:45.425 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
125 | 14:03:45.426 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
126 | 14:03:45.466 | →enobeB PCAP frame→ TCP |  |  |  |
127 | 14:03:45.506 | →enobeB PCAP frame→ TCP |  |  |  |
128 | 14:03:47.346 | →enobeB PCAP frame→ TCP |  |  |  |
129 | 14:03:47.349 |  | ←enobeB PCAP frame← TCP |  |  |
130 | 14:03:47.386 | →enobeB PCAP frame→ TCP |  |  |  |
131 | 14:03:47.405 |  | ←enobeB PCAP frame← TCP |  |  |
132 | 14:03:47.411 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
133 | 14:03:47.672 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
134 | 14:03:47.677 |  | ←enobeB PCAP frame← TCP |  |  |
135 | 14:03:47.678 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
136 | 14:03:47.706 | →enobeB PCAP frame→ TCP |  |  |  |
137 | 14:03:47.752 |  |  |  |  | →HTTP GET | IDMS-Endpoint
138 | 14:03:47.754 | →enobeB PCAP frame→ TCP |  |  |  |
139 | 14:03:47.757 |  | ←enobeB PCAP frame← TCP |  |  |
140 | 14:03:47.768 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
141 | 14:03:47.772 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:524: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
142 | 14:03:47.773 |  |  |  |  | MMICmd: Please provide user credentials: username and password
143 | 14:03:47.774 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
144 | 14:03:47.866 | →enobeB PCAP frame→ TCP |  |  |  |
145 | 14:03:52.314 | →enobeB PCAP frame→ TCP |  |  |  |
146 | 14:03:52.314 |  |  |  |  | →HTTP POST | IDMS-Endpoint
147 | 14:03:52.317 |  | ←enobeB PCAP frame← TCP |  |  |
148 | 14:03:52.329 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
149 | 14:03:52.331 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:529: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
150 | 14:03:52.335 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
151 | 14:03:52.346 | →enobeB PCAP frame→ TCP |  |  |  |
152 | 14:03:52.383 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:693: IdM port - Client closed the connection (id 18)
153 | 14:03:52.386 | →enobeB PCAP frame→ TCP |  |  |  |
154 | 14:03:52.389 |  | ←enobeB PCAP frame← TCP |  |  |
155 | 14:03:52.426 | →enobeB PCAP frame→ TCP |  |  |  |
156 | 14:03:52.906 | →enobeB PCAP frame→ TCP |  |  |  |
157 | 14:03:52.909 |  | ←enobeB PCAP frame← TCP |  |  |
158 | 14:03:52.946 | →enobeB PCAP frame→ TCP |  |  |  |
159 | 14:03:53.034 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
160 | 14:03:53.036 |  | ←enobeB PCAP frame← TCP |  |  |
161 | 14:03:53.038 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
162 | 14:03:53.066 | →enobeB PCAP frame→ TCP |  |  |  |
163 | 14:03:53.152 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
164 | 14:03:53.154 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
165 | 14:03:53.157 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
166 | 14:03:53.186 | →enobeB PCAP frame→ TCP |  |  |  |
167 | 14:03:53.232 |  |  |  |  | →HTTP POST | IDMS-Endpoint
168 | 14:03:53.234 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
169 | 14:03:53.238 |  | ←enobeB PCAP frame← TCP |  |  |
170 | 14:03:53.264 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:534: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
171 | 14:03:53.264 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
172 | 14:03:53.271 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
173 | 14:03:53.346 | →enobeB PCAP frame→ TCP |  |  |  |
174 | 14:03:53.626 | →enobeB PCAP frame→ TCP |  |  |  |
175 | 14:03:53.682 |  | ←enobeB PCAP frame← TCP |  |  |
176 | 14:03:53.706 | →enobeB PCAP frame→ TCP |  |  |  |
177 | 14:03:53.714 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
178 | 14:03:53.717 |  | ←enobeB PCAP frame← TCP |  |  |
179 | 14:03:53.720 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
180 | 14:03:53.746 | →enobeB PCAP frame→ TCP |  |  |  |
181 | 14:03:53.752 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 19)
182 | 14:03:53.754 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
183 | 14:03:53.757 |  | ←enobeB PCAP frame← TCP |  |  |
184 | 14:03:53.758 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
185 | 14:03:53.794 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
186 | 14:03:53.794 |  |  |  |  | →HTTP POST | HTTP-Proxy
187 | 14:03:53.797 |  | ←enobeB PCAP frame← TCP |  |  |
188 | 14:03:53.818 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:554: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
189 | 14:03:53.825 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
190 | 14:03:53.936 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
191 | 14:03:53.986 | →enobeB PCAP frame→ TCP |  |  |  |
192 | 14:03:54.002 | →enobeB PCAP frame→ TCP |  |  |  |
193 | 14:03:54.017 |  | ←enobeB PCAP frame← TCP |  |  |
194 | 14:03:54.066 | →enobeB PCAP frame→ TCP |  |  |  |
195 | 14:03:54.074 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
196 | 14:03:54.078 |  | ←enobeB PCAP frame← TCP |  |  |
197 | 14:03:54.083 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
198 | 14:03:54.106 | →enobeB PCAP frame→ TCP |  |  |  |
199 | 14:03:54.114 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
200 | 14:03:54.220 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 20)
201 | 14:03:54.225 |  | ←enobeB PCAP frame← TCP |  |  |
202 | 14:03:54.226 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
203 | 14:03:54.274 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
204 | 14:03:54.296 |  |  |  |  | →HTTP POST | HTTP-Proxy
205 | 14:03:54.300 |  | ←enobeB PCAP frame← TCP |  |  |
206 | 14:03:54.364 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
207 | 14:03:54.364 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:558: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
208 | 14:03:54.461 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
209 | 14:03:54.462 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
210 | 14:03:54.506 | →enobeB PCAP frame→ TCP |  |  |  |
211 | 14:03:54.546 | →enobeB PCAP frame→ TCP |  |  |  |
212 | 14:03:54.554 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
213 | 14:03:54.602 |  |  |  |  | →SIP REGISTER | P-CSCF
214 | 14:03:54.626 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:833: IMS UDP_s port 192.168.2.3:5062 configured
215 | 14:03:54.631 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:784: IMS TCP_s port 192.168.2.3:5062 configured!
216 | 14:03:54.633 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:842: IMS UDP_c port 192.168.2.3:5061 configured
217 | 14:03:54.644 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
218 | 14:03:55.474 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
219 | 14:03:55.525 |  |  |  |  | →SIP REGISTER | P-CSCF
220 | 14:03:55.549 |  |  |  |  | ←SIP 200 OK | P-CSCF
221 | 14:03:55.557 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
222 | 14:03:55.874 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
223 | 14:03:55.875 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 SIP over IPSEC: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 |  |  |  |
224 | 14:03:55.886 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
225 | 14:03:55.943 |  |  |  |  | ←SIP 200 OK | P-CSCF
226 | 14:03:55.943 |  |  |  |  | MIKEY | Media-Server
227 | 14:03:55.950 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
228 | 14:03:56.148 |  |  |  |  | XML→ | Media-Server
229 | 14:03:56.150 |  |  |  |  | XML→ | Media-Server
230 | 14:03:56.153 |  |  |  |  | ←XML | Media-Server
231 | 14:03:56.156 |  |  |  |  | ←SIP NOTIFY | P-CSCF
232 | 14:03:56.163 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:38214;transp... |  |  |
233 | 14:03:56.192 |  |  |  |  | →SIP 200 OK | P-CSCF
234 | 14:03:56.194 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
235 | 14:03:56.426 | →enobeB PCAP frame→ TCP |  |  |  |
236 | 14:03:56.429 |  | ←enobeB PCAP frame← TCP |  |  |
237 | 14:03:56.466 | →enobeB PCAP frame→ TCP |  |  |  |
238 | 14:03:56.474 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
239 | 14:03:56.477 |  | ←enobeB PCAP frame← TCP |  |  |
240 | 14:03:56.481 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
241 | 14:03:56.506 | →enobeB PCAP frame→ TCP |  |  |  |
242 | 14:03:56.553 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
243 | 14:03:56.554 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
244 | 14:03:56.557 |  | ←enobeB PCAP frame← TCP |  |  |
245 | 14:03:56.558 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
246 | 14:03:56.586 | →enobeB PCAP frame→ TCP |  |  |  |
247 | 14:03:56.593 |  |  |  |  | →HTTP GET | HTTP-Proxy
248 | 14:03:56.594 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
249 | 14:03:56.597 |  | ←enobeB PCAP frame← TCP |  |  |
250 | 14:03:56.602 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:655: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcptt-ue-configuration.xml
251 | 14:03:56.610 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
252 | 14:03:56.617 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
253 | 14:03:56.663 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
254 | 14:03:56.666 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
255 | 14:03:56.669 |  | ←enobeB PCAP frame← TCP |  |  |
256 | 14:03:56.674 | →enobeB PCAP frame→ TCP |  |  |  |
257 | 14:03:56.677 |  | ←enobeB PCAP frame← TCP |  |  |
258 | 14:03:56.706 | →enobeB PCAP frame→ TCP |  |  |  |
259 | 14:03:56.906 | →enobeB PCAP frame→ TCP |  |  |  |
260 | 14:03:56.909 |  | ←enobeB PCAP frame← TCP |  |  |
261 | 14:03:56.946 | →enobeB PCAP frame→ TCP |  |  |  |
262 | 14:03:56.954 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
263 | 14:03:56.957 |  | ←enobeB PCAP frame← TCP |  |  |
264 | 14:03:56.961 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
265 | 14:03:56.986 | →enobeB PCAP frame→ TCP |  |  |  |
266 | 14:03:57.072 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
267 | 14:03:57.074 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
268 | 14:03:57.078 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
269 | 14:03:57.106 | →enobeB PCAP frame→ TCP |  |  |  |
270 | 14:03:57.112 |  |  |  |  | →HTTP GET | HTTP-Proxy
271 | 14:03:57.114 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
272 | 14:03:57.117 |  | ←enobeB PCAP frame← TCP |  |  |
273 | 14:03:57.125 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:660: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcptt-user-profile-49.xml
274 | 14:03:57.166 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
275 | 14:03:57.178 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
276 | 14:03:57.179 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
277 | 14:03:57.226 | →enobeB PCAP frame→ TCP |  |  |  |
278 | 14:03:57.231 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
279 | 14:03:57.234 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
280 | 14:03:57.238 |  | ←enobeB PCAP frame← TCP |  |  |
281 | 14:03:57.266 | →enobeB PCAP frame→ TCP |  |  |  |
282 | 14:03:57.874 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
283 | 14:03:57.875 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
284 | 14:03:57.884 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
285 | 14:03:57.942 |  |  |  |  | MIKEY | Media-Server
286 | 14:03:57.942 |  |  |  |  | ←SIP 200 OK | P-CSCF
287 | 14:03:57.949 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
288 | 14:03:57.986 | →enobeB PCAP frame→ TCP |  |  |  |
289 | 14:03:57.989 |  | ←enobeB PCAP frame← TCP |  |  |
290 | 14:03:58.026 | →enobeB PCAP frame→ TCP |  |  |  |
291 | 14:03:58.034 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
292 | 14:03:58.037 |  | ←enobeB PCAP frame← TCP |  |  |
293 | 14:03:58.038 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
294 | 14:03:58.066 | →enobeB PCAP frame→ TCP |  |  |  |
295 | 14:03:58.147 |  |  |  |  | XML→ | Media-Server
296 | 14:03:58.148 |  |  |  |  | XML→ | Media-Server
297 | 14:03:58.151 |  |  |  |  | ←XML | Media-Server
298 | 14:03:58.151 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
299 | 14:03:58.154 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
300 | 14:03:58.154 |  |  |  |  | ←SIP NOTIFY | P-CSCF
301 | 14:03:58.157 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
302 | 14:03:58.161 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:38214;transp... |  |  |
303 | 14:03:58.186 | →enobeB PCAP frame→ TCP |  |  |  |
304 | 14:03:58.193 |  |  |  |  | →SIP 200 OK | P-CSCF
305 | 14:03:58.193 |  |  |  |  | →HTTP GET | HTTP-Proxy
306 | 14:03:58.194 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
307 | 14:03:58.197 |  | ←enobeB PCAP frame← TCP |  |  |
308 | 14:03:58.205 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:665: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
309 | 14:03:58.223 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
310 | 14:03:58.230 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
311 | 14:03:58.266 | →enobeB PCAP frame→ TCP |  |  |  |
312 | 14:03:58.271 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
313 | 14:03:58.274 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
314 | 14:03:58.277 |  | ←enobeB PCAP frame← TCP |  |  |
315 | 14:03:58.306 | →enobeB PCAP frame→ TCP |  |  |  |
316 | 14:03:58.386 | →enobeB PCAP frame→ TCP |  |  |  |
317 | 14:03:58.389 |  | ←enobeB PCAP frame← TCP |  |  |
318 | 14:03:58.426 | →enobeB PCAP frame→ TCP |  |  |  |
319 | 14:03:58.434 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
320 | 14:03:58.437 |  | ←enobeB PCAP frame← TCP |  |  |
321 | 14:03:58.440 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
322 | 14:03:58.466 | →enobeB PCAP frame→ TCP |  |  |  |
323 | 14:03:58.552 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
324 | 14:03:58.554 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
325 | 14:03:58.557 |  | ←enobeB PCAP frame← TCP |  |  |
326 | 14:03:58.558 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
327 | 14:03:58.586 | →enobeB PCAP frame→ TCP |  |  |  |
328 | 14:03:58.592 |  |  |  |  | →HTTP GET | HTTP-Proxy
329 | 14:03:58.594 | →enobeB PCAP frame→ HTTPS: GET http://xcap.gms.mcstaasting.com/org.openmobile... |  |  |  |
330 | 14:03:58.597 |  | ←enobeB PCAP frame← TCP |  |  |
331 | 14:03:58.604 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:670: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at http://xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
332 | 14:03:58.633 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
333 | 14:03:58.642 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
334 | 14:03:58.666 | →enobeB PCAP frame→ TCP |  |  |  |
335 | 14:03:58.704 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
336 | 14:03:58.706 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
337 | 14:03:58.709 |  | ←enobeB PCAP frame← TCP |  |  |
338 | 14:03:58.746 | →enobeB PCAP frame→ TCP |  |  |  |
339 | 14:03:58.954 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
340 | 14:03:58.955 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
341 | 14:03:58.965 |  |  |  |  | →SIP PUBLISH | P-CSCF
342 | 14:03:59.013 |  |  |  |  | MIKEY | Media-Server
343 | 14:03:59.074 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
344 | 14:03:59.075 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
345 | 14:03:59.075 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
346 | 14:03:59.228 |  |  |  |  | XML→ | Media-Server
347 | 14:03:59.232 |  |  |  |  | ←SIP 200 OK | P-CSCF
348 | 14:03:59.235 |  |  |  |  | ←SIP 200 OK | P-CSCF
349 | 14:03:59.235 |  |  |  |  | MIKEY | Media-Server
350 | 14:03:59.238 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
351 | 14:03:59.241 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
352 | 14:03:59.429 |  |  |  |  | XML→ | Media-Server
353 | 14:03:59.431 |  |  |  |  | XML→ | Media-Server
354 | 14:03:59.464 |  |  |  |  | MIKEY | Media-Server
355 | 14:03:59.465 |  |  |  |  | ←XML | Media-Server
356 | 14:03:59.470 |  |  |  |  | ←SIP NOTIFY | P-CSCF
357 | 14:03:59.477 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:38214;transp... |  |  |
358 | 14:03:59.512 |  |  |  |  | →SIP 200 OK | P-CSCF
359 | 14:03:59.514 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
360 | 14:03:59.519 |  |  |  |  | ←XML | Media-Server
361 | 14:03:59.527 |  |  |  |  | ←SIP MESSAGE | P-CSCF
362 | 14:03:59.533 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
363 | 14:04:00.512 |  |  |  |  | →SIP 200 OK | P-CSCF
364 | 14:04:00.514 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
365 | 14:04:00.519 |  |  |  |  | Info: MCX_IMS_CommonProcedures.ttcn:228: MESSAGE/200OK Table 5.3.2.3-2 Steps 7-8 Done
366 | 14:04:02.522 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
367 | 14:04:02.551 |  | ←RRC DCCH RRC Connection Release |  |  |
368 | 14:04:02.552 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
369 | 14:04:02.567 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
370 | 14:04:02.570 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
371 | 14:04:02.570 |  |  |  |  | MMICmd: Make the UE (MCPTT User) request the establishment of an MCPTT private call, manual commencement mode, and no floor control
372 | 14:04:19.093 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
373 | 14:04:19.093 |  | →RRC CCCH RRC Connection Request |  |  |
374 | 14:04:19.093 |  | ←RRC CCCH RRC Connection Setup |  |  |
375 | 14:04:19.093 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
376 | 14:04:19.146 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
377 | 14:04:19.146 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
378 | 14:04:19.146 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
379 | 14:04:19.146 |  |  |  | →NAS EMM Service request |  |
380 | 14:04:19.146 |  |  |  | NAS K-enb 8b8e68c6c1f2461ca006d19650fe5d85c... |  |
381 | 14:04:19.147 |  | ←RRC DCCH Security Mode Command |  |  |
382 | 14:04:19.147 |  |  | RRC K-enb 8b8e68c6c1f2461ca006d19650fe5d85c... |  |  |
383 | 14:04:19.147 |  |  | RRC rrc-cip 1de9a87fc1eaf5b61a163c8b290e798... |  |  |
384 | 14:04:19.147 |  |  | RRC rrc-int 9aece006acd208f778cb6186607e1be... |  |  |
385 | 14:04:19.147 |  |  | RRC up-cip 1aee9a6ad1280e5367a389e95c842829... |  |  |
386 | 14:04:19.147 |  |  | RRC up-int b49d9c12d203174381cbf6328972c7d3... |  |  |
387 | 14:04:19.148 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
388 | 14:04:19.186 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
389 | 14:04:19.186 |  | →RRC DCCH Security Mode Complete |  |  |
390 | 14:04:19.186 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
391 | 14:04:19.186 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
392 | 14:04:19.226 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
393 | 14:04:19.226 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
394 | 14:04:19.234 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
395 | 14:04:19.235 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |  |
396 | 14:04:19.246 |  |  |  |  | →SIP INVITE | P-CSCF
397 | 14:04:19.278 |  |  |  |  | MIKEY | Media-Server
398 | 14:04:19.481 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:754: SRTP config: Master Key: 63F27B8189CE5F6DFA685714A499400E, Master Salt: 0532C80A41CCCEEE679E5C34, MKI: 28AC6A74
399 | 14:04:19.481 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
400 | 14:04:19.485 |  |  |  |  | XML→ | Media-Server
401 | 14:04:19.485 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
402 | 14:04:19.486 |  |  |  |  | XML→ | Media-Server
403 | 14:04:19.488 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1257: INVITE Verdict: Pass
404 | 14:04:19.489 |  |  |  |  | ←SIP 100 Trying | P-CSCF
405 | 14:04:19.490 |  |  |  |  | ←SIP 180 Ringing | P-CSCF
406 | 14:04:19.491 |  |  |  |  | ←SIP 200 OK | P-CSCF
407 | 14:04:19.495 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
408 | 14:04:19.496 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 180 Ringing |  |  |
409 | 14:04:19.498 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
410 | 14:04:20.122 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
411 | 14:04:20.123 |  | [EMBEDDED NAS IN NEXT RRC] ESM Unknown message (type=0xa1) |  |  |
412 | 14:04:20.123 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
413 | 14:04:20.124 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration |  |  |
414 | 14:04:20.186 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
415 | 14:04:20.186 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
416 | 14:04:20.186 |  | →RRC DCCH UL Information Transfer |  |  |
417 | 14:04:20.186 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x3) |  |  |
418 | 14:04:20.186 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
419 | 14:04:20.250 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
420 | 14:04:20.472 |  |  |  |  | →SIP ACK | P-CSCF
421 | 14:04:20.474 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
422 | 14:04:20.478 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1262: ACK Verdict: Pass
423 | 14:04:21.026 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
424 | 14:04:21.034 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
425 | 14:04:21.042 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
426 | 14:04:21.066 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
427 | 14:04:21.074 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
428 | 14:04:21.229 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:480: Step 6 Verdict: Pass
429 | 14:04:21.335 |  |  |  |  | MMICmd: Release call (hang up the call)
430 | 14:04:23.122 |  |  |  |  | →SIP BYE | P-CSCF
431 | 14:04:23.143 |  |  |  |  | ←SIP 200 OK | P-CSCF
432 | 14:04:23.149 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
433 | 14:04:23.386 | →enobeB PCAP frame→ |  |  |  |
434 | 14:04:25.140 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
435 | 14:04:25.161 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
436 | 14:04:25.161 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xb) |  |  |
437 | 14:04:25.161 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
438 | 14:04:25.162 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
439 | 14:04:25.186 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
440 | 14:04:25.186 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
441 | 14:04:25.186 |  | →RRC DCCH UL Information Transfer |  |  |
442 | 14:04:25.186 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xc) |  |  |
443 | 14:04:25.186 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
444 | 14:04:25.276 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
445 | 14:04:25.278 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
446 | 14:04:25.317 |  | ←RRC DCCH RRC Connection Release |  |  |
447 | 14:04:25.318 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
448 | 14:04:25.332 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
449 | 14:04:25.334 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:486: Step 10 Verdict: Pass
450 | 14:04:25.335 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
451 | 14:04:25.337 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
452 | 14:04:26.085 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.