ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 15:04:56.084 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 15:04:56.088 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 15:04:56.088 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 15:04:56.090 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 15:04:56.090 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 15:04:56.091 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:824: IMS UDP port 192.168.2.3:5060 configured
7 | 15:04:56.094 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:774: IMS TCP port 192.168.2.3:5060 configured!
8 | 15:04:56.096 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:795: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 15:04:56.096 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:806: IdM port 192.168.2.3:8080 configured!
10 | 15:04:56.099 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 15:04:57.300 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 15:04:57.302 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 15:05:02.140 |  | ←RRC BCCH SIB1 |  |  |
14 | 15:05:02.215 |  | ←RRC BCCH SIB |  |  |
15 | 15:05:02.220 |  | ←RRC BCCH SIB1 |  |  |
16 | 15:05:02.235 |  | ←RRC BCCH SIB |  |  |
17 | 15:05:02.255 |  | ←RRC BCCH SIB |  |  |
18 | 15:05:54.424 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 15:05:54.424 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 15:05:54.424 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 15:05:54.424 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 15:05:54.475 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 15:05:54.475 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 15:05:54.475 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 15:05:54.475 |  |  |  | →NAS EMM Attach request |  |
26 | 15:05:54.475 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 15:05:54.476 |  |  |  | NAS K-asme 9f6549133f36f1f5643de3b76dce3a5f... |  |
28 | 15:05:54.476 |  |  |  | NAS ← EMM Authentication request |  |
29 | 15:05:54.476 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 15:05:54.476 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 15:05:54.477 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 15:05:54.547 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 15:05:54.547 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 15:05:54.547 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 15:05:54.547 |  |  |  | →NAS EMM Authentication response |  |
36 | 15:05:54.547 |  |  |  | NAS UE auth OK |  |
37 | 15:05:54.547 |  |  |  | NAS K-nas-cip 42f54610e4478fd60946633f02089... |  |
38 | 15:05:54.547 |  |  |  | NAS K-nas-int 4834f5f887a602c161f5ca0807555... |  |
39 | 15:05:54.547 |  |  |  | NAS ← EMM Security mode command |  |
40 | 15:05:54.548 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 15:05:54.548 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 15:05:54.549 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 15:05:54.587 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
44 | 15:05:54.587 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 15:05:54.587 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xc) |  |  |
46 | 15:05:54.587 |  |  |  | →NAS EMM Security mode complete |  |
47 | 15:05:54.587 |  |  |  | NAS ← ESM ESM information request |  |
48 | 15:05:54.588 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xd) |  |  |
49 | 15:05:54.588 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 15:05:54.589 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
51 | 15:05:54.597 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
52 | 15:05:54.635 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
53 | 15:05:54.635 |  | →RRC DCCH UL Information Transfer |  |  |
54 | 15:05:54.635 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x9) |  |  |
55 | 15:05:54.635 |  |  |  | →NAS ESM ESM information response |  |
56 | 15:05:54.635 |  |  |  | NAS ← EMM Attach accept |  |
57 | 15:05:54.635 |  |  |  | NAS K-enb 12372e33aa8431e8b2f1648d326cbcdfb... |  |
58 | 15:05:54.636 |  | ←RRC DCCH Security Mode Command |  |  |
59 | 15:05:54.636 |  |  | RRC K-enb 12372e33aa8431e8b2f1648d326cbcdfb... |  |  |
60 | 15:05:54.636 |  |  | RRC rrc-cip b6c89bfa8b003386bc9654a22450aa8... |  |  |
61 | 15:05:54.636 |  |  | RRC rrc-int 3e2e8444f2ea388ffb3728720ed6163... |  |  |
62 | 15:05:54.636 |  |  | RRC up-cip 4dbbe713e502e906be8c6c48a9589016... |  |  |
63 | 15:05:54.636 |  |  | RRC up-int 345f4dadbaecb7a4b615285fda22f464... |  |  |
64 | 15:05:54.637 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
65 | 15:05:54.667 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
66 | 15:05:54.667 |  | →RRC DCCH Security Mode Complete |  |  |
67 | 15:05:54.667 |  | ←RRC DCCH UE Capability Enquiry |  |  |
68 | 15:05:54.667 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
69 | 15:05:54.717 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
70 | 15:05:54.717 |  | →RRC DCCH UE Capability Information |  |  |
71 | 15:05:54.718 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x3) |  |  |
72 | 15:05:54.718 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
73 | 15:05:54.718 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
74 | 15:05:54.747 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
75 | 15:05:54.747 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
76 | 15:05:54.787 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
77 | 15:05:54.787 |  | →RRC DCCH UL Information Transfer |  |  |
78 | 15:05:54.787 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xb) |  |  |
79 | 15:05:54.787 |  |  |  | →NAS EMM Attach complete |  |
80 | 15:05:54.787 |  |  |  | NAS ← EMM EMM information |  |
81 | 15:05:54.788 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x9) |  |  |
82 | 15:05:54.788 |  | ←RRC DCCH DL Information Transfer |  |  |
83 | 15:05:54.789 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
84 | 15:05:59.454 |  | ←RRC DCCH RRC Connection Release |  |  |
85 | 15:05:59.454 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
86 | 15:06:00.964 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
87 | 15:06:00.964 |  | →RRC CCCH RRC Connection Request |  |  |
88 | 15:06:00.964 |  | ←RRC CCCH RRC Connection Setup |  |  |
89 | 15:06:00.964 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
90 | 15:06:01.027 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
91 | 15:06:01.027 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
92 | 15:06:01.027 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
93 | 15:06:01.028 |  |  | RRC K-enb 5f33f3a0c8fd3389dd6c7120429947397... |  |  |
94 | 15:06:01.028 |  |  |  | →NAS EMM Service request |  |
95 | 15:06:01.028 |  |  |  | NAS K-enb 5f33f3a0c8fd3389dd6c7120429947397... |  |
96 | 15:06:01.029 |  |  | RRC rrc-cip 453626e4610a0b3393ce085a71ebf94... |  |  |
97 | 15:06:01.029 |  |  | RRC rrc-int 14a4aa2b547ff04e607c77ca220c90e... |  |  |
98 | 15:06:01.029 |  |  | RRC up-cip d9ba2b74c8e7da912fae275a766b9b7f... |  |  |
99 | 15:06:01.029 |  |  | RRC up-int ef412c329bcab8b2b484ab7eaa915c1c... |  |  |
100 | 15:06:01.029 |  | ←RRC DCCH Security Mode Command |  |  |
101 | 15:06:01.029 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
102 | 15:06:01.067 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
103 | 15:06:01.067 |  | →RRC DCCH Security Mode Complete |  |  |
104 | 15:06:01.067 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
105 | 15:06:01.067 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
106 | 15:06:01.107 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
107 | 15:06:01.107 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
108 | 15:06:32.107 | →enobeB PCAP frame→ TCP |  |  |  |
109 | 15:06:32.111 |  | ←enobeB PCAP frame← TCP |  |  |
110 | 15:06:32.147 | →enobeB PCAP frame→ TCP |  |  |  |
111 | 15:06:32.235 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
112 | 15:06:32.238 |  | ←enobeB PCAP frame← TCP |  |  |
113 | 15:06:32.244 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
114 | 15:06:32.267 | →enobeB PCAP frame→ TCP |  |  |  |
115 | 15:06:32.355 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
116 | 15:06:32.357 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 16)
117 | 15:06:32.358 |  | ←enobeB PCAP frame← TCP |  |  |
118 | 15:06:32.359 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
119 | 15:06:32.387 | →enobeB PCAP frame→ TCP |  |  |  |
120 | 15:06:32.395 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
121 | 15:06:32.397 |  |  |  |  | →HTTP GET | HTTP-Proxy
122 | 15:06:32.398 |  | ←enobeB PCAP frame← TCP |  |  |
123 | 15:06:32.403 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:301: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
124 | 15:06:32.424 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
125 | 15:06:32.429 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
126 | 15:06:32.467 | →enobeB PCAP frame→ TCP |  |  |  |
127 | 15:06:34.347 | →enobeB PCAP frame→ TCP |  |  |  |
128 | 15:06:34.350 |  | ←enobeB PCAP frame← TCP |  |  |
129 | 15:06:34.387 | →enobeB PCAP frame→ TCP |  |  |  |
130 | 15:06:34.395 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
131 | 15:06:34.398 |  | ←enobeB PCAP frame← TCP |  |  |
132 | 15:06:34.404 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
133 | 15:06:34.427 | →enobeB PCAP frame→ TCP |  |  |  |
134 | 15:06:34.715 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
135 | 15:06:34.717 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
136 | 15:06:34.718 |  | ←enobeB PCAP frame← TCP |  |  |
137 | 15:06:34.719 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
138 | 15:06:34.747 | →enobeB PCAP frame→ TCP |  |  |  |
139 | 15:06:34.755 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
140 | 15:06:34.758 |  |  |  |  | →HTTP GET | IDMS-Endpoint
141 | 15:06:34.759 |  | ←enobeB PCAP frame← TCP |  |  |
142 | 15:06:34.792 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
143 | 15:06:34.795 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
144 | 15:06:34.795 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:524: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
145 | 15:06:34.796 |  |  |  |  | MMICmd: Please provide user credentials: username and password
146 | 15:06:34.867 | →enobeB PCAP frame→ TCP |  |  |  |
147 | 15:06:39.715 | →enobeB PCAP frame→ HTTPS: POST /idms/userauth HTTP/1.1 |  |  |  |
148 | 15:06:39.718 |  | ←enobeB PCAP frame← TCP |  |  |
149 | 15:06:39.719 |  |  |  |  | →HTTP POST | IDMS-Endpoint
150 | 15:06:39.736 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
151 | 15:06:39.738 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
152 | 15:06:39.738 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:529: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
153 | 15:06:39.747 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
154 | 15:06:39.752 |  | ←enobeB PCAP frame← TCP |  |  |
155 | 15:06:39.787 | →enobeB PCAP frame→ TCP |  |  |  |
156 | 15:06:39.788 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:693: IdM port - Client closed the connection (id 18)
157 | 15:06:39.791 |  | ←enobeB PCAP frame← TCP |  |  |
158 | 15:06:39.827 | →enobeB PCAP frame→ TCP |  |  |  |
159 | 15:06:40.227 | →enobeB PCAP frame→ TCP |  |  |  |
160 | 15:06:40.230 |  | ←enobeB PCAP frame← TCP |  |  |
161 | 15:06:40.267 | →enobeB PCAP frame→ TCP |  |  |  |
162 | 15:06:40.275 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
163 | 15:06:40.278 |  | ←enobeB PCAP frame← TCP |  |  |
164 | 15:06:40.280 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
165 | 15:06:40.307 | →enobeB PCAP frame→ TCP |  |  |  |
166 | 15:06:40.395 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
167 | 15:06:40.396 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
168 | 15:06:40.398 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
169 | 15:06:40.427 | →enobeB PCAP frame→ TCP |  |  |  |
170 | 15:06:40.444 |  |  |  |  | →HTTP POST | IDMS-Endpoint
171 | 15:06:40.446 |  | ←enobeB PCAP frame← TCP |  |  |
172 | 15:06:40.454 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
173 | 15:06:40.457 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
174 | 15:06:40.457 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:534: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
175 | 15:06:40.910 |  | ←enobeB PCAP frame← TCP |  |  |
176 | 15:06:40.947 | →enobeB PCAP frame→ TCP |  |  |  |
177 | 15:06:40.955 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
178 | 15:06:40.958 |  | ←enobeB PCAP frame← TCP |  |  |
179 | 15:06:40.962 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
180 | 15:06:40.987 | →enobeB PCAP frame→ TCP |  |  |  |
181 | 15:06:41.035 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
182 | 15:06:41.037 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 19)
183 | 15:06:41.038 |  | ←enobeB PCAP frame← TCP |  |  |
184 | 15:06:41.039 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
185 | 15:06:41.075 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
186 | 15:06:41.078 |  | ←enobeB PCAP frame← TCP |  |  |
187 | 15:06:41.078 |  |  |  |  | →HTTP POST | HTTP-Proxy
188 | 15:06:41.105 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:554: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
189 | 15:06:41.113 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
190 | 15:06:41.117 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
191 | 15:06:41.147 | →enobeB PCAP frame→ TCP |  |  |  |
192 | 15:06:41.187 | →enobeB PCAP frame→ TCP |  |  |  |
193 | 15:06:41.190 |  | ←enobeB PCAP frame← TCP |  |  |
194 | 15:06:41.227 | →enobeB PCAP frame→ TCP |  |  |  |
195 | 15:06:41.235 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
196 | 15:06:41.238 |  | ←enobeB PCAP frame← TCP |  |  |
197 | 15:06:41.241 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
198 | 15:06:41.267 | →enobeB PCAP frame→ TCP |  |  |  |
199 | 15:06:41.275 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
200 | 15:06:41.277 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 20)
201 | 15:06:41.278 |  | ←enobeB PCAP frame← TCP |  |  |
202 | 15:06:41.279 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
203 | 15:06:41.315 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
204 | 15:06:41.318 |  | ←enobeB PCAP frame← TCP |  |  |
205 | 15:06:41.318 |  |  |  |  | →HTTP POST | HTTP-Proxy
206 | 15:06:41.382 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
207 | 15:06:41.383 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:558: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
208 | 15:06:41.385 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
209 | 15:06:41.427 | →enobeB PCAP frame→ TCP |  |  |  |
210 | 15:06:41.475 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
211 | 15:06:41.479 |  |  |  |  | →SIP REGISTER | P-CSCF
212 | 15:06:41.489 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:833: IMS UDP_s port 192.168.2.3:5062 configured
213 | 15:06:41.490 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:784: IMS TCP_s port 192.168.2.3:5062 configured!
214 | 15:06:41.491 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:842: IMS UDP_c port 192.168.2.3:5061 configured
215 | 15:06:41.494 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
216 | 15:06:42.208 |  |  |  |  | →SIP REGISTER | P-CSCF
217 | 15:06:42.232 |  |  |  |  | ←SIP 200 OK | P-CSCF
218 | 15:06:42.236 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
219 | 15:06:42.556 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
220 | 15:06:42.568 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
221 | 15:06:42.582 |  |  |  |  | ←SIP 200 OK | P-CSCF
222 | 15:06:42.582 |  |  |  |  | MIKEY | Media-Server
223 | 15:06:42.585 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
224 | 15:06:42.785 |  |  |  |  | XML→ | Media-Server
225 | 15:06:42.786 |  |  |  |  | XML→ | Media-Server
226 | 15:06:42.789 |  |  |  |  | ←XML | Media-Server
227 | 15:06:42.792 |  |  |  |  | ←SIP NOTIFY | P-CSCF
228 | 15:06:42.795 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:39425;transp... |  |  |
229 | 15:06:42.836 |  |  |  |  | →SIP 200 OK | P-CSCF
230 | 15:06:43.070 |  | ←enobeB PCAP frame← TCP |  |  |
231 | 15:06:43.107 | →enobeB PCAP frame→ TCP |  |  |  |
232 | 15:06:43.115 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
233 | 15:06:43.118 |  | ←enobeB PCAP frame← TCP |  |  |
234 | 15:06:43.121 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
235 | 15:06:43.147 | →enobeB PCAP frame→ TCP |  |  |  |
236 | 15:06:43.195 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
237 | 15:06:43.197 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
238 | 15:06:43.198 |  | ←enobeB PCAP frame← TCP |  |  |
239 | 15:06:43.199 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
240 | 15:06:43.227 | →enobeB PCAP frame→ TCP |  |  |  |
241 | 15:06:43.235 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
242 | 15:06:43.237 |  |  |  |  | →HTTP GET | HTTP-Proxy
243 | 15:06:43.238 |  | ←enobeB PCAP frame← TCP |  |  |
244 | 15:06:43.247 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:655: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcptt-ue-configuration.xml
245 | 15:06:43.256 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
246 | 15:06:43.259 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
247 | 15:06:43.347 | →enobeB PCAP frame→ TCP |  |  |  |
248 | 15:06:43.355 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
249 | 15:06:43.357 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
250 | 15:06:43.359 |  | ←enobeB PCAP frame← TCP |  |  |
251 | 15:06:43.387 | →enobeB PCAP frame→ TCP |  |  |  |
252 | 15:06:43.507 | →enobeB PCAP frame→ TCP |  |  |  |
253 | 15:06:43.511 |  | ←enobeB PCAP frame← TCP |  |  |
254 | 15:06:43.547 | →enobeB PCAP frame→ TCP |  |  |  |
255 | 15:06:43.555 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
256 | 15:06:43.558 |  | ←enobeB PCAP frame← TCP |  |  |
257 | 15:06:43.561 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
258 | 15:06:43.587 | →enobeB PCAP frame→ TCP |  |  |  |
259 | 15:06:43.635 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
260 | 15:06:43.638 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
261 | 15:06:43.639 |  | ←enobeB PCAP frame← TCP |  |  |
262 | 15:06:43.640 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
263 | 15:06:43.667 | →enobeB PCAP frame→ TCP |  |  |  |
264 | 15:06:43.675 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
265 | 15:06:43.678 |  | ←enobeB PCAP frame← TCP |  |  |
266 | 15:06:43.678 |  |  |  |  | →HTTP GET | HTTP-Proxy
267 | 15:06:43.691 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:660: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcptt-user-profile-49.xml
268 | 15:06:43.733 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
269 | 15:06:43.740 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
270 | 15:06:43.741 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
271 | 15:06:43.787 | →enobeB PCAP frame→ TCP |  |  |  |
272 | 15:06:43.795 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
273 | 15:06:43.796 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
274 | 15:06:43.798 |  | ←enobeB PCAP frame← TCP |  |  |
275 | 15:06:43.827 | →enobeB PCAP frame→ TCP |  |  |  |
276 | 15:06:44.476 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
277 | 15:06:44.476 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
278 | 15:06:44.489 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
279 | 15:06:44.551 |  |  |  |  | ←SIP 200 OK | P-CSCF
280 | 15:06:44.551 |  |  |  |  | MIKEY | Media-Server
281 | 15:06:44.554 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
282 | 15:06:44.587 | →enobeB PCAP frame→ TCP |  |  |  |
283 | 15:06:44.590 |  | ←enobeB PCAP frame← TCP |  |  |
284 | 15:06:44.627 | →enobeB PCAP frame→ TCP |  |  |  |
285 | 15:06:44.635 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
286 | 15:06:44.638 |  | ←enobeB PCAP frame← TCP |  |  |
287 | 15:06:44.639 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
288 | 15:06:44.667 | →enobeB PCAP frame→ TCP |  |  |  |
289 | 15:06:44.715 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
290 | 15:06:44.716 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
291 | 15:06:44.718 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
292 | 15:06:44.747 | →enobeB PCAP frame→ TCP |  |  |  |
293 | 15:06:44.755 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
294 | 15:06:44.756 |  |  |  |  | →HTTP GET | HTTP-Proxy
295 | 15:06:44.757 |  |  |  |  | XML→ | Media-Server
296 | 15:06:44.758 |  | ←enobeB PCAP frame← TCP |  |  |
297 | 15:06:44.758 |  |  |  |  | XML→ | Media-Server
298 | 15:06:44.759 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:665: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
299 | 15:06:44.761 |  |  |  |  | ←XML | Media-Server
300 | 15:06:44.764 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
301 | 15:06:44.765 |  |  |  |  | ←SIP NOTIFY | P-CSCF
302 | 15:06:44.767 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
303 | 15:06:44.768 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:39425;transp... HTTPS: HTTP/1.1 200 OK |  |  |
304 | 15:06:44.787 | →enobeB PCAP frame→ TCP |  |  |  |
305 | 15:06:44.795 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
306 | 15:06:44.797 |  |  |  |  | →SIP 200 OK | P-CSCF
307 | 15:06:44.827 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
308 | 15:06:44.828 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
309 | 15:06:44.830 |  | ←enobeB PCAP frame← TCP |  |  |
310 | 15:06:44.835 | →enobeB PCAP frame→ TCP |  |  |  |
311 | 15:06:44.838 |  | ←enobeB PCAP frame← TCP |  |  |
312 | 15:06:44.867 | →enobeB PCAP frame→ TCP |  |  |  |
313 | 15:06:44.907 | →enobeB PCAP frame→ TCP |  |  |  |
314 | 15:06:44.910 |  | ←enobeB PCAP frame← TCP |  |  |
315 | 15:06:44.947 | →enobeB PCAP frame→ TCP |  |  |  |
316 | 15:06:44.955 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
317 | 15:06:44.958 |  | ←enobeB PCAP frame← TCP |  |  |
318 | 15:06:44.961 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
319 | 15:06:44.987 | →enobeB PCAP frame→ TCP |  |  |  |
320 | 15:06:45.035 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
321 | 15:06:45.037 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
322 | 15:06:45.038 |  | ←enobeB PCAP frame← TCP |  |  |
323 | 15:06:45.039 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
324 | 15:06:45.067 | →enobeB PCAP frame→ TCP |  |  |  |
325 | 15:06:45.075 | →enobeB PCAP frame→ HTTPS: GET http://xcap.gms.mcstaasting.com/org.openmobile... |  |  |  |
326 | 15:06:45.077 |  |  |  |  | →HTTP GET | HTTP-Proxy
327 | 15:06:45.078 |  | ←enobeB PCAP frame← TCP |  |  |
328 | 15:06:45.089 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:670: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at http://xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
329 | 15:06:45.118 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
330 | 15:06:45.124 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
331 | 15:06:45.147 | →enobeB PCAP frame→ TCP |  |  |  |
332 | 15:06:45.187 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
333 | 15:06:45.188 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
334 | 15:06:45.190 |  | ←enobeB PCAP frame← TCP |  |  |
335 | 15:06:45.195 | →enobeB PCAP frame→ TCP |  |  |  |
336 | 15:06:45.198 |  | ←enobeB PCAP frame← TCP |  |  |
337 | 15:06:45.227 | →enobeB PCAP frame→ TCP |  |  |  |
338 | 15:06:45.476 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
339 | 15:06:45.476 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
340 | 15:06:45.489 |  |  |  |  | →SIP PUBLISH | P-CSCF
341 | 15:06:45.538 |  |  |  |  | MIKEY | Media-Server
342 | 15:06:45.595 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
343 | 15:06:45.596 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
344 | 15:06:45.599 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
345 | 15:06:45.746 |  |  |  |  | XML→ | Media-Server
346 | 15:06:45.750 |  |  |  |  | ←SIP 200 OK | P-CSCF
347 | 15:06:45.752 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
348 | 15:06:45.753 |  |  |  |  | ←SIP 200 OK | P-CSCF
349 | 15:06:45.753 |  |  |  |  | MIKEY | Media-Server
350 | 15:06:45.756 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
351 | 15:06:45.947 |  |  |  |  | XML→ | Media-Server
352 | 15:06:45.948 |  |  |  |  | XML→ | Media-Server
353 | 15:06:45.982 |  |  |  |  | MIKEY | Media-Server
354 | 15:06:45.983 |  |  |  |  | ←XML | Media-Server
355 | 15:06:45.988 |  |  |  |  | ←SIP NOTIFY | P-CSCF
356 | 15:06:45.991 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:39425;transp... |  |  |
357 | 15:06:46.035 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
358 | 15:06:46.036 |  |  |  |  | →SIP 200 OK | P-CSCF
359 | 15:06:46.040 |  |  |  |  | ←XML | Media-Server
360 | 15:06:46.051 |  |  |  |  | ←SIP MESSAGE | P-CSCF
361 | 15:06:46.054 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
362 | 15:06:46.915 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
363 | 15:06:46.917 |  |  |  |  | →SIP 200 OK | P-CSCF
364 | 15:06:46.925 |  |  |  |  | Info: MCX_IMS_CommonProcedures.ttcn:228: MESSAGE/200OK Table 5.3.2.3-2 Steps 7-8 Done
365 | 15:06:48.928 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
366 | 15:06:48.973 |  | ←RRC DCCH RRC Connection Release |  |  |
367 | 15:06:48.974 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
368 | 15:06:48.993 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
369 | 15:06:49.068 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:754: SRTP config: Master Key: 06AC2AE901F84010FAE0F4ECA6EF0DFF, Master Salt: 0FFBDD646C9D2F34D10CCC19, MKI: 251BAD28
370 | 15:06:49.068 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
371 | 15:06:49.069 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
372 | 15:06:49.071 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
373 | 15:06:49.074 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
374 | 15:06:49.074 |  |  |  |  | ←XML | Media-Server
375 | 15:06:49.083 |  |  |  |  | ←SIP INVITE | P-CSCF
376 | 15:06:49.634 |  | ←enobeB PCAP frame← LTE RRC PCCH Paging (1 PagingRecord) |  |  |
377 | 15:06:49.634 |  | ←RRC PCCH Paging |  |  |
378 | 15:06:49.674 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
379 | 15:06:49.674 |  | →RRC CCCH RRC Connection Request |  |  |
380 | 15:06:49.674 |  | ←RRC CCCH RRC Connection Setup |  |  |
381 | 15:06:49.674 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
382 | 15:06:49.707 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
383 | 15:06:49.707 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
384 | 15:06:49.707 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
385 | 15:06:49.707 |  |  |  | →NAS EMM Service request |  |
386 | 15:06:49.707 |  |  |  | NAS K-enb 1096f05d4b826842b9f3e5704daf78cb1... |  |
387 | 15:06:49.708 |  |  | RRC K-enb 1096f05d4b826842b9f3e5704daf78cb1... |  |  |
388 | 15:06:49.709 |  |  | RRC rrc-cip 47edbb825337dfb9893edf4e58f21c5... |  |  |
389 | 15:06:49.709 |  |  | RRC rrc-int f9dd3abc7ecb0976fac61ef210d7b84... |  |  |
390 | 15:06:49.709 |  |  | RRC up-cip 961dca5fa5c250f6874246fe091a4d54... |  |  |
391 | 15:06:49.709 |  |  | RRC up-int daae323702035daedbcfc7b6cfdb58d9... |  |  |
392 | 15:06:49.709 |  | ←RRC DCCH Security Mode Command |  |  |
393 | 15:06:49.709 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
394 | 15:06:49.747 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
395 | 15:06:49.747 |  | →RRC DCCH Security Mode Complete |  |  |
396 | 15:06:49.747 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
397 | 15:06:49.747 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
398 | 15:06:49.787 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
399 | 15:06:49.787 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
400 | 15:06:49.789 |  | ←enobeB PCAP frame← SIP over IPSEC: INVITE sip:PublicUserId-A@192.168.3.2:39425;transp... |  |  |
401 | 15:06:49.835 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 100 Trying |  |  |  |
402 | 15:06:49.837 |  |  |  |  | →SIP 100 Trying | P-CSCF
403 | 15:06:50.075 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 180 Ringing |  |  |  |
404 | 15:06:50.078 |  |  |  |  | →SIP 180 Ringing | P-CSCF
405 | 15:06:50.092 |  |  |  |  | ←SIP PRACK | P-CSCF
406 | 15:06:50.095 |  | ←enobeB PCAP frame← SIP over IPSEC: PRACK sip:PublicUserId-A@192.168.3.2:39425;transpo... |  |  |
407 | 15:06:50.155 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
408 | 15:06:50.157 |  |  |  |  | →SIP 200 OK | P-CSCF
409 | 15:06:50.165 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:623: 180 Ringing Verdict: Pass
410 | 15:06:50.216 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
411 | 15:06:50.216 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x0) |  |  |
412 | 15:06:50.216 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
413 | 15:06:50.217 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
414 | 15:06:50.267 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
415 | 15:06:50.267 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
416 | 15:06:50.267 |  | →RRC DCCH UL Information Transfer |  |  |
417 | 15:06:50.267 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xd) |  |  |
418 | 15:06:50.267 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
419 | 15:06:50.337 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
420 | 15:06:50.916 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:635: Verdict: Pass
421 | 15:06:51.018 |  |  |  |  | MMICmd: Please Accept the Call
422 | 15:06:59.075 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
423 | 15:06:59.084 |  |  |  |  | →SIP 200 OK | P-CSCF
424 | 15:06:59.112 |  |  |  |  | XML→ | Media-Server
425 | 15:06:59.115 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:644: 200 OK Verdict: Pass
426 | 15:06:59.115 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:505: Step 1 Verdict: Pass
427 | 15:06:59.116 |  |  |  |  | ←SIP ACK | P-CSCF
428 | 15:06:59.119 |  | ←enobeB PCAP frame← SIP over IPSEC: ACK sip:PublicUserId-A@192.168.3.2:39425;transport... |  |  |
429 | 15:07:00.547 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
430 | 15:07:00.587 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
431 | 15:07:00.595 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
432 | 15:07:00.603 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
433 | 15:07:00.627 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
434 | 15:07:04.127 |  |  |  |  | ←SIP BYE | P-CSCF
435 | 15:07:04.130 |  | ←enobeB PCAP frame← SIP over IPSEC: BYE sip:PublicUserId-A@192.168.3.2:39425;transport... |  |  |
436 | 15:07:04.155 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK SRTP frame: |  |  |  |
437 | 15:07:04.157 |  |  |  |  | →SIP 200 OK | P-CSCF
438 | 15:07:04.159 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
439 | 15:07:04.160 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
440 | 15:07:04.163 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
441 | 15:07:04.166 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
442 | 15:07:04.387 | →enobeB PCAP frame→ |  |  |  |
443 | 15:07:06.166 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
444 | 15:07:06.170 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
445 | 15:07:06.170 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x4) |  |  |
446 | 15:07:06.170 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
447 | 15:07:06.171 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
448 | 15:07:06.227 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
449 | 15:07:06.227 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
450 | 15:07:06.227 |  | →RRC DCCH UL Information Transfer |  |  |
451 | 15:07:06.227 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x1) |  |  |
452 | 15:07:06.227 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
453 | 15:07:06.290 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
454 | 15:07:06.290 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
455 | 15:07:06.327 |  | ←RRC DCCH RRC Connection Release |  |  |
456 | 15:07:06.328 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
457 | 15:07:06.346 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
458 | 15:07:06.348 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:514: Step 8 Verdict: Pass
459 | 15:07:06.349 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
460 | 15:07:06.351 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
461 | 15:07:07.099 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.