ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 11:12:56.941 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 11:12:56.943 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 11:12:56.944 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 11:12:56.946 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 11:12:56.946 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 11:12:56.947 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:824: IMS UDP port 192.168.2.3:5060 configured
7 | 11:12:56.949 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:774: IMS TCP port 192.168.2.3:5060 configured!
8 | 11:12:56.950 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:795: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 11:12:56.951 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:806: IdM port 192.168.2.3:8080 configured!
10 | 11:12:56.953 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 11:12:58.154 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 11:12:58.157 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 11:13:07.240 |  | ←RRC BCCH SIB1 |  |  |
14 | 11:13:07.315 |  | ←RRC BCCH SIB |  |  |
15 | 11:13:07.320 |  | ←RRC BCCH SIB1 |  |  |
16 | 11:13:07.334 |  | ←RRC BCCH SIB |  |  |
17 | 11:13:07.355 |  | ←RRC BCCH SIB |  |  |
18 | 11:14:32.804 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 11:14:32.804 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 11:14:32.804 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 11:14:32.804 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 11:14:32.855 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 11:14:32.855 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 11:14:32.855 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 11:14:32.855 |  |  |  | →NAS EMM Attach request |  |
26 | 11:14:32.855 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 11:14:32.855 |  |  |  | NAS K-asme 23e3d3ef036a2277e85090b49cbc43f8... |  |
28 | 11:14:32.855 |  |  |  | NAS ← EMM Authentication request |  |
29 | 11:14:32.856 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 11:14:32.856 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 11:14:32.857 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 11:14:32.927 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 11:14:32.927 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 11:14:32.927 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 11:14:32.927 |  |  |  | →NAS EMM Authentication response |  |
36 | 11:14:32.927 |  |  |  | NAS UE auth OK |  |
37 | 11:14:32.927 |  |  |  | NAS K-nas-cip 27f5f0dbc2e7a62cb336df2612cff... |  |
38 | 11:14:32.927 |  |  |  | NAS K-nas-int cc4b610e682e3eafa24466ce49ebd... |  |
39 | 11:14:32.927 |  |  |  | NAS ← EMM Security mode command |  |
40 | 11:14:32.928 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 11:14:32.928 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 11:14:32.929 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 11:14:32.937 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
44 | 11:14:32.967 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
45 | 11:14:32.967 |  | →RRC DCCH UL Information Transfer |  |  |
46 | 11:14:32.967 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x8) |  |  |
47 | 11:14:32.967 |  |  |  | →NAS EMM Security mode complete |  |
48 | 11:14:32.967 |  |  |  | NAS ← ESM ESM information request |  |
49 | 11:14:32.968 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xc) |  |  |
50 | 11:14:32.968 |  | ←RRC DCCH DL Information Transfer |  |  |
51 | 11:14:32.969 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
52 | 11:14:33.015 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
53 | 11:14:33.015 |  | →RRC DCCH UL Information Transfer |  |  |
54 | 11:14:33.015 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x6) |  |  |
55 | 11:14:33.015 |  |  |  | →NAS ESM ESM information response |  |
56 | 11:14:33.015 |  |  |  | NAS ← EMM Attach accept |  |
57 | 11:14:33.015 |  |  |  | NAS K-enb 7150e049e2c3a681548dfa179f09ea7c0... |  |
58 | 11:14:33.016 |  | ←RRC DCCH Security Mode Command |  |  |
59 | 11:14:33.016 |  |  | RRC K-enb 7150e049e2c3a681548dfa179f09ea7c0... |  |  |
60 | 11:14:33.016 |  |  | RRC rrc-cip 5de8dcaee64752c2fba1614dc818233... |  |  |
61 | 11:14:33.016 |  |  | RRC rrc-int f6e3203bb825c74768ee15838d27d16... |  |  |
62 | 11:14:33.016 |  |  | RRC up-cip 018ad2a0c239d494e02b1de2978b656e... |  |  |
63 | 11:14:33.016 |  |  | RRC up-int 5fef93f8a79e2763ed1c0ba4984406d2... |  |  |
64 | 11:14:33.017 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
65 | 11:14:33.047 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
66 | 11:14:33.047 |  | →RRC DCCH Security Mode Complete |  |  |
67 | 11:14:33.047 |  | ←RRC DCCH UE Capability Enquiry |  |  |
68 | 11:14:33.047 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
69 | 11:14:33.097 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
70 | 11:14:33.097 |  | →RRC DCCH UE Capability Information |  |  |
71 | 11:14:33.097 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x9) |  |  |
72 | 11:14:33.097 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
73 | 11:14:33.097 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
74 | 11:14:33.127 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
75 | 11:14:33.127 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
76 | 11:14:33.167 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
77 | 11:14:33.167 |  | →RRC DCCH UL Information Transfer |  |  |
78 | 11:14:33.167 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x3) |  |  |
79 | 11:14:33.167 |  |  |  | →NAS EMM Attach complete |  |
80 | 11:14:33.167 |  |  |  | NAS ← EMM EMM information |  |
81 | 11:14:33.168 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xb) |  |  |
82 | 11:14:33.168 |  | ←RRC DCCH DL Information Transfer |  |  |
83 | 11:14:33.169 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
84 | 11:14:40.461 |  | ←RRC DCCH RRC Connection Release |  |  |
85 | 11:14:40.462 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
86 | 11:14:41.904 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
87 | 11:14:41.904 |  | →RRC CCCH RRC Connection Request |  |  |
88 | 11:14:41.904 |  | ←RRC CCCH RRC Connection Setup |  |  |
89 | 11:14:41.904 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
90 | 11:14:41.927 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
91 | 11:14:41.927 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
92 | 11:14:41.927 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
93 | 11:14:41.927 |  |  |  | →NAS EMM Service request |  |
94 | 11:14:41.927 |  |  |  | NAS K-enb 0645b55ef6da82a2c16f9f6611a808c1f... |  |
95 | 11:14:41.928 |  | ←RRC DCCH Security Mode Command |  |  |
96 | 11:14:41.928 |  |  | RRC K-enb 0645b55ef6da82a2c16f9f6611a808c1f... |  |  |
97 | 11:14:41.928 |  |  | RRC rrc-cip a919995cd7c5e576a1572d058fad8e7... |  |  |
98 | 11:14:41.928 |  |  | RRC rrc-int 32dae1b9a6f80e78df030b2c6777673... |  |  |
99 | 11:14:41.928 |  |  | RRC up-cip fa4c5985ff6d3c3cc5fd92f66d6ad62d... |  |  |
100 | 11:14:41.928 |  |  | RRC up-int fa9c381b5c568f624e1718fcd0c62c06... |  |  |
101 | 11:14:41.929 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
102 | 11:14:41.967 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
103 | 11:14:41.967 |  | →RRC DCCH Security Mode Complete |  |  |
104 | 11:14:41.967 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
105 | 11:14:41.967 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
106 | 11:14:42.007 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
107 | 11:14:42.007 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
108 | 11:15:00.527 | →enobeB PCAP frame→ TCP |  |  |  |
109 | 11:15:01.527 | →enobeB PCAP frame→ TCP |  |  |  |
110 | 11:15:01.552 |  | ←enobeB PCAP frame← TCP |  |  |
111 | 11:15:01.607 | →enobeB PCAP frame→ TCP |  |  |  |
112 | 11:15:01.695 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
113 | 11:15:01.699 |  | ←enobeB PCAP frame← TCP |  |  |
114 | 11:15:01.704 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
115 | 11:15:01.727 | →enobeB PCAP frame→ TCP |  |  |  |
116 | 11:15:01.815 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
117 | 11:15:01.816 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 16)
118 | 11:15:01.818 |  | ←enobeB PCAP frame← TCP |  |  |
119 | 11:15:01.819 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
120 | 11:15:01.847 | →enobeB PCAP frame→ TCP |  |  |  |
121 | 11:15:01.855 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
122 | 11:15:01.856 |  |  |  |  | →HTTP GET | HTTP-Proxy
123 | 11:15:01.859 |  | ←enobeB PCAP frame← TCP |  |  |
124 | 11:15:01.862 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:302: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
125 | 11:15:01.881 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
126 | 11:15:01.888 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
127 | 11:15:01.889 |  | ←enobeB PCAP frame← TCP |  |  |
128 | 11:15:01.890 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
129 | 11:15:01.927 | →enobeB PCAP frame→ TCP |  |  |  |
130 | 11:15:01.967 | →enobeB PCAP frame→ TCP |  |  |  |
131 | 11:15:03.607 | →enobeB PCAP frame→ TCP |  |  |  |
132 | 11:15:03.610 |  | ←enobeB PCAP frame← TCP |  |  |
133 | 11:15:03.647 | →enobeB PCAP frame→ TCP |  |  |  |
134 | 11:15:03.655 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
135 | 11:15:03.658 |  | ←enobeB PCAP frame← TCP |  |  |
136 | 11:15:03.664 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
137 | 11:15:03.687 | →enobeB PCAP frame→ TCP |  |  |  |
138 | 11:15:03.935 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
139 | 11:15:03.935 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
140 | 11:15:03.938 |  | ←enobeB PCAP frame← TCP |  |  |
141 | 11:15:03.939 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
142 | 11:15:03.967 | →enobeB PCAP frame→ TCP |  |  |  |
143 | 11:15:03.975 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
144 | 11:15:03.976 |  |  |  |  | →HTTP GET | IDMS-Endpoint
145 | 11:15:03.979 |  | ←enobeB PCAP frame← TCP |  |  |
146 | 11:15:03.987 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
147 | 11:15:03.991 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
148 | 11:15:03.991 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:525: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
149 | 11:15:03.991 |  |  |  |  | MMICmd: Please provide user credentials: username and password
150 | 11:15:04.047 | →enobeB PCAP frame→ TCP |  |  |  |
151 | 11:15:08.416 | →enobeB PCAP frame→ HTTPS: POST /idms/userauth HTTP/1.1 |  |  |  |
152 | 11:15:08.420 |  | ←enobeB PCAP frame← TCP |  |  |
153 | 11:15:08.420 |  |  |  |  | →HTTP POST | IDMS-Endpoint
154 | 11:15:08.434 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
155 | 11:15:08.437 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:530: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
156 | 11:15:08.438 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
157 | 11:15:08.487 | →enobeB PCAP frame→ TCP |  |  |  |
158 | 11:15:08.495 | →enobeB PCAP frame→ TCP |  |  |  |
159 | 11:15:08.495 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:693: IdM port - Client closed the connection (id 18)
160 | 11:15:08.498 |  | ←enobeB PCAP frame← TCP |  |  |
161 | 11:15:08.527 | →enobeB PCAP frame→ TCP |  |  |  |
162 | 11:15:08.967 | →enobeB PCAP frame→ TCP |  |  |  |
163 | 11:15:08.970 |  | ←enobeB PCAP frame← TCP |  |  |
164 | 11:15:09.007 | →enobeB PCAP frame→ TCP |  |  |  |
165 | 11:15:09.015 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
166 | 11:15:09.019 |  | ←enobeB PCAP frame← TCP |  |  |
167 | 11:15:09.023 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
168 | 11:15:09.047 | →enobeB PCAP frame→ TCP |  |  |  |
169 | 11:15:09.135 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
170 | 11:15:09.136 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
171 | 11:15:09.139 |  | ←enobeB PCAP frame← TCP |  |  |
172 | 11:15:09.140 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
173 | 11:15:09.167 | →enobeB PCAP frame→ TCP |  |  |  |
174 | 11:15:09.175 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
175 | 11:15:09.176 |  |  |  |  | →HTTP POST | IDMS-Endpoint
176 | 11:15:09.178 |  | ←enobeB PCAP frame← TCP |  |  |
177 | 11:15:09.191 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
178 | 11:15:09.194 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
179 | 11:15:09.194 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:535: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
180 | 11:15:09.247 | →enobeB PCAP frame→ TCP |  |  |  |
181 | 11:15:09.567 | →enobeB PCAP frame→ TCP |  |  |  |
182 | 11:15:09.570 |  | ←enobeB PCAP frame← TCP |  |  |
183 | 11:15:09.607 | →enobeB PCAP frame→ TCP |  |  |  |
184 | 11:15:09.615 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
185 | 11:15:09.618 |  | ←enobeB PCAP frame← TCP |  |  |
186 | 11:15:09.623 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
187 | 11:15:09.647 | →enobeB PCAP frame→ TCP |  |  |  |
188 | 11:15:09.695 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
189 | 11:15:09.696 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 19)
190 | 11:15:09.699 |  | ←enobeB PCAP frame← TCP |  |  |
191 | 11:15:09.700 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
192 | 11:15:09.735 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
193 | 11:15:09.737 |  |  |  |  | →HTTP POST | HTTP-Proxy
194 | 11:15:09.738 |  | ←enobeB PCAP frame← TCP |  |  |
195 | 11:15:09.761 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:555: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
196 | 11:15:09.767 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
197 | 11:15:09.774 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
198 | 11:15:09.775 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
199 | 11:15:09.807 | →enobeB PCAP frame→ TCP |  |  |  |
200 | 11:15:09.847 | →enobeB PCAP frame→ TCP |  |  |  |
201 | 11:15:09.851 |  | ←enobeB PCAP frame← TCP |  |  |
202 | 11:15:09.887 | →enobeB PCAP frame→ TCP |  |  |  |
203 | 11:15:09.895 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
204 | 11:15:09.899 |  | ←enobeB PCAP frame← TCP |  |  |
205 | 11:15:09.902 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
206 | 11:15:09.927 | →enobeB PCAP frame→ TCP |  |  |  |
207 | 11:15:09.935 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
208 | 11:15:09.936 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 20)
209 | 11:15:09.939 |  | ←enobeB PCAP frame← TCP |  |  |
210 | 11:15:09.940 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
211 | 11:15:09.975 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
212 | 11:15:09.978 |  |  |  |  | →HTTP POST | HTTP-Proxy
213 | 11:15:09.979 |  | ←enobeB PCAP frame← TCP |  |  |
214 | 11:15:10.037 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
215 | 11:15:10.037 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:559: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
216 | 11:15:10.042 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
217 | 11:15:10.043 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
218 | 11:15:10.087 | →enobeB PCAP frame→ TCP |  |  |  |
219 | 11:15:10.127 | →enobeB PCAP frame→ TCP |  |  |  |
220 | 11:15:10.135 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
221 | 11:15:10.137 |  |  |  |  | →SIP REGISTER | P-CSCF
222 | 11:15:10.159 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:833: IMS UDP_s port 192.168.2.3:5062 configured
223 | 11:15:10.183 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:784: IMS TCP_s port 192.168.2.3:5062 configured!
224 | 11:15:10.185 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:842: IMS UDP_c port 192.168.2.3:5061 configured
225 | 11:15:10.189 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
226 | 11:15:10.193 |  | ←enobeB PCAP frame← SIP -cleartext-: SIP/2.0 401 Unauthorized |  |  |
227 | 11:15:10.775 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
228 | 11:15:10.780 |  |  |  |  | →SIP REGISTER | P-CSCF
229 | 11:15:10.803 |  |  |  |  | ←SIP 200 OK | P-CSCF
230 | 11:15:10.808 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
231 | 11:15:11.095 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
232 | 11:15:11.097 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 SIP over IPSEC: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 |  |  |  |
233 | 11:15:11.110 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
234 | 11:15:11.162 |  |  |  |  | ←SIP 200 OK | P-CSCF
235 | 11:15:11.163 |  |  |  |  | MIKEY | Media-Server
236 | 11:15:11.166 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
237 | 11:15:11.372 |  |  |  |  | XML→ | Media-Server
238 | 11:15:11.373 |  |  |  |  | XML→ | Media-Server
239 | 11:15:11.376 |  |  |  |  | ←XML | Media-Server
240 | 11:15:11.380 |  |  |  |  | ←SIP NOTIFY | P-CSCF
241 | 11:15:11.384 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
242 | 11:15:11.385 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:48740;transp... |  |  |
243 | 11:15:11.415 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
244 | 11:15:11.415 |  |  |  |  | →SIP 200 OK | P-CSCF
245 | 11:15:11.567 | →enobeB PCAP frame→ TCP |  |  |  |
246 | 11:15:11.579 |  | ←enobeB PCAP frame← TCP |  |  |
247 | 11:15:11.607 | →enobeB PCAP frame→ TCP |  |  |  |
248 | 11:15:11.615 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
249 | 11:15:11.628 |  | ←enobeB PCAP frame← TCP |  |  |
250 | 11:15:11.629 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
251 | 11:15:11.687 | →enobeB PCAP frame→ TCP |  |  |  |
252 | 11:15:11.695 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
253 | 11:15:11.698 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
254 | 11:15:11.704 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
255 | 11:15:11.775 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
256 | 11:15:11.776 |  |  |  |  | →HTTP GET | HTTP-Proxy
257 | 11:15:11.778 |  | ←enobeB PCAP frame← TCP |  |  |
258 | 11:15:11.785 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:656: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcptt-ue-configuration.xml
259 | 11:15:11.794 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
260 | 11:15:11.798 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
261 | 11:15:11.847 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
262 | 11:15:11.847 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
263 | 11:15:11.851 |  | ←enobeB PCAP frame← TCP |  |  |
264 | 11:15:11.855 | →enobeB PCAP frame→ TCP |  |  |  |
265 | 11:15:11.858 |  | ←enobeB PCAP frame← TCP |  |  |
266 | 11:15:11.887 | →enobeB PCAP frame→ TCP |  |  |  |
267 | 11:15:12.007 | →enobeB PCAP frame→ TCP |  |  |  |
268 | 11:15:13.007 | →enobeB PCAP frame→ TCP |  |  |  |
269 | 11:15:13.010 |  | ←enobeB PCAP frame← TCP |  |  |
270 | 11:15:13.047 | →enobeB PCAP frame→ TCP |  |  |  |
271 | 11:15:13.057 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
272 | 11:15:13.065 |  | ←enobeB PCAP frame← TCP |  |  |
273 | 11:15:13.073 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
274 | 11:15:13.127 | →enobeB PCAP frame→ TCP |  |  |  |
275 | 11:15:13.135 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
276 | 11:15:13.141 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
277 | 11:15:13.147 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
278 | 11:15:13.167 | →enobeB PCAP frame→ TCP |  |  |  |
279 | 11:15:13.175 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
280 | 11:15:13.180 |  |  |  |  | →HTTP GET | HTTP-Proxy
281 | 11:15:13.194 |  | ←enobeB PCAP frame← TCP |  |  |
282 | 11:15:13.253 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:661: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcptt-user-profile-49.xml
283 | 11:15:13.290 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
284 | 11:15:13.298 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
285 | 11:15:13.299 |  | ←enobeB PCAP frame← TCP |  |  |
286 | 11:15:13.300 |  | ←enobeB PCAP frame← TCP |  |  |
287 | 11:15:13.301 |  | ←enobeB PCAP frame← TCP |  |  |
288 | 11:15:13.302 |  | ←enobeB PCAP frame← TCP |  |  |
289 | 11:15:13.303 |  | ←enobeB PCAP frame← TCP |  |  |
290 | 11:15:13.305 |  | ←enobeB PCAP frame← TCP |  |  |
291 | 11:15:13.306 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
292 | 11:15:13.327 | →enobeB PCAP frame→ TCP |  |  |  |
293 | 11:15:13.335 | →enobeB PCAP frame→ TCP |  |  |  |
294 | 11:15:13.367 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
295 | 11:15:13.367 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
296 | 11:15:13.370 |  | ←enobeB PCAP frame← TCP |  |  |
297 | 11:15:13.376 | →enobeB PCAP frame→ TCP |  |  |  |
298 | 11:15:13.379 |  | ←enobeB PCAP frame← TCP |  |  |
299 | 11:15:13.407 | →enobeB PCAP frame→ TCP |  |  |  |
300 | 11:15:14.015 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
301 | 11:15:14.016 | →enobeB PCAP frame→ IP DATA: Info RLC-LTE |  |  |  |
302 | 11:15:14.017 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
303 | 11:15:14.060 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
304 | 11:15:14.102 |  |  |  |  | ←SIP 200 OK | P-CSCF
305 | 11:15:14.103 |  |  |  |  | MIKEY | Media-Server
306 | 11:15:14.110 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
307 | 11:15:14.127 | →enobeB PCAP frame→ TCP |  |  |  |
308 | 11:15:14.136 |  | ←enobeB PCAP frame← TCP |  |  |
309 | 11:15:14.167 | →enobeB PCAP frame→ TCP |  |  |  |
310 | 11:15:14.175 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
311 | 11:15:14.192 |  | ←enobeB PCAP frame← TCP |  |  |
312 | 11:15:14.193 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
313 | 11:15:14.207 | →enobeB PCAP frame→ TCP |  |  |  |
314 | 11:15:14.255 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
315 | 11:15:14.260 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
316 | 11:15:14.267 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
317 | 11:15:14.295 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
318 | 11:15:14.295 |  |  |  |  | →HTTP GET | HTTP-Proxy
319 | 11:15:14.298 |  | ←enobeB PCAP frame← TCP |  |  |
320 | 11:15:14.298 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:666: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
321 | 11:15:14.304 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
322 | 11:15:14.310 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
323 | 11:15:14.311 |  | ←enobeB PCAP frame← TCP |  |  |
324 | 11:15:14.312 |  | ←enobeB PCAP frame← TCP |  |  |
325 | 11:15:14.313 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
326 | 11:15:14.313 |  |  |  |  | XML→ | Media-Server
327 | 11:15:14.314 |  |  |  |  | XML→ | Media-Server
328 | 11:15:14.317 |  |  |  |  | ←XML | Media-Server
329 | 11:15:14.320 |  |  |  |  | ←SIP NOTIFY | P-CSCF
330 | 11:15:14.325 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:48740;transp... |  |  |
331 | 11:15:14.367 | →enobeB PCAP frame→ TCP |  |  |  |
332 | 11:15:14.375 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK TLS: Mix Info |  |  |  |
333 | 11:15:14.377 |  |  |  |  | →SIP 200 OK | P-CSCF
334 | 11:15:14.377 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
335 | 11:15:14.379 |  | ←enobeB PCAP frame← TCP |  |  |
336 | 11:15:14.407 | →enobeB PCAP frame→ TCP |  |  |  |
337 | 11:15:14.415 | →enobeB PCAP frame→ TCP |  |  |  |
338 | 11:15:14.418 |  | ←enobeB PCAP frame← TCP |  |  |
339 | 11:15:14.447 | →enobeB PCAP frame→ TCP |  |  |  |
340 | 11:15:14.455 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
341 | 11:15:14.458 |  | ←enobeB PCAP frame← TCP |  |  |
342 | 11:15:14.462 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
343 | 11:15:14.487 | →enobeB PCAP frame→ TCP |  |  |  |
344 | 11:15:14.575 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
345 | 11:15:14.576 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
346 | 11:15:14.579 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
347 | 11:15:14.607 | →enobeB PCAP frame→ TCP |  |  |  |
348 | 11:15:14.615 | →enobeB PCAP frame→ HTTPS: GET http://xcap.gms.mcstaasting.com/org.openmobile... |  |  |  |
349 | 11:15:14.616 |  |  |  |  | →HTTP GET | HTTP-Proxy
350 | 11:15:14.618 |  | ←enobeB PCAP frame← TCP |  |  |
351 | 11:15:14.627 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:671: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at http://xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
352 | 11:15:14.653 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
353 | 11:15:14.661 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
354 | 11:15:14.662 |  | ←enobeB PCAP frame← TCP |  |  |
355 | 11:15:14.663 |  | ←enobeB PCAP frame← TCP |  |  |
356 | 11:15:14.664 |  | ←enobeB PCAP frame← TCP |  |  |
357 | 11:15:14.665 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
358 | 11:15:14.687 | →enobeB PCAP frame→ TCP |  |  |  |
359 | 11:15:14.695 | →enobeB PCAP frame→ TCP |  |  |  |
360 | 11:15:14.727 | →enobeB PCAP frame→ TCP |  |  |  |
361 | 11:15:14.735 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
362 | 11:15:14.736 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
363 | 11:15:14.738 |  | ←enobeB PCAP frame← TCP |  |  |
364 | 11:15:14.739 |  | ←enobeB PCAP frame← TCP |  |  |
365 | 11:15:14.767 | →enobeB PCAP frame→ TCP |  |  |  |
366 | 11:15:14.935 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
367 | 11:15:14.936 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
368 | 11:15:14.948 |  |  |  |  | →SIP PUBLISH | P-CSCF
369 | 11:15:14.996 |  |  |  |  | MIKEY | Media-Server
370 | 11:15:15.015 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
371 | 11:15:15.016 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
372 | 11:15:15.022 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
373 | 11:15:15.217 |  |  |  |  | XML→ | Media-Server
374 | 11:15:15.221 |  |  |  |  | ←SIP 200 OK | P-CSCF
375 | 11:15:15.224 |  |  |  |  | ←SIP 200 OK | P-CSCF
376 | 11:15:15.224 |  |  |  |  | MIKEY | Media-Server
377 | 11:15:15.226 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
378 | 11:15:15.230 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
379 | 11:15:15.427 |  |  |  |  | XML→ | Media-Server
380 | 11:15:15.428 |  |  |  |  | XML→ | Media-Server
381 | 11:15:15.462 |  |  |  |  | MIKEY | Media-Server
382 | 11:15:15.463 |  |  |  |  | ←XML | Media-Server
383 | 11:15:15.468 |  |  |  |  | ←SIP NOTIFY | P-CSCF
384 | 11:15:15.475 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
385 | 11:15:15.476 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
386 | 11:15:15.477 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:48740;transp... |  |  |
387 | 11:15:15.535 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
388 | 11:15:15.536 |  |  |  |  | →SIP 200 OK | P-CSCF
389 | 11:15:15.547 |  |  |  |  | ←XML | Media-Server
390 | 11:15:15.580 |  |  |  |  | ←SIP MESSAGE | P-CSCF
391 | 11:15:15.587 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
392 | 11:15:15.588 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
393 | 11:15:15.589 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
394 | 11:15:16.415 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
395 | 11:15:16.416 |  |  |  |  | →SIP 200 OK | P-CSCF
396 | 11:15:16.424 |  |  |  |  | Info: MCX_IMS_CommonProcedures.ttcn:228: MESSAGE/200OK Table 5.3.2.3-2 Steps 7-8 Done
397 | 11:15:18.488 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
398 | 11:15:18.536 |  | ←RRC DCCH RRC Connection Release |  |  |
399 | 11:15:18.537 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
400 | 11:15:18.555 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
401 | 11:15:18.556 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:1232: Test-Body Step 1
402 | 11:15:18.626 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:754: SRTP config: Master Key: A0C851C747E4F8A30600BE2D17F66A34, Master Salt: CA6A4AA7E07C9E7B8162D97E, MKI: 214CEC6E
403 | 11:15:18.626 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
404 | 11:15:18.627 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
405 | 11:15:18.629 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
406 | 11:15:18.633 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
407 | 11:15:18.633 |  |  |  |  | ←XML | Media-Server
408 | 11:15:18.642 |  |  |  |  | ←SIP INVITE | P-CSCF
409 | 11:15:19.374 |  | ←enobeB PCAP frame← LTE RRC PCCH Paging (1 PagingRecord) |  |  |
410 | 11:15:19.374 |  | ←RRC PCCH Paging |  |  |
411 | 11:15:19.414 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
412 | 11:15:19.414 |  | →RRC CCCH RRC Connection Request |  |  |
413 | 11:15:19.414 |  | ←RRC CCCH RRC Connection Setup |  |  |
414 | 11:15:19.414 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
415 | 11:15:19.447 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
416 | 11:15:19.447 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
417 | 11:15:19.447 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
418 | 11:15:19.447 |  |  |  | →NAS EMM Service request |  |
419 | 11:15:19.447 |  |  |  | NAS K-enb 46700134378ceb868c4b68ee3bcd5c8ab... |  |
420 | 11:15:19.448 |  | ←RRC DCCH Security Mode Command |  |  |
421 | 11:15:19.448 |  |  | RRC K-enb 46700134378ceb868c4b68ee3bcd5c8ab... |  |  |
422 | 11:15:19.448 |  |  | RRC rrc-cip 331a3cc1e049bae38b5b23a6f952a22... |  |  |
423 | 11:15:19.448 |  |  | RRC rrc-int f621e10d7645456468e7ebd6cf46a27... |  |  |
424 | 11:15:19.448 |  |  | RRC up-cip a38e03421edc9e744c787e8a59b9c5ca... |  |  |
425 | 11:15:19.448 |  |  | RRC up-int ce12b3cc7ffb50fcfa9f3a5a995869b6... |  |  |
426 | 11:15:19.449 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
427 | 11:15:19.487 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
428 | 11:15:19.487 |  | →RRC DCCH Security Mode Complete |  |  |
429 | 11:15:19.487 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
430 | 11:15:19.487 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
431 | 11:15:19.527 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
432 | 11:15:19.527 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
433 | 11:15:19.529 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
434 | 11:15:19.530 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
435 | 11:15:19.531 |  | ←enobeB PCAP frame← SIP over IPSEC: INVITE sip:PublicUserId-A@192.168.3.2:48740;transp... |  |  |
436 | 11:15:19.575 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 100 Trying |  |  |  |
437 | 11:15:19.576 |  |  |  |  | →SIP 100 Trying | P-CSCF
438 | 11:15:19.815 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
439 | 11:15:19.822 |  |  |  |  | →SIP 200 OK | P-CSCF
440 | 11:15:19.858 |  |  |  |  | XML→ | Media-Server
441 | 11:15:19.866 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:1235: Test-Body Step 2
442 | 11:15:19.867 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:1237: Test-Body Step 3
443 | 11:15:19.867 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:1240: Test-Body Step 3A
444 | 11:15:19.871 |  |  |  |  | ←SIP ACK | P-CSCF
445 | 11:15:19.872 |  |  |  |  | ←Floor Taken | Media-Server
446 | 11:15:19.875 |  | ←enobeB PCAP frame← SIP over IPSEC: ACK sip:PublicUserId-A@192.168.3.2:48740;transport... |  |  |
447 | 11:15:19.876 |  | ←enobeB PCAP frame← |  |  |
448 | 11:15:19.955 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
449 | 11:15:19.955 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x6) |  |  |
450 | 11:15:19.955 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
451 | 11:15:19.956 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
452 | 11:15:20.007 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
453 | 11:15:20.007 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
454 | 11:15:20.007 |  | →RRC DCCH UL Information Transfer |  |  |
455 | 11:15:20.007 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xa) |  |  |
456 | 11:15:20.007 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
457 | 11:15:20.079 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
458 | 11:15:20.618 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:1241: Step 3A Verdict: Pass
459 | 11:15:20.618 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:1243: Test-Body Step 4
460 | 11:15:20.618 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:1246: Test-Body Step 4A
461 | 11:15:20.719 |  |  |  |  | MMICmd: Request PTT token
462 | 11:15:25.622 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:1249: Test-Body Step 5
463 | 11:15:25.629 |  |  |  |  | ←SIP BYE | P-CSCF
464 | 11:15:25.634 |  | ←enobeB PCAP frame← SIP over IPSEC: BYE sip:PublicUserId-A@192.168.3.2:48740;transport... |  |  |
465 | 11:15:25.695 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
466 | 11:15:25.696 |  |  |  |  | →SIP 200 OK | P-CSCF
467 | 11:15:26.207 | →enobeB PCAP frame→ |  |  |  |
468 | 11:15:27.705 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
469 | 11:15:27.723 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
470 | 11:15:27.723 |  | [EMBEDDED NAS IN NEXT RRC] ESM Deactivate EPS bearer context reque... |  |  |
471 | 11:15:27.723 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
472 | 11:15:27.724 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration Deactivate EPS bearer context request (Unknown) |  |  |
473 | 11:15:27.767 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
474 | 11:15:27.767 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
475 | 11:15:27.767 |  | →RRC DCCH UL Information Transfer |  |  |
476 | 11:15:27.767 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x1) |  |  |
477 | 11:15:27.767 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
478 | 11:15:27.841 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
479 | 11:15:27.842 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
480 | 11:15:27.890 |  | ←RRC DCCH RRC Connection Release |  |  |
481 | 11:15:27.891 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
482 | 11:15:27.898 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
483 | 11:15:27.899 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:1251: Step 5 Verdict: Pass
484 | 11:15:27.901 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
485 | 11:15:27.903 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
486 | 11:15:28.651 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.