MSG #456 2021-10-26 11:15:20.007
NAS

     ESM: Activate dedicated EPS bearer context accept
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x2 (Integrity protected and ciphered)
    Auth code = 0x6592893e
    Sequence number = 0x05
    Protocol discriminator = 0x2 (EPS Session Management)
    EPS bearer identity = 6
    Procedure transaction identity = 0
    Message type = 0xc6 (Activate dedicated EPS bearer context accept)