MSG #375 2021-12-17 08:42:31.911

SIP INVITE message at 08:42:31.911

    INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0
    Via: SIP/2.0/UDP 192.168.3.2:48554;branch=z9hG4bK-63661453;rport
    From: <sip:PublicUserId-A@mcstaasting.com>;tag=864935061
    To: <sip:mcptt-server-A@mcstaasting.com>
    Contact: <sip:PublicUserId-A@192.168.3.2:48554;transport=udp>;+g.3gpp.mcptt;+g.3gpp.icsi-ref="urn%3Aurn-7%3A3gpp-service.ims.icsi.mcptt";audio;text;+g.3gpp.mcdata;+g.3gpp.icsi-ref="urn%3Aurn-7%3A3gpp-service.ims.icsi.mcdata";+g.3gpp.mcdata.sds;+g.3gpp.icsi-ref="urn%3Aurn-7%3A3gpp-service.ims.icsi.mcdata.sds"
    Call-ID: 9fb86225-8229-5a72-d8ad-4f200a0daa99
    CSeq: 1073743541 INVITE
    Content-Type: application/sdp
    Content-Length: 815
    Max-Forwards: 70
    Route: <sip:192.168.2.3:5062;lr>
    Route: <sip:scscf.3gpp.org;lr>
    Allow: INVITE, ACK, CANCEL, BYE, MESSAGE, OPTIONS, NOTIFY, PRACK, UPDATE, REFER
    Privacy: none
    P-Access-Network-Info: 3GPP-E-UTRAN-FDD;utran-cell-id-3gpp=0000000000000000
    User-Agent: MCS CLIENT SDK Nemergent 1.0 /v 7.2.6
    P-Preferred-Identity: <sip:PublicUserId-A@mcstaasting.com>
    Session-Expires: 3600;refresher=uac
    Supported: timer
    Supported: 100rel
    Accept-Contact: *;+g.3gpp.mcptt;require;explicit,*;+g.3gpp.icsi-ref="urn%3Aurn-7%3A3gpp-service.ims.icsi.mcptt";require;explicit
    Accept: application/sdp,application/vnd.3gpp.mcptt-info+xml
    P-Preferred-Service: urn:urn-7:3gpp-service.ims.icsi.mcptt
    Security-Client: ipsec-3gpp;alg=hmac-sha-1-96;ealg=aes-cbc;prot=esp;mod=trans;spi-c=1961244141;spi-s=564602719;port-c=47405;port-s=48554;q=0.9
    Security-Verify: ipsec-3gpp;alg=hmac-sha-1-96;ealg=aes-cbc;spi-c=257;spi-s=256;port-c=5061;port-s=5062;q=0.9
    Security-Verify: ipsec-3gpp;alg=hmac-md5-96;ealg=aes-cbc;spi-c=257;spi-s=256;port-c=5061;port-s=5062;q=0.7
    Require: sec-agree
    Proxy-Require: sec-agree

    v=0
    o=organization 1983 678901 IN IP4 192.168.3.2
    s=-
    c=IN IP4 192.168.3.2
    b=AS:24
    t=0 0
    a=ice-lite
    a=tcap:1
    m=audio 27448 RTP/SAVP 114 115
    i=speech
    b=AS:24
    a=ptime:20
    a=minptime:1
    a=maxptime:255
    a=rtpmap:114 AMR-WB/16000/1
    a=fmtp:114 octet-align=1;mode-change-capability=2;max-red=0
    a=rtpmap:115 AMR-WB/16000/1
    a=fmtp:115 octet-align=1;mode-change-capability=2;max-red=0
    a=sendrecv
    a=ssrc:2898908271 cname:75f62b27ef5a2631d1545c6a221cbd49
    a=ssrc:2898908271 mslabel:6994f7d1-6ce9-4fbd-acfd-84e511ca2e2
    a=ssrc:2898908271 label:organization@audio
    a=candidate:fhost 1 UDP 10 192.168.3.2 27448 typ host
    a=candidate:fhost 2 UDP 10 192.168.3.2 27449 typ host
    m=application 48266 udp MCPTT
    a=fmtp:MCPTT mc_priority=10;mc_granted;mc_queueing
    a=candidate:fhost 1 UDP 10 192.168.3.2 48266 typ host