ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 08:40:03.435 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 08:40:03.440 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 08:40:03.440 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 08:40:03.443 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 08:40:03.443 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 08:40:03.444 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:824: IMS UDP port 192.168.2.3:5060 configured
7 | 08:40:03.447 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:774: IMS TCP port 192.168.2.3:5060 configured!
8 | 08:40:03.449 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:795: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 08:40:03.450 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:806: IdM port 192.168.2.3:8080 configured!
10 | 08:40:03.453 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 08:40:04.654 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 08:40:04.656 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 08:40:08.553 |  | ←RRC BCCH SIB |  |  |
14 | 08:40:08.558 |  | ←RRC BCCH SIB1 |  |  |
15 | 08:40:08.638 |  | ←RRC BCCH SIB1 |  |  |
16 | 08:40:08.713 |  | ←RRC BCCH SIB |  |  |
17 | 08:40:08.718 |  | ←RRC BCCH SIB1 |  |  |
18 | 08:41:05.192 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 08:41:05.192 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 08:41:05.192 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 08:41:05.192 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 08:41:05.253 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 08:41:05.253 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 08:41:05.253 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 08:41:05.253 |  |  |  | →NAS EMM Attach request |  |
26 | 08:41:05.253 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 08:41:05.253 |  |  |  | NAS K-asme 885a5a4cf0e3c1105de399536653bbc3... |  |
28 | 08:41:05.253 |  |  |  | NAS ← EMM Authentication request |  |
29 | 08:41:05.254 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 08:41:05.254 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 08:41:05.255 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 08:41:05.325 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 08:41:05.325 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 08:41:05.325 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 08:41:05.325 |  |  |  | →NAS EMM Authentication response |  |
36 | 08:41:05.325 |  |  |  | NAS UE auth OK |  |
37 | 08:41:05.325 |  |  |  | NAS K-nas-cip 00000000000000000000000000000... |  |
38 | 08:41:05.325 |  |  |  | NAS K-nas-int 22eaeb26c88986fe8e75cbccdb245... |  |
39 | 08:41:05.325 |  |  |  | NAS ← EMM Security mode command |  |
40 | 08:41:05.326 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 08:41:05.326 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 08:41:05.327 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 08:41:05.365 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Security mode complete |  |  |  |
44 | 08:41:05.365 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 08:41:05.365 |  | [EMBEDDED NAS IN PREV RRC] EMM Security mode complete |  |  |
46 | 08:41:05.365 |  |  |  | →NAS EMM Security mode complete |  |
47 | 08:41:05.365 |  |  |  | NAS ← ESM ESM information request |  |
48 | 08:41:05.366 |  | [EMBEDDED NAS IN NEXT RRC] ESM ESM information request |  |  |
49 | 08:41:05.366 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 08:41:05.367 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer ESM information request |  |  |
51 | 08:41:05.413 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer ESM information response |  |  |  |
52 | 08:41:05.413 |  | →RRC DCCH UL Information Transfer |  |  |
53 | 08:41:05.413 |  | [EMBEDDED NAS IN PREV RRC] ESM ESM information response |  |  |
54 | 08:41:05.413 |  |  |  | →NAS ESM ESM information response |  |
55 | 08:41:05.413 |  |  |  | NAS K-enb 127044dea94ce4cce5d16f94636e71746... |  |
56 | 08:41:05.413 |  |  |  | NAS ← EMM Attach accept |  |
57 | 08:41:05.414 |  | ←RRC DCCH Security Mode Command |  |  |
58 | 08:41:05.414 |  |  | RRC K-enb 127044dea94ce4cce5d16f94636e71746... |  |  |
59 | 08:41:05.414 |  |  | RRC rrc-cip b0fd3c18fa9d7c739689259784cf38b... |  |  |
60 | 08:41:05.414 |  |  | RRC rrc-int 067facf8876942b21d1dce950a2e341... |  |  |
61 | 08:41:05.414 |  |  | RRC up-cip 4d3f5dd14c43d636d9a0d7d14d304ec5... |  |  |
62 | 08:41:05.414 |  |  | RRC up-int 2ae62898e18fd4a0424f42a47a78d855... |  |  |
63 | 08:41:05.415 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
64 | 08:41:05.445 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
65 | 08:41:05.445 |  | →RRC DCCH Security Mode Complete |  |  |
66 | 08:41:05.445 |  | ←RRC DCCH UE Capability Enquiry |  |  |
67 | 08:41:05.445 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
68 | 08:41:05.495 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
69 | 08:41:05.495 |  | →RRC DCCH UE Capability Information |  |  |
70 | 08:41:05.495 |  | [EMBEDDED NAS IN NEXT RRC] EMM Attach accept |  |  |
71 | 08:41:05.495 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
72 | 08:41:05.495 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration Attach accept Activate default EPS bearer context request (PDN ... |  |  |
73 | 08:41:05.525 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
74 | 08:41:05.525 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
75 | 08:41:05.565 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Attach complete Activate default EPS bearer context accept |  |  |  |
76 | 08:41:05.565 |  | →RRC DCCH UL Information Transfer |  |  |
77 | 08:41:05.565 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach complete |  |  |
78 | 08:41:05.565 |  |  |  | →NAS EMM Attach complete |  |
79 | 08:41:05.565 |  |  |  | NAS ← EMM EMM information |  |
80 | 08:41:05.566 |  | [EMBEDDED NAS IN NEXT RRC] EMM EMM information |  |  |
81 | 08:41:05.566 |  | ←RRC DCCH DL Information Transfer |  |  |
82 | 08:41:05.567 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer EMM information |  |  |
83 | 08:41:12.015 |  | ←RRC DCCH RRC Connection Release |  |  |
84 | 08:41:12.016 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
85 | 08:41:13.652 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
86 | 08:41:13.652 |  | →RRC CCCH RRC Connection Request |  |  |
87 | 08:41:13.652 |  | ←RRC CCCH RRC Connection Setup |  |  |
88 | 08:41:13.652 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
89 | 08:41:13.685 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
90 | 08:41:13.685 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
91 | 08:41:13.685 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
92 | 08:41:13.685 |  |  |  | →NAS EMM Service request |  |
93 | 08:41:13.685 |  |  |  | NAS K-enb 98a2f4ddc090f9708ad40ac8ae7ca50b7... |  |
94 | 08:41:13.686 |  | ←RRC DCCH Security Mode Command |  |  |
95 | 08:41:13.686 |  |  | RRC K-enb 98a2f4ddc090f9708ad40ac8ae7ca50b7... |  |  |
96 | 08:41:13.686 |  |  | RRC rrc-cip 450526863ea5acf289cd1c4f0d4232f... |  |  |
97 | 08:41:13.686 |  |  | RRC rrc-int bb76d41030dd61ebd6207bc3990644d... |  |  |
98 | 08:41:13.686 |  |  | RRC up-cip 29c2f397edcb743f4d250bc17fdd890d... |  |  |
99 | 08:41:13.686 |  |  | RRC up-int 0e86a589b83cc181bd640068f439cb23... |  |  |
100 | 08:41:13.687 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
101 | 08:41:13.725 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
102 | 08:41:13.725 |  | →RRC DCCH Security Mode Complete |  |  |
103 | 08:41:13.725 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
104 | 08:41:13.725 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
105 | 08:41:13.765 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
106 | 08:41:13.765 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
107 | 08:42:04.525 | →enobeB PCAP frame→ TCP |  |  |  |
108 | 08:42:04.529 |  | ←enobeB PCAP frame← TCP |  |  |
109 | 08:42:04.565 | →enobeB PCAP frame→ TCP |  |  |  |
110 | 08:42:04.653 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
111 | 08:42:04.657 |  | ←enobeB PCAP frame← TCP |  |  |
112 | 08:42:04.662 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
113 | 08:42:04.685 | →enobeB PCAP frame→ TCP |  |  |  |
114 | 08:42:04.853 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
115 | 08:42:04.857 |  | ←enobeB PCAP frame← TCP |  |  |
116 | 08:42:04.858 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
117 | 08:42:04.866 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 16)
118 | 08:42:04.885 | →enobeB PCAP frame→ TCP |  |  |  |
119 | 08:42:04.893 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
120 | 08:42:04.896 |  | ←enobeB PCAP frame← TCP |  |  |
121 | 08:42:04.906 |  |  |  |  | →HTTP GET | HTTP-Proxy
122 | 08:42:04.912 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:307: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
123 | 08:42:04.925 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
124 | 08:42:04.930 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
125 | 08:42:04.965 | →enobeB PCAP frame→ TCP |  |  |  |
126 | 08:42:07.285 | →enobeB PCAP frame→ TCP |  |  |  |
127 | 08:42:07.289 |  | ←enobeB PCAP frame← TCP |  |  |
128 | 08:42:07.325 | →enobeB PCAP frame→ TCP |  |  |  |
129 | 08:42:07.333 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
130 | 08:42:07.337 |  | ←enobeB PCAP frame← TCP |  |  |
131 | 08:42:07.342 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
132 | 08:42:07.365 | →enobeB PCAP frame→ TCP |  |  |  |
133 | 08:42:07.733 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
134 | 08:42:07.737 |  | ←enobeB PCAP frame← TCP |  |  |
135 | 08:42:07.738 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
136 | 08:42:07.746 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
137 | 08:42:07.765 | →enobeB PCAP frame→ TCP |  |  |  |
138 | 08:42:07.773 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
139 | 08:42:07.776 |  | ←enobeB PCAP frame← TCP |  |  |
140 | 08:42:07.782 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
141 | 08:42:07.785 |  |  |  |  | →HTTP GET | IDMS-Endpoint
142 | 08:42:07.790 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
143 | 08:42:07.794 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:526: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
144 | 08:42:07.794 |  |  |  |  | MMICmd: Please provide user credentials: username and password
145 | 08:42:07.845 | →enobeB PCAP frame→ TCP |  |  |  |
146 | 08:42:12.853 | →enobeB PCAP frame→ HTTPS: POST /idms/userauth HTTP/1.1 |  |  |  |
147 | 08:42:12.861 |  | ←enobeB PCAP frame← TCP |  |  |
148 | 08:42:12.868 |  |  |  |  | →HTTP POST | IDMS-Endpoint
149 | 08:42:12.874 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
150 | 08:42:12.881 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
151 | 08:42:12.884 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:531: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
152 | 08:42:12.925 | →enobeB PCAP frame→ TCP |  |  |  |
153 | 08:42:12.933 | →enobeB PCAP frame→ TCP |  |  |  |
154 | 08:42:12.937 |  | ←enobeB PCAP frame← TCP |  |  |
155 | 08:42:12.945 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:693: IdM port - Client closed the connection (id 18)
156 | 08:42:12.965 | →enobeB PCAP frame→ TCP |  |  |  |
157 | 08:42:13.565 | →enobeB PCAP frame→ TCP |  |  |  |
158 | 08:42:13.569 |  | ←enobeB PCAP frame← TCP |  |  |
159 | 08:42:13.605 | →enobeB PCAP frame→ TCP |  |  |  |
160 | 08:42:13.653 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
161 | 08:42:13.657 |  | ←enobeB PCAP frame← TCP |  |  |
162 | 08:42:13.659 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
163 | 08:42:13.685 | →enobeB PCAP frame→ TCP |  |  |  |
164 | 08:42:13.853 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
165 | 08:42:13.857 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
166 | 08:42:13.866 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
167 | 08:42:13.885 | →enobeB PCAP frame→ TCP |  |  |  |
168 | 08:42:13.893 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
169 | 08:42:13.897 |  | ←enobeB PCAP frame← TCP |  |  |
170 | 08:42:13.902 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
171 | 08:42:13.905 |  |  |  |  | →HTTP POST | IDMS-Endpoint
172 | 08:42:13.910 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
173 | 08:42:13.914 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:536: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
174 | 08:42:13.965 | →enobeB PCAP frame→ TCP |  |  |  |
175 | 08:42:14.325 | →enobeB PCAP frame→ TCP |  |  |  |
176 | 08:42:14.329 |  | ←enobeB PCAP frame← TCP |  |  |
177 | 08:42:14.365 | →enobeB PCAP frame→ TCP |  |  |  |
178 | 08:42:14.373 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
179 | 08:42:14.377 |  | ←enobeB PCAP frame← TCP |  |  |
180 | 08:42:14.380 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
181 | 08:42:14.405 | →enobeB PCAP frame→ TCP |  |  |  |
182 | 08:42:14.413 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
183 | 08:42:14.417 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
184 | 08:42:14.426 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 19)
185 | 08:42:14.453 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
186 | 08:42:14.458 |  | ←enobeB PCAP frame← TCP |  |  |
187 | 08:42:14.468 |  |  |  |  | →HTTP POST | HTTP-Proxy
188 | 08:42:14.492 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:554: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
189 | 08:42:14.493 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
190 | 08:42:14.500 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
191 | 08:42:14.525 | →enobeB PCAP frame→ TCP |  |  |  |
192 | 08:42:14.565 | →enobeB PCAP frame→ TCP |  |  |  |
193 | 08:42:14.569 |  | ←enobeB PCAP frame← TCP |  |  |
194 | 08:42:14.605 | →enobeB PCAP frame→ TCP |  |  |  |
195 | 08:42:14.613 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
196 | 08:42:14.617 |  | ←enobeB PCAP frame← TCP |  |  |
197 | 08:42:14.620 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
198 | 08:42:14.645 | →enobeB PCAP frame→ TCP |  |  |  |
199 | 08:42:14.653 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
200 | 08:42:14.657 |  | ←enobeB PCAP frame← TCP |  |  |
201 | 08:42:14.658 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
202 | 08:42:14.666 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 20)
203 | 08:42:14.693 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
204 | 08:42:14.697 |  | ←enobeB PCAP frame← TCP |  |  |
205 | 08:42:14.708 |  |  |  |  | →HTTP POST | HTTP-Proxy
206 | 08:42:14.762 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
207 | 08:42:14.770 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
208 | 08:42:14.770 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:558: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
209 | 08:42:14.805 | →enobeB PCAP frame→ TCP |  |  |  |
210 | 08:42:14.876 |  |  |  |  | →SIP REGISTER | P-CSCF
211 | 08:42:14.900 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:833: IMS UDP_s port 192.168.2.3:5062 configured
212 | 08:42:14.930 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:784: IMS TCP_s port 192.168.2.3:5062 configured!
213 | 08:42:14.931 |  | ←enobeB PCAP frame← SIP -cleartext-: SIP/2.0 401 Unauthorized |  |  |
214 | 08:42:14.932 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:842: IMS UDP_c port 192.168.2.3:5061 configured
215 | 08:42:14.939 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
216 | 08:42:15.848 |  |  |  |  | →SIP REGISTER | P-CSCF
217 | 08:42:15.852 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
218 | 08:42:15.860 |  |  |  |  | ←SIP 200 OK | P-CSCF
219 | 08:42:16.255 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
220 | 08:42:16.264 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
221 | 08:42:16.272 |  |  |  |  | ←SIP 200 OK | P-CSCF
222 | 08:42:16.273 |  |  |  |  | MIKEY | Media-Server
223 | 08:42:16.467 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:48554;transp... |  |  |
224 | 08:42:16.467 |  |  |  |  | XML→ | Media-Server
225 | 08:42:16.468 |  |  |  |  | XML→ | Media-Server
226 | 08:42:16.472 |  |  |  |  | ←XML | Media-Server
227 | 08:42:16.475 |  |  |  |  | ←SIP NOTIFY | P-CSCF
228 | 08:42:16.506 |  |  |  |  | →SIP 200 OK | P-CSCF
229 | 08:42:16.929 |  | ←enobeB PCAP frame← TCP |  |  |
230 | 08:42:16.965 | →enobeB PCAP frame→ TCP |  |  |  |
231 | 08:42:16.973 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
232 | 08:42:16.977 |  | ←enobeB PCAP frame← TCP |  |  |
233 | 08:42:16.980 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
234 | 08:42:17.005 | →enobeB PCAP frame→ TCP |  |  |  |
235 | 08:42:17.093 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
236 | 08:42:17.097 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
237 | 08:42:17.106 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
238 | 08:42:17.125 | →enobeB PCAP frame→ TCP |  |  |  |
239 | 08:42:17.173 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
240 | 08:42:17.179 |  | ←enobeB PCAP frame← TCP |  |  |
241 | 08:42:17.187 |  |  |  |  | →HTTP GET | HTTP-Proxy
242 | 08:42:17.196 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:691: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcpttue-configuration.xml
243 | 08:42:17.197 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
244 | 08:42:17.204 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
245 | 08:42:17.245 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
246 | 08:42:17.249 |  | ←enobeB PCAP frame← TCP |  |  |
247 | 08:42:17.253 | →enobeB PCAP frame→ TCP |  |  |  |
248 | 08:42:17.257 |  | ←enobeB PCAP frame← TCP |  |  |
249 | 08:42:17.258 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
250 | 08:42:17.285 | →enobeB PCAP frame→ TCP |  |  |  |
251 | 08:42:17.445 | →enobeB PCAP frame→ TCP |  |  |  |
252 | 08:42:17.448 |  | ←enobeB PCAP frame← TCP |  |  |
253 | 08:42:17.485 | →enobeB PCAP frame→ TCP |  |  |  |
254 | 08:42:17.493 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
255 | 08:42:17.499 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
256 | 08:42:17.525 | →enobeB PCAP frame→ TCP |  |  |  |
257 | 08:42:17.573 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
258 | 08:42:17.577 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
259 | 08:42:17.586 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
260 | 08:42:17.605 | →enobeB PCAP frame→ TCP |  |  |  |
261 | 08:42:17.625 |  | ←enobeB PCAP frame← TCP |  |  |
262 | 08:42:17.634 |  |  |  |  | →HTTP GET | HTTP-Proxy
263 | 08:42:17.647 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:696: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcpttuser-profile-49.xml
264 | 08:42:17.692 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
265 | 08:42:17.693 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
266 | 08:42:17.693 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
267 | 08:42:17.741 | →enobeB PCAP frame→ TCP |  |  |  |
268 | 08:42:17.745 |  | ←enobeB PCAP frame← TCP |  |  |
269 | 08:42:17.753 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
270 | 08:42:17.765 | →enobeB PCAP frame→ TCP |  |  |  |
271 | 08:42:18.569 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
272 | 08:42:18.574 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
273 | 08:42:18.582 |  |  |  |  | ←SIP 200 OK | P-CSCF
274 | 08:42:18.582 |  |  |  |  | MIKEY | Media-Server
275 | 08:42:18.728 |  | ←enobeB PCAP frame← TCP |  |  |
276 | 08:42:18.771 |  |  |  |  | XML→ | Media-Server
277 | 08:42:18.772 |  |  |  |  | XML→ | Media-Server
278 | 08:42:18.773 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
279 | 08:42:18.775 |  |  |  |  | ←XML | Media-Server
280 | 08:42:18.776 |  | ←enobeB PCAP frame← TCP |  |  |
281 | 08:42:18.777 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
282 | 08:42:18.805 | →enobeB PCAP frame→ TCP |  |  |  |
283 | 08:42:18.893 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
284 | 08:42:18.897 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
285 | 08:42:18.902 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:48554;transp... |  |  |
286 | 08:42:18.906 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
287 | 08:42:18.909 |  |  |  |  | ←SIP NOTIFY | P-CSCF
288 | 08:42:18.925 | →enobeB PCAP frame→ TCP |  |  |  |
289 | 08:42:18.945 |  | ←enobeB PCAP frame← TCP |  |  |
290 | 08:42:18.954 |  |  |  |  | →SIP 200 OK | P-CSCF
291 | 08:42:18.954 |  |  |  |  | →HTTP GET | HTTP-Proxy
292 | 08:42:18.957 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
293 | 08:42:18.957 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:701: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
294 | 08:42:18.958 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
295 | 08:42:18.964 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
296 | 08:42:19.025 |  | ←enobeB PCAP frame← TCP |  |  |
297 | 08:42:19.029 | →enobeB PCAP frame→ TCP |  |  |  |
298 | 08:42:19.033 |  | ←enobeB PCAP frame← TCP |  |  |
299 | 08:42:19.034 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
300 | 08:42:19.045 | →enobeB PCAP frame→ TCP |  |  |  |
301 | 08:42:19.125 | →enobeB PCAP frame→ TCP |  |  |  |
302 | 08:42:19.129 |  | ←enobeB PCAP frame← TCP |  |  |
303 | 08:42:19.165 | →enobeB PCAP frame→ TCP |  |  |  |
304 | 08:42:19.253 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
305 | 08:42:19.256 |  | ←enobeB PCAP frame← TCP |  |  |
306 | 08:42:19.260 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
307 | 08:42:19.285 | →enobeB PCAP frame→ TCP |  |  |  |
308 | 08:42:19.493 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
309 | 08:42:19.497 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
310 | 08:42:19.506 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
311 | 08:42:19.525 | →enobeB PCAP frame→ TCP |  |  |  |
312 | 08:42:19.573 | →enobeB PCAP frame→ HTTPS: GET http://xcap.gms.mcstaasting.com/org.openmobile... |  |  |  |
313 | 08:42:19.577 |  | ←enobeB PCAP frame← TCP |  |  |
314 | 08:42:19.586 |  |  |  |  | →HTTP GET | HTTP-Proxy
315 | 08:42:19.594 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:706: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at http://xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
316 | 08:42:19.606 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
317 | 08:42:19.613 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
318 | 08:42:19.645 | →enobeB PCAP frame→ TCP |  |  |  |
319 | 08:42:19.653 | →enobeB PCAP frame→ TCP |  |  |  |
320 | 08:42:19.685 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
321 | 08:42:19.689 |  | ←enobeB PCAP frame← TCP |  |  |
322 | 08:42:19.693 | →enobeB PCAP frame→ TCP |  |  |  |
323 | 08:42:19.696 |  | ←enobeB PCAP frame← TCP |  |  |
324 | 08:42:19.698 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
325 | 08:42:19.725 | →enobeB PCAP frame→ TCP |  |  |  |
326 | 08:42:19.855 |  |  |  |  | →SIP PUBLISH | P-CSCF
327 | 08:42:19.879 |  |  |  |  | MIKEY | Media-Server
328 | 08:42:19.924 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
329 | 08:42:20.066 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
330 | 08:42:20.069 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
331 | 08:42:20.071 |  |  |  |  | XML→ | Media-Server
332 | 08:42:20.074 |  |  |  |  | ←SIP 200 OK | P-CSCF
333 | 08:42:20.077 |  |  |  |  | ←SIP 200 OK | P-CSCF
334 | 08:42:20.078 |  |  |  |  | MIKEY | Media-Server
335 | 08:42:20.266 |  |  |  |  | XML→ | Media-Server
336 | 08:42:20.267 |  |  |  |  | XML→ | Media-Server
337 | 08:42:20.298 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:48554;transp... |  |  |
338 | 08:42:20.301 |  |  |  |  | MIKEY | Media-Server
339 | 08:42:20.301 |  |  |  |  | ←XML | Media-Server
340 | 08:42:20.306 |  |  |  |  | ←SIP NOTIFY | P-CSCF
341 | 08:42:20.346 |  |  |  |  | →SIP 200 OK | P-CSCF
342 | 08:42:20.348 |  |  |  |  | ←XML | Media-Server
343 | 08:42:20.350 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
344 | 08:42:20.357 |  |  |  |  | ←SIP MESSAGE | P-CSCF
345 | 08:42:21.267 |  |  |  |  | →SIP 200 OK | P-CSCF
346 | 08:42:23.276 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
347 | 08:42:23.344 |  | ←RRC DCCH RRC Connection Release |  |  |
348 | 08:42:23.345 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
349 | 08:42:23.375 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
350 | 08:42:23.379 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
351 | 08:42:23.379 |  |  |  |  | MMICmd: Make the MCPTT User request the creation of a pre-established session
352 | 08:42:31.752 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
353 | 08:42:31.752 |  | →RRC CCCH RRC Connection Request |  |  |
354 | 08:42:31.752 |  | ←RRC CCCH RRC Connection Setup |  |  |
355 | 08:42:31.752 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
356 | 08:42:31.805 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
357 | 08:42:31.805 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
358 | 08:42:31.805 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
359 | 08:42:31.805 |  |  |  | →NAS EMM Service request |  |
360 | 08:42:31.805 |  |  |  | NAS K-enb 3636b4e1d96ac881b3a6c363a0513b327... |  |
361 | 08:42:31.806 |  |  | RRC K-enb 3636b4e1d96ac881b3a6c363a0513b327... |  |  |
362 | 08:42:31.807 |  |  | RRC rrc-cip 37adeb2a39cc6d177873c30d9da34cc... |  |  |
363 | 08:42:31.807 |  |  | RRC rrc-int 81446611e684534ef319d352baa9cf8... |  |  |
364 | 08:42:31.807 |  |  | RRC up-cip 2c97b83bad64ff6d91daf1a2c265a944... |  |  |
365 | 08:42:31.807 |  |  | RRC up-int 673a5f531ca8018e4687b8caa1712d5c... |  |  |
366 | 08:42:31.807 |  | ←RRC DCCH Security Mode Command |  |  |
367 | 08:42:31.807 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
368 | 08:42:31.845 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
369 | 08:42:31.845 |  | →RRC DCCH Security Mode Complete |  |  |
370 | 08:42:31.845 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
371 | 08:42:31.845 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
372 | 08:42:31.885 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
373 | 08:42:31.885 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
374 | 08:42:31.893 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
375 | 08:42:31.911 |  |  |  |  | →SIP INVITE | P-CSCF
376 | 08:42:31.935 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
377 | 08:42:31.943 |  |  |  |  | ←SIP 100 Trying | P-CSCF
378 | 08:42:31.949 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
379 | 08:42:31.952 |  |  |  |  | ←SIP 200 OK | P-CSCF
380 | 08:42:31.955 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
381 | 08:42:32.590 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
382 | 08:42:32.590 |  | [EMBEDDED NAS IN NEXT RRC] ESM Activate dedicated EPS bearer conte... |  |  |
383 | 08:42:32.590 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
384 | 08:42:32.591 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration Activate dedicated EPS bearer context request |  |  |
385 | 08:42:32.645 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Activate dedicated EPS bearer context accept |  |  |  |
386 | 08:42:32.645 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
387 | 08:42:32.645 |  | →RRC DCCH UL Information Transfer |  |  |
388 | 08:42:32.645 |  | [EMBEDDED NAS IN PREV RRC] ESM Activate dedicated EPS bearer conte... |  |  |
389 | 08:42:32.645 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
390 | 08:42:32.728 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
391 | 08:42:32.773 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:sessionB@cf.mcstaasting.com SIP/2.0 |  |  |  |
392 | 08:42:32.788 |  |  |  |  | →SIP ACK | P-CSCF
393 | 08:42:34.799 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
394 | 08:42:34.844 |  | ←RRC DCCH RRC Connection Release |  |  |
395 | 08:42:34.845 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
396 | 08:42:34.875 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
397 | 08:42:34.876 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:733: Test-Body Step 1
398 | 08:42:34.878 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
399 | 08:42:34.878 |  |  |  |  | MMICmd: Make the MCPTT User request the establishment of an MCPTT pre-arranged group call using a pre-established session, automatic commencement mode, with implicit Floor Control
400 | 08:42:34.879 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:736: Test-Body Step 2
401 | 08:42:45.752 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
402 | 08:42:45.752 |  | →RRC CCCH RRC Connection Request |  |  |
403 | 08:42:45.752 |  | ←RRC CCCH RRC Connection Setup |  |  |
404 | 08:42:45.752 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
405 | 08:42:45.805 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
406 | 08:42:45.805 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
407 | 08:42:45.805 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
408 | 08:42:45.805 |  |  |  | →NAS EMM Service request |  |
409 | 08:42:45.805 |  |  |  | NAS K-enb dcb6c4203da3cded8489fd491011152d5... |  |
410 | 08:42:45.806 |  | ←RRC DCCH Security Mode Command |  |  |
411 | 08:42:45.806 |  |  | RRC K-enb dcb6c4203da3cded8489fd491011152d5... |  |  |
412 | 08:42:45.806 |  |  | RRC rrc-cip 67c21f65e1591c275f68aef127d2010... |  |  |
413 | 08:42:45.806 |  |  | RRC rrc-int a0c4c25c48dfb39ccfe67d4b64d2b1c... |  |  |
414 | 08:42:45.806 |  |  | RRC up-cip 69dde0086fa38439cfcc4d40da561d9e... |  |  |
415 | 08:42:45.806 |  |  | RRC up-int c9532f7c507f2de94b652154c0443030... |  |  |
416 | 08:42:45.807 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
417 | 08:42:45.845 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
418 | 08:42:45.845 |  | →RRC DCCH Security Mode Complete |  |  |
419 | 08:42:45.845 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
420 | 08:42:45.845 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
421 | 08:42:45.885 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
422 | 08:42:45.885 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
423 | 08:42:45.893 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
424 | 08:42:45.894 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
425 | 08:42:45.895 | →enobeB PCAP frame→ SIP over IPSEC: REFER sip:sessionB@cf.mcstaasting.com SIP/2.0 SIP XML: application/vnd.3gpp.mcptt-signed+xml SRTP frame: |  |  |  |
426 | 08:42:45.901 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
427 | 08:42:45.902 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
428 | 08:42:45.915 |  |  |  |  | →SIP REFER | P-CSCF
429 | 08:42:45.925 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
430 | 08:42:45.933 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
431 | 08:42:45.941 |  |  |  |  | XML→ | Media-Server
432 | 08:42:45.946 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
433 | 08:42:45.947 |  |  |  |  | XML→ | Media-Server
434 | 08:42:45.952 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:754: SRTP config: Master Key: 37E86B73BB0A19278421B5E9D9CEFF09, Master Salt: F36A7D9BDA463D2B79B3A202, MKI: 235C2777
435 | 08:42:45.952 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
436 | 08:42:45.955 |  |  |  |  | ←SIP 200 OK | P-CSCF
437 | 08:42:45.955 |  |  |  |  | ←Connect | Media-Server
438 | 08:42:45.965 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
439 | 08:42:45.973 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
440 | 08:42:45.979 |  | ←enobeB PCAP frame← |  |  |
441 | 08:42:45.985 |  |  |  |  | MCPC Acknowledgement→ | Media-Server
442 | 08:42:45.986 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:465: PreestablishedSessionAcknowledge Verdict: Pass
443 | 08:42:45.986 |  |  |  |  | Verdict PASS: MCPTT_GroupCall_MCX_IMS.ttcn:740: Step 2 Verdict: Pass
444 | 08:42:45.986 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:742: Test-Body Step 2A
445 | 08:42:45.986 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:747: Test-Body Step 7
446 | 08:42:45.987 |  |  |  |  | MMICmd: Make the MCPTT User leave the MCPTT session
447 | 08:42:45.987 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:750: Test-Body Step 8
448 | 08:42:45.987 |  |  |  |  | ←Floor Granted | Media-Server
449 | 08:42:46.005 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
450 | 08:42:46.013 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
451 | 08:42:46.045 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
452 | 08:42:46.053 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
453 | 08:42:46.085 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
454 | 08:42:49.188 |  |  |  |  | →SIP REFER | P-CSCF
455 | 08:42:49.192 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
456 | 08:42:49.200 |  |  |  |  | ←SIP 200 OK | P-CSCF
457 | 08:42:49.213 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
458 | 08:42:49.217 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
459 | 08:42:49.245 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
460 | 08:42:49.249 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
461 | 08:42:49.253 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
462 | 08:42:51.241 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
463 | 08:42:51.275 |  | ←RRC DCCH RRC Connection Release |  |  |
464 | 08:42:51.276 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
465 | 08:42:51.293 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
466 | 08:42:51.296 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
467 | 08:42:51.298 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
468 | 08:42:51.301 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
469 | 08:42:51.309 |  |  |  |  | ←SIP BYE | P-CSCF
470 | 08:42:51.372 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
471 | 08:42:51.372 |  | →RRC CCCH RRC Connection Request |  |  |
472 | 08:42:51.372 |  | ←RRC CCCH RRC Connection Setup |  |  |
473 | 08:42:51.372 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
474 | 08:42:51.405 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
475 | 08:42:51.405 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
476 | 08:42:51.405 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
477 | 08:42:51.405 |  |  |  | →NAS EMM Service request |  |
478 | 08:42:51.405 |  |  |  | NAS K-enb 974a9340b0deff0fca250c6d0e91492e9... |  |
479 | 08:42:51.406 |  | ←RRC DCCH Security Mode Command |  |  |
480 | 08:42:51.406 |  |  | RRC K-enb 974a9340b0deff0fca250c6d0e91492e9... |  |  |
481 | 08:42:51.406 |  |  | RRC rrc-cip ce5327e353029e6bc24c084ccd6d0c8... |  |  |
482 | 08:42:51.406 |  |  | RRC rrc-int c5d83a59f355954c31ad16c803d487a... |  |  |
483 | 08:42:51.406 |  |  | RRC up-cip 67f1178044fbabb00eb069fe7edbad85... |  |  |
484 | 08:42:51.406 |  |  | RRC up-int 6df54af467864d5253573e5bc194c87a... |  |  |
485 | 08:42:51.407 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
486 | 08:42:51.445 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
487 | 08:42:51.445 |  | →RRC DCCH Security Mode Complete |  |  |
488 | 08:42:51.445 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
489 | 08:42:51.445 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
490 | 08:42:51.485 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
491 | 08:42:51.485 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
492 | 08:42:51.487 |  | ←enobeB PCAP frame← SIP over IPSEC: BYE sip:sessionB@cf.mcstaasting.com SIP/2.0 |  |  |
493 | 08:42:51.493 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
494 | 08:42:51.497 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
495 | 08:42:51.498 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
496 | 08:42:51.501 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
497 | 08:42:51.505 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
498 | 08:42:51.546 |  |  |  |  | →SIP 200 OK | P-CSCF
499 | 08:42:51.765 | →enobeB PCAP frame→ |  |  |  |
500 | 08:42:52.452 |  | ←enobeB PCAP frame← LTE RRC PCCH Paging (1 PagingRecord) |  |  |
501 | 08:42:52.452 |  | ←RRC PCCH Paging |  |  |
502 | 08:42:53.549 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
503 | 08:42:53.549 |  | [EMBEDDED NAS IN NEXT RRC] ESM Deactivate EPS bearer context reque... |  |  |
504 | 08:42:53.549 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
505 | 08:42:53.550 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration Deactivate EPS bearer context request (Regular de... |  |  |
506 | 08:42:53.551 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
507 | 08:42:53.605 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Deactivate EPS bearer context accept |  |  |  |
508 | 08:42:53.605 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
509 | 08:42:53.605 |  | →RRC DCCH UL Information Transfer |  |  |
510 | 08:42:53.605 |  | [EMBEDDED NAS IN PREV RRC] ESM Deactivate EPS bearer context accep... |  |  |
511 | 08:42:53.605 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
512 | 08:42:53.681 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
513 | 08:42:53.682 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
514 | 08:42:53.707 |  | ←RRC DCCH RRC Connection Release |  |  |
515 | 08:42:53.708 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
516 | 08:42:53.738 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
517 | 08:42:53.740 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
518 | 08:42:53.742 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
519 | 08:42:54.490 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.