MSG #511 2021-12-17 08:42:53.605
NAS

     ESM: Deactivate EPS bearer context accept
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x2 (Integrity protected and ciphered)
    Auth code = 0xc1e7151f
    Sequence number = 0x08
    Protocol discriminator = 0x2 (EPS Session Management)
    EPS bearer identity = 6
    Procedure transaction identity = 0
    Message type = 0xce (Deactivate EPS bearer context accept)