ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 08:45:30.221 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 08:45:30.224 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 08:45:30.224 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 08:45:30.226 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 08:45:30.227 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 08:45:30.227 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:824: IMS UDP port 192.168.2.3:5060 configured
7 | 08:45:30.229 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:774: IMS TCP port 192.168.2.3:5060 configured!
8 | 08:45:30.230 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:795: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 08:45:30.231 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:806: IdM port 192.168.2.3:8080 configured!
10 | 08:45:30.233 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 08:45:31.435 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 08:45:31.437 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 08:45:32.713 |  | ←RRC BCCH SIB |  |  |
14 | 08:45:32.718 |  | ←RRC BCCH SIB1 |  |  |
15 | 08:45:32.798 |  | ←RRC BCCH SIB1 |  |  |
16 | 08:45:32.873 |  | ←RRC BCCH SIB |  |  |
17 | 08:45:32.878 |  | ←RRC BCCH SIB1 |  |  |
18 | 08:46:16.442 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 08:46:16.442 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 08:46:16.442 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 08:46:16.442 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 08:46:16.493 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 08:46:16.493 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 08:46:16.493 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 08:46:16.493 |  |  |  | →NAS EMM Attach request |  |
26 | 08:46:16.493 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 08:46:16.493 |  |  |  | NAS K-asme bba947d54ce375926f5c9f03a3bf4efd... |  |
28 | 08:46:16.493 |  |  |  | NAS ← EMM Authentication request |  |
29 | 08:46:16.494 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 08:46:16.494 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 08:46:16.495 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 08:46:16.565 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 08:46:16.565 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 08:46:16.565 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 08:46:16.565 |  |  |  | →NAS EMM Authentication response |  |
36 | 08:46:16.565 |  |  |  | NAS UE auth OK |  |
37 | 08:46:16.565 |  |  |  | NAS K-nas-cip 00000000000000000000000000000... |  |
38 | 08:46:16.565 |  |  |  | NAS K-nas-int a1a3fc2f2c63721482ed2bcdef415... |  |
39 | 08:46:16.565 |  |  |  | NAS ← EMM Security mode command |  |
40 | 08:46:16.566 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 08:46:16.566 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 08:46:16.567 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 08:46:16.605 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Security mode complete |  |  |  |
44 | 08:46:16.605 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 08:46:16.605 |  | [EMBEDDED NAS IN PREV RRC] EMM Security mode complete |  |  |
46 | 08:46:16.605 |  |  |  | →NAS EMM Security mode complete |  |
47 | 08:46:16.605 |  |  |  | NAS ← ESM ESM information request |  |
48 | 08:46:16.606 |  | [EMBEDDED NAS IN NEXT RRC] ESM ESM information request |  |  |
49 | 08:46:16.606 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 08:46:16.607 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer ESM information request |  |  |
51 | 08:46:16.653 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer ESM information response |  |  |  |
52 | 08:46:16.653 |  | →RRC DCCH UL Information Transfer |  |  |
53 | 08:46:16.653 |  | [EMBEDDED NAS IN PREV RRC] ESM ESM information response |  |  |
54 | 08:46:16.653 |  |  |  | →NAS ESM ESM information response |  |
55 | 08:46:16.653 |  |  |  | NAS K-enb bf37165ee4d06570522b2e0069a83ed0f... |  |
56 | 08:46:16.653 |  |  |  | NAS ← EMM Attach accept |  |
57 | 08:46:16.654 |  | ←RRC DCCH Security Mode Command |  |  |
58 | 08:46:16.654 |  |  | RRC K-enb bf37165ee4d06570522b2e0069a83ed0f... |  |  |
59 | 08:46:16.654 |  |  | RRC rrc-cip 20c87a7e5d934eb3af414178c2f6e34... |  |  |
60 | 08:46:16.654 |  |  | RRC rrc-int d4d1585d5d1f351f24a11152f41d09c... |  |  |
61 | 08:46:16.654 |  |  | RRC up-cip 5fbfdafe89bc5961e6164efb382292b3... |  |  |
62 | 08:46:16.654 |  |  | RRC up-int 10101a672f9b6274d21838c7afa3c3ea... |  |  |
63 | 08:46:16.655 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
64 | 08:46:16.685 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
65 | 08:46:16.685 |  | →RRC DCCH Security Mode Complete |  |  |
66 | 08:46:16.685 |  | ←RRC DCCH UE Capability Enquiry |  |  |
67 | 08:46:16.685 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
68 | 08:46:16.735 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
69 | 08:46:16.735 |  | →RRC DCCH UE Capability Information |  |  |
70 | 08:46:16.735 |  | [EMBEDDED NAS IN NEXT RRC] EMM Attach accept |  |  |
71 | 08:46:16.735 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
72 | 08:46:16.735 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration Attach accept Activate default EPS bearer context request (PDN ... |  |  |
73 | 08:46:16.765 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
74 | 08:46:16.765 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
75 | 08:46:16.805 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Attach complete Activate default EPS bearer context accept |  |  |  |
76 | 08:46:16.805 |  | →RRC DCCH UL Information Transfer |  |  |
77 | 08:46:16.805 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach complete |  |  |
78 | 08:46:16.805 |  |  |  | →NAS EMM Attach complete |  |
79 | 08:46:16.805 |  |  |  | NAS ← EMM EMM information |  |
80 | 08:46:16.806 |  | [EMBEDDED NAS IN NEXT RRC] EMM EMM information |  |  |
81 | 08:46:16.806 |  | ←RRC DCCH DL Information Transfer |  |  |
82 | 08:46:16.807 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer EMM information |  |  |
83 | 08:46:23.617 |  | ←RRC DCCH RRC Connection Release |  |  |
84 | 08:46:23.618 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
85 | 08:46:25.492 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
86 | 08:46:25.492 |  | →RRC CCCH RRC Connection Request |  |  |
87 | 08:46:25.492 |  | ←RRC CCCH RRC Connection Setup |  |  |
88 | 08:46:25.492 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
89 | 08:46:25.525 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
90 | 08:46:25.525 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
91 | 08:46:25.525 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
92 | 08:46:25.525 |  |  |  | →NAS EMM Service request |  |
93 | 08:46:25.525 |  |  |  | NAS K-enb 9ec0427ca076ab7aa2d444e5b92958f76... |  |
94 | 08:46:25.526 |  | ←RRC DCCH Security Mode Command |  |  |
95 | 08:46:25.526 |  |  | RRC K-enb 9ec0427ca076ab7aa2d444e5b92958f76... |  |  |
96 | 08:46:25.526 |  |  | RRC rrc-cip 145f8e6ca40fdf161cfbce23e708b1c... |  |  |
97 | 08:46:25.526 |  |  | RRC rrc-int a670e63ae7fa65b0cb8ee9033d3ba6c... |  |  |
98 | 08:46:25.526 |  |  | RRC up-cip 3316917161800121526cc1ca00cd8c79... |  |  |
99 | 08:46:25.526 |  |  | RRC up-int 158a5c606a65b3bba52084d6f48e9dce... |  |  |
100 | 08:46:25.527 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
101 | 08:46:25.565 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
102 | 08:46:25.565 |  | →RRC DCCH Security Mode Complete |  |  |
103 | 08:46:25.565 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
104 | 08:46:25.565 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
105 | 08:46:25.605 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
106 | 08:46:25.605 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
107 | 08:47:33.845 | →enobeB PCAP frame→ TCP |  |  |  |
108 | 08:47:33.849 |  | ←enobeB PCAP frame← TCP |  |  |
109 | 08:47:33.885 | →enobeB PCAP frame→ TCP |  |  |  |
110 | 08:47:33.973 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
111 | 08:47:33.977 |  | ←enobeB PCAP frame← TCP |  |  |
112 | 08:47:33.982 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
113 | 08:47:34.005 | →enobeB PCAP frame→ TCP |  |  |  |
114 | 08:47:34.173 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
115 | 08:47:34.177 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
116 | 08:47:34.188 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 16)
117 | 08:47:34.205 | →enobeB PCAP frame→ TCP |  |  |  |
118 | 08:47:34.265 |  | ←enobeB PCAP frame← TCP |  |  |
119 | 08:47:34.276 |  |  |  |  | →HTTP GET | HTTP-Proxy
120 | 08:47:34.277 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
121 | 08:47:34.282 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:307: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
122 | 08:47:34.287 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
123 | 08:47:36.805 | →enobeB PCAP frame→ TCP |  |  |  |
124 | 08:47:36.809 |  | ←enobeB PCAP frame← TCP |  |  |
125 | 08:47:36.845 | →enobeB PCAP frame→ TCP |  |  |  |
126 | 08:47:36.853 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
127 | 08:47:36.856 |  | ←enobeB PCAP frame← TCP |  |  |
128 | 08:47:36.862 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
129 | 08:47:36.885 | →enobeB PCAP frame→ TCP |  |  |  |
130 | 08:47:37.253 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
131 | 08:47:37.257 |  | ←enobeB PCAP frame← TCP |  |  |
132 | 08:47:37.258 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
133 | 08:47:37.268 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
134 | 08:47:37.285 | →enobeB PCAP frame→ TCP |  |  |  |
135 | 08:47:37.293 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
136 | 08:47:37.297 |  | ←enobeB PCAP frame← TCP |  |  |
137 | 08:47:37.300 |  | ←enobeB PCAP frame← TCP |  |  |
138 | 08:47:37.309 |  |  |  |  | →HTTP GET | IDMS-Endpoint
139 | 08:47:37.316 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
140 | 08:47:37.325 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
141 | 08:47:37.327 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:526: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
142 | 08:47:37.328 |  |  |  |  | MMICmd: Please provide user credentials: username and password
143 | 08:47:37.365 | →enobeB PCAP frame→ TCP |  |  |  |
144 | 08:47:41.893 | →enobeB PCAP frame→ HTTPS: POST /idms/userauth HTTP/1.1 |  |  |  |
145 | 08:47:41.897 |  | ←enobeB PCAP frame← TCP |  |  |
146 | 08:47:41.909 |  |  |  |  | →HTTP POST | IDMS-Endpoint
147 | 08:47:41.913 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
148 | 08:47:41.923 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
149 | 08:47:41.925 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:531: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
150 | 08:47:41.965 | →enobeB PCAP frame→ TCP |  |  |  |
151 | 08:47:41.973 | →enobeB PCAP frame→ TCP |  |  |  |
152 | 08:47:41.977 |  | ←enobeB PCAP frame← TCP |  |  |
153 | 08:47:41.987 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:693: IdM port - Client closed the connection (id 18)
154 | 08:47:42.005 | →enobeB PCAP frame→ TCP |  |  |  |
155 | 08:47:42.485 | →enobeB PCAP frame→ TCP |  |  |  |
156 | 08:47:42.489 |  | ←enobeB PCAP frame← TCP |  |  |
157 | 08:47:42.525 | →enobeB PCAP frame→ TCP |  |  |  |
158 | 08:47:42.613 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
159 | 08:47:42.617 |  | ←enobeB PCAP frame← TCP |  |  |
160 | 08:47:42.618 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
161 | 08:47:42.645 | →enobeB PCAP frame→ TCP |  |  |  |
162 | 08:47:42.773 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
163 | 08:47:42.777 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
164 | 08:47:42.787 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
165 | 08:47:42.805 | →enobeB PCAP frame→ TCP |  |  |  |
166 | 08:47:42.813 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
167 | 08:47:42.817 |  | ←enobeB PCAP frame← TCP |  |  |
168 | 08:47:42.826 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
169 | 08:47:42.828 |  |  |  |  | →HTTP POST | IDMS-Endpoint
170 | 08:47:42.835 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
171 | 08:47:42.839 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:536: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
172 | 08:47:42.885 | →enobeB PCAP frame→ TCP |  |  |  |
173 | 08:47:43.165 | →enobeB PCAP frame→ TCP |  |  |  |
174 | 08:47:43.169 |  | ←enobeB PCAP frame← TCP |  |  |
175 | 08:47:43.205 | →enobeB PCAP frame→ TCP |  |  |  |
176 | 08:47:43.213 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
177 | 08:47:43.217 |  | ←enobeB PCAP frame← TCP |  |  |
178 | 08:47:43.220 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
179 | 08:47:43.245 | →enobeB PCAP frame→ TCP |  |  |  |
180 | 08:47:43.253 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
181 | 08:47:43.256 |  | ←enobeB PCAP frame← TCP |  |  |
182 | 08:47:43.257 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
183 | 08:47:43.268 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 19)
184 | 08:47:43.293 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
185 | 08:47:43.297 |  | ←enobeB PCAP frame← TCP |  |  |
186 | 08:47:43.309 |  |  |  |  | →HTTP POST | HTTP-Proxy
187 | 08:47:43.333 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
188 | 08:47:43.333 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:554: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
189 | 08:47:43.341 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
190 | 08:47:43.365 | →enobeB PCAP frame→ TCP |  |  |  |
191 | 08:47:43.381 | →enobeB PCAP frame→ TCP |  |  |  |
192 | 08:47:43.385 |  | ←enobeB PCAP frame← TCP |  |  |
193 | 08:47:43.405 | →enobeB PCAP frame→ TCP |  |  |  |
194 | 08:47:43.413 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
195 | 08:47:43.417 |  | ←enobeB PCAP frame← TCP |  |  |
196 | 08:47:43.418 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
197 | 08:47:43.445 | →enobeB PCAP frame→ TCP |  |  |  |
198 | 08:47:43.453 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
199 | 08:47:43.457 |  | ←enobeB PCAP frame← TCP |  |  |
200 | 08:47:43.458 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
201 | 08:47:43.468 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 20)
202 | 08:47:43.512 |  | ←enobeB PCAP frame← TCP |  |  |
203 | 08:47:43.513 |  | ←enobeB PCAP frame← TCP |  |  |
204 | 08:47:43.525 |  |  |  |  | →HTTP POST | HTTP-Proxy
205 | 08:47:43.537 |  | ←enobeB PCAP frame← TCP |  |  |
206 | 08:47:43.581 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
207 | 08:47:43.590 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
208 | 08:47:43.590 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:558: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
209 | 08:47:43.718 |  |  |  |  | →SIP REGISTER | P-CSCF
210 | 08:47:43.741 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:833: IMS UDP_s port 192.168.2.3:5062 configured
211 | 08:47:43.765 |  | ←enobeB PCAP frame← SIP -cleartext-: SIP/2.0 401 Unauthorized |  |  |
212 | 08:47:43.768 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:784: IMS TCP_s port 192.168.2.3:5062 configured!
213 | 08:47:43.769 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:842: IMS UDP_c port 192.168.2.3:5061 configured
214 | 08:47:43.774 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
215 | 08:47:44.573 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
216 | 08:47:44.591 |  |  |  |  | →SIP REGISTER | P-CSCF
217 | 08:47:44.607 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
218 | 08:47:44.616 |  |  |  |  | ←SIP 200 OK | P-CSCF
219 | 08:47:44.933 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
220 | 08:47:44.934 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 SIP over IPSEC: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 |  |  |  |
221 | 08:47:44.961 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
222 | 08:47:45.018 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
223 | 08:47:45.027 |  |  |  |  | ←SIP 200 OK | P-CSCF
224 | 08:47:45.028 |  |  |  |  | MIKEY | Media-Server
225 | 08:47:45.232 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:39298;transp... |  |  |
226 | 08:47:45.233 |  |  |  |  | XML→ | Media-Server
227 | 08:47:45.234 |  |  |  |  | XML→ | Media-Server
228 | 08:47:45.238 |  |  |  |  | ←XML | Media-Server
229 | 08:47:45.242 |  |  |  |  | ←SIP NOTIFY | P-CSCF
230 | 08:47:45.293 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
231 | 08:47:45.308 |  |  |  |  | →SIP 200 OK | P-CSCF
232 | 08:47:45.485 | →enobeB PCAP frame→ TCP |  |  |  |
233 | 08:47:45.489 |  | ←enobeB PCAP frame← TCP |  |  |
234 | 08:47:45.525 | →enobeB PCAP frame→ TCP |  |  |  |
235 | 08:47:45.533 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
236 | 08:47:45.537 |  | ←enobeB PCAP frame← TCP |  |  |
237 | 08:47:45.541 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
238 | 08:47:45.565 | →enobeB PCAP frame→ TCP |  |  |  |
239 | 08:47:45.653 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
240 | 08:47:45.656 |  | ←enobeB PCAP frame← TCP |  |  |
241 | 08:47:45.657 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
242 | 08:47:45.668 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
243 | 08:47:45.685 | →enobeB PCAP frame→ TCP |  |  |  |
244 | 08:47:45.733 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
245 | 08:47:45.737 |  | ←enobeB PCAP frame← TCP |  |  |
246 | 08:47:45.748 |  |  |  |  | →HTTP GET | HTTP-Proxy
247 | 08:47:45.757 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
248 | 08:47:45.757 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:691: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcpttue-configuration.xml
249 | 08:47:45.765 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
250 | 08:47:45.805 | →enobeB PCAP frame→ TCP |  |  |  |
251 | 08:47:45.813 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
252 | 08:47:45.818 |  | ←enobeB PCAP frame← TCP |  |  |
253 | 08:47:45.828 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
254 | 08:47:45.845 | →enobeB PCAP frame→ TCP |  |  |  |
255 | 08:47:45.853 | →enobeB PCAP frame→ TCP |  |  |  |
256 | 08:47:45.857 |  | ←enobeB PCAP frame← TCP |  |  |
257 | 08:47:46.085 | →enobeB PCAP frame→ TCP |  |  |  |
258 | 08:47:46.090 |  | ←enobeB PCAP frame← TCP |  |  |
259 | 08:47:46.125 | →enobeB PCAP frame→ TCP |  |  |  |
260 | 08:47:46.133 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
261 | 08:47:46.137 |  | ←enobeB PCAP frame← TCP |  |  |
262 | 08:47:46.140 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
263 | 08:47:46.165 | →enobeB PCAP frame→ TCP |  |  |  |
264 | 08:47:46.213 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
265 | 08:47:46.217 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
266 | 08:47:46.228 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
267 | 08:47:46.245 | →enobeB PCAP frame→ TCP |  |  |  |
268 | 08:47:46.305 |  | ←enobeB PCAP frame← TCP |  |  |
269 | 08:47:46.316 |  |  |  |  | →HTTP GET | HTTP-Proxy
270 | 08:47:46.329 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:696: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcpttuser-profile-49.xml
271 | 08:47:46.377 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
272 | 08:47:46.378 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
273 | 08:47:46.380 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
274 | 08:47:46.421 | →enobeB PCAP frame→ TCP |  |  |  |
275 | 08:47:46.425 |  | ←enobeB PCAP frame← TCP |  |  |
276 | 08:47:46.429 | →enobeB PCAP frame→ TCP |  |  |  |
277 | 08:47:46.432 |  | ←enobeB PCAP frame← TCP |  |  |
278 | 08:47:46.435 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
279 | 08:47:46.445 | →enobeB PCAP frame→ TCP |  |  |  |
280 | 08:47:47.053 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
281 | 08:47:47.089 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
282 | 08:47:47.120 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
283 | 08:47:47.129 |  |  |  |  | ←SIP 200 OK | P-CSCF
284 | 08:47:47.129 |  |  |  |  | MIKEY | Media-Server
285 | 08:47:47.168 |  | ←enobeB PCAP frame← TCP |  |  |
286 | 08:47:47.213 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
287 | 08:47:47.216 |  | ←enobeB PCAP frame← TCP |  |  |
288 | 08:47:47.217 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
289 | 08:47:47.245 | →enobeB PCAP frame→ TCP |  |  |  |
290 | 08:47:47.326 |  |  |  |  | XML→ | Media-Server
291 | 08:47:47.326 |  |  |  |  | XML→ | Media-Server
292 | 08:47:47.330 |  |  |  |  | ←XML | Media-Server
293 | 08:47:47.333 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
294 | 08:47:47.336 |  | ←enobeB PCAP frame← TCP |  |  |
295 | 08:47:47.337 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
296 | 08:47:47.338 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:39298;transp... |  |  |
297 | 08:47:47.347 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
298 | 08:47:47.347 |  |  |  |  | ←SIP NOTIFY | P-CSCF
299 | 08:47:47.365 | →enobeB PCAP frame→ TCP |  |  |  |
300 | 08:47:47.385 |  | ←enobeB PCAP frame← TCP |  |  |
301 | 08:47:47.397 |  |  |  |  | →SIP 200 OK | P-CSCF
302 | 08:47:47.397 |  |  |  |  | →HTTP GET | HTTP-Proxy
303 | 08:47:47.402 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
304 | 08:47:47.405 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:701: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
305 | 08:47:47.411 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
306 | 08:47:47.453 | →enobeB PCAP frame→ TCP |  |  |  |
307 | 08:47:47.457 |  | ←enobeB PCAP frame← TCP |  |  |
308 | 08:47:47.467 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
309 | 08:47:47.485 | →enobeB PCAP frame→ TCP |  |  |  |
310 | 08:47:47.525 | →enobeB PCAP frame→ TCP |  |  |  |
311 | 08:47:47.528 |  | ←enobeB PCAP frame← TCP |  |  |
312 | 08:47:47.565 | →enobeB PCAP frame→ TCP |  |  |  |
313 | 08:47:47.573 | →enobeB PCAP frame→ TLS: Mix Info DNS |  |  |  |
314 | 08:47:47.577 |  | ←enobeB PCAP frame← TCP |  |  |
315 | 08:47:47.580 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
316 | 08:47:47.605 | →enobeB PCAP frame→ TCP |  |  |  |
317 | 08:47:47.693 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
318 | 08:47:47.696 |  | ←enobeB PCAP frame← TCP |  |  |
319 | 08:47:47.697 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
320 | 08:47:47.707 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
321 | 08:47:47.725 | →enobeB PCAP frame→ TCP |  |  |  |
322 | 08:47:47.733 | →enobeB PCAP frame→ HTTPS: GET http://xcap.gms.mcstaasting.com/org.openmobile... |  |  |  |
323 | 08:47:47.737 |  | ←enobeB PCAP frame← TCP |  |  |
324 | 08:47:47.748 |  |  |  |  | →HTTP GET | HTTP-Proxy
325 | 08:47:47.758 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:706: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at http://xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
326 | 08:47:47.782 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
327 | 08:47:47.783 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
328 | 08:47:47.788 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
329 | 08:47:47.805 | →enobeB PCAP frame→ TCP |  |  |  |
330 | 08:47:47.813 | →enobeB PCAP frame→ TCP |  |  |  |
331 | 08:47:47.845 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
332 | 08:47:47.849 |  | ←enobeB PCAP frame← TCP |  |  |
333 | 08:47:47.853 | →enobeB PCAP frame→ TCP |  |  |  |
334 | 08:47:47.856 |  | ←enobeB PCAP frame← TCP |  |  |
335 | 08:47:47.859 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
336 | 08:47:47.885 | →enobeB PCAP frame→ TCP |  |  |  |
337 | 08:47:48.056 |  |  |  |  | →SIP PUBLISH | P-CSCF
338 | 08:47:48.106 |  |  |  |  | MIKEY | Media-Server
339 | 08:47:48.129 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
340 | 08:47:48.314 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
341 | 08:47:48.317 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
342 | 08:47:48.320 |  |  |  |  | XML→ | Media-Server
343 | 08:47:48.323 |  |  |  |  | ←SIP 200 OK | P-CSCF
344 | 08:47:48.327 |  |  |  |  | ←SIP 200 OK | P-CSCF
345 | 08:47:48.327 |  |  |  |  | MIKEY | Media-Server
346 | 08:47:48.518 |  |  |  |  | XML→ | Media-Server
347 | 08:47:48.519 |  |  |  |  | XML→ | Media-Server
348 | 08:47:48.549 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:39298;transp... |  |  |
349 | 08:47:48.553 |  |  |  |  | MIKEY | Media-Server
350 | 08:47:48.553 |  |  |  |  | ←XML | Media-Server
351 | 08:47:48.558 |  |  |  |  | ←SIP NOTIFY | P-CSCF
352 | 08:47:48.627 |  |  |  |  | →SIP 200 OK | P-CSCF
353 | 08:47:48.632 |  |  |  |  | ←XML | Media-Server
354 | 08:47:48.640 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
355 | 08:47:48.648 |  |  |  |  | ←SIP MESSAGE | P-CSCF
356 | 08:47:49.508 |  |  |  |  | →SIP 200 OK | P-CSCF
357 | 08:47:51.518 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
358 | 08:47:51.594 |  | ←RRC DCCH RRC Connection Release |  |  |
359 | 08:47:51.595 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
360 | 08:47:51.627 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
361 | 08:47:51.630 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
362 | 08:47:51.630 |  |  |  |  | MMICmd: Make the MCPTT User request the creation of a pre-established session
363 | 08:47:58.452 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
364 | 08:47:58.452 |  | →RRC CCCH RRC Connection Request |  |  |
365 | 08:47:58.452 |  | ←RRC CCCH RRC Connection Setup |  |  |
366 | 08:47:58.452 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
367 | 08:47:58.485 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
368 | 08:47:58.485 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
369 | 08:47:58.485 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
370 | 08:47:58.485 |  |  |  | →NAS EMM Service request |  |
371 | 08:47:58.485 |  |  |  | NAS K-enb d7cef0806bf5bee89a28e91075155c08d... |  |
372 | 08:47:58.486 |  | ←RRC DCCH Security Mode Command |  |  |
373 | 08:47:58.486 |  |  | RRC K-enb d7cef0806bf5bee89a28e91075155c08d... |  |  |
374 | 08:47:58.486 |  |  | RRC rrc-cip 907f43f8ef94df042f5110844ecf640... |  |  |
375 | 08:47:58.486 |  |  | RRC rrc-int 932442a4742c0ccc7ff6d6d922b1b62... |  |  |
376 | 08:47:58.486 |  |  | RRC up-cip 6742597b7683b04fe8b00a1488fae9f1... |  |  |
377 | 08:47:58.486 |  |  | RRC up-int 5ff9e2c3f1f9a15f6334a561453e5cc3... |  |  |
378 | 08:47:58.487 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
379 | 08:47:58.525 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
380 | 08:47:58.525 |  | →RRC DCCH Security Mode Complete |  |  |
381 | 08:47:58.525 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
382 | 08:47:58.525 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
383 | 08:47:58.565 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
384 | 08:47:58.565 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
385 | 08:47:58.573 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
386 | 08:47:58.592 |  |  |  |  | →SIP INVITE | P-CSCF
387 | 08:47:58.598 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
388 | 08:47:58.601 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
389 | 08:47:58.606 |  |  |  |  | ←SIP 100 Trying | P-CSCF
390 | 08:47:58.610 |  |  |  |  | ←SIP 200 OK | P-CSCF
391 | 08:47:58.611 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
392 | 08:47:59.246 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
393 | 08:47:59.246 |  | [EMBEDDED NAS IN NEXT RRC] ESM Activate dedicated EPS bearer conte... |  |  |
394 | 08:47:59.246 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
395 | 08:47:59.247 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration Activate dedicated EPS bearer context request |  |  |
396 | 08:47:59.285 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Activate dedicated EPS bearer context accept |  |  |  |
397 | 08:47:59.285 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
398 | 08:47:59.285 |  | →RRC DCCH UL Information Transfer |  |  |
399 | 08:47:59.285 |  | [EMBEDDED NAS IN PREV RRC] ESM Activate dedicated EPS bearer conte... |  |  |
400 | 08:47:59.285 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
401 | 08:47:59.392 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
402 | 08:47:59.413 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:sessionB@cf.mcstaasting.com SIP/2.0 |  |  |  |
403 | 08:47:59.428 |  |  |  |  | →SIP ACK | P-CSCF
404 | 08:48:01.439 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
405 | 08:48:01.482 |  | ←RRC DCCH RRC Connection Release |  |  |
406 | 08:48:01.483 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
407 | 08:48:01.515 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
408 | 08:48:01.515 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:770: Test-Body Step 1
409 | 08:48:01.516 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
410 | 08:48:01.518 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
411 | 08:48:01.525 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:754: SRTP config: Master Key: 1AC21A293F77889E6456C89577E84464, Master Salt: C47B7CBC19F8D0D0C0A4A6DF, MKI: 2024ED92
412 | 08:48:01.525 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
413 | 08:48:01.528 |  |  |  |  | ←Connect | Media-Server
414 | 08:48:02.212 |  | ←enobeB PCAP frame← LTE RRC PCCH Paging (1 PagingRecord) |  |  |
415 | 08:48:02.212 |  | ←RRC PCCH Paging |  |  |
416 | 08:48:02.242 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
417 | 08:48:02.242 |  | →RRC CCCH RRC Connection Request |  |  |
418 | 08:48:02.242 |  | ←RRC CCCH RRC Connection Setup |  |  |
419 | 08:48:02.242 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
420 | 08:48:02.285 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
421 | 08:48:02.285 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
422 | 08:48:02.285 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
423 | 08:48:02.285 |  |  |  | →NAS EMM Service request |  |
424 | 08:48:02.285 |  |  |  | NAS K-enb 7235b074a58071662b48970f360aaf3ed... |  |
425 | 08:48:02.286 |  | ←RRC DCCH Security Mode Command |  |  |
426 | 08:48:02.286 |  |  | RRC K-enb 7235b074a58071662b48970f360aaf3ed... |  |  |
427 | 08:48:02.286 |  |  | RRC rrc-cip 7a283933f5d8c784ff26fe548641321... |  |  |
428 | 08:48:02.286 |  |  | RRC rrc-int bab1139bff8bd0db45bddc8f31a2738... |  |  |
429 | 08:48:02.286 |  |  | RRC up-cip 4fa83baddfb72403ef7a73791860b47b... |  |  |
430 | 08:48:02.286 |  |  | RRC up-int 622c1992af8c55df46582a2eb4550abc... |  |  |
431 | 08:48:02.287 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
432 | 08:48:02.325 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
433 | 08:48:02.325 |  | →RRC DCCH Security Mode Complete |  |  |
434 | 08:48:02.325 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
435 | 08:48:02.325 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
436 | 08:48:02.365 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
437 | 08:48:02.365 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
438 | 08:48:02.367 |  | ←enobeB PCAP frame← |  |  |
439 | 08:48:02.405 | →enobeB PCAP frame→ |  |  |  |
440 | 08:48:02.416 |  | ←enobeB PCAP frame← |  |  |
441 | 08:48:02.419 |  |  |  |  | MCPC Acknowledgement→ | Media-Server
442 | 08:48:02.422 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:465: PreestablishedSessionAcknowledge Verdict: Pass
443 | 08:48:02.422 |  |  |  |  | Verdict PASS: MCPTT_GroupCall_MCX_IMS.ttcn:772: Step 1 Verdict: Pass
444 | 08:48:02.422 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:776: Test-Body Step 3
445 | 08:48:02.425 |  |  |  |  | ←Disconnect | Media-Server
446 | 08:48:02.445 | →enobeB PCAP frame→ |  |  |  |
447 | 08:48:02.459 |  |  |  |  | MCPC Acknowledgement→ | Media-Server
448 | 08:48:02.462 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:465: PreestablishedSessionAcknowledge Verdict: Pass
449 | 08:48:04.463 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
450 | 08:48:04.496 |  | ←RRC DCCH RRC Connection Release |  |  |
451 | 08:48:04.497 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
452 | 08:48:04.528 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
453 | 08:48:04.529 |  |  |  |  | Verdict PASS: MCPTT_GroupCall_MCX_IMS.ttcn:778: Step 3 Verdict: Pass
454 | 08:48:04.530 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
455 | 08:48:04.533 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
456 | 08:48:04.541 |  |  |  |  | ←SIP BYE | P-CSCF
457 | 08:48:04.772 |  | ←enobeB PCAP frame← LTE RRC PCCH Paging (1 PagingRecord) |  |  |
458 | 08:48:04.772 |  | ←RRC PCCH Paging |  |  |
459 | 08:48:04.802 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
460 | 08:48:04.802 |  | →RRC CCCH RRC Connection Request |  |  |
461 | 08:48:04.802 |  | ←RRC CCCH RRC Connection Setup |  |  |
462 | 08:48:04.802 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
463 | 08:48:04.845 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
464 | 08:48:04.845 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
465 | 08:48:04.845 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
466 | 08:48:04.845 |  |  |  | →NAS EMM Service request |  |
467 | 08:48:04.845 |  |  |  | NAS K-enb 5a5f3c3900cd709469a2d7922724e3898... |  |
468 | 08:48:04.846 |  | ←RRC DCCH Security Mode Command |  |  |
469 | 08:48:04.846 |  |  | RRC K-enb 5a5f3c3900cd709469a2d7922724e3898... |  |  |
470 | 08:48:04.846 |  |  | RRC rrc-cip 92bffd6cc39171c4a1a32539f61299b... |  |  |
471 | 08:48:04.846 |  |  | RRC rrc-int 568a2a6b7a0c5296a15a0b40fa5adc3... |  |  |
472 | 08:48:04.846 |  |  | RRC up-cip b4875bd6cacd7255f834f082826783d0... |  |  |
473 | 08:48:04.846 |  |  | RRC up-int adc0904a73ef17f6d0f70cfc3689c9c3... |  |  |
474 | 08:48:04.847 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
475 | 08:48:04.885 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
476 | 08:48:04.885 |  | →RRC DCCH Security Mode Complete |  |  |
477 | 08:48:04.885 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
478 | 08:48:04.885 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
479 | 08:48:04.925 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
480 | 08:48:04.925 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
481 | 08:48:04.927 |  | ←enobeB PCAP frame← SIP over IPSEC: BYE sip:sessionB@cf.mcstaasting.com SIP/2.0 |  |  |
482 | 08:48:04.973 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
483 | 08:48:04.987 |  |  |  |  | →SIP 200 OK | P-CSCF
484 | 08:48:05.405 | →enobeB PCAP frame→ |  |  |  |
485 | 08:48:06.992 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
486 | 08:48:07.001 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
487 | 08:48:07.002 |  | [EMBEDDED NAS IN NEXT RRC] ESM Deactivate EPS bearer context reque... |  |  |
488 | 08:48:07.002 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
489 | 08:48:07.003 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration Deactivate EPS bearer context request (Regular de... |  |  |
490 | 08:48:07.045 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Deactivate EPS bearer context accept |  |  |  |
491 | 08:48:07.045 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
492 | 08:48:07.045 |  | →RRC DCCH UL Information Transfer |  |  |
493 | 08:48:07.045 |  | [EMBEDDED NAS IN PREV RRC] ESM Deactivate EPS bearer context accep... |  |  |
494 | 08:48:07.045 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
495 | 08:48:07.131 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
496 | 08:48:07.132 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
497 | 08:48:07.155 |  | ←RRC DCCH RRC Connection Release |  |  |
498 | 08:48:07.156 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
499 | 08:48:07.239 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
500 | 08:48:07.241 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
501 | 08:48:07.243 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
502 | 08:48:07.991 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.