MSG #35 2021-12-17 08:46:16.565
NAS

     EMM: Authentication response
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x1 (Integrity protected)
    Auth code = 0x95cd16fd
    Sequence number = 0x0c
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x0 (Plain NAS message, not security protected)
    Message type = 0x53 (Authentication response)
    Authentication response parameter:
      Length = 8
      Data = a3 a1 05 a1 ca 37 cb a9